(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "HSYNC_DAC2_B")
  (net 2 "HSYNC2")
  (net 3 "VSYNC_DAC1_B")
  (net 4 "GND")
  (net 5 "VSYNC_DAC2_B")
  (net 6 "VSYNC1")
  (net 7 "VSYNC2")
  (net 8 "+5V")
  (net 9 "HSYNC1")
  (net 10 "HSYNC_DAC1_B")
  (net 11 "+5V_VESA")
  (net 12 "+MVDD")
  (net 13 "XTALOUT")
  (net 14 "XTALIN")
  (net 15 "LDO6_VREF")
  (net 16 "LDO6_FB")
  (net 17 "+VDDCI_LDO")
  (net 18 "LDO6_VIN")
  (net 19 "N87118008")
  (net 20 "N87118444")
  (net 21 "LDO2_FB")
  (net 22 "+1.8V")
  (net 23 "LDO2_VIN")
  (net 24 "LDO_EN")
  (net 25 "N87118142")
  (net 26 "LDO3_FB")
  (net 27 "+1.1V")
  (net 28 "LDO3_VIN")
  (net 29 "N87118495")
  (net 30 "N87118038")
  (net 31 "+3.3V_BUS")
  (net 32 "N87118360")
  (net 33 "+12V_BUS")
  (net 34 "N87188969")
  (net 35 "+3.3V")
  (net 36 "+VDDCI")
  (net 37 "A_DAC2_B")
  (net 38 "A_B_DAC2_F")
  (net 39 "A_DAC2_G")
  (net 40 "A_G_DAC2_F")
  (net 41 "A_DAC2_R")
  (net 42 "A_R_DAC2_F")
  (net 43 "A_DAC1_B")
  (net 44 "A_B_DAC1_F")
  (net 45 "A_DAC1_G")
  (net 46 "A_G_DAC1_F")
  (net 47 "A_DAC1_R")
  (net 48 "A_R_DAC1_F")
  (net 49 "HSYNC_DAC2_R")
  (net 50 "DDCCLK_DAC2_R")
  (net 51 "VSYNC_DAC2_R")
  (net 52 "DDCDATA_DAC2_R")
  (net 53 "HSYNC_DAC1_R")
  (net 54 "DDCCLK_DAC1_R")
  (net 55 "VSYNC_DAC1_R")
  (net 56 "DDCDATA_DAC1_R")
  (net 57 "N86495082")
  (net 58 "N85769340")
  (net 59 "N85769021")
  (net 60 "+12V_EXT")
  (net 61 "N85769551")
  (net 62 "N85769539")
  (net 63 "UG2")
  (net 64 "BOOT2")
  (net 65 "BOOT1")
  (net 66 "UG1")
  (net 67 "LG2")
  (net 68 "APHASE_2")
  (net 69 "LG1")
  (net 70 "APHASE_1")
  (net 71 "PWM1")
  (net 72 "PWM2")
  (net 73 "PERST#")
  (net 74 "PERST#_BUF")
  (net 75 "THERMINT")
  (net 76 "GPU_DPLUS")
  (net 77 "GPU_DMINUS")
  (net 78 "LM63_PWM")
  (net 79 "SCL_R")
  (net 80 "SDA_R")
  (net 81 "N87528545")
  (net 82 "VDD_+5V")
  (net 83 "N86495804")
  (net 84 "MAD_4")
  (net 85 "MAD_5")
  (net 86 "MAD_8")
  (net 87 "MAD_7")
  (net 88 "MAD_6")
  (net 89 "MAD_9")
  (net 90 "MAD_0")
  (net 91 "MAD_1")
  (net 92 "MAD_2")
  (net 93 "MAD_11")
  (net 94 "MAD_10")
  (net 95 "MAD_3")
  (net 96 "MAD_BA1")
  (net 97 "MAD_BA0")
  (net 98 "RASD1B")
  (net 99 "CLKD1")
  (net 100 "WED1B")
  (net 101 "CSD1B_0")
  (net 102 "CLKD1B")
  (net 103 "CASD1B")
  (net 104 "DQMDB_5")
  (net 105 "DQMDB_7")
  (net 106 "DQMDB_6")
  (net 107 "DQMDB_4")
  (net 108 "DQD_45")
  (net 109 "DQD_46")
  (net 110 "DQD_58")
  (net 111 "DQD_62")
  (net 112 "DQD_63")
  (net 113 "DQD_61")
  (net 114 "DQD_56")
  (net 115 "DQD_59")
  (net 116 "DQD_48")
  (net 117 "DQD_51")
  (net 118 "DQD_49")
  (net 119 "DQD_50")
  (net 120 "DQD_44")
  (net 121 "DQD_52")
  (net 122 "DQD_54")
  (net 123 "DQD_53")
  (net 124 "DQD_55")
  (net 125 "DQD_37")
  (net 126 "DQD_39")
  (net 127 "DQD_36")
  (net 128 "DQD_38")
  (net 129 "DQD_35")
  (net 130 "DQD_34")
  (net 131 "DQD_47")
  (net 132 "DQD_33")
  (net 133 "DQD_32")
  (net 134 "DQD_43")
  (net 135 "DQD_42")
  (net 136 "DQD_41")
  (net 137 "DQD_40")
  (net 138 "DQD_57")
  (net 139 "DQD_60")
  (net 140 "QSD_5")
  (net 141 "QSD_7")
  (net 142 "QSD_6")
  (net 143 "QSD_4")
  (net 144 "DRAM_RST")
  (net 145 "MAD_BA2")
  (net 146 "N48570141")
  (net 147 "N48570039")
  (net 148 "N48570085")
  (net 149 "N48570109")
  (net 150 "QSDB_5")
  (net 151 "QSDB_7")
  (net 152 "QSDB_6")
  (net 153 "QSDB_4")
  (net 154 "CKED1")
  (net 155 "N48570117")
  (net 156 "RASD0B")
  (net 157 "CLKD0")
  (net 158 "WED0B")
  (net 159 "CSD0B_0")
  (net 160 "CLKD0B")
  (net 161 "CASD0B")
  (net 162 "DQMDB_1")
  (net 163 "DQMDB_2")
  (net 164 "DQMDB_3")
  (net 165 "DQMDB_0")
  (net 166 "DQD_13")
  (net 167 "DQD_12")
  (net 168 "DQD_20")
  (net 169 "DQD_23")
  (net 170 "DQD_18")
  (net 171 "DQD_19")
  (net 172 "DQD_16")
  (net 173 "DQD_17")
  (net 174 "DQD_31")
  (net 175 "DQD_30")
  (net 176 "DQD_24")
  (net 177 "DQD_25")
  (net 178 "DQD_15")
  (net 179 "DQD_28")
  (net 180 "DQD_27")
  (net 181 "DQD_29")
  (net 182 "DQD_26")
  (net 183 "DQD_5")
  (net 184 "DQD_7")
  (net 185 "DQD_4")
  (net 186 "DQD_6")
  (net 187 "DQD_3")
  (net 188 "DQD_1")
  (net 189 "DQD_14")
  (net 190 "DQD_2")
  (net 191 "DQD_0")
  (net 192 "DQD_8")
  (net 193 "DQD_9")
  (net 194 "DQD_10")
  (net 195 "DQD_11")
  (net 196 "DQD_21")
  (net 197 "DQD_22")
  (net 198 "QSD_1")
  (net 199 "QSD_2")
  (net 200 "QSD_3")
  (net 201 "QSD_0")
  (net 202 "N48569853")
  (net 203 "N48569969")
  (net 204 "N48569889")
  (net 205 "N48569804")
  (net 206 "QSDB_1")
  (net 207 "QSDB_2")
  (net 208 "QSDB_3")
  (net 209 "QSDB_0")
  (net 210 "CKED0")
  (net 211 "N48569967")
  (net 212 "MAC_4")
  (net 213 "MAC_5")
  (net 214 "MAC_8")
  (net 215 "MAC_7")
  (net 216 "MAC_6")
  (net 217 "MAC_9")
  (net 218 "MAC_0")
  (net 219 "MAC_1")
  (net 220 "MAC_2")
  (net 221 "MAC_11")
  (net 222 "MAC_10")
  (net 223 "MAC_3")
  (net 224 "MAC_BA1")
  (net 225 "MAC_BA0")
  (net 226 "RASC1B")
  (net 227 "CLKC1")
  (net 228 "WEC1B")
  (net 229 "CSC1B_0")
  (net 230 "CLKC1B")
  (net 231 "CASC1B")
  (net 232 "DQMCB_4")
  (net 233 "DQMCB_5")
  (net 234 "DQMCB_7")
  (net 235 "DQMCB_6")
  (net 236 "DQC_39")
  (net 237 "DQC_36")
  (net 238 "DQC_42")
  (net 239 "DQC_43")
  (net 240 "DQC_45")
  (net 241 "DQC_46")
  (net 242 "DQC_47")
  (net 243 "DQC_44")
  (net 244 "DQC_58")
  (net 245 "DQC_59")
  (net 246 "DQC_56")
  (net 247 "DQC_57")
  (net 248 "DQC_38")
  (net 249 "DQC_60")
  (net 250 "DQC_62")
  (net 251 "DQC_61")
  (net 252 "DQC_63")
  (net 253 "DQC_53")
  (net 254 "DQC_55")
  (net 255 "DQC_52")
  (net 256 "DQC_54")
  (net 257 "DQC_51")
  (net 258 "DQC_49")
  (net 259 "DQC_37")
  (net 260 "DQC_50")
  (net 261 "DQC_48")
  (net 262 "DQC_34")
  (net 263 "DQC_35")
  (net 264 "DQC_33")
  (net 265 "DQC_32")
  (net 266 "DQC_40")
  (net 267 "DQC_41")
  (net 268 "QSC_4")
  (net 269 "QSC_5")
  (net 270 "QSC_7")
  (net 271 "QSC_6")
  (net 272 "MAC_BA2")
  (net 273 "N48027876")
  (net 274 "N48027825")
  (net 275 "N48027848")
  (net 276 "N48027858")
  (net 277 "QSCB_4")
  (net 278 "QSCB_5")
  (net 279 "QSCB_7")
  (net 280 "QSCB_6")
  (net 281 "CKEC1")
  (net 282 "N48027864")
  (net 283 "RASC0B")
  (net 284 "CLKC0")
  (net 285 "WEC0B")
  (net 286 "CSC0B_0")
  (net 287 "CLKC0B")
  (net 288 "CASC0B")
  (net 289 "DQMCB_1")
  (net 290 "DQMCB_2")
  (net 291 "DQMCB_3")
  (net 292 "DQMCB_0")
  (net 293 "DQC_15")
  (net 294 "DQC_14")
  (net 295 "DQC_23")
  (net 296 "DQC_20")
  (net 297 "DQC_19")
  (net 298 "DQC_18")
  (net 299 "DQC_16")
  (net 300 "DQC_17")
  (net 301 "DQC_26")
  (net 302 "DQC_27")
  (net 303 "DQC_24")
  (net 304 "DQC_25")
  (net 305 "DQC_13")
  (net 306 "DQC_28")
  (net 307 "DQC_30")
  (net 308 "DQC_29")
  (net 309 "DQC_31")
  (net 310 "DQC_5")
  (net 311 "DQC_6")
  (net 312 "DQC_4")
  (net 313 "DQC_7")
  (net 314 "DQC_3")
  (net 315 "DQC_1")
  (net 316 "DQC_12")
  (net 317 "DQC_2")
  (net 318 "DQC_0")
  (net 319 "DQC_11")
  (net 320 "DQC_10")
  (net 321 "DQC_9")
  (net 322 "DQC_8")
  (net 323 "DQC_22")
  (net 324 "DQC_21")
  (net 325 "QSC_1")
  (net 326 "QSC_2")
  (net 327 "QSC_3")
  (net 328 "QSC_0")
  (net 329 "N48027732")
  (net 330 "N48027790")
  (net 331 "N48027750")
  (net 332 "N48027731")
  (net 333 "QSCB_1")
  (net 334 "QSCB_2")
  (net 335 "QSCB_3")
  (net 336 "QSCB_0")
  (net 337 "CKEC0")
  (net 338 "N48027789")
  (net 339 "MAB_4")
  (net 340 "MAB_5")
  (net 341 "MAB_8")
  (net 342 "MAB_7")
  (net 343 "MAB_6")
  (net 344 "MAB_9")
  (net 345 "MAB_0")
  (net 346 "MAB_1")
  (net 347 "MAB_2")
  (net 348 "MAB_11")
  (net 349 "MAB_10")
  (net 350 "MAB_3")
  (net 351 "MAB_BA1")
  (net 352 "MAB_BA0")
  (net 353 "RASB1B")
  (net 354 "CLKB1")
  (net 355 "WEB1B")
  (net 356 "CSB1B_0")
  (net 357 "CLKB1B")
  (net 358 "CASB1B")
  (net 359 "DQMBB_5")
  (net 360 "DQMBB_7")
  (net 361 "DQMBB_6")
  (net 362 "DQMBB_4")
  (net 363 "DQB_45")
  (net 364 "DQB_46")
  (net 365 "DQB_63")
  (net 366 "DQB_61")
  (net 367 "DQB_59")
  (net 368 "DQB_58")
  (net 369 "DQB_56")
  (net 370 "DQB_57")
  (net 371 "DQB_50")
  (net 372 "DQB_51")
  (net 373 "DQB_48")
  (net 374 "DQB_49")
  (net 375 "DQB_44")
  (net 376 "DQB_54")
  (net 377 "DQB_52")
  (net 378 "DQB_53")
  (net 379 "DQB_55")
  (net 380 "DQB_37")
  (net 381 "DQB_39")
  (net 382 "DQB_38")
  (net 383 "DQB_36")
  (net 384 "DQB_35")
  (net 385 "DQB_33")
  (net 386 "DQB_47")
  (net 387 "DQB_34")
  (net 388 "DQB_32")
  (net 389 "DQB_43")
  (net 390 "DQB_42")
  (net 391 "DQB_41")
  (net 392 "DQB_40")
  (net 393 "DQB_60")
  (net 394 "DQB_62")
  (net 395 "QSB_5")
  (net 396 "QSB_7")
  (net 397 "QSB_6")
  (net 398 "QSB_4")
  (net 399 "MAB_BA2")
  (net 400 "N49338068")
  (net 401 "N49337966")
  (net 402 "N49338012")
  (net 403 "N49337708")
  (net 404 "QSBB_5")
  (net 405 "QSBB_7")
  (net 406 "QSBB_6")
  (net 407 "QSBB_4")
  (net 408 "CKEB1")
  (net 409 "N49338044")
  (net 410 "RASB0B")
  (net 411 "CLKB0")
  (net 412 "WEB0B")
  (net 413 "CSB0B_0")
  (net 414 "CLKB0B")
  (net 415 "CASB0B")
  (net 416 "DQMBB_2")
  (net 417 "DQMBB_1")
  (net 418 "DQMBB_3")
  (net 419 "DQMBB_0")
  (net 420 "DQB_20")
  (net 421 "DQB_23")
  (net 422 "DQB_15")
  (net 423 "DQB_12")
  (net 424 "DQB_10")
  (net 425 "DQB_11")
  (net 426 "DQB_8")
  (net 427 "DQB_9")
  (net 428 "DQB_26")
  (net 429 "DQB_27")
  (net 430 "DQB_24")
  (net 431 "DQB_25")
  (net 432 "DQB_22")
  (net 433 "DQB_31")
  (net 434 "DQB_30")
  (net 435 "DQB_29")
  (net 436 "DQB_28")
  (net 437 "DQB_5")
  (net 438 "DQB_7")
  (net 439 "DQB_4")
  (net 440 "DQB_6")
  (net 441 "DQB_3")
  (net 442 "DQB_1")
  (net 443 "DQB_21")
  (net 444 "DQB_2")
  (net 445 "DQB_0")
  (net 446 "DQB_17")
  (net 447 "DQB_16")
  (net 448 "DQB_18")
  (net 449 "DQB_19")
  (net 450 "DQB_13")
  (net 451 "DQB_14")
  (net 452 "QSB_2")
  (net 453 "QSB_1")
  (net 454 "QSB_3")
  (net 455 "QSB_0")
  (net 456 "N49337776")
  (net 457 "N49337896")
  (net 458 "N49337065")
  (net 459 "N49337758")
  (net 460 "QSBB_2")
  (net 461 "QSBB_1")
  (net 462 "QSBB_3")
  (net 463 "QSBB_0")
  (net 464 "CKEB0")
  (net 465 "N49337894")
  (net 466 "MAA_4")
  (net 467 "MAA_5")
  (net 468 "MAA_8")
  (net 469 "MAA_7")
  (net 470 "MAA_6")
  (net 471 "MAA_9")
  (net 472 "MAA_0")
  (net 473 "MAA_1")
  (net 474 "MAA_2")
  (net 475 "MAA_11")
  (net 476 "MAA_10")
  (net 477 "MAA_3")
  (net 478 "MAA_BA1")
  (net 479 "MAA_BA0")
  (net 480 "RASA1B")
  (net 481 "CLKA1")
  (net 482 "WEA1B")
  (net 483 "CSA1B_0")
  (net 484 "CLKA1B")
  (net 485 "CASA1B")
  (net 486 "DQMAB_4")
  (net 487 "DQMAB_5")
  (net 488 "DQMAB_7")
  (net 489 "DQMAB_6")
  (net 490 "DQA_38")
  (net 491 "DQA_39")
  (net 492 "DQA_46")
  (net 493 "DQA_45")
  (net 494 "DQA_43")
  (net 495 "DQA_42")
  (net 496 "DQA_40")
  (net 497 "DQA_41")
  (net 498 "DQA_57")
  (net 499 "DQA_58")
  (net 500 "DQA_56")
  (net 501 "DQA_59")
  (net 502 "DQA_32")
  (net 503 "DQA_60")
  (net 504 "DQA_62")
  (net 505 "DQA_63")
  (net 506 "DQA_61")
  (net 507 "DQA_53")
  (net 508 "DQA_55")
  (net 509 "DQA_54")
  (net 510 "DQA_52")
  (net 511 "DQA_50")
  (net 512 "DQA_51")
  (net 513 "DQA_37")
  (net 514 "DQA_49")
  (net 515 "DQA_48")
  (net 516 "DQA_35")
  (net 517 "DQA_36")
  (net 518 "DQA_34")
  (net 519 "DQA_33")
  (net 520 "DQA_44")
  (net 521 "DQA_47")
  (net 522 "QSA_4")
  (net 523 "QSA_5")
  (net 524 "QSA_7")
  (net 525 "QSA_6")
  (net 526 "MAA_BA2")
  (net 527 "N25405207")
  (net 528 "N25405099")
  (net 529 "N25405147")
  (net 530 "N25405167")
  (net 531 "QSAB_4")
  (net 532 "QSAB_5")
  (net 533 "QSAB_7")
  (net 534 "QSAB_6")
  (net 535 "CKEA1")
  (net 536 "N25405181")
  (net 537 "RASA0B")
  (net 538 "CLKA0")
  (net 539 "WEA0B")
  (net 540 "CSA0B_0")
  (net 541 "CLKA0B")
  (net 542 "CASA0B")
  (net 543 "DQMAB_1")
  (net 544 "DQMAB_2")
  (net 545 "DQMAB_3")
  (net 546 "DQMAB_0")
  (net 547 "DQA_13")
  (net 548 "DQA_14")
  (net 549 "DQA_23")
  (net 550 "DQA_20")
  (net 551 "DQA_19")
  (net 552 "DQA_18")
  (net 553 "DQA_16")
  (net 554 "DQA_17")
  (net 555 "DQA_25")
  (net 556 "DQA_27")
  (net 557 "DQA_24")
  (net 558 "DQA_26")
  (net 559 "DQA_15")
  (net 560 "DQA_30")
  (net 561 "DQA_29")
  (net 562 "DQA_31")
  (net 563 "DQA_28")
  (net 564 "DQA_7")
  (net 565 "DQA_5")
  (net 566 "DQA_4")
  (net 567 "DQA_6")
  (net 568 "DQA_3")
  (net 569 "DQA_1")
  (net 570 "DQA_12")
  (net 571 "DQA_2")
  (net 572 "DQA_0")
  (net 573 "DQA_11")
  (net 574 "DQA_10")
  (net 575 "DQA_9")
  (net 576 "DQA_8")
  (net 577 "DQA_21")
  (net 578 "DQA_22")
  (net 579 "QSA_1")
  (net 580 "QSA_2")
  (net 581 "QSA_3")
  (net 582 "QSA_0")
  (net 583 "N25404817")
  (net 584 "N25405001")
  (net 585 "N25404871")
  (net 586 "N25404815")
  (net 587 "QSAB_1")
  (net 588 "QSAB_2")
  (net 589 "QSAB_3")
  (net 590 "QSAB_0")
  (net 591 "CKEA0")
  (net 592 "N25404999")
  (net 593 "ROMCSB_R")
  (net 594 "GPIO_10_R")
  (net 595 "GPIO_9_R")
  (net 596 "GPIO_8_R")
  (net 597 "LG3")
  (net 598 "APHASE_3")
  (net 599 "UG3")
  (net 600 "N86495166")
  (net 601 "PWM3")
  (net 602 "A_DAC1_BB")
  (net 603 "PETN6_GFXRN6")
  (net 604 "PETP6_GFXRP6")
  (net 605 "PETN7_GFXRN7")
  (net 606 "PETP7_GFXRP7")
  (net 607 "PETN8_GFXRN8")
  (net 608 "PETP8_GFXRP8")
  (net 609 "PETN9_GFXRN9")
  (net 610 "PETP9_GFXRP9")
  (net 611 "PETN10_GFXRN10")
  (net 612 "PETP10_GFXRP10")
  (net 613 "PETN11_GFXRN11")
  (net 614 "PETP11_GFXRP11")
  (net 615 "A_DAC1_RB")
  (net 616 "+PCIE_VDDR")
  (net 617 "GND_VSS1DI")
  (net 618 "+PCIE_PVDD")
  (net 619 "PETN0_GFXRN0")
  (net 620 "PETP0_GFXRP0")
  (net 621 "PETN1_GFXRN1")
  (net 622 "PETP1_GFXRP1")
  (net 623 "PETN2_GFXRN2")
  (net 624 "PETP2_GFXRP2")
  (net 625 "PETN3_GFXRN3")
  (net 626 "PETP3_GFXRP3")
  (net 627 "PETN4_GFXRN4")
  (net 628 "PETP4_GFXRP4")
  (net 629 "PETN5_GFXRN5")
  (net 630 "PETP5_GFXRP5")
  (net 631 "GND_AVSSQ")
  (net 632 "+AVDD")
  (net 633 "GFXTN6_PERN6")
  (net 634 "GFXTN7_PERN7")
  (net 635 "GFXTN8_PERN8")
  (net 636 "GFXTN9_PERN9")
  (net 637 "GFXTN10_PERN10")
  (net 638 "GFXTN11_PERN11")
  (net 639 "PCIE_REFCLKN")
  (net 640 "GFXTN0_PERN0")
  (net 641 "GFXTP0_PERP0")
  (net 642 "GFXTN1_PERN1")
  (net 643 "GFXTP1_PERP1")
  (net 644 "GFXTN2_PERN2")
  (net 645 "GFXTN3_PERN3")
  (net 646 "GFXTN4_PERN4")
  (net 647 "GFXTN5_PERN5")
  (net 648 "A_DAC1_GB")
  (net 649 "DDC4DATA")
  (net 650 "VID_3")
  (net 651 "A_DAC2_Y")
  (net 652 "A_DAC2_RB")
  (net 653 "T2X3M")
  (net 654 "A_DAC2_COMP")
  (net 655 "+T2PVDD")
  (net 656 "T2X3P")
  (net 657 "VID_1")
  (net 658 "VID_2")
  (net 659 "VID_6")
  (net 660 "VID_5")
  (net 661 "GPIO_22_ROMCSB")
  (net 662 "R2SET")
  (net 663 "T2X4M")
  (net 664 "GPIO_6")
  (net 665 "VID_4")
  (net 666 "T1X3M")
  (net 667 "+DPLL_PVDD")
  (net 668 "A_DAC2_C")
  (net 669 "+T2XVDD")
  (net 670 "T1X3P")
  (net 671 "GENERICC")
  (net 672 "DVPDATA_18")
  (net 673 "GND_PVSS")
  (net 674 "+DPLL_VDDC")
  (net 675 "DDC3DATA")
  (net 676 "+A2VDD")
  (net 677 "GND_T2PVSS")
  (net 678 "T1XCM")
  (net 679 "T1XCP")
  (net 680 "+VDDR_DVP")
  (net 681 "DVPDATA_21")
  (net 682 "+TXVDDR")
  (net 683 "T1X0M")
  (net 684 "T1X0P")
  (net 685 "T1X1M")
  (net 686 "T1X1P")
  (net 687 "T1X2M")
  (net 688 "T1X2P")
  (net 689 "+TPVDD")
  (net 690 "GND_TPVSS")
  (net 691 "T1X4P")
  (net 692 "T1X4M")
  (net 693 "GND_VSS2DI")
  (net 694 "+VDD2DI")
  (net 695 "T1X5P")
  (net 696 "T1X5M")
  (net 697 "T2XCP")
  (net 698 "T2XCM")
  (net 699 "T2X0P")
  (net 700 "T2X0M")
  (net 701 "T2X1P")
  (net 702 "T2X1M")
  (net 703 "T2X2P")
  (net 704 "T2X2M")
  (net 705 "A_DAC2_BB")
  (net 706 "A_DAC2_GB")
  (net 707 "VID_0")
  (net 708 "PLL_TEST")
  (net 709 "DDC4CLK")
  (net 710 "VID_7")
  (net 711 "DDC2DATA")
  (net 712 "T2X4P")
  (net 713 "T2X5M")
  (net 714 "T2X5P")
  (net 715 "DDC2CLK")
  (net 716 "+PCIE_VDDC")
  (net 717 "PETN14_GFXRN14")
  (net 718 "+VDDRHA")
  (net 719 "MVREFS_A")
  (net 720 "GND_VSSRHA")
  (net 721 "GFXTP14_PERP14")
  (net 722 "GFXTN14_PERN14")
  (net 723 "PETP15_GFXRP15")
  (net 724 "PETN15_GFXRN15")
  (net 725 "PETN12_GFXRN12")
  (net 726 "PETN13_GFXRN13")
  (net 727 "GFXTN15_PERN15")
  (net 728 "GFXTP15_PERP15")
  (net 729 "PETP13_GFXRP13")
  (net 730 "MVREFD_A")
  (net 731 "+MPVDD")
  (net 732 "GND_MPVSS")
  (net 733 "GND_VSSRHB")
  (net 734 "MVREFS_C")
  (net 735 "+VDDC")
  (net 736 "GND_VSSRHD")
  (net 737 "+VDDRHD")
  (net 738 "MVREFS_D")
  (net 739 "MVREFD_D")
  (net 740 "N72779223")
  (net 741 "PCIE_REFCLKP")
  (net 742 "GFXTP9_PERP9")
  (net 743 "GFXTP11_PERP11")
  (net 744 "GFXTP3_PERP3")
  (net 745 "GFXTN13_PERN13")
  (net 746 "GFXTP5_PERP5")
  (net 747 "GFXTN12_PERN12")
  (net 748 "GFXTP13_PERP13")
  (net 749 "GFXTP12_PERP12")
  (net 750 "DVPDATA_17")
  (net 751 "HPD1")
  (net 752 "DVPDATA_14")
  (net 753 "DVALID")
  (net 754 "GENERICA")
  (net 755 "MVREFS_B")
  (net 756 "DDC3CLK")
  (net 757 "GFXTP7_PERP7")
  (net 758 "+VDDRHC")
  (net 759 "MVREFD_C")
  (net 760 "MVREFD_B")
  (net 761 "+VDDRHB")
  (net 762 "PETP14_GFXRP14")
  (net 763 "GND_VSSRHC")
  (net 764 "+VDD1DI")
  (net 765 "DDC1CLK")
  (net 766 "DDC1DATA")
  (net 767 "GND_A2VSSQ")
  (net 768 "RSET")
  (net 769 "N16984571")
  (net 770 "GFXTP6_PERP6")
  (net 771 "N16984567")
  (net 772 "GFXTP4_PERP4")
  (net 773 "TEST_EN")
  (net 774 "GFXTP2_PERP2")
  (net 775 "PETP12_GFXRP12")
  (net 776 "GFXTP10_PERP10")
  (net 777 "GFXTP8_PERP8")
  (net 778 "GPIO_12")
  (net 779 "N74256579")
  (net 780 "DVPDATA_23")
  (net 781 "+A2VDDQ")
  (net 782 "DVPDATA_9")
  (net 783 "DVPCNTL_2")
  (net 784 "GPIO_9")
  (net 785 "GPIO_0")
  (net 786 "DVPDATA_15")
  (net 787 "GPIO_5")
  (net 788 "GPIO_1")
  (net 789 "GPIO_3")
  (net 790 "GPIO_17_INT")
  (net 791 "GPIO_4")
  (net 792 "PSYNC")
  (net 793 "N52040509")
  (net 794 "DVPCNTL_1")
  (net 795 "+VDD_CT")
  (net 796 "N52040505")
  (net 797 "DVPDATA_10")
  (net 798 "GPIO_11")
  (net 799 "DVPDATA_20")
  (net 800 "GENERICB")
  (net 801 "DVPDATA_19")
  (net 802 "DVPDATA_5")
  (net 803 "DVPDATA_8")
  (net 804 "DVPDATA_7")
  (net 805 "DVPDATA_3")
  (net 806 "PCIE_CLK_REQB")
  (net 807 "JTAG_MODE")
  (net 808 "DVPCNTL_0")
  (net 809 "DVPDATA_6")
  (net 810 "DVPDATA_11")
  (net 811 "DVOCLK")
  (net 812 "DVPDATA_4")
  (net 813 "DVPDATA_0")
  (net 814 "DVPDATA_1")
  (net 815 "DVPDATA_2")
  (net 816 "DVP_MVP_CNTL_1")
  (net 817 "DVP_MVP_CNTL_0")
  (net 818 "HPD2")
  (net 819 "DVPDATA_12")
  (net 820 "GPIO_8")
  (net 821 "VREFG")
  (net 822 "GPIO_10")
  (net 823 "GPIO_13")
  (net 824 "TS_FDO")
  (net 825 "DVPDATA_13")
  (net 826 "GPIO_7")
  (net 827 "GPIO_2")
  (net 828 "DVPDATA_22")
  (net 829 "DVPDATA_16")
  (net 830 "N49971242")
  (net 831 "N72974574")
  (net 832 "TACH")
  (net 833 "N87189147")
  (net 834 "N49971220")
  (net 835 "N49971448")
  (net 836 "N72984167")
  (net 837 "N87189157")
  (net 838 "N87189202")
  (net 839 "PWM")
  (net 840 "N81403017")
  (net 841 "DDCCLK_DAC2_5V")
  (net 842 "DDCDATA_DAC2_5V")
  (net 843 "DDCCLK_DAC1_5V")
  (net 844 "DDCDATA_DAC1_5V")
  (net 845 "GENERICB_R")
  (net 846 "DVALID_R")
  (net 847 "PIN6")
  (net 848 "JTDI")
  (net 849 "JTDO")
  (net 850 "N84002959")
  (net 851 "N86495700")
  (net 852 "N86495698")
  (net 853 "LVT_EN")
  (net 854 "N87188971")
  (net 855 "N73051201")
  (net 856 "N73046901")
  (net 857 "N85769033")
  (net 858 "N85769031")
  (net 859 "N49971328")
  (net 860 "N21778115")
  (net 861 "N26590941")
  (net 862 "N42099087")
  (net 863 "PWM3_VIN")
  (net 864 "N86495503")
  (net 865 "PWM2_VIN")
  (net 866 "N86494416")
  (net 867 "PWM1_VIN")
  (net 868 "N86496210")
  (net 869 "PERN0")
  (net 870 "PERN1")
  (net 871 "PERN10")
  (net 872 "PERN11")
  (net 873 "PERN12")
  (net 874 "PERN13")
  (net 875 "PERN14")
  (net 876 "PERN15")
  (net 877 "PERN2")
  (net 878 "PERN3")
  (net 879 "PERN4")
  (net 880 "PERN5")
  (net 881 "PERN6")
  (net 882 "PERN7")
  (net 883 "PERN8")
  (net 884 "PERN9")
  (net 885 "PERP0")
  (net 886 "PERP1")
  (net 887 "PERP10")
  (net 888 "PERP11")
  (net 889 "PERP12")
  (net 890 "PERP13")
  (net 891 "PERP14")
  (net 892 "PERP15")
  (net 893 "PERP2")
  (net 894 "PERP3")
  (net 895 "PERP4")
  (net 896 "PERP5")
  (net 897 "PERP6")
  (net 898 "PERP7")
  (net 899 "PERP8")
  (net 900 "PERP9")
  (net 901 "PRESENCE")
  (net 902 "DAC2_COMP_F")
  (net 903 "DAC2_C_F")
  (net 904 "DAC2_Y_F")
  (net 905 "HPD_DVI1")
  (net 906 "HPD_DVI2")
  (net 907 "N85769402")
  (net 908 "N85769514")
  (net 909 "N85769388")
  (net 910 "N85769537")
  (net 911 "N85769434")
  (net 912 "N85769464")
  (net 913 "N85769062")
  (net 914 "N86494319")
  (net 915 "N85769214")
  (net 916 "N86495541")
  (net 917 "N86495162")
  (net 918 "N86494866")
  (net 919 "N86496570")
  (net 920 "N86496268")
  (net 921 "N86494727")
  (net 922 "N86494729")
  (net 923 "N86494909")
  (net 924 "N86494873")
  (net 925 "N86495210")
  (net 926 "VID_SEL")
  (net 927 "N86495035")
  (net 928 "N86496297")
  (net 929 "N86496246")
  (net 930 "N86495047")
  (net 931 "N86495281")
  (net 932 "AICSN24")
  (net 933 "AICSN35")
  (net 934 "ACISP1")
  (net 935 "ACISP2")
  (net 936 "ACISP3")
  (net 937 "N86494646")
  (net 938 "N86495516")
  (net 939 "N86494697")
  (net 940 "N864960700")
  (net 941 "N864966460")
  (net 942 "N864945390")
  (net 943 "N86494757")
  (net 944 "N86495338")
  (net 945 "AICSN1")
  (net 946 "N86495180")
  (footprint "RES1608_1" (layer "F.Cu")
    (tedit 0)
    (at -41.995377 83.351007 90)
    (fp_text reference "R1023" (at -2.540025 2.222475 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 90) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 818 "HPD2"))
    (pad "2" smd rect (at 0 0.7874 90) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "560UF_4V_R71D55_1" (layer "F.Cu")
    (tedit 0)
    (at 112.526615 48.540002 180)
    (fp_text reference "EC1156" (at 1.346835 0.005715 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole rect (at -1.75006 0 180) (size 1.8034 1.8034) (drill 1.397) (layers *.Cu *.Mask)
      (net 735 "+VDDC"))
    (pad "2" thru_hole circle (at 1.75006 0 180) (size 1.8034 1.8034) (drill 1.397) (layers *.Cu *.Mask)
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at 158.246615 39.904002 180)
    (fp_text reference "AC9" (at -1.5875 -1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 945 "AICSN1"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 934 "ACISP1"))
  )
  (footprint "CAP1608_1" (layer "F.Cu")
    (tedit 0)
    (at -40.69538 60.551002)
    (fp_text reference "C3005" (at 2.222475 2.540025 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 903 "DAC2_C_F"))
    (pad "2" smd rect (at 0 0.7874) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "GEOM0012_1" (layer "F.Cu")
    (tedit 0)
    (at 162.564615 66.828002 180)
    (fp_text reference "EB17" (at -1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 -2.500122 180) (size 1.905 1.905) (drill 1.143) (layers *.Cu *.Mask)
      (net 60 "+12V_EXT"))
    (pad "2" thru_hole circle (at 0 2.500122 180) (size 1.905 1.905) (drill 1.143) (layers *.Cu *.Mask)
      (net 867 "PWM1_VIN"))
  )
  (footprint "CHK4417C_3R3S01_1" (layer "F.Cu")
    (tedit 0)
    (at 122.686615 22.632002 90)
    (fp_text reference "EL64" (at -1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 5.0038 90) (size 3.048 3.048) (drill 2.032) (layers *.Cu *.Mask)
      (net 59 "N85769021"))
    (pad "2" thru_hole circle (at 0 -5.0038 90) (size 3.048 3.048) (drill 2.032) (layers *.Cu *.Mask)
      (net 12 "+MVDD"))
  )
  (footprint "C1206_113_1" (layer "F.Cu")
    (tedit 0)
    (at 112.526615 62.891002 180)
    (fp_text reference "EC1149" (at 0.981075 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd oval (at -1.4351 0 180) (size 0.9779 1.1938) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd oval (at 1.4351 0 180) (size 0.9779 1.1938) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1608_1" (layer "F.Cu")
    (tedit 0)
    (at 153.776215 61.443202 90)
    (fp_text reference "AC75" (at -1.905025 1.904975 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 90) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 939 "N86494697"))
    (pad "2" smd rect (at 0 0.7874 90) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "APHASE_1"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at 148.086615 32.220502 -90)
    (fp_text reference "AR54" (at 1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 943 "N86494757"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "TP055PRI_1" (layer "F.Cu")
    (tedit 0)
    (at 25.604615 84.151005)
    (fp_text reference "TP11" (at -1.27 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd circle (at 0 0) (size 0.550012 0.550012) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 626 "PETP3_GFXRP3"))
  )
  (footprint "CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at 154.055615 26.696002)
    (fp_text reference "AC17" (at 1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 920 "N86496268"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at 21.104624 64.950993 180)
    (fp_text reference "R106" (at -1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 697 "T2XCP"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 698 "T2XCM"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at 154.119115 39.904002)
    (fp_text reference "AR31" (at 1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 936 "ACISP3"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 598 "APHASE_3"))
  )
  (footprint "IND2012_1" (layer "F.Cu")
    (tedit 0)
    (at -37.895385 60.651001)
    (fp_text reference "L3002" (at 1.024655 1.158837 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 0.889 180) (size 1.799996 0.999998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 668 "A_DAC2_C"))
    (pad "2" smd rect (at 0 -0.889 180) (size 1.799996 0.999998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 903 "DAC2_C_F"))
  )
  (footprint "RES1608_1" (layer "F.Cu")
    (tedit 0)
    (at 148.543815 52.578602 180)
    (fp_text reference "AR63" (at -1.904975 -1.905025 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 180) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "+12V_EXT"))
    (pad "2" smd rect (at 0 0.7874 180) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 916 "N86495541"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at 20.204625 63.750995 180)
    (fp_text reference "R115" (at -1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 695 "T1X5P"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 696 "T1X5M"))
  )
  (footprint "TP089X043_1" (layer "F.Cu")
    (tedit 0)
    (at -26.411385 8.090502)
    (fp_text reference "TP86" (at -1.27 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 0.5588 0.5588) (drill 0.250012) (layers *.Cu *.Mask)
      (net 794 "DVPCNTL_1"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at 150.753615 36.729002 90)
    (fp_text reference "AR40" (at -1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 932 "AICSN24"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 927 "N86495035"))
  )
  (footprint "TP089X043_1" (layer "F.Cu")
    (tedit 0)
    (at -19.895396 8.305005)
    (fp_text reference "TP63" (at -1.27 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 0.5588 0.5588) (drill 0.250012) (layers *.Cu *.Mask)
      (net 805 "DVPDATA_3"))
  )
  (footprint "IND2012_1" (layer "F.Cu")
    (tedit 0)
    (at -38.095385 67.751013)
    (fp_text reference "L3001" (at 1.024655 1.158837 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 0.889 180) (size 1.799996 0.999998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 651 "A_DAC2_Y"))
    (pad "2" smd rect (at 0 -0.889 180) (size 1.799996 0.999998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 904 "DAC2_Y_F"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at 42.404606 21.851003 -90)
    (fp_text reference "R410" (at 1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 282 "N48027864"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -49.395388 8.151005 180)
    (fp_text reference "MR54" (at -1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 791 "GPIO_4"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at 20.204625 68.651011)
    (fp_text reference "R102" (at 1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 704 "T2X2M"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 703 "T2X2P"))
  )
  (footprint "GEOM0013_1" (layer "F.Cu")
    (tedit 0)
    (at 96.397615 11.964002)
    (fp_text reference "C4009" (at 1.111516 1.27033 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144) (size 1.27 1.219987) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 830 "N49971242"))
    (pad "2" smd rect (at 0 0.9144) (size 1.27 1.219987) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "SOT23_3PIN_1" (layer "F.Cu")
    (tedit 0)
    (at 151.515615 52.731002 -90)
    (fp_text reference "ED30" (at 1.381125 -1.38115 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.9398 1.143 270) (size 0.640004 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 916 "N86495541"))
    (pad "2" smd rect (at 0.9398 1.143 270) (size 0.640004 1.27) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "3" smd rect (at 0 -1.143 270) (size 0.640004 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 64 "BOOT2"))
  )
  (footprint "TP055PRI_1" (layer "F.Cu")
    (tedit 0)
    (at 24.704616 83.151007)
    (fp_text reference "TP10" (at -1.27 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd circle (at 0 0) (size 0.550012 0.550012) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 623 "PETN2_GFXRN2"))
  )
  (footprint "CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at 163.453615 35.205002 90)
    (fp_text reference "AC6" (at -1.27 1.5875 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 931 "N86495281"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at 21.104624 57.651007)
    (fp_text reference "R110" (at 1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 683 "T1X0M"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 684 "T1X0P"))
  )
  (footprint "C1206_113_1" (layer "F.Cu")
    (tedit 0)
    (at 165.485615 27.585002)
    (fp_text reference "EC138" (at -0.981075 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd oval (at -1.4351 0) (size 0.9779 1.1938) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 82 "VDD_+5V"))
    (pad "2" smd oval (at 1.4351 0) (size 0.9779 1.1938) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "SO8_1" (layer "F.Cu")
    (tedit 0)
    (at -5.653895 64.361205 180)
    (fp_text reference "U4001" (at -2.2225 -2.54 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd oval (at -2.032 2.6797 180) (size 0.8636 1.6002) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "+3.3V"))
    (pad "2" smd oval (at -0.635 2.6797 180) (size 0.6096 1.7272) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 76 "GPU_DPLUS"))
    (pad "3" smd oval (at 0.635 2.6797 180) (size 0.6096 1.7272) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 77 "GPU_DMINUS"))
    (pad "4" smd oval (at 2.032 2.6797 180) (size 0.8636 1.6002) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 78 "LM63_PWM"))
    (pad "5" smd oval (at 2.032 -2.6797 180) (size 0.8636 1.6002) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "6" smd oval (at 0.635 -2.6797 180) (size 0.6096 1.7272) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 75 "THERMINT"))
    (pad "7" smd oval (at -0.635 -2.6797 180) (size 0.6096 1.7272) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 80 "SDA_R"))
    (pad "8" smd oval (at -2.032 -2.6797 180) (size 0.8636 1.6002) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 79 "SCL_R"))
  )
  (footprint "RES1608_1" (layer "F.Cu")
    (tedit 0)
    (at 133.105187 13.615002 90)
    (fp_text reference "ER307" (at -2.540025 2.222475 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 90) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 909 "N85769388"))
    (pad "2" smd rect (at 0 0.7874 90) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 910 "N85769537"))
  )
  (footprint "TP055PRI_1" (layer "F.Cu")
    (tedit 0)
    (at 44.004603 83.151007)
    (fp_text reference "TP26" (at -1.27 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd circle (at 0 0) (size 0.550012 0.550012) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 717 "PETN14_GFXRN14"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -0.795383 42.951011 -90)
    (fp_text reference "R297" (at 1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 793 "N52040509"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "SOIC8_1" (layer "F.Cu")
    (tedit 0)
    (at 121.416615 7.519002 90)
    (fp_text reference "EMU42" (at -2.54 2.2225 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd oval (at -2.032 2.58064 90) (size 0.889 1.4605) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 915 "N85769214"))
    (pad "2" smd oval (at -0.635 2.58064 90) (size 0.635 1.5875) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 909 "N85769388"))
    (pad "3" smd oval (at 0.635 2.58064 90) (size 0.635 1.5875) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "4" smd oval (at 2.032 2.58064 90) (size 0.889 1.4605) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 907 "N85769402"))
    (pad "5" smd oval (at 2.032 -2.58064 90) (size 0.889 1.4605) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "+12V_EXT"))
    (pad "6" smd oval (at 0.635 -2.58064 90) (size 0.635 1.5875) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 911 "N85769434"))
    (pad "7" smd oval (at -0.635 -2.58064 90) (size 0.635 1.5875) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 913 "N85769062"))
    (pad "8" smd oval (at -2.032 -2.58064 90) (size 0.889 1.4605) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 59 "N85769021"))
  )
  (footprint "SOT23_3PIN_1" (layer "F.Cu")
    (tedit 0)
    (at 93.095615 10.059002)
    (fp_text reference "TQ4010" (at 1.227697 1.534579 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.9398 1.143) (size 0.640004 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 856 "N73046901"))
    (pad "2" smd rect (at 0.9398 1.143) (size 0.640004 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "3" smd rect (at 0 -1.143) (size 0.640004 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 831 "N72974574"))
  )
  (footprint "TP089X043_1" (layer "F.Cu")
    (tedit 0)
    (at -10.545377 48.000989)
    (fp_text reference "TP80" (at -1.27 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 0.5588 0.5588) (drill 0.250012) (layers *.Cu *.Mask)
      (net 799 "DVPDATA_20"))
  )
  (footprint "TP089X043_1" (layer "F.Cu")
    (tedit 0)
    (at -7.995394 50.450996)
    (fp_text reference "TP78" (at -1.27 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 0.5588 0.5588) (drill 0.250012) (layers *.Cu *.Mask)
      (net 672 "DVPDATA_18"))
  )
  (footprint "TP089X043_1" (layer "F.Cu")
    (tedit 0)
    (at -26.395383 6.905008)
    (fp_text reference "TP85" (at -1.27 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 0.5588 0.5588) (drill 0.250012) (layers *.Cu *.Mask)
      (net 808 "DVPCNTL_0"))
  )
  (footprint "CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -28.010391 75.771012)
    (fp_text reference "C844" (at 1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 854 "N87188971"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -40.995379 88.450997)
    (fp_text reference "C1003" (at 2.2225 2.54 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 44 "A_B_DAC1_F"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "SOT23_3PIN_1" (layer "F.Cu")
    (tedit 0)
    (at -20.895394 71.751005)
    (fp_text reference "Q845" (at 1.38115 1.381125 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.9398 1.143) (size 0.640004 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 853 "LVT_EN"))
    (pad "2" smd rect (at 0.9398 1.143) (size 0.640004 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "+3.3V"))
    (pad "3" smd rect (at 0 -1.143) (size 0.640004 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "+3.3V_BUS"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at 150.753615 34.443002 -90)
    (fp_text reference "AR52" (at 1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 929 "N86496246"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 925 "N86495210"))
  )
  (footprint "CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at 104.271615 94.133002 90)
    (fp_text reference "C1035" (at -2.54 2.2225 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "560UF_4V_R71D55_1" (layer "F.Cu")
    (tedit 0)
    (at 112.653615 37.618002 180)
    (fp_text reference "EC1155" (at 1.346835 0.005715 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole rect (at -1.75006 0 180) (size 1.8034 1.8034) (drill 1.397) (layers *.Cu *.Mask)
      (net 735 "+VDDC"))
    (pad "2" thru_hole circle (at 1.75006 0 180) (size 1.8034 1.8034) (drill 1.397) (layers *.Cu *.Mask)
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at 78.871615 18.060002 90)
    (fp_text reference "C1030" (at -2.54 2.2225 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -12.407882 61.361211 180)
    (fp_text reference "R4032" (at -2.2225 -2.54 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "+3.3V"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 824 "TS_FDO"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -2.39538 68.95101 180)
    (fp_text reference "R40" (at -1.5875 -1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "+3.3V"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 675 "DDC3DATA"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at 21.104624 62.550998 180)
    (fp_text reference "R114" (at -1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 691 "T1X4P"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 692 "T1X4M"))
  )
  (footprint "SOIC8_1" (layer "F.Cu")
    (tedit 0)
    (at 151.642615 76.861002 90)
    (fp_text reference "U10" (at -1.27 1.5875 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd oval (at -2.032 2.58064 90) (size 0.889 1.4605) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 600 "N86495166"))
    (pad "2" smd oval (at -0.635 2.58064 90) (size 0.635 1.5875) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 601 "PWM3"))
    (pad "3" smd oval (at 0.635 2.58064 90) (size 0.635 1.5875) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "4" smd oval (at 2.032 2.58064 90) (size 0.889 1.4605) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "+12V_EXT"))
    (pad "5" smd oval (at 2.032 -2.58064 90) (size 0.889 1.4605) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 597 "LG3"))
    (pad "6" smd oval (at 0.635 -2.58064 90) (size 0.635 1.5875) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "7" smd oval (at -0.635 -2.58064 90) (size 0.635 1.5875) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 598 "APHASE_3"))
    (pad "8" smd oval (at -2.032 -2.58064 90) (size 0.889 1.4605) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 599 "UG3"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at 20.204625 61.251 180)
    (fp_text reference "R113" (at -1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 670 "T1X3P"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 666 "T1X3M"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at 100.842615 10.821002 90)
    (fp_text reference "R4033" (at -2.54 2.2225 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 832 "TACH"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at 161.167615 26.696002 180)
    (fp_text reference "AR16" (at -1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 914 "N86494319"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 82 "VDD_+5V"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at 159.643615 24.918002 90)
    (fp_text reference "AR80" (at -1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 946 "N86495180"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -7.495395 41.450989 -135)
    (fp_text reference "R52" (at -0.224506 -2.020558 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 225) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "+3.3V"))
    (pad "2" smd rect (at 0 0.492608 225) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 827 "GPIO_2"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -27.700384 73.951 -90)
    (fp_text reference "R847" (at 1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 854 "N87188971"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "+1.8V"))
  )
  (footprint "CAP1608_1" (layer "F.Cu")
    (tedit 0)
    (at 130.052615 54.890002 180)
    (fp_text reference "AC26" (at -1.904975 -1.905025 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 180) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 942 "N864945390"))
    (pad "2" smd rect (at 0 0.7874 180) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "TP089X043_1" (layer "F.Cu")
    (tedit 0)
    (at -16.095378 8.205005)
    (fp_text reference "TP87" (at -1.27 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 0.5588 0.5588) (drill 0.250012) (layers *.Cu *.Mask)
      (net 783 "DVPCNTL_2"))
  )
  (footprint "C1206_113_1" (layer "F.Cu")
    (tedit 0)
    (at 150.626615 11.583002 -90)
    (fp_text reference "MC1604" (at 0 0.981075 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd oval (at -1.4351 0 270) (size 0.9779 1.1938) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "+12V_EXT"))
    (pad "2" smd oval (at 1.4351 0 270) (size 0.9779 1.1938) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at 20.204625 66.25099)
    (fp_text reference "R100" (at 1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 700 "T2X0M"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 699 "T2X0P"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -1.395382 66.751015 180)
    (fp_text reference "R4001" (at -2.2225 -2.54 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 756 "DDC3CLK"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 79 "SCL_R"))
  )
  (footprint "GEOM0002_1" (layer "F.Cu")
    (tedit 0)
    (at 40.004611 14.151018 180)
    (fp_text reference "U402" (at -1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "A1" smd circle (at -4.399991 -6.399987 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "A2" smd circle (at -3.599993 -6.400013 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "A3" smd circle (at -2.799994 -6.400013 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "A4" smd circle (at -1.999996 -6.400013 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 282 "N48027864"))
    (pad "A9" smd circle (at 1.999996 -6.400013 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "A10" smd circle (at 2.799994 -6.400013 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "A11" smd circle (at 3.599993 -6.400013 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "A12" smd circle (at 4.399991 -6.399987 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "B1" smd circle (at -4.399991 -5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "B2" smd circle (at -3.599993 -5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 236 "DQC_39"))
    (pad "B3" smd circle (at -2.799994 -5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 237 "DQC_36"))
    (pad "B4" smd circle (at -1.999996 -5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "B9" smd circle (at 1.999996 -5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "B10" smd circle (at 2.799994 -5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 267 "DQC_41"))
    (pad "B11" smd circle (at 3.599993 -5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 266 "DQC_40"))
    (pad "B12" smd circle (at 4.399991 -5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "C1" smd circle (at -4.399991 -4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "C2" smd circle (at -3.599993 -4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 248 "DQC_38"))
    (pad "C3" smd circle (at -2.799994 -4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 259 "DQC_37"))
    (pad "C4" smd circle (at -1.999996 -4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "C9" smd circle (at 1.999996 -4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "C10" smd circle (at 2.799994 -4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 239 "DQC_43"))
    (pad "C11" smd circle (at 3.599993 -4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 238 "DQC_42"))
    (pad "C12" smd circle (at 4.399991 -4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "D1" smd circle (at -4.399991 -3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "D2" smd circle (at -3.599993 -3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 277 "QSCB_4"))
    (pad "D3" smd circle (at -2.799994 -3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 268 "QSC_4"))
    (pad "D4" smd circle (at -1.999996 -3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "D9" smd circle (at 1.999996 -3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "D10" smd circle (at 2.799994 -3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 269 "QSC_5"))
    (pad "D11" smd circle (at 3.599993 -3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 278 "QSCB_5"))
    (pad "D12" smd circle (at 4.399991 -3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "E1" smd circle (at -4.399991 -3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "E2" smd circle (at -3.599993 -3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 262 "DQC_34"))
    (pad "E3" smd circle (at -2.799994 -3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 232 "DQMCB_4"))
    (pad "E4" smd circle (at -1.999996 -3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "E9" smd circle (at 1.999996 -3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "E10" smd circle (at 2.799994 -3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 233 "DQMCB_5"))
    (pad "E11" smd circle (at 3.599993 -3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 240 "DQC_45"))
    (pad "E12" smd circle (at 4.399991 -3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "F1" smd circle (at -4.399991 -2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "F2" smd circle (at -3.599993 -2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 264 "DQC_33"))
    (pad "F3" smd circle (at -2.799994 -2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 263 "DQC_35"))
    (pad "F4" smd circle (at -1.999996 -2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 229 "CSC1B_0"))
    (pad "F9" smd circle (at 1.999996 -2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 231 "CASC1B"))
    (pad "F10" smd circle (at 2.799994 -2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 241 "DQC_46"))
    (pad "F11" smd circle (at 3.599993 -2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 242 "DQC_47"))
    (pad "F12" smd circle (at 4.399991 -2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "G1" smd circle (at -4.399991 -1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "G2" smd circle (at -3.599993 -1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "G3" smd circle (at -2.799994 -1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 265 "DQC_32"))
    (pad "G4" smd circle (at -1.999996 -1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 224 "MAC_BA1"))
    (pad "G9" smd circle (at 1.999996 -1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 225 "MAC_BA0"))
    (pad "G10" smd circle (at 2.799994 -1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 243 "DQC_44"))
    (pad "G11" smd circle (at 3.599993 -1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "G12" smd circle (at 4.399991 -1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "H1" smd circle (at -4.399991 -0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 275 "N48027848"))
    (pad "H2" smd circle (at -3.599993 -0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 213 "MAC_5"))
    (pad "H3" smd circle (at -2.799994 -0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 272 "MAC_BA2"))
    (pad "H4" smd circle (at -1.999996 -0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 228 "WEC1B"))
    (pad "H9" smd circle (at 1.999996 -0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 281 "CKEC1"))
    (pad "H10" smd circle (at 2.799994 -0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 226 "RASC1B"))
    (pad "H11" smd circle (at 3.599993 -0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 219 "MAC_1"))
    (pad "H12" smd circle (at 4.399991 -0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 276 "N48027858"))
    (pad "J1" smd circle (at -4.399991 0 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "J2" smd circle (at -3.599993 0 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "J3" smd circle (at -2.799994 0 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "J4" smd circle (at -1.999996 0 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "J9" smd circle (at 1.999996 0 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "J10" smd circle (at 2.799994 0 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 230 "CLKC1B"))
    (pad "J11" smd circle (at 3.599993 0 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 227 "CLKC1"))
    (pad "J12" smd circle (at 4.399991 0 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "K1" smd circle (at -4.399991 0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 273 "N48027876"))
    (pad "K2" smd circle (at -3.599993 0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 214 "MAC_8"))
    (pad "K3" smd circle (at -2.799994 0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 216 "MAC_6"))
    (pad "K4" smd circle (at -1.999996 0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 212 "MAC_4"))
    (pad "K9" smd circle (at 1.999996 0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 218 "MAC_0"))
    (pad "K10" smd circle (at 2.799994 0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 220 "MAC_2"))
    (pad "K11" smd circle (at 3.599993 0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 222 "MAC_10"))
    (pad "K12" smd circle (at 4.399991 0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 274 "N48027825"))
    (pad "L1" smd circle (at -4.399991 1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "L2" smd circle (at -3.599993 1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "L3" smd circle (at -2.799994 1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 254 "DQC_55"))
    (pad "L4" smd circle (at -1.999996 1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 215 "MAC_7"))
    (pad "L9" smd circle (at 1.999996 1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 221 "MAC_11"))
    (pad "L10" smd circle (at 2.799994 1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 245 "DQC_59"))
    (pad "L11" smd circle (at 3.599993 1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "L12" smd circle (at 4.399991 1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "M1" smd circle (at -4.399991 2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "M2" smd circle (at -3.599993 2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 253 "DQC_53"))
    (pad "M3" smd circle (at -2.799994 2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 256 "DQC_54"))
    (pad "M4" smd circle (at -1.999996 2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 217 "MAC_9"))
    (pad "M9" smd circle (at 1.999996 2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 223 "MAC_3"))
    (pad "M10" smd circle (at 2.799994 2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 247 "DQC_57"))
    (pad "M11" smd circle (at 3.599993 2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 244 "DQC_58"))
    (pad "M12" smd circle (at 4.399991 2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "N1" smd circle (at -4.399991 3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "N2" smd circle (at -3.599993 3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 255 "DQC_52"))
    (pad "N3" smd circle (at -2.799994 3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 235 "DQMCB_6"))
    (pad "N4" smd circle (at -1.999996 3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "N9" smd circle (at 1.999996 3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "N10" smd circle (at 2.799994 3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 234 "DQMCB_7"))
    (pad "N11" smd circle (at 3.599993 3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 246 "DQC_56"))
    (pad "N12" smd circle (at 4.399991 3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "P1" smd circle (at -4.399991 3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "P2" smd circle (at -3.599993 3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 280 "QSCB_6"))
    (pad "P3" smd circle (at -2.799994 3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 271 "QSC_6"))
    (pad "P4" smd circle (at -1.999996 3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "P9" smd circle (at 1.999996 3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "P10" smd circle (at 2.799994 3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 270 "QSC_7"))
    (pad "P11" smd circle (at 3.599993 3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 279 "QSCB_7"))
    (pad "P12" smd circle (at 4.399991 3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "R1" smd circle (at -4.399991 4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "R2" smd circle (at -3.599993 4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 257 "DQC_51"))
    (pad "R3" smd circle (at -2.799994 4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 258 "DQC_49"))
    (pad "R4" smd circle (at -1.999996 4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "R9" smd circle (at 1.999996 4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "R10" smd circle (at 2.799994 4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 250 "DQC_62"))
    (pad "R11" smd circle (at 3.599993 4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 249 "DQC_60"))
    (pad "R12" smd circle (at 4.399991 4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "T1" smd circle (at -4.399991 5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "T2" smd circle (at -3.599993 5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 260 "DQC_50"))
    (pad "T3" smd circle (at -2.799994 5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 261 "DQC_48"))
    (pad "T4" smd circle (at -1.999996 5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "T9" smd circle (at 1.999996 5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "T10" smd circle (at 2.799994 5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 252 "DQC_63"))
    (pad "T11" smd circle (at 3.599993 5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 251 "DQC_61"))
    (pad "T12" smd circle (at 4.399991 5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "V1" smd circle (at -4.399991 6.399987 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "V2" smd circle (at -3.599993 6.400013 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "V3" smd circle (at -2.799994 6.400013 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "V4" smd circle (at -1.999996 6.400013 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "V9" smd circle (at 1.999996 6.400013 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 144 "DRAM_RST"))
    (pad "V10" smd circle (at 2.799994 6.400013 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "V11" smd circle (at 3.599993 6.400013 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "V12" smd circle (at 4.399991 6.399987 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -38.495384 94.851009)
    (fp_text reference "C1004" (at 2.2225 2.54 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 47 "A_DAC1_R"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "GEOM0010_1" (layer "F.Cu")
    (tedit 0)
    (at -56.98539 59.970993 180)
    (fp_text reference "J3001" (at 5.557241 -2.54 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at -8.560791 -3.3528 180) (size 1.397 1.397) (drill 0.899998) (layers *.Cu *.Mask)
      (net 4 "GND"))
    (pad "2" thru_hole circle (at -8.560791 3.3528 180) (size 1.397 1.397) (drill 0.899998) (layers *.Cu *.Mask)
      (net 4 "GND"))
    (pad "3" thru_hole circle (at -11.049991 -3.3528 180) (size 1.397 1.397) (drill 0.899998) (layers *.Cu *.Mask)
      (net 904 "DAC2_Y_F"))
    (pad "4" thru_hole circle (at -11.049991 3.3528 180) (size 1.397 1.397) (drill 0.899998) (layers *.Cu *.Mask)
      (net 903 "DAC2_C_F"))
    (pad "5" thru_hole circle (at -11.049991 -1.2954 180) (size 1.397 1.397) (drill 0.899998) (layers *.Cu *.Mask)
      (net 4 "GND"))
    (pad "6" thru_hole circle (at -11.049991 5.3848 180) (size 1.397 1.397) (drill 0.899998) (layers *.Cu *.Mask)
      (net 847 "PIN6"))
    (pad "7" thru_hole circle (at -11.049991 0.8128 180) (size 1.397 1.397) (drill 0.899998) (layers *.Cu *.Mask)
      (net 902 "DAC2_COMP_F"))
    (pad "8" thru_hole oval (at -5.563591 -6.731 270) (size 1.778 2.286) (drill 0.029997) (layers *.Cu *.Mask)
      (net 4 "GND"))
    (pad "9" thru_hole oval (at -4.699991 0 180) (size 1.778 2.286) (drill 0.029997) (layers *.Cu *.Mask)
      (net 4 "GND"))
    (pad "10" thru_hole oval (at -5.563591 6.731 270) (size 1.778 2.286) (drill 0.029997) (layers *.Cu *.Mask)
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -5.653794 59.761316 -90)
    (fp_text reference "C4004" (at 2.54 -2.2225 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 76 "GPU_DPLUS"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 77 "GPU_DMINUS"))
  )
  (footprint "DPAKSGD_1" (layer "F.Cu")
    (tedit 0)
    (at 137.677187 18.568002 -90)
    (fp_text reference "EQ36" (at 1.146175 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "D" smd rect (at 0 -3.7465 270) (size 5.6896 5.6388) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 62 "N85769539"))
    (pad "G" smd oval (at -2.286 3.7465 270) (size 1.651 2.6797) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 910 "N85769537"))
    (pad "S" smd oval (at 2.286 3.7465 270) (size 1.651 2.6797) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 59 "N85769021"))
  )
  (footprint "TP089X043_1" (layer "F.Cu")
    (tedit 0)
    (at 21.304623 48.351001)
    (fp_text reference "TP84" (at -1.27 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 0.5588 0.5588) (drill 0.250012) (layers *.Cu *.Mask)
      (net 811 "DVOCLK"))
  )
  (footprint "GEOM0012_1" (layer "F.Cu")
    (tedit 0)
    (at 138.185187 7.773002)
    (fp_text reference "EB16" (at 1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 -2.500122) (size 1.905 1.905) (drill 1.143) (layers *.Cu *.Mask)
      (net 60 "+12V_EXT"))
    (pad "2" thru_hole circle (at 0 2.500122) (size 1.905 1.905) (drill 1.143) (layers *.Cu *.Mask)
      (net 62 "N85769539"))
  )
  (footprint "TP055PRI_1" (layer "F.Cu")
    (tedit 0)
    (at 33.604624 83.151007)
    (fp_text reference "TP17" (at -1.27 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd circle (at 0 0) (size 0.550012 0.550012) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 608 "PETP8_GFXRP8"))
  )
  (footprint "560UF_4V_R71D55_1" (layer "F.Cu")
    (tedit 0)
    (at 112.399615 17.044002 180)
    (fp_text reference "EC184" (at 1.36398 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole rect (at -1.75006 0 180) (size 1.8034 1.8034) (drill 1.397) (layers *.Cu *.Mask)
      (net 12 "+MVDD"))
    (pad "2" thru_hole circle (at 1.75006 0 180) (size 1.8034 1.8034) (drill 1.397) (layers *.Cu *.Mask)
      (net 4 "GND"))
  )
  (footprint "HD2MM1X4_KEY_1" (layer "F.Cu")
    (tedit 0)
    (at 97.540615 4.344002)
    (fp_text reference "J4030" (at 1.412494 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole rect (at 0 0) (size 1.397 1.397) (drill 0.799998) (layers *.Cu *.Mask)
      (net 4 "GND"))
    (pad "2" thru_hole circle (at 1.999996 0) (size 1.397 1.397) (drill 0.799998) (layers *.Cu *.Mask)
      (net 830 "N49971242"))
    (pad "3" thru_hole circle (at 3.999992 0) (size 1.397 1.397) (drill 0.799998) (layers *.Cu *.Mask)
      (net 834 "N49971220"))
    (pad "4" thru_hole circle (at 6.000013 0) (size 1.397 1.397) (drill 0.799998) (layers *.Cu *.Mask)
      (net 859 "N49971328"))
  )
  (footprint "RES1608_1" (layer "F.Cu")
    (tedit 0)
    (at -44.595397 42.351013)
    (fp_text reference "R2023" (at 2.222475 2.540025 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 751 "HPD1"))
    (pad "2" smd rect (at 0 0.7874) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "C1206_113_1" (layer "F.Cu")
    (tedit 0)
    (at 107.065615 80.036002 90)
    (fp_text reference "EC1162" (at 0 -0.981075 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd oval (at -1.4351 0 90) (size 0.9779 1.1938) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd oval (at 1.4351 0 90) (size 0.9779 1.1938) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "GEOM0002_1" (layer "F.Cu")
    (tedit 0)
    (at 93.004607 85.151003 90)
    (fp_text reference "U201" (at -1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "A1" smd circle (at -4.399991 -6.399987 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "A2" smd circle (at -3.599993 -6.400013 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "A3" smd circle (at -2.799994 -6.400013 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "A4" smd circle (at -1.999996 -6.400013 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 592 "N25404999"))
    (pad "A9" smd circle (at 1.999996 -6.400013 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "A10" smd circle (at 2.799994 -6.400013 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "A11" smd circle (at 3.599993 -6.400013 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "A12" smd circle (at 4.399991 -6.399987 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "B1" smd circle (at -4.399991 -5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "B2" smd circle (at -3.599993 -5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 547 "DQA_13"))
    (pad "B3" smd circle (at -2.799994 -5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 548 "DQA_14"))
    (pad "B4" smd circle (at -1.999996 -5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "B9" smd circle (at 1.999996 -5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "B10" smd circle (at 2.799994 -5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 578 "DQA_22"))
    (pad "B11" smd circle (at 3.599993 -5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 577 "DQA_21"))
    (pad "B12" smd circle (at 4.399991 -5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "C1" smd circle (at -4.399991 -4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "C2" smd circle (at -3.599993 -4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 559 "DQA_15"))
    (pad "C3" smd circle (at -2.799994 -4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 570 "DQA_12"))
    (pad "C4" smd circle (at -1.999996 -4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "C9" smd circle (at 1.999996 -4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "C10" smd circle (at 2.799994 -4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 550 "DQA_20"))
    (pad "C11" smd circle (at 3.599993 -4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 549 "DQA_23"))
    (pad "C12" smd circle (at 4.399991 -4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "D1" smd circle (at -4.399991 -3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "D2" smd circle (at -3.599993 -3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 587 "QSAB_1"))
    (pad "D3" smd circle (at -2.799994 -3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 579 "QSA_1"))
    (pad "D4" smd circle (at -1.999996 -3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "D9" smd circle (at 1.999996 -3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "D10" smd circle (at 2.799994 -3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 580 "QSA_2"))
    (pad "D11" smd circle (at 3.599993 -3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 588 "QSAB_2"))
    (pad "D12" smd circle (at 4.399991 -3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "E1" smd circle (at -4.399991 -3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "E2" smd circle (at -3.599993 -3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 573 "DQA_11"))
    (pad "E3" smd circle (at -2.799994 -3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 543 "DQMAB_1"))
    (pad "E4" smd circle (at -1.999996 -3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "E9" smd circle (at 1.999996 -3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "E10" smd circle (at 2.799994 -3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 544 "DQMAB_2"))
    (pad "E11" smd circle (at 3.599993 -3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 551 "DQA_19"))
    (pad "E12" smd circle (at 4.399991 -3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "F1" smd circle (at -4.399991 -2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "F2" smd circle (at -3.599993 -2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 575 "DQA_9"))
    (pad "F3" smd circle (at -2.799994 -2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 574 "DQA_10"))
    (pad "F4" smd circle (at -1.999996 -2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 540 "CSA0B_0"))
    (pad "F9" smd circle (at 1.999996 -2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 542 "CASA0B"))
    (pad "F10" smd circle (at 2.799994 -2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 552 "DQA_18"))
    (pad "F11" smd circle (at 3.599993 -2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 553 "DQA_16"))
    (pad "F12" smd circle (at 4.399991 -2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "G1" smd circle (at -4.399991 -1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "G2" smd circle (at -3.599993 -1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "G3" smd circle (at -2.799994 -1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 576 "DQA_8"))
    (pad "G4" smd circle (at -1.999996 -1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 478 "MAA_BA1"))
    (pad "G9" smd circle (at 1.999996 -1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 479 "MAA_BA0"))
    (pad "G10" smd circle (at 2.799994 -1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 554 "DQA_17"))
    (pad "G11" smd circle (at 3.599993 -1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "G12" smd circle (at 4.399991 -1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "H1" smd circle (at -4.399991 -0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 585 "N25404871"))
    (pad "H2" smd circle (at -3.599993 -0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 467 "MAA_5"))
    (pad "H3" smd circle (at -2.799994 -0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 526 "MAA_BA2"))
    (pad "H4" smd circle (at -1.999996 -0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 539 "WEA0B"))
    (pad "H9" smd circle (at 1.999996 -0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 591 "CKEA0"))
    (pad "H10" smd circle (at 2.799994 -0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 537 "RASA0B"))
    (pad "H11" smd circle (at 3.599993 -0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 473 "MAA_1"))
    (pad "H12" smd circle (at 4.399991 -0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 586 "N25404815"))
    (pad "J1" smd circle (at -4.399991 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "J2" smd circle (at -3.599993 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "J3" smd circle (at -2.799994 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "J4" smd circle (at -1.999996 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "J9" smd circle (at 1.999996 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "J10" smd circle (at 2.799994 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 541 "CLKA0B"))
    (pad "J11" smd circle (at 3.599993 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 538 "CLKA0"))
    (pad "J12" smd circle (at 4.399991 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "K1" smd circle (at -4.399991 0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 583 "N25404817"))
    (pad "K2" smd circle (at -3.599993 0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 468 "MAA_8"))
    (pad "K3" smd circle (at -2.799994 0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 470 "MAA_6"))
    (pad "K4" smd circle (at -1.999996 0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 466 "MAA_4"))
    (pad "K9" smd circle (at 1.999996 0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 472 "MAA_0"))
    (pad "K10" smd circle (at 2.799994 0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 474 "MAA_2"))
    (pad "K11" smd circle (at 3.599993 0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 476 "MAA_10"))
    (pad "K12" smd circle (at 4.399991 0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 584 "N25405001"))
    (pad "L1" smd circle (at -4.399991 1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "L2" smd circle (at -3.599993 1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "L3" smd circle (at -2.799994 1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 565 "DQA_5"))
    (pad "L4" smd circle (at -1.999996 1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 469 "MAA_7"))
    (pad "L9" smd circle (at 1.999996 1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 475 "MAA_11"))
    (pad "L10" smd circle (at 2.799994 1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 556 "DQA_27"))
    (pad "L11" smd circle (at 3.599993 1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "L12" smd circle (at 4.399991 1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "M1" smd circle (at -4.399991 2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "M2" smd circle (at -3.599993 2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 564 "DQA_7"))
    (pad "M3" smd circle (at -2.799994 2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 567 "DQA_6"))
    (pad "M4" smd circle (at -1.999996 2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 471 "MAA_9"))
    (pad "M9" smd circle (at 1.999996 2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 477 "MAA_3"))
    (pad "M10" smd circle (at 2.799994 2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 558 "DQA_26"))
    (pad "M11" smd circle (at 3.599993 2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 555 "DQA_25"))
    (pad "M12" smd circle (at 4.399991 2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "N1" smd circle (at -4.399991 3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "N2" smd circle (at -3.599993 3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 566 "DQA_4"))
    (pad "N3" smd circle (at -2.799994 3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 546 "DQMAB_0"))
    (pad "N4" smd circle (at -1.999996 3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "N9" smd circle (at 1.999996 3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "N10" smd circle (at 2.799994 3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 545 "DQMAB_3"))
    (pad "N11" smd circle (at 3.599993 3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 557 "DQA_24"))
    (pad "N12" smd circle (at 4.399991 3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "P1" smd circle (at -4.399991 3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "P2" smd circle (at -3.599993 3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 590 "QSAB_0"))
    (pad "P3" smd circle (at -2.799994 3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 582 "QSA_0"))
    (pad "P4" smd circle (at -1.999996 3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "P9" smd circle (at 1.999996 3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "P10" smd circle (at 2.799994 3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 581 "QSA_3"))
    (pad "P11" smd circle (at 3.599993 3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 589 "QSAB_3"))
    (pad "P12" smd circle (at 4.399991 3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "R1" smd circle (at -4.399991 4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "R2" smd circle (at -3.599993 4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 568 "DQA_3"))
    (pad "R3" smd circle (at -2.799994 4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 569 "DQA_1"))
    (pad "R4" smd circle (at -1.999996 4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "R9" smd circle (at 1.999996 4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "R10" smd circle (at 2.799994 4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 561 "DQA_29"))
    (pad "R11" smd circle (at 3.599993 4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 560 "DQA_30"))
    (pad "R12" smd circle (at 4.399991 4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "T1" smd circle (at -4.399991 5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "T2" smd circle (at -3.599993 5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 571 "DQA_2"))
    (pad "T3" smd circle (at -2.799994 5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 572 "DQA_0"))
    (pad "T4" smd circle (at -1.999996 5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "T9" smd circle (at 1.999996 5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "T10" smd circle (at 2.799994 5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 563 "DQA_28"))
    (pad "T11" smd circle (at 3.599993 5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 562 "DQA_31"))
    (pad "T12" smd circle (at 4.399991 5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "V1" smd circle (at -4.399991 6.399987 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "V2" smd circle (at -3.599993 6.400013 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "V3" smd circle (at -2.799994 6.400013 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "V4" smd circle (at -1.999996 6.400013 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "V9" smd circle (at 1.999996 6.400013 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 144 "DRAM_RST"))
    (pad "V10" smd circle (at 2.799994 6.400013 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "V11" smd circle (at 3.599993 6.400013 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "V12" smd circle (at 4.399991 6.399987 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -1.795381 41.951013 90)
    (fp_text reference "R296" (at -1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 796 "N52040505"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at 150.753615 35.586002 90)
    (fp_text reference "AR38" (at -1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 945 "AICSN1"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 928 "N86496297"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at 150.753615 30.252002 -90)
    (fp_text reference "AR17" (at 1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 923 "N86494909"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "GEOM0007_1" (layer "F.Cu")
    (tedit 0)
    (at 122.686615 62.891002 90)
    (fp_text reference "L63" (at -1.27 1.5875 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 4.500118 90) (size 3.81 3.81) (drill 2.413) (layers *.Cu *.Mask)
      (net 70 "APHASE_1"))
    (pad "2" thru_hole circle (at 0 -4.500118 90) (size 3.81 3.81) (drill 2.413) (layers *.Cu *.Mask)
      (net 735 "+VDDC"))
  )
  (footprint "TP055PRI_1" (layer "F.Cu")
    (tedit 0)
    (at 28.804608 83.151007)
    (fp_text reference "TP13" (at -1.27 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd circle (at 0 0) (size 0.550012 0.550012) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 630 "PETP5_GFXRP5"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -8.795393 79.25099)
    (fp_text reference "R84" (at 1.5875 1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "XTALIN"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "XTALOUT"))
  )
  (footprint "C1206_113_1" (layer "F.Cu")
    (tedit 0)
    (at 107.065615 25.172002 -90)
    (fp_text reference "EC164" (at 0 0.981075 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd oval (at -1.4351 0 270) (size 0.9779 1.1938) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd oval (at 1.4351 0 270) (size 0.9779 1.1938) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "C1206_113_1" (layer "F.Cu")
    (tedit 0)
    (at 107.065615 40.666002 90)
    (fp_text reference "EC1157" (at 0 -0.981075 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd oval (at -1.4351 0 90) (size 0.9779 1.1938) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd oval (at 1.4351 0 90) (size 0.9779 1.1938) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "GEOM0008_1" (layer "F.Cu")
    (tedit 0)
    (at -37.095387 90.750992)
    (fp_text reference "L1002" (at 1.111516 1.27033 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144) (size 1.27 1.219987) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "A_DAC1_G"))
    (pad "2" smd rect (at 0 0.9144) (size 1.27 1.219987) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 46 "A_G_DAC1_F"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -23.295389 77.596002)
    (fp_text reference "R848" (at 1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "+12V_BUS"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "N87188969"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -35.195391 87.750998)
    (fp_text reference "R1029" (at 2.2225 2.54 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 602 "A_DAC1_BB"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "F_PAD_M120_1" (layer "F.Cu")
    (tedit 0)
    (at -19.680385 96.038002)
    (fp_text reference "FM1" (at -0.762501 -0.000013 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd circle (at 0 0) (size 1.020064 1.020064) (layers "F.Cu" "F.Paste" "F.Mask"))
  )
  (footprint "GEOM0008_1" (layer "F.Cu")
    (tedit 0)
    (at -41.495378 95.551008 -90)
    (fp_text reference "L1001" (at 1.27033 -1.111516 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144 270) (size 1.27 1.219987) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 47 "A_DAC1_R"))
    (pad "2" smd rect (at 0 0.9144 270) (size 1.27 1.219987) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 48 "A_R_DAC1_F"))
  )
  (footprint "IND2012_1" (layer "F.Cu")
    (tedit 0)
    (at -37.695386 64.050995 90)
    (fp_text reference "L3003" (at -1.158837 1.024655 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 0.889 270) (size 1.799996 0.999998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 654 "A_DAC2_COMP"))
    (pad "2" smd rect (at 0 -0.889 270) (size 1.799996 0.999998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 902 "DAC2_COMP_F"))
  )
  (footprint "RES1608_1" (layer "F.Cu")
    (tedit 0)
    (at 115.320615 4.979002 90)
    (fp_text reference "ER13" (at -1.905025 1.904975 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 90) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "2" smd rect (at 0 0.7874 90) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 911 "N85769434"))
  )
  (footprint "TP089X043_1" (layer "F.Cu")
    (tedit 0)
    (at -19.895396 6.905008)
    (fp_text reference "TP64" (at -1.27 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 0.5588 0.5588) (drill 0.250012) (layers *.Cu *.Mask)
      (net 812 "DVPDATA_4"))
  )
  (footprint "GEOM0004_1" (layer "F.Cu")
    (tedit 0)
    (at -52.068382 12.231007)
    (fp_text reference "MT1" (at -0.9525 -2.475001 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 -2.475001) (size 0.500024 0.500024) (drill 0.250012) (layers *.Cu *.Mask)
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -40.995379 57.551008 180)
    (fp_text reference "R3008" (at -2.2225 -2.54 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "+3.3V"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 754 "GENERICA"))
  )
  (footprint "GEOM0008_1" (layer "F.Cu")
    (tedit 0)
    (at -38.695384 87.750998 -90)
    (fp_text reference "L1003" (at 1.27033 -1.111516 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144 270) (size 1.27 1.219987) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "A_DAC1_B"))
    (pad "2" smd rect (at 0 0.9144 270) (size 1.27 1.219987) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 44 "A_B_DAC1_F"))
  )
  (footprint "RES1608_1" (layer "F.Cu")
    (tedit 0)
    (at 130.052615 78.004002)
    (fp_text reference "AR73" (at 1.904975 1.905025 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 940 "N864960700"))
    (pad "2" smd rect (at 0 0.7874) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 598 "APHASE_3"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at 150.753615 31.268002 -90)
    (fp_text reference "AR53" (at 1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 57 "N86495082"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at 20.204625 71.151006 180)
    (fp_text reference "R104" (at -1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 712 "T2X4P"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 663 "T2X4M"))
  )
  (footprint "C1206_113_1" (layer "F.Cu")
    (tedit 0)
    (at 155.452615 22.632002 180)
    (fp_text reference "EC137" (at 0.981075 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd oval (at -1.4351 0 180) (size 0.9779 1.1938) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "+12V_EXT"))
    (pad "2" smd oval (at 1.4351 0 180) (size 0.9779 1.1938) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at 156.659115 39.904002)
    (fp_text reference "AR29" (at 1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 935 "ACISP2"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 68 "APHASE_2"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at 75.144622 19.430992 90)
    (fp_text reference "R495" (at -1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 144 "DRAM_RST"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -4.253797 69.061195 -90)
    (fp_text reference "R4002" (at 2.54 -2.2225 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 675 "DDC3DATA"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 80 "SDA_R"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at 148.086615 37.872002 90)
    (fp_text reference "AR37" (at -1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 933 "AICSN35"))
  )
  (footprint "CAP1608_1" (layer "F.Cu")
    (tedit 0)
    (at 148.467615 12.218002)
    (fp_text reference "C1609" (at 2.222475 2.540025 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "+12V_EXT"))
    (pad "2" smd rect (at 0 0.7874) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "TP055PRI_1" (layer "F.Cu")
    (tedit 0)
    (at 31.204603 84.151005)
    (fp_text reference "TP16" (at -1.27 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd circle (at 0 0) (size 0.550012 0.550012) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 603 "PETN6_GFXRN6"))
  )
  (footprint "CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at 159.580115 55.423402 180)
    (fp_text reference "AC27" (at -1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "+12V_EXT"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "GEOM0002_1" (layer "F.Cu")
    (tedit 0)
    (at 93.004607 25.150996 90)
    (fp_text reference "U302" (at -1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "A1" smd circle (at -4.399991 -6.399987 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "A2" smd circle (at -3.599993 -6.400013 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "A3" smd circle (at -2.799994 -6.400013 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "A4" smd circle (at -1.999996 -6.400013 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 409 "N49338044"))
    (pad "A9" smd circle (at 1.999996 -6.400013 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "A10" smd circle (at 2.799994 -6.400013 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "A11" smd circle (at 3.599993 -6.400013 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "A12" smd circle (at 4.399991 -6.399987 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "B1" smd circle (at -4.399991 -5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "B2" smd circle (at -3.599993 -5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 363 "DQB_45"))
    (pad "B3" smd circle (at -2.799994 -5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 364 "DQB_46"))
    (pad "B4" smd circle (at -1.999996 -5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "B9" smd circle (at 1.999996 -5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "B10" smd circle (at 2.799994 -5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 394 "DQB_62"))
    (pad "B11" smd circle (at 3.599993 -5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 393 "DQB_60"))
    (pad "B12" smd circle (at 4.399991 -5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "C1" smd circle (at -4.399991 -4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "C2" smd circle (at -3.599993 -4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 375 "DQB_44"))
    (pad "C3" smd circle (at -2.799994 -4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 386 "DQB_47"))
    (pad "C4" smd circle (at -1.999996 -4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "C9" smd circle (at 1.999996 -4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "C10" smd circle (at 2.799994 -4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 366 "DQB_61"))
    (pad "C11" smd circle (at 3.599993 -4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 365 "DQB_63"))
    (pad "C12" smd circle (at 4.399991 -4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "D1" smd circle (at -4.399991 -3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "D2" smd circle (at -3.599993 -3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 404 "QSBB_5"))
    (pad "D3" smd circle (at -2.799994 -3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 395 "QSB_5"))
    (pad "D4" smd circle (at -1.999996 -3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "D9" smd circle (at 1.999996 -3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "D10" smd circle (at 2.799994 -3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 396 "QSB_7"))
    (pad "D11" smd circle (at 3.599993 -3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 405 "QSBB_7"))
    (pad "D12" smd circle (at 4.399991 -3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "E1" smd circle (at -4.399991 -3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "E2" smd circle (at -3.599993 -3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 389 "DQB_43"))
    (pad "E3" smd circle (at -2.799994 -3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 359 "DQMBB_5"))
    (pad "E4" smd circle (at -1.999996 -3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "E9" smd circle (at 1.999996 -3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "E10" smd circle (at 2.799994 -3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 360 "DQMBB_7"))
    (pad "E11" smd circle (at 3.599993 -3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 367 "DQB_59"))
    (pad "E12" smd circle (at 4.399991 -3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "F1" smd circle (at -4.399991 -2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "F2" smd circle (at -3.599993 -2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 391 "DQB_41"))
    (pad "F3" smd circle (at -2.799994 -2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 390 "DQB_42"))
    (pad "F4" smd circle (at -1.999996 -2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 356 "CSB1B_0"))
    (pad "F9" smd circle (at 1.999996 -2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 358 "CASB1B"))
    (pad "F10" smd circle (at 2.799994 -2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 368 "DQB_58"))
    (pad "F11" smd circle (at 3.599993 -2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 369 "DQB_56"))
    (pad "F12" smd circle (at 4.399991 -2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "G1" smd circle (at -4.399991 -1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "G2" smd circle (at -3.599993 -1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "G3" smd circle (at -2.799994 -1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 392 "DQB_40"))
    (pad "G4" smd circle (at -1.999996 -1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 351 "MAB_BA1"))
    (pad "G9" smd circle (at 1.999996 -1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 352 "MAB_BA0"))
    (pad "G10" smd circle (at 2.799994 -1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 370 "DQB_57"))
    (pad "G11" smd circle (at 3.599993 -1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "G12" smd circle (at 4.399991 -1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "H1" smd circle (at -4.399991 -0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 402 "N49338012"))
    (pad "H2" smd circle (at -3.599993 -0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 340 "MAB_5"))
    (pad "H3" smd circle (at -2.799994 -0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 399 "MAB_BA2"))
    (pad "H4" smd circle (at -1.999996 -0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 355 "WEB1B"))
    (pad "H9" smd circle (at 1.999996 -0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 408 "CKEB1"))
    (pad "H10" smd circle (at 2.799994 -0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 353 "RASB1B"))
    (pad "H11" smd circle (at 3.599993 -0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 346 "MAB_1"))
    (pad "H12" smd circle (at 4.399991 -0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 403 "N49337708"))
    (pad "J1" smd circle (at -4.399991 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "J2" smd circle (at -3.599993 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "J3" smd circle (at -2.799994 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "J4" smd circle (at -1.999996 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "J9" smd circle (at 1.999996 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "J10" smd circle (at 2.799994 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 357 "CLKB1B"))
    (pad "J11" smd circle (at 3.599993 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 354 "CLKB1"))
    (pad "J12" smd circle (at 4.399991 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "K1" smd circle (at -4.399991 0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 400 "N49338068"))
    (pad "K2" smd circle (at -3.599993 0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 341 "MAB_8"))
    (pad "K3" smd circle (at -2.799994 0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 343 "MAB_6"))
    (pad "K4" smd circle (at -1.999996 0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 339 "MAB_4"))
    (pad "K9" smd circle (at 1.999996 0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 345 "MAB_0"))
    (pad "K10" smd circle (at 2.799994 0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 347 "MAB_2"))
    (pad "K11" smd circle (at 3.599993 0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 349 "MAB_10"))
    (pad "K12" smd circle (at 4.399991 0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 401 "N49337966"))
    (pad "L1" smd circle (at -4.399991 1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "L2" smd circle (at -3.599993 1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "L3" smd circle (at -2.799994 1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 381 "DQB_39"))
    (pad "L4" smd circle (at -1.999996 1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 342 "MAB_7"))
    (pad "L9" smd circle (at 1.999996 1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 348 "MAB_11"))
    (pad "L10" smd circle (at 2.799994 1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 372 "DQB_51"))
    (pad "L11" smd circle (at 3.599993 1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "L12" smd circle (at 4.399991 1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "M1" smd circle (at -4.399991 2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "M2" smd circle (at -3.599993 2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 380 "DQB_37"))
    (pad "M3" smd circle (at -2.799994 2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 383 "DQB_36"))
    (pad "M4" smd circle (at -1.999996 2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 344 "MAB_9"))
    (pad "M9" smd circle (at 1.999996 2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 350 "MAB_3"))
    (pad "M10" smd circle (at 2.799994 2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 374 "DQB_49"))
    (pad "M11" smd circle (at 3.599993 2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 371 "DQB_50"))
    (pad "M12" smd circle (at 4.399991 2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "N1" smd circle (at -4.399991 3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "N2" smd circle (at -3.599993 3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 382 "DQB_38"))
    (pad "N3" smd circle (at -2.799994 3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 362 "DQMBB_4"))
    (pad "N4" smd circle (at -1.999996 3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "N9" smd circle (at 1.999996 3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "N10" smd circle (at 2.799994 3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 361 "DQMBB_6"))
    (pad "N11" smd circle (at 3.599993 3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 373 "DQB_48"))
    (pad "N12" smd circle (at 4.399991 3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "P1" smd circle (at -4.399991 3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "P2" smd circle (at -3.599993 3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 407 "QSBB_4"))
    (pad "P3" smd circle (at -2.799994 3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 398 "QSB_4"))
    (pad "P4" smd circle (at -1.999996 3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "P9" smd circle (at 1.999996 3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "P10" smd circle (at 2.799994 3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 397 "QSB_6"))
    (pad "P11" smd circle (at 3.599993 3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 406 "QSBB_6"))
    (pad "P12" smd circle (at 4.399991 3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "R1" smd circle (at -4.399991 4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "R2" smd circle (at -3.599993 4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 384 "DQB_35"))
    (pad "R3" smd circle (at -2.799994 4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 385 "DQB_33"))
    (pad "R4" smd circle (at -1.999996 4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "R9" smd circle (at 1.999996 4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "R10" smd circle (at 2.799994 4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 377 "DQB_52"))
    (pad "R11" smd circle (at 3.599993 4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 376 "DQB_54"))
    (pad "R12" smd circle (at 4.399991 4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "T1" smd circle (at -4.399991 5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "T2" smd circle (at -3.599993 5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 387 "DQB_34"))
    (pad "T3" smd circle (at -2.799994 5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 388 "DQB_32"))
    (pad "T4" smd circle (at -1.999996 5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "T9" smd circle (at 1.999996 5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "T10" smd circle (at 2.799994 5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 379 "DQB_55"))
    (pad "T11" smd circle (at 3.599993 5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 378 "DQB_53"))
    (pad "T12" smd circle (at 4.399991 5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "V1" smd circle (at -4.399991 6.399987 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "V2" smd circle (at -3.599993 6.400013 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "V3" smd circle (at -2.799994 6.400013 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "V4" smd circle (at -1.999996 6.400013 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "V9" smd circle (at 1.999996 6.400013 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 144 "DRAM_RST"))
    (pad "V10" smd circle (at 2.799994 6.400013 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "V11" smd circle (at 3.599993 6.400013 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "V12" smd circle (at 4.399991 6.399987 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at 104.271615 93.117002 90)
    (fp_text reference "C1031" (at -2.54 2.2225 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1608_1" (layer "F.Cu")
    (tedit 0)
    (at -35.095391 64.150994 180)
    (fp_text reference "C3003" (at -2.222475 -2.540025 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 180) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 654 "A_DAC2_COMP"))
    (pad "2" smd rect (at 0 0.7874 180) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1608_1" (layer "F.Cu")
    (tedit 0)
    (at 150.499615 80.798002 -90)
    (fp_text reference "AC39" (at 1.905025 -1.904975 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 270) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 937 "N86494646"))
    (pad "2" smd rect (at 0 0.7874 270) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 598 "APHASE_3"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at 85.404622 27.450992 180)
    (fp_text reference "R310" (at -1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 409 "N49338044"))
  )
  (footprint "TP089X043_1" (layer "F.Cu")
    (tedit 0)
    (at -23.795388 8.305005)
    (fp_text reference "TP69" (at -1.27 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 0.5588 0.5588) (drill 0.250012) (layers *.Cu *.Mask)
      (net 782 "DVPDATA_9"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at 163.453615 36.221002 90)
    (fp_text reference "AR13" (at -1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 931 "N86495281"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 82 "VDD_+5V"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at 0.904613 24.850997 -45)
    (fp_text reference "R510" (at 2.694077 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 315) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "2" smd rect (at 0 0.492608 315) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 155 "N48570117"))
  )
  (footprint "CAP1608_1" (layer "F.Cu")
    (tedit 0)
    (at 130.052615 35.205002 180)
    (fp_text reference "AC33" (at -1.904975 -1.905025 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 180) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 941 "N864966460"))
    (pad "2" smd rect (at 0 0.7874 180) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "GEOM0002_1" (layer "F.Cu")
    (tedit 0)
    (at 20.004626 14.151018 180)
    (fp_text reference "U501" (at -1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "A1" smd circle (at -4.399991 -6.399987 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "A2" smd circle (at -3.599993 -6.400013 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "A3" smd circle (at -2.799994 -6.400013 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "A4" smd circle (at -1.999996 -6.400013 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 211 "N48569967"))
    (pad "A9" smd circle (at 1.999996 -6.400013 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "A10" smd circle (at 2.799994 -6.400013 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "A11" smd circle (at 3.599993 -6.400013 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "A12" smd circle (at 4.399991 -6.399987 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "B1" smd circle (at -4.399991 -5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "B2" smd circle (at -3.599993 -5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 166 "DQD_13"))
    (pad "B3" smd circle (at -2.799994 -5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 167 "DQD_12"))
    (pad "B4" smd circle (at -1.999996 -5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "B9" smd circle (at 1.999996 -5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "B10" smd circle (at 2.799994 -5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 197 "DQD_22"))
    (pad "B11" smd circle (at 3.599993 -5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 196 "DQD_21"))
    (pad "B12" smd circle (at 4.399991 -5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "C1" smd circle (at -4.399991 -4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "C2" smd circle (at -3.599993 -4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 178 "DQD_15"))
    (pad "C3" smd circle (at -2.799994 -4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 189 "DQD_14"))
    (pad "C4" smd circle (at -1.999996 -4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "C9" smd circle (at 1.999996 -4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "C10" smd circle (at 2.799994 -4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 169 "DQD_23"))
    (pad "C11" smd circle (at 3.599993 -4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 168 "DQD_20"))
    (pad "C12" smd circle (at 4.399991 -4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "D1" smd circle (at -4.399991 -3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "D2" smd circle (at -3.599993 -3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 206 "QSDB_1"))
    (pad "D3" smd circle (at -2.799994 -3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 198 "QSD_1"))
    (pad "D4" smd circle (at -1.999996 -3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "D9" smd circle (at 1.999996 -3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "D10" smd circle (at 2.799994 -3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 199 "QSD_2"))
    (pad "D11" smd circle (at 3.599993 -3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 207 "QSDB_2"))
    (pad "D12" smd circle (at 4.399991 -3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "E1" smd circle (at -4.399991 -3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "E2" smd circle (at -3.599993 -3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 192 "DQD_8"))
    (pad "E3" smd circle (at -2.799994 -3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 162 "DQMDB_1"))
    (pad "E4" smd circle (at -1.999996 -3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "E9" smd circle (at 1.999996 -3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "E10" smd circle (at 2.799994 -3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 163 "DQMDB_2"))
    (pad "E11" smd circle (at 3.599993 -3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 170 "DQD_18"))
    (pad "E12" smd circle (at 4.399991 -3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "F1" smd circle (at -4.399991 -2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "F2" smd circle (at -3.599993 -2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 194 "DQD_10"))
    (pad "F3" smd circle (at -2.799994 -2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 193 "DQD_9"))
    (pad "F4" smd circle (at -1.999996 -2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 159 "CSD0B_0"))
    (pad "F9" smd circle (at 1.999996 -2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 161 "CASD0B"))
    (pad "F10" smd circle (at 2.799994 -2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 171 "DQD_19"))
    (pad "F11" smd circle (at 3.599993 -2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 172 "DQD_16"))
    (pad "F12" smd circle (at 4.399991 -2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "G1" smd circle (at -4.399991 -1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "G2" smd circle (at -3.599993 -1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "G3" smd circle (at -2.799994 -1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 195 "DQD_11"))
    (pad "G4" smd circle (at -1.999996 -1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 96 "MAD_BA1"))
    (pad "G9" smd circle (at 1.999996 -1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 97 "MAD_BA0"))
    (pad "G10" smd circle (at 2.799994 -1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 173 "DQD_17"))
    (pad "G11" smd circle (at 3.599993 -1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "G12" smd circle (at 4.399991 -1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "H1" smd circle (at -4.399991 -0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 204 "N48569889"))
    (pad "H2" smd circle (at -3.599993 -0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 85 "MAD_5"))
    (pad "H3" smd circle (at -2.799994 -0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 145 "MAD_BA2"))
    (pad "H4" smd circle (at -1.999996 -0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 158 "WED0B"))
    (pad "H9" smd circle (at 1.999996 -0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 210 "CKED0"))
    (pad "H10" smd circle (at 2.799994 -0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 156 "RASD0B"))
    (pad "H11" smd circle (at 3.599993 -0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 91 "MAD_1"))
    (pad "H12" smd circle (at 4.399991 -0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 205 "N48569804"))
    (pad "J1" smd circle (at -4.399991 0 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "J2" smd circle (at -3.599993 0 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "J3" smd circle (at -2.799994 0 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "J4" smd circle (at -1.999996 0 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "J9" smd circle (at 1.999996 0 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "J10" smd circle (at 2.799994 0 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 160 "CLKD0B"))
    (pad "J11" smd circle (at 3.599993 0 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 157 "CLKD0"))
    (pad "J12" smd circle (at 4.399991 0 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "K1" smd circle (at -4.399991 0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 202 "N48569853"))
    (pad "K2" smd circle (at -3.599993 0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 86 "MAD_8"))
    (pad "K3" smd circle (at -2.799994 0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 88 "MAD_6"))
    (pad "K4" smd circle (at -1.999996 0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 84 "MAD_4"))
    (pad "K9" smd circle (at 1.999996 0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 90 "MAD_0"))
    (pad "K10" smd circle (at 2.799994 0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 92 "MAD_2"))
    (pad "K11" smd circle (at 3.599993 0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 94 "MAD_10"))
    (pad "K12" smd circle (at 4.399991 0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 203 "N48569969"))
    (pad "L1" smd circle (at -4.399991 1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "L2" smd circle (at -3.599993 1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "L3" smd circle (at -2.799994 1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 184 "DQD_7"))
    (pad "L4" smd circle (at -1.999996 1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 87 "MAD_7"))
    (pad "L9" smd circle (at 1.999996 1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 93 "MAD_11"))
    (pad "L10" smd circle (at 2.799994 1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 175 "DQD_30"))
    (pad "L11" smd circle (at 3.599993 1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "L12" smd circle (at 4.399991 1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "M1" smd circle (at -4.399991 2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "M2" smd circle (at -3.599993 2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 183 "DQD_5"))
    (pad "M3" smd circle (at -2.799994 2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 186 "DQD_6"))
    (pad "M4" smd circle (at -1.999996 2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 89 "MAD_9"))
    (pad "M9" smd circle (at 1.999996 2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 95 "MAD_3"))
    (pad "M10" smd circle (at 2.799994 2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 177 "DQD_25"))
    (pad "M11" smd circle (at 3.599993 2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 174 "DQD_31"))
    (pad "M12" smd circle (at 4.399991 2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "N1" smd circle (at -4.399991 3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "N2" smd circle (at -3.599993 3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 185 "DQD_4"))
    (pad "N3" smd circle (at -2.799994 3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 165 "DQMDB_0"))
    (pad "N4" smd circle (at -1.999996 3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "N9" smd circle (at 1.999996 3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "N10" smd circle (at 2.799994 3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 164 "DQMDB_3"))
    (pad "N11" smd circle (at 3.599993 3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 176 "DQD_24"))
    (pad "N12" smd circle (at 4.399991 3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "P1" smd circle (at -4.399991 3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "P2" smd circle (at -3.599993 3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 209 "QSDB_0"))
    (pad "P3" smd circle (at -2.799994 3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 201 "QSD_0"))
    (pad "P4" smd circle (at -1.999996 3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "P9" smd circle (at 1.999996 3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "P10" smd circle (at 2.799994 3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 200 "QSD_3"))
    (pad "P11" smd circle (at 3.599993 3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 208 "QSDB_3"))
    (pad "P12" smd circle (at 4.399991 3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "R1" smd circle (at -4.399991 4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "R2" smd circle (at -3.599993 4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 187 "DQD_3"))
    (pad "R3" smd circle (at -2.799994 4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 188 "DQD_1"))
    (pad "R4" smd circle (at -1.999996 4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "R9" smd circle (at 1.999996 4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "R10" smd circle (at 2.799994 4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 180 "DQD_27"))
    (pad "R11" smd circle (at 3.599993 4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 179 "DQD_28"))
    (pad "R12" smd circle (at 4.399991 4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "T1" smd circle (at -4.399991 5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "T2" smd circle (at -3.599993 5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 190 "DQD_2"))
    (pad "T3" smd circle (at -2.799994 5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 191 "DQD_0"))
    (pad "T4" smd circle (at -1.999996 5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "T9" smd circle (at 1.999996 5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "T10" smd circle (at 2.799994 5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 182 "DQD_26"))
    (pad "T11" smd circle (at 3.599993 5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 181 "DQD_29"))
    (pad "T12" smd circle (at 4.399991 5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "V1" smd circle (at -4.399991 6.399987 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "V2" smd circle (at -3.599993 6.400013 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "V3" smd circle (at -2.799994 6.400013 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "V4" smd circle (at -1.999996 6.400013 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "V9" smd circle (at 1.999996 6.400013 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 144 "DRAM_RST"))
    (pad "V10" smd circle (at 2.799994 6.400013 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "V11" smd circle (at 3.599993 6.400013 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "V12" smd circle (at 4.399991 6.399987 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "GEOM0002_1" (layer "F.Cu")
    (tedit 0)
    (at 93.004607 65.150992 90)
    (fp_text reference "U202" (at -1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "A1" smd circle (at -4.399991 -6.399987 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "A2" smd circle (at -3.599993 -6.400013 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "A3" smd circle (at -2.799994 -6.400013 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "A4" smd circle (at -1.999996 -6.400013 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 536 "N25405181"))
    (pad "A9" smd circle (at 1.999996 -6.400013 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "A10" smd circle (at 2.799994 -6.400013 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "A11" smd circle (at 3.599993 -6.400013 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "A12" smd circle (at 4.399991 -6.399987 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "B1" smd circle (at -4.399991 -5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "B2" smd circle (at -3.599993 -5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 490 "DQA_38"))
    (pad "B3" smd circle (at -2.799994 -5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 491 "DQA_39"))
    (pad "B4" smd circle (at -1.999996 -5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "B9" smd circle (at 1.999996 -5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "B10" smd circle (at 2.799994 -5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 521 "DQA_47"))
    (pad "B11" smd circle (at 3.599993 -5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 520 "DQA_44"))
    (pad "B12" smd circle (at 4.399991 -5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "C1" smd circle (at -4.399991 -4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "C2" smd circle (at -3.599993 -4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 502 "DQA_32"))
    (pad "C3" smd circle (at -2.799994 -4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 513 "DQA_37"))
    (pad "C4" smd circle (at -1.999996 -4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "C9" smd circle (at 1.999996 -4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "C10" smd circle (at 2.799994 -4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 493 "DQA_45"))
    (pad "C11" smd circle (at 3.599993 -4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 492 "DQA_46"))
    (pad "C12" smd circle (at 4.399991 -4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "D1" smd circle (at -4.399991 -3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "D2" smd circle (at -3.599993 -3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 531 "QSAB_4"))
    (pad "D3" smd circle (at -2.799994 -3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 522 "QSA_4"))
    (pad "D4" smd circle (at -1.999996 -3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "D9" smd circle (at 1.999996 -3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "D10" smd circle (at 2.799994 -3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 523 "QSA_5"))
    (pad "D11" smd circle (at 3.599993 -3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 532 "QSAB_5"))
    (pad "D12" smd circle (at 4.399991 -3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "E1" smd circle (at -4.399991 -3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "E2" smd circle (at -3.599993 -3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 516 "DQA_35"))
    (pad "E3" smd circle (at -2.799994 -3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 486 "DQMAB_4"))
    (pad "E4" smd circle (at -1.999996 -3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "E9" smd circle (at 1.999996 -3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "E10" smd circle (at 2.799994 -3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 487 "DQMAB_5"))
    (pad "E11" smd circle (at 3.599993 -3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 494 "DQA_43"))
    (pad "E12" smd circle (at 4.399991 -3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "F1" smd circle (at -4.399991 -2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "F2" smd circle (at -3.599993 -2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 518 "DQA_34"))
    (pad "F3" smd circle (at -2.799994 -2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 517 "DQA_36"))
    (pad "F4" smd circle (at -1.999996 -2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 483 "CSA1B_0"))
    (pad "F9" smd circle (at 1.999996 -2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 485 "CASA1B"))
    (pad "F10" smd circle (at 2.799994 -2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 495 "DQA_42"))
    (pad "F11" smd circle (at 3.599993 -2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 496 "DQA_40"))
    (pad "F12" smd circle (at 4.399991 -2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "G1" smd circle (at -4.399991 -1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "G2" smd circle (at -3.599993 -1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "G3" smd circle (at -2.799994 -1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 519 "DQA_33"))
    (pad "G4" smd circle (at -1.999996 -1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 478 "MAA_BA1"))
    (pad "G9" smd circle (at 1.999996 -1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 479 "MAA_BA0"))
    (pad "G10" smd circle (at 2.799994 -1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 497 "DQA_41"))
    (pad "G11" smd circle (at 3.599993 -1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "G12" smd circle (at 4.399991 -1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "H1" smd circle (at -4.399991 -0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 529 "N25405147"))
    (pad "H2" smd circle (at -3.599993 -0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 467 "MAA_5"))
    (pad "H3" smd circle (at -2.799994 -0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 526 "MAA_BA2"))
    (pad "H4" smd circle (at -1.999996 -0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 482 "WEA1B"))
    (pad "H9" smd circle (at 1.999996 -0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 535 "CKEA1"))
    (pad "H10" smd circle (at 2.799994 -0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 480 "RASA1B"))
    (pad "H11" smd circle (at 3.599993 -0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 473 "MAA_1"))
    (pad "H12" smd circle (at 4.399991 -0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 530 "N25405167"))
    (pad "J1" smd circle (at -4.399991 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "J2" smd circle (at -3.599993 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "J3" smd circle (at -2.799994 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "J4" smd circle (at -1.999996 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "J9" smd circle (at 1.999996 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "J10" smd circle (at 2.799994 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 484 "CLKA1B"))
    (pad "J11" smd circle (at 3.599993 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 481 "CLKA1"))
    (pad "J12" smd circle (at 4.399991 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "K1" smd circle (at -4.399991 0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 527 "N25405207"))
    (pad "K2" smd circle (at -3.599993 0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 468 "MAA_8"))
    (pad "K3" smd circle (at -2.799994 0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 470 "MAA_6"))
    (pad "K4" smd circle (at -1.999996 0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 466 "MAA_4"))
    (pad "K9" smd circle (at 1.999996 0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 472 "MAA_0"))
    (pad "K10" smd circle (at 2.799994 0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 474 "MAA_2"))
    (pad "K11" smd circle (at 3.599993 0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 476 "MAA_10"))
    (pad "K12" smd circle (at 4.399991 0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 528 "N25405099"))
    (pad "L1" smd circle (at -4.399991 1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "L2" smd circle (at -3.599993 1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "L3" smd circle (at -2.799994 1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 508 "DQA_55"))
    (pad "L4" smd circle (at -1.999996 1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 469 "MAA_7"))
    (pad "L9" smd circle (at 1.999996 1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 475 "MAA_11"))
    (pad "L10" smd circle (at 2.799994 1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 499 "DQA_58"))
    (pad "L11" smd circle (at 3.599993 1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "L12" smd circle (at 4.399991 1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "M1" smd circle (at -4.399991 2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "M2" smd circle (at -3.599993 2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 507 "DQA_53"))
    (pad "M3" smd circle (at -2.799994 2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 510 "DQA_52"))
    (pad "M4" smd circle (at -1.999996 2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 471 "MAA_9"))
    (pad "M9" smd circle (at 1.999996 2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 477 "MAA_3"))
    (pad "M10" smd circle (at 2.799994 2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 501 "DQA_59"))
    (pad "M11" smd circle (at 3.599993 2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 498 "DQA_57"))
    (pad "M12" smd circle (at 4.399991 2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "N1" smd circle (at -4.399991 3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "N2" smd circle (at -3.599993 3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 509 "DQA_54"))
    (pad "N3" smd circle (at -2.799994 3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 489 "DQMAB_6"))
    (pad "N4" smd circle (at -1.999996 3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "N9" smd circle (at 1.999996 3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "N10" smd circle (at 2.799994 3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 488 "DQMAB_7"))
    (pad "N11" smd circle (at 3.599993 3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 500 "DQA_56"))
    (pad "N12" smd circle (at 4.399991 3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "P1" smd circle (at -4.399991 3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "P2" smd circle (at -3.599993 3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 534 "QSAB_6"))
    (pad "P3" smd circle (at -2.799994 3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 525 "QSA_6"))
    (pad "P4" smd circle (at -1.999996 3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "P9" smd circle (at 1.999996 3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "P10" smd circle (at 2.799994 3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 524 "QSA_7"))
    (pad "P11" smd circle (at 3.599993 3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 533 "QSAB_7"))
    (pad "P12" smd circle (at 4.399991 3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "R1" smd circle (at -4.399991 4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "R2" smd circle (at -3.599993 4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 511 "DQA_50"))
    (pad "R3" smd circle (at -2.799994 4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 512 "DQA_51"))
    (pad "R4" smd circle (at -1.999996 4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "R9" smd circle (at 1.999996 4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "R10" smd circle (at 2.799994 4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 504 "DQA_62"))
    (pad "R11" smd circle (at 3.599993 4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 503 "DQA_60"))
    (pad "R12" smd circle (at 4.399991 4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "T1" smd circle (at -4.399991 5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "T2" smd circle (at -3.599993 5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 514 "DQA_49"))
    (pad "T3" smd circle (at -2.799994 5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 515 "DQA_48"))
    (pad "T4" smd circle (at -1.999996 5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "T9" smd circle (at 1.999996 5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "T10" smd circle (at 2.799994 5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 506 "DQA_61"))
    (pad "T11" smd circle (at 3.599993 5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 505 "DQA_63"))
    (pad "T12" smd circle (at 4.399991 5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "V1" smd circle (at -4.399991 6.399987 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "V2" smd circle (at -3.599993 6.400013 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "V3" smd circle (at -2.799994 6.400013 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "V4" smd circle (at -1.999996 6.400013 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "V9" smd circle (at 1.999996 6.400013 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 144 "DRAM_RST"))
    (pad "V10" smd circle (at 2.799994 6.400013 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "V11" smd circle (at 3.599993 6.400013 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "V12" smd circle (at 4.399991 6.399987 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "560UF_4V_R71D55_1" (layer "F.Cu")
    (tedit 0)
    (at 112.399615 28.220002 180)
    (fp_text reference "EC185" (at 1.36398 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole rect (at -1.75006 0 180) (size 1.8034 1.8034) (drill 1.397) (layers *.Cu *.Mask)
      (net 12 "+MVDD"))
    (pad "2" thru_hole circle (at 1.75006 0 180) (size 1.8034 1.8034) (drill 1.397) (layers *.Cu *.Mask)
      (net 4 "GND"))
  )
  (footprint "GEOM0002_1" (layer "F.Cu")
    (tedit 0)
    (at 93.004607 45.151007 90)
    (fp_text reference "U301" (at -1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "A1" smd circle (at -4.399991 -6.399987 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "A2" smd circle (at -3.599993 -6.400013 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "A3" smd circle (at -2.799994 -6.400013 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "A4" smd circle (at -1.999996 -6.400013 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 465 "N49337894"))
    (pad "A9" smd circle (at 1.999996 -6.400013 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "A10" smd circle (at 2.799994 -6.400013 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "A11" smd circle (at 3.599993 -6.400013 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "A12" smd circle (at 4.399991 -6.399987 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "B1" smd circle (at -4.399991 -5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "B2" smd circle (at -3.599993 -5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 420 "DQB_20"))
    (pad "B3" smd circle (at -2.799994 -5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 421 "DQB_23"))
    (pad "B4" smd circle (at -1.999996 -5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "B9" smd circle (at 1.999996 -5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "B10" smd circle (at 2.799994 -5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 451 "DQB_14"))
    (pad "B11" smd circle (at 3.599993 -5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 450 "DQB_13"))
    (pad "B12" smd circle (at 4.399991 -5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "C1" smd circle (at -4.399991 -4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "C2" smd circle (at -3.599993 -4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 432 "DQB_22"))
    (pad "C3" smd circle (at -2.799994 -4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 443 "DQB_21"))
    (pad "C4" smd circle (at -1.999996 -4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "C9" smd circle (at 1.999996 -4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "C10" smd circle (at 2.799994 -4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 423 "DQB_12"))
    (pad "C11" smd circle (at 3.599993 -4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 422 "DQB_15"))
    (pad "C12" smd circle (at 4.399991 -4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "D1" smd circle (at -4.399991 -3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "D2" smd circle (at -3.599993 -3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 460 "QSBB_2"))
    (pad "D3" smd circle (at -2.799994 -3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 452 "QSB_2"))
    (pad "D4" smd circle (at -1.999996 -3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "D9" smd circle (at 1.999996 -3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "D10" smd circle (at 2.799994 -3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 453 "QSB_1"))
    (pad "D11" smd circle (at 3.599993 -3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 461 "QSBB_1"))
    (pad "D12" smd circle (at 4.399991 -3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "E1" smd circle (at -4.399991 -3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "E2" smd circle (at -3.599993 -3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 446 "DQB_17"))
    (pad "E3" smd circle (at -2.799994 -3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 416 "DQMBB_2"))
    (pad "E4" smd circle (at -1.999996 -3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "E9" smd circle (at 1.999996 -3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "E10" smd circle (at 2.799994 -3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 417 "DQMBB_1"))
    (pad "E11" smd circle (at 3.599993 -3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 424 "DQB_10"))
    (pad "E12" smd circle (at 4.399991 -3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "F1" smd circle (at -4.399991 -2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "F2" smd circle (at -3.599993 -2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 448 "DQB_18"))
    (pad "F3" smd circle (at -2.799994 -2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 447 "DQB_16"))
    (pad "F4" smd circle (at -1.999996 -2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 413 "CSB0B_0"))
    (pad "F9" smd circle (at 1.999996 -2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 415 "CASB0B"))
    (pad "F10" smd circle (at 2.799994 -2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 425 "DQB_11"))
    (pad "F11" smd circle (at 3.599993 -2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 426 "DQB_8"))
    (pad "F12" smd circle (at 4.399991 -2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "G1" smd circle (at -4.399991 -1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "G2" smd circle (at -3.599993 -1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "G3" smd circle (at -2.799994 -1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 449 "DQB_19"))
    (pad "G4" smd circle (at -1.999996 -1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 351 "MAB_BA1"))
    (pad "G9" smd circle (at 1.999996 -1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 352 "MAB_BA0"))
    (pad "G10" smd circle (at 2.799994 -1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 427 "DQB_9"))
    (pad "G11" smd circle (at 3.599993 -1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "G12" smd circle (at 4.399991 -1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "H1" smd circle (at -4.399991 -0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 458 "N49337065"))
    (pad "H2" smd circle (at -3.599993 -0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 340 "MAB_5"))
    (pad "H3" smd circle (at -2.799994 -0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 399 "MAB_BA2"))
    (pad "H4" smd circle (at -1.999996 -0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 412 "WEB0B"))
    (pad "H9" smd circle (at 1.999996 -0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 464 "CKEB0"))
    (pad "H10" smd circle (at 2.799994 -0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 410 "RASB0B"))
    (pad "H11" smd circle (at 3.599993 -0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 346 "MAB_1"))
    (pad "H12" smd circle (at 4.399991 -0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 459 "N49337758"))
    (pad "J1" smd circle (at -4.399991 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "J2" smd circle (at -3.599993 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "J3" smd circle (at -2.799994 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "J4" smd circle (at -1.999996 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "J9" smd circle (at 1.999996 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "J10" smd circle (at 2.799994 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 414 "CLKB0B"))
    (pad "J11" smd circle (at 3.599993 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 411 "CLKB0"))
    (pad "J12" smd circle (at 4.399991 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "K1" smd circle (at -4.399991 0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 456 "N49337776"))
    (pad "K2" smd circle (at -3.599993 0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 341 "MAB_8"))
    (pad "K3" smd circle (at -2.799994 0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 343 "MAB_6"))
    (pad "K4" smd circle (at -1.999996 0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 339 "MAB_4"))
    (pad "K9" smd circle (at 1.999996 0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 345 "MAB_0"))
    (pad "K10" smd circle (at 2.799994 0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 347 "MAB_2"))
    (pad "K11" smd circle (at 3.599993 0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 349 "MAB_10"))
    (pad "K12" smd circle (at 4.399991 0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 457 "N49337896"))
    (pad "L1" smd circle (at -4.399991 1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "L2" smd circle (at -3.599993 1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "L3" smd circle (at -2.799994 1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 438 "DQB_7"))
    (pad "L4" smd circle (at -1.999996 1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 342 "MAB_7"))
    (pad "L9" smd circle (at 1.999996 1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 348 "MAB_11"))
    (pad "L10" smd circle (at 2.799994 1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 429 "DQB_27"))
    (pad "L11" smd circle (at 3.599993 1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "L12" smd circle (at 4.399991 1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "M1" smd circle (at -4.399991 2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "M2" smd circle (at -3.599993 2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 437 "DQB_5"))
    (pad "M3" smd circle (at -2.799994 2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 440 "DQB_6"))
    (pad "M4" smd circle (at -1.999996 2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 344 "MAB_9"))
    (pad "M9" smd circle (at 1.999996 2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 350 "MAB_3"))
    (pad "M10" smd circle (at 2.799994 2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 431 "DQB_25"))
    (pad "M11" smd circle (at 3.599993 2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 428 "DQB_26"))
    (pad "M12" smd circle (at 4.399991 2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "N1" smd circle (at -4.399991 3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "N2" smd circle (at -3.599993 3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 439 "DQB_4"))
    (pad "N3" smd circle (at -2.799994 3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 419 "DQMBB_0"))
    (pad "N4" smd circle (at -1.999996 3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "N9" smd circle (at 1.999996 3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "N10" smd circle (at 2.799994 3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 418 "DQMBB_3"))
    (pad "N11" smd circle (at 3.599993 3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 430 "DQB_24"))
    (pad "N12" smd circle (at 4.399991 3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "P1" smd circle (at -4.399991 3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "P2" smd circle (at -3.599993 3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 463 "QSBB_0"))
    (pad "P3" smd circle (at -2.799994 3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 455 "QSB_0"))
    (pad "P4" smd circle (at -1.999996 3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "P9" smd circle (at 1.999996 3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "P10" smd circle (at 2.799994 3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 454 "QSB_3"))
    (pad "P11" smd circle (at 3.599993 3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 462 "QSBB_3"))
    (pad "P12" smd circle (at 4.399991 3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "R1" smd circle (at -4.399991 4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "R2" smd circle (at -3.599993 4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 441 "DQB_3"))
    (pad "R3" smd circle (at -2.799994 4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 442 "DQB_1"))
    (pad "R4" smd circle (at -1.999996 4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "R9" smd circle (at 1.999996 4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "R10" smd circle (at 2.799994 4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 434 "DQB_30"))
    (pad "R11" smd circle (at 3.599993 4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 433 "DQB_31"))
    (pad "R12" smd circle (at 4.399991 4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "T1" smd circle (at -4.399991 5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "T2" smd circle (at -3.599993 5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 444 "DQB_2"))
    (pad "T3" smd circle (at -2.799994 5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 445 "DQB_0"))
    (pad "T4" smd circle (at -1.999996 5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "T9" smd circle (at 1.999996 5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "T10" smd circle (at 2.799994 5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 436 "DQB_28"))
    (pad "T11" smd circle (at 3.599993 5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 435 "DQB_29"))
    (pad "T12" smd circle (at 4.399991 5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "V1" smd circle (at -4.399991 6.399987 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "V2" smd circle (at -3.599993 6.400013 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "V3" smd circle (at -2.799994 6.400013 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "V4" smd circle (at -1.999996 6.400013 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "V9" smd circle (at 1.999996 6.400013 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 144 "DRAM_RST"))
    (pad "V10" smd circle (at 2.799994 6.400013 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "V11" smd circle (at 3.599993 6.400013 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "V12" smd circle (at 4.399991 6.399987 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at 21.104624 72.251004 180)
    (fp_text reference "R105" (at -1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 714 "T2X5P"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 713 "T2X5M"))
  )
  (footprint "TP055PRI_1" (layer "F.Cu")
    (tedit 0)
    (at 22.204621 84.151005)
    (fp_text reference "TP8" (at -0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd circle (at 0 0) (size 0.550012 0.550012) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 619 "PETN0_GFXRN0"))
  )
  (footprint "CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -18.605381 76.380993)
    (fp_text reference "C843" (at 1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 853 "LVT_EN"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1608_1" (layer "F.Cu")
    (tedit 0)
    (at 154.563615 52.731002)
    (fp_text reference "AR85" (at 1.904975 1.905025 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 938 "N86495516"))
    (pad "2" smd rect (at 0 0.7874) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 64 "BOOT2"))
  )
  (footprint "CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at 21.768122 55.151012 180)
    (fp_text reference "C111" (at -1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 690 "GND_TPVSS"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 689 "+TPVDD"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -34.695392 89.750994 -90)
    (fp_text reference "R1002" (at 2.54 -2.2225 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "A_DAC1_G"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1608_1" (layer "F.Cu")
    (tedit 0)
    (at 156.341615 52.731002)
    (fp_text reference "AC32" (at 1.904975 1.905025 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 938 "N86495516"))
    (pad "2" smd rect (at 0 0.7874) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 68 "APHASE_2"))
  )
  (footprint "TP055PRI_1" (layer "F.Cu")
    (tedit 0)
    (at 44.804627 84.151005)
    (fp_text reference "TP27" (at -1.27 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd circle (at 0 0) (size 0.550012 0.550012) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 723 "PETP15_GFXRP15"))
  )
  (footprint "SOT23_3PIN_1" (layer "F.Cu")
    (tedit 0)
    (at 104.144615 11.456002)
    (fp_text reference "Q4030" (at 1.289075 1.4732 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.9398 1.143) (size 0.640004 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 836 "N72984167"))
    (pad "2" smd rect (at 0.9398 1.143) (size 0.640004 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "3" smd rect (at 0 -1.143) (size 0.640004 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 859 "N49971328"))
  )
  (footprint "TP089X043_1" (layer "F.Cu")
    (tedit 0)
    (at -11.545375 47.201016)
    (fp_text reference "TP81" (at -1.27 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 0.5588 0.5588) (drill 0.250012) (layers *.Cu *.Mask)
      (net 681 "DVPDATA_21"))
  )
  (footprint "CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at 157.611615 28.474002 90)
    (fp_text reference "AC14" (at -1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 921 "N86494727"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 922 "N86494729"))
  )
  (footprint "RES1608_1" (layer "F.Cu")
    (tedit 0)
    (at 133.486187 40.666002 90)
    (fp_text reference "AR89" (at -1.905025 1.904975 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 90) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 866 "N86494416"))
    (pad "2" smd rect (at 0 0.7874 90) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 63 "UG2"))
  )
  (footprint "CAP1608_1" (layer "F.Cu")
    (tedit 0)
    (at 116.209615 9.551002 180)
    (fp_text reference "EC7" (at -1.587475 -1.270025 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 180) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 912 "N85769464"))
    (pad "2" smd rect (at 0 0.7874 180) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 911 "N85769434"))
  )
  (footprint "C1206_113_1" (layer "F.Cu")
    (tedit 0)
    (at 145.927615 42.952002 90)
    (fp_text reference "C1585" (at 0 -0.981075 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd oval (at -1.4351 0 90) (size 0.9779 1.1938) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 865 "PWM2_VIN"))
    (pad "2" smd oval (at 1.4351 0 90) (size 0.9779 1.1938) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "DPAKSGD_1" (layer "F.Cu")
    (tedit 0)
    (at 138.820187 26.569002 90)
    (fp_text reference "EQ37" (at -1.146175 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "D" smd rect (at 0 -3.7465 90) (size 5.6896 5.6388) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 59 "N85769021"))
    (pad "G" smd oval (at -2.286 3.7465 90) (size 1.651 2.6797) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 908 "N85769514"))
    (pad "S" smd oval (at 2.286 3.7465 90) (size 1.651 2.6797) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at 86.618615 8.535002)
    (fp_text reference "R4030" (at 2.2225 2.54 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "+3.3V_BUS"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 835 "N49971448"))
  )
  (footprint "CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -9.153787 64.661306)
    (fp_text reference "C4003" (at 2.2225 2.54 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "+3.3V"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "TP089X043_1" (layer "F.Cu")
    (tedit 0)
    (at -21.183379 6.895)
    (fp_text reference "TP66" (at -1.27 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 0.5588 0.5588) (drill 0.250012) (layers *.Cu *.Mask)
      (net 809 "DVPDATA_6"))
  )
  (footprint "GEOM0007_1" (layer "F.Cu")
    (tedit 0)
    (at 122.686615 43.206002 90)
    (fp_text reference "L64" (at -1.27 1.5875 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 4.500118 90) (size 3.81 3.81) (drill 2.413) (layers *.Cu *.Mask)
      (net 68 "APHASE_2"))
    (pad "2" thru_hole circle (at 0 -4.500118 90) (size 3.81 3.81) (drill 2.413) (layers *.Cu *.Mask)
      (net 735 "+VDDC"))
  )
  (footprint "SOT23-6PIN_1_45H_1" (layer "F.Cu")
    (tedit 0)
    (at -43.195375 88.950996)
    (fp_text reference "D1001" (at 1.444537 1.650873 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.950011 1.500099) (size 0.640004 0.999998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 48 "A_R_DAC1_F"))
    (pad "2" smd rect (at 0 1.500099) (size 0.640004 0.999998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "3" smd rect (at 0.950011 1.500099) (size 0.640004 0.999998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 46 "A_G_DAC1_F"))
    (pad "4" smd rect (at 0.950011 -1.500099) (size 0.640004 0.999998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 44 "A_B_DAC1_F"))
    (pad "5" smd rect (at 0 -1.500099) (size 0.640004 0.999998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "+3.3V"))
    (pad "6" smd rect (at -0.950011 -1.500099) (size 0.640004 0.999998) (layers "F.Cu" "F.Paste" "F.Mask"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at 150.753615 29.236002 -90)
    (fp_text reference "AR23" (at 1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 923 "N86494909"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "+12V_EXT"))
  )
  (footprint "C1206_113_1" (layer "F.Cu")
    (tedit 0)
    (at 165.485615 25.172002)
    (fp_text reference "EC136" (at -0.981075 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd oval (at -1.4351 0) (size 0.9779 1.1938) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 82 "VDD_+5V"))
    (pad "2" smd oval (at 1.4351 0) (size 0.9779 1.1938) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "SOT23_3PIN_1" (layer "F.Cu")
    (tedit 0)
    (at 127.639615 8.281002 180)
    (fp_text reference "ED2" (at -1.534586 -1.227671 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.9398 1.143 180) (size 0.640004 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "N85769551"))
    (pad "2" smd rect (at 0.9398 1.143 180) (size 0.640004 1.27) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "3" smd rect (at 0 -1.143 180) (size 0.640004 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 915 "N85769214"))
  )
  (footprint "C1206_113_1" (layer "F.Cu")
    (tedit 0)
    (at 112.526615 82.576002 180)
    (fp_text reference "EC1160" (at 0.981075 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd oval (at -1.4351 0 180) (size 0.9779 1.1938) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd oval (at 1.4351 0 180) (size 0.9779 1.1938) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "C1206_113_1" (layer "F.Cu")
    (tedit 0)
    (at 112.272615 22.632002 180)
    (fp_text reference "EC169" (at 0.981075 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd oval (at -1.4351 0 180) (size 0.9779 1.1938) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd oval (at 1.4351 0 180) (size 0.9779 1.1938) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -43.995373 93.851011)
    (fp_text reference "C1001" (at 2.2225 2.54 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 48 "A_R_DAC1_F"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "F_PAD_M120_1" (layer "F.Cu")
    (tedit 0)
    (at 146.435615 91.593002)
    (fp_text reference "FM3" (at -0.762501 -0.000013 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd circle (at 0 0) (size 1.020064 1.020064) (layers "F.Cu" "F.Paste" "F.Mask"))
  )
  (footprint "SOT23_3PIN_1" (layer "F.Cu")
    (tedit 0)
    (at -41.495378 80.651012 -90)
    (fp_text reference "Q1021" (at 1.4732 -1.289075 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.9398 1.143 270) (size 0.640004 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 861 "N26590941"))
    (pad "2" smd rect (at 0.9398 1.143 270) (size 0.640004 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 818 "HPD2"))
    (pad "3" smd rect (at 0 -1.143 270) (size 0.640004 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "+3.3V"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at 148.086615 36.729002 90)
    (fp_text reference "AR36" (at -1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 932 "AICSN24"))
  )
  (footprint "DPAKSGD_1" (layer "F.Cu")
    (tedit 0)
    (at 137.677187 84.862002 -90)
    (fp_text reference "MQ1309" (at 2.416175 -2.54 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "D" smd rect (at 0 -3.7465 270) (size 5.6896 5.6388) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 863 "PWM3_VIN"))
    (pad "G" smd oval (at -2.286 3.7465 270) (size 1.651 2.6797) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 864 "N86495503"))
    (pad "S" smd oval (at 2.286 3.7465 270) (size 1.651 2.6797) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 598 "APHASE_3"))
  )
  (footprint "CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -35.195391 91.250991)
    (fp_text reference "C1005" (at 2.2225 2.54 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "A_DAC1_G"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "TP089X043_1" (layer "F.Cu")
    (tedit 0)
    (at -16.095378 6.905008)
    (fp_text reference "TP60" (at -1.27 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 0.5588 0.5588) (drill 0.250012) (layers *.Cu *.Mask)
      (net 813 "DVPDATA_0"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -33.495394 64.150994 180)
    (fp_text reference "R3003" (at -2.2225 -2.54 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 654 "A_DAC2_COMP"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "TP089X043_1" (layer "F.Cu")
    (tedit 0)
    (at -38.995383 9.751002)
    (fp_text reference "TP83" (at -1.27 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 0.5588 0.5588) (drill 0.250012) (layers *.Cu *.Mask)
      (net 780 "DVPDATA_23"))
  )
  (footprint "CAP3216_1_80H_1" (layer "F.Cu")
    (tedit 0)
    (at -9.195392 97.251004 90)
    (fp_text reference "C1" (at -0.635 1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -1.4478 90) (size 1.799996 1.399997) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "+12V_BUS"))
    (pad "2" smd rect (at 0 1.4478 90) (size 1.799996 1.399997) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "TP055PRI_1" (layer "F.Cu")
    (tedit 0)
    (at 39.204613 83.151007)
    (fp_text reference "TP22" (at -1.27 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd circle (at 0 0) (size 0.550012 0.550012) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 613 "PETN11_GFXRN11"))
  )
  (footprint "GEOM0003_1" (layer "F.Cu")
    (tedit 0)
    (at 41.004609 57.151008 -90)
    (fp_text reference "U1" (at 0 0.635 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "A3" smd circle (at -15.299995 -16.299993 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 320 "DQC_10"))
    (pad "A6" smd circle (at -14.499996 -16.799992 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "A8" smd circle (at -13.624992 -16.399993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 311 "DQC_6"))
    (pad "A10" smd circle (at -12.8 -16.799992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 312 "DQC_4"))
    (pad "A12" smd circle (at -11.200003 -16.799992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 317 "DQC_2"))
    (pad "A14" smd circle (at -9.600006 -16.799992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 378 "DQB_53"))
    (pad "A16" smd circle (at -8.000009 -16.799992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 372 "DQB_51"))
    (pad "A18" smd circle (at -6.400013 -16.799992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 383 "DQB_36"))
    (pad "A20" smd circle (at -4.800016 -16.799992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 362 "DQMBB_4"))
    (pad "A22" smd circle (at -3.199994 -16.799992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 436 "DQB_28"))
    (pad "A24" smd circle (at -1.599997 -16.799992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 462 "QSBB_3"))
    (pad "A26" smd circle (at 0 -16.799992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 430 "DQB_24"))
    (pad "A28" smd circle (at 1.599997 -16.799992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 452 "QSB_2"))
    (pad "A30" smd circle (at 3.199994 -16.799992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 446 "DQB_17"))
    (pad "A32" smd circle (at 4.79999 -16.799992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 439 "DQB_4"))
    (pad "A34" smd circle (at 6.399987 -16.799992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 444 "DQB_2"))
    (pad "A36" smd circle (at 7.999984 -16.799992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 505 "DQA_63"))
    (pad "A38" smd circle (at 9.600006 -16.799992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 499 "DQA_58"))
    (pad "A40" smd circle (at 11.200003 -16.799992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 510 "DQA_52"))
    (pad "A42" smd circle (at 12.8 -16.799992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 525 "QSA_6"))
    (pad "A44" smd circle (at 13.624992 -16.399993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 512 "DQA_51"))
    (pad "A46" smd circle (at 14.499996 -16.799992 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 513 "DQA_37"))
    (pad "A49" smd circle (at 15.299995 -16.299993 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AA2" smd circle (at -16.399993 -3.999992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AA4" smd circle (at -15.599994 -3.999992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 235 "DQMCB_6"))
    (pad "AA6" smd circle (at -14.799996 -3.999992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 280 "QSCB_6"))
    (pad "AA9" smd circle (at -13.599998 -4.399991 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 266 "DQC_40"))
    (pad "AA10" smd circle (at -12.8 -4.399991 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 267 "DQC_41"))
    (pad "AA11" smd circle (at -12.000001 -4.399991 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 239 "DQC_43"))
    (pad "AA12" smd circle (at -11.200003 -4.399991 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 221 "MAC_11"))
    (pad "AA13" smd circle (at -10.400005 -4.399991 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AA14" smd circle (at -9.600006 -4.399991 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "AA15" smd circle (at -8.800008 -4.399991 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 224 "MAC_BA1"))
    (pad "AA16" smd circle (at -8.000009 -4.399991 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AA19" smd circle (at -6.000013 -3.999992 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "+VDDCI"))
    (pad "AA20" smd circle (at -5.000015 -3.999992 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AA21" smd circle (at -3.999992 -3.999992 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "+VDDCI"))
    (pad "AA22" smd circle (at -2.999994 -3.999992 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AA24" smd circle (at -1.999996 -3.999992 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AA25" smd circle (at -0.999998 -3.999992 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AA26" smd circle (at 0 -3.999992 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AA27" smd circle (at 0.999998 -3.999992 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AA28" smd circle (at 1.999996 -3.999992 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AA30" smd circle (at 2.999994 -3.999992 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AA31" smd circle (at 3.999992 -3.999992 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AA32" smd circle (at 4.99999 -3.999992 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AA33" smd circle (at 5.999988 -3.999992 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AA36" smd circle (at 7.999984 -3.999992 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AA37" smd circle (at 8.800008 -3.999992 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 466 "MAA_4"))
    (pad "AA38" smd circle (at 9.600006 -3.999992 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 540 "CSA0B_0"))
    (pad "AA39" smd circle (at 10.400005 -3.999992 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AA40" smd circle (at 11.200003 -3.999992 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "AA41" smd circle (at 12.000001 -3.999992 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AA42" smd circle (at 12.8 -3.999992 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 577 "DQA_21"))
    (pad "AA43" smd circle (at 13.599998 -3.999992 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 588 "QSAB_2"))
    (pad "AA46" smd circle (at 14.799996 -3.999992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 568 "DQA_3"))
    (pad "AA48" smd circle (at 15.599994 -3.999992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AA50" smd circle (at 16.399993 -3.999992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 582 "QSA_0"))
    (pad "AB1" smd circle (at -16.799992 -3.199994 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 256 "DQC_54"))
    (pad "AB3" smd circle (at -15.999993 -3.199994 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 253 "DQC_53"))
    (pad "AB5" smd circle (at -15.199995 -3.199994 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 255 "DQC_52"))
    (pad "AB7" smd circle (at -14.399997 -3.199994 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "AB9" smd circle (at -13.599998 -3.199994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 238 "DQC_42"))
    (pad "AB10" smd circle (at -12.8 -3.199994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "AB11" smd circle (at -12.000001 -3.199994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AB12" smd circle (at -11.200003 -3.199994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 222 "MAC_10"))
    (pad "AB13" smd circle (at -10.400005 -3.199994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 214 "MAC_8"))
    (pad "AB14" smd circle (at -9.600006 -3.199994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 217 "MAC_9"))
    (pad "AB15" smd circle (at -8.800008 -3.199994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AB16" smd circle (at -8.000009 -3.199994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AB19" smd circle (at -6.000013 -2.999994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AB20" smd circle (at -5.000015 -2.999994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "+VDDCI"))
    (pad "AB21" smd circle (at -3.999992 -2.999994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AB22" smd circle (at -2.999994 -2.999994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AB24" smd circle (at -1.999996 -2.999994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AB25" smd circle (at -0.999998 -2.999994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AB26" smd circle (at 0 -2.999994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AB27" smd circle (at 0.999998 -2.999994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AB28" smd circle (at 1.999996 -2.999994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AB30" smd circle (at 2.999994 -2.999994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AB31" smd circle (at 3.999992 -2.999994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AB32" smd circle (at 4.99999 -2.999994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AB33" smd circle (at 5.999988 -2.999994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AB45" smd circle (at 14.399997 -3.199994 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "AB47" smd circle (at 15.199995 -3.199994 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 572 "DQA_0"))
    (pad "AB49" smd circle (at 15.999993 -3.199994 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 569 "DQA_1"))
    (pad "AB51" smd circle (at 16.799992 -3.199994 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 571 "DQA_2"))
    (pad "AC2" smd circle (at -16.399993 -2.399995 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 246 "DQC_56"))
    (pad "AC4" smd circle (at -15.599994 -2.399995 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AC6" smd circle (at -14.799996 -2.399995 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 254 "DQC_55"))
    (pad "AC36" smd circle (at 7.999984 -2.799994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AC37" smd circle (at 8.800008 -2.799994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "AC38" smd circle (at 9.600006 -2.799994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AC39" smd circle (at 10.400005 -2.799994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 550 "DQA_20"))
    (pad "AC40" smd circle (at 11.200003 -2.799994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AC41" smd circle (at 12.000001 -2.799994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 580 "QSA_2"))
    (pad "AC42" smd circle (at 12.8 -2.799994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 544 "DQMAB_2"))
    (pad "AC43" smd circle (at 13.599998 -2.799994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 719 "MVREFS_A"))
    (pad "AC46" smd circle (at 14.799996 -2.399995 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 730 "MVREFD_A"))
    (pad "AC48" smd circle (at 15.599994 -2.399995 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AC50" smd circle (at 16.399993 -2.399995 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AD1" smd circle (at -16.799992 -1.599997 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 245 "DQC_59"))
    (pad "AD3" smd circle (at -15.999993 -1.599997 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 244 "DQC_58"))
    (pad "AD5" smd circle (at -15.199995 -1.599997 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 247 "DQC_57"))
    (pad "AD7" smd circle (at -14.399997 -1.599997 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AD9" smd circle (at -13.599998 -1.999996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 278 "QSCB_5"))
    (pad "AD10" smd circle (at -12.8 -1.999996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 269 "QSC_5"))
    (pad "AD11" smd circle (at -12.000001 -1.999996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 233 "DQMCB_5"))
    (pad "AD12" smd circle (at -11.200003 -1.999996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 231 "CASC1B"))
    (pad "AD13" smd circle (at -10.400005 -1.999996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AD14" smd circle (at -9.600006 -1.999996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 281 "CKEC1"))
    (pad "AD15" smd circle (at -8.800008 -1.999996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "AD16" smd circle (at -8.000009 -1.999996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AD19" smd circle (at -6.000013 -1.999996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "+VDDCI"))
    (pad "AD20" smd circle (at -5.000015 -1.999996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AD21" smd circle (at -3.999992 -1.999996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AD22" smd circle (at -2.999994 -1.999996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AD24" smd circle (at -1.999996 -1.999996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AD25" smd circle (at -0.999998 -1.999996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AD26" smd circle (at 0 -1.999996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AD27" smd circle (at 0.999998 -1.999996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AD28" smd circle (at 1.999996 -1.999996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AD30" smd circle (at 2.999994 -1.999996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AD31" smd circle (at 3.999992 -1.999996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AD32" smd circle (at 4.99999 -1.999996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AD33" smd circle (at 5.999988 -1.999996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AD36" smd circle (at 7.999984 -1.599997 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AD37" smd circle (at 8.800008 -1.599997 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AD38" smd circle (at 9.600006 -1.599997 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 553 "DQA_16"))
    (pad "AD39" smd circle (at 10.400005 -1.599997 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 554 "DQA_17"))
    (pad "AD40" smd circle (at 11.200003 -1.599997 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 552 "DQA_18"))
    (pad "AD41" smd circle (at 12.000001 -1.599997 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 551 "DQA_19"))
    (pad "AD42" smd circle (at 12.8 -1.599997 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AD43" smd circle (at 13.599998 -1.599997 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "AD45" smd circle (at 14.399997 -1.599997 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AD47" smd circle (at 15.199995 -1.599997 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AD49" smd circle (at 15.999993 -1.599997 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 724 "PETN15_GFXRN15"))
    (pad "AD51" smd circle (at 16.799992 -1.599997 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 723 "PETP15_GFXRP15"))
    (pad "AE2" smd circle (at -16.399993 -0.799998 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AE4" smd circle (at -15.599994 -0.799998 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 279 "QSCB_7"))
    (pad "AE6" smd circle (at -14.799996 -0.799998 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 234 "DQMCB_7"))
    (pad "AE9" smd circle (at -13.599998 -0.799998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 242 "DQC_47"))
    (pad "AE10" smd circle (at -12.8 -0.799998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 241 "DQC_46"))
    (pad "AE11" smd circle (at -12.000001 -0.799998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 240 "DQC_45"))
    (pad "AE12" smd circle (at -11.200003 -0.799998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AE13" smd circle (at -10.400005 -0.799998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "AE14" smd circle (at -9.600006 -0.799998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 226 "RASC1B"))
    (pad "AE15" smd circle (at -8.800008 -0.799998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 84 "MAD_4"))
    (pad "AE16" smd circle (at -8.000009 -0.799998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AE19" smd circle (at -6.000013 -0.999998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AE20" smd circle (at -5.000015 -0.999998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AE21" smd circle (at -3.999992 -0.999998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AE22" smd circle (at -2.999994 -0.999998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AE24" smd circle (at -1.999996 -0.999998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AE25" smd circle (at -0.999998 -0.999998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AE26" smd circle (at 0 -0.999998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AE27" smd circle (at 0.999998 -0.999998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AE28" smd circle (at 1.999996 -0.999998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AE30" smd circle (at 2.999994 -0.999998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AE31" smd circle (at 3.999992 -0.999998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AE32" smd circle (at 4.99999 -0.999998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AE33" smd circle (at 5.999988 -0.999998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AE46" smd circle (at 14.799996 -0.799998 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 717 "PETN14_GFXRN14"))
    (pad "AE48" smd circle (at 15.599994 -0.799998 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 762 "PETP14_GFXRP14"))
    (pad "AE50" smd circle (at 16.399993 -0.799998 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AF1" smd circle (at -16.799992 0 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 251 "DQC_61"))
    (pad "AF3" smd circle (at -15.999993 0 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 249 "DQC_60"))
    (pad "AF5" smd circle (at -15.199995 0 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 270 "QSC_7"))
    (pad "AF7" smd circle (at -14.399997 0 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "AF9" smd circle (at -13.599998 0.399999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 243 "DQC_44"))
    (pad "AF10" smd circle (at -12.8 0.399999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AF11" smd circle (at -12.000001 0.399999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 172 "DQD_16"))
    (pad "AF12" smd circle (at -11.200003 0.399999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 173 "DQD_17"))
    (pad "AF13" smd circle (at -10.400005 0.399999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 170 "DQD_18"))
    (pad "AF14" smd circle (at -9.600006 0.399999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 159 "CSD0B_0"))
    (pad "AF15" smd circle (at -8.800008 0.399999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "AF16" smd circle (at -8.000009 0.399999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AF19" smd circle (at -6.000013 0 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AF20" smd circle (at -5.000015 0 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AF21" smd circle (at -3.999992 0 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AF22" smd circle (at -2.999994 0 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AF24" smd circle (at -1.999996 0 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AF25" smd circle (at -0.999998 0 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AF26" smd circle (at 0 0 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AF27" smd circle (at 0.999998 0 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AF28" smd circle (at 1.999996 0 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AF30" smd circle (at 2.999994 0 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AF31" smd circle (at 3.999992 0 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AF32" smd circle (at 4.99999 0 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AF33" smd circle (at 5.999988 0 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AF36" smd circle (at 7.999984 -0.399999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 716 "+PCIE_VDDC"))
    (pad "AF37" smd circle (at 8.800008 -0.399999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 716 "+PCIE_VDDC"))
    (pad "AF38" smd circle (at 9.600006 -0.399999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 716 "+PCIE_VDDC"))
    (pad "AF39" smd circle (at 10.400005 -0.399999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AF40" smd circle (at 11.200003 -0.399999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AF41" smd circle (at 12.000001 -0.399999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AF42" smd circle (at 12.8 -0.399999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AF43" smd circle (at 13.599998 -0.399999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AF45" smd circle (at 14.399997 0 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AF47" smd circle (at 15.199995 0 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AF49" smd circle (at 15.999993 0 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 726 "PETN13_GFXRN13"))
    (pad "AF51" smd circle (at 16.799992 0 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 729 "PETP13_GFXRP13"))
    (pad "AG2" smd circle (at -16.399993 0.799998 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 252 "DQC_63"))
    (pad "AG4" smd circle (at -15.599994 0.799998 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AG6" smd circle (at -14.799996 0.799998 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 250 "DQC_62"))
    (pad "AG19" smd circle (at -6.000013 0.999998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AG20" smd circle (at -5.000015 0.999998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AG21" smd circle (at -3.999992 0.999998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AG22" smd circle (at -2.999994 0.999998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AG24" smd circle (at -1.999996 0.999998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AG25" smd circle (at -0.999998 0.999998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AG26" smd circle (at 0 0.999998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AG27" smd circle (at 0.999998 0.999998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AG28" smd circle (at 1.999996 0.999998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AG30" smd circle (at 2.999994 0.999998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AG31" smd circle (at 3.999992 0.999998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AG32" smd circle (at 4.99999 0.999998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AG33" smd circle (at 5.999988 0.999998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AG36" smd circle (at 7.999984 0.799998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 716 "+PCIE_VDDC"))
    (pad "AG37" smd circle (at 8.800008 0.799998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 716 "+PCIE_VDDC"))
    (pad "AG38" smd circle (at 9.600006 0.799998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AG39" smd circle (at 10.400005 0.799998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 722 "GFXTN14_PERN14"))
    (pad "AG40" smd circle (at 11.200003 0.799998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 721 "GFXTP14_PERP14"))
    (pad "AG41" smd circle (at 12.000001 0.799998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AG42" smd circle (at 12.8 0.799998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 727 "GFXTN15_PERN15"))
    (pad "AG43" smd circle (at 13.599998 0.799998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 728 "GFXTP15_PERP15"))
    (pad "AG46" smd circle (at 14.799996 0.799998 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 725 "PETN12_GFXRN12"))
    (pad "AG48" smd circle (at 15.599994 0.799998 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 775 "PETP12_GFXRP12"))
    (pad "AG50" smd circle (at 16.399993 0.799998 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AH1" smd circle (at -16.799992 1.599997 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 190 "DQD_2"))
    (pad "AH3" smd circle (at -15.999993 1.599997 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 188 "DQD_1"))
    (pad "AH5" smd circle (at -15.199995 1.599997 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 191 "DQD_0"))
    (pad "AH7" smd circle (at -14.399997 1.599997 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AH9" smd circle (at -13.599998 1.599997 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 738 "MVREFS_D"))
    (pad "AH10" smd circle (at -12.8 1.599997 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AH11" smd circle (at -12.000001 1.599997 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "AH12" smd circle (at -11.200003 1.599997 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 171 "DQD_19"))
    (pad "AH13" smd circle (at -10.400005 1.599997 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AH14" smd circle (at -9.600006 1.599997 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 158 "WED0B"))
    (pad "AH15" smd circle (at -8.800008 1.599997 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 85 "MAD_5"))
    (pad "AH16" smd circle (at -8.000009 1.599997 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AH19" smd circle (at -6.000013 1.999996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AH20" smd circle (at -5.000015 1.999996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AH21" smd circle (at -3.999992 1.999996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AH22" smd circle (at -2.999994 1.999996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AH24" smd circle (at -1.999996 1.999996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AH25" smd circle (at -0.999998 1.999996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AH26" smd circle (at 0 1.999996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AH27" smd circle (at 0.999998 1.999996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AH28" smd circle (at 1.999996 1.999996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AH30" smd circle (at 2.999994 1.999996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AH31" smd circle (at 3.999992 1.999996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AH32" smd circle (at 4.99999 1.999996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AH33" smd circle (at 5.999988 1.999996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AH36" smd circle (at 7.999984 1.999996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 716 "+PCIE_VDDC"))
    (pad "AH37" smd circle (at 8.800008 1.999996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 716 "+PCIE_VDDC"))
    (pad "AH38" smd circle (at 9.600006 1.999996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AH39" smd circle (at 10.400005 1.999996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 747 "GFXTN12_PERN12"))
    (pad "AH40" smd circle (at 11.200003 1.999996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 749 "GFXTP12_PERP12"))
    (pad "AH41" smd circle (at 12.000001 1.999996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AH42" smd circle (at 12.8 1.999996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 745 "GFXTN13_PERN13"))
    (pad "AH43" smd circle (at 13.599998 1.999996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 748 "GFXTP13_PERP13"))
    (pad "AH45" smd circle (at 14.399997 1.599997 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AH47" smd circle (at 15.199995 1.599997 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AH49" smd circle (at 15.999993 1.599997 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 613 "PETN11_GFXRN11"))
    (pad "AH51" smd circle (at 16.799992 1.599997 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 614 "PETP11_GFXRP11"))
    (pad "AJ2" smd circle (at -16.399993 2.399995 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AJ4" smd circle (at -15.599994 2.399995 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 201 "QSD_0"))
    (pad "AJ6" smd circle (at -14.799996 2.399995 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 187 "DQD_3"))
    (pad "AJ9" smd circle (at -13.599998 2.799994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 739 "MVREFD_D"))
    (pad "AJ10" smd circle (at -12.8 2.799994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 163 "DQMDB_2"))
    (pad "AJ11" smd circle (at -12.000001 2.799994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 207 "QSDB_2"))
    (pad "AJ12" smd circle (at -11.200003 2.799994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 199 "QSD_2"))
    (pad "AJ13" smd circle (at -10.400005 2.799994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 88 "MAD_6"))
    (pad "AJ14" smd circle (at -9.600006 2.799994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AJ15" smd circle (at -8.800008 2.799994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 87 "MAD_7"))
    (pad "AJ16" smd circle (at -8.000009 2.799994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 90 "MAD_0"))
    (pad "AJ46" smd circle (at 14.799996 2.399995 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 611 "PETN10_GFXRN10"))
    (pad "AJ48" smd circle (at 15.599994 2.399995 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 612 "PETP10_GFXRP10"))
    (pad "AJ50" smd circle (at 16.399993 2.399995 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AK1" smd circle (at -16.799992 3.199994 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 185 "DQD_4"))
    (pad "AK3" smd circle (at -15.999993 3.199994 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 165 "DQMDB_0"))
    (pad "AK5" smd circle (at -15.199995 3.199994 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 209 "QSDB_0"))
    (pad "AK7" smd circle (at -14.399997 3.199994 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "AK19" smd circle (at -6.000013 2.999994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AK20" smd circle (at -5.000015 2.999994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AK21" smd circle (at -3.999992 2.999994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AK22" smd circle (at -2.999994 2.999994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AK24" smd circle (at -1.999996 2.999994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AK25" smd circle (at -0.999998 2.999994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AK26" smd circle (at 0 2.999994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AK27" smd circle (at 0.999998 2.999994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AK28" smd circle (at 1.999996 2.999994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AK30" smd circle (at 2.999994 2.999994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AK31" smd circle (at 3.999992 2.999994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AK32" smd circle (at 4.99999 2.999994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AK33" smd circle (at 5.999988 2.999994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AK36" smd circle (at 7.999984 3.199994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 716 "+PCIE_VDDC"))
    (pad "AK37" smd circle (at 8.800008 3.199994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 716 "+PCIE_VDDC"))
    (pad "AK38" smd circle (at 9.600006 3.199994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AK39" smd circle (at 10.400005 3.199994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 637 "GFXTN10_PERN10"))
    (pad "AK40" smd circle (at 11.200003 3.199994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 776 "GFXTP10_PERP10"))
    (pad "AK41" smd circle (at 12.000001 3.199994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AK42" smd circle (at 12.8 3.199994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 638 "GFXTN11_PERN11"))
    (pad "AK43" smd circle (at 13.599998 3.199994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 743 "GFXTP11_PERP11"))
    (pad "AK45" smd circle (at 14.399997 3.199994 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AK47" smd circle (at 15.199995 3.199994 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AK49" smd circle (at 15.999993 3.199994 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 609 "PETN9_GFXRN9"))
    (pad "AK51" smd circle (at 16.799992 3.199994 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 610 "PETP9_GFXRP9"))
    (pad "AL2" smd circle (at -16.399993 3.999992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 186 "DQD_6"))
    (pad "AL4" smd circle (at -15.599994 3.999992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AL6" smd circle (at -14.799996 3.999992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 183 "DQD_5"))
    (pad "AL9" smd circle (at -13.599998 3.999992 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AL10" smd circle (at -12.8 3.999992 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 169 "DQD_23"))
    (pad "AL11" smd circle (at -12.000001 3.999992 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 197 "DQD_22"))
    (pad "AL12" smd circle (at -11.200003 3.999992 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AL13" smd circle (at -10.400005 3.999992 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "AL14" smd circle (at -9.600006 3.999992 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 95 "MAD_3"))
    (pad "AL15" smd circle (at -8.800008 3.999992 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AL16" smd circle (at -8.000009 3.999992 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AL19" smd circle (at -6.000013 3.999992 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AL20" smd circle (at -5.000015 3.999992 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AL21" smd circle (at -3.999992 3.999992 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AL22" smd circle (at -2.999994 3.999992 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AL24" smd circle (at -1.999996 3.999992 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AL25" smd circle (at -0.999998 3.999992 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AL26" smd circle (at 0 3.999992 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AL27" smd circle (at 0.999998 3.999992 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AL28" smd circle (at 1.999996 3.999992 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AL30" smd circle (at 2.999994 3.999992 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AL31" smd circle (at 3.999992 3.999992 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AL32" smd circle (at 4.99999 3.999992 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AL33" smd circle (at 5.999988 3.999992 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AL36" smd circle (at 7.999984 4.399991 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 716 "+PCIE_VDDC"))
    (pad "AL37" smd circle (at 8.800008 4.399991 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 716 "+PCIE_VDDC"))
    (pad "AL38" smd circle (at 9.600006 4.399991 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AL39" smd circle (at 10.400005 4.399991 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 635 "GFXTN8_PERN8"))
    (pad "AL40" smd circle (at 11.200003 4.399991 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 777 "GFXTP8_PERP8"))
    (pad "AL41" smd circle (at 12.000001 4.399991 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AL42" smd circle (at 12.8 4.399991 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 636 "GFXTN9_PERN9"))
    (pad "AL43" smd circle (at 13.599998 4.399991 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 742 "GFXTP9_PERP9"))
    (pad "AL46" smd circle (at 14.799996 3.999992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 607 "PETN8_GFXRN8"))
    (pad "AL48" smd circle (at 15.599994 3.999992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 608 "PETP8_GFXRP8"))
    (pad "AL50" smd circle (at 16.399993 3.999992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AM1" smd circle (at -16.799992 4.79999 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 193 "DQD_9"))
    (pad "AM3" smd circle (at -15.999993 4.79999 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 192 "DQD_8"))
    (pad "AM5" smd circle (at -15.199995 4.79999 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 184 "DQD_7"))
    (pad "AM7" smd circle (at -14.399997 4.79999 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AM9" smd circle (at -13.599998 5.19999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 196 "DQD_21"))
    (pad "AM10" smd circle (at -12.8 5.19999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 168 "DQD_20"))
    (pad "AM11" smd circle (at -12.000001 5.19999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 736 "GND_VSSRHD"))
    (pad "AM12" smd circle (at -11.200003 5.19999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 737 "+VDDRHD"))
    (pad "AM13" smd circle (at -10.400005 5.19999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 92 "MAD_2"))
    (pad "AM14" smd circle (at -9.600006 5.19999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 91 "MAD_1"))
    (pad "AM15" smd circle (at -8.800008 5.19999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 161 "CASD0B"))
    (pad "AM16" smd circle (at -8.000009 5.19999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 101 "CSD1B_0"))
    (pad "AM19" smd circle (at -6.000013 4.99999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AM20" smd circle (at -5.000015 4.99999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AM21" smd circle (at -3.999992 4.99999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AM22" smd circle (at -2.999994 4.99999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AM24" smd circle (at -1.999996 4.99999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AM25" smd circle (at -0.999998 4.99999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AM26" smd circle (at 0 4.99999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AM27" smd circle (at 0.999998 4.99999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AM28" smd circle (at 1.999996 4.99999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AM30" smd circle (at 2.999994 4.99999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AM31" smd circle (at 3.999992 4.99999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AM32" smd circle (at 4.99999 4.99999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AM33" smd circle (at 5.999988 4.99999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AM45" smd circle (at 14.399997 4.79999 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AM47" smd circle (at 15.199995 4.79999 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AM49" smd circle (at 15.999993 4.79999 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 605 "PETN7_GFXRN7"))
    (pad "AM51" smd circle (at 16.799992 4.79999 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 606 "PETP7_GFXRP7"))
    (pad "AN2" smd circle (at -16.399993 5.599989 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AN4" smd circle (at -15.599994 5.599989 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 195 "DQD_11"))
    (pad "AN6" smd circle (at -14.799996 5.599989 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 194 "DQD_10"))
    (pad "AN19" smd circle (at -6.000013 5.999988 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AN20" smd circle (at -5.000015 5.999988 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AN21" smd circle (at -3.999992 5.999988 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AN22" smd circle (at -2.999994 5.999988 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AN24" smd circle (at -1.999996 5.999988 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AN25" smd circle (at -0.999998 5.999988 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AN26" smd circle (at 0 5.999988 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AN27" smd circle (at 0.999998 5.999988 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AN28" smd circle (at 1.999996 5.999988 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AN30" smd circle (at 2.999994 5.999988 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AN31" smd circle (at 3.999992 5.999988 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AN32" smd circle (at 4.99999 5.999988 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AN33" smd circle (at 5.999988 5.999988 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "AN36" smd circle (at 7.999984 5.599989 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 716 "+PCIE_VDDC"))
    (pad "AN37" smd circle (at 8.800008 5.599989 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 769 "N16984571"))
    (pad "AN38" smd circle (at 9.600006 5.599989 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AN39" smd circle (at 10.400005 5.599989 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 633 "GFXTN6_PERN6"))
    (pad "AN40" smd circle (at 11.200003 5.599989 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 770 "GFXTP6_PERP6"))
    (pad "AN41" smd circle (at 12.000001 5.599989 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AN42" smd circle (at 12.8 5.599989 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 634 "GFXTN7_PERN7"))
    (pad "AN43" smd circle (at 13.599998 5.599989 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 757 "GFXTP7_PERP7"))
    (pad "AN46" smd circle (at 14.799996 5.599989 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 603 "PETN6_GFXRN6"))
    (pad "AN48" smd circle (at 15.599994 5.599989 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 604 "PETP6_GFXRP6"))
    (pad "AN50" smd circle (at 16.399993 5.599989 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AP1" smd circle (at -16.799992 6.399987 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 198 "QSD_1"))
    (pad "AP3" smd circle (at -15.999993 6.399987 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 206 "QSDB_1"))
    (pad "AP5" smd circle (at -15.199995 6.399987 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 162 "DQMDB_1"))
    (pad "AP7" smd circle (at -14.399997 6.399987 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "AP9" smd circle (at -13.599998 6.399987 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 160 "CLKD0B"))
    (pad "AP10" smd circle (at -12.8 6.399987 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 157 "CLKD0"))
    (pad "AP11" smd circle (at -12.000001 6.399987 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AP12" smd circle (at -11.200003 6.399987 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "AP13" smd circle (at -10.400005 6.399987 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 210 "CKED0"))
    (pad "AP14" smd circle (at -9.600006 6.399987 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AP15" smd circle (at -8.800008 6.399987 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AP16" smd circle (at -8.000009 6.399987 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AP36" smd circle (at 7.999984 6.799986 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 74 "PERST#_BUF"))
    (pad "AP37" smd circle (at 8.800008 6.799986 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 771 "N16984567"))
    (pad "AP38" smd circle (at 9.600006 6.799986 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AP39" smd circle (at 10.400005 6.799986 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 646 "GFXTN4_PERN4"))
    (pad "AP40" smd circle (at 11.200003 6.799986 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 772 "GFXTP4_PERP4"))
    (pad "AP41" smd circle (at 12.000001 6.799986 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AP42" smd circle (at 12.8 6.799986 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 647 "GFXTN5_PERN5"))
    (pad "AP43" smd circle (at 13.599998 6.799986 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 746 "GFXTP5_PERP5"))
    (pad "AP45" smd circle (at 14.399997 6.399987 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AP47" smd circle (at 15.199995 6.399987 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AP49" smd circle (at 15.999993 6.399987 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 629 "PETN5_GFXRN5"))
    (pad "AP51" smd circle (at 16.799992 6.399987 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 630 "PETP5_GFXRP5"))
    (pad "AR2" smd circle (at -16.399993 7.200011 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 166 "DQD_13"))
    (pad "AR4" smd circle (at -15.599994 7.200011 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AR6" smd circle (at -14.799996 7.200011 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 167 "DQD_12"))
    (pad "AR16" smd circle (at -8.000009 7.50001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 145 "MAD_BA2"))
    (pad "AR46" smd circle (at 14.799996 7.200011 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 627 "PETN4_GFXRN4"))
    (pad "AR48" smd circle (at 15.599994 7.200011 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 628 "PETP4_GFXRP4"))
    (pad "AR50" smd circle (at 16.399993 7.200011 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AT1" smd circle (at -16.799992 8.000009 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 176 "DQD_24"))
    (pad "AT3" smd circle (at -15.999993 8.000009 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 178 "DQD_15"))
    (pad "AT5" smd circle (at -15.199995 8.000009 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 189 "DQD_14"))
    (pad "AT7" smd circle (at -14.399997 8.000009 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AT9" smd circle (at -13.599998 7.60001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 102 "CLKD1B"))
    (pad "AT10" smd circle (at -12.8 7.60001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 99 "CLKD1"))
    (pad "AT11" smd circle (at -12.000001 7.60001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 136 "DQD_41"))
    (pad "AT12" smd circle (at -11.200003 7.60001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 156 "RASD0B"))
    (pad "AT13" smd circle (at -10.400005 7.60001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AT14" smd circle (at -9.600006 7.60001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AT15" smd circle (at -8.800008 7.60001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "AT17" smd circle (at -7.300011 8.000009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 96 "MAD_BA1"))
    (pad "AT18" smd circle (at -6.200013 8.000009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AT20" smd circle (at -5.000015 8.000009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 821 "VREFG"))
    (pad "AT21" smd circle (at -3.799992 8.000009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 824 "TS_FDO"))
    (pad "AT23" smd circle (at -2.599995 8.000009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AT24" smd circle (at -1.399997 8.000009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AT26" smd circle (at -0.2 8.000009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "+3.3V"))
    (pad "AT27" smd circle (at 0.999998 8.000009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "+3.3V"))
    (pad "AT29" smd circle (at 2.199996 8.000009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "+3.3V"))
    (pad "AT30" smd circle (at 3.399993 8.000009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "+3.3V"))
    (pad "AT32" smd circle (at 4.599991 8.000009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 756 "DDC3CLK"))
    (pad "AT33" smd circle (at 5.799988 8.000009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AT35" smd circle (at 6.999986 8.000009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AT37" smd circle (at 8.800008 8.000009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 773 "TEST_EN"))
    (pad "AT38" smd circle (at 9.600006 8.000009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AT39" smd circle (at 10.400005 8.000009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 644 "GFXTN2_PERN2"))
    (pad "AT40" smd circle (at 11.200003 8.000009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 774 "GFXTP2_PERP2"))
    (pad "AT41" smd circle (at 12.000001 8.000009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AT42" smd circle (at 12.8 8.000009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 645 "GFXTN3_PERN3"))
    (pad "AT43" smd circle (at 13.599998 8.000009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 744 "GFXTP3_PERP3"))
    (pad "AT45" smd circle (at 14.399997 8.000009 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AT47" smd circle (at 15.199995 8.000009 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AT49" smd circle (at 15.999993 8.000009 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 625 "PETN3_GFXRN3"))
    (pad "AT51" smd circle (at 16.799992 8.000009 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 626 "PETP3_GFXRP3"))
    (pad "AU2" smd circle (at -16.399993 8.800008 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AU4" smd circle (at -15.599994 8.800008 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 174 "DQD_31"))
    (pad "AU6" smd circle (at -14.799996 8.800008 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 177 "DQD_25"))
    (pad "AU9" smd circle (at -13.599998 8.800008 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 137 "DQD_40"))
    (pad "AU10" smd circle (at -12.8 8.800008 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AU11" smd circle (at -12.000001 8.800008 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "AU12" smd circle (at -11.200003 8.800008 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 100 "WED1B"))
    (pad "AU13" smd circle (at -10.400005 8.800008 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AU14" smd circle (at -9.600006 8.800008 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 97 "MAD_BA0"))
    (pad "AU15" smd circle (at -8.600008 8.800008 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 86 "MAD_8"))
    (pad "AU17" smd circle (at -7.400011 8.800008 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AU18" smd circle (at -6.200013 8.800008 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 788 "GPIO_1"))
    (pad "AU20" smd circle (at -5.000015 8.800008 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 826 "GPIO_7"))
    (pad "AU21" smd circle (at -3.799992 8.800008 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 822 "GPIO_10"))
    (pad "AU23" smd circle (at -2.599995 8.800008 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AU24" smd circle (at -1.399997 8.800008 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 807 "JTAG_MODE"))
    (pad "AU26" smd circle (at -0.2 8.800008 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AU27" smd circle (at 0.999998 8.800008 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AU29" smd circle (at 2.199996 8.800008 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AU30" smd circle (at 3.399993 8.800008 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AU32" smd circle (at 4.599991 8.800008 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 675 "DDC3DATA"))
    (pad "AU33" smd circle (at 5.799988 8.800008 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AU35" smd circle (at 6.999986 8.800008 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AU36" smd circle (at 8.199984 8.800008 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 708 "PLL_TEST"))
    (pad "AU38" smd circle (at 9.600006 9.000007 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AU39" smd circle (at 10.400005 9.000007 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 640 "GFXTN0_PERN0"))
    (pad "AU40" smd circle (at 11.200003 9.000007 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 641 "GFXTP0_PERP0"))
    (pad "AU41" smd circle (at 12.000001 9.000007 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AU42" smd circle (at 12.8 9.000007 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 642 "GFXTN1_PERN1"))
    (pad "AU43" smd circle (at 13.599998 9.000007 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 643 "GFXTP1_PERP1"))
    (pad "AU46" smd circle (at 14.799996 8.800008 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 623 "PETN2_GFXRN2"))
    (pad "AU48" smd circle (at 15.599994 8.800008 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 624 "PETP2_GFXRP2"))
    (pad "AU50" smd circle (at 16.399993 8.800008 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AV1" smd circle (at -16.799992 9.600006 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 208 "QSDB_3"))
    (pad "AV3" smd circle (at -15.999993 9.600006 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 164 "DQMDB_3"))
    (pad "AV5" smd circle (at -15.199995 9.600006 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 175 "DQD_30"))
    (pad "AV7" smd circle (at -14.399997 9.600006 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "AV9" smd circle (at -13.599998 9.800006 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 135 "DQD_42"))
    (pad "AV10" smd circle (at -12.8 9.800006 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 134 "DQD_43"))
    (pad "AV11" smd circle (at -12.000001 9.800006 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 150 "QSDB_5"))
    (pad "AV12" smd circle (at -11.200003 9.800006 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AV13" smd circle (at -10.400005 9.800006 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AV14" smd circle (at -9.600006 9.600006 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 93 "MAD_11"))
    (pad "AV15" smd circle (at -8.600008 9.600006 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AV17" smd circle (at -7.400011 9.600006 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 94 "MAD_10"))
    (pad "AV18" smd circle (at -6.200013 9.600006 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 785 "GPIO_0"))
    (pad "AV20" smd circle (at -5.000015 9.600006 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 827 "GPIO_2"))
    (pad "AV21" smd circle (at -3.799992 9.600006 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 784 "GPIO_9"))
    (pad "AV23" smd circle (at -2.599995 9.600006 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 818 "HPD2"))
    (pad "AV24" smd circle (at -1.399997 9.600006 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 806 "PCIE_CLK_REQB"))
    (pad "AV26" smd circle (at -0.2 9.600006 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AV27" smd circle (at 0.999998 9.600006 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AV29" smd circle (at 2.199996 9.600006 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AV30" smd circle (at 3.399993 9.600006 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 779 "N74256579"))
    (pad "AV32" smd circle (at 4.599991 9.600006 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AV33" smd circle (at 5.799988 9.600006 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 650 "VID_3"))
    (pad "AV35" smd circle (at 6.999986 9.600006 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 649 "DDC4DATA"))
    (pad "AV36" smd circle (at 8.199984 9.600006 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 711 "DDC2DATA"))
    (pad "AV45" smd circle (at 14.399997 9.600006 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AV47" smd circle (at 15.199995 9.600006 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AV49" smd circle (at 15.999993 9.600006 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 621 "PETN1_GFXRN1"))
    (pad "AV51" smd circle (at 16.799992 9.600006 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 622 "PETP1_GFXRP1"))
    (pad "AW2" smd circle (at -16.399993 10.400005 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 179 "DQD_28"))
    (pad "AW4" smd circle (at -15.599994 10.400005 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AW6" smd circle (at -14.799996 10.400005 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 200 "QSD_3"))
    (pad "AW12" smd circle (at -11.200003 10.700004 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 109 "DQD_46"))
    (pad "AW14" smd circle (at -9.600006 10.400005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "AW15" smd circle (at -8.600008 10.400005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 89 "MAD_9"))
    (pad "AW17" smd circle (at -7.400011 10.400005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AW18" smd circle (at -6.200013 10.400005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 789 "GPIO_3"))
    (pad "AW20" smd circle (at -5.000015 10.400005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AW21" smd circle (at -3.799992 10.400005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 820 "GPIO_8"))
    (pad "AW23" smd circle (at -2.599995 10.400005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 823 "GPIO_13"))
    (pad "AW24" smd circle (at -1.399997 10.400005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 661 "GPIO_22_ROMCSB"))
    (pad "AW26" smd circle (at -0.2 10.400005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AW27" smd circle (at 0.999998 10.400005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AW29" smd circle (at 2.199996 10.400005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AW30" smd circle (at 3.399993 10.400005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AW32" smd circle (at 4.599991 10.400005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 659 "VID_6"))
    (pad "AW33" smd circle (at 5.799988 10.400005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 658 "VID_2"))
    (pad "AW35" smd circle (at 6.999986 10.400005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 709 "DDC4CLK"))
    (pad "AW36" smd circle (at 8.199984 10.400005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 715 "DDC2CLK"))
    (pad "AW37" smd circle (at 9.200007 10.400005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 654 "A_DAC2_COMP"))
    (pad "AW40" smd circle (at 11.200003 10.000005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 616 "+PCIE_VDDR"))
    (pad "AW41" smd circle (at 12.000001 10.000005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 616 "+PCIE_VDDR"))
    (pad "AW42" smd circle (at 12.8 10.000005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 639 "PCIE_REFCLKN"))
    (pad "AW43" smd circle (at 13.599998 10.000005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 741 "PCIE_REFCLKP"))
    (pad "AW46" smd circle (at 14.799996 10.400005 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 619 "PETN0_GFXRN0"))
    (pad "AW48" smd circle (at 15.599994 10.400005 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 620 "PETP0_GFXRP0"))
    (pad "AW50" smd circle (at 16.399993 10.400005 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AY1" smd circle (at -16.799992 11.200003 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 182 "DQD_26"))
    (pad "AY3" smd circle (at -15.999993 11.200003 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 180 "DQD_27"))
    (pad "AY5" smd circle (at -15.199995 11.200003 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 181 "DQD_29"))
    (pad "AY7" smd circle (at -14.399997 11.200003 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AY9" smd circle (at -13.599998 10.800004 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AY10" smd circle (at -12.8 10.800004 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 104 "DQMDB_5"))
    (pad "AY11" smd circle (at -12.000001 10.800004 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 140 "QSD_5"))
    (pad "AY13" smd circle (at -10.500004 11.200003 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 113 "DQD_61"))
    (pad "AY14" smd circle (at -9.600006 11.200003 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AY15" smd circle (at -8.600008 11.200003 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 98 "RASD1B"))
    (pad "AY17" smd circle (at -7.400011 11.200003 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AY18" smd circle (at -6.200013 11.200003 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 790 "GPIO_17_INT"))
    (pad "AY20" smd circle (at -5.000015 11.200003 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 828 "DVPDATA_22"))
    (pad "AY21" smd circle (at -3.799992 11.200003 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 819 "DVPDATA_12"))
    (pad "AY23" smd circle (at -2.599995 11.200003 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 778 "GPIO_12"))
    (pad "AY24" smd circle (at -1.399997 11.200003 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 664 "GPIO_6"))
    (pad "AY26" smd circle (at -0.2 11.200003 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AY27" smd circle (at 0.999998 11.200003 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AY29" smd circle (at 2.199996 11.200003 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 792 "PSYNC"))
    (pad "AY30" smd circle (at 3.399993 11.200003 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AY32" smd circle (at 4.599991 11.200003 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 660 "VID_5"))
    (pad "AY33" smd circle (at 5.799988 11.200003 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 657 "VID_1"))
    (pad "AY35" smd circle (at 6.999986 11.200003 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AY36" smd circle (at 8.199984 11.200003 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "VSYNC2"))
    (pad "AY37" smd circle (at 9.200007 11.200003 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 651 "A_DAC2_Y"))
    (pad "AY39" smd circle (at 10.200005 11.200003 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 652 "A_DAC2_RB"))
    (pad "AY41" smd circle (at 12.000001 11.000003 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 616 "+PCIE_VDDR"))
    (pad "AY42" smd circle (at 12.8 11.000003 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 616 "+PCIE_VDDR"))
    (pad "AY43" smd circle (at 13.599998 11.000003 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 616 "+PCIE_VDDR"))
    (pad "AY45" smd circle (at 14.399997 11.200003 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 616 "+PCIE_VDDR"))
    (pad "AY47" smd circle (at 15.199995 11.200003 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 616 "+PCIE_VDDR"))
    (pad "AY49" smd circle (at 15.999993 11.200003 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "AY51" smd circle (at 16.799992 11.200003 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 618 "+PCIE_PVDD"))
    (pad "B11" smd circle (at -12.000001 -16.399993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 328 "QSC_0"))
    (pad "B13" smd circle (at -10.400005 -16.399993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "B15" smd circle (at -8.800008 -16.399993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 406 "QSBB_6"))
    (pad "B17" smd circle (at -7.200011 -16.399993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "B19" smd circle (at -5.600014 -16.399993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 398 "QSB_4"))
    (pad "B21" smd circle (at -3.999992 -16.399993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "B23" smd circle (at -2.399995 -16.399993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 433 "DQB_31"))
    (pad "B25" smd circle (at -0.799998 -16.399993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "B27" smd circle (at 0.799998 -16.399993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 420 "DQB_20"))
    (pad "B29" smd circle (at 2.399995 -16.399993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "B31" smd circle (at 3.999992 -16.399993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 440 "DQB_6"))
    (pad "B33" smd circle (at 5.599989 -16.399993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "B35" smd circle (at 7.199986 -16.399993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 506 "DQA_61"))
    (pad "B37" smd circle (at 8.800008 -16.399993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "B39" smd circle (at 10.400005 -16.399993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 500 "DQA_56"))
    (pad "B41" smd circle (at 12.000001 -16.399993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "BA2" smd circle (at -16.399993 12.000001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "BA4" smd circle (at -15.599994 12.000001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 130 "DQD_34"))
    (pad "BA6" smd circle (at -14.799996 12.000001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 133 "DQD_32"))
    (pad "BA9" smd circle (at -13.599998 11.800002 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 108 "DQD_45"))
    (pad "BA10" smd circle (at -12.8 11.800002 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "BA11" smd circle (at -11.600002 12.000001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "BA13" smd circle (at -10.600004 12.000001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 151 "QSDB_7"))
    (pad "BA14" smd circle (at -9.600006 12.000001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 154 "CKED1"))
    (pad "BA15" smd circle (at -8.600008 12.000001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 103 "CASD1B"))
    (pad "BA17" smd circle (at -7.400011 12.000001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "BA18" smd circle (at -6.200013 12.000001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 787 "GPIO_5"))
    (pad "BA20" smd circle (at -5.000015 12.000001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 780 "DVPDATA_23"))
    (pad "BA21" smd circle (at -3.799992 12.000001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 825 "DVPDATA_13"))
    (pad "BA23" smd circle (at -2.599995 12.000001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 798 "GPIO_11"))
    (pad "BA24" smd circle (at -1.399997 12.000001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "BA26" smd circle (at -0.2 12.000001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "BA27" smd circle (at 0.999998 12.000001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "BA29" smd circle (at 2.199996 12.000001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "BA30" smd circle (at 3.399993 12.000001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 710 "VID_7"))
    (pad "BA32" smd circle (at 4.599991 12.000001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 665 "VID_4"))
    (pad "BA33" smd circle (at 5.799988 12.000001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 707 "VID_0"))
    (pad "BA35" smd circle (at 6.999986 12.000001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 667 "+DPLL_PVDD"))
    (pad "BA36" smd circle (at 8.199984 12.000001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "HSYNC2"))
    (pad "BA37" smd circle (at 9.200007 12.000001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 668 "A_DAC2_C"))
    (pad "BA39" smd circle (at 10.200005 12.000001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "A_DAC2_R"))
    (pad "BA40" smd circle (at 11.200003 12.000001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 662 "R2SET"))
    (pad "BA42" smd circle (at 12.8 12.000001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "HSYNC1"))
    (pad "BA43" smd circle (at 13.599998 12.000001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "VSYNC1"))
    (pad "BA46" smd circle (at 14.799996 12.000001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 616 "+PCIE_VDDR"))
    (pad "BA48" smd circle (at 15.599994 12.000001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 617 "GND_VSS1DI"))
    (pad "BA50" smd circle (at 16.399993 12.000001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 764 "+VDD1DI"))
    (pad "BB1" smd circle (at -16.799992 12.8 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 107 "DQMDB_4"))
    (pad "BB3" smd circle (at -15.999993 12.8 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 129 "DQD_35"))
    (pad "BB5" smd circle (at -15.199995 12.8 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 132 "DQD_33"))
    (pad "BB7" smd circle (at -14.399997 12.8 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 153 "QSDB_4"))
    (pad "BB9" smd circle (at -13.599998 12.6 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 131 "DQD_47"))
    (pad "BB10" smd circle (at -12.6 12.8 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 120 "DQD_44"))
    (pad "BB11" smd circle (at -11.600002 12.8 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 105 "DQMDB_7"))
    (pad "BB13" smd circle (at -10.600004 12.8 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 141 "QSD_7"))
    (pad "BB14" smd circle (at -9.600006 12.8 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 114 "DQD_56"))
    (pad "BB15" smd circle (at -8.600008 12.8 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 138 "DQD_57"))
    (pad "BB17" smd circle (at -7.400011 12.8 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 791 "GPIO_4"))
    (pad "BB18" smd circle (at -6.200013 12.8 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 786 "DVPDATA_15"))
    (pad "BB20" smd circle (at -5.000015 12.8 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 817 "DVP_MVP_CNTL_0"))
    (pad "BB21" smd circle (at -3.799992 12.8 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "BB23" smd circle (at -2.599995 12.8 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 800 "GENERICB"))
    (pad "BB24" smd circle (at -1.399997 12.8 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "BB26" smd circle (at -0.2 12.8 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 671 "GENERICC"))
    (pad "BB27" smd circle (at 0.999998 12.8 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 76 "GPU_DPLUS"))
    (pad "BB29" smd circle (at 2.199996 12.8 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 751 "HPD1"))
    (pad "BB30" smd circle (at 3.399993 12.8 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "BB32" smd circle (at 4.599991 12.8 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "BB33" smd circle (at 5.799988 12.8 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "BB35" smd circle (at 6.999986 12.8 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 673 "GND_PVSS"))
    (pad "BB36" smd circle (at 8.199984 12.8 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 693 "GND_VSS2DI"))
    (pad "BB37" smd circle (at 9.200007 12.8 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 705 "A_DAC2_BB"))
    (pad "BB39" smd circle (at 10.200005 12.8 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 706 "A_DAC2_GB"))
    (pad "BB40" smd circle (at 11.200003 12.8 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "BB41" smd circle (at 12.200001 12.8 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 767 "GND_A2VSSQ"))
    (pad "BB43" smd circle (at 13.599998 12.999999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 768 "RSET"))
    (pad "BB45" smd circle (at 14.399997 12.8 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 766 "DDC1DATA"))
    (pad "BB47" smd circle (at 15.199995 12.8 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 765 "DDC1CLK"))
    (pad "BB49" smd circle (at 15.999993 12.8 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 47 "A_DAC1_R"))
    (pad "BB51" smd circle (at 16.799992 12.8 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 615 "A_DAC1_RB"))
    (pad "BC9" smd circle (at -13.399999 13.399999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 116 "DQD_48"))
    (pad "BC10" smd circle (at -12.6 13.599998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 115 "DQD_59"))
    (pad "BC11" smd circle (at -11.600002 13.599998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 139 "DQD_60"))
    (pad "BC13" smd circle (at -10.600004 13.599998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 111 "DQD_62"))
    (pad "BC14" smd circle (at -9.600006 13.599998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "BC15" smd circle (at -8.600008 13.599998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 110 "DQD_58"))
    (pad "BC17" smd circle (at -7.400011 13.599998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 750 "DVPDATA_17"))
    (pad "BC18" smd circle (at -6.200013 13.599998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 829 "DVPDATA_16"))
    (pad "BC20" smd circle (at -5.000015 13.599998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 816 "DVP_MVP_CNTL_1"))
    (pad "BC21" smd circle (at -3.799992 13.599998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 752 "DVPDATA_14"))
    (pad "BC23" smd circle (at -2.599995 13.599998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 753 "DVALID"))
    (pad "BC24" smd circle (at -1.399997 13.599998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "BC26" smd circle (at -0.2 13.599998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 754 "GENERICA"))
    (pad "BC27" smd circle (at 0.999998 13.599998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 77 "GPU_DMINUS"))
    (pad "BC29" smd circle (at 2.199996 13.599998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "BC30" smd circle (at 3.399993 13.599998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "BC32" smd circle (at 4.599991 13.599998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "BC33" smd circle (at 5.799988 13.599998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "BC35" smd circle (at 6.999986 13.599998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 674 "+DPLL_VDDC"))
    (pad "BC36" smd circle (at 8.199984 13.599998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 694 "+VDD2DI"))
    (pad "BC37" smd circle (at 9.200007 13.599998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "A_DAC2_B"))
    (pad "BC39" smd circle (at 10.200005 13.599998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "A_DAC2_G"))
    (pad "BC40" smd circle (at 11.200003 13.599998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "BC41" smd circle (at 12.200001 13.599998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 676 "+A2VDD"))
    (pad "BC42" smd circle (at 12.999999 13.599998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 781 "+A2VDDQ"))
    (pad "BD1" smd circle (at -16.399993 13.624992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 127 "DQD_36"))
    (pad "BD3" smd circle (at -15.599994 13.624992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 125 "DQD_37"))
    (pad "BD6" smd circle (at -14.799996 13.624992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 143 "QSD_4"))
    (pad "BD8" smd circle (at -13.975004 13.975004 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "BD44" smd circle (at 13.975004 13.975004 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 631 "GND_AVSSQ"))
    (pad "BD46" smd circle (at 14.799996 13.624992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 632 "+AVDD"))
    (pad "BD49" smd circle (at 15.599994 13.624992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "A_DAC1_G"))
    (pad "BD51" smd circle (at 16.399993 13.624992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 648 "A_DAC1_GB"))
    (pad "BE10" smd circle (at -12.8 14.399997 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "BE12" smd circle (at -11.200003 14.399997 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 112 "DQD_63"))
    (pad "BE14" smd circle (at -9.600006 14.399997 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "BE16" smd circle (at -8.000009 14.399997 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "BE18" smd circle (at -6.400013 14.399997 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "BE20" smd circle (at -4.800016 14.399997 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "BE22" smd circle (at -3.199994 14.399997 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 680 "+VDDR_DVP"))
    (pad "BE24" smd circle (at -1.599997 14.399997 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "BE26" smd circle (at 0 14.399997 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 682 "+TXVDDR"))
    (pad "BE28" smd circle (at 1.599997 14.399997 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "BE30" smd circle (at 3.199994 14.399997 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "BE32" smd circle (at 4.79999 14.399997 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "BE34" smd circle (at 6.399987 14.399997 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "BE36" smd circle (at 7.999984 14.399997 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "BE38" smd circle (at 9.600006 14.399997 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 655 "+T2PVDD"))
    (pad "BE40" smd circle (at 11.200003 14.399997 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 677 "GND_T2PVSS"))
    (pad "BE42" smd circle (at 12.8 14.399997 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "BF1" smd circle (at -16.799992 14.499996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "BF3" smd circle (at -15.850006 14.499996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 128 "DQD_38"))
    (pad "BF6" smd circle (at -14.699996 14.699996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 118 "DQD_49"))
    (pad "BF8" smd circle (at -13.624992 14.799996 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 152 "QSDB_6"))
    (pad "BF11" smd circle (at -12.000001 14.799996 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 144 "DRAM_RST"))
    (pad "BF13" smd circle (at -10.400005 14.799996 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "BF15" smd circle (at -8.800008 14.799996 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 811 "DVOCLK"))
    (pad "BF17" smd circle (at -7.200011 14.799996 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 802 "DVPDATA_5"))
    (pad "BF19" smd circle (at -5.600014 14.799996 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 810 "DVPDATA_11"))
    (pad "BF21" smd circle (at -3.999992 14.799996 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 799 "DVPDATA_20"))
    (pad "BF23" smd circle (at -2.399995 14.799996 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 680 "+VDDR_DVP"))
    (pad "BF25" smd circle (at -0.799998 14.799996 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 682 "+TXVDDR"))
    (pad "BF27" smd circle (at 0.799998 14.799996 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 684 "T1X0P"))
    (pad "BF29" smd circle (at 2.399995 14.799996 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 688 "T1X2P"))
    (pad "BF31" smd circle (at 3.999992 14.799996 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 670 "T1X3P"))
    (pad "BF33" smd circle (at 5.599989 14.799996 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 695 "T1X5P"))
    (pad "BF35" smd circle (at 7.199986 14.799996 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 697 "T2XCP"))
    (pad "BF37" smd circle (at 8.800008 14.799996 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 701 "T2X1P"))
    (pad "BF39" smd circle (at 10.400005 14.799996 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 656 "T2X3P"))
    (pad "BF41" smd circle (at 12.000001 14.799996 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 712 "T2X4P"))
    (pad "BF44" smd circle (at 13.624992 14.799996 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "BF46" smd circle (at 14.699996 14.699996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "XTALOUT"))
    (pad "BF49" smd circle (at 15.850006 14.499996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "A_DAC1_B"))
    (pad "BF51" smd circle (at 16.799992 14.499996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 602 "A_DAC1_BB"))
    (pad "BG10" smd circle (at -12.8 15.199995 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 121 "DQD_52"))
    (pad "BG12" smd circle (at -11.200003 15.199995 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "BG14" smd circle (at -9.600006 15.199995 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 795 "+VDD_CT"))
    (pad "BG16" smd circle (at -8.000009 15.199995 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 814 "DVPDATA_1"))
    (pad "BG18" smd circle (at -6.400013 15.199995 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 803 "DVPDATA_8"))
    (pad "BG20" smd circle (at -4.800016 15.199995 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 794 "DVPCNTL_1"))
    (pad "BG22" smd circle (at -3.199994 15.199995 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 680 "+VDDR_DVP"))
    (pad "BG24" smd circle (at -1.599997 15.199995 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "BG26" smd circle (at 0 15.199995 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "BG28" smd circle (at 1.599997 15.199995 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "BG30" smd circle (at 3.199994 15.199995 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "BG32" smd circle (at 4.79999 15.199995 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "BG34" smd circle (at 6.399987 15.199995 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 669 "+T2XVDD"))
    (pad "BG36" smd circle (at 7.999984 15.199995 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "BG38" smd circle (at 9.600006 15.199995 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "BG40" smd circle (at 11.200003 15.199995 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "BG42" smd circle (at 12.8 15.199995 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "BH11" smd circle (at -12.000001 15.599994 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 124 "DQD_55"))
    (pad "BH13" smd circle (at -10.400005 15.599994 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "BH15" smd circle (at -8.800008 15.599994 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 813 "DVPDATA_0"))
    (pad "BH17" smd circle (at -7.200011 15.599994 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 812 "DVPDATA_4"))
    (pad "BH19" smd circle (at -5.600014 15.599994 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 797 "DVPDATA_10"))
    (pad "BH21" smd circle (at -3.999992 15.599994 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 801 "DVPDATA_19"))
    (pad "BH23" smd circle (at -2.399995 15.599994 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 680 "+VDDR_DVP"))
    (pad "BH25" smd circle (at -0.799998 15.599994 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 682 "+TXVDDR"))
    (pad "BH27" smd circle (at 0.799998 15.599994 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 683 "T1X0M"))
    (pad "BH29" smd circle (at 2.399995 15.599994 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 687 "T1X2M"))
    (pad "BH31" smd circle (at 3.999992 15.599994 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 666 "T1X3M"))
    (pad "BH33" smd circle (at 5.599989 15.599994 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 696 "T1X5M"))
    (pad "BH35" smd circle (at 7.199986 15.599994 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 698 "T2XCM"))
    (pad "BH37" smd circle (at 8.800008 15.599994 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 702 "T2X1M"))
    (pad "BH39" smd circle (at 10.400005 15.599994 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 653 "T2X3M"))
    (pad "BH41" smd circle (at 12.000001 15.599994 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 663 "T2X4M"))
    (pad "BJ1" smd circle (at -16.299993 15.299995 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 126 "DQD_39"))
    (pad "BJ3" smd circle (at -15.399995 15.399995 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 119 "DQD_50"))
    (pad "BJ6" smd circle (at -14.499996 15.850006 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 117 "DQD_51"))
    (pad "BJ8" smd circle (at -13.624992 15.599994 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "BJ10" smd circle (at -12.8 15.999993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 122 "DQD_54"))
    (pad "BJ12" smd circle (at -11.200003 15.999993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 793 "N52040509"))
    (pad "BJ14" smd circle (at -9.600006 15.999993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 795 "+VDD_CT"))
    (pad "BJ16" smd circle (at -8.000009 15.999993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 815 "DVPDATA_2"))
    (pad "BJ18" smd circle (at -6.400013 15.999993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 804 "DVPDATA_7"))
    (pad "BJ20" smd circle (at -4.800016 15.999993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 808 "DVPCNTL_0"))
    (pad "BJ22" smd circle (at -3.199994 15.999993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 680 "+VDDR_DVP"))
    (pad "BJ24" smd circle (at -1.599997 15.999993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 690 "GND_TPVSS"))
    (pad "BJ26" smd circle (at 0 15.999993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 679 "T1XCP"))
    (pad "BJ28" smd circle (at 1.599997 15.999993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 686 "T1X1P"))
    (pad "BJ30" smd circle (at 3.199994 15.999993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "BJ32" smd circle (at 4.79999 15.999993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 691 "T1X4P"))
    (pad "BJ34" smd circle (at 6.399987 15.999993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 669 "+T2XVDD"))
    (pad "BJ36" smd circle (at 7.999984 15.999993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 699 "T2X0P"))
    (pad "BJ38" smd circle (at 9.600006 15.999993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 703 "T2X2P"))
    (pad "BJ40" smd circle (at 11.200003 15.999993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "BJ42" smd circle (at 12.8 15.999993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 714 "T2X5P"))
    (pad "BJ44" smd circle (at 13.624992 15.599994 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "BJ46" smd circle (at 14.499996 15.850006 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "BJ49" smd circle (at 15.399995 15.399995 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "XTALIN"))
    (pad "BJ51" smd circle (at 16.299993 15.299995 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "BK11" smd circle (at -12.000001 16.399993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "BK13" smd circle (at -10.400005 16.399993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "BK15" smd circle (at -8.800008 16.399993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 783 "DVPCNTL_2"))
    (pad "BK17" smd circle (at -7.200011 16.399993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "BK19" smd circle (at -5.600014 16.399993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 782 "DVPDATA_9"))
    (pad "BK21" smd circle (at -3.999992 16.399993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 672 "DVPDATA_18"))
    (pad "BK23" smd circle (at -2.399995 16.399993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 680 "+VDDR_DVP"))
    (pad "BK25" smd circle (at -0.799998 16.399993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 682 "+TXVDDR"))
    (pad "BK27" smd circle (at 0.799998 16.399993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "BK29" smd circle (at 2.399995 16.399993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "BK31" smd circle (at 3.999992 16.399993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "BK33" smd circle (at 5.599989 16.399993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "BK35" smd circle (at 7.199986 16.399993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 669 "+T2XVDD"))
    (pad "BK37" smd circle (at 8.800008 16.399993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "BK39" smd circle (at 10.400005 16.399993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "BK41" smd circle (at 12.000001 16.399993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "BL3" smd circle (at -15.299995 16.299993 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "BL6" smd circle (at -14.499996 16.799992 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 142 "QSD_6"))
    (pad "BL8" smd circle (at -13.624992 16.399993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 106 "DQMDB_6"))
    (pad "BL10" smd circle (at -12.8 16.799992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 123 "DQD_53"))
    (pad "BL12" smd circle (at -11.200003 16.799992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 796 "N52040505"))
    (pad "BL14" smd circle (at -9.600006 16.799992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 795 "+VDD_CT"))
    (pad "BL16" smd circle (at -8.000009 16.799992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 805 "DVPDATA_3"))
    (pad "BL18" smd circle (at -6.400013 16.799992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 809 "DVPDATA_6"))
    (pad "BL20" smd circle (at -4.800016 16.799992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "BL22" smd circle (at -3.199994 16.799992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 681 "DVPDATA_21"))
    (pad "BL24" smd circle (at -1.599997 16.799992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 689 "+TPVDD"))
    (pad "BL26" smd circle (at 0 16.799992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 678 "T1XCM"))
    (pad "BL28" smd circle (at 1.599997 16.799992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 685 "T1X1M"))
    (pad "BL30" smd circle (at 3.199994 16.799992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "BL32" smd circle (at 4.79999 16.799992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 692 "T1X4M"))
    (pad "BL34" smd circle (at 6.399987 16.799992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 669 "+T2XVDD"))
    (pad "BL36" smd circle (at 7.999984 16.799992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 700 "T2X0M"))
    (pad "BL38" smd circle (at 9.600006 16.799992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 704 "T2X2M"))
    (pad "BL40" smd circle (at 11.200003 16.799992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "BL42" smd circle (at 12.8 16.799992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 713 "T2X5M"))
    (pad "BL44" smd circle (at 13.624992 16.399993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "BL46" smd circle (at 14.499996 16.799992 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "BL49" smd circle (at 15.299995 16.299993 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "C1" smd circle (at -16.299993 -15.299995 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "C3" smd circle (at -15.399995 -15.399995 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 289 "DQMCB_1"))
    (pad "C6" smd circle (at -14.499996 -15.850006 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 321 "DQC_9"))
    (pad "C8" smd circle (at -13.624992 -15.599994 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 322 "DQC_8"))
    (pad "C10" smd circle (at -12.8 -15.999993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 292 "DQMCB_0"))
    (pad "C12" smd circle (at -11.200003 -15.999993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 315 "DQC_1"))
    (pad "C14" smd circle (at -9.600006 -15.999993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 376 "DQB_54"))
    (pad "C16" smd circle (at -8.000009 -15.999993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 371 "DQB_50"))
    (pad "C18" smd circle (at -6.400013 -15.999993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 380 "DQB_37"))
    (pad "C20" smd circle (at -4.800016 -15.999993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 384 "DQB_35"))
    (pad "C22" smd circle (at -3.199994 -15.999993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 434 "DQB_30"))
    (pad "C24" smd circle (at -1.599997 -15.999993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 418 "DQMBB_3"))
    (pad "C26" smd circle (at 0 -15.999993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 421 "DQB_23"))
    (pad "C28" smd circle (at 1.599997 -15.999993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 460 "QSBB_2"))
    (pad "C30" smd circle (at 3.199994 -15.999993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 447 "DQB_16"))
    (pad "C32" smd circle (at 4.79999 -15.999993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 419 "DQMBB_0"))
    (pad "C34" smd circle (at 6.399987 -15.999993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 442 "DQB_1"))
    (pad "C36" smd circle (at 7.999984 -15.999993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 503 "DQA_60"))
    (pad "C38" smd circle (at 9.600006 -15.999993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 498 "DQA_57"))
    (pad "C40" smd circle (at 11.200003 -15.999993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 507 "DQA_53"))
    (pad "C42" smd circle (at 12.8 -15.999993 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 511 "DQA_50"))
    (pad "C44" smd circle (at 13.624992 -15.599994 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "C46" smd circle (at 14.499996 -15.850006 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 491 "DQA_39"))
    (pad "C49" smd circle (at 15.399995 -15.399995 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 490 "DQA_38"))
    (pad "C51" smd circle (at 16.299993 -15.299995 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 522 "QSA_4"))
    (pad "D11" smd circle (at -12.000001 -15.599994 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "D13" smd circle (at -10.400005 -15.599994 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 379 "DQB_55"))
    (pad "D15" smd circle (at -8.800008 -15.599994 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "D17" smd circle (at -7.200011 -15.599994 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 373 "DQB_48"))
    (pad "D19" smd circle (at -5.600014 -15.599994 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "D21" smd circle (at -3.999992 -15.599994 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 385 "DQB_33"))
    (pad "D23" smd circle (at -2.399995 -15.599994 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "D25" smd circle (at -0.799998 -15.599994 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 428 "DQB_26"))
    (pad "D27" smd circle (at 0.799998 -15.599994 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "D29" smd circle (at 2.399995 -15.599994 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 449 "DQB_19"))
    (pad "D31" smd circle (at 3.999992 -15.599994 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "D33" smd circle (at 5.599989 -15.599994 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 455 "QSB_0"))
    (pad "D35" smd circle (at 7.199986 -15.599994 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "D37" smd circle (at 8.800008 -15.599994 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 488 "DQMAB_7"))
    (pad "D39" smd circle (at 10.400005 -15.599994 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "D41" smd circle (at 12.000001 -15.599994 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 534 "QSAB_6"))
    (pad "E10" smd circle (at -12.8 -15.199995 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 336 "QSCB_0"))
    (pad "E12" smd circle (at -11.200003 -15.199995 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 318 "DQC_0"))
    (pad "E14" smd circle (at -9.600006 -15.199995 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 361 "DQMBB_6"))
    (pad "E16" smd circle (at -8.000009 -15.199995 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 374 "DQB_49"))
    (pad "E18" smd circle (at -6.400013 -15.199995 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 382 "DQB_38"))
    (pad "E20" smd circle (at -4.800016 -15.199995 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 387 "DQB_34"))
    (pad "E22" smd circle (at -3.199994 -15.199995 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 435 "DQB_29"))
    (pad "E24" smd circle (at -1.599997 -15.199995 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 429 "DQB_27"))
    (pad "E26" smd circle (at 0 -15.199995 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 443 "DQB_21"))
    (pad "E28" smd circle (at 1.599997 -15.199995 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 416 "DQMBB_2"))
    (pad "E30" smd circle (at 3.199994 -15.199995 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 438 "DQB_7"))
    (pad "E32" smd circle (at 4.79999 -15.199995 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 463 "QSBB_0"))
    (pad "E34" smd circle (at 6.399987 -15.199995 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 445 "DQB_0"))
    (pad "E36" smd circle (at 7.999984 -15.199995 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 524 "QSA_7"))
    (pad "E38" smd circle (at 9.600006 -15.199995 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 501 "DQA_59"))
    (pad "E40" smd circle (at 11.200003 -15.199995 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 509 "DQA_54"))
    (pad "E42" smd circle (at 12.8 -15.199995 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 514 "DQA_49"))
    (pad "F1" smd circle (at -16.799992 -14.499996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 316 "DQC_12"))
    (pad "F3" smd circle (at -15.850006 -14.499996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 325 "QSC_1"))
    (pad "F6" smd circle (at -14.699996 -14.699996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 319 "DQC_11"))
    (pad "F8" smd circle (at -13.624992 -14.799996 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 313 "DQC_7"))
    (pad "F11" smd circle (at -12.000001 -14.799996 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 314 "DQC_3"))
    (pad "F13" smd circle (at -10.400005 -14.799996 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 377 "DQB_52"))
    (pad "F15" smd circle (at -8.800008 -14.799996 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 397 "QSB_6"))
    (pad "F17" smd circle (at -7.200011 -14.799996 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 381 "DQB_39"))
    (pad "F19" smd circle (at -5.600014 -14.799996 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 407 "QSBB_4"))
    (pad "F21" smd circle (at -3.999992 -14.799996 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 388 "DQB_32"))
    (pad "F23" smd circle (at -2.399995 -14.799996 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 454 "QSB_3"))
    (pad "F25" smd circle (at -0.799998 -14.799996 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 431 "DQB_25"))
    (pad "F27" smd circle (at 0.799998 -14.799996 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 432 "DQB_22"))
    (pad "F29" smd circle (at 2.399995 -14.799996 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 448 "DQB_18"))
    (pad "F31" smd circle (at 3.999992 -14.799996 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 437 "DQB_5"))
    (pad "F33" smd circle (at 5.599989 -14.799996 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 441 "DQB_3"))
    (pad "F35" smd circle (at 7.199986 -14.799996 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 504 "DQA_62"))
    (pad "F37" smd circle (at 8.800008 -14.799996 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 533 "QSAB_7"))
    (pad "F39" smd circle (at 10.400005 -14.799996 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 508 "DQA_55"))
    (pad "F41" smd circle (at 12.000001 -14.799996 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 489 "DQMAB_6"))
    (pad "F44" smd circle (at 13.624992 -14.799996 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 515 "DQA_48"))
    (pad "F46" smd circle (at 14.699996 -14.699996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 531 "QSAB_4"))
    (pad "F49" smd circle (at 15.850006 -14.499996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 486 "DQMAB_4"))
    (pad "F51" smd circle (at 16.799992 -14.499996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "G10" smd circle (at -12.8 -14.399997 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 310 "DQC_5"))
    (pad "G12" smd circle (at -11.200003 -14.399997 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 759 "MVREFD_C"))
    (pad "G14" smd circle (at -9.600006 -14.399997 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "G16" smd circle (at -8.000009 -14.399997 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "G18" smd circle (at -6.400013 -14.399997 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "G20" smd circle (at -4.800016 -14.399997 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "G22" smd circle (at -3.199994 -14.399997 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "G24" smd circle (at -1.599997 -14.399997 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "G26" smd circle (at 0 -14.399997 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "G28" smd circle (at 1.599997 -14.399997 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "G30" smd circle (at 3.199994 -14.399997 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "G32" smd circle (at 4.79999 -14.399997 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "G34" smd circle (at 6.399987 -14.399997 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 755 "MVREFS_B"))
    (pad "G36" smd circle (at 7.999984 -14.399997 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "G38" smd circle (at 9.600006 -14.399997 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 481 "CLKA1"))
    (pad "G40" smd circle (at 11.200003 -14.399997 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "G42" smd circle (at 12.8 -14.399997 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "H1" smd circle (at -16.399993 -13.624992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 305 "DQC_13"))
    (pad "H3" smd circle (at -15.599994 -13.624992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "H6" smd circle (at -14.799996 -13.624992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 294 "DQC_14"))
    (pad "H8" smd circle (at -13.975004 -13.975004 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "H44" smd circle (at 13.975004 -13.975004 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "H46" smd circle (at 14.799996 -13.624992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 518 "DQA_34"))
    (pad "H49" smd circle (at 15.599994 -13.624992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 516 "DQA_35"))
    (pad "H51" smd circle (at 16.399993 -13.624992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 517 "DQA_36"))
    (pad "J10" smd circle (at -12.999999 -13.599998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 333 "QSCB_1"))
    (pad "J11" smd circle (at -12.200001 -13.599998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 300 "DQC_17"))
    (pad "J12" smd circle (at -11.200003 -13.599998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 734 "MVREFS_C"))
    (pad "J13" smd circle (at -10.200005 -13.599998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 393 "DQB_60"))
    (pad "J14" smd circle (at -9.200007 -13.599998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 405 "QSBB_7"))
    (pad "J16" smd circle (at -8.200009 -13.599998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 367 "DQB_59"))
    (pad "J17" smd circle (at -7.000011 -13.599998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 360 "DQMBB_7"))
    (pad "J19" smd circle (at -5.800014 -13.599998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 354 "CLKB1"))
    (pad "J20" smd circle (at -4.600016 -13.599998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 364 "DQB_46"))
    (pad "J22" smd circle (at -3.399993 -13.599998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "J23" smd circle (at -2.199996 -13.599998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 359 "DQMBB_5"))
    (pad "J25" smd circle (at -0.999998 -13.599998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 390 "DQB_42"))
    (pad "J26" smd circle (at 0.2 -13.599998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "J28" smd circle (at 1.399997 -13.599998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 414 "CLKB0B"))
    (pad "J29" smd circle (at 2.599995 -13.599998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "J31" smd circle (at 3.799992 -13.599998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 422 "DQB_15"))
    (pad "J32" smd circle (at 4.99999 -13.599998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 461 "QSBB_1"))
    (pad "J34" smd circle (at 6.199988 -13.599998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 760 "MVREFD_B"))
    (pad "J35" smd circle (at 7.400011 -13.599998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 485 "CASA1B"))
    (pad "J37" smd circle (at 8.600008 -13.599998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 480 "RASA1B"))
    (pad "J38" smd circle (at 9.600006 -13.599998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "J39" smd circle (at 10.600004 -13.599998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 484 "CLKA1B"))
    (pad "J40" smd circle (at 11.600002 -13.599998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 520 "DQA_44"))
    (pad "J42" smd circle (at 12.6 -13.599998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "J43" smd circle (at 13.399999 -13.399999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 502 "DQA_32"))
    (pad "K1" smd circle (at -16.799992 -12.8 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 304 "DQC_25"))
    (pad "K3" smd circle (at -15.999993 -12.8 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 303 "DQC_24"))
    (pad "K5" smd circle (at -15.199995 -12.8 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 293 "DQC_15"))
    (pad "K7" smd circle (at -14.399997 -12.8 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "K9" smd circle (at -13.599998 -12.999999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 290 "DQMCB_2"))
    (pad "K11" smd circle (at -12.200001 -12.8 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "K12" smd circle (at -11.200003 -12.8 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 299 "DQC_16"))
    (pad "K13" smd circle (at -10.200005 -12.8 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 365 "DQB_63"))
    (pad "K14" smd circle (at -9.200007 -12.8 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 394 "DQB_62"))
    (pad "K16" smd circle (at -8.200009 -12.8 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 396 "QSB_7"))
    (pad "K17" smd circle (at -7.000011 -12.8 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 369 "DQB_56"))
    (pad "K19" smd circle (at -5.800014 -12.8 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 357 "CLKB1B"))
    (pad "K20" smd circle (at -4.600016 -12.8 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 386 "DQB_47"))
    (pad "K22" smd circle (at -3.399993 -12.8 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 404 "QSBB_5"))
    (pad "K23" smd circle (at -2.199996 -12.8 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 395 "QSB_5"))
    (pad "K25" smd circle (at -0.999998 -12.8 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "K26" smd circle (at 0.2 -12.8 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 464 "CKEB0"))
    (pad "K28" smd circle (at 1.399997 -12.8 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 411 "CLKB0"))
    (pad "K29" smd circle (at 2.599995 -12.8 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "K31" smd circle (at 3.799992 -12.8 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 451 "DQB_14"))
    (pad "K32" smd circle (at 4.99999 -12.8 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 450 "DQB_13"))
    (pad "K34" smd circle (at 6.199988 -12.8 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 453 "QSB_1"))
    (pad "K35" smd circle (at 7.400011 -12.8 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "K37" smd circle (at 8.600008 -12.8 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "K38" smd circle (at 9.600006 -12.8 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 471 "MAA_9"))
    (pad "K39" smd circle (at 10.600004 -12.8 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 468 "MAA_8"))
    (pad "K40" smd circle (at 11.600002 -12.8 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 478 "MAA_BA1"))
    (pad "K42" smd circle (at 12.6 -12.8 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 492 "DQA_46"))
    (pad "K43" smd circle (at 13.599998 -12.6 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "K45" smd circle (at 14.399997 -12.8 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 519 "DQA_33"))
    (pad "K47" smd circle (at 15.199995 -12.8 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 562 "DQA_31"))
    (pad "K49" smd circle (at 15.999993 -12.8 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 561 "DQA_29"))
    (pad "K51" smd circle (at 16.799992 -12.8 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 563 "DQA_28"))
    (pad "L2" smd circle (at -16.399993 -12.000001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 302 "DQC_27"))
    (pad "L4" smd circle (at -15.599994 -12.000001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "L6" smd circle (at -14.799996 -12.000001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 301 "DQC_26"))
    (pad "L9" smd circle (at -13.599998 -12.000001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 298 "DQC_18"))
    (pad "L10" smd circle (at -12.8 -12.000001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "L12" smd circle (at -11.200003 -12.000001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 297 "DQC_19"))
    (pad "L13" smd circle (at -10.200005 -12.000001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "L14" smd circle (at -9.200007 -12.000001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 285 "WEC0B"))
    (pad "L16" smd circle (at -8.200009 -12.000001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 212 "MAC_4"))
    (pad "L17" smd circle (at -7.000011 -12.000001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 370 "DQB_57"))
    (pad "L19" smd circle (at -5.800014 -12.000001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 368 "DQB_58"))
    (pad "L20" smd circle (at -4.600016 -12.000001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "L22" smd circle (at -3.399993 -12.000001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "L23" smd circle (at -2.199996 -12.000001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 389 "DQB_43"))
    (pad "L25" smd circle (at -0.999998 -12.000001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 391 "DQB_41"))
    (pad "L26" smd circle (at 0.2 -12.000001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "L28" smd circle (at 1.399997 -12.000001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 345 "MAB_0"))
    (pad "L29" smd circle (at 2.599995 -12.000001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 733 "GND_VSSRHB"))
    (pad "L31" smd circle (at 3.799992 -12.000001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 761 "+VDDRHB"))
    (pad "L32" smd circle (at 4.99999 -12.000001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "L34" smd circle (at 6.199988 -12.000001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 417 "DQMBB_1"))
    (pad "L35" smd circle (at 7.400011 -12.000001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "L37" smd circle (at 8.600008 -12.000001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 535 "CKEA1"))
    (pad "L38" smd circle (at 9.600006 -12.000001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "L39" smd circle (at 10.600004 -12.000001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "L40" smd circle (at 11.600002 -12.000001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 479 "MAA_BA0"))
    (pad "L42" smd circle (at 12.8 -11.800002 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 493 "DQA_45"))
    (pad "L43" smd circle (at 13.599998 -11.800002 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "L46" smd circle (at 14.799996 -12.000001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 581 "QSA_3"))
    (pad "L48" smd circle (at 15.599994 -12.000001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 560 "DQA_30"))
    (pad "L50" smd circle (at 16.399993 -12.000001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "M1" smd circle (at -16.799992 -11.200003 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 327 "QSC_3"))
    (pad "M3" smd circle (at -15.999993 -11.200003 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 335 "QSCB_3"))
    (pad "M5" smd circle (at -15.199995 -11.200003 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 291 "DQMCB_3"))
    (pad "M7" smd circle (at -14.399997 -11.200003 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "M9" smd circle (at -13.599998 -11.000003 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 326 "QSC_2"))
    (pad "M10" smd circle (at -12.8 -11.000003 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 334 "QSCB_2"))
    (pad "M11" smd circle (at -12.000001 -11.000003 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 216 "MAC_6"))
    (pad "M13" smd circle (at -10.200005 -11.200003 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 223 "MAC_3"))
    (pad "M14" smd circle (at -9.200007 -11.200003 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 215 "MAC_7"))
    (pad "M16" smd circle (at -8.200009 -11.200003 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "M17" smd circle (at -7.000011 -11.200003 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 366 "DQB_61"))
    (pad "M19" smd circle (at -5.800014 -11.200003 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "M20" smd circle (at -4.600016 -11.200003 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 363 "DQB_45"))
    (pad "M22" smd circle (at -3.399993 -11.200003 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 375 "DQB_44"))
    (pad "M23" smd circle (at -2.199996 -11.200003 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 392 "DQB_40"))
    (pad "M25" smd circle (at -0.999998 -11.200003 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 356 "CSB1B_0"))
    (pad "M26" smd circle (at 0.2 -11.200003 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "M28" smd circle (at 1.399997 -11.200003 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "M29" smd circle (at 2.599995 -11.200003 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "M31" smd circle (at 3.799992 -11.200003 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 342 "MAB_7"))
    (pad "M32" smd circle (at 4.99999 -11.200003 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "M34" smd circle (at 6.199988 -11.200003 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "M35" smd circle (at 7.400011 -11.200003 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 425 "DQB_11"))
    (pad "M37" smd circle (at 8.600008 -11.200003 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 475 "MAA_11"))
    (pad "M38" smd circle (at 9.600006 -11.200003 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 476 "MAA_10"))
    (pad "M39" smd circle (at 10.500004 -11.200003 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "M45" smd circle (at 14.399997 -11.200003 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "M47" smd circle (at 15.199995 -11.200003 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 556 "DQA_27"))
    (pad "M49" smd circle (at 15.999993 -11.200003 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 545 "DQMAB_3"))
    (pad "M51" smd circle (at 16.799992 -11.200003 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 589 "QSAB_3"))
    (pad "N2" smd circle (at -16.399993 -10.400005 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "N4" smd circle (at -15.599994 -10.400005 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 308 "DQC_29"))
    (pad "N6" smd circle (at -14.799996 -10.400005 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 306 "DQC_28"))
    (pad "N14" smd circle (at -9.200007 -10.400005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "N16" smd circle (at -8.200009 -10.400005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "N17" smd circle (at -7.000011 -10.400005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 353 "RASB1B"))
    (pad "N19" smd circle (at -5.800014 -10.400005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "N20" smd circle (at -4.600016 -10.400005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "N22" smd circle (at -3.399993 -10.400005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 341 "MAB_8"))
    (pad "N23" smd circle (at -2.199996 -10.400005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 351 "MAB_BA1"))
    (pad "N25" smd circle (at -0.999998 -10.400005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "N26" smd circle (at 0.2 -10.400005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 355 "WEB1B"))
    (pad "N28" smd circle (at 1.399997 -10.400005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 346 "MAB_1"))
    (pad "N29" smd circle (at 2.599995 -10.400005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "N31" smd circle (at 3.799992 -10.400005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "N32" smd circle (at 4.99999 -10.400005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 343 "MAB_6"))
    (pad "N34" smd circle (at 6.199988 -10.400005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 423 "DQB_12"))
    (pad "N35" smd circle (at 7.400011 -10.400005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 424 "DQB_10"))
    (pad "N37" smd circle (at 8.600008 -10.400005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 482 "WEA1B"))
    (pad "N38" smd circle (at 9.600006 -10.400005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "N40" smd circle (at 11.200003 -10.700004 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "N41" smd circle (at 12.000001 -10.800004 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 521 "DQA_47"))
    (pad "N42" smd circle (at 12.8 -10.800004 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 532 "QSAB_5"))
    (pad "N43" smd circle (at 13.599998 -10.800004 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 523 "QSA_5"))
    (pad "N46" smd circle (at 14.799996 -10.400005 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 558 "DQA_26"))
    (pad "N48" smd circle (at 15.599994 -10.400005 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "N50" smd circle (at 16.399993 -10.400005 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 555 "DQA_25"))
    (pad "P1" smd circle (at -16.799992 -9.600006 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 265 "DQC_32"))
    (pad "P3" smd circle (at -15.999993 -9.600006 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 309 "DQC_31"))
    (pad "P5" smd circle (at -15.199995 -9.600006 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 307 "DQC_30"))
    (pad "P7" smd circle (at -14.399997 -9.600006 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "P9" smd circle (at -13.599998 -10.000005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 324 "DQC_21"))
    (pad "P10" smd circle (at -12.8 -10.000005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 323 "DQC_22"))
    (pad "P11" smd circle (at -12.000001 -10.000005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 296 "DQC_20"))
    (pad "P12" smd circle (at -11.200003 -10.000005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "P16" smd circle (at -8.200009 -9.600006 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 286 "CSC0B_0"))
    (pad "P17" smd circle (at -7.000011 -9.600006 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "P19" smd circle (at -5.800014 -9.600006 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "P20" smd circle (at -4.600016 -9.600006 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 358 "CASB1B"))
    (pad "P22" smd circle (at -3.399993 -9.600006 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "P23" smd circle (at -2.199996 -9.600006 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "P25" smd circle (at -0.999998 -9.600006 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "P26" smd circle (at 0.2 -9.600006 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 352 "MAB_BA0"))
    (pad "P28" smd circle (at 1.399997 -9.600006 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 415 "CASB0B"))
    (pad "P29" smd circle (at 2.599995 -9.600006 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "P31" smd circle (at 3.799992 -9.600006 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 350 "MAB_3"))
    (pad "P32" smd circle (at 4.99999 -9.600006 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 340 "MAB_5"))
    (pad "P34" smd circle (at 6.199988 -9.600006 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "P35" smd circle (at 7.400011 -9.600006 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 427 "DQB_9"))
    (pad "P37" smd circle (at 8.600008 -9.600006 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 537 "RASA0B"))
    (pad "P38" smd circle (at 9.600006 -9.600006 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "P39" smd circle (at 10.400005 -9.800006 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 526 "MAA_BA2"))
    (pad "P40" smd circle (at 11.200003 -9.800006 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 483 "CSA1B_0"))
    (pad "P41" smd circle (at 12.000001 -9.800006 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "P42" smd circle (at 12.8 -9.800006 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "P43" smd circle (at 13.599998 -9.800006 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 487 "DQMAB_5"))
    (pad "P45" smd circle (at 14.399997 -9.600006 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "P47" smd circle (at 15.199995 -9.600006 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 547 "DQA_13"))
    (pad "P49" smd circle (at 15.999993 -9.600006 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 570 "DQA_12"))
    (pad "P51" smd circle (at 16.799992 -9.600006 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 557 "DQA_24"))
    (pad "R2" smd circle (at -16.399993 -8.800008 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 263 "DQC_35"))
    (pad "R4" smd circle (at -15.599994 -8.800008 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "R6" smd circle (at -14.799996 -8.800008 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 264 "DQC_33"))
    (pad "R9" smd circle (at -13.599998 -9.000007 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 284 "CLKC0"))
    (pad "R10" smd circle (at -12.8 -9.000007 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 287 "CLKC0B"))
    (pad "R11" smd circle (at -12.000001 -9.000007 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 295 "DQC_23"))
    (pad "R12" smd circle (at -11.200003 -9.000007 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "R13" smd circle (at -10.400005 -9.000007 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 220 "MAC_2"))
    (pad "R14" smd circle (at -9.600006 -9.000007 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 218 "MAC_0"))
    (pad "R16" smd circle (at -8.200009 -8.800008 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "R17" smd circle (at -7.000011 -8.800008 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 213 "MAC_5"))
    (pad "R19" smd circle (at -5.800014 -8.800008 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 740 "N72779223"))
    (pad "R20" smd circle (at -4.600016 -8.800008 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "R22" smd circle (at -3.399993 -8.800008 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "R23" smd circle (at -2.199996 -8.800008 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 344 "MAB_9"))
    (pad "R25" smd circle (at -0.999998 -8.800008 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 408 "CKEB1"))
    (pad "R26" smd circle (at 0.2 -8.800008 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 348 "MAB_11"))
    (pad "R28" smd circle (at 1.399997 -8.800008 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 399 "MAB_BA2"))
    (pad "R29" smd circle (at 2.599995 -8.800008 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "R31" smd circle (at 3.799992 -8.800008 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 412 "WEB0B"))
    (pad "R32" smd circle (at 4.99999 -8.800008 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 339 "MAB_4"))
    (pad "R34" smd circle (at 6.199988 -8.800008 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "R35" smd circle (at 7.400011 -8.800008 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 426 "DQB_8"))
    (pad "R37" smd circle (at 8.600008 -8.800008 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 474 "MAA_2"))
    (pad "R38" smd circle (at 9.600006 -8.800008 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 591 "CKEA0"))
    (pad "R39" smd circle (at 10.400005 -8.800008 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "R40" smd circle (at 11.200003 -8.800008 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 542 "CASA0B"))
    (pad "R41" smd circle (at 12.000001 -8.800008 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 497 "DQA_41"))
    (pad "R42" smd circle (at 12.8 -8.800008 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 495 "DQA_42"))
    (pad "R43" smd circle (at 13.599998 -8.800008 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 494 "DQA_43"))
    (pad "R46" smd circle (at 14.799996 -8.800008 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 559 "DQA_15"))
    (pad "R48" smd circle (at 15.599994 -8.800008 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 548 "DQA_14"))
    (pad "R50" smd circle (at 16.399993 -8.800008 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "T1" smd circle (at -16.799992 -8.000009 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 277 "QSCB_4"))
    (pad "T3" smd circle (at -15.999993 -8.000009 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 232 "DQMCB_4"))
    (pad "T5" smd circle (at -15.199995 -8.000009 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 262 "DQC_34"))
    (pad "T7" smd circle (at -14.399997 -8.000009 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "T9" smd circle (at -13.599998 -8.000009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 288 "CASC0B"))
    (pad "T10" smd circle (at -12.8 -8.000009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 337 "CKEC0"))
    (pad "T11" smd circle (at -12.000001 -8.000009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "T12" smd circle (at -11.200003 -8.000009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "T13" smd circle (at -10.400005 -8.000009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 219 "MAC_1"))
    (pad "T14" smd circle (at -9.600006 -8.000009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "T15" smd circle (at -8.800008 -8.000009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "T17" smd circle (at -7.000011 -8.000009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "T19" smd circle (at -5.800014 -8.000009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "T20" smd circle (at -4.600016 -8.000009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "T22" smd circle (at -3.399993 -8.000009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 731 "+MPVDD"))
    (pad "T23" smd circle (at -2.199996 -8.000009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 732 "GND_MPVSS"))
    (pad "T25" smd circle (at -0.999998 -8.000009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 349 "MAB_10"))
    (pad "T26" smd circle (at 0.2 -8.000009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "T28" smd circle (at 1.399997 -8.000009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 410 "RASB0B"))
    (pad "T29" smd circle (at 2.599995 -8.000009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 347 "MAB_2"))
    (pad "T31" smd circle (at 3.799992 -8.000009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 413 "CSB0B_0"))
    (pad "T32" smd circle (at 4.99999 -8.000009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "T34" smd circle (at 6.199988 -8.000009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "T35" smd circle (at 7.299985 -8.000009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "T45" smd circle (at 14.399997 -8.000009 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "T47" smd circle (at 15.199995 -8.000009 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 543 "DQMAB_1"))
    (pad "T49" smd circle (at 15.999993 -8.000009 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 587 "QSAB_1"))
    (pad "T51" smd circle (at 16.799992 -8.000009 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 579 "QSA_1"))
    (pad "U2" smd circle (at -16.399993 -7.200011 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "U4" smd circle (at -15.599994 -7.200011 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 248 "DQC_38"))
    (pad "U6" smd circle (at -14.799996 -7.200011 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 268 "QSC_4"))
    (pad "U36" smd circle (at 7.999984 -7.50001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "U37" smd circle (at 8.800008 -7.60001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "U38" smd circle (at 9.600006 -7.60001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 472 "MAA_0"))
    (pad "U39" smd circle (at 10.400005 -7.60001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 473 "MAA_1"))
    (pad "U40" smd circle (at 11.200003 -7.60001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "U41" smd circle (at 12.000001 -7.60001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "U42" smd circle (at 12.8 -7.60001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 496 "DQA_40"))
    (pad "U43" smd circle (at 13.599998 -7.60001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 541 "CLKA0B"))
    (pad "U46" smd circle (at 14.799996 -7.200011 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 574 "DQA_10"))
    (pad "U48" smd circle (at 15.599994 -7.200011 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "U50" smd circle (at 16.399993 -7.200011 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 573 "DQA_11"))
    (pad "V1" smd circle (at -16.799992 -6.400013 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 237 "DQC_36"))
    (pad "V3" smd circle (at -15.999993 -6.400013 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 259 "DQC_37"))
    (pad "V5" smd circle (at -15.199995 -6.400013 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 236 "DQC_39"))
    (pad "V7" smd circle (at -14.399997 -6.400013 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "V9" smd circle (at -13.599998 -6.800012 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "V10" smd circle (at -12.8 -6.800012 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 229 "CSC1B_0"))
    (pad "V11" smd circle (at -12.000001 -6.800012 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 228 "WEC1B"))
    (pad "V12" smd circle (at -11.200003 -6.800012 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 283 "RASC0B"))
    (pad "V13" smd circle (at -10.400005 -6.800012 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "V14" smd circle (at -9.600006 -6.800012 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "V15" smd circle (at -8.800008 -6.800012 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "V16" smd circle (at -8.000009 -6.800012 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "V36" smd circle (at 7.999984 -6.400013 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "V37" smd circle (at 8.800008 -6.400013 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "V38" smd circle (at 9.600006 -6.400013 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "V39" smd circle (at 10.400005 -6.400013 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "V40" smd circle (at 11.200003 -6.400013 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "V41" smd circle (at 12.000001 -6.400013 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 720 "GND_VSSRHA"))
    (pad "V42" smd circle (at 12.8 -6.400013 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 718 "+VDDRHA"))
    (pad "V43" smd circle (at 13.599998 -6.400013 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 538 "CLKA0"))
    (pad "V45" smd circle (at 14.399997 -6.400013 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "V47" smd circle (at 15.199995 -6.400013 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 565 "DQA_5"))
    (pad "V49" smd circle (at 15.999993 -6.400013 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 576 "DQA_8"))
    (pad "V51" smd circle (at 16.799992 -6.400013 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 575 "DQA_9"))
    (pad "W2" smd circle (at -16.399993 -5.599989 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 258 "DQC_49"))
    (pad "W4" smd circle (at -15.599994 -5.599989 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "W6" smd circle (at -14.799996 -5.599989 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 261 "DQC_48"))
    (pad "W9" smd circle (at -13.599998 -5.599989 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 227 "CLKC1"))
    (pad "W10" smd circle (at -12.8 -5.599989 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 230 "CLKC1B"))
    (pad "W11" smd circle (at -12.000001 -5.599989 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 763 "GND_VSSRHC"))
    (pad "W12" smd circle (at -11.200003 -5.599989 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 758 "+VDDRHC"))
    (pad "W13" smd circle (at -10.400005 -5.599989 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 272 "MAC_BA2"))
    (pad "W14" smd circle (at -9.600006 -5.599989 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "W15" smd circle (at -8.800008 -5.599989 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "W16" smd circle (at -8.000009 -5.599989 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 225 "MAC_BA0"))
    (pad "W19" smd circle (at -6.000013 -6.000013 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "W20" smd circle (at -5.000015 -6.000013 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "W21" smd circle (at -3.999992 -6.000013 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "+VDDCI"))
    (pad "W22" smd circle (at -2.999994 -6.000013 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "W24" smd circle (at -1.999996 -6.000013 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "+VDDCI"))
    (pad "W25" smd circle (at -0.999998 -6.000013 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "W26" smd circle (at 0 -6.000013 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "W27" smd circle (at 0.999998 -6.000013 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "W28" smd circle (at 1.999996 -6.000013 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "W30" smd circle (at 2.999994 -6.000013 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "W31" smd circle (at 3.999992 -6.000013 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "W32" smd circle (at 4.99999 -6.000013 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "W33" smd circle (at 5.999988 -6.000013 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "W46" smd circle (at 14.799996 -5.599989 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 564 "DQA_7"))
    (pad "W48" smd circle (at 15.599994 -5.599989 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 567 "DQA_6"))
    (pad "W50" smd circle (at 16.399993 -5.599989 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "Y1" smd circle (at -16.799992 -4.79999 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 271 "QSC_6"))
    (pad "Y3" smd circle (at -15.999993 -4.79999 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 257 "DQC_51"))
    (pad "Y5" smd circle (at -15.199995 -4.79999 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 260 "DQC_50"))
    (pad "Y7" smd circle (at -14.399997 -4.79999 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "Y19" smd circle (at -6.000013 -4.99999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "Y20" smd circle (at -5.000015 -4.99999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "+VDDCI"))
    (pad "Y21" smd circle (at -3.999992 -4.99999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "Y22" smd circle (at -2.999994 -4.99999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "+VDDCI"))
    (pad "Y24" smd circle (at -1.999996 -4.99999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "Y25" smd circle (at -0.999998 -4.99999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "Y26" smd circle (at 0 -4.99999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "Y27" smd circle (at 0.999998 -4.99999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "Y28" smd circle (at 1.999996 -4.99999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "Y30" smd circle (at 2.999994 -4.99999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "Y31" smd circle (at 3.999992 -4.99999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "Y32" smd circle (at 4.99999 -4.99999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "Y33" smd circle (at 5.999988 -4.99999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "Y36" smd circle (at 7.999984 -5.19999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 539 "WEA0B"))
    (pad "Y37" smd circle (at 8.800008 -5.19999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 467 "MAA_5"))
    (pad "Y38" smd circle (at 9.600006 -5.19999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 477 "MAA_3"))
    (pad "Y39" smd circle (at 10.400005 -5.19999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 470 "MAA_6"))
    (pad "Y40" smd circle (at 11.200003 -5.19999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 469 "MAA_7"))
    (pad "Y41" smd circle (at 12.000001 -5.19999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "Y42" smd circle (at 12.8 -5.19999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 549 "DQA_23"))
    (pad "Y43" smd circle (at 13.599998 -5.19999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 578 "DQA_22"))
    (pad "Y45" smd circle (at 14.399997 -4.79999 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "Y47" smd circle (at 15.199995 -4.79999 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 590 "QSAB_0"))
    (pad "Y49" smd circle (at 15.999993 -4.79999 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 546 "DQMAB_0"))
    (pad "Y51" smd circle (at 16.799992 -4.79999 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 566 "DQA_4"))
  )
  (footprint "TP089X043_1" (layer "F.Cu")
    (tedit 0)
    (at -17.395376 8.205005)
    (fp_text reference "TP61" (at -1.27 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 0.5588 0.5588) (drill 0.250012) (layers *.Cu *.Mask)
      (net 814 "DVPDATA_1"))
  )
  (footprint "C1206_113_1" (layer "F.Cu")
    (tedit 0)
    (at 145.927615 48.032002 -90)
    (fp_text reference "C1605" (at 0 0.981075 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd oval (at -1.4351 0 270) (size 0.9779 1.1938) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 865 "PWM2_VIN"))
    (pad "2" smd oval (at 1.4351 0 270) (size 0.9779 1.1938) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at 85.404622 87.550998 180)
    (fp_text reference "R218" (at -1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 592 "N25404999"))
  )
  (footprint "RES1608_0_8H_1" (layer "F.Cu")
    (tedit 0)
    (at -41.585396 93.406003 -90)
    (fp_text reference "ML1001" (at 3.175025 -2.539975 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 270) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 47 "A_DAC1_R"))
    (pad "2" smd rect (at 0 0.7874 270) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 48 "A_R_DAC1_F"))
  )
  (footprint "CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at 160.151615 26.696002 180)
    (fp_text reference "AC13" (at -1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 922 "N86494729"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 946 "N86495180"))
  )
  (footprint "CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at 150.753615 33.173002 90)
    (fp_text reference "AC18" (at -1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 924 "N86494873"))
  )
  (footprint "CAP1608_1" (layer "F.Cu")
    (tedit 0)
    (at 119.257615 3.912202 -90)
    (fp_text reference "EC168" (at 2.540025 -2.222475 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 270) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "+12V_EXT"))
    (pad "2" smd rect (at 0 0.7874 270) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -47.239385 8.154002 180)
    (fp_text reference "R8001" (at -2.2225 -2.54 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 753 "DVALID"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 846 "DVALID_R"))
  )
  (footprint "C1206_113_1" (layer "F.Cu")
    (tedit 0)
    (at 107.065615 45.746002 -90)
    (fp_text reference "EC1158" (at 0 0.981075 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd oval (at -1.4351 0 270) (size 0.9779 1.1938) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd oval (at 1.4351 0 270) (size 0.9779 1.1938) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "TP055PRI_1" (layer "F.Cu")
    (tedit 0)
    (at 40.004611 84.151005)
    (fp_text reference "TP23" (at -1.27 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd circle (at 0 0) (size 0.550012 0.550012) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 775 "PETP12_GFXRP12"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at 158.119615 26.696002 180)
    (fp_text reference "AR82" (at -1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 922 "N86494729"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "GEOM0009_1" (layer "F.Cu")
    (tedit 0)
    (at -20.04739 0.01 180)
    (fp_text reference "J8002" (at 1.5875 1.999996 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -7.60001 -1.999996 180) (size 0.599999 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "2" smd rect (at -7.60001 -1.999996 180) (size 0.599999 2.999994) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "3" smd rect (at -6.799986 -1.999996 180) (size 0.599999 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 811 "DVOCLK"))
    (pad "4" smd rect (at -6.799986 -1.999996 180) (size 0.599999 2.999994) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "5" smd rect (at -5.999988 -1.999996 180) (size 0.599999 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "6" smd rect (at -5.999988 -1.999996 180) (size 0.599999 2.999994) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "7" smd rect (at -5.19999 -1.999996 180) (size 0.599999 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 783 "DVPCNTL_2"))
    (pad "8" smd rect (at -5.19999 -1.999996 180) (size 0.599999 2.999994) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "9" smd rect (at -4.399991 -1.999996 180) (size 0.599999 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "10" smd rect (at -4.399991 -1.999996 180) (size 0.599999 2.999994) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 813 "DVPDATA_0"))
    (pad "11" smd rect (at -3.599993 -1.999996 180) (size 0.599999 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 814 "DVPDATA_1"))
    (pad "12" smd rect (at -3.599993 -1.999996 180) (size 0.599999 2.999994) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "13" smd rect (at -2.799994 -1.999996 180) (size 0.599999 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "14" smd rect (at -2.799994 -1.999996 180) (size 0.599999 2.999994) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 815 "DVPDATA_2"))
    (pad "15" smd rect (at -1.999996 -1.999996 180) (size 0.599999 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 805 "DVPDATA_3"))
    (pad "16" smd rect (at -1.999996 -1.999996 180) (size 0.599999 2.999994) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "17" smd rect (at -1.199998 -1.999996 180) (size 0.599999 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "18" smd rect (at -1.199998 -1.999996 180) (size 0.599999 2.999994) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 812 "DVPDATA_4"))
    (pad "19" smd rect (at -0.399999 -1.999996 180) (size 0.599999 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 802 "DVPDATA_5"))
    (pad "20" smd rect (at -0.399999 -1.999996 180) (size 0.599999 2.999994) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "21" smd rect (at 0.399999 -1.999996 180) (size 0.599999 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "22" smd rect (at 0.399999 -1.999996 180) (size 0.599999 2.999994) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 809 "DVPDATA_6"))
    (pad "23" smd rect (at 1.199998 -1.999996 180) (size 0.599999 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 804 "DVPDATA_7"))
    (pad "24" smd rect (at 1.199998 -1.999996 180) (size 0.599999 2.999994) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "25" smd rect (at 1.999996 -1.999996 180) (size 0.599999 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "26" smd rect (at 1.999996 -1.999996 180) (size 0.599999 2.999994) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 803 "DVPDATA_8"))
    (pad "27" smd rect (at 2.799994 -1.999996 180) (size 0.599999 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 782 "DVPDATA_9"))
    (pad "28" smd rect (at 2.799994 -1.999996 180) (size 0.599999 2.999994) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "29" smd rect (at 3.599993 -1.999996 180) (size 0.599999 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "30" smd rect (at 3.599993 -1.999996 180) (size 0.599999 2.999994) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 797 "DVPDATA_10"))
    (pad "31" smd rect (at 4.399991 -1.999996 180) (size 0.599999 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 810 "DVPDATA_11"))
    (pad "32" smd rect (at 4.399991 -1.999996 180) (size 0.599999 2.999994) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "33" smd rect (at 5.19999 -1.999996 180) (size 0.599999 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "34" smd rect (at 5.19999 -1.999996 180) (size 0.599999 2.999994) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 808 "DVPCNTL_0"))
    (pad "35" smd rect (at 6.000013 -1.999996 180) (size 0.599999 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 794 "DVPCNTL_1"))
    (pad "36" smd rect (at 6.000013 -1.999996 180) (size 0.599999 2.999994) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "37" smd rect (at 6.799986 -1.999996 180) (size 0.599999 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "38" smd rect (at 6.799986 -1.999996 180) (size 0.599999 2.999994) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 787 "GPIO_5"))
    (pad "39" smd rect (at 7.60001 -1.999996 180) (size 0.599999 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 789 "GPIO_3"))
    (pad "40" smd rect (at 7.60001 -1.999996 180) (size 0.599999 2.999994) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "R0805_67_1" (layer "F.Cu")
    (tedit 0)
    (at 127.639615 5.106002 180)
    (fp_text reference "ER1595" (at 1.905 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd oval (at -0.8509 0 180) (size 0.7747 0.9906) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "N85769551"))
    (pad "2" smd oval (at 0.8509 0 180) (size 0.7747 0.9906) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "+12V_EXT"))
  )
  (footprint "QFN40_6X6_1" (layer "F.Cu")
    (tedit 0)
    (at 157.103615 33.554002 -90)
    (fp_text reference "AU1" (at 0 0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd oval (at -2.999994 -2.249424 90) (size 0.8636 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 914 "N86494319"))
    (pad "2" smd oval (at -2.999994 -1.749552 90) (size 0.8636 0.3048) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "3" smd oval (at -2.999994 -1.24968 90) (size 0.8636 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "4" smd oval (at -2.999994 -0.749808 90) (size 0.8636 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 922 "N86494729"))
    (pad "5" smd oval (at -2.999994 -0.249936 90) (size 0.8636 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 921 "N86494727"))
    (pad "6" smd oval (at -2.999994 0.249936 90) (size 0.8636 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 920 "N86496268"))
    (pad "7" smd oval (at -2.999994 0.749808 90) (size 0.8636 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 919 "N86496570"))
    (pad "8" smd oval (at -2.999994 1.24968 90) (size 0.8636 0.3048) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "9" smd oval (at -2.999994 1.749552 90) (size 0.8636 0.3048) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "10" smd oval (at -2.999994 2.249424 90) (size 0.8636 0.3048) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "11" smd oval (at -2.249424 2.999994 180) (size 0.8636 0.3048) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "12" smd oval (at -1.749552 2.999994 180) (size 0.8636 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 923 "N86494909"))
    (pad "13" smd oval (at -1.24968 2.999994 180) (size 0.8636 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 57 "N86495082"))
    (pad "14" smd oval (at -0.749808 2.999994 180) (size 0.8636 0.3048) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "15" smd oval (at -0.249936 2.999994 180) (size 0.8636 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 924 "N86494873"))
    (pad "16" smd oval (at 0.249936 2.999994 180) (size 0.8636 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 925 "N86495210"))
    (pad "17" smd oval (at 0.749808 2.999994 180) (size 0.8636 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 929 "N86496246"))
    (pad "18" smd oval (at 1.24968 2.999994 180) (size 0.8636 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 928 "N86496297"))
    (pad "19" smd oval (at 1.749552 2.999994 180) (size 0.8636 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 927 "N86495035"))
    (pad "20" smd oval (at 2.249424 2.999994 180) (size 0.8636 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 930 "N86495047"))
    (pad "21" smd oval (at 2.999994 2.249424 270) (size 0.8636 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 933 "AICSN35"))
    (pad "22" smd oval (at 2.999994 1.749552 270) (size 0.8636 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 932 "AICSN24"))
    (pad "23" smd oval (at 2.999994 1.24968 270) (size 0.8636 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 936 "ACISP3"))
    (pad "24" smd oval (at 2.999994 0.749808 270) (size 0.8636 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 935 "ACISP2"))
    (pad "25" smd oval (at 2.999994 0.249936 270) (size 0.8636 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 934 "ACISP1"))
    (pad "26" smd oval (at 2.999994 -0.249936 270) (size 0.8636 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 71 "PWM1"))
    (pad "27" smd oval (at 2.999994 -0.749808 270) (size 0.8636 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 72 "PWM2"))
    (pad "28" smd oval (at 2.999994 -1.24968 270) (size 0.8636 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 601 "PWM3"))
    (pad "29" smd oval (at 2.999994 -1.749552 270) (size 0.8636 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 82 "VDD_+5V"))
    (pad "30" smd oval (at 2.999994 -2.249424 270) (size 0.8636 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 82 "VDD_+5V"))
    (pad "31" smd oval (at 2.249424 -2.999994) (size 0.8636 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 931 "N86495281"))
    (pad "32" smd oval (at 1.749552 -2.999994) (size 0.8636 0.3048) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "33" smd oval (at 1.24968 -2.999994) (size 0.8636 0.3048) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "34" smd oval (at 0.749808 -2.999994) (size 0.8636 0.3048) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "35" smd oval (at 0.249936 -2.999994) (size 0.8636 0.3048) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "36" smd oval (at -0.249936 -2.999994) (size 0.8636 0.3048) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "37" smd oval (at -0.749808 -2.999994) (size 0.8636 0.3048) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "38" smd oval (at -1.24968 -2.999994) (size 0.8636 0.3048) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "39" smd oval (at -1.749552 -2.999994) (size 0.8636 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "40" smd oval (at -2.249424 -2.999994) (size 0.8636 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 926 "VID_SEL"))
    (pad "41" smd rect (at 0 0 270) (size 4.191 4.191) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "F_PAD_M120_1" (layer "F.Cu")
    (tedit 0)
    (at 107.446615 6.757002)
    (fp_text reference "FM2" (at -0.762501 -0.000013 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd circle (at 0 0) (size 1.020064 1.020064) (layers "F.Cu" "F.Paste" "F.Mask"))
  )
  (footprint "CAP1608_1" (layer "F.Cu")
    (tedit 0)
    (at -40.69538 64.150994)
    (fp_text reference "C3006" (at 2.222475 2.540025 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 902 "DAC2_COMP_F"))
    (pad "2" smd rect (at 0 0.7874) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at 155.071615 26.696002)
    (fp_text reference "AC16" (at 1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 921 "N86494727"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at 160.405615 39.904002)
    (fp_text reference "AR47" (at 1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 601 "PWM3"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 82 "VDD_+5V"))
  )
  (footprint "CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at 157.103615 26.696002)
    (fp_text reference "AC15" (at 1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 944 "N86495338"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 922 "N86494729"))
  )
  (footprint "GEOM0013_1" (layer "F.Cu")
    (tedit 0)
    (at -2.39538 97.351004 90)
    (fp_text reference "C4" (at -0.635 1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144 90) (size 1.27 1.219987) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "+3.3V_BUS"))
    (pad "2" smd rect (at 0 0.9144 90) (size 1.27 1.219987) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at 155.643115 39.904002)
    (fp_text reference "AC10" (at 1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 932 "AICSN24"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 935 "ACISP2"))
  )
  (footprint "TP055PRI_1" (layer "F.Cu")
    (tedit 0)
    (at 21.404623 84.151005)
    (fp_text reference "TP7" (at -0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd circle (at 0 0) (size 0.550012 0.550012) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 620 "PETP0_GFXRP0"))
  )
  (footprint "C1206_113_1" (layer "F.Cu")
    (tedit 0)
    (at 112.526615 43.206002 180)
    (fp_text reference "EC1152" (at 0.981075 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd oval (at -1.4351 0 180) (size 0.9779 1.1938) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd oval (at 1.4351 0 180) (size 0.9779 1.1938) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1608_1" (layer "F.Cu")
    (tedit 0)
    (at 130.052615 58.319002)
    (fp_text reference "AR65" (at 1.904975 1.905025 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 942 "N864945390"))
    (pad "2" smd rect (at 0 0.7874) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "APHASE_1"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at 62.149627 21.766014 -90)
    (fp_text reference "R418" (at 1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 338 "N48027789"))
  )
  (footprint "XTAL_ABLS_1" (layer "F.Cu")
    (tedit 0)
    (at -13.205392 79.385991 -90)
    (fp_text reference "Y82" (at 0 0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd oval (at -4.318 0 270) (size 3.820008 1.500022) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "XTALIN"))
    (pad "2" smd oval (at 4.318 0 270) (size 3.820008 1.500022) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "XTALOUT"))
  )
  (footprint "GEOM0009_1" (layer "F.Cu")
    (tedit 0)
    (at -42.039395 0.01 180)
    (fp_text reference "J8001" (at 1.5875 1.999996 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -7.60001 -1.999996 180) (size 0.599999 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "2" smd rect (at -7.60001 -1.999996 180) (size 0.599999 2.999994) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "3" smd rect (at -6.799986 -1.999996 180) (size 0.599999 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 816 "DVP_MVP_CNTL_1"))
    (pad "4" smd rect (at -6.799986 -1.999996 180) (size 0.599999 2.999994) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "5" smd rect (at -5.999988 -1.999996 180) (size 0.599999 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "6" smd rect (at -5.999988 -1.999996 180) (size 0.599999 2.999994) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "7" smd rect (at -5.19999 -1.999996 180) (size 0.599999 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 817 "DVP_MVP_CNTL_0"))
    (pad "8" smd rect (at -5.19999 -1.999996 180) (size 0.599999 2.999994) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "9" smd rect (at -4.399991 -1.999996 180) (size 0.599999 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "10" smd rect (at -4.399991 -1.999996 180) (size 0.599999 2.999994) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 819 "DVPDATA_12"))
    (pad "11" smd rect (at -3.599993 -1.999996 180) (size 0.599999 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 825 "DVPDATA_13"))
    (pad "12" smd rect (at -3.599993 -1.999996 180) (size 0.599999 2.999994) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "13" smd rect (at -2.799994 -1.999996 180) (size 0.599999 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "14" smd rect (at -2.799994 -1.999996 180) (size 0.599999 2.999994) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 752 "DVPDATA_14"))
    (pad "15" smd rect (at -1.999996 -1.999996 180) (size 0.599999 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 786 "DVPDATA_15"))
    (pad "16" smd rect (at -1.999996 -1.999996 180) (size 0.599999 2.999994) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "17" smd rect (at -1.199998 -1.999996 180) (size 0.599999 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "18" smd rect (at -1.199998 -1.999996 180) (size 0.599999 2.999994) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 829 "DVPDATA_16"))
    (pad "19" smd rect (at -0.399999 -1.999996 180) (size 0.599999 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 750 "DVPDATA_17"))
    (pad "20" smd rect (at -0.399999 -1.999996 180) (size 0.599999 2.999994) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "21" smd rect (at 0.399999 -1.999996 180) (size 0.599999 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "22" smd rect (at 0.399999 -1.999996 180) (size 0.599999 2.999994) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 672 "DVPDATA_18"))
    (pad "23" smd rect (at 1.199998 -1.999996 180) (size 0.599999 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 801 "DVPDATA_19"))
    (pad "24" smd rect (at 1.199998 -1.999996 180) (size 0.599999 2.999994) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "25" smd rect (at 1.999996 -1.999996 180) (size 0.599999 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "26" smd rect (at 1.999996 -1.999996 180) (size 0.599999 2.999994) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 799 "DVPDATA_20"))
    (pad "27" smd rect (at 2.799994 -1.999996 180) (size 0.599999 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 681 "DVPDATA_21"))
    (pad "28" smd rect (at 2.799994 -1.999996 180) (size 0.599999 2.999994) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "29" smd rect (at 3.599993 -1.999996 180) (size 0.599999 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "30" smd rect (at 3.599993 -1.999996 180) (size 0.599999 2.999994) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 828 "DVPDATA_22"))
    (pad "31" smd rect (at 4.399991 -1.999996 180) (size 0.599999 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 780 "DVPDATA_23"))
    (pad "32" smd rect (at 4.399991 -1.999996 180) (size 0.599999 2.999994) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "33" smd rect (at 5.19999 -1.999996 180) (size 0.599999 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "34" smd rect (at 5.19999 -1.999996 180) (size 0.599999 2.999994) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 846 "DVALID_R"))
    (pad "35" smd rect (at 6.000013 -1.999996 180) (size 0.599999 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 845 "GENERICB_R"))
    (pad "36" smd rect (at 6.000013 -1.999996 180) (size 0.599999 2.999994) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "37" smd rect (at 6.799986 -1.999996 180) (size 0.599999 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "38" smd rect (at 6.799986 -1.999996 180) (size 0.599999 2.999994) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 664 "GPIO_6"))
    (pad "39" smd rect (at 7.60001 -1.999996 180) (size 0.599999 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 791 "GPIO_4"))
    (pad "40" smd rect (at 7.60001 -1.999996 180) (size 0.599999 2.999994) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -13.507779 61.361211 180)
    (fp_text reference "R4003" (at -2.2225 -2.54 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "+3.3V"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 75 "THERMINT"))
  )
  (footprint "GEOM0011_1" (layer "F.Cu")
    (tedit 0)
    (at -58.055391 86.761008 -90)
    (fp_text reference "J1001" (at -7.532624 1.5875 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at -9.525 -9.652 270) (size 1.397 1.397) (drill 0.899998) (layers *.Cu *.Mask)
      (net 704 "T2X2M"))
    (pad "2" thru_hole circle (at -7.62 -9.652 270) (size 1.397 1.397) (drill 0.899998) (layers *.Cu *.Mask)
      (net 703 "T2X2P"))
    (pad "3" thru_hole circle (at -5.715 -9.652 270) (size 1.397 1.397) (drill 0.899998) (layers *.Cu *.Mask)
      (net 4 "GND"))
    (pad "4" thru_hole circle (at -3.81 -9.652 270) (size 1.397 1.397) (drill 0.899998) (layers *.Cu *.Mask)
      (net 663 "T2X4M"))
    (pad "5" thru_hole circle (at -1.905 -9.652 270) (size 1.397 1.397) (drill 0.899998) (layers *.Cu *.Mask)
      (net 712 "T2X4P"))
    (pad "6" thru_hole circle (at 0 -9.652 270) (size 1.397 1.397) (drill 0.899998) (layers *.Cu *.Mask)
      (net 54 "DDCCLK_DAC1_R"))
    (pad "7" thru_hole circle (at 1.905 -9.652 270) (size 1.397 1.397) (drill 0.899998) (layers *.Cu *.Mask)
      (net 56 "DDCDATA_DAC1_R"))
    (pad "8" thru_hole circle (at 3.81 -9.652 270) (size 1.397 1.397) (drill 0.899998) (layers *.Cu *.Mask)
      (net 55 "VSYNC_DAC1_R"))
    (pad "9" thru_hole circle (at -9.525 -7.747 270) (size 1.397 1.397) (drill 0.899998) (layers *.Cu *.Mask)
      (net 702 "T2X1M"))
    (pad "10" thru_hole circle (at -7.62 -7.747 270) (size 1.397 1.397) (drill 0.899998) (layers *.Cu *.Mask)
      (net 701 "T2X1P"))
    (pad "11" thru_hole circle (at -5.715 -7.747 270) (size 1.397 1.397) (drill 0.899998) (layers *.Cu *.Mask)
      (net 4 "GND"))
    (pad "12" thru_hole circle (at -3.81 -7.747 270) (size 1.397 1.397) (drill 0.899998) (layers *.Cu *.Mask)
      (net 653 "T2X3M"))
    (pad "13" thru_hole circle (at -1.905 -7.747 270) (size 1.397 1.397) (drill 0.899998) (layers *.Cu *.Mask)
      (net 656 "T2X3P"))
    (pad "14" thru_hole circle (at 0 -7.747 270) (size 1.397 1.397) (drill 0.899998) (layers *.Cu *.Mask)
      (net 11 "+5V_VESA"))
    (pad "15" thru_hole circle (at 1.905 -7.747 270) (size 1.397 1.397) (drill 0.899998) (layers *.Cu *.Mask)
      (net 4 "GND"))
    (pad "16" thru_hole circle (at 3.81 -7.747 270) (size 1.397 1.397) (drill 0.899998) (layers *.Cu *.Mask)
      (net 906 "HPD_DVI2"))
    (pad "17" thru_hole circle (at -9.525 -5.842 270) (size 1.397 1.397) (drill 0.899998) (layers *.Cu *.Mask)
      (net 700 "T2X0M"))
    (pad "18" thru_hole circle (at -7.62 -5.842 270) (size 1.397 1.397) (drill 0.899998) (layers *.Cu *.Mask)
      (net 699 "T2X0P"))
    (pad "19" thru_hole circle (at -5.715 -5.842 270) (size 1.397 1.397) (drill 0.899998) (layers *.Cu *.Mask)
      (net 4 "GND"))
    (pad "20" thru_hole circle (at -3.81 -5.842 270) (size 1.397 1.397) (drill 0.899998) (layers *.Cu *.Mask)
      (net 713 "T2X5M"))
    (pad "21" thru_hole circle (at -1.905 -5.842 270) (size 1.397 1.397) (drill 0.899998) (layers *.Cu *.Mask)
      (net 714 "T2X5P"))
    (pad "22" thru_hole circle (at 0 -5.842 270) (size 1.397 1.397) (drill 0.899998) (layers *.Cu *.Mask)
      (net 4 "GND"))
    (pad "23" thru_hole circle (at 1.905 -5.842 270) (size 1.397 1.397) (drill 0.899998) (layers *.Cu *.Mask)
      (net 697 "T2XCP"))
    (pad "24" thru_hole circle (at 3.81 -5.842 270) (size 1.397 1.397) (drill 0.899998) (layers *.Cu *.Mask)
      (net 698 "T2XCM"))
    (pad "25" thru_hole oval (at 15.364993 -4.572 270) (size 2.999994 4.000017) (drill 0.189992) (layers *.Cu *.Mask)
      (net 4 "GND"))
    (pad "26" thru_hole oval (at -15.364993 -4.572 270) (size 2.999994 4.000017) (drill 0.189992) (layers *.Cu *.Mask)
      (net 4 "GND"))
    (pad "27" thru_hole circle (at -3.799992 -11.700002 270) (size 1.519987 1.519987) (drill 1.099998) (layers *.Cu *.Mask)
      (net 4 "GND"))
    (pad "28" thru_hole circle (at 3.259988 -11.700002 270) (size 1.519987 1.519987) (drill 1.099998) (layers *.Cu *.Mask)
      (net 4 "GND"))
    (pad "29" thru_hole circle (at 13.499998 -11.700002 270) (size 1.519987 1.519987) (drill 1.099998) (layers *.Cu *.Mask)
      (net 4 "GND"))
    (pad "30" thru_hole circle (at -13.499998 -11.700002 270) (size 1.519987 1.519987) (drill 1.099998) (layers *.Cu *.Mask)
      (net 4 "GND"))
    (pad "C1" thru_hole circle (at 6.985 -9.019007 270) (size 1.143 1.143) (drill 0.650011) (layers *.Cu *.Mask)
      (net 48 "A_R_DAC1_F"))
    (pad "C2" thru_hole circle (at 9.525 -9.019007 270) (size 1.143 1.143) (drill 0.650011) (layers *.Cu *.Mask)
      (net 46 "A_G_DAC1_F"))
    (pad "C3" thru_hole circle (at 6.985 -6.479007 270) (size 1.143 1.143) (drill 0.650011) (layers *.Cu *.Mask)
      (net 44 "A_B_DAC1_F"))
    (pad "C4" thru_hole circle (at 9.525 -6.479007 270) (size 1.143 1.143) (drill 0.650011) (layers *.Cu *.Mask)
      (net 53 "HSYNC_DAC1_R"))
    (pad "C5" thru_hole circle (at 8.255 -10.292004 270) (size 1.143 1.143) (drill 0.650011) (layers *.Cu *.Mask)
      (net 4 "GND"))
    (pad "C6" thru_hole circle (at 8.255 -5.212004 270) (size 1.143 1.143) (drill 0.650011) (layers *.Cu *.Mask)
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at 104.144615 8.662002 -90)
    (fp_text reference "R4036" (at 2.54 -2.2225 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "+3.3V_BUS"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 859 "N49971328"))
  )
  (footprint "RES1608_1" (layer "F.Cu")
    (tedit 0)
    (at 158.246615 19.012502)
    (fp_text reference "ER306" (at 2.222475 2.540025 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 83 "N86495804"))
    (pad "2" smd rect (at 0 0.7874) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 82 "VDD_+5V"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at 85.304622 67.451013 180)
    (fp_text reference "R210" (at -1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 536 "N25405181"))
  )
  (footprint "CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -2.29538 98.651002 90)
    (fp_text reference "C0" (at -0.635 1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "+3.3V_BUS"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "560UF_4V_R71D55_1" (layer "F.Cu")
    (tedit 0)
    (at 112.653615 68.161502 180)
    (fp_text reference "EC1154" (at 1.346835 0.005715 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole rect (at -1.75006 0 180) (size 1.8034 1.8034) (drill 1.397) (layers *.Cu *.Mask)
      (net 735 "+VDDC"))
    (pad "2" thru_hole circle (at 1.75006 0 180) (size 1.8034 1.8034) (drill 1.397) (layers *.Cu *.Mask)
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -2.795379 39.551018 -135)
    (fp_text reference "MR295" (at 0.224506 -3.367596 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 225) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 144 "DRAM_RST"))
    (pad "2" smd rect (at 0 0.492608 225) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at 159.135615 26.696002)
    (fp_text reference "AR49" (at 1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 922 "N86494729"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -37.995385 93.351012 -90)
    (fp_text reference "R1001" (at 2.54 -2.2225 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 47 "A_DAC1_R"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "C1206_113_1" (layer "F.Cu")
    (tedit 0)
    (at 145.927615 82.322002 90)
    (fp_text reference "C1584" (at 0 -0.981075 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd oval (at -1.4351 0 90) (size 0.9779 1.1938) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 863 "PWM3_VIN"))
    (pad "2" smd oval (at 1.4351 0 90) (size 0.9779 1.1938) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "560UF_4V_R71D55_1" (layer "F.Cu")
    (tedit 0)
    (at 112.526615 76.988002 180)
    (fp_text reference "EC1159" (at 1.346835 0.005715 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole rect (at -1.75006 0 180) (size 1.8034 1.8034) (drill 1.397) (layers *.Cu *.Mask)
      (net 735 "+VDDC"))
    (pad "2" thru_hole circle (at 1.75006 0 180) (size 1.8034 1.8034) (drill 1.397) (layers *.Cu *.Mask)
      (net 4 "GND"))
  )
  (footprint "C1206_113_1" (layer "F.Cu")
    (tedit 0)
    (at 107.065615 60.224002 90)
    (fp_text reference "EC1150" (at 0 -0.981075 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd oval (at -1.4351 0 90) (size 0.9779 1.1938) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd oval (at 1.4351 0 90) (size 0.9779 1.1938) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "TP089X043_1" (layer "F.Cu")
    (tedit 0)
    (at -22.495391 8.305005)
    (fp_text reference "TP67" (at -1.27 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 0.5588 0.5588) (drill 0.250012) (layers *.Cu *.Mask)
      (net 804 "DVPDATA_7"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at 23.00462 22.051002 -90)
    (fp_text reference "R518" (at 1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 211 "N48569967"))
  )
  (footprint "GEOM0013_1" (layer "F.Cu")
    (tedit 0)
    (at 98.556615 11.964002)
    (fp_text reference "C4008" (at 1.111516 1.27033 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144) (size 1.27 1.219987) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 830 "N49971242"))
    (pad "2" smd rect (at 0 0.9144) (size 1.27 1.219987) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at 157.357615 74.575002 90)
    (fp_text reference "AC38" (at -1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "+12V_EXT"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "C1206_113_1" (layer "F.Cu")
    (tedit 0)
    (at 145.927615 67.717002 -90)
    (fp_text reference "C1586" (at 0 0.981075 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd oval (at -1.4351 0 270) (size 0.9779 1.1938) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 867 "PWM1_VIN"))
    (pad "2" smd oval (at 1.4351 0 270) (size 0.9779 1.1938) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "TO_261_1" (layer "F.Cu")
    (tedit 0)
    (at 163.707615 20.346002 -90)
    (fp_text reference "U6" (at 0.508 -1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd circle (at -2.29997 3.124962 270) (size 1.016 1.016) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 83 "N86495804"))
    (pad "2" smd circle (at 0 3.124962 270) (size 1.016 1.016) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 82 "VDD_+5V"))
    (pad "3" smd circle (at 2.29997 3.124962 270) (size 1.016 1.016) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "+12V_EXT"))
    (pad "4" smd rect (at 0 -3.124962 270) (size 3.302 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 82 "VDD_+5V"))
  )
  (footprint "CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at 148.086615 33.173002 90)
    (fp_text reference "AC19" (at -1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 943 "N86494757"))
  )
  (footprint "TP055PRI_1" (layer "F.Cu")
    (tedit 0)
    (at 35.204621 84.151005)
    (fp_text reference "TP19" (at -1.27 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd circle (at 0 0) (size 0.550012 0.550012) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 610 "PETP9_GFXRP9"))
  )
  (footprint "CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -36.195389 87.750998)
    (fp_text reference "C1006" (at 2.2225 2.54 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "A_DAC1_B"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "560UF_4V_R71D55_1" (layer "F.Cu")
    (tedit 0)
    (at 151.388615 46.762002 -90)
    (fp_text reference "C1604" (at 0 1.36398 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole rect (at -1.75006 0 270) (size 1.8034 1.8034) (drill 1.397) (layers *.Cu *.Mask)
      (net 865 "PWM2_VIN"))
    (pad "2" thru_hole circle (at 1.75006 0 270) (size 1.8034 1.8034) (drill 1.397) (layers *.Cu *.Mask)
      (net 4 "GND"))
  )
  (footprint "TP055PRI_1" (layer "F.Cu")
    (tedit 0)
    (at 30.404605 84.151005)
    (fp_text reference "TP15" (at -1.27 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd circle (at 0 0) (size 0.550012 0.550012) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 604 "PETP6_GFXRP6"))
  )
  (footprint "RES1608_0_8H_1" (layer "F.Cu")
    (tedit 0)
    (at -38.695384 85.351003 -90)
    (fp_text reference "ML1003" (at 3.175025 -2.539975 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 270) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "A_DAC1_B"))
    (pad "2" smd rect (at 0 0.7874 270) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 44 "A_B_DAC1_F"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at 163.453615 31.268002 90)
    (fp_text reference "R737" (at -1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 926 "VID_SEL"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 82 "VDD_+5V"))
  )
  (footprint "TP055PRI_1" (layer "F.Cu")
    (tedit 0)
    (at 23.904618 83.151007)
    (fp_text reference "TP9" (at -0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd circle (at 0 0) (size 0.550012 0.550012) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 624 "PETP2_GFXRP2"))
  )
  (footprint "TP055PRI_1" (layer "F.Cu")
    (tedit 0)
    (at 40.80461 84.151005)
    (fp_text reference "TP24" (at -1.27 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd circle (at 0 0) (size 0.550012 0.550012) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 725 "PETN12_GFXRN12"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at 150.753615 32.220502 -90)
    (fp_text reference "AR55" (at 1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 924 "N86494873"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 943 "N86494757"))
  )
  (footprint "MLFP_16_3X3_1" (layer "F.Cu")
    (tedit 0)
    (at 156.976615 58.065002 90)
    (fp_text reference "U706" (at 0 -0.771398 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd oval (at -0.749808 1.199896 270) (size 0.3048 0.6096) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "2" smd oval (at -0.249936 1.199896 270) (size 0.3048 0.6096) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 69 "LG1"))
    (pad "3" smd oval (at 0.249936 1.199896 270) (size 0.3048 0.6096) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "4" smd oval (at 0.749808 1.199896 270) (size 0.3048 0.6096) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "5" smd oval (at 1.199896 0.749808 90) (size 0.6096 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "+12V_EXT"))
    (pad "6" smd oval (at 1.199896 0.249936 90) (size 0.6096 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 67 "LG2"))
    (pad "7" smd oval (at 1.199896 -0.249936 90) (size 0.6096 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 68 "APHASE_2"))
    (pad "8" smd oval (at 1.199896 -0.749808 90) (size 0.6096 0.3048) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "9" smd oval (at 0.749808 -1.199896 90) (size 0.3048 0.6096) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 63 "UG2"))
    (pad "10" smd oval (at 0.249936 -1.199896 90) (size 0.3048 0.6096) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 64 "BOOT2"))
    (pad "11" smd oval (at -0.249936 -1.199896 90) (size 0.3048 0.6096) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 65 "BOOT1"))
    (pad "12" smd oval (at -0.749808 -1.199896 90) (size 0.3048 0.6096) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 66 "UG1"))
    (pad "13" smd oval (at -1.199896 -0.749808 270) (size 0.6096 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "APHASE_1"))
    (pad "14" smd oval (at -1.199896 -0.249936 270) (size 0.6096 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "+12V_EXT"))
    (pad "15" smd oval (at -1.199896 0.249936 270) (size 0.6096 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 71 "PWM1"))
    (pad "16" smd oval (at -1.199896 0.749808 270) (size 0.6096 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 72 "PWM2"))
    (pad "17" smd rect (at 0 0 90) (size 1.2446 1.2446) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "GEOM0002_1" (layer "F.Cu")
    (tedit 0)
    (at -6.495397 20.751005 -135)
    (fp_text reference "U502" (at 0 -2.694077 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "A1" smd circle (at -4.399991 -6.399987 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "A2" smd circle (at -3.599993 -6.400013 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "A3" smd circle (at -2.799994 -6.400013 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "A4" smd circle (at -1.999996 -6.400013 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 155 "N48570117"))
    (pad "A9" smd circle (at 1.999996 -6.400013 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "A10" smd circle (at 2.799994 -6.400013 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "A11" smd circle (at 3.599993 -6.400013 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "A12" smd circle (at 4.399991 -6.399987 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "B1" smd circle (at -4.399991 -5.599989 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "B2" smd circle (at -3.599993 -5.599989 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 108 "DQD_45"))
    (pad "B3" smd circle (at -2.799994 -5.599989 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 109 "DQD_46"))
    (pad "B4" smd circle (at -1.999996 -5.599989 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "B9" smd circle (at 1.999996 -5.599989 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "B10" smd circle (at 2.799994 -5.599989 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 139 "DQD_60"))
    (pad "B11" smd circle (at 3.599993 -5.599989 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 138 "DQD_57"))
    (pad "B12" smd circle (at 4.399991 -5.599989 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "C1" smd circle (at -4.399991 -4.79999 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "C2" smd circle (at -3.599993 -4.79999 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 120 "DQD_44"))
    (pad "C3" smd circle (at -2.799994 -4.79999 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 131 "DQD_47"))
    (pad "C4" smd circle (at -1.999996 -4.79999 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "C9" smd circle (at 1.999996 -4.79999 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "C10" smd circle (at 2.799994 -4.79999 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 111 "DQD_62"))
    (pad "C11" smd circle (at 3.599993 -4.79999 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 110 "DQD_58"))
    (pad "C12" smd circle (at 4.399991 -4.79999 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "D1" smd circle (at -4.399991 -3.999992 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "D2" smd circle (at -3.599993 -3.999992 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 150 "QSDB_5"))
    (pad "D3" smd circle (at -2.799994 -3.999992 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 140 "QSD_5"))
    (pad "D4" smd circle (at -1.999996 -3.999992 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "D9" smd circle (at 1.999996 -3.999992 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "D10" smd circle (at 2.799994 -3.999992 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 141 "QSD_7"))
    (pad "D11" smd circle (at 3.599993 -3.999992 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 151 "QSDB_7"))
    (pad "D12" smd circle (at 4.399991 -3.999992 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "E1" smd circle (at -4.399991 -3.199994 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "E2" smd circle (at -3.599993 -3.199994 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 134 "DQD_43"))
    (pad "E3" smd circle (at -2.799994 -3.199994 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 104 "DQMDB_5"))
    (pad "E4" smd circle (at -1.999996 -3.199994 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "E9" smd circle (at 1.999996 -3.199994 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "E10" smd circle (at 2.799994 -3.199994 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 105 "DQMDB_7"))
    (pad "E11" smd circle (at 3.599993 -3.199994 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 112 "DQD_63"))
    (pad "E12" smd circle (at 4.399991 -3.199994 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "F1" smd circle (at -4.399991 -2.399995 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "F2" smd circle (at -3.599993 -2.399995 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 136 "DQD_41"))
    (pad "F3" smd circle (at -2.799994 -2.399995 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 135 "DQD_42"))
    (pad "F4" smd circle (at -1.999996 -2.399995 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 101 "CSD1B_0"))
    (pad "F9" smd circle (at 1.999996 -2.399995 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 103 "CASD1B"))
    (pad "F10" smd circle (at 2.799994 -2.399995 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 113 "DQD_61"))
    (pad "F11" smd circle (at 3.599993 -2.399995 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 114 "DQD_56"))
    (pad "F12" smd circle (at 4.399991 -2.399995 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "G1" smd circle (at -4.399991 -1.599997 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "G2" smd circle (at -3.599993 -1.599997 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "G3" smd circle (at -2.799994 -1.599997 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 137 "DQD_40"))
    (pad "G4" smd circle (at -1.999996 -1.599997 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 96 "MAD_BA1"))
    (pad "G9" smd circle (at 1.999996 -1.599997 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 97 "MAD_BA0"))
    (pad "G10" smd circle (at 2.799994 -1.599997 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 115 "DQD_59"))
    (pad "G11" smd circle (at 3.599993 -1.599997 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "G12" smd circle (at 4.399991 -1.599997 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "H1" smd circle (at -4.399991 -0.799998 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 148 "N48570085"))
    (pad "H2" smd circle (at -3.599993 -0.799998 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 85 "MAD_5"))
    (pad "H3" smd circle (at -2.799994 -0.799998 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 145 "MAD_BA2"))
    (pad "H4" smd circle (at -1.999996 -0.799998 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 100 "WED1B"))
    (pad "H9" smd circle (at 1.999996 -0.799998 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 154 "CKED1"))
    (pad "H10" smd circle (at 2.799994 -0.799998 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 98 "RASD1B"))
    (pad "H11" smd circle (at 3.599993 -0.799998 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 91 "MAD_1"))
    (pad "H12" smd circle (at 4.399991 -0.799998 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 149 "N48570109"))
    (pad "J1" smd circle (at -4.399991 0 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "J2" smd circle (at -3.599993 0 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "J3" smd circle (at -2.799994 0 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "J4" smd circle (at -1.999996 0 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "J9" smd circle (at 1.999996 0 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "J10" smd circle (at 2.799994 0 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 102 "CLKD1B"))
    (pad "J11" smd circle (at 3.599993 0 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 99 "CLKD1"))
    (pad "J12" smd circle (at 4.399991 0 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "K1" smd circle (at -4.399991 0.799998 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 146 "N48570141"))
    (pad "K2" smd circle (at -3.599993 0.799998 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 86 "MAD_8"))
    (pad "K3" smd circle (at -2.799994 0.799998 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 88 "MAD_6"))
    (pad "K4" smd circle (at -1.999996 0.799998 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 84 "MAD_4"))
    (pad "K9" smd circle (at 1.999996 0.799998 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 90 "MAD_0"))
    (pad "K10" smd circle (at 2.799994 0.799998 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 92 "MAD_2"))
    (pad "K11" smd circle (at 3.599993 0.799998 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 94 "MAD_10"))
    (pad "K12" smd circle (at 4.399991 0.799998 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 147 "N48570039"))
    (pad "L1" smd circle (at -4.399991 1.599997 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "L2" smd circle (at -3.599993 1.599997 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "L3" smd circle (at -2.799994 1.599997 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 126 "DQD_39"))
    (pad "L4" smd circle (at -1.999996 1.599997 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 87 "MAD_7"))
    (pad "L9" smd circle (at 1.999996 1.599997 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 93 "MAD_11"))
    (pad "L10" smd circle (at 2.799994 1.599997 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 117 "DQD_51"))
    (pad "L11" smd circle (at 3.599993 1.599997 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "L12" smd circle (at 4.399991 1.599997 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "M1" smd circle (at -4.399991 2.399995 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "M2" smd circle (at -3.599993 2.399995 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 125 "DQD_37"))
    (pad "M3" smd circle (at -2.799994 2.399995 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 128 "DQD_38"))
    (pad "M4" smd circle (at -1.999996 2.399995 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 89 "MAD_9"))
    (pad "M9" smd circle (at 1.999996 2.399995 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 95 "MAD_3"))
    (pad "M10" smd circle (at 2.799994 2.399995 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 119 "DQD_50"))
    (pad "M11" smd circle (at 3.599993 2.399995 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 116 "DQD_48"))
    (pad "M12" smd circle (at 4.399991 2.399995 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "N1" smd circle (at -4.399991 3.199994 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "N2" smd circle (at -3.599993 3.199994 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 127 "DQD_36"))
    (pad "N3" smd circle (at -2.799994 3.199994 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 107 "DQMDB_4"))
    (pad "N4" smd circle (at -1.999996 3.199994 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "N9" smd circle (at 1.999996 3.199994 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "N10" smd circle (at 2.799994 3.199994 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 106 "DQMDB_6"))
    (pad "N11" smd circle (at 3.599993 3.199994 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 118 "DQD_49"))
    (pad "N12" smd circle (at 4.399991 3.199994 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "P1" smd circle (at -4.399991 3.999992 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "P2" smd circle (at -3.599993 3.999992 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 153 "QSDB_4"))
    (pad "P3" smd circle (at -2.799994 3.999992 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 143 "QSD_4"))
    (pad "P4" smd circle (at -1.999996 3.999992 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "P9" smd circle (at 1.999996 3.999992 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "P10" smd circle (at 2.799994 3.999992 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 142 "QSD_6"))
    (pad "P11" smd circle (at 3.599993 3.999992 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 152 "QSDB_6"))
    (pad "P12" smd circle (at 4.399991 3.999992 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "R1" smd circle (at -4.399991 4.79999 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "R2" smd circle (at -3.599993 4.79999 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 129 "DQD_35"))
    (pad "R3" smd circle (at -2.799994 4.79999 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 130 "DQD_34"))
    (pad "R4" smd circle (at -1.999996 4.79999 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "R9" smd circle (at 1.999996 4.79999 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "R10" smd circle (at 2.799994 4.79999 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 122 "DQD_54"))
    (pad "R11" smd circle (at 3.599993 4.79999 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 121 "DQD_52"))
    (pad "R12" smd circle (at 4.399991 4.79999 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "T1" smd circle (at -4.399991 5.599989 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "T2" smd circle (at -3.599993 5.599989 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 132 "DQD_33"))
    (pad "T3" smd circle (at -2.799994 5.599989 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 133 "DQD_32"))
    (pad "T4" smd circle (at -1.999996 5.599989 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "T9" smd circle (at 1.999996 5.599989 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "T10" smd circle (at 2.799994 5.599989 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 124 "DQD_55"))
    (pad "T11" smd circle (at 3.599993 5.599989 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 123 "DQD_53"))
    (pad "T12" smd circle (at 4.399991 5.599989 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "V1" smd circle (at -4.399991 6.399987 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "V2" smd circle (at -3.599993 6.400013 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "V3" smd circle (at -2.799994 6.400013 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "V4" smd circle (at -1.999996 6.400013 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "V9" smd circle (at 1.999996 6.400013 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 144 "DRAM_RST"))
    (pad "V10" smd circle (at 2.799994 6.400013 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "V11" smd circle (at 3.599993 6.400013 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "V12" smd circle (at 4.399991 6.399987 225) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -8.195394 40.751016 45)
    (fp_text reference "MR52" (at 0 2.694077 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 45) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "2" smd rect (at 0 0.492608 45) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 827 "GPIO_2"))
  )
  (footprint "CAP1608_1" (layer "F.Cu")
    (tedit 0)
    (at 130.052615 74.575002 180)
    (fp_text reference "AC40" (at -1.904975 -1.905025 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 180) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 940 "N864960700"))
    (pad "2" smd rect (at 0 0.7874 180) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "GEOM0005_1" (layer "F.Cu")
    (tedit 0)
    (at 0.004615 111.151002)
    (fp_text reference "MPCIE1" (at 28.094991 -3.499993 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "A1" smd rect (at -11.500002 -3.999992) (size 0.699999 3.199994) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 901 "PRESENCE"))
    (pad "A2" smd rect (at -10.500004 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 33 "+12V_BUS"))
    (pad "A3" smd rect (at -9.500006 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 33 "+12V_BUS"))
    (pad "A4" smd rect (at -8.500008 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "A5" smd rect (at -7.50001 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "A6" smd rect (at -6.500012 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 848 "JTDI"))
    (pad "A7" smd rect (at -5.499989 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 849 "JTDO"))
    (pad "A8" smd rect (at -4.499991 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "A9" smd rect (at -3.499993 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 31 "+3.3V_BUS"))
    (pad "A10" smd rect (at -2.499995 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 31 "+3.3V_BUS"))
    (pad "A11" smd rect (at -1.499997 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 73 "PERST#"))
    (pad "A12" smd rect (at 1.499997 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "A13" smd rect (at 2.499995 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 741 "PCIE_REFCLKP"))
    (pad "A14" smd rect (at 3.499993 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 639 "PCIE_REFCLKN"))
    (pad "A15" smd rect (at 4.499991 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "A16" smd rect (at 5.499989 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 885 "PERP0"))
    (pad "A17" smd rect (at 6.500012 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 869 "PERN0"))
    (pad "A18" smd rect (at 7.50001 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "A19" smd rect (at 8.500008 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "A20" smd rect (at 9.500006 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "A21" smd rect (at 10.500004 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 886 "PERP1"))
    (pad "A22" smd rect (at 11.500002 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 870 "PERN1"))
    (pad "A23" smd rect (at 12.5 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "A24" smd rect (at 13.499998 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "A25" smd rect (at 14.499996 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 893 "PERP2"))
    (pad "A26" smd rect (at 15.499994 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 877 "PERN2"))
    (pad "A27" smd rect (at 16.499992 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "A28" smd rect (at 17.49999 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "A29" smd rect (at 18.500014 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 894 "PERP3"))
    (pad "A30" smd rect (at 19.500012 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 878 "PERN3"))
    (pad "A31" smd rect (at 20.50001 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "A32" smd rect (at 21.500008 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "A33" smd rect (at 22.500006 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "A34" smd rect (at 23.500004 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "A35" smd rect (at 24.500002 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 895 "PERP4"))
    (pad "A36" smd rect (at 25.5 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 879 "PERN4"))
    (pad "A37" smd rect (at 26.499998 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "A38" smd rect (at 27.499996 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "A39" smd rect (at 28.499994 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 896 "PERP5"))
    (pad "A40" smd rect (at 29.499992 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 880 "PERN5"))
    (pad "A41" smd rect (at 30.49999 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "A42" smd rect (at 31.499988 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "A43" smd rect (at 32.500011 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 897 "PERP6"))
    (pad "A44" smd rect (at 33.500009 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 881 "PERN6"))
    (pad "A45" smd rect (at 34.500007 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "A46" smd rect (at 35.500005 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "A47" smd rect (at 36.500003 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 898 "PERP7"))
    (pad "A48" smd rect (at 37.500001 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 882 "PERN7"))
    (pad "A49" smd rect (at 38.499999 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "A50" smd rect (at 39.499997 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "A51" smd rect (at 40.499995 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "A52" smd rect (at 41.499993 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 899 "PERP8"))
    (pad "A53" smd rect (at 42.499991 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 883 "PERN8"))
    (pad "A54" smd rect (at 43.499989 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "A55" smd rect (at 44.500013 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "A56" smd rect (at 45.500011 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 900 "PERP9"))
    (pad "A57" smd rect (at 46.500009 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 884 "PERN9"))
    (pad "A58" smd rect (at 47.500007 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "A59" smd rect (at 48.500005 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "A60" smd rect (at 49.500003 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 887 "PERP10"))
    (pad "A61" smd rect (at 50.500001 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 871 "PERN10"))
    (pad "A62" smd rect (at 51.499999 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "A63" smd rect (at 52.499997 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "A64" smd rect (at 53.499995 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 888 "PERP11"))
    (pad "A65" smd rect (at 54.499993 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 872 "PERN11"))
    (pad "A66" smd rect (at 55.499991 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "A67" smd rect (at 56.499989 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "A68" smd rect (at 57.499987 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 889 "PERP12"))
    (pad "A69" smd rect (at 58.50001 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 873 "PERN12"))
    (pad "A70" smd rect (at 59.500008 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "A71" smd rect (at 60.500006 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "A72" smd rect (at 61.500004 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 890 "PERP13"))
    (pad "A73" smd rect (at 62.500002 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 874 "PERN13"))
    (pad "A74" smd rect (at 63.5 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "A75" smd rect (at 64.499998 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "A76" smd rect (at 65.499996 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 891 "PERP14"))
    (pad "A77" smd rect (at 66.499994 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 875 "PERN14"))
    (pad "A78" smd rect (at 67.499992 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "A79" smd rect (at 68.49999 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "A80" smd rect (at 69.500013 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 892 "PERP15"))
    (pad "A81" smd rect (at 70.500011 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 876 "PERN15"))
    (pad "A82" smd rect (at 71.500009 -3.499993) (size 0.699999 4.199992) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "B1" smd rect (at -11.500002 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "+12V_BUS"))
    (pad "B2" smd rect (at -10.500004 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "+12V_BUS"))
    (pad "B3" smd rect (at -9.500006 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "+12V_BUS"))
    (pad "B4" smd rect (at -8.500008 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "B5" smd rect (at -7.50001 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "B6" smd rect (at -6.500012 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "B7" smd rect (at -5.499989 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 850 "N84002959"))
    (pad "B8" smd rect (at -4.499991 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "+3.3V_BUS"))
    (pad "B9" smd rect (at -3.499993 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "B10" smd rect (at -2.499995 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "B11" smd rect (at -1.499997 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "B12" smd rect (at 1.499997 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "B13" smd rect (at 2.499995 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "B14" smd rect (at 3.499993 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 620 "PETP0_GFXRP0"))
    (pad "B15" smd rect (at 4.499991 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 619 "PETN0_GFXRN0"))
    (pad "B16" smd rect (at 5.499989 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "B17" smd rect (at 6.500012 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "B18" smd rect (at 7.50001 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "B19" smd rect (at 8.500008 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 622 "PETP1_GFXRP1"))
    (pad "B20" smd rect (at 9.500006 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 621 "PETN1_GFXRN1"))
    (pad "B21" smd rect (at 10.500004 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "B22" smd rect (at 11.500002 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "B23" smd rect (at 12.5 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 624 "PETP2_GFXRP2"))
    (pad "B24" smd rect (at 13.499998 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 623 "PETN2_GFXRN2"))
    (pad "B25" smd rect (at 14.499996 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "B26" smd rect (at 15.499994 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "B27" smd rect (at 16.499992 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 626 "PETP3_GFXRP3"))
    (pad "B28" smd rect (at 17.49999 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 625 "PETN3_GFXRN3"))
    (pad "B29" smd rect (at 18.500014 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "B30" smd rect (at 19.500012 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "B31" smd rect (at 20.50001 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "B32" smd rect (at 21.500008 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "B33" smd rect (at 22.500006 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 628 "PETP4_GFXRP4"))
    (pad "B34" smd rect (at 23.500004 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 627 "PETN4_GFXRN4"))
    (pad "B35" smd rect (at 24.500002 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "B36" smd rect (at 25.5 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "B37" smd rect (at 26.499998 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 630 "PETP5_GFXRP5"))
    (pad "B38" smd rect (at 27.499996 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 629 "PETN5_GFXRN5"))
    (pad "B39" smd rect (at 28.499994 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "B40" smd rect (at 29.499992 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "B41" smd rect (at 30.49999 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 604 "PETP6_GFXRP6"))
    (pad "B42" smd rect (at 31.499988 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 603 "PETN6_GFXRN6"))
    (pad "B43" smd rect (at 32.500011 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "B44" smd rect (at 33.500009 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "B45" smd rect (at 34.500007 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 606 "PETP7_GFXRP7"))
    (pad "B46" smd rect (at 35.500005 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 605 "PETN7_GFXRN7"))
    (pad "B47" smd rect (at 36.500003 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "B48" smd rect (at 37.500001 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "B49" smd rect (at 38.499999 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "B50" smd rect (at 39.499997 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 608 "PETP8_GFXRP8"))
    (pad "B51" smd rect (at 40.499995 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 607 "PETN8_GFXRN8"))
    (pad "B52" smd rect (at 41.499993 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "B53" smd rect (at 42.499991 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "B54" smd rect (at 43.499989 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 610 "PETP9_GFXRP9"))
    (pad "B55" smd rect (at 44.500013 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 609 "PETN9_GFXRN9"))
    (pad "B56" smd rect (at 45.500011 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "B57" smd rect (at 46.500009 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "B58" smd rect (at 47.500007 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 612 "PETP10_GFXRP10"))
    (pad "B59" smd rect (at 48.500005 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 611 "PETN10_GFXRN10"))
    (pad "B60" smd rect (at 49.500003 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "B61" smd rect (at 50.500001 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "B62" smd rect (at 51.499999 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 614 "PETP11_GFXRP11"))
    (pad "B63" smd rect (at 52.499997 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 613 "PETN11_GFXRN11"))
    (pad "B64" smd rect (at 53.499995 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "B65" smd rect (at 54.499993 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "B66" smd rect (at 55.499991 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 775 "PETP12_GFXRP12"))
    (pad "B67" smd rect (at 56.499989 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 725 "PETN12_GFXRN12"))
    (pad "B68" smd rect (at 57.499987 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "B69" smd rect (at 58.50001 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "B70" smd rect (at 59.500008 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 729 "PETP13_GFXRP13"))
    (pad "B71" smd rect (at 60.500006 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 726 "PETN13_GFXRN13"))
    (pad "B72" smd rect (at 61.500004 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "B73" smd rect (at 62.500002 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "B74" smd rect (at 63.5 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 762 "PETP14_GFXRP14"))
    (pad "B75" smd rect (at 64.499998 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 717 "PETN14_GFXRN14"))
    (pad "B76" smd rect (at 65.499996 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "B77" smd rect (at 66.499994 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "B78" smd rect (at 67.499992 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 723 "PETP15_GFXRP15"))
    (pad "B79" smd rect (at 68.49999 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 724 "PETN15_GFXRN15"))
    (pad "B80" smd rect (at 69.500013 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "B81" smd rect (at 70.500011 -3.999992) (size 0.699999 3.199994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 901 "PRESENCE"))
    (pad "B82" smd rect (at 71.500009 -3.499993) (size 0.699999 4.199992) (layers "F.Cu" "F.Paste" "F.Mask"))
  )
  (footprint "GEOM0008_1" (layer "F.Cu")
    (tedit 0)
    (at 97.413615 9.043002 90)
    (fp_text reference "B4001" (at -1.27033 1.111516 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144 90) (size 1.27 1.219987) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "+12V_BUS"))
    (pad "2" smd rect (at 0 0.9144 90) (size 1.27 1.219987) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 830 "N49971242"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at 156.087615 26.696002)
    (fp_text reference "AR50" (at 1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 944 "N86495338"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 921 "N86494727"))
  )
  (footprint "RES1608_0_8H_1" (layer "F.Cu")
    (tedit 0)
    (at -39.540391 90.590997)
    (fp_text reference "ML1002" (at 2.539975 3.175025 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "A_DAC1_G"))
    (pad "2" smd rect (at 0 0.7874) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 46 "A_G_DAC1_F"))
  )
  (footprint "CON_6P_HDER_TH_1" (layer "F.Cu")
    (tedit 0)
    (at 180.598615 9.043002 -90)
    (fp_text reference "J1602" (at 24.629999 1.5875 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at -4.199992 22.530003 270) (size 3.048 3.048) (drill 1.799996) (layers *.Cu *.Mask)
      (net 60 "+12V_EXT"))
    (pad "2" thru_hole circle (at 0 22.530003 270) (size 3.048 3.048) (drill 1.799996) (layers *.Cu *.Mask)
      (net 60 "+12V_EXT"))
    (pad "3" thru_hole rect (at 4.199992 22.530003 270) (size 3.048 3.048) (drill 1.799996) (layers *.Cu *.Mask)
      (net 60 "+12V_EXT"))
    (pad "4" thru_hole circle (at -4.199992 26.729995 270) (size 3.048 3.048) (drill 1.799996) (layers *.Cu *.Mask)
      (net 4 "GND"))
    (pad "5" thru_hole circle (at 0 26.729995 270) (size 3.048 3.048) (drill 1.799996) (layers *.Cu *.Mask)
      (net 4 "GND"))
    (pad "6" thru_hole circle (at 4.199992 26.729995 270) (size 3.048 3.048) (drill 1.799996) (layers *.Cu *.Mask)
      (net 4 "GND"))
  )
  (footprint "C1206_113_1" (layer "F.Cu")
    (tedit 0)
    (at 78.744615 16.282002)
    (fp_text reference "EC347" (at -0.981075 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd oval (at -1.4351 0) (size 0.9779 1.1938) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd oval (at 1.4351 0) (size 0.9779 1.1938) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "560UF_4V_R71D55_1" (layer "F.Cu")
    (tedit 0)
    (at 151.388615 68.733002 -90)
    (fp_text reference "C1606" (at 0 1.36398 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole rect (at -1.75006 0 270) (size 1.8034 1.8034) (drill 1.397) (layers *.Cu *.Mask)
      (net 867 "PWM1_VIN"))
    (pad "2" thru_hole circle (at 1.75006 0 270) (size 1.8034 1.8034) (drill 1.397) (layers *.Cu *.Mask)
      (net 4 "GND"))
  )
  (footprint "RES1608_1" (layer "F.Cu")
    (tedit 0)
    (at 130.052615 38.634002)
    (fp_text reference "AR69" (at 1.904975 1.905025 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 941 "N864966460"))
    (pad "2" smd rect (at 0 0.7874) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 68 "APHASE_2"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -11.895387 37.550997)
    (fp_text reference "R64" (at 1.5875 1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 790 "GPIO_17_INT"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 75 "THERMINT"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at 21.104624 67.551013)
    (fp_text reference "R101" (at 1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 702 "T2X1M"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 701 "T2X1P"))
  )
  (footprint "TP055PRI_1" (layer "F.Cu")
    (tedit 0)
    (at 34.404622 83.151007)
    (fp_text reference "TP18" (at -1.27 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd circle (at 0 0) (size 0.550012 0.550012) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 607 "PETN8_GFXRN8"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at 150.753615 37.872002 90)
    (fp_text reference "AR42" (at -1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 933 "AICSN35"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 930 "N86495047"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at 100.842615 13.107002 90)
    (fp_text reference "R4031" (at -2.54 2.2225 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 835 "N49971448"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 836 "N72984167"))
  )
  (footprint "SOT23_3PIN_1" (layer "F.Cu")
    (tedit 0)
    (at 83.951615 10.059002 180)
    (fp_text reference "Q4001" (at -1.289075 -1.4732 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.9398 1.143 180) (size 0.640004 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 840 "N81403017"))
    (pad "2" smd rect (at 0.9398 1.143 180) (size 0.640004 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "3" smd rect (at 0 -1.143 180) (size 0.640004 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 835 "N49971448"))
  )
  (footprint "GEOM0013_1" (layer "F.Cu")
    (tedit 0)
    (at -24.295387 71.551005)
    (fp_text reference "C842" (at 1.181837 1.195476 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144) (size 1.27 1.219987) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "+3.3V_BUS"))
    (pad "2" smd rect (at 0 0.9144) (size 1.27 1.219987) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at 86.618615 11.075002)
    (fp_text reference "TR4010" (at 2.54 3.175 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 835 "N49971448"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 855 "N73051201"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at 100.784601 84.186006 180)
    (fp_text reference "R395" (at -1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 144 "DRAM_RST"))
  )
  (footprint "C1206_113_1" (layer "F.Cu")
    (tedit 0)
    (at 145.927615 87.402002 -90)
    (fp_text reference "C1582" (at 0 0.981075 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd oval (at -1.4351 0 270) (size 0.9779 1.1938) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 863 "PWM3_VIN"))
    (pad "2" smd oval (at 1.4351 0 270) (size 0.9779 1.1938) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at 21.104624 69.851008 180)
    (fp_text reference "R103" (at -1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 656 "T2X3P"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 653 "T2X3M"))
  )
  (footprint "C1206_113_1" (layer "F.Cu")
    (tedit 0)
    (at 107.065615 85.116002 -90)
    (fp_text reference "EC1163" (at 0 0.981075 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd oval (at -1.4351 0 270) (size 0.9779 1.1938) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd oval (at 1.4351 0 270) (size 0.9779 1.1938) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -37.495386 94.851009)
    (fp_text reference "R1027" (at 2.2225 2.54 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 615 "A_DAC1_RB"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "HD2MM1X2_KEY_1" (layer "F.Cu")
    (tedit 0)
    (at 90.809615 4.344002)
    (fp_text reference "TJ4010" (at 0.118986 0.000013 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole rect (at 0 0) (size 1.397 1.397) (drill 0.999998) (layers *.Cu *.Mask)
      (net 830 "N49971242"))
    (pad "2" thru_hole circle (at 1.999996 0) (size 1.397 1.397) (drill 0.999998) (layers *.Cu *.Mask)
      (net 831 "N72974574"))
  )
  (footprint "RES1608_1" (layer "F.Cu")
    (tedit 0)
    (at 114.431615 9.551002 180)
    (fp_text reference "ER11" (at -1.904975 -1.905025 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 180) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 912 "N85769464"))
    (pad "2" smd rect (at 0 0.7874 180) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "CAP1608_1" (layer "F.Cu")
    (tedit 0)
    (at -9.395392 99.451 90)
    (fp_text reference "C3" (at -0.635025 1.269975 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 90) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "+12V_BUS"))
    (pad "2" smd rect (at 0 0.7874 90) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at 148.086615 35.586002 90)
    (fp_text reference "AR35" (at -1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 945 "AICSN1"))
  )
  (footprint "TP089X043_1" (layer "F.Cu")
    (tedit 0)
    (at -22.495391 6.905008)
    (fp_text reference "TP68" (at -1.27 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 0.5588 0.5588) (drill 0.250012) (layers *.Cu *.Mask)
      (net 803 "DVPDATA_8"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -48.382385 8.154002 180)
    (fp_text reference "R8002" (at -2.2225 -2.54 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 800 "GENERICB"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 845 "GENERICB_R"))
  )
  (footprint "RES1608_1" (layer "F.Cu")
    (tedit 0)
    (at 156.468615 19.012502 180)
    (fp_text reference "ER309" (at -2.222475 -2.540025 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 180) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "2" smd rect (at 0 0.7874 180) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 83 "N86495804"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at 20.329619 56.246006 180)
    (fp_text reference "R116" (at -1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 679 "T1XCP"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 678 "T1XCM"))
  )
  (footprint "CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at 153.103115 39.904002 180)
    (fp_text reference "AC11" (at -1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 933 "AICSN35"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 936 "ACISP3"))
  )
  (footprint "RES1608_1" (layer "F.Cu")
    (tedit 0)
    (at 143.011187 31.522002 90)
    (fp_text reference "ER308" (at -2.540025 2.222475 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 90) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 907 "N85769402"))
    (pad "2" smd rect (at 0 0.7874 90) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 908 "N85769514"))
  )
  (footprint "GEOM0012_1" (layer "F.Cu")
    (tedit 0)
    (at 162.564615 47.143002 180)
    (fp_text reference "EB19" (at -1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 -2.500122 180) (size 1.905 1.905) (drill 1.143) (layers *.Cu *.Mask)
      (net 60 "+12V_EXT"))
    (pad "2" thru_hole circle (at 0 2.500122 180) (size 1.905 1.905) (drill 1.143) (layers *.Cu *.Mask)
      (net 865 "PWM2_VIN"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -35.69539 86.251001 -90)
    (fp_text reference "R1003" (at 2.54 -2.2225 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "A_DAC1_B"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "GEOM0013_1" (layer "F.Cu")
    (tedit 0)
    (at -11.853781 64.661204)
    (fp_text reference "C4001" (at 1.111516 1.27033 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144) (size 1.27 1.219987) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "+3.3V"))
    (pad "2" smd rect (at 0 0.9144) (size 1.27 1.219987) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1608_1" (layer "F.Cu")
    (tedit 0)
    (at 133.486187 60.351002 90)
    (fp_text reference "AR87" (at -1.905025 1.904975 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 90) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 868 "N86496210"))
    (pad "2" smd rect (at 0 0.7874 90) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 66 "UG1"))
  )
  (footprint "SOT23_3PIN_1" (layer "F.Cu")
    (tedit 0)
    (at -41.495378 39.350993 -90)
    (fp_text reference "Q2021" (at 1.4732 -1.289075 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.9398 1.143 270) (size 0.640004 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 860 "N21778115"))
    (pad "2" smd rect (at 0.9398 1.143 270) (size 0.640004 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 751 "HPD1"))
    (pad "3" smd rect (at 0 -1.143 270) (size 0.640004 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "+3.3V"))
  )
  (footprint "TP089X043_1" (layer "F.Cu")
    (tedit 0)
    (at -9.295392 49.550998)
    (fp_text reference "TP79" (at -1.27 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 0.5588 0.5588) (drill 0.250012) (layers *.Cu *.Mask)
      (net 801 "DVPDATA_19"))
  )
  (footprint "GEOM0012_1" (layer "F.Cu")
    (tedit 0)
    (at 162.564615 86.513002 180)
    (fp_text reference "EB18" (at -1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 -2.500122 180) (size 1.905 1.905) (drill 1.143) (layers *.Cu *.Mask)
      (net 60 "+12V_EXT"))
    (pad "2" thru_hole circle (at 0 2.500122 180) (size 1.905 1.905) (drill 1.143) (layers *.Cu *.Mask)
      (net 863 "PWM3_VIN"))
  )
  (footprint "CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at 78.871615 19.076002 90)
    (fp_text reference "C1034" (at -2.54 2.2225 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at 78.871615 20.092002 90)
    (fp_text reference "C1038" (at -2.54 2.2225 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "C1206_113_1" (layer "F.Cu")
    (tedit 0)
    (at 150.626615 6.503002 90)
    (fp_text reference "C1610" (at 0 -0.981075 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd oval (at -1.4351 0 90) (size 0.9779 1.1938) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "+12V_EXT"))
    (pad "2" smd oval (at 1.4351 0 90) (size 0.9779 1.1938) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at 83.951615 7.265002 90)
    (fp_text reference "R4005" (at -2.54 2.2225 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 839 "PWM"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 840 "N81403017"))
  )
  (footprint "C1206_113_1" (layer "F.Cu")
    (tedit 0)
    (at 107.065615 20.092002 90)
    (fp_text reference "EC159" (at 0 -0.981075 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd oval (at -1.4351 0 90) (size 0.9779 1.1938) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd oval (at 1.4351 0 90) (size 0.9779 1.1938) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -11.307783 61.361211)
    (fp_text reference "R4007" (at 2.2225 2.54 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 824 "TS_FDO"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 839 "PWM"))
  )
  (footprint "GEOM0013_1" (layer "F.Cu")
    (tedit 0)
    (at 87.507615 5.614002 180)
    (fp_text reference "TC4011" (at -1.058571 -1.323263 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144 180) (size 1.27 1.219987) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 856 "N73046901"))
    (pad "2" smd rect (at 0 0.9144 180) (size 1.27 1.219987) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -46.122395 10.751 -90)
    (fp_text reference "MR60" (at 1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 753 "DVALID"))
  )
  (footprint "GEOM0002_1" (layer "F.Cu")
    (tedit 0)
    (at 60.004622 14.151018 180)
    (fp_text reference "U401" (at -1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "A1" smd circle (at -4.399991 -6.399987 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "A2" smd circle (at -3.599993 -6.400013 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "A3" smd circle (at -2.799994 -6.400013 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "A4" smd circle (at -1.999996 -6.400013 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 338 "N48027789"))
    (pad "A9" smd circle (at 1.999996 -6.400013 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "A10" smd circle (at 2.799994 -6.400013 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "A11" smd circle (at 3.599993 -6.400013 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "A12" smd circle (at 4.399991 -6.399987 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "B1" smd circle (at -4.399991 -5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "B2" smd circle (at -3.599993 -5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 293 "DQC_15"))
    (pad "B3" smd circle (at -2.799994 -5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 294 "DQC_14"))
    (pad "B4" smd circle (at -1.999996 -5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "B9" smd circle (at 1.999996 -5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "B10" smd circle (at 2.799994 -5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 324 "DQC_21"))
    (pad "B11" smd circle (at 3.599993 -5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 323 "DQC_22"))
    (pad "B12" smd circle (at 4.399991 -5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "C1" smd circle (at -4.399991 -4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "C2" smd circle (at -3.599993 -4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 305 "DQC_13"))
    (pad "C3" smd circle (at -2.799994 -4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 316 "DQC_12"))
    (pad "C4" smd circle (at -1.999996 -4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "C9" smd circle (at 1.999996 -4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "C10" smd circle (at 2.799994 -4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 296 "DQC_20"))
    (pad "C11" smd circle (at 3.599993 -4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 295 "DQC_23"))
    (pad "C12" smd circle (at 4.399991 -4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "D1" smd circle (at -4.399991 -3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "D2" smd circle (at -3.599993 -3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 333 "QSCB_1"))
    (pad "D3" smd circle (at -2.799994 -3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 325 "QSC_1"))
    (pad "D4" smd circle (at -1.999996 -3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "D9" smd circle (at 1.999996 -3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "D10" smd circle (at 2.799994 -3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 326 "QSC_2"))
    (pad "D11" smd circle (at 3.599993 -3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 334 "QSCB_2"))
    (pad "D12" smd circle (at 4.399991 -3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "E1" smd circle (at -4.399991 -3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "E2" smd circle (at -3.599993 -3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 319 "DQC_11"))
    (pad "E3" smd circle (at -2.799994 -3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 289 "DQMCB_1"))
    (pad "E4" smd circle (at -1.999996 -3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "E9" smd circle (at 1.999996 -3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "E10" smd circle (at 2.799994 -3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 290 "DQMCB_2"))
    (pad "E11" smd circle (at 3.599993 -3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 297 "DQC_19"))
    (pad "E12" smd circle (at 4.399991 -3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "F1" smd circle (at -4.399991 -2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "F2" smd circle (at -3.599993 -2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 321 "DQC_9"))
    (pad "F3" smd circle (at -2.799994 -2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 320 "DQC_10"))
    (pad "F4" smd circle (at -1.999996 -2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 286 "CSC0B_0"))
    (pad "F9" smd circle (at 1.999996 -2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 288 "CASC0B"))
    (pad "F10" smd circle (at 2.799994 -2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 298 "DQC_18"))
    (pad "F11" smd circle (at 3.599993 -2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 299 "DQC_16"))
    (pad "F12" smd circle (at 4.399991 -2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "G1" smd circle (at -4.399991 -1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "G2" smd circle (at -3.599993 -1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "G3" smd circle (at -2.799994 -1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 322 "DQC_8"))
    (pad "G4" smd circle (at -1.999996 -1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 224 "MAC_BA1"))
    (pad "G9" smd circle (at 1.999996 -1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 225 "MAC_BA0"))
    (pad "G10" smd circle (at 2.799994 -1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 300 "DQC_17"))
    (pad "G11" smd circle (at 3.599993 -1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "G12" smd circle (at 4.399991 -1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "H1" smd circle (at -4.399991 -0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 331 "N48027750"))
    (pad "H2" smd circle (at -3.599993 -0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 213 "MAC_5"))
    (pad "H3" smd circle (at -2.799994 -0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 272 "MAC_BA2"))
    (pad "H4" smd circle (at -1.999996 -0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 285 "WEC0B"))
    (pad "H9" smd circle (at 1.999996 -0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 337 "CKEC0"))
    (pad "H10" smd circle (at 2.799994 -0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 283 "RASC0B"))
    (pad "H11" smd circle (at 3.599993 -0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 219 "MAC_1"))
    (pad "H12" smd circle (at 4.399991 -0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 332 "N48027731"))
    (pad "J1" smd circle (at -4.399991 0 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "J2" smd circle (at -3.599993 0 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "J3" smd circle (at -2.799994 0 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "J4" smd circle (at -1.999996 0 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "J9" smd circle (at 1.999996 0 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "J10" smd circle (at 2.799994 0 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 287 "CLKC0B"))
    (pad "J11" smd circle (at 3.599993 0 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 284 "CLKC0"))
    (pad "J12" smd circle (at 4.399991 0 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "K1" smd circle (at -4.399991 0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 329 "N48027732"))
    (pad "K2" smd circle (at -3.599993 0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 214 "MAC_8"))
    (pad "K3" smd circle (at -2.799994 0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 216 "MAC_6"))
    (pad "K4" smd circle (at -1.999996 0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 212 "MAC_4"))
    (pad "K9" smd circle (at 1.999996 0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 218 "MAC_0"))
    (pad "K10" smd circle (at 2.799994 0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 220 "MAC_2"))
    (pad "K11" smd circle (at 3.599993 0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 222 "MAC_10"))
    (pad "K12" smd circle (at 4.399991 0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 330 "N48027790"))
    (pad "L1" smd circle (at -4.399991 1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "L2" smd circle (at -3.599993 1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "L3" smd circle (at -2.799994 1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 311 "DQC_6"))
    (pad "L4" smd circle (at -1.999996 1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 215 "MAC_7"))
    (pad "L9" smd circle (at 1.999996 1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 221 "MAC_11"))
    (pad "L10" smd circle (at 2.799994 1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 302 "DQC_27"))
    (pad "L11" smd circle (at 3.599993 1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "L12" smd circle (at 4.399991 1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "M1" smd circle (at -4.399991 2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "M2" smd circle (at -3.599993 2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 310 "DQC_5"))
    (pad "M3" smd circle (at -2.799994 2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 313 "DQC_7"))
    (pad "M4" smd circle (at -1.999996 2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 217 "MAC_9"))
    (pad "M9" smd circle (at 1.999996 2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 223 "MAC_3"))
    (pad "M10" smd circle (at 2.799994 2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 304 "DQC_25"))
    (pad "M11" smd circle (at 3.599993 2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 301 "DQC_26"))
    (pad "M12" smd circle (at 4.399991 2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "N1" smd circle (at -4.399991 3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "N2" smd circle (at -3.599993 3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 312 "DQC_4"))
    (pad "N3" smd circle (at -2.799994 3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 292 "DQMCB_0"))
    (pad "N4" smd circle (at -1.999996 3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "N9" smd circle (at 1.999996 3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "N10" smd circle (at 2.799994 3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 291 "DQMCB_3"))
    (pad "N11" smd circle (at 3.599993 3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 303 "DQC_24"))
    (pad "N12" smd circle (at 4.399991 3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "P1" smd circle (at -4.399991 3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "P2" smd circle (at -3.599993 3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 336 "QSCB_0"))
    (pad "P3" smd circle (at -2.799994 3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 328 "QSC_0"))
    (pad "P4" smd circle (at -1.999996 3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "P9" smd circle (at 1.999996 3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "P10" smd circle (at 2.799994 3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 327 "QSC_3"))
    (pad "P11" smd circle (at 3.599993 3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 335 "QSCB_3"))
    (pad "P12" smd circle (at 4.399991 3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "R1" smd circle (at -4.399991 4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "R2" smd circle (at -3.599993 4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 314 "DQC_3"))
    (pad "R3" smd circle (at -2.799994 4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 315 "DQC_1"))
    (pad "R4" smd circle (at -1.999996 4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "R9" smd circle (at 1.999996 4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "R10" smd circle (at 2.799994 4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 307 "DQC_30"))
    (pad "R11" smd circle (at 3.599993 4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 306 "DQC_28"))
    (pad "R12" smd circle (at 4.399991 4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "T1" smd circle (at -4.399991 5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "T2" smd circle (at -3.599993 5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 317 "DQC_2"))
    (pad "T3" smd circle (at -2.799994 5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 318 "DQC_0"))
    (pad "T4" smd circle (at -1.999996 5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "T9" smd circle (at 1.999996 5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "T10" smd circle (at 2.799994 5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 309 "DQC_31"))
    (pad "T11" smd circle (at 3.599993 5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 308 "DQC_29"))
    (pad "T12" smd circle (at 4.399991 5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "V1" smd circle (at -4.399991 6.399987 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "V2" smd circle (at -3.599993 6.400013 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "V3" smd circle (at -2.799994 6.400013 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "V4" smd circle (at -1.999996 6.400013 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "V9" smd circle (at 1.999996 6.400013 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 144 "DRAM_RST"))
    (pad "V10" smd circle (at 2.799994 6.400013 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "V11" smd circle (at 3.599993 6.400013 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "V12" smd circle (at 4.399991 6.399987 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "TP089X043_1" (layer "F.Cu")
    (tedit 0)
    (at -21.195393 8.305005)
    (fp_text reference "TP65" (at -1.27 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 0.5588 0.5588) (drill 0.250012) (layers *.Cu *.Mask)
      (net 802 "DVPDATA_5"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at 153.039615 26.696002)
    (fp_text reference "AR22" (at 1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 919 "N86496570"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at 85.856615 5.614002)
    (fp_text reference "TR4011" (at 2.54 3.175 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "+12V_BUS"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 856 "N73046901"))
  )
  (footprint "TP055PRI_1" (layer "F.Cu")
    (tedit 0)
    (at 43.304605 83.151007)
    (fp_text reference "TP25" (at -1.27 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd circle (at 0 0) (size 0.550012 0.550012) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 762 "PETP14_GFXRP14"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -27.695355 10.251026 -90)
    (fp_text reference "MR53" (at 1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 789 "GPIO_3"))
  )
  (footprint "SOT23_3PIN_1" (layer "F.Cu")
    (tedit 0)
    (at -20.865371 76.13601)
    (fp_text reference "Q844" (at 1.38115 1.381125 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.9398 1.143) (size 0.640004 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "N87188969"))
    (pad "2" smd rect (at 0.9398 1.143) (size 0.640004 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "3" smd rect (at 0 -1.143) (size 0.640004 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 853 "LVT_EN"))
  )
  (footprint "RES1608_1" (layer "F.Cu")
    (tedit 0)
    (at 157.992615 76.099002 90)
    (fp_text reference "AR70" (at -1.905025 1.904975 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 90) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "+12V_EXT"))
    (pad "2" smd rect (at 0 0.7874 90) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 918 "N86494866"))
  )
  (footprint "RES1608_1" (layer "F.Cu")
    (tedit 0)
    (at 115.320615 6.884002 90)
    (fp_text reference "ER12" (at -1.905025 1.904975 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 90) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.7874 90) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 911 "N85769434"))
  )
  (footprint "C1206_113_1" (layer "F.Cu")
    (tedit 0)
    (at 104.271615 91.339002)
    (fp_text reference "EC348" (at -0.981075 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd oval (at -1.4351 0) (size 0.9779 1.1938) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd oval (at 1.4351 0) (size 0.9779 1.1938) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1608_1" (layer "F.Cu")
    (tedit 0)
    (at 148.467615 5.868002 180)
    (fp_text reference "C1608" (at -2.222475 -2.540025 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 180) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "+12V_EXT"))
    (pad "2" smd rect (at 0 0.7874 180) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -9.107787 61.361211 180)
    (fp_text reference "R4004" (at -2.2225 -2.54 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "+3.3V"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 78 "LM63_PWM"))
  )
  (footprint "CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at 100.842615 11.964002 90)
    (fp_text reference "C4030" (at -2.54 2.2225 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 832 "TACH"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "DPAKSGD_1" (layer "F.Cu")
    (tedit 0)
    (at 137.677187 45.492002 -90)
    (fp_text reference "MQ1306" (at 2.416175 -2.54 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "D" smd rect (at 0 -3.7465 270) (size 5.6896 5.6388) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 865 "PWM2_VIN"))
    (pad "G" smd oval (at -2.286 3.7465 270) (size 1.651 2.6797) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 866 "N86494416"))
    (pad "S" smd oval (at 2.286 3.7465 270) (size 1.651 2.6797) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 68 "APHASE_2"))
  )
  (footprint "RES1608_1" (layer "F.Cu")
    (tedit 0)
    (at 133.486187 80.036002 90)
    (fp_text reference "AR90" (at -1.905025 1.904975 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 90) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 864 "N86495503"))
    (pad "2" smd rect (at 0 0.7874 90) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 599 "UG3"))
  )
  (footprint "C1206_113_1" (layer "F.Cu")
    (tedit 0)
    (at 107.065615 65.304002 -90)
    (fp_text reference "EC1151" (at 0 0.981075 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd oval (at -1.4351 0 270) (size 0.9779 1.1938) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd oval (at 1.4351 0 270) (size 0.9779 1.1938) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "TP089X043_1" (layer "F.Cu")
    (tedit 0)
    (at -17.395376 6.905008)
    (fp_text reference "TP62" (at -1.27 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 0.5588 0.5588) (drill 0.250012) (layers *.Cu *.Mask)
      (net 815 "DVPDATA_2"))
  )
  (footprint "RES1608_1" (layer "F.Cu")
    (tedit 0)
    (at -44.595397 39.050994 180)
    (fp_text reference "R2022" (at -2.222475 -2.540025 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 180) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 860 "N21778115"))
    (pad "2" smd rect (at 0 0.7874 180) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 905 "HPD_DVI1"))
  )
  (footprint "TP089X043_1" (layer "F.Cu")
    (tedit 0)
    (at -23.795388 6.905008)
    (fp_text reference "TP70" (at -1.27 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 0.5588 0.5588) (drill 0.250012) (layers *.Cu *.Mask)
      (net 797 "DVPDATA_10"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at 20.204625 58.851005)
    (fp_text reference "R111" (at 1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 685 "T1X1M"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 686 "T1X1P"))
  )
  (footprint "560UF_4V_R71D55_1" (layer "F.Cu")
    (tedit 0)
    (at 151.388615 87.910002 -90)
    (fp_text reference "C1607" (at 0 1.36398 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole rect (at -1.75006 0 270) (size 1.8034 1.8034) (drill 1.397) (layers *.Cu *.Mask)
      (net 863 "PWM3_VIN"))
    (pad "2" thru_hole circle (at 1.75006 0 270) (size 1.8034 1.8034) (drill 1.397) (layers *.Cu *.Mask)
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at 148.086615 34.443002 -90)
    (fp_text reference "AR81" (at 1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 925 "N86495210"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "560UF_4V_R71D55_1" (layer "F.Cu")
    (tedit 0)
    (at 112.653615 57.404602 180)
    (fp_text reference "EC1153" (at 1.346835 0.005715 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole rect (at -1.75006 0 180) (size 1.8034 1.8034) (drill 1.397) (layers *.Cu *.Mask)
      (net 735 "+VDDC"))
    (pad "2" thru_hole circle (at 1.75006 0 180) (size 1.8034 1.8034) (drill 1.397) (layers *.Cu *.Mask)
      (net 4 "GND"))
  )
  (footprint "TP055PRI_1" (layer "F.Cu")
    (tedit 0)
    (at 45.604625 84.151005)
    (fp_text reference "TP28" (at -1.27 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd circle (at 0 0) (size 0.550012 0.550012) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 724 "PETN15_GFXRN15"))
  )
  (footprint "CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -10.253785 64.661306)
    (fp_text reference "C4002" (at 2.2225 2.54 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "+3.3V"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at 21.104624 60.051003)
    (fp_text reference "R112" (at 1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 687 "T1X2M"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 688 "T1X2P"))
  )
  (footprint "TP055PRI_1" (layer "F.Cu")
    (tedit 0)
    (at 26.404613 84.151005)
    (fp_text reference "TP12" (at -1.27 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd circle (at 0 0) (size 0.550012 0.550012) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 625 "PETN3_GFXRN3"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -33.595394 60.551002 180)
    (fp_text reference "R3002" (at -2.2225 -2.54 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 668 "A_DAC2_C"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "C1206_113_1" (layer "F.Cu")
    (tedit 0)
    (at 137.423187 13.361002 180)
    (fp_text reference "EC182" (at 0.981075 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd oval (at -1.4351 0 180) (size 0.9779 1.1938) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 62 "N85769539"))
    (pad "2" smd oval (at 1.4351 0 180) (size 0.9779 1.1938) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -40.995379 55.251012)
    (fp_text reference "R3009" (at 2.2225 2.54 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 847 "PIN6"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 754 "GENERICA"))
  )
  (footprint "TP055PRI_1" (layer "F.Cu")
    (tedit 0)
    (at 36.004619 84.151005)
    (fp_text reference "TP20" (at -1.27 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd circle (at 0 0) (size 0.550012 0.550012) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 609 "PETN9_GFXRN9"))
  )
  (footprint "GEOM0007_1" (layer "F.Cu")
    (tedit 0)
    (at 122.686615 82.576002 90)
    (fp_text reference "L65" (at -1.27 1.5875 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 4.500118 90) (size 3.81 3.81) (drill 2.413) (layers *.Cu *.Mask)
      (net 598 "APHASE_3"))
    (pad "2" thru_hole circle (at 0 -4.500118 90) (size 3.81 3.81) (drill 2.413) (layers *.Cu *.Mask)
      (net 735 "+VDDC"))
  )
  (footprint "CAP1608_1" (layer "F.Cu")
    (tedit 0)
    (at -35.095391 60.551002 180)
    (fp_text reference "C3002" (at -2.222475 -2.540025 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 180) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 668 "A_DAC2_C"))
    (pad "2" smd rect (at 0 0.7874 180) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1608_1" (layer "F.Cu")
    (tedit 0)
    (at -42.695376 85.751002 90)
    (fp_text reference "C1010" (at -2.540025 2.222475 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 90) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "+5V_VESA"))
    (pad "2" smd rect (at 0 0.7874 90) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -10.105398 73.386003 180)
    (fp_text reference "C82" (at -1.5875 -1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "XTALIN"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -9.973394 85.386004)
    (fp_text reference "C83" (at 1.5875 1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "XTALOUT"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "C1206_113_1" (layer "F.Cu")
    (tedit 0)
    (at 144.594115 13.361002)
    (fp_text reference "EC181" (at -0.981075 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd oval (at -1.4351 0) (size 0.9779 1.1938) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 62 "N85769539"))
    (pad "2" smd oval (at 1.4351 0) (size 0.9779 1.1938) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1608_1" (layer "F.Cu")
    (tedit 0)
    (at 123.321615 11.583002 90)
    (fp_text reference "EC124" (at -2.540025 2.222475 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 90) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 58 "N85769340"))
    (pad "2" smd rect (at 0 0.7874 90) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 915 "N85769214"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at 100.842615 8.535002 90)
    (fp_text reference "R4035" (at -2.54 2.2225 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 830 "N49971242"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 834 "N49971220"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -10.207785 61.361211)
    (fp_text reference "R4006" (at 2.2225 2.54 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 78 "LM63_PWM"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 839 "PWM"))
  )
  (footprint "RES1608_1" (layer "F.Cu")
    (tedit 0)
    (at -44.595397 82.751008)
    (fp_text reference "R1022" (at 2.222475 2.540025 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 861 "N26590941"))
    (pad "2" smd rect (at 0 0.7874) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 906 "HPD_DVI2"))
  )
  (footprint "CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at 157.230615 61.875002 -90)
    (fp_text reference "AC25" (at 1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "+12V_EXT"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at 159.389615 39.904002)
    (fp_text reference "AR27" (at 1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 934 "ACISP1"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "APHASE_1"))
  )
  (footprint "CAP1608_1" (layer "F.Cu")
    (tedit 0)
    (at -35.095391 67.751013 180)
    (fp_text reference "C3001" (at -2.222475 -2.540025 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 180) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 651 "A_DAC2_Y"))
    (pad "2" smd rect (at 0 0.7874 180) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -2.098784 40.247613 -135)
    (fp_text reference "R295" (at 0 -2.694077 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 225) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 225) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 144 "DRAM_RST"))
  )
  (footprint "CAP1608_1" (layer "F.Cu")
    (tedit 0)
    (at -40.69538 67.751013)
    (fp_text reference "C3004" (at 2.222475 2.540025 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 904 "DAC2_Y_F"))
    (pad "2" smd rect (at 0 0.7874) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -33.595394 67.651013 180)
    (fp_text reference "R3001" (at -2.2225 -2.54 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 651 "A_DAC2_Y"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at 104.271615 95.149002 90)
    (fp_text reference "C1039" (at -2.54 2.2225 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "SOT23_3PIN_1" (layer "F.Cu")
    (tedit 0)
    (at -25.695384 76.650995 180)
    (fp_text reference "Q843" (at -1.38115 -1.381125 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.9398 1.143 180) (size 0.640004 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 854 "N87188971"))
    (pad "2" smd rect (at 0.9398 1.143 180) (size 0.640004 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "3" smd rect (at 0 -1.143 180) (size 0.640004 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "N87188969"))
  )
  (footprint "TP055PRI_1" (layer "F.Cu")
    (tedit 0)
    (at 29.604607 83.151007)
    (fp_text reference "TP14" (at -1.27 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd circle (at 0 0) (size 0.550012 0.550012) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 629 "PETN5_GFXRN5"))
  )
  (footprint "TP089X043_1" (layer "F.Cu")
    (tedit 0)
    (at -25.095386 6.905008)
    (fp_text reference "TP71" (at -1.27 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 0.5588 0.5588) (drill 0.250012) (layers *.Cu *.Mask)
      (net 810 "DVPDATA_11"))
  )
  (footprint "NET_SHORT_1" (layer "F.Cu")
    (tedit 0)
    (at 23.749627 78.366003)
    (fp_text reference "NS1021" (at -1.905 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 0.550012 0.550012) (drill 0.250012) (layers *.Cu *.Mask)
      (net 4 "GND"))
    (pad "2" smd circle (at 0.2 0) (size 0.127 0.127) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 617 "GND_VSS1DI"))
  )
  (footprint "R0805_67_1" (layer "F.Cu")
    (tedit 0)
    (at 119.638615 11.583002)
    (fp_text reference "ER1596" (at -1.905 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd oval (at -0.8509 0) (size 0.7747 0.9906) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 59 "N85769021"))
    (pad "2" smd oval (at 0.8509 0) (size 0.7747 0.9906) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 58 "N85769340"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at 100.842615 9.678002 90)
    (fp_text reference "R4034" (at -2.54 2.2225 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 832 "TACH"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 834 "N49971220"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -23.295389 75.096007 180)
    (fp_text reference "R849" (at -1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "+12V_BUS"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 853 "LVT_EN"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -18.580387 73.170992 180)
    (fp_text reference "R840" (at -1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "+3.3V"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "C1206_113_1" (layer "F.Cu")
    (tedit 0)
    (at 145.927615 62.637002 90)
    (fp_text reference "C1583" (at 0 -0.981075 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd oval (at -1.4351 0 90) (size 0.9779 1.1938) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 867 "PWM1_VIN"))
    (pad "2" smd oval (at 1.4351 0 90) (size 0.9779 1.1938) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "SOT23_3PIN_1" (layer "F.Cu")
    (tedit 0)
    (at 157.992615 79.274002 180)
    (fp_text reference "ED28" (at -1.38115 -1.381125 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.9398 1.143 180) (size 0.640004 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 918 "N86494866"))
    (pad "2" smd rect (at 0.9398 1.143 180) (size 0.640004 1.27) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "3" smd rect (at 0 -1.143 180) (size 0.640004 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 600 "N86495166"))
  )
  (footprint "SOT23_3PIN_1" (layer "F.Cu")
    (tedit 0)
    (at 151.515615 56.515602 -90)
    (fp_text reference "ED29" (at 1.381125 -1.38115 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.9398 1.143 270) (size 0.640004 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 917 "N86495162"))
    (pad "2" smd rect (at 0.9398 1.143 270) (size 0.640004 1.27) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "3" smd rect (at 0 -1.143 270) (size 0.640004 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 65 "BOOT1"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -28.695353 10.251026 90)
    (fp_text reference "R53" (at -1.27 1.5875 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "+3.3V"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 789 "GPIO_3"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -34.195393 91.250991)
    (fp_text reference "R1028" (at 2.2225 2.54 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 648 "A_DAC1_GB"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -46.595393 11.250999 180)
    (fp_text reference "R60" (at -1.5875 -1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "+3.3V"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 753 "DVALID"))
  )
  (footprint "560UF_4V_R71D55_1" (layer "F.Cu")
    (tedit 0)
    (at 149.107187 18.568002 -90)
    (fp_text reference "EC108" (at 0 1.36398 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole rect (at -1.75006 0 270) (size 1.8034 1.8034) (drill 1.397) (layers *.Cu *.Mask)
      (net 62 "N85769539"))
    (pad "2" thru_hole circle (at 1.75006 0 270) (size 1.8034 1.8034) (drill 1.397) (layers *.Cu *.Mask)
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -1.395382 68.95101 180)
    (fp_text reference "R41" (at -1.5875 -1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "+3.3V"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 756 "DDC3CLK"))
  )
  (footprint "560UF_4V_R71D55_1" (layer "F.Cu")
    (tedit 0)
    (at 112.653615 88.164002 180)
    (fp_text reference "EC1161" (at 1.346835 0.005715 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole rect (at -1.75006 0 180) (size 1.8034 1.8034) (drill 1.397) (layers *.Cu *.Mask)
      (net 735 "+VDDC"))
    (pad "2" thru_hole circle (at 1.75006 0 180) (size 1.8034 1.8034) (drill 1.397) (layers *.Cu *.Mask)
      (net 4 "GND"))
  )
  (footprint "TP055PRI_1" (layer "F.Cu")
    (tedit 0)
    (at 38.404614 83.151007)
    (fp_text reference "TP21" (at -1.27 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd circle (at 0 0) (size 0.550012 0.550012) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 614 "PETP11_GFXRP11"))
  )
  (footprint "RES1608_1" (layer "F.Cu")
    (tedit 0)
    (at 153.801615 80.798002 90)
    (fp_text reference "AR88" (at -1.905025 1.904975 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 90) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 937 "N86494646"))
    (pad "2" smd rect (at 0 0.7874 90) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 600 "N86495166"))
  )
  (footprint "GEOM0011_1" (layer "F.Cu")
    (tedit 0)
    (at -58.055391 32.970996 -90)
    (fp_text reference "J2001" (at -7.532624 1.5875 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at -9.525 -9.652 270) (size 1.397 1.397) (drill 0.899998) (layers *.Cu *.Mask)
      (net 687 "T1X2M"))
    (pad "2" thru_hole circle (at -7.62 -9.652 270) (size 1.397 1.397) (drill 0.899998) (layers *.Cu *.Mask)
      (net 688 "T1X2P"))
    (pad "3" thru_hole circle (at -5.715 -9.652 270) (size 1.397 1.397) (drill 0.899998) (layers *.Cu *.Mask)
      (net 4 "GND"))
    (pad "4" thru_hole circle (at -3.81 -9.652 270) (size 1.397 1.397) (drill 0.899998) (layers *.Cu *.Mask)
      (net 692 "T1X4M"))
    (pad "5" thru_hole circle (at -1.905 -9.652 270) (size 1.397 1.397) (drill 0.899998) (layers *.Cu *.Mask)
      (net 691 "T1X4P"))
    (pad "6" thru_hole circle (at 0 -9.652 270) (size 1.397 1.397) (drill 0.899998) (layers *.Cu *.Mask)
      (net 50 "DDCCLK_DAC2_R"))
    (pad "7" thru_hole circle (at 1.905 -9.652 270) (size 1.397 1.397) (drill 0.899998) (layers *.Cu *.Mask)
      (net 52 "DDCDATA_DAC2_R"))
    (pad "8" thru_hole circle (at 3.81 -9.652 270) (size 1.397 1.397) (drill 0.899998) (layers *.Cu *.Mask)
      (net 51 "VSYNC_DAC2_R"))
    (pad "9" thru_hole circle (at -9.525 -7.747 270) (size 1.397 1.397) (drill 0.899998) (layers *.Cu *.Mask)
      (net 685 "T1X1M"))
    (pad "10" thru_hole circle (at -7.62 -7.747 270) (size 1.397 1.397) (drill 0.899998) (layers *.Cu *.Mask)
      (net 686 "T1X1P"))
    (pad "11" thru_hole circle (at -5.715 -7.747 270) (size 1.397 1.397) (drill 0.899998) (layers *.Cu *.Mask)
      (net 4 "GND"))
    (pad "12" thru_hole circle (at -3.81 -7.747 270) (size 1.397 1.397) (drill 0.899998) (layers *.Cu *.Mask)
      (net 666 "T1X3M"))
    (pad "13" thru_hole circle (at -1.905 -7.747 270) (size 1.397 1.397) (drill 0.899998) (layers *.Cu *.Mask)
      (net 670 "T1X3P"))
    (pad "14" thru_hole circle (at 0 -7.747 270) (size 1.397 1.397) (drill 0.899998) (layers *.Cu *.Mask)
      (net 11 "+5V_VESA"))
    (pad "15" thru_hole circle (at 1.905 -7.747 270) (size 1.397 1.397) (drill 0.899998) (layers *.Cu *.Mask)
      (net 4 "GND"))
    (pad "16" thru_hole circle (at 3.81 -7.747 270) (size 1.397 1.397) (drill 0.899998) (layers *.Cu *.Mask)
      (net 905 "HPD_DVI1"))
    (pad "17" thru_hole circle (at -9.525 -5.842 270) (size 1.397 1.397) (drill 0.899998) (layers *.Cu *.Mask)
      (net 683 "T1X0M"))
    (pad "18" thru_hole circle (at -7.62 -5.842 270) (size 1.397 1.397) (drill 0.899998) (layers *.Cu *.Mask)
      (net 684 "T1X0P"))
    (pad "19" thru_hole circle (at -5.715 -5.842 270) (size 1.397 1.397) (drill 0.899998) (layers *.Cu *.Mask)
      (net 4 "GND"))
    (pad "20" thru_hole circle (at -3.81 -5.842 270) (size 1.397 1.397) (drill 0.899998) (layers *.Cu *.Mask)
      (net 696 "T1X5M"))
    (pad "21" thru_hole circle (at -1.905 -5.842 270) (size 1.397 1.397) (drill 0.899998) (layers *.Cu *.Mask)
      (net 695 "T1X5P"))
    (pad "22" thru_hole circle (at 0 -5.842 270) (size 1.397 1.397) (drill 0.899998) (layers *.Cu *.Mask)
      (net 4 "GND"))
    (pad "23" thru_hole circle (at 1.905 -5.842 270) (size 1.397 1.397) (drill 0.899998) (layers *.Cu *.Mask)
      (net 679 "T1XCP"))
    (pad "24" thru_hole circle (at 3.81 -5.842 270) (size 1.397 1.397) (drill 0.899998) (layers *.Cu *.Mask)
      (net 678 "T1XCM"))
    (pad "25" thru_hole oval (at 15.364993 -4.572 270) (size 2.999994 4.000017) (drill 0.189992) (layers *.Cu *.Mask)
      (net 4 "GND"))
    (pad "26" thru_hole oval (at -15.364993 -4.572 270) (size 2.999994 4.000017) (drill 0.189992) (layers *.Cu *.Mask)
      (net 4 "GND"))
    (pad "27" thru_hole circle (at -3.799992 -11.700002 270) (size 1.519987 1.519987) (drill 1.099998) (layers *.Cu *.Mask)
      (net 4 "GND"))
    (pad "28" thru_hole circle (at 3.259988 -11.700002 270) (size 1.519987 1.519987) (drill 1.099998) (layers *.Cu *.Mask)
      (net 4 "GND"))
    (pad "29" thru_hole circle (at 13.499998 -11.700002 270) (size 1.519987 1.519987) (drill 1.099998) (layers *.Cu *.Mask)
      (net 4 "GND"))
    (pad "30" thru_hole circle (at -13.499998 -11.700002 270) (size 1.519987 1.519987) (drill 1.099998) (layers *.Cu *.Mask)
      (net 4 "GND"))
    (pad "C1" thru_hole circle (at 6.985 -9.019007 270) (size 1.143 1.143) (drill 0.650011) (layers *.Cu *.Mask)
      (net 42 "A_R_DAC2_F"))
    (pad "C2" thru_hole circle (at 9.525 -9.019007 270) (size 1.143 1.143) (drill 0.650011) (layers *.Cu *.Mask)
      (net 40 "A_G_DAC2_F"))
    (pad "C3" thru_hole circle (at 6.985 -6.479007 270) (size 1.143 1.143) (drill 0.650011) (layers *.Cu *.Mask)
      (net 38 "A_B_DAC2_F"))
    (pad "C4" thru_hole circle (at 9.525 -6.479007 270) (size 1.143 1.143) (drill 0.650011) (layers *.Cu *.Mask)
      (net 49 "HSYNC_DAC2_R"))
    (pad "C5" thru_hole circle (at 8.255 -10.292004 270) (size 1.143 1.143) (drill 0.650011) (layers *.Cu *.Mask)
      (net 4 "GND"))
    (pad "C6" thru_hole circle (at 8.255 -5.212004 270) (size 1.143 1.143) (drill 0.650011) (layers *.Cu *.Mask)
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at 85.204622 47.931012 180)
    (fp_text reference "R318" (at -1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 465 "N49337894"))
  )
  (footprint "RES1608_1" (layer "F.Cu")
    (tedit 0)
    (at 148.569215 56.363202)
    (fp_text reference "AR62" (at 1.904975 1.905025 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 917 "N86495162"))
    (pad "2" smd rect (at 0 0.7874) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "+12V_EXT"))
  )
  (footprint "DPAKSGD_1" (layer "F.Cu")
    (tedit 0)
    (at 137.677187 65.177002 -90)
    (fp_text reference "MQ1303" (at 2.416175 -2.54 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "D" smd rect (at 0 -3.7465 270) (size 5.6896 5.6388) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 867 "PWM1_VIN"))
    (pad "G" smd oval (at -2.286 3.7465 270) (size 1.651 2.6797) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 868 "N86496210"))
    (pad "S" smd oval (at 2.286 3.7465 270) (size 1.651 2.6797) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "APHASE_1"))
  )
  (footprint "SOT23_3PIN_1" (layer "F.Cu")
    (tedit 0)
    (at 89.158615 10.059002)
    (fp_text reference "TQ4011" (at 1.227697 1.534579 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.9398 1.143) (size 0.640004 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 855 "N73051201"))
    (pad "2" smd rect (at 0.9398 1.143) (size 0.640004 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "3" smd rect (at 0 -1.143) (size 0.640004 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 856 "N73046901"))
  )
  (footprint "GEOM0006_1" (layer "F.Cu")
    (tedit 0)
    (at -58.055391 32.970996 -90)
    (fp_text reference "MJ2001" (at -2.685898 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 3.81 -2.185899 270) (size 0.9652 0.9652) (drill 0.599999) (layers *.Cu *.Mask)
      (net 42 "A_R_DAC2_F"))
    (pad "2" thru_hole circle (at 1.524 -3.185897 270) (size 0.9652 0.9652) (drill 0.599999) (layers *.Cu *.Mask)
      (net 40 "A_G_DAC2_F"))
    (pad "3" thru_hole circle (at -0.762 -2.185899 270) (size 0.9652 0.9652) (drill 0.599999) (layers *.Cu *.Mask)
      (net 38 "A_B_DAC2_F"))
    (pad "4" thru_hole circle (at -3.048 -3.185897 270) (size 0.9652 0.9652) (drill 0.599999) (layers *.Cu *.Mask))
    (pad "5" thru_hole circle (at -5.334 -2.185899 270) (size 0.9652 0.9652) (drill 0.599999) (layers *.Cu *.Mask)
      (net 4 "GND"))
    (pad "6" thru_hole circle (at 5.334 -2.185899 270) (size 0.9652 0.9652) (drill 0.599999) (layers *.Cu *.Mask)
      (net 4 "GND"))
    (pad "7" thru_hole circle (at 3.048 -3.185897 270) (size 0.9652 0.9652) (drill 0.599999) (layers *.Cu *.Mask)
      (net 4 "GND"))
    (pad "8" thru_hole circle (at 0.762 -2.185899 270) (size 0.9652 0.9652) (drill 0.599999) (layers *.Cu *.Mask)
      (net 4 "GND"))
    (pad "9" thru_hole circle (at -1.524 -3.185897 270) (size 0.9652 0.9652) (drill 0.599999) (layers *.Cu *.Mask)
      (net 11 "+5V_VESA"))
    (pad "10" thru_hole circle (at -3.81 -2.185899 270) (size 0.9652 0.9652) (drill 0.599999) (layers *.Cu *.Mask)
      (net 4 "GND"))
    (pad "11" thru_hole circle (at 4.572 -3.185897 270) (size 0.9652 0.9652) (drill 0.599999) (layers *.Cu *.Mask))
    (pad "12" thru_hole circle (at 2.286 -2.185899 270) (size 0.9652 0.9652) (drill 0.599999) (layers *.Cu *.Mask)
      (net 52 "DDCDATA_DAC2_R"))
    (pad "13" thru_hole circle (at 0 -3.185897 270) (size 0.9652 0.9652) (drill 0.599999) (layers *.Cu *.Mask)
      (net 49 "HSYNC_DAC2_R"))
    (pad "14" thru_hole circle (at -2.286 -2.185899 270) (size 0.9652 0.9652) (drill 0.599999) (layers *.Cu *.Mask)
      (net 51 "VSYNC_DAC2_R"))
    (pad "15" thru_hole circle (at -4.572 -3.185897 270) (size 0.9652 0.9652) (drill 0.599999) (layers *.Cu *.Mask)
      (net 50 "DDCCLK_DAC2_R"))
    (pad "16" thru_hole oval (at 12.510008 -2.785897) (size 1.726997 2.736494) (drill 0.110007) (layers *.Cu *.Mask)
      (net 4 "GND"))
    (pad "17" thru_hole oval (at -12.510008 -2.785897) (size 1.726997 2.736494) (drill 0.110007) (layers *.Cu *.Mask)
      (net 4 "GND"))
  )
  (footprint "RES1608_1" (layer "F.Cu")
    (tedit 0)
    (at 150.499615 61.443202 -90)
    (fp_text reference "AR84" (at 1.905025 -1.904975 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 270) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 939 "N86494697"))
    (pad "2" smd rect (at 0 0.7874 270) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 65 "BOOT1"))
  )
  (footprint "GEOM0006_1" (layer "F.Cu")
    (tedit 0)
    (at -58.055391 86.761008 -90)
    (fp_text reference "MJ1001" (at -2.685898 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 3.81 -2.185899 270) (size 0.9652 0.9652) (drill 0.599999) (layers *.Cu *.Mask)
      (net 48 "A_R_DAC1_F"))
    (pad "2" thru_hole circle (at 1.524 -3.185897 270) (size 0.9652 0.9652) (drill 0.599999) (layers *.Cu *.Mask)
      (net 46 "A_G_DAC1_F"))
    (pad "3" thru_hole circle (at -0.762 -2.185899 270) (size 0.9652 0.9652) (drill 0.599999) (layers *.Cu *.Mask)
      (net 44 "A_B_DAC1_F"))
    (pad "4" thru_hole circle (at -3.048 -3.185897 270) (size 0.9652 0.9652) (drill 0.599999) (layers *.Cu *.Mask))
    (pad "5" thru_hole circle (at -5.334 -2.185899 270) (size 0.9652 0.9652) (drill 0.599999) (layers *.Cu *.Mask)
      (net 4 "GND"))
    (pad "6" thru_hole circle (at 5.334 -2.185899 270) (size 0.9652 0.9652) (drill 0.599999) (layers *.Cu *.Mask)
      (net 4 "GND"))
    (pad "7" thru_hole circle (at 3.048 -3.185897 270) (size 0.9652 0.9652) (drill 0.599999) (layers *.Cu *.Mask)
      (net 4 "GND"))
    (pad "8" thru_hole circle (at 0.762 -2.185899 270) (size 0.9652 0.9652) (drill 0.599999) (layers *.Cu *.Mask)
      (net 4 "GND"))
    (pad "9" thru_hole circle (at -1.524 -3.185897 270) (size 0.9652 0.9652) (drill 0.599999) (layers *.Cu *.Mask)
      (net 11 "+5V_VESA"))
    (pad "10" thru_hole circle (at -3.81 -2.185899 270) (size 0.9652 0.9652) (drill 0.599999) (layers *.Cu *.Mask)
      (net 4 "GND"))
    (pad "11" thru_hole circle (at 4.572 -3.185897 270) (size 0.9652 0.9652) (drill 0.599999) (layers *.Cu *.Mask))
    (pad "12" thru_hole circle (at 2.286 -2.185899 270) (size 0.9652 0.9652) (drill 0.599999) (layers *.Cu *.Mask)
      (net 56 "DDCDATA_DAC1_R"))
    (pad "13" thru_hole circle (at 0 -3.185897 270) (size 0.9652 0.9652) (drill 0.599999) (layers *.Cu *.Mask)
      (net 53 "HSYNC_DAC1_R"))
    (pad "14" thru_hole circle (at -2.286 -2.185899 270) (size 0.9652 0.9652) (drill 0.599999) (layers *.Cu *.Mask)
      (net 55 "VSYNC_DAC1_R"))
    (pad "15" thru_hole circle (at -4.572 -3.185897 270) (size 0.9652 0.9652) (drill 0.599999) (layers *.Cu *.Mask)
      (net 54 "DDCCLK_DAC1_R"))
    (pad "16" thru_hole oval (at 12.510008 -2.785897) (size 1.726997 2.736494) (drill 0.110007) (layers *.Cu *.Mask)
      (net 4 "GND"))
    (pad "17" thru_hole oval (at -12.510008 -2.785897) (size 1.726997 2.736494) (drill 0.110007) (layers *.Cu *.Mask)
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -42.395376 92.151015 -90)
    (fp_text reference "C1002" (at 2.54 -2.2225 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 46 "A_G_DAC1_F"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -17.755395 51.95841)
    (fp_text reference "R65" (at 1.5875 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "+3.3V"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 671 "GENERICC"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -10.19539 28.051016 -135)
    (fp_text reference "C554" (at 0 -2.694077 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 225) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 225) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 97.904622 86.751 -90)
    (fp_text reference "C215" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 98.90462 22.951001 90)
    (fp_text reference "C384" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 103.763615 44.222002 90)
    (fp_text reference "C1032" (at -2.54 2.2225 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 38.009949 59.635001)
    (fp_text reference "C186" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -9.295392 20.951005 180)
    (fp_text reference "R552" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 102 "CLKD1B"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "GEOM0013_1" (layer "B.Cu")
    (tedit 0)
    (at 41.304609 63.751554 -90)
    (fp_text reference "C1125" (at 1.27033 -1.111516 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144 270) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.9144 270) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 48.904619 41.650989 180)
    (fp_text reference "C965" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1608_1" (layer "B.Cu")
    (tedit 0)
    (at 86.60462 17.551011 -90)
    (fp_text reference "C379" (at 1.905025 -1.904975 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 270) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.7874 270) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 40.619621 46.23099 1.9)
    (fp_text reference "C150" (at 1.840792 1.967113 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 1.9) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 1.9) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -34.412385 56.033002)
    (fp_text reference "R78" (at 1.5875 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "+3.3V"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "VSYNC2"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 22.604621 70.251008 -90)
    (fp_text reference "C2030" (at 2.54 -2.2225 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 676 "+A2VDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 27.504611 68.151012 138.2)
    (fp_text reference "R2030" (at -3.349813 -0.412141 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 138.2) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 662 "R2SET"))
    (pad "2" smd rect (at 0 0.492608 138.2) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 767 "GND_A2VSSQ"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 90.404612 19.351008 -90)
    (fp_text reference "C386" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 403 "N49337708"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 24.504617 100.650998 180)
    (fp_text reference "C15" (at -1.5875 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 895 "PERP4"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 772 "GFXTP4_PERP4"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 36.604618 22.351002 90)
    (fp_text reference "C457" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 34.304623 21.851003 -90)
    (fp_text reference "C480" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 54.504608 100.650998 180)
    (fp_text reference "C30" (at -1.5875 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 872 "PERN11"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 638 "GFXTN11_PERN11"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -0.195385 50.950995 -90)
    (fp_text reference "R876" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "LDO6_VREF"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 8 "+5V"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 88.949624 26.846014 -90)
    (fp_text reference "C353" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 5.404604 57.351008)
    (fp_text reference "R875" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 17 "+VDDCI_LDO"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "LDO6_FB"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -7.595395 14.850991 45)
    (fp_text reference "C557" (at 0 2.694077 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 45) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 45) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 155.643115 39.904002)
    (fp_text reference "AR94" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 932 "AICSN24"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 935 "ACISP2"))
  )
  (footprint "CAP1608_1" (layer "B.Cu")
    (tedit 0)
    (at 54.404608 6.251009 90)
    (fp_text reference "C426" (at -1.905025 1.904975 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 90) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.7874 90) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 92.604608 58.151006 90)
    (fp_text reference "C287" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 530 "N25405167"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 23.35961 55.830996 90)
    (fp_text reference "C115" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 682 "+TXVDDR"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 42.654619 68.651011 180)
    (fp_text reference "C140" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1608_1" (layer "B.Cu")
    (tedit 0)
    (at 51.004615 76.350995 63.4)
    (fp_text reference "MC128" (at -1.276041 3.124555 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 63.4) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.7874 63.4) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 94.604604 41.550989 45)
    (fp_text reference "R301" (at 0 2.694077 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 45) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 411 "CLKB0"))
    (pad "2" smd rect (at 0 0.492608 45) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 7.704625 58.051007 90)
    (fp_text reference "C874" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 17 "+VDDCI_LDO"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 41.704608 20.551005)
    (fp_text reference "C473" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1608_1" (layer "B.Cu")
    (tedit 0)
    (at 61.504619 69.25101 127.4)
    (fp_text reference "MC127" (at -3.367711 0.222817 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 127.4) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.7874 127.4) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 37.504616 100.650998 180)
    (fp_text reference "C22" (at -1.5875 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 882 "PERN7"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 634 "GFXTN7_PERN7"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -39.619385 56.033002 180)
    (fp_text reference "R2010" (at -2.2225 -2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "HSYNC_DAC2_B"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 49 "HSYNC_DAC2_R"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -27.695355 10.251026 -90)
    (fp_text reference "MR55" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 787 "GPIO_5"))
  )
  (footprint "GEOM0013_1" (layer "B.Cu")
    (tedit 0)
    (at 51.004615 76.350995 63)
    (fp_text reference "C128" (at -0.528634 1.595759 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144 63) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.9144 63) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -6.091385 75.591002 90)
    (fp_text reference "C841" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 833 "N87189147"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 35.994459 59.670561)
    (fp_text reference "C177" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 42.604606 66.35099)
    (fp_text reference "C141" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 23.604619 7.751006 -90)
    (fp_text reference "C511" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 19.329621 50.920998)
    (fp_text reference "C96" (at 1.5875 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 680 "+VDDR_DVP"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 38.999787 59.650241 180)
    (fp_text reference "C948" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "GEOM0013_1" (layer "B.Cu")
    (tedit 0)
    (at 7.504625 54.851013 90)
    (fp_text reference "C872" (at -1.195476 1.181837 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144 90) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 17 "+VDDCI_LDO"))
    (pad "2" smd rect (at 0 0.9144 90) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 62.504617 100.650998 180)
    (fp_text reference "C34" (at -1.5875 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 874 "PERN13"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 745 "GFXTN13_PERN13"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 45.504626 100.650998 180)
    (fp_text reference "C25" (at -1.5875 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 900 "PERP9"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 742 "GFXTP9_PERP9"))
  )
  (footprint "SMIND1005_0_5H_1" (layer "B.Cu")
    (tedit 0)
    (at 16.304608 56.15101 -90)
    (fp_text reference "B69" (at 1.27 -1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 667 "+DPLL_PVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 22 "+1.8V"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 97.904622 60.951001)
    (fp_text reference "C263" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 5.504604 100.650998 180)
    (fp_text reference "C7" (at -1.27 -0.635 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 885 "PERP0"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 641 "GFXTP0_PERP0"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 90.274615 39.346015 90)
    (fp_text reference "C322" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "SMIND1005_0_5H_1" (layer "B.Cu")
    (tedit 0)
    (at 34.594614 40.090997 90)
    (fp_text reference "B123" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 737 "+VDDRHD"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -5.270381 23.471015 135)
    (fp_text reference "R557" (at -2.694077 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 135) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 103 "CASD1B"))
    (pad "2" smd rect (at 0 0.492608 135) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 59.904622 14.450992 90)
    (fp_text reference "C408" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 38.404614 21.851003)
    (fp_text reference "C460" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -2.29538 98.651002 -90)
    (fp_text reference "C6" (at 0.635 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 31 "+3.3V_BUS"))
  )
  (footprint "GEOM0008_1" (layer "B.Cu")
    (tedit 0)
    (at 23.204619 85.651002 -90)
    (fp_text reference "B920" (at 1.195476 -1.181837 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144 270) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 716 "+PCIE_VDDC"))
    (pad "2" smd rect (at 0 0.9144 270) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 27 "+1.1V"))
  )
  (footprint "CAP1608_1" (layer "B.Cu")
    (tedit 0)
    (at 34.504622 58.951005 180)
    (fp_text reference "MC1138" (at -2.539975 -3.175025 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 180) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.7874 180) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 96.204626 51.350995 90)
    (fp_text reference "C312" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 66.504609 13.450994 180)
    (fp_text reference "C433" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 331 "N48027750"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "CAP1608_1" (layer "B.Cu")
    (tedit 0)
    (at 100.904616 79.551014)
    (fp_text reference "C227" (at 1.904975 1.905025 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.7874) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 10.504619 100.650998 180)
    (fp_text reference "C9" (at -1.27 -0.635 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 886 "PERP1"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 643 "GFXTP1_PERP1"))
  )
  (footprint "DPAKSGD_1" (layer "B.Cu")
    (tedit 0)
    (at 138.820187 76.988002 90)
    (fp_text reference "MQ1310" (at -2.416175 2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "D" smd rect (at 0 -3.7465 90) (size 5.6896 5.6388) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 598 "APHASE_3"))
    (pad "G" smd oval (at 2.286 3.7465 90) (size 1.651 2.6797) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 597 "LG3"))
    (pad "S" smd oval (at -2.286 3.7465 90) (size 1.651 2.6797) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 17.64461 10.440993 180)
    (fp_text reference "C534" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "SMIND1005_0_5H_1" (layer "B.Cu")
    (tedit 0)
    (at 53.804609 11.650998 -90)
    (fp_text reference "B402" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 330 "N48027790"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -22.595391 34.351003 90)
    (fp_text reference "R58" (at -1.27 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "+3.3V"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 596 "GPIO_8_R"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 154.119115 39.904002 180)
    (fp_text reference "AC80" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 933 "AICSN35"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -31.280387 46.351005 180)
    (fp_text reference "R2003" (at -2.2225 -2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 37 "A_DAC2_B"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 38.413936 51.970678 90)
    (fp_text reference "C1111" (at -2.54 2.2225 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 45.008513 61.711248)
    (fp_text reference "C943" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 45.44773 51.980584 90)
    (fp_text reference "C914" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 36 "+VDDCI"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 58.404625 44.551008 180)
    (fp_text reference "R492" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 759 "MVREFD_C"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 46.504624 100.650998 180)
    (fp_text reference "C26" (at -1.5875 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 884 "PERN9"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 636 "GFXTN9_PERN9"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 96.204626 31.351009 90)
    (fp_text reference "C369" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 41.104609 15.351016 -90)
    (fp_text reference "R455" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 228 "WEC1B"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "RES1608_1" (layer "B.Cu")
    (tedit 0)
    (at 161.421615 24.156002 -90)
    (fp_text reference "ER18" (at 1.905025 -1.904975 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 270) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 852 "N86495698"))
    (pad "2" smd rect (at 0 0.7874 270) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "SOT23_3PIN_1" (layer "B.Cu")
    (tedit 0)
    (at 15.604609 62.250998 -90)
    (fp_text reference "Q100" (at 1.381125 -1.38115 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9398 1.143 270) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 853 "LVT_EN"))
    (pad "2" smd rect (at -0.9398 1.143 270) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 22 "+1.8V"))
    (pad "3" smd rect (at 0 -1.143 270) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 862 "N42099087"))
  )
  (footprint "GEOM0013_1" (layer "B.Cu")
    (tedit 0)
    (at 7.304626 67.251014 90)
    (fp_text reference "C862" (at -1.195476 1.181837 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144 90) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 22 "+1.8V"))
    (pad "2" smd rect (at 0 0.9144 90) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 26.104614 64.950993)
    (fp_text reference "C2026" (at 2.2225 2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 694 "+VDD2DI"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 693 "GND_VSS2DI"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -38.630385 35.426007 90)
    (fp_text reference "R2008" (at -2.54 2.2225 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 8 "+5V"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 841 "DDCCLK_DAC2_5V"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 43.604604 7.751006 -90)
    (fp_text reference "C465" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "DPAKSGD_1" (layer "B.Cu")
    (tedit 0)
    (at 138.820187 68.479002 90)
    (fp_text reference "MQ1305" (at -2.416175 2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "D" smd rect (at 0 -3.7465 90) (size 5.6896 5.6388) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 70 "APHASE_1"))
    (pad "G" smd oval (at 2.286 3.7465 90) (size 1.651 2.6797) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 69 "LG1"))
    (pad "S" smd oval (at -2.286 3.7465 90) (size 1.651 2.6797) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1608_1" (layer "B.Cu")
    (tedit 0)
    (at 34.459613 62.331008)
    (fp_text reference "MC183" (at 2.222475 2.540025 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.7874) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 6.504627 100.650998 180)
    (fp_text reference "C8" (at -1.27 -0.635 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 869 "PERN0"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 640 "GFXTN0_PERN0"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 88.039618 39.096003 -90)
    (fp_text reference "C320" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "SMIND1005_0_5H_1" (layer "B.Cu")
    (tedit 0)
    (at 95.104628 78.750991 180)
    (fp_text reference "B202" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 584 "N25405001"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 95.209606 36.596008 90)
    (fp_text reference "R322" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 459 "N49337758"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 91.50461 51.450994 -90)
    (fp_text reference "C331" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 458 "N49337065"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 85.804621 88.050997 90)
    (fp_text reference "C218" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1608_1" (layer "B.Cu")
    (tedit 0)
    (at 12.704615 20.600993)
    (fp_text reference "C527" (at 1.904975 1.905025 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.7874) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "GEOM0008_1" (layer "B.Cu")
    (tedit 0)
    (at 28.904608 80.351013 180)
    (fp_text reference "B900" (at -1.181837 -1.195476 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144 180) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 22 "+1.8V"))
    (pad "2" smd rect (at 0 0.9144 180) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 616 "+PCIE_VDDR"))
  )
  (footprint "DPAKSGD_1" (layer "B.Cu")
    (tedit 0)
    (at 138.820187 37.618002 90)
    (fp_text reference "MQ1307" (at -2.416175 2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "D" smd rect (at 0 -3.7465 90) (size 5.6896 5.6388) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 68 "APHASE_2"))
    (pad "G" smd oval (at 2.286 3.7465 90) (size 1.651 2.6797) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 67 "LG2"))
    (pad "S" smd oval (at -2.286 3.7465 90) (size 1.651 2.6797) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 29.404607 72.651003)
    (fp_text reference "C904" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 616 "+PCIE_VDDR"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 95.704601 86.751 -90)
    (fp_text reference "C214" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 94.009609 69.055988 180)
    (fp_text reference "C283" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 527 "N25405207"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "NET_SHORT_1" (layer "B.Cu")
    (tedit 0)
    (at 19.404627 66.851014)
    (fp_text reference "NS2021" (at -1.905 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 0.550012 0.550012) (drill 0.250012) (layers *.Cu *.Mask)
      (net 4 "GND"))
    (pad "2" smd circle (at -0.2 0) (size 0.127 0.127) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 693 "GND_VSS2DI"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 84.804623 21.751003)
    (fp_text reference "C365" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 85.304622 59.451004 180)
    (fp_text reference "C275" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 94.749612 83.046004 45)
    (fp_text reference "R202" (at 0 2.694077 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 45) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 541 "CLKA0B"))
    (pad "2" smd rect (at 0 0.492608 45) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 84.804623 81.75101)
    (fp_text reference "C206" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 96.704625 42.951011 90)
    (fp_text reference "C316" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 37.204617 14.550992 90)
    (fp_text reference "R456" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 226 "RASC1B"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 25.304615 64.950993)
    (fp_text reference "C2024" (at 2.2225 2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 694 "+VDD2DI"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 693 "GND_VSS2DI"))
  )
  (footprint "SMIND1005_0_5H_1" (layer "B.Cu")
    (tedit 0)
    (at 95.104628 58.751005 180)
    (fp_text reference "B252" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 528 "N25405099"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 33.604624 18.35101 -90)
    (fp_text reference "C464" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 43.504604 73.951 -90)
    (fp_text reference "R292" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 730 "MVREFD_A"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -16.405385 56.343593 180)
    (fp_text reference "MR71" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 657 "VID_1"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 21.01961 15.346012 -90)
    (fp_text reference "R505" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 158 "WED0B"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 57.704601 65.950991 180)
    (fp_text reference "R391" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 760 "MVREFD_B"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 45.004627 67.151014 180)
    (fp_text reference "C142" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 47.304622 49.450998 90)
    (fp_text reference "C963" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 58.504625 100.650998 180)
    (fp_text reference "C32" (at -1.5875 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 873 "PERN12"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 747 "GFXTN12_PERN12"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 40.014771 57.649991)
    (fp_text reference "C940" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "TP056X025_1" (layer "B.Cu")
    (tedit 0)
    (at 31.904627 66.050991)
    (fp_text reference "TP42" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 0.550012 0.550012) (drill 0.250012) (layers *.Cu *.Mask)
      (net 708 "PLL_TEST"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 37.804616 8.251005 180)
    (fp_text reference "C472" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "TP089X043_1" (layer "B.Cu")
    (tedit 0)
    (at -38.695384 8.851003)
    (fp_text reference "TP89" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 0.5588 0.5588) (drill 0.250012) (layers *.Cu *.Mask)
      (net 816 "DVP_MVP_CNTL_1"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -30.348385 63.272002 180)
    (fp_text reference "C839" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 8 "+5V"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 95.264623 26.061002 -90)
    (fp_text reference "C362" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 18.444609 18.421012)
    (fp_text reference "C510" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 22.90462 21.351004 180)
    (fp_text reference "C530" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -32.515386 35.735989 180)
    (fp_text reference "R2007" (at -2.2225 -2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 715 "DDC2CLK"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "+3.3V"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -6.395398 21.051004 135)
    (fp_text reference "C559" (at -2.694077 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 135) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 135) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -10.495389 25.350996 -135)
    (fp_text reference "C587" (at 0 -2.694077 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 225) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 149 "N48570109"))
    (pad "2" smd rect (at 0 0.492608 225) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 98.404621 91.450991 90)
    (fp_text reference "C202" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 34.604622 43.050986 180)
    (fp_text reference "C159" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 32.904625 64.750993)
    (fp_text reference "R7" (at 1.27 0.635 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 773 "TEST_EN"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -40.715395 14.161 180)
    (fp_text reference "MR56" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 664 "GPIO_6"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -29.280391 49.150999 180)
    (fp_text reference "R2002" (at -2.2225 -2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 39 "A_DAC2_G"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 25.504615 6.851007 90)
    (fp_text reference "C519" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 27.612231 64.101007 90)
    (fp_text reference "C63" (at -1.27 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 674 "+DPLL_VDDC"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 673 "GND_PVSS"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -2.195381 27.350992 45)
    (fp_text reference "C556" (at 0 2.694077 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 45) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 45) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 0.904613 24.16601 45)
    (fp_text reference "C575" (at 0 2.694077 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 45) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 45) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 38.993437 61.690852)
    (fp_text reference "C1116" (at 2.2225 2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "GEOM0013_1" (layer "B.Cu")
    (tedit 0)
    (at 15.00461 58.551006 180)
    (fp_text reference "C62" (at -1.323232 -1.058608 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144 180) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 674 "+DPLL_VDDC"))
    (pad "2" smd rect (at 0 0.9144 180) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 673 "GND_PVSS"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -12.355381 52.9436 180)
    (fp_text reference "MR62" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 778 "GPIO_12"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 50.504616 100.650998 180)
    (fp_text reference "C28" (at -1.5875 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 871 "PERN10"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 637 "GFXTN10_PERN10"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 85.804621 68.051012 90)
    (fp_text reference "C253" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 96.604625 29.551013 90)
    (fp_text reference "C374" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -39.295383 86.051001 -90)
    (fp_text reference "R1009" (at 2.54 -2.2225 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 843 "DDCCLK_DAC1_5V"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 54 "DDCCLK_DAC1_R"))
  )
  (footprint "GEOM0008_1" (layer "B.Cu")
    (tedit 0)
    (at 9.204622 48.251001 -90)
    (fp_text reference "B910" (at 1.195476 -1.181837 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144 270) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 36 "+VDDCI"))
    (pad "2" smd rect (at 0 0.9144 270) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 46.964618 40.246013 90)
    (fp_text reference "C122" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 758 "+VDDRHC"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 763 "GND_VSSRHC"))
  )
  (footprint "DPAKSGD_1" (layer "B.Cu")
    (tedit 0)
    (at 138.820187 57.303002 90)
    (fp_text reference "MQ1304" (at -2.416175 2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "D" smd rect (at 0 -3.7465 90) (size 5.6896 5.6388) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 70 "APHASE_1"))
    (pad "G" smd oval (at 2.286 3.7465 90) (size 1.651 2.6797) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 69 "LG1"))
    (pad "S" smd oval (at -2.286 3.7465 90) (size 1.651 2.6797) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 36.601062 66.402298)
    (fp_text reference "C922" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 716 "+PCIE_VDDC"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -36.550303 10.381074 90)
    (fp_text reference "MR51" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 788 "GPIO_1"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 67.204608 15.651015)
    (fp_text reference "C435" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 331 "N48027750"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 47.104622 41.951013 180)
    (fp_text reference "C157" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -0.995383 49.250999 180)
    (fp_text reference "C879" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "LDO6_VREF"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 13.504613 8.351004)
    (fp_text reference "C513" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 90.249621 79.341007 90)
    (fp_text reference "C225" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 51.092626 54.95561 90)
    (fp_text reference "C148" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "GEOM0001_1" (layer "B.Cu")
    (tedit 0)
    (at 1.004613 57.451008 -90)
    (fp_text reference "U871" (at 1.8923 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd oval (at 1.905 2.8448 270) (size 0.639978 1.579982) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "2" smd oval (at 0.635 2.8448 270) (size 0.639978 1.579982) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 19 "N87118008"))
    (pad "3" smd oval (at -0.635 2.8448 270) (size 0.639978 1.579982) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 18 "LDO6_VIN"))
    (pad "4" smd oval (at -1.905 2.8448 270) (size 0.639978 1.579982) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 8 "+5V"))
    (pad "5" smd oval (at -1.905 -2.8702 270) (size 0.639978 1.579982) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "LDO6_VREF"))
    (pad "6" smd oval (at -0.635 -2.8702 270) (size 0.639978 1.579982) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 17 "+VDDCI_LDO"))
    (pad "7" smd oval (at 0.635 -2.8702 270) (size 0.639978 1.579982) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "LDO6_FB"))
    (pad "8" smd oval (at 1.905 -2.8702 270) (size 0.639978 1.579982) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "9" smd rect (at 0 0 270) (size 4.099992 2.799994) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 97.904622 20.651005)
    (fp_text reference "C352" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 27.404611 13.450994 180)
    (fp_text reference "R520" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 204 "N48569889"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 56.504604 50.550996 180)
    (fp_text reference "C979" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -39.295383 90.950992 -90)
    (fp_text reference "R1006" (at 2.54 -2.2225 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 844 "DDCDATA_DAC1_5V"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 56 "DDCDATA_DAC1_R"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -17.755395 56.343593 180)
    (fp_text reference "MR70" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 707 "VID_0"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 95.704601 66.751015 -90)
    (fp_text reference "C257" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 94.414612 37.375991 90)
    (fp_text reference "C337" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 459 "N49337758"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "GEOM0013_1" (layer "B.Cu")
    (tedit 0)
    (at 34.460604 58.924005 180)
    (fp_text reference "C1138" (at -1.111516 -1.27033 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144 180) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.9144 180) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "SO8W_2_16H_1" (layer "B.Cu")
    (tedit 0)
    (at -23.668287 27.530798)
    (fp_text reference "U2" (at 1.27 0.635 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd oval (at 1.905 3.175) (size 0.639978 2.17998) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 593 "ROMCSB_R"))
    (pad "2" smd oval (at 0.635 3.175) (size 0.639978 2.17998) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 596 "GPIO_8_R"))
    (pad "3" smd oval (at -0.635 3.175) (size 0.639978 2.17998) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "+3.3V"))
    (pad "4" smd oval (at -1.905 3.175) (size 0.639978 2.17998) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "5" smd oval (at -1.905 -3.175) (size 0.639978 2.17998) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 595 "GPIO_9_R"))
    (pad "6" smd oval (at -0.635 -3.175) (size 0.639978 2.17998) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 594 "GPIO_10_R"))
    (pad "7" smd oval (at 0.635 -3.175) (size 0.639978 2.17998) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "+3.3V"))
    (pad "8" smd oval (at 1.905 -3.175) (size 0.639978 2.17998) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "+3.3V"))
  )
  (footprint "SOT23SGD_T_1" (layer "B.Cu")
    (tedit 0)
    (at 163.326615 27.077002 90)
    (fp_text reference "EQ107" (at -1.532001 1.347788 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "D" smd rect (at 0 -1.2065 90) (size 1.016 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 914 "N86494319"))
    (pad "G" smd rect (at 0.9525 1.2065 90) (size 1.016 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 851 "N86495700"))
    (pad "S" smd rect (at -0.9525 1.2065 90) (size 1.016 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "GEOM0008_1" (layer "B.Cu")
    (tedit 0)
    (at -32.780384 46.351005)
    (fp_text reference "L2003" (at 1.111516 1.27033 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 37 "A_DAC2_B"))
    (pad "2" smd rect (at 0 0.9144) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 38 "A_B_DAC2_F"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 91.83961 26.350994 180)
    (fp_text reference "R355" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 355 "WEB1B"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 92.518324 29.423606 135)
    (fp_text reference "C385" (at -2.694077 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 135) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 402 "N49338012"))
    (pad "2" smd rect (at 0 0.492608 135) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 22.304621 49.650998 90)
    (fp_text reference "R43" (at -1.27 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 22 "+1.8V"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 821 "VREFG"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 92.704607 85.051003)
    (fp_text reference "C222" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "TP089X043_1" (layer "B.Cu")
    (tedit 0)
    (at 28.604609 52.750992)
    (fp_text reference "TP88" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 0.5588 0.5588) (drill 0.250012) (layers *.Cu *.Mask)
      (net 817 "DVP_MVP_CNTL_0"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 33.904623 51.450994)
    (fp_text reference "C46" (at 1.5875 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 821 "VREFG"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 49.604617 48.751 90)
    (fp_text reference "C136" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 44.009709 59.655321)
    (fp_text reference "C161" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 97.404623 27.750991 -135)
    (fp_text reference "C373" (at 0 -2.694077 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 225) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 225) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "TO_261_1" (layer "B.Cu")
    (tedit 0)
    (at -33.777385 75.718002 90)
    (fp_text reference "U4" (at -0.508 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd circle (at 2.29997 3.124962 90) (size 1.016 1.016) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 81 "N87528545"))
    (pad "2" smd circle (at 0 3.124962 90) (size 1.016 1.016) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 8 "+5V"))
    (pad "3" smd circle (at -2.29997 3.124962 90) (size 1.016 1.016) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 33 "+12V_BUS"))
    (pad "4" smd rect (at 0 -3.124962 90) (size 3.302 1.524) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 8 "+5V"))
  )
  (footprint "CAP1608_1" (layer "B.Cu")
    (tedit 0)
    (at 100.904616 39.551018)
    (fp_text reference "C326" (at 1.904975 1.905025 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.7874) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 90.204612 24.356002)
    (fp_text reference "R357" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 358 "CASB1B"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 26.371593 48.151001)
    (fp_text reference "C151" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -11.005396 55.358403)
    (fp_text reference "R77" (at 1.5875 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "+3.3V"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 710 "VID_7"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 30.265616 67.925003 139.7)
    (fp_text reference "C900" (at -2.685018 -0.220749 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 139.7) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 616 "+PCIE_VDDR"))
    (pad "2" smd rect (at 0 0.492608 139.7) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 84.554611 43.346007 -90)
    (fp_text reference "C303" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 103.763615 45.238002 90)
    (fp_text reference "C1036" (at -2.54 2.2225 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 44.304603 10.551 180)
    (fp_text reference "C450" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 88.034614 79.116014 -90)
    (fp_text reference "C234" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -11.195388 26.050994 -135)
    (fp_text reference "R562" (at 0 -2.694077 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 225) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 149 "N48570109"))
    (pad "2" smd rect (at 0 0.492608 225) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 13.204614 16.751013)
    (fp_text reference "C536" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 205 "N48569804"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 13.204614 14.550992 180)
    (fp_text reference "C537" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 205 "N48569804"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -38.615374 36.536013 -90)
    (fp_text reference "R2009" (at 2.54 -2.2225 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 841 "DDCCLK_DAC2_5V"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 50 "DDCCLK_DAC2_R"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 58.204626 59.451004)
    (fp_text reference "C980" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "SMIND1005_0_5H_1" (layer "B.Cu")
    (tedit 0)
    (at 95.104628 38.750994 180)
    (fp_text reference "B302" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 457 "N49337896"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "RES3225_0_7H_1" (layer "B.Cu")
    (tedit 0)
    (at 8.504623 75.901009 -90)
    (fp_text reference "MR858" (at 1.76784 -1.54686 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -1.4478 270) (size 2.794 1.397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 1.4478 270) (size 2.794 1.397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 28 "LDO3_VIN"))
  )
  (footprint "CAP1608_1" (layer "B.Cu")
    (tedit 0)
    (at 63.104616 5.65101 -90)
    (fp_text reference "C427" (at 1.905025 -1.904975 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 270) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.7874 270) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 94.604604 81.55101 45)
    (fp_text reference "R201" (at 0 2.694077 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 45) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 538 "CLKA0"))
    (pad "2" smd rect (at 0 0.492608 45) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 16.104608 15.446012 -90)
    (fp_text reference "R506" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 156 "RASD0B"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 45.004881 53.649237 180)
    (fp_text reference "C1114" (at -2.2225 -2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1608_1" (layer "B.Cu")
    (tedit 0)
    (at 41.75462 50.650996 90)
    (fp_text reference "MC1136" (at -3.175025 2.539975 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 90) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.7874 90) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -5.945386 14.860999 -135)
    (fp_text reference "C558" (at 0 -2.694077 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 225) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 225) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -22.095392 20.851005 180)
    (fp_text reference "R54" (at -1.5875 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "+3.3V"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 791 "GPIO_4"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 39.904611 14.450992 90)
    (fp_text reference "C466" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1608_2012_1" (layer "B.Cu")
    (tedit 0)
    (at 10.10462 51.050995)
    (fp_text reference "MR910" (at 1.111516 1.27033 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 36 "+VDDCI"))
    (pad "2" smd rect (at 0 0.9144) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 17 "+VDDCI_LDO"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 93.704605 51.450994 -90)
    (fp_text reference "R319" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 458 "N49337065"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -5.825396 12.126003 -135)
    (fp_text reference "C567" (at 0 -2.694077 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 225) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 225) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 48.804619 53.350991 38.6)
    (fp_text reference "C66" (at 0.448337 1.98294 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 38.6) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 731 "+MPVDD"))
    (pad "2" smd rect (at 0 0.492608 38.6) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 732 "GND_MPVSS"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 5.404604 59.551004)
    (fp_text reference "R874" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "LDO6_FB"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 12.249625 16.746009 180)
    (fp_text reference "C525" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -4.895375 20.851005 -45)
    (fp_text reference "R555" (at 2.694077 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 315) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 100 "WED1B"))
    (pad "2" smd rect (at 0 0.492608 315) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 46.464619 14.320995)
    (fp_text reference "C483" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 275 "N48027848"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 92.704607 45.051007)
    (fp_text reference "C306" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 31.204603 71.651005)
    (fp_text reference "C906" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 616 "+PCIE_VDDR"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 56.904628 65.950991 180)
    (fp_text reference "C391" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 760 "MVREFD_B"))
  )
  (footprint "CAP1608_1" (layer "B.Cu")
    (tedit 0)
    (at -15.795379 22.851001 45)
    (fp_text reference "C578" (at -0.000035 2.694077 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 45) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.7874 45) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1608_1" (layer "B.Cu")
    (tedit 0)
    (at 47.384607 51.955997 180)
    (fp_text reference "C918" (at -1.904975 -1.905025 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 180) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 36 "+VDDCI"))
    (pad "2" smd rect (at 0 0.7874 180) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 53.704609 8.251005 90)
    (fp_text reference "C405" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 100.304618 70.651007)
    (fp_text reference "C254" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 18.504629 20.626012)
    (fp_text reference "C512" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "DPAKSGD_1" (layer "B.Cu")
    (tedit 0)
    (at 138.820187 88.164002 90)
    (fp_text reference "MQ1311" (at -2.416175 2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "D" smd rect (at 0 -3.7465 90) (size 5.6896 5.6388) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 598 "APHASE_3"))
    (pad "G" smd oval (at 2.286 3.7465 90) (size 1.651 2.6797) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 597 "LG3"))
    (pad "S" smd oval (at -2.286 3.7465 90) (size 1.651 2.6797) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 8.404624 80.251013)
    (fp_text reference "C858" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 8 "+5V"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 61.504619 100.650998 180)
    (fp_text reference "C33" (at -1.5875 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 890 "PERP13"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 748 "GFXTP13_PERP13"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -6.595372 29.050988 45)
    (fp_text reference "C563" (at 0 2.694077 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 45) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 45) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -38.222385 67.082002)
    (fp_text reference "R1011" (at 2.2225 2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "VSYNC_DAC1_B"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 55 "VSYNC_DAC1_R"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -47.905373 10.575994 180)
    (fp_text reference "R56" (at -1.5875 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "+3.3V"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 664 "GPIO_6"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 66.20461 10.950999 180)
    (fp_text reference "C418" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 58.204626 63.950995)
    (fp_text reference "R393" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 755 "MVREFS_B"))
  )
  (footprint "RES1608_1" (layer "B.Cu")
    (tedit 0)
    (at 121.289615 8.916002 180)
    (fp_text reference "ER10" (at -1.904975 -1.905025 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 180) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 59 "N85769021"))
    (pad "2" smd rect (at 0 0.7874 180) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 913 "N85769062"))
  )
  (footprint "TP089X043_1" (layer "B.Cu")
    (tedit 0)
    (at 26.794605 51.610989)
    (fp_text reference "TP76" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 0.5588 0.5588) (drill 0.250012) (layers *.Cu *.Mask)
      (net 829 "DVPDATA_16"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 48.93962 50.785997 180)
    (fp_text reference "C960" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 87.004619 70.151008 -45)
    (fp_text reference "C264" (at 2.694077 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 315) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 315) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 46.004879 59.655067)
    (fp_text reference "C1122" (at 2.2225 2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 50.804615 50.150997 90)
    (fp_text reference "C976" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "SOT23-6PIN_1_45H_1" (layer "B.Cu")
    (tedit 0)
    (at -38.595384 46.951003)
    (fp_text reference "D2001" (at 1.444537 1.650873 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.950011 1.500099) (size 0.640004 0.999998) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 42 "A_R_DAC2_F"))
    (pad "2" smd rect (at 0 1.500099) (size 0.640004 0.999998) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "3" smd rect (at -0.950011 1.500099) (size 0.640004 0.999998) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 40 "A_G_DAC2_F"))
    (pad "4" smd rect (at -0.950011 -1.500099) (size 0.640004 0.999998) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 38 "A_B_DAC2_F"))
    (pad "5" smd rect (at 0 -1.500099) (size 0.640004 0.999998) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "+3.3V"))
    (pad "6" smd rect (at 0.950011 -1.500099) (size 0.640004 0.999998) (layers "B.Cu" "B.Paste" "B.Mask"))
  )
  (footprint "RES3225_0_7H_1" (layer "B.Cu")
    (tedit 0)
    (at -14.745394 71.598808 180)
    (fp_text reference "R871" (at -1.643634 -1.664208 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -1.4478 180) (size 2.794 1.397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 32 "N87118360"))
    (pad "2" smd rect (at 0 1.4478 180) (size 2.794 1.397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 30 "N87118038"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 96.604625 18.651009 90)
    (fp_text reference "C355" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 92.599604 31.335998 -90)
    (fp_text reference "C381" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 402 "N49338012"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "NET_SHORT_1" (layer "B.Cu")
    (tedit 0)
    (at 46.804623 69.551009 -90)
    (fp_text reference "NS120" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0 270) (size 0.550012 0.550012) (drill 0.250012) (layers *.Cu *.Mask)
      (net 4 "GND"))
    (pad "2" smd circle (at -0.2 0 270) (size 0.127 0.127) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 720 "GND_VSSRHA"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -8.495393 13.650994 -45)
    (fp_text reference "C572" (at 2.694077 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 315) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 315) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -16.405385 51.95841)
    (fp_text reference "R61" (at 1.5875 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "+3.3V"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 798 "GPIO_11"))
  )
  (footprint "DIOSOD_323_1_1H_1" (layer "B.Cu")
    (tedit 0)
    (at 6.504627 49.350999 180)
    (fp_text reference "D870" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -1.143 180) (size 0.635 1.016) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 17 "+VDDCI_LDO"))
    (pad "2" smd rect (at 0 1.143 180) (size 0.635 1.016) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 14.004612 19.984027)
    (fp_text reference "C523" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 51.004615 53.701003 90)
    (fp_text reference "C984" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "SMIND1005_0_5H_1" (layer "B.Cu")
    (tedit 0)
    (at 16.904607 51.701007 90)
    (fp_text reference "B94" (at -1.27 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 22 "+1.8V"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 680 "+VDDR_DVP"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -37.587385 56.033002)
    (fp_text reference "R79" (at 1.5875 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "+3.3V"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "HSYNC2"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 44.004603 57.659897)
    (fp_text reference "C175" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 46.004625 57.649991)
    (fp_text reference "C1112" (at 2.2225 2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1608_1" (layer "B.Cu")
    (tedit 0)
    (at 14.404612 6.251009 90)
    (fp_text reference "C528" (at -1.905025 1.904975 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 90) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.7874 90) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 48.559611 67.251014 180)
    (fp_text reference "C146" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 30.304605 72.551003)
    (fp_text reference "C903" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 616 "+PCIE_VDDR"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 96.304626 20.851005 90)
    (fp_text reference "C350" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES3225_0_7H_1" (layer "B.Cu")
    (tedit 0)
    (at -5.995373 54.901)
    (fp_text reference "MR878" (at 1.54686 1.76784 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -1.4478) (size 2.794 1.397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 1.4478) (size 2.794 1.397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 18 "LDO6_VIN"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 65.004612 20.151006 45)
    (fp_text reference "C416" (at 0 2.694077 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 45) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 45) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 158.246615 39.904002 180)
    (fp_text reference "AR86" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 945 "AICSN1"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 934 "ACISP1"))
  )
  (footprint "GEOM0013_1" (layer "B.Cu")
    (tedit 0)
    (at 17.704605 48.751 -90)
    (fp_text reference "C117" (at 1.195476 -1.181837 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144 270) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 682 "+TXVDDR"))
    (pad "2" smd rect (at 0 0.9144 270) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 92.989621 38.806011 180)
    (fp_text reference "C336" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 459 "N49337758"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 98.804621 18.651009 -90)
    (fp_text reference "C370" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES3225_0_7H_1" (layer "B.Cu")
    (tedit 0)
    (at -5.495374 66.650989)
    (fp_text reference "MR868" (at 1.54686 1.76784 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -1.4478) (size 2.794 1.397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 31 "+3.3V_BUS"))
    (pad "2" smd rect (at 0 1.4478) (size 2.794 1.397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 23 "LDO2_VIN"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 40.204611 65.450992)
    (fp_text reference "C925" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 716 "+PCIE_VDDC"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 34.539623 41.251015 90)
    (fp_text reference "C123" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 736 "GND_VSSRHD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 737 "+VDDRHD"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 21.09962 17.606002 -90)
    (fp_text reference "C509" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 100.304618 30.75101)
    (fp_text reference "C354" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "GEOM0013_1" (layer "B.Cu")
    (tedit 0)
    (at 20.504625 69.15101)
    (fp_text reference "C100" (at 1.181837 1.195476 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 655 "+T2PVDD"))
    (pad "2" smd rect (at 0 0.9144) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 677 "GND_T2PVSS"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 90.609615 86.19601 180)
    (fp_text reference "R204" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 540 "CSA0B_0"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -4.895375 30.350986 -45)
    (fp_text reference "C562" (at 2.694077 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 315) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 315) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 63.604615 7.751006 -90)
    (fp_text reference "C414" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -39.995381 38.450995 180)
    (fp_text reference "R2006" (at -2.2225 -2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 842 "DDCDATA_DAC2_5V"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 52 "DDCDATA_DAC2_R"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 39.004613 66.388582)
    (fp_text reference "C921" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 716 "+PCIE_VDDC"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 94.916008 63.218002 45.1)
    (fp_text reference "R252" (at -0.004702 2.694073 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 45.1) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 484 "CLKA1B"))
    (pad "2" smd rect (at 0 0.492608 45.1) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "F_PAD_M120_1" (layer "B.Cu")
    (tedit 0)
    (at 143.895615 10.440002)
    (fp_text reference "FM4" (at -0.762501 -0.000013 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd circle (at 0 0) (size 1.020064 1.020064) (layers "B.Cu" "B.Paste" "B.Mask"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 66.304609 15.651015 180)
    (fp_text reference "R419" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 331 "N48027750"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -2.405388 15.585991 -135)
    (fp_text reference "C585" (at 0 -2.694077 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 225) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 148 "N48570085"))
    (pad "2" smd rect (at 0 0.492608 225) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 57.604601 44.551008)
    (fp_text reference "R491" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 759 "MVREFD_C"))
  )
  (footprint "CAP1608_1" (layer "B.Cu")
    (tedit 0)
    (at 100.904616 19.551007)
    (fp_text reference "C377" (at 1.904975 1.905025 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.7874) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -8.795393 26.650993 45)
    (fp_text reference "C586" (at 0 2.694077 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 45) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 149 "N48570109"))
    (pad "2" smd rect (at 0 0.492608 45) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -35.682385 56.033002 180)
    (fp_text reference "R2011" (at -2.2225 -2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 5 "VSYNC_DAC2_B"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 51 "VSYNC_DAC2_R"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 37.999535 57.644657)
    (fp_text reference "C941" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 43.749613 12.996004 -90)
    (fp_text reference "C482" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 273 "N48027876"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 96.704625 23.051 90)
    (fp_text reference "C358" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 43.009939 53.654571 180)
    (fp_text reference "C1131" (at -2.2225 -2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 26.004614 69.951008 180)
    (fp_text reference "C2021" (at -2.2225 -2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 781 "+A2VDDQ"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 767 "GND_A2VSSQ"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 0.504614 18.951009 45)
    (fp_text reference "C550" (at 0 2.694077 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 45) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 45) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 37.209697 64.943881 90)
    (fp_text reference "C924" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 716 "+PCIE_VDDC"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 26.304613 8.751004 180)
    (fp_text reference "C500" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 7.804625 95.051009 180)
    (fp_text reference "R13" (at -1.5875 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 741 "PCIE_REFCLKP"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 49.330018 64.512894 -90)
    (fp_text reference "C989" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "GEOM0008_1" (layer "B.Cu")
    (tedit 0)
    (at 8.804623 45.451006 -90)
    (fp_text reference "B911" (at 1.195476 -1.181837 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144 270) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 36 "+VDDCI"))
    (pad "2" smd rect (at 0 0.9144 270) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 4.068615 11.075002 -90)
    (fp_text reference "C1029" (at 2.54 -2.2225 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -8.095394 28.251015 -45)
    (fp_text reference "C569" (at 2.694077 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 315) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 315) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "NET_SHORT_1" (layer "B.Cu")
    (tedit 0)
    (at 18.034627 55.576005 180)
    (fp_text reference "NS110" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0 180) (size 0.550012 0.550012) (drill 0.250012) (layers *.Cu *.Mask)
      (net 4 "GND"))
    (pad "2" smd circle (at -0.2 0 180) (size 0.127 0.127) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 690 "GND_TPVSS"))
  )
  (footprint "CAP1608_1" (layer "B.Cu")
    (tedit 0)
    (at 47.479603 62.605989 180)
    (fp_text reference "MC187" (at -2.222475 -2.540025 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 180) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.7874 180) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 37.013761 61.680692)
    (fp_text reference "C1104" (at 2.2225 2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -1.795381 23.251 45)
    (fp_text reference "C560" (at 0 2.694077 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 45) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 45) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 20.804624 65.350992 180)
    (fp_text reference "C108" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 669 "+T2XVDD"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 44.104603 76.750995 180)
    (fp_text reference "C292" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 730 "MVREFD_A"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 13.604613 13.050995 -90)
    (fp_text reference "C531" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 203 "N48569969"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "GEOM0013_1" (layer "B.Cu")
    (tedit 0)
    (at 7.504625 56.55101 90)
    (fp_text reference "C871" (at -1.195476 1.181837 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144 90) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 17 "+VDDCI_LDO"))
    (pad "2" smd rect (at 0 0.9144 90) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -17.755395 55.358403)
    (fp_text reference "R70" (at 1.5875 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "+3.3V"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 707 "VID_0"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 37.808172 66.398767)
    (fp_text reference "C923" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 716 "+PCIE_VDDC"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 47.304622 74.450999 180)
    (fp_text reference "C294" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 719 "MVREFS_A"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 98.804621 38.650995 -90)
    (fp_text reference "C315" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1608_1" (layer "B.Cu")
    (tedit 0)
    (at 122.305615 5.995002 90)
    (fp_text reference "ER15" (at -1.905025 1.904975 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 90) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.7874 90) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 858 "N85769031"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 23.604619 57.300995 90)
    (fp_text reference "C116" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 682 "+TXVDDR"))
  )
  (footprint "GEOM0013_1" (layer "B.Cu")
    (tedit 0)
    (at 7.659616 88.363011)
    (fp_text reference "C852" (at 1.181837 1.195476 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 27 "+1.1V"))
    (pad "2" smd rect (at 0 0.9144) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 25.504615 100.650998 180)
    (fp_text reference "C16" (at -1.5875 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 879 "PERN4"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 646 "GFXTN4_PERN4"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 53.804609 14.151018 -90)
    (fp_text reference "C436" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 332 "N48027731"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "GEOM0013_1" (layer "B.Cu")
    (tedit 0)
    (at 30.004606 38.750994 -135)
    (fp_text reference "C954" (at 0.009644 -1.681014 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144 225) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.9144 225) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 48.50462 54.350989 36.2)
    (fp_text reference "C65" (at 0.53098 1.962426 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 36.2) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 731 "+MPVDD"))
    (pad "2" smd rect (at 0 0.492608 36.2) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 732 "GND_MPVSS"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 19.889615 14.376011 90)
    (fp_text reference "C517" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 59.504623 46.951003 180)
    (fp_text reference "R493" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 734 "MVREFS_C"))
  )
  (footprint "CAP1608_1" (layer "B.Cu")
    (tedit 0)
    (at 19.434624 41.285991 -135)
    (fp_text reference "MC956" (at 0.224542 -3.367596 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 225) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.7874 225) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 31.396627 57.281996 90)
    (fp_text reference "TR50" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 806 "PCIE_CLK_REQB"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "+3.3V"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 87.204618 59.151004 -90)
    (fp_text reference "C284" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 41.004863 53.649491 180)
    (fp_text reference "C171" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 35.70462 10.850999 180)
    (fp_text reference "C453" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 86.664614 66.720992 -90)
    (fp_text reference "C274" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -4.495376 24.150998 135)
    (fp_text reference "C574" (at -2.694077 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 135) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 135) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 89.204614 64.185996)
    (fp_text reference "C267" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 30.004606 42.651012 135)
    (fp_text reference "C135" (at -2.694077 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 135) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 135) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 85.036906 29.986699 180)
    (fp_text reference "C351" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 37.904615 12.350996 135)
    (fp_text reference "R452" (at -2.694077 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 135) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 230 "CLKC1B"))
    (pad "2" smd rect (at 0 0.492608 135) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 40.904609 17.750986)
    (fp_text reference "R454" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 229 "CSC1B_0"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 22.604621 65.350992 180)
    (fp_text reference "C106" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 669 "+T2XVDD"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 96.304626 80.851012 90)
    (fp_text reference "C204" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1608_1" (layer "B.Cu")
    (tedit 0)
    (at 86.50462 57.451008 -90)
    (fp_text reference "C278" (at 1.905025 -1.904975 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 270) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.7874 270) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 36.004873 53.634251)
    (fp_text reference "C167" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "DPAKSGD_1" (layer "B.Cu")
    (tedit 0)
    (at 138.820187 48.794002 90)
    (fp_text reference "MQ1308" (at -2.416175 2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "D" smd rect (at 0 -3.7465 90) (size 5.6896 5.6388) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 68 "APHASE_2"))
    (pad "G" smd oval (at 2.286 3.7465 90) (size 1.651 2.6797) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 67 "LG2"))
    (pad "S" smd oval (at -2.286 3.7465 90) (size 1.651 2.6797) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 46.004625 55.659647)
    (fp_text reference "C915" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 36 "+VDDCI"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "NET_SHORT_1" (layer "B.Cu")
    (tedit 0)
    (at 36.354606 45.551006 -90)
    (fp_text reference "NS123" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0 270) (size 0.550012 0.550012) (drill 0.250012) (layers *.Cu *.Mask)
      (net 4 "GND"))
    (pad "2" smd circle (at -0.2 0 270) (size 0.127 0.127) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 736 "GND_VSSRHD"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 6.304602 58.551006)
    (fp_text reference "C875" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 17 "+VDDCI_LDO"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "LDO6_FB"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 26.104614 79.551014 -90)
    (fp_text reference "C930" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 618 "+PCIE_PVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "GEOM0013_1" (layer "B.Cu")
    (tedit 0)
    (at 38.504614 50.550996 90)
    (fp_text reference "C1137" (at -1.27033 1.111516 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144 90) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.9144 90) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 43.004605 48.051001 180)
    (fp_text reference "C969" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 89.244619 65.850991 -90)
    (fp_text reference "R254" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 483 "CSA1B_0"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 25.084626 21.921005 -90)
    (fp_text reference "C518" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 90.404612 59.351004 -90)
    (fp_text reference "C286" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 530 "N25405167"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 97.904622 46.751004 -90)
    (fp_text reference "C300" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 18.899624 16.825994 90)
    (fp_text reference "R507" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 161 "CASD0B"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 57.404602 63.950995)
    (fp_text reference "C393" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 755 "MVREFS_B"))
  )
  (footprint "SMIND1005_0_5H_1" (layer "B.Cu")
    (tedit 0)
    (at 13.604613 59.151004)
    (fp_text reference "B60" (at 1.5875 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 27 "+1.1V"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 674 "+DPLL_VDDC"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 8.704623 96.751005)
    (fp_text reference "R14" (at 1.5875 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 639 "PCIE_REFCLKN"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 85.304622 63.550996 -90)
    (fp_text reference "C265" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 44.004857 53.649491)
    (fp_text reference "C1130" (at 2.2225 2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 84.629617 83.440999 -90)
    (fp_text reference "C223" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 39.004867 53.654571 180)
    (fp_text reference "C173" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 32.504626 61.151)
    (fp_text reference "C91" (at 1.5875 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "+3.3V"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "SMIND1005_0_5H_1" (layer "B.Cu")
    (tedit 0)
    (at 33.604624 12.050997 -90)
    (fp_text reference "B452" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 274 "N48027825"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "SOT23_3PIN_1" (layer "B.Cu")
    (tedit 0)
    (at 126.369615 5.106002 -90)
    (fp_text reference "Q992" (at 1.381125 -1.38115 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9398 1.143 270) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 858 "N85769031"))
    (pad "2" smd rect (at -0.9398 1.143 270) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "3" smd rect (at 0 -1.143 270) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 857 "N85769033"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 56.404604 12.550996 135)
    (fp_text reference "R401" (at -2.694077 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 135) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 284 "CLKC0"))
    (pad "2" smd rect (at 0 0.492608 135) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 57.539603 100.671013 180)
    (fp_text reference "C31" (at -1.5875 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 889 "PERP12"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 749 "GFXTP12_PERP12"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 91.704609 86.151001 180)
    (fp_text reference "R205" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 539 "WEA0B"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 69.504628 100.650998 180)
    (fp_text reference "C37" (at -1.5875 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 892 "PERP15"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 728 "GFXTP15_PERP15"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 6.104603 71.051006)
    (fp_text reference "R865" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 22 "+1.8V"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 21 "LDO2_FB"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 92.704607 65.050993)
    (fp_text reference "C268" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 97.904622 80.951012)
    (fp_text reference "C213" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -30.280389 46.351005 180)
    (fp_text reference "C2006" (at -2.2225 -2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 37 "A_DAC2_B"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 85.304622 23.550999 -90)
    (fp_text reference "C366" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES3216_1" (layer "B.Cu")
    (tedit 0)
    (at 8.504623 75.901009 -90)
    (fp_text reference "R858" (at 1.65848 -1.658468 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -1.4478 270) (size 1.799996 1.399997) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 1.4478 270) (size 1.799996 1.399997) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 28 "LDO3_VIN"))
  )
  (footprint "CAP1608_1" (layer "B.Cu")
    (tedit 0)
    (at 42.904605 38.301008 180)
    (fp_text reference "MC955" (at -2.222475 -2.540025 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 180) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.7874 180) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 14.559602 21.851003 -90)
    (fp_text reference "C514" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 99.404619 88.750996 180)
    (fp_text reference "C224" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1608_0_8H_1" (layer "B.Cu")
    (tedit 0)
    (at -32.795396 46.351005)
    (fp_text reference "ML2003" (at 2.539975 3.175025 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 37 "A_DAC2_B"))
    (pad "2" smd rect (at 0 0.7874) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 38 "A_B_DAC2_F"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 39.014773 55.649487 180)
    (fp_text reference "C169" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 96.039602 35.771016 -90)
    (fp_text reference "R321" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 459 "N49337758"))
  )
  (footprint "RES1608_1" (layer "B.Cu")
    (tedit 0)
    (at -28.443385 73.940002)
    (fp_text reference "ER305" (at 2.222475 2.540025 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "2" smd rect (at 0 0.7874) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 81 "N87528545"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 93.604606 88.950996 180)
    (fp_text reference "C233" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 583 "N25404817"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 48.044626 8.011 180)
    (fp_text reference "R460" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 275 "N48027848"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "SOIC14_1" (layer "B.Cu")
    (tedit 0)
    (at -35.712382 61.575993)
    (fp_text reference "U1999" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd oval (at 3.937 2.582672) (size 0.8636 1.4478) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "2" smd oval (at 2.54 2.582672) (size 0.6096 1.5748) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "HSYNC1"))
    (pad "3" smd oval (at 1.27 2.582672) (size 0.6096 1.5748) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 10 "HSYNC_DAC1_B"))
    (pad "4" smd oval (at 0 2.582672) (size 0.6096 1.5748) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "5" smd oval (at -1.27 2.582672) (size 0.6096 1.5748) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 6 "VSYNC1"))
    (pad "6" smd oval (at -2.54 2.582672) (size 0.6096 1.5748) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "VSYNC_DAC1_B"))
    (pad "7" smd oval (at -3.937 2.582672) (size 0.8636 1.4478) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "8" smd oval (at -3.937 -2.582672) (size 0.8636 1.4478) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "HSYNC_DAC2_B"))
    (pad "9" smd oval (at -2.54 -2.582672) (size 0.6096 1.5748) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "HSYNC2"))
    (pad "10" smd oval (at -1.27 -2.582672) (size 0.6096 1.5748) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "11" smd oval (at 0 -2.582672) (size 0.6096 1.5748) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 5 "VSYNC_DAC2_B"))
    (pad "12" smd oval (at 1.27 -2.582672) (size 0.6096 1.5748) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "VSYNC2"))
    (pad "13" smd oval (at 2.54 -2.582672) (size 0.6096 1.5748) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "14" smd oval (at 3.937 -2.582672) (size 0.8636 1.4478) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 8 "+5V"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 46.026113 61.6907 180)
    (fp_text reference "C1121" (at -2.2225 -2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 47.144627 8.011)
    (fp_text reference "R459" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 275 "N48027848"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 46.804623 65.850991 -90)
    (fp_text reference "C120" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 718 "+VDDRHA"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 720 "GND_VSSRHA"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 37.204617 40.250991 -90)
    (fp_text reference "C154" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "NET_SHORT_1" (layer "B.Cu")
    (tedit 0)
    (at 22.604621 74.051 180)
    (fp_text reference "NS1020" (at 1.905 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0 180) (size 0.550012 0.550012) (drill 0.250012) (layers *.Cu *.Mask)
      (net 4 "GND"))
    (pad "2" smd circle (at -0.2 0 180) (size 0.127 0.127) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 631 "GND_AVSSQ"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 92.604608 19.151008 90)
    (fp_text reference "C387" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 403 "N49337708"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 90.404612 18.35101 90)
    (fp_text reference "R361" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 403 "N49337708"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 41.008673 61.685772)
    (fp_text reference "C1115" (at 2.2225 2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 57.804626 8.251005 180)
    (fp_text reference "C413" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 4.068615 12.091002 -90)
    (fp_text reference "C1033" (at 2.54 -2.2225 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 100.304618 50.650996)
    (fp_text reference "C311" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 25.204615 66.851014 180)
    (fp_text reference "C101" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 677 "GND_T2PVSS"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 655 "+T2PVDD"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 40.204611 39.250993 -90)
    (fp_text reference "C593" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 738 "MVREFS_D"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 13.604613 18.35101 -90)
    (fp_text reference "C524" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "SMIND1005_0_5H_1" (layer "B.Cu")
    (tedit 0)
    (at -12.495385 23.850999 -45)
    (fp_text reference "B552" (at 2.694077 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 315) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 147 "N48570039"))
    (pad "2" smd rect (at 0 0.492608 135) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 66.504609 100.650998 180)
    (fp_text reference "C36" (at -1.5875 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 875 "PERN14"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 722 "GFXTN14_PERN14"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 32.204627 16.751013 180)
    (fp_text reference "C452" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "SOT23_3PIN_1" (layer "B.Cu")
    (tedit 0)
    (at -35.215381 35.23599 90)
    (fp_text reference "Q2002" (at -1.4732 1.289075 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9398 1.143 90) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "+3.3V"))
    (pad "2" smd rect (at -0.9398 1.143 90) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 715 "DDC2CLK"))
    (pad "3" smd rect (at 0 -1.143 90) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 841 "DDCCLK_DAC2_5V"))
  )
  (footprint "CAP1608_1" (layer "B.Cu")
    (tedit 0)
    (at 43.104605 5.65101 -90)
    (fp_text reference "C478" (at 1.905025 -1.904975 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 270) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.7874 270) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -1.805389 14.985992 -135)
    (fp_text reference "R560" (at 0 -2.694077 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 225) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 148 "N48570085"))
    (pad "2" smd rect (at 0 0.492608 225) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 96.604625 69.451009 90)
    (fp_text reference "C252" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 98.90462 62.950997 90)
    (fp_text reference "C259" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 56.004605 47.651002)
    (fp_text reference "C149" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 91.704609 63.950995)
    (fp_text reference "R253" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 535 "CKEA1"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 87.004619 50.150997 -45)
    (fp_text reference "C309" (at 2.694077 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 315) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 315) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 63.904614 13.550994 -90)
    (fp_text reference "C432" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 329 "N48027732"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 60.104622 68.551011 129)
    (fp_text reference "C973" (at -2.679318 0.281608 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 129) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 129) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 91.844614 79.716013 180)
    (fp_text reference "R206" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 537 "RASA0B"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 65.504611 6.851007 90)
    (fp_text reference "C400" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 66.304609 8.751004 180)
    (fp_text reference "C401" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -9.924677 31.980294 -135)
    (fp_text reference "MR50" (at 0 -2.694077 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 225) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "2" smd rect (at 0 0.492608 225) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 785 "GPIO_0"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 87.604618 86.851 -90)
    (fp_text reference "C220" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 91.804609 46.251005 180)
    (fp_text reference "R305" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 412 "WEB0B"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "CAP1608_1" (layer "B.Cu")
    (tedit 0)
    (at 54.604607 37.650997 135)
    (fp_text reference "MC958" (at -3.367596 -0.224542 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 135) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.7874 135) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 40.004611 59.650241)
    (fp_text reference "C180" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -4.095377 58.051007 90)
    (fp_text reference "MR877" (at -2.54 2.2225 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 24 "LDO_EN"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 19 "N87118008"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 5.204605 71.951004)
    (fp_text reference "R864" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 21 "LDO2_FB"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 91.879615 39.301006 180)
    (fp_text reference "R306" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 410 "RASB0B"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 16.104608 14.550992 90)
    (fp_text reference "R501" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 157 "CLKD0"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -12.355381 51.95841)
    (fp_text reference "R62" (at 1.5875 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "+3.3V"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 778 "GPIO_12"))
  )
  (footprint "TP089X043_1" (layer "B.Cu")
    (tedit 0)
    (at 27.80461 50.350997)
    (fp_text reference "TP77" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 0.5588 0.5588) (drill 0.250012) (layers *.Cu *.Mask)
      (net 750 "DVPDATA_17"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 96.704625 62.750997 90)
    (fp_text reference "C271" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 28.504609 100.650998 180)
    (fp_text reference "C17" (at -1.5875 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 896 "PERP5"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 746 "GFXTP5_PERP5"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -6.091385 74.575002 -90)
    (fp_text reference "R841" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 833 "N87189147"))
  )
  (footprint "GEOM0013_1" (layer "B.Cu")
    (tedit 0)
    (at 24.104618 80.751012 180)
    (fp_text reference "C932" (at -1.181837 -1.195476 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144 180) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 618 "+PCIE_PVDD"))
    (pad "2" smd rect (at 0 0.9144 180) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "SMIND1005_0_5H_1" (layer "B.Cu")
    (tedit 0)
    (at 16.004608 52.850992 90)
    (fp_text reference "B112" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 22 "+1.8V"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 689 "+TPVDD"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 54.604607 15.351016 -90)
    (fp_text reference "R406" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 283 "RASC0B"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -13.705391 55.358403)
    (fp_text reference "R75" (at 1.5875 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "+3.3V"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 660 "VID_5"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 41.404608 66.25099)
    (fp_text reference "C920" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 716 "+PCIE_VDDC"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 40.423838 51.970424 90)
    (fp_text reference "C1103" (at -2.54 2.2225 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 33.204625 16.751013 180)
    (fp_text reference "R461" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 276 "N48027858"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 41.999527 57.654817)
    (fp_text reference "C165" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 24.364612 13.485995 -90)
    (fp_text reference "C532" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 202 "N48569853"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 52.563616 57.395001 -90)
    (fp_text reference "C144" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 33.404624 43.050986 180)
    (fp_text reference "C156" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 15.504609 100.650998 180)
    (fp_text reference "C12" (at -1.5875 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 877 "PERN2"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 644 "GFXTN2_PERN2"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 100.304618 90.650992)
    (fp_text reference "C203" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 99.364614 33.151006 90)
    (fp_text reference "R360" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 402 "N49338012"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 52.865622 59.723012 -90)
    (fp_text reference "C121" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 733 "GND_VSSRHB"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 761 "+VDDRHB"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 85.024613 28.055994 90)
    (fp_text reference "C356" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 48.942084 47.256083 4.4)
    (fp_text reference "C961" (at 1.753236 2.045535 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 4.4) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 4.4) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RESN2012_1" (layer "B.Cu")
    (tedit 0)
    (at 24.704616 50.550996 -90)
    (fp_text reference "RP60" (at 0.899833 -0.885698 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.500101 -0.875005 270) (size 0.610006 0.510007) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 820 "GPIO_8"))
    (pad "2" smd oval (at 0.500101 -0.249911 270) (size 0.485013 0.249987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 784 "GPIO_9"))
    (pad "3" smd oval (at 0.500101 0.249911 270) (size 0.485013 0.249987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 822 "GPIO_10"))
    (pad "4" smd rect (at 0.500101 0.875005 270) (size 0.610006 0.510007) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 661 "GPIO_22_ROMCSB"))
    (pad "5" smd rect (at -0.500101 0.875005 270) (size 0.610006 0.510007) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 593 "ROMCSB_R"))
    (pad "6" smd oval (at -0.500101 0.249911 270) (size 0.485013 0.249987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 594 "GPIO_10_R"))
    (pad "7" smd oval (at -0.500101 -0.249911 270) (size 0.485013 0.249987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 595 "GPIO_9_R"))
    (pad "8" smd rect (at -0.500101 -0.875005 270) (size 0.610006 0.510007) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 596 "GPIO_8_R"))
  )
  (footprint "SMIND1005_0_5H_1" (layer "B.Cu")
    (tedit 0)
    (at 43.454617 11.410993 180)
    (fp_text reference "B451" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 273 "N48027876"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 51.304614 68.651011 45)
    (fp_text reference "C147" (at 0 2.694077 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 45) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 45) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 46.204624 10.950999 180)
    (fp_text reference "C455" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1608_1" (layer "B.Cu")
    (tedit 0)
    (at 56.004605 24.250998 90)
    (fp_text reference "C428" (at -1.905025 1.904975 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 90) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.7874 90) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 92.714615 62.366009)
    (fp_text reference "R256" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 480 "RASA1B"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -30.195375 14.250993)
    (fp_text reference "R57" (at 1.5875 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "+3.3V"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 826 "GPIO_7"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 87.604618 46.851004 -90)
    (fp_text reference "C307" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 98.404621 51.450994 90)
    (fp_text reference "C334" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "TP089X043_1" (layer "B.Cu")
    (tedit 0)
    (at 31.004604 59.951003)
    (fp_text reference "TP90" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 0.5588 0.5588) (drill 0.250012) (layers *.Cu *.Mask)
      (net 779 "N74256579"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -3.795377 25.750995 45)
    (fp_text reference "C553" (at 0 2.694077 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 45) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 45) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "SMD075M_1" (layer "B.Cu")
    (tedit 0)
    (at -40.381385 75.718002 180)
    (fp_text reference "EF1" (at -1.5875 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -2.160016 180) (size 3.429 1.778) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 11 "+5V_VESA"))
    (pad "2" smd rect (at 0 2.160016 180) (size 3.429 1.778) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 8 "+5V"))
  )
  (footprint "NET_SHORT_1" (layer "B.Cu")
    (tedit 0)
    (at 19.604601 72.651003 -90)
    (fp_text reference "NS2020" (at 0 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0 270) (size 0.550012 0.550012) (drill 0.250012) (layers *.Cu *.Mask)
      (net 4 "GND"))
    (pad "2" smd circle (at -0.2 0 270) (size 0.127 0.127) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 767 "GND_A2VSSQ"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 56.804628 46.751004 180)
    (fp_text reference "C493" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 734 "MVREFS_C"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 26.604613 75.450997)
    (fp_text reference "C1023" (at 2.2225 2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 764 "+VDD1DI"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 617 "GND_VSS1DI"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -7.795395 11.650998 135)
    (fp_text reference "C568" (at -2.694077 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 135) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 135) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 44.189617 14.431002 -135)
    (fp_text reference "C485" (at 0 -2.694077 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 225) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 275 "N48027848"))
    (pad "2" smd rect (at 0 0.492608 225) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 28.704608 40.350991 -135)
    (fp_text reference "C134" (at 0 -2.694077 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 225) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 225) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1608_1" (layer "B.Cu")
    (tedit 0)
    (at 47.504622 59.651003)
    (fp_text reference "MC181" (at 2.222475 2.540025 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.7874) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 20.704624 46.651004 180)
    (fp_text reference "C79" (at -1.5875 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 795 "+VDD_CT"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 34.004623 14.550992 180)
    (fp_text reference "R462" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 276 "N48027858"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 61.20462 17.451012 -90)
    (fp_text reference "C420" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 2.30461 22.351002 -45)
    (fp_text reference "C551" (at 2.694077 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 315) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 315) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 98.804621 78.650991 -90)
    (fp_text reference "C212" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 97.904622 40.951015)
    (fp_text reference "C318" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 36.404618 12.550996 135)
    (fp_text reference "R451" (at -2.694077 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 135) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 227 "CLKC1"))
    (pad "2" smd rect (at 0 0.492608 135) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 37.204617 39.451018 90)
    (fp_text reference "R591" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 739 "MVREFD_D"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -30.348385 59.462002 180)
    (fp_text reference "C1999" (at -2.2225 -2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 8 "+5V"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 54.204608 16.851013 180)
    (fp_text reference "C403" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 86.764614 43.446007 -90)
    (fp_text reference "C302" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 29.304607 62.90101 -90)
    (fp_text reference "C69" (at 1.27 -1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 667 "+DPLL_PVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 673 "GND_PVSS"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 39.999531 55.644407)
    (fp_text reference "C178" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -9.495391 27.450992 -135)
    (fp_text reference "R561" (at 0 -2.694077 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 225) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 225) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 149 "N48570109"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 66.20461 17.851011)
    (fp_text reference "C406" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 61.604619 11.450998)
    (fp_text reference "C407" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -6.395398 22.551001 135)
    (fp_text reference "R553" (at -2.694077 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 135) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 154 "CKED1"))
    (pad "2" smd rect (at 0 0.492608 135) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 31.304603 62.350998)
    (fp_text reference "TR40" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "+3.3V"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 649 "DDC4DATA"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 46.304624 8.751004 180)
    (fp_text reference "C470" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 3.804607 66.050991 90)
    (fp_text reference "R866" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 20 "N87118444"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 8 "+5V"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 5.159621 86.263015 -90)
    (fp_text reference "R855" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 27 "+1.1V"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 26 "LDO3_FB"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 14.204612 14.550992 180)
    (fp_text reference "R522" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 205 "N48569804"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 56.504604 22.351002 90)
    (fp_text reference "C425" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -16.405385 55.358403)
    (fp_text reference "R71" (at 1.5875 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "+3.3V"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 657 "VID_1"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -35.174385 51.334002 -90)
    (fp_text reference "C2001" (at 2.54 -2.2225 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 42 "A_R_DAC2_F"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -19.23238 55.358403)
    (fp_text reference "R72" (at 1.5875 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "+3.3V"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 658 "VID_2"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -34.98038 46.051005 -90)
    (fp_text reference "C2003" (at 2.54 -2.2225 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 38 "A_B_DAC2_F"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -33.095395 92.650988 180)
    (fp_text reference "R1004" (at -2.2225 -2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 766 "DDC1DATA"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "+3.3V"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 18.804603 15.331001 90)
    (fp_text reference "R503" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 210 "CKED0"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 4.068615 13.107002 -90)
    (fp_text reference "C1037" (at 2.54 -2.2225 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -6.895397 16.250989 135)
    (fp_text reference "C552" (at -2.694077 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 135) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 135) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 84.574626 80.136002 -90)
    (fp_text reference "C210" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 61.20462 16.551013 -90)
    (fp_text reference "R404" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 286 "CSC0B_0"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 39.004613 16.951013 90)
    (fp_text reference "R457" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 231 "CASC1B"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 99.404619 68.751011 180)
    (fp_text reference "C272" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 91.689623 66.25099 180)
    (fp_text reference "R255" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 482 "WEA1B"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 93.704605 92.351014 90)
    (fp_text reference "R220" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 585 "N25404871"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 92.604608 59.151004 90)
    (fp_text reference "R262" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 530 "N25405167"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 39.009693 57.644657 180)
    (fp_text reference "C174" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -32.126385 67.082002 180)
    (fp_text reference "MR67" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "HSYNC1"))
  )
  (footprint "GEOM0013_1" (layer "B.Cu")
    (tedit 0)
    (at 9.959612 79.963002)
    (fp_text reference "C856" (at 1.181837 1.195476 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 28 "LDO3_VIN"))
    (pad "2" smd rect (at 0 0.9144) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "F_PAD_M120_1" (layer "B.Cu")
    (tedit 0)
    (at 157.103615 89.434002)
    (fp_text reference "FM5" (at -0.762501 -0.000013 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd circle (at 0 0) (size 1.020064 1.020064) (layers "B.Cu" "B.Paste" "B.Mask"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -35.540374 10.369492 -90)
    (fp_text reference "R51" (at 1.27 -1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "+3.3V"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 788 "GPIO_1"))
  )
  (footprint "RES1608_0_8H_1" (layer "B.Cu")
    (tedit 0)
    (at -32.695396 49.250999 -90)
    (fp_text reference "ML2002" (at 3.175025 -2.539975 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 270) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 39 "A_DAC2_G"))
    (pad "2" smd rect (at 0 0.7874 270) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 40 "A_G_DAC2_F"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 64.304613 10.551 180)
    (fp_text reference "C417" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 85.404622 70.251008 180)
    (fp_text reference "C270" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 50.971112 52.542509 90)
    (fp_text reference "C975" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 89.204614 24.250998)
    (fp_text reference "C372" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 90.244617 31.260992 90)
    (fp_text reference "C361" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 96.304626 40.851016 90)
    (fp_text reference "C319" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "SMIND1005_0_5H_1" (layer "B.Cu")
    (tedit 0)
    (at 46.904623 64.850993 -90)
    (fp_text reference "B120" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 718 "+VDDRHA"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 2.079617 76.966006 90)
    (fp_text reference "C838" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 8 "+5V"))
  )
  (footprint "RES3225_0_7H_1" (layer "B.Cu")
    (tedit 0)
    (at -9.99539 71.598808 180)
    (fp_text reference "R873" (at -1.643634 -1.664208 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -1.4478 180) (size 2.794 1.397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 29 "N87118495"))
    (pad "2" smd rect (at 0 1.4478 180) (size 2.794 1.397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 30 "N87118038"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 90.609615 84.026012)
    (fp_text reference "R207" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 542 "CASA0B"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 36.418766 51.980584 90)
    (fp_text reference "C1107" (at -2.54 2.2225 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES3225_0_7H_1" (layer "B.Cu")
    (tedit 0)
    (at -12.520379 65.290997 90)
    (fp_text reference "NR878" (at -1.76784 1.54686 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -1.4478 90) (size 2.794 1.397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 30 "N87118038"))
    (pad "2" smd rect (at 0 1.4478 90) (size 2.794 1.397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 18 "LDO6_VIN"))
  )
  (footprint "SOT23-6PIN_1_45H_1" (layer "B.Cu")
    (tedit 0)
    (at -36.015379 39.036008 -90)
    (fp_text reference "D2002" (at 1.650873 -1.444537 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.950011 1.500099 270) (size 0.640004 0.999998) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 52 "DDCDATA_DAC2_R"))
    (pad "2" smd rect (at 0 1.500099 270) (size 0.640004 0.999998) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "3" smd rect (at -0.950011 1.500099 270) (size 0.640004 0.999998) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 50 "DDCCLK_DAC2_R"))
    (pad "4" smd rect (at -0.950011 -1.500099 270) (size 0.640004 0.999998) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 49 "HSYNC_DAC2_R"))
    (pad "5" smd rect (at 0 -1.500099 270) (size 0.640004 0.999998) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 11 "+5V_VESA"))
    (pad "6" smd rect (at 0.950011 -1.500099 270) (size 0.640004 0.999998) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 51 "VSYNC_DAC2_R"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 89.06461 83.451007 -90)
    (fp_text reference "C207" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -9.795391 95.951007 -90)
    (fp_text reference "R1" (at 0.635 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 850 "N84002959"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 98.90462 82.951008 90)
    (fp_text reference "C217" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 48.804619 74.450999 180)
    (fp_text reference "R293" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 719 "MVREFS_A"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -29.280391 51.850994 180)
    (fp_text reference "R2027" (at -2.2225 -2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 652 "A_DAC2_RB"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 44.382606 68.676004 90)
    (fp_text reference "C966" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 38.003599 61.685772 180)
    (fp_text reference "C1123" (at -2.2225 -2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 62.904616 21.351004 180)
    (fp_text reference "C424" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 96.604625 89.450995 90)
    (fp_text reference "C200" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "TP089X043_1" (layer "B.Cu")
    (tedit 0)
    (at -44.370633 8.653747)
    (fp_text reference "TP73" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 0.5588 0.5588) (drill 0.250012) (layers *.Cu *.Mask)
      (net 825 "DVPDATA_13"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 92.924622 25.105987)
    (fp_text reference "C380" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -12.355381 55.358403)
    (fp_text reference "R74" (at 1.5875 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "+3.3V"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 665 "VID_4"))
  )
  (footprint "CAP1608_1" (layer "B.Cu")
    (tedit 0)
    (at 23.10462 5.65101 -90)
    (fp_text reference "C529" (at 1.905025 -1.904975 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 270) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.7874 270) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -2.29538 97.651004 90)
    (fp_text reference "C5" (at -0.635 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 31 "+3.3V_BUS"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 43.008669 61.695932)
    (fp_text reference "C1100" (at 2.2225 2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "C1206_113_1" (layer "B.Cu")
    (tedit 0)
    (at 103.763615 42.444002 180)
    (fp_text reference "EC349" (at 0.981075 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd oval (at 1.4351 0 180) (size 0.9779 1.1938) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd oval (at -1.4351 0 180) (size 0.9779 1.1938) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 87.004619 90.150993 -45)
    (fp_text reference "C208" (at 2.694077 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 315) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 315) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1608_1" (layer "B.Cu")
    (tedit 0)
    (at 43.704604 23.650999 90)
    (fp_text reference "C476" (at -1.905025 1.904975 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 90) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.7874 90) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -33.396385 56.033002)
    (fp_text reference "MR78" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "VSYNC2"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -36.952385 67.082002 180)
    (fp_text reference "MR66" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 6 "VSYNC1"))
  )
  (footprint "NET_SHORT_1" (layer "B.Cu")
    (tedit 0)
    (at 18.804603 70.051008 -90)
    (fp_text reference "NS100" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0 270) (size 0.550012 0.550012) (drill 0.250012) (layers *.Cu *.Mask)
      (net 4 "GND"))
    (pad "2" smd circle (at -0.2 0 270) (size 0.127 0.127) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 677 "GND_T2PVSS"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 85.804621 48.051001 90)
    (fp_text reference "C314" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 25.87962 45.400994 180)
    (fp_text reference "C130" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 46.004879 53.659651)
    (fp_text reference "C911" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 36 "+VDDCI"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 94.604604 21.551003 45)
    (fp_text reference "R351" (at 0 2.694077 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 45) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 354 "CLKB1"))
    (pad "2" smd rect (at 0 0.492608 45) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 41.704608 18.35101)
    (fp_text reference "C484" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 55.704605 50.550996)
    (fp_text reference "C983" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 94.804629 23.051 45)
    (fp_text reference "R352" (at 0 2.694077 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 45) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 357 "CLKB1B"))
    (pad "2" smd rect (at 0 0.492608 45) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -31.280387 51.850994 180)
    (fp_text reference "C2004" (at -2.2225 -2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 41 "A_DAC2_R"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -11.795387 24.550997 -45)
    (fp_text reference "C581" (at 2.694077 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 315) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 147 "N48570039"))
    (pad "2" smd rect (at 0 0.492608 315) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 27.204611 15.651015)
    (fp_text reference "C535" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 204 "N48569889"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 103.763615 46.254002 90)
    (fp_text reference "C1040" (at -2.54 2.2225 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -3.995377 13.650994 -135)
    (fp_text reference "C564" (at 0 -2.694077 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 225) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 225) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 85.404622 50.250997 180)
    (fp_text reference "C313" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 18.504629 100.650998 180)
    (fp_text reference "C13" (at -1.5875 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 894 "PERP3"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 744 "GFXTP3_PERP3"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 53.904609 19.051008)
    (fp_text reference "C402" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 99.349628 32.281005 -90)
    (fp_text reference "R359" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 402 "N49338012"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 96.204626 91.350991 90)
    (fp_text reference "C201" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "SMIND1005_0_5H_1" (layer "B.Cu")
    (tedit 0)
    (at 46.404624 39.350993 90)
    (fp_text reference "B122" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 758 "+VDDRHC"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 96.154613 75.756 -90)
    (fp_text reference "R221" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 586 "N25404815"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 94.104605 58.751005 180)
    (fp_text reference "C282" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 528 "N25405099"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -21.610175 34.351003 -90)
    (fp_text reference "MR58" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 596 "GPIO_8_R"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 96.604625 38.650995 90)
    (fp_text reference "C325" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "NET_SHORT_1" (layer "B.Cu")
    (tedit 0)
    (at 13.504613 57.251008)
    (fp_text reference "NS70" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 0.550012 0.550012) (drill 0.250012) (layers *.Cu *.Mask)
      (net 4 "GND"))
    (pad "2" smd circle (at -0.2 0) (size 0.127 0.127) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 673 "GND_PVSS"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 153.103115 39.904002 180)
    (fp_text reference "AR93" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 933 "AICSN35"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 936 "ACISP3"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 33.404624 48.950999)
    (fp_text reference "C139" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 51.504614 11.650998 180)
    (fp_text reference "R422" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 332 "N48027731"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 41.804608 47.051003 180)
    (fp_text reference "C970" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 91.50461 52.350993 -90)
    (fp_text reference "R320" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 458 "N49337065"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 90.404612 58.351006 90)
    (fp_text reference "R261" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 530 "N25405167"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 51.904613 74.450999 57.1)
    (fp_text reference "C974" (at -0.564729 2.634223 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 57.1) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 57.1) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -4.315392 17.51601 -45)
    (fp_text reference "C582" (at 2.694077 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 315) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 146 "N48570141"))
    (pad "2" smd rect (at 0 0.492608 315) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 18.231706 13.058005 90)
    (fp_text reference "R502" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 160 "CLKD0B"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 45.504626 6.851007 90)
    (fp_text reference "C469" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 33.504624 8.351004)
    (fp_text reference "C471" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 13.439615 10.551 180)
    (fp_text reference "C521" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 36.004619 57.654817)
    (fp_text reference "C184" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 56.504604 63.950995)
    (fp_text reference "C394" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 755 "MVREFS_B"))
  )
  (footprint "GEOM0013_1" (layer "B.Cu")
    (tedit 0)
    (at 45.104626 50.601009 90)
    (fp_text reference "C919" (at -1.195476 1.181837 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144 90) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 36 "+VDDCI"))
    (pad "2" smd rect (at 0 0.9144 90) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "GEOM0013_1" (layer "B.Cu")
    (tedit 0)
    (at 42.904605 38.301008 180)
    (fp_text reference "C955" (at -1.181837 -1.195476 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144 180) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.9144 180) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 45.004627 76.750995 180)
    (fp_text reference "R291" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 730 "MVREFD_A"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 41.504608 100.650998 180)
    (fp_text reference "C23" (at -1.5875 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 899 "PERP8"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 777 "GFXTP8_PERP8"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 88.894607 66.725996 -90)
    (fp_text reference "C258" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -16.405385 52.9436 180)
    (fp_text reference "MR61" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 798 "GPIO_11"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 32.654613 59.351004 -90)
    (fp_text reference "C93" (at 1.27 -1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "+3.3V"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 0.004615 49.250999 180)
    (fp_text reference "MR876" (at -2.2225 -2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "LDO6_VREF"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 37.004617 55.659647 180)
    (fp_text reference "C160" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -28.695353 10.251026 90)
    (fp_text reference "R55" (at -1.27 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "+3.3V"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 787 "GPIO_5"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 90.204612 64.371009)
    (fp_text reference "R257" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 485 "CASA1B"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 96.104626 71.451005 90)
    (fp_text reference "C260" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 34.204623 65.550992)
    (fp_text reference "R9" (at 1.27 0.635 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 771 "N16984567"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 34.004623 19.951007)
    (fp_text reference "C462" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -6.875381 95.800995 90)
    (fp_text reference "R2" (at -0.635 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 848 "JTDI"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 849 "JTDO"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -0.995383 17.351012 45)
    (fp_text reference "C583" (at 0 2.694077 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 45) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 148 "N48570085"))
    (pad "2" smd rect (at 0 0.492608 45) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 56.004605 68.451011)
    (fp_text reference "C985" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 36.504618 100.650998 180)
    (fp_text reference "C21" (at -1.5875 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 898 "PERP7"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 757 "GFXTP7_PERP7"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -15.19538 21.451004 45)
    (fp_text reference "C580" (at 0 2.694077 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 45) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 45) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -13.705391 56.343593 180)
    (fp_text reference "MR75" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 660 "VID_5"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 45.104626 21.751003 -90)
    (fp_text reference "C451" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "SMIND1005_0_5H_1" (layer "B.Cu")
    (tedit 0)
    (at 14.104612 71.951004 180)
    (fp_text reference "B2030" (at -2.2225 -2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "+3.3V"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 676 "+A2VDD"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 98.404621 71.451005 90)
    (fp_text reference "C273" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 33.404624 46.440997)
    (fp_text reference "C132" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 53.904609 21.251004)
    (fp_text reference "C409" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 97.748108 68.651189 -135)
    (fp_text reference "C255" (at 0 -2.694077 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 225) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 225) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 42.004607 55.659647)
    (fp_text reference "C1128" (at 2.2225 2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 21.504623 52.750992 -90)
    (fp_text reference "C95" (at 1.27 -1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 680 "+VDDR_DVP"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 40.004865 53.659397)
    (fp_text reference "C164" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 51.704613 62.150998 -90)
    (fp_text reference "C145" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 40.999529 55.644407 180)
    (fp_text reference "C176" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1608_1" (layer "B.Cu")
    (tedit 0)
    (at -10.29539 12.550996 -45)
    (fp_text reference "C579" (at 2.694077 0.000035 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 315) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.7874 315) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 37.004617 57.644911 180)
    (fp_text reference "C949" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 99.404619 48.751 180)
    (fp_text reference "C301" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -19.23238 51.95841)
    (fp_text reference "R73" (at 1.5875 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "+3.3V"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 650 "VID_3"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 44.191928 45.461166 -1.7)
    (fp_text reference "C968" (at 1.960676 1.847647 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 358.3) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 358.3) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 58.004626 22.551001)
    (fp_text reference "C419" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 156.659115 39.904002 180)
    (fp_text reference "AC81" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 932 "AICSN24"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 85.819607 39.090999 -90)
    (fp_text reference "C317" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 48.804619 72.251004)
    (fp_text reference "C977" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 52.504612 67.251014 135)
    (fp_text reference "C982" (at -2.694077 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 135) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 135) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "C1206_113_1" (layer "B.Cu")
    (tedit 0)
    (at -35.682385 80.544002 180)
    (fp_text reference "EC135" (at 0.981075 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd oval (at 1.4351 0 180) (size 0.9779 1.1938) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 8 "+5V"))
    (pad "2" smd oval (at -1.4351 0 180) (size 0.9779 1.1938) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 89.704613 46.351005 180)
    (fp_text reference "C305" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 52.104612 39.625999 135)
    (fp_text reference "C137" (at -2.694077 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 135) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 135) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 25.504615 68.351011 -90)
    (fp_text reference "C2031" (at 2.54 -2.2225 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 676 "+A2VDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 53.20461 44.251009 180)
    (fp_text reference "C962" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1608_1" (layer "B.Cu")
    (tedit 0)
    (at 82.811815 29.312304)
    (fp_text reference "C376" (at 1.904975 1.905025 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.7874) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 42.424088 51.970424 -90)
    (fp_text reference "C913" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 36 "+VDDCI"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 86.989226 30.123707 -45)
    (fp_text reference "C371" (at 2.694077 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 315) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 315) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1608_1" (layer "B.Cu")
    (tedit 0)
    (at 3.354621 23.240992 -45)
    (fp_text reference "C577" (at 2.694077 0.000035 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 315) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.7874 315) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 65.104612 21.751003 -90)
    (fp_text reference "C430" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 98.404621 31.451009 90)
    (fp_text reference "C359" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 45.404626 45.551006)
    (fp_text reference "C967" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1608_1" (layer "B.Cu")
    (tedit 0)
    (at 28.804608 77.650993 90)
    (fp_text reference "C907" (at -1.905025 1.904975 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 90) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 616 "+PCIE_VDDR"))
    (pad "2" smd rect (at 0 0.7874 90) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES3225_0_7H_1" (layer "B.Cu")
    (tedit 0)
    (at -14.745394 77.848808 180)
    (fp_text reference "R870" (at -1.643634 -1.664208 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -1.4478 180) (size 2.794 1.397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 31 "+3.3V_BUS"))
    (pad "2" smd rect (at 0 1.4478 180) (size 2.794 1.397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 32 "N87118360"))
  )
  (footprint "SOT23_3PIN_1" (layer "B.Cu")
    (tedit 0)
    (at -35.31538 42.636001 90)
    (fp_text reference "Q2001" (at -1.4732 1.289075 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9398 1.143 90) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "+3.3V"))
    (pad "2" smd rect (at -0.9398 1.143 90) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 711 "DDC2DATA"))
    (pad "3" smd rect (at 0 -1.143 90) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 842 "DDCDATA_DAC2_5V"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 29.004608 74.850998 90)
    (fp_text reference "C901" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 616 "+PCIE_VDDR"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1608_1" (layer "B.Cu")
    (tedit 0)
    (at 59.419609 56.965995 135)
    (fp_text reference "MC126" (at -3.367596 -0.224542 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 135) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.7874 135) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 56.104604 65.950991 180)
    (fp_text reference "C392" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 760 "MVREFD_B"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 3.959624 87.163013 -90)
    (fp_text reference "C855" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 27 "+1.1V"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 26 "LDO3_FB"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 26.404613 63.250996 90)
    (fp_text reference "C61" (at -1.27 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 674 "+DPLL_VDDC"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 673 "GND_PVSS"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 21.604623 11.450998)
    (fp_text reference "C522" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 44.804627 49.350999 -90)
    (fp_text reference "C158" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "SMIND1005_0_5H_1" (layer "B.Cu")
    (tedit 0)
    (at 94.504604 49.050999 180)
    (fp_text reference "B301" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 456 "N49337776"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -30.280389 51.850994 180)
    (fp_text reference "R2001" (at -2.2225 -2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 41 "A_DAC2_R"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1608_1" (layer "B.Cu")
    (tedit 0)
    (at 38.504614 50.550996 90)
    (fp_text reference "MC1137" (at -3.175025 2.539975 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 90) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.7874 90) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 99.404619 28.750989 180)
    (fp_text reference "C367" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "TP089X043_1" (layer "B.Cu")
    (tedit 0)
    (at 30.204605 53.951015)
    (fp_text reference "TP72" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 0.5588 0.5588) (drill 0.250012) (layers *.Cu *.Mask)
      (net 819 "DVPDATA_12"))
  )
  (footprint "CAP1608_1" (layer "B.Cu")
    (tedit 0)
    (at 101.504615 28.251015 180)
    (fp_text reference "C378" (at -1.904975 -1.905025 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 180) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.7874 180) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 70.504626 100.650998 180)
    (fp_text reference "C38" (at -1.5875 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 876 "PERN15"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 727 "GFXTN15_PERN15"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 90.604612 46.351005 180)
    (fp_text reference "R304" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 413 "CSB0B_0"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "RES1608_1" (layer "B.Cu")
    (tedit 0)
    (at 166.501615 27.077002 180)
    (fp_text reference "ER17" (at -1.904975 -1.905025 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 180) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 60 "+12V_EXT"))
    (pad "2" smd rect (at 0 0.7874 180) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 851 "N86495700"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 26.204613 17.851011)
    (fp_text reference "C507" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 88.804615 18.751009 180)
    (fp_text reference "C360" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 99.644624 72.251004 -90)
    (fp_text reference "R259" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 529 "N25405147"))
  )
  (footprint "SMIND1005_0_5H_1" (layer "B.Cu")
    (tedit 0)
    (at 15.00461 69.651009 -90)
    (fp_text reference "B102" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 655 "+T2PVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 22 "+1.8V"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 4.559622 88.563011)
    (fp_text reference "C854" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 27 "+1.1V"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "C1206_113_1" (layer "B.Cu")
    (tedit 0)
    (at -35.682385 70.892002 180)
    (fp_text reference "EC134" (at 0.981075 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd oval (at 1.4351 0 180) (size 0.9779 1.1938) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 8 "+5V"))
    (pad "2" smd oval (at -1.4351 0 180) (size 0.9779 1.1938) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 46.204624 68.051012)
    (fp_text reference "C981" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 29.004608 74.051 90)
    (fp_text reference "C905" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 616 "+PCIE_VDDR"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 33.504624 100.650998 180)
    (fp_text reference "C20" (at -1.5875 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 881 "PERN6"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 633 "GFXTN6_PERN6"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 99.644624 73.101015 90)
    (fp_text reference "R260" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 529 "N25405147"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 24.504617 64.950993)
    (fp_text reference "C2025" (at 2.2225 2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 694 "+VDD2DI"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 693 "GND_VSS2DI"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 95.804601 17.251012 -90)
    (fp_text reference "C364" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -39.295383 84.851004 90)
    (fp_text reference "R1008" (at -2.54 2.2225 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 8 "+5V"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 843 "DDCCLK_DAC1_5V"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -28.280393 49.150999 180)
    (fp_text reference "R2028" (at -2.2225 -2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 706 "A_DAC2_GB"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "GEOM0013_1" (layer "B.Cu")
    (tedit 0)
    (at -1.045396 65.050993 90)
    (fp_text reference "C866" (at -1.195476 1.181837 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144 90) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 23 "LDO2_VIN"))
    (pad "2" smd rect (at 0 0.9144 90) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 58.804624 16.350988 90)
    (fp_text reference "R407" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 288 "CASC0B"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "CAP1608_1" (layer "B.Cu")
    (tedit 0)
    (at 82.574605 81.376004)
    (fp_text reference "C226" (at 1.904975 1.905025 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.7874) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 61.704619 19.551007)
    (fp_text reference "C434" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 49.504618 100.650998 180)
    (fp_text reference "C27" (at -1.5875 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 887 "PERP10"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 776 "GFXTP10_PERP10"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 43.204605 76.750995 180)
    (fp_text reference "C291" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 730 "MVREFD_A"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 21.904622 55.551012 180)
    (fp_text reference "C112" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 690 "GND_TPVSS"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 689 "+TPVDD"))
  )
  (footprint "GEOM0013_1" (layer "B.Cu")
    (tedit 0)
    (at 21.404623 62.750997 -90)
    (fp_text reference "C103" (at 1.195476 -1.181837 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144 270) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 669 "+T2XVDD"))
    (pad "2" smd rect (at 0 0.9144 270) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 22.604621 71.251006 -90)
    (fp_text reference "C2032" (at 2.54 -2.2225 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 676 "+A2VDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "SOT23SGD_T_1" (layer "B.Cu")
    (tedit 0)
    (at 124.464615 8.916002 90)
    (fp_text reference "EQ106" (at -1.532001 1.347788 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "D" smd rect (at 0 -1.2065 90) (size 1.016 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 913 "N85769062"))
    (pad "G" smd rect (at 0.9525 1.2065 90) (size 1.016 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 857 "N85769033"))
    (pad "S" smd rect (at -0.9525 1.2065 90) (size 1.016 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 17.804605 8.251005 180)
    (fp_text reference "C504" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 14.204612 16.751013 180)
    (fp_text reference "R521" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 205 "N48569804"))
  )
  (footprint "SMIND1005_0_5H_1" (layer "B.Cu")
    (tedit 0)
    (at 94.504604 88.950996 180)
    (fp_text reference "B201" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 583 "N25404817"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -2.154385 80.925002 -90)
    (fp_text reference "R844" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 837 "N87189157"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 838 "N87189202"))
  )
  (footprint "GEOM0013_1" (layer "B.Cu")
    (tedit 0)
    (at 44.604627 63.701008 -90)
    (fp_text reference "C182" (at 1.195476 -1.181837 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144 270) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.9144 270) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 36.999791 53.639331 180)
    (fp_text reference "C947" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 93.604606 49.050999 180)
    (fp_text reference "C333" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 456 "N49337776"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "SMIND1005_0_5H_1" (layer "B.Cu")
    (tedit 0)
    (at 95.629621 68.386013 90)
    (fp_text reference "B251" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 527 "N25405207"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 45.009681 55.654567 180)
    (fp_text reference "C1102" (at -2.2225 -2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 42.004861 53.649491)
    (fp_text reference "C168" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "GEOM0013_1" (layer "B.Cu")
    (tedit 0)
    (at 19.204627 54.050989)
    (fp_text reference "C113" (at 1.181837 1.195476 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 689 "+TPVDD"))
    (pad "2" smd rect (at 0 0.9144) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 690 "GND_TPVSS"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -19.23238 56.343593 180)
    (fp_text reference "MR72" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 658 "VID_2"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 37.004871 59.644907 180)
    (fp_text reference "C162" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -26.165386 22.231012 90)
    (fp_text reference "R59" (at -1.27 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "+3.3V"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 595 "GPIO_9_R"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 44.004857 55.644407)
    (fp_text reference "C1133" (at 2.2225 2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 29.604607 64.201007 -90)
    (fp_text reference "C68" (at 1.27 -1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 667 "+DPLL_PVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 673 "GND_PVSS"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 21.604623 9.251003)
    (fp_text reference "C503" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 11.504617 100.650998 180)
    (fp_text reference "C10" (at -1.5875 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 870 "PERN1"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 642 "GFXTN1_PERN1"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 35.80462 9.251003 90)
    (fp_text reference "C463" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "SMIND1005_0_5H_1" (layer "B.Cu")
    (tedit 0)
    (at 16.804607 75.750997 90)
    (fp_text reference "B1021" (at -2.54 2.2225 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 22 "+1.8V"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 764 "+VDD1DI"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 56.804628 44.551008)
    (fp_text reference "C492" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 759 "MVREFD_C"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 50.654603 51.136009 -90)
    (fp_text reference "R298" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 740 "N72779223"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 94.149613 29.095997 180)
    (fp_text reference "C383" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 400 "N49338068"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -3.595378 58.551006 180)
    (fp_text reference "R877" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 8 "+5V"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 19 "N87118008"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 18.504629 22.826007)
    (fp_text reference "C516" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 59.804622 63.650995 90)
    (fp_text reference "R394" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 755 "MVREFS_B"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 40.003595 61.685772 180)
    (fp_text reference "C1117" (at -2.2225 -2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 96.604625 78.650991 90)
    (fp_text reference "C205" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 92.814615 78.960998 180)
    (fp_text reference "C236" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 586 "N25404815"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 55.704605 10.850999 180)
    (fp_text reference "C411" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "SMIND1005_0_5H_1" (layer "B.Cu")
    (tedit 0)
    (at -4.91539 16.816012 -45)
    (fp_text reference "B551" (at 2.694077 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 315) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 146 "N48570141"))
    (pad "2" smd rect (at 0 0.492608 135) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 38.804614 15.451016 90)
    (fp_text reference "R453" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 281 "CKEC1"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 98.90462 42.951011 90)
    (fp_text reference "C321" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "GEOM0013_1" (layer "B.Cu")
    (tedit 0)
    (at 17.28962 50.401009 -90)
    (fp_text reference "C94" (at 1.058608 -1.323232 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144 270) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 680 "+VDDR_DVP"))
    (pad "2" smd rect (at 0 0.9144 270) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "GEOM0013_1" (layer "B.Cu")
    (tedit 0)
    (at 59.404623 56.951009 135)
    (fp_text reference "C126" (at -1.681014 -0.009644 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144 135) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.9144 135) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 90.404612 57.351008 90)
    (fp_text reference "C256" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "GEOM0013_1" (layer "B.Cu")
    (tedit 0)
    (at 34.404622 54.150989)
    (fp_text reference "C1139" (at 1.111516 1.27033 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.9144) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 14.504611 100.650998 180)
    (fp_text reference "C11" (at -1.5875 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 893 "PERP2"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 774 "GFXTP2_PERP2"))
  )
  (footprint "GEOM0008_1" (layer "B.Cu")
    (tedit 0)
    (at 3.404608 48.351001 90)
    (fp_text reference "B67" (at -1.058608 1.323232 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144 90) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 731 "+MPVDD"))
    (pad "2" smd rect (at 0 0.9144 90) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 43.004605 57.654817 180)
    (fp_text reference "C942" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "GEOM0013_1" (layer "B.Cu")
    (tedit 0)
    (at 34.459613 62.331008)
    (fp_text reference "C183" (at 1.181837 1.195476 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.9144) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 52.304612 12.250997 180)
    (fp_text reference "C437" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 332 "N48027731"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 0.604614 95.141001 90)
    (fp_text reference "R3" (at -0.635 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 73 "PERST#"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 74 "PERST#_BUF"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 57.704601 46.751004 180)
    (fp_text reference "C494" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 734 "MVREFS_C"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 59.204624 61.351)
    (fp_text reference "C153" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 86.644625 26.866004 -90)
    (fp_text reference "C368" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "SOT23-6PIN_1_45H_1" (layer "B.Cu")
    (tedit 0)
    (at -36.695388 88.450997 -90)
    (fp_text reference "D1002" (at 1.650873 -1.444537 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.950011 1.500099 270) (size 0.640004 0.999998) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 56 "DDCDATA_DAC1_R"))
    (pad "2" smd rect (at 0 1.500099 270) (size 0.640004 0.999998) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "3" smd rect (at -0.950011 1.500099 270) (size 0.640004 0.999998) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 54 "DDCCLK_DAC1_R"))
    (pad "4" smd rect (at -0.950011 -1.500099 270) (size 0.640004 0.999998) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 53 "HSYNC_DAC1_R"))
    (pad "5" smd rect (at 0 -1.500099 270) (size 0.640004 0.999998) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 11 "+5V_VESA"))
    (pad "6" smd rect (at 0.950011 -1.500099 270) (size 0.640004 0.999998) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 55 "VSYNC_DAC1_R"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -6.091385 80.925002 -90)
    (fp_text reference "R843" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 838 "N87189202"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 33 "+12V_BUS"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 40.004611 37.850996 90)
    (fp_text reference "R594" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 738 "MVREFS_D"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -12.355381 56.343593 180)
    (fp_text reference "MR74" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 665 "VID_4"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -11.895387 21.451004 -135)
    (fp_text reference "C584" (at 0 -2.694077 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 225) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 225) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -3.200382 23.066012 45)
    (fp_text reference "R554" (at 0 2.694077 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 45) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 101 "CSD1B_0"))
    (pad "2" smd rect (at 0 0.492608 45) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 90.259603 71.126012 90)
    (fp_text reference "C262" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "SMIND1005_0_5H_1" (layer "B.Cu")
    (tedit 0)
    (at 19.504627 46.851004 180)
    (fp_text reference "B76" (at -1.5875 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 22 "+1.8V"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 795 "+VDD_CT"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 34.654609 47.151003)
    (fp_text reference "C138" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 33.004625 14.550992 180)
    (fp_text reference "C487" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 276 "N48027858"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -22.607583 33.258397 -90)
    (fp_text reference "R46" (at 1.27 -1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 593 "ROMCSB_R"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "+3.3V"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -39.495382 40.350991 -90)
    (fp_text reference "R2005" (at 2.54 -2.2225 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 8 "+5V"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 842 "DDCDATA_DAC2_5V"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 26.304613 15.651015)
    (fp_text reference "C533" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 204 "N48569889"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "SOT353_1_1H_1" (layer "B.Cu")
    (tedit 0)
    (at 0.604614 95.141001 180)
    (fp_text reference "U5" (at -1.27 -0.635 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd oval (at 0.650011 0.950011 180) (size 0.300025 0.610006) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "+3.3V"))
    (pad "2" smd oval (at 0 0.950011 180) (size 0.300025 0.610006) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 73 "PERST#"))
    (pad "3" smd oval (at -0.650011 0.950011 180) (size 0.300025 0.610006) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "4" smd oval (at -0.650011 -0.950011 180) (size 0.300025 0.610006) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 74 "PERST#_BUF"))
    (pad "5" smd oval (at 0.650011 -0.950011 180) (size 0.300025 0.610006) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "+3.3V"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -25.011794 33.258397 -90)
    (fp_text reference "C47" (at 1.27 -1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "+3.3V"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 38.404614 19.651007)
    (fp_text reference "C475" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES3216_1" (layer "B.Cu")
    (tedit 0)
    (at -5.995373 54.901)
    (fp_text reference "R878" (at 1.658468 1.65848 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -1.4478) (size 1.799996 1.399997) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 1.4478) (size 1.799996 1.399997) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 18 "LDO6_VIN"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -13.705391 52.9436 180)
    (fp_text reference "MR63" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 823 "GPIO_13"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 25.704614 76.250996)
    (fp_text reference "C1025" (at 2.2225 2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 764 "+VDD1DI"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 617 "GND_VSS1DI"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 21.704622 65.350992 180)
    (fp_text reference "C109" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 669 "+T2XVDD"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 33.024615 55.652002 180)
    (fp_text reference "R5" (at -1.27 -0.635 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 807 "JTAG_MODE"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 50.404616 42.451012 90)
    (fp_text reference "C964" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "TP089X043_1" (layer "B.Cu")
    (tedit 0)
    (at 30.969933 56.311742)
    (fp_text reference "TP50" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 0.5588 0.5588) (drill 0.250012) (layers *.Cu *.Mask)
      (net 806 "PCIE_CLK_REQB"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 21.604623 46.651004 180)
    (fp_text reference "C78" (at -1.5875 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 795 "+VDD_CT"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -32.215387 42.136002 180)
    (fp_text reference "R2004" (at -2.2225 -2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 711 "DDC2DATA"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "+3.3V"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 32.654613 58.151006 -90)
    (fp_text reference "C92" (at 1.27 -1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "+3.3V"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES3216_1" (layer "B.Cu")
    (tedit 0)
    (at -5.495374 66.650989)
    (fp_text reference "R868" (at 1.658468 1.65848 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -1.4478) (size 1.799996 1.399997) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 31 "+3.3V_BUS"))
    (pad "2" smd rect (at 0 1.4478) (size 1.799996 1.399997) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 23 "LDO2_VIN"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -34.895391 47.851002 -90)
    (fp_text reference "C2002" (at 2.54 -2.2225 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 40 "A_G_DAC2_F"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 90.574614 44.151009)
    (fp_text reference "R307" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 415 "CASB0B"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 2.004611 20.551005 45)
    (fp_text reference "C565" (at 0 2.694077 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 45) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 45) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 24.304617 10.551 180)
    (fp_text reference "C501" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 27.204611 71.851004 -135)
    (fp_text reference "R1030" (at 0.224506 -3.367596 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 225) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 768 "RSET"))
    (pad "2" smd rect (at 0 0.492608 225) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 631 "GND_AVSSQ"))
  )
  (footprint "CAP1608_1" (layer "B.Cu")
    (tedit 0)
    (at 83.284611 69.416008)
    (fp_text reference "C276" (at 1.904975 1.905025 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.7874) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 86.849628 83.451007 -90)
    (fp_text reference "C211" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 30.104606 61.051001)
    (fp_text reference "TR41" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "+3.3V"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 709 "DDC4CLK"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 29.504607 100.650998 180)
    (fp_text reference "C18" (at -1.5875 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 880 "PERN5"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 647 "GFXTN5_PERN5"))
  )
  (footprint "CAP1608_1" (layer "B.Cu")
    (tedit 0)
    (at 65.104612 23.351 -90)
    (fp_text reference "C429" (at 1.905025 -1.904975 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 270) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.7874 270) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 26.004614 66.851014 180)
    (fp_text reference "C102" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 677 "GND_T2PVSS"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 655 "+T2PVDD"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 53.50461 9.751002 180)
    (fp_text reference "C410" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -0.395384 16.751013 -135)
    (fp_text reference "R559" (at 0 -2.694077 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 225) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 225) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 148 "N48570085"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 37.279623 37.541015 -90)
    (fp_text reference "R592" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 739 "MVREFD_D"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "GEOM0013_1" (layer "B.Cu")
    (tedit 0)
    (at -0.895383 52.550992 90)
    (fp_text reference "C876" (at -1.195476 1.181837 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144 90) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 18 "LDO6_VIN"))
    (pad "2" smd rect (at 0 0.9144 90) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 26.504613 13.450994)
    (fp_text reference "R519" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 204 "N48569889"))
  )
  (footprint "RES3225_0_7H_1" (layer "B.Cu")
    (tedit 0)
    (at -9.99539 77.848808 180)
    (fp_text reference "R872" (at -1.643634 -1.664208 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -1.4478 180) (size 2.794 1.397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 31 "+3.3V_BUS"))
    (pad "2" smd rect (at 0 1.4478 180) (size 2.794 1.397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 29 "N87118495"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 26.104614 78.550991 -90)
    (fp_text reference "C933" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 618 "+PCIE_PVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 24.804616 76.350995)
    (fp_text reference "C1024" (at 2.2225 2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 764 "+VDD1DI"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 617 "GND_VSS1DI"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 46.014607 16.536002 180)
    (fp_text reference "C459" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 43.009939 59.649987 180)
    (fp_text reference "C163" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 20.334623 51.131005)
    (fp_text reference "C98" (at 1.5875 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 680 "+VDDR_DVP"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -31.745385 14.250002)
    (fp_text reference "MR57" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 826 "GPIO_7"))
  )
  (footprint "SOT23_3PIN_1" (layer "B.Cu")
    (tedit 0)
    (at -2.154385 78.258002)
    (fp_text reference "Q841" (at 1.38115 1.381125 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9398 1.143) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 837 "N87189157"))
    (pad "2" smd rect (at -0.9398 1.143) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "3" smd rect (at 0 -1.143) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 24 "LDO_EN"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 40.204611 40.150992 -90)
    (fp_text reference "R593" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 738 "MVREFS_D"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 89.574616 25.880992 -90)
    (fp_text reference "R354" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 356 "CSB1B_0"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 94.104605 18.751009 180)
    (fp_text reference "C382" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 401 "N49337966"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 26.304613 72.651003 -135)
    (fp_text reference "C1020" (at 0.224506 -3.367596 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 225) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 632 "+AVDD"))
    (pad "2" smd rect (at 0 0.492608 225) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 631 "GND_AVSSQ"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 93.704605 52.350993 90)
    (fp_text reference "C335" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 458 "N49337065"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1608_1" (layer "B.Cu")
    (tedit 0)
    (at 82.649611 41.441007)
    (fp_text reference "C327" (at 1.904975 1.905025 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.7874) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 58.804624 15.451016 90)
    (fp_text reference "R403" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 337 "CKEC0"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "SMIND1005_0_5H_1" (layer "B.Cu")
    (tedit 0)
    (at 95.84961 28.431 90)
    (fp_text reference "B351" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 400 "N49338068"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -15.055375 55.358403)
    (fp_text reference "R76" (at 1.5875 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "+3.3V"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 659 "VID_6"))
  )
  (footprint "GEOM0013_1" (layer "B.Cu")
    (tedit 0)
    (at 59.328804 49.275205 45)
    (fp_text reference "C959" (at -0.009644 1.681014 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144 45) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.9144 45) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "GEOM0001_1" (layer "B.Cu")
    (tedit 0)
    (at 5.059621 81.862999 180)
    (fp_text reference "U851" (at -1.905 -1.8923 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd oval (at 1.905 2.8448 180) (size 0.639978 1.579982) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "2" smd oval (at 0.635 2.8448 180) (size 0.639978 1.579982) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 24 "LDO_EN"))
    (pad "3" smd oval (at -0.635 2.8448 180) (size 0.639978 1.579982) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 28 "LDO3_VIN"))
    (pad "4" smd oval (at -1.905 2.8448 180) (size 0.639978 1.579982) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 8 "+5V"))
    (pad "5" smd oval (at -1.905 -2.8702 180) (size 0.639978 1.579982) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 25 "N87118142"))
    (pad "6" smd oval (at -0.635 -2.8702 180) (size 0.639978 1.579982) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 27 "+1.1V"))
    (pad "7" smd oval (at 0.635 -2.8702 180) (size 0.639978 1.579982) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 26 "LDO3_FB"))
    (pad "8" smd oval (at 1.905 -2.8702 180) (size 0.639978 1.579982) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "9" smd rect (at 0 0 180) (size 4.099992 2.799994) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "C1206_113_1" (layer "B.Cu")
    (tedit 0)
    (at 3.941615 9.424002)
    (fp_text reference "EC346" (at -0.981075 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd oval (at 1.4351 0) (size 0.9779 1.1938) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd oval (at -1.4351 0) (size 0.9779 1.1938) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1608_1" (layer "B.Cu")
    (tedit 0)
    (at 30.004606 38.750994 -135)
    (fp_text reference "MC954" (at 0.224542 -3.367596 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 225) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.7874 225) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 7.504625 70.451007 90)
    (fp_text reference "C864" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 22 "+1.8V"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 96.604625 49.450998 90)
    (fp_text reference "C330" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 45.004627 20.151006 45)
    (fp_text reference "C474" (at 0 2.694077 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 45) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 45) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 58.304625 20.251006)
    (fp_text reference "C421" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1608_1" (layer "B.Cu")
    (tedit 0)
    (at 83.804625 50.250997 180)
    (fp_text reference "C328" (at -1.904975 -1.905025 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 180) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.7874 180) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "GEOM0013_1" (layer "B.Cu")
    (tedit 0)
    (at 41.804608 50.550996 90)
    (fp_text reference "C1136" (at -1.27033 1.111516 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144 90) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.9144 90) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 26.104614 80.551012 -90)
    (fp_text reference "C931" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 618 "+PCIE_PVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 45.904625 75.950996 180)
    (fp_text reference "C293" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 719 "MVREFS_A"))
  )
  (footprint "SMIND1005_0_5H_1" (layer "B.Cu")
    (tedit 0)
    (at 13.604613 12.050997 -90)
    (fp_text reference "B502" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 203 "N48569969"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 53.804609 70.651007 90)
    (fp_text reference "C986" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 25.704614 73.251002 -135)
    (fp_text reference "C1021" (at 0.224506 -3.367596 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 225) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 632 "+AVDD"))
    (pad "2" smd rect (at 0 0.492608 225) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 631 "GND_AVSSQ"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -17.755395 52.9436 180)
    (fp_text reference "MR65" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 671 "GENERICC"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 32.504626 100.650998 180)
    (fp_text reference "C19" (at -1.5875 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 897 "PERP6"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 770 "GFXTP6_PERP6"))
  )
  (footprint "GEOM0013_1" (layer "B.Cu")
    (tedit 0)
    (at 61.504619 69.25101 127.6)
    (fp_text reference "C127" (at -1.668255 0.206943 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144 127.6) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.9144 127.6) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -10.695389 19.651007 -135)
    (fp_text reference "C555" (at 0 -2.694077 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 225) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 225) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1608_1" (layer "B.Cu")
    (tedit 0)
    (at -7.395396 30.651011 45)
    (fp_text reference "C576" (at -0.000035 2.694077 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 45) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.7874 45) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 87.504618 63.550996 -90)
    (fp_text reference "C266" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -39.295383 92.050989 90)
    (fp_text reference "R1005" (at -2.54 2.2225 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 8 "+5V"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 844 "DDCDATA_DAC1_5V"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 92.564603 71.181003 -90)
    (fp_text reference "C281" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 529 "N25405147"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 34.204623 16.751013)
    (fp_text reference "C486" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 276 "N48027858"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 45.004881 57.659897 180)
    (fp_text reference "C1132" (at -2.2225 -2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "SMIND1005_0_5H_1" (layer "B.Cu")
    (tedit 0)
    (at 16.804607 74.650999 90)
    (fp_text reference "B1020" (at -2.54 2.2225 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 22 "+1.8V"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 632 "+AVDD"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 67.404607 13.450994 180)
    (fp_text reference "R420" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 331 "N48027750"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "GEOM0008_1" (layer "B.Cu")
    (tedit 0)
    (at 21.104624 60.851001 -90)
    (fp_text reference "B100" (at 1.195476 -1.181837 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144 270) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 669 "+T2XVDD"))
    (pad "2" smd rect (at 0 0.9144 270) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 862 "N42099087"))
  )
  (footprint "CAP1608_1" (layer "B.Cu")
    (tedit 0)
    (at 44.604627 63.650995 -90)
    (fp_text reference "MC182" (at 2.540025 -2.222475 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 270) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.7874 270) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1608_1" (layer "B.Cu")
    (tedit 0)
    (at 122.305615 4.217002 -90)
    (fp_text reference "ER16" (at 1.905025 -1.904975 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 270) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 858 "N85769031"))
    (pad "2" smd rect (at 0 0.7874 270) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 61.604619 9.251003)
    (fp_text reference "C415" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 41.604608 11.450998)
    (fp_text reference "C454" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1608_1" (layer "B.Cu")
    (tedit 0)
    (at 32.404626 20.551005)
    (fp_text reference "C477" (at 1.904975 1.905025 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.7874) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 89.709617 86.19601 180)
    (fp_text reference "C221" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "SMIND1005_0_5H_1" (layer "B.Cu")
    (tedit 0)
    (at 25.704614 82.351009 180)
    (fp_text reference "B930" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 22 "+1.8V"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 618 "+PCIE_PVDD"))
  )
  (footprint "TP089X043_1" (layer "B.Cu")
    (tedit 0)
    (at 27.90461 53.951015)
    (fp_text reference "TP74" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 0.5588 0.5588) (drill 0.250012) (layers *.Cu *.Mask)
      (net 752 "DVPDATA_14"))
  )
  (footprint "CAP1608_1" (layer "B.Cu")
    (tedit 0)
    (at 101.4846 88.361004 180)
    (fp_text reference "C228" (at -1.904975 -1.905025 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 180) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.7874 180) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 58.304625 18.05101)
    (fp_text reference "C422" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -30.380389 49.150999 180)
    (fp_text reference "C2005" (at -2.2225 -2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 39 "A_DAC2_G"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 60.304621 46.851004)
    (fp_text reference "R494" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 734 "MVREFS_C"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -33.142385 67.082002 180)
    (fp_text reference "R67" (at -1.5875 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "+3.3V"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "HSYNC1"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 21.704622 19.551007)
    (fp_text reference "C508" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 22.404621 47.351003 180)
    (fp_text reference "C76" (at -1.5875 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 795 "+VDD_CT"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "SOT23_3PIN_1" (layer "B.Cu")
    (tedit 0)
    (at -35.895389 84.751004 90)
    (fp_text reference "Q1002" (at -1.4732 1.289075 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9398 1.143 90) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "+3.3V"))
    (pad "2" smd rect (at -0.9398 1.143 90) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 765 "DDC1CLK"))
    (pad "3" smd rect (at 0 -1.143 90) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 843 "DDCCLK_DAC1_5V"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 91.50461 91.450991 90)
    (fp_text reference "R219" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 585 "N25404871"))
  )
  (footprint "CAP1608_1" (layer "B.Cu")
    (tedit 0)
    (at 15.40461 71.951004)
    (fp_text reference "C2033" (at 2.222475 2.540025 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 676 "+A2VDD"))
    (pad "2" smd rect (at 0 0.7874) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 35.40462 65.550992)
    (fp_text reference "R8" (at 1.27 0.635 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 716 "+PCIE_VDDC"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 769 "N16984571"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 91.734607 44.041002)
    (fp_text reference "R303" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 464 "CKEB0"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "CAP1608_1" (layer "B.Cu")
    (tedit 0)
    (at 83.804625 90.250993 180)
    (fp_text reference "C229" (at -1.904975 -1.905025 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 180) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.7874 180) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 26.204613 10.950999 180)
    (fp_text reference "C502" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1608_1" (layer "B.Cu")
    (tedit 0)
    (at -9.395392 99.451 90)
    (fp_text reference "C2" (at -0.635025 1.269975 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 90) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 33 "+12V_BUS"))
    (pad "2" smd rect (at 0 0.7874 90) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 56.004605 44.551008)
    (fp_text reference "C491" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 759 "MVREFD_C"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 15.494602 9.086004 90)
    (fp_text reference "C505" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 5.204605 69.751009)
    (fp_text reference "C865" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 22 "+1.8V"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 21 "LDO2_FB"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 15.604609 10.661007 180)
    (fp_text reference "C520" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "GEOM0013_1" (layer "B.Cu")
    (tedit 0)
    (at 37.904615 63.750995 -90)
    (fp_text reference "C926" (at 1.195476 -1.181837 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144 270) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 716 "+PCIE_VDDC"))
    (pad "2" smd rect (at 0 0.9144 270) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "GEOM0013_1" (layer "B.Cu")
    (tedit 0)
    (at 20.604625 57.851007)
    (fp_text reference "C60" (at 1.323232 1.058608 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 667 "+DPLL_PVDD"))
    (pad "2" smd rect (at 0 0.9144) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 673 "GND_PVSS"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 57.804626 10.451 180)
    (fp_text reference "C412" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 21.09962 16.711592 -90)
    (fp_text reference "R504" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 159 "CSD0B_0"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 36.004619 55.659647)
    (fp_text reference "C172" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "GEOM0008_1" (layer "B.Cu")
    (tedit 0)
    (at -32.780384 52.151018)
    (fp_text reference "L2001" (at 1.111516 1.27033 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 41 "A_DAC2_R"))
    (pad "2" smd rect (at 0 0.9144) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 42 "A_R_DAC2_F"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -8.100398 24.991002 45)
    (fp_text reference "R556" (at 0 2.694077 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 45) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 98 "RASD1B"))
    (pad "2" smd rect (at 0 0.492608 45) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 19.504627 100.650998 180)
    (fp_text reference "C14" (at -1.5875 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 878 "PERN3"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 645 "GFXTN3_PERN3"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 53.50461 100.650998 180)
    (fp_text reference "C29" (at -1.5875 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 888 "PERP11"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 743 "GFXTP11_PERP11"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 33.504624 10.551 180)
    (fp_text reference "C456" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -15.055375 56.343593 180)
    (fp_text reference "MR76" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 659 "VID_6"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 36.904617 36.550999 90)
    (fp_text reference "C592" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 739 "MVREFD_D"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 91.704609 83.951006)
    (fp_text reference "R203" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 591 "CKEA0"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -34.412385 67.082002)
    (fp_text reference "R1010" (at 2.2225 2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 10 "HSYNC_DAC1_B"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 53 "HSYNC_DAC1_R"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 2.959626 86.263015 -90)
    (fp_text reference "R854" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 26 "LDO3_FB"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 57.904626 12.350996 135)
    (fp_text reference "R402" (at -2.694077 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 135) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 287 "CLKC0B"))
    (pad "2" smd rect (at 0 0.492608 135) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -12.195386 18.15101 -135)
    (fp_text reference "C570" (at 0 -2.694077 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 225) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 225) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -0.595384 54.150989 90)
    (fp_text reference "C878" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 8 "+5V"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 92.495007 69.422307 135)
    (fp_text reference "C285" (at -2.694077 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 135) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 529 "N25405147"))
    (pad "2" smd rect (at 0 0.492608 135) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 44.018827 61.706092 180)
    (fp_text reference "C1113" (at -2.2225 -2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 29.004608 75.650997 90)
    (fp_text reference "C902" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 616 "+PCIE_VDDR"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 84.804623 61.750999)
    (fp_text reference "C250" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "NET_SHORT_1" (layer "B.Cu")
    (tedit 0)
    (at 48.50462 59.151004)
    (fp_text reference "NS64" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 0.550012 0.550012) (drill 0.250012) (layers *.Cu *.Mask)
      (net 4 "GND"))
    (pad "2" smd circle (at -0.2 0) (size 0.127 0.127) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 732 "GND_MPVSS"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 98.804621 58.651005 -90)
    (fp_text reference "C269" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "GEOM0013_1" (layer "B.Cu")
    (tedit 0)
    (at 47.559613 56.595993)
    (fp_text reference "C67" (at 1.323232 1.058608 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 731 "+MPVDD"))
    (pad "2" smd rect (at 0 0.9144) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 732 "GND_MPVSS"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 61.10462 15.351016 -90)
    (fp_text reference "R405" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 285 "WEC0B"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 41.994447 59.649987)
    (fp_text reference "C185" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 89.304614 51.350995 -90)
    (fp_text reference "C308" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 16.764602 22.351002 90)
    (fp_text reference "C515" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 25.004616 69.951008 180)
    (fp_text reference "C2022" (at -2.2225 -2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 781 "+A2VDDQ"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 767 "GND_A2VSSQ"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 38.004869 53.644157)
    (fp_text reference "C170" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1608_2012_1" (layer "B.Cu")
    (tedit 0)
    (at 8.304624 51.050995)
    (fp_text reference "MR911" (at 1.111516 1.27033 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 36 "+VDDCI"))
    (pad "2" smd rect (at 0 0.9144) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 17 "+VDDCI_LDO"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 92.604608 18.15101 90)
    (fp_text reference "R362" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 403 "N49337708"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "C1206_113_1" (layer "B.Cu")
    (tedit 0)
    (at -30.729385 80.544002)
    (fp_text reference "EC133" (at -0.981075 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd oval (at 1.4351 0) (size 0.9779 1.1938) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 33 "+12V_BUS"))
    (pad "2" smd oval (at -1.4351 0) (size 0.9779 1.1938) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "NET_SHORT_1" (layer "B.Cu")
    (tedit 0)
    (at 47.218618 45.611001 -90)
    (fp_text reference "NS122" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0 270) (size 0.550012 0.550012) (drill 0.250012) (layers *.Cu *.Mask)
      (net 4 "GND"))
    (pad "2" smd circle (at -0.2 0 270) (size 0.127 0.127) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 763 "GND_VSSRHC"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -13.705391 51.95841)
    (fp_text reference "R63" (at 1.5875 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "+3.3V"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 823 "GPIO_13"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -10.631787 31.273209 45)
    (fp_text reference "R50" (at 0.224506 2.020558 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 45) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "+3.3V"))
    (pad "2" smd rect (at 0 0.492608 45) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 785 "GPIO_0"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 85.78961 79.120992 -90)
    (fp_text reference "C209" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -12.895385 20.251006 135)
    (fp_text reference "C566" (at -2.694077 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 135) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 135) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "GEOM0013_1" (layer "B.Cu")
    (tedit 0)
    (at 19.434624 41.285991 -135)
    (fp_text reference "C956" (at 0.009644 -1.681014 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144 225) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.9144 225) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 45.014761 59.650241 180)
    (fp_text reference "C1110" (at -2.2225 -2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 36.904617 35.651001 90)
    (fp_text reference "C591" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 739 "MVREFD_D"))
  )
  (footprint "SOT23_3PIN_1" (layer "B.Cu")
    (tedit 0)
    (at -6.091385 78.258002 180)
    (fp_text reference "Q840" (at -1.38115 -1.381125 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9398 1.143 180) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 833 "N87189147"))
    (pad "2" smd rect (at -0.9398 1.143 180) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "3" smd rect (at 0 -1.143 180) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 838 "N87189202"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -13.695383 22.951001 -135)
    (fp_text reference "C561" (at 0 -2.694077 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 225) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 225) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "SMIND1005_0_5H_1" (layer "B.Cu")
    (tedit 0)
    (at 95.104628 18.751009 180)
    (fp_text reference "B352" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 401 "N49337966"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 58.324818 50.707816 45)
    (fp_text reference "C971" (at 0 2.694077 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 45) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 45) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 50.504616 66.951014 -90)
    (fp_text reference "C978" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "NET_SHORT_1" (layer "B.Cu")
    (tedit 0)
    (at 53.405804 59.098706)
    (fp_text reference "NS121" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 0.550012 0.550012) (drill 0.250012) (layers *.Cu *.Mask)
      (net 4 "GND"))
    (pad "2" smd circle (at -0.2 0) (size 0.127 0.127) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 733 "GND_VSSRHB"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 43.004605 55.644407 180)
    (fp_text reference "C1134" (at -2.2225 -2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1608_1" (layer "B.Cu")
    (tedit 0)
    (at 100.904616 59.451004)
    (fp_text reference "C279" (at 1.904975 1.905025 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.7874) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 96.704625 82.951008 90)
    (fp_text reference "C219" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 26.206214 20.226012)
    (fp_text reference "C506" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 41.973111 61.690852 180)
    (fp_text reference "C1127" (at -2.2225 -2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 84.804623 41.750988)
    (fp_text reference "C323" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 88.804615 58.751005 180)
    (fp_text reference "C280" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "GEOM0001_1" (layer "B.Cu")
    (tedit 0)
    (at 0.804613 69.851008 -90)
    (fp_text reference "U861" (at 1.8923 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd oval (at 1.905 2.8448 270) (size 0.639978 1.579982) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "2" smd oval (at 0.635 2.8448 270) (size 0.639978 1.579982) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 24 "LDO_EN"))
    (pad "3" smd oval (at -0.635 2.8448 270) (size 0.639978 1.579982) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 23 "LDO2_VIN"))
    (pad "4" smd oval (at -1.905 2.8448 270) (size 0.639978 1.579982) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 8 "+5V"))
    (pad "5" smd oval (at -1.905 -2.8702 270) (size 0.639978 1.579982) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 20 "N87118444"))
    (pad "6" smd oval (at -0.635 -2.8702 270) (size 0.639978 1.579982) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 22 "+1.8V"))
    (pad "7" smd oval (at 0.635 -2.8702 270) (size 0.639978 1.579982) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 21 "LDO2_FB"))
    (pad "8" smd oval (at 1.905 -2.8702 270) (size 0.639978 1.579982) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "9" smd rect (at 0 0 270) (size 4.099992 2.799994) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 37.804616 10.451 180)
    (fp_text reference "C468" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 59.504623 66.050991)
    (fp_text reference "R392" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 760 "MVREFD_B"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 20.004626 45.051007 90)
    (fp_text reference "C77" (at -1.27 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 795 "+VDD_CT"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 35.982851 61.673072 180)
    (fp_text reference "C1129" (at -2.2225 -2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1608_1" (layer "B.Cu")
    (tedit 0)
    (at -28.443385 77.496002)
    (fp_text reference "ER304" (at 2.222475 2.540025 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 81 "N87528545"))
    (pad "2" smd rect (at 0 0.7874) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 8 "+5V"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 50.804615 72.051004 90)
    (fp_text reference "C987" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1608_1" (layer "B.Cu")
    (tedit 0)
    (at 101.504615 48.251001 180)
    (fp_text reference "C329" (at -1.904975 -1.905025 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 180) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.7874 180) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 8.759614 84.862993)
    (fp_text reference "R856" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 25 "N87118142"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 8 "+5V"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -15.055375 51.95841)
    (fp_text reference "R68" (at 1.5875 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "+3.3V"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 792 "PSYNC"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -1.963885 75.464002 -90)
    (fp_text reference "R845" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 24 "LDO_EN"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 31 "+3.3V_BUS"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 89.304614 91.350991 -90)
    (fp_text reference "C230" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1608_1" (layer "B.Cu")
    (tedit 0)
    (at 161.421615 22.378002 90)
    (fp_text reference "ER19" (at -1.905025 1.904975 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 90) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 31 "+3.3V_BUS"))
    (pad "2" smd rect (at 0 0.7874 90) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 852 "N86495698"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 85.304622 19.451008 180)
    (fp_text reference "C375" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -10.145377 22.151002 180)
    (fp_text reference "R551" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 99 "CLKD1"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "GEOM0008_1" (layer "B.Cu")
    (tedit 0)
    (at 17.204606 46.251005)
    (fp_text reference "B110" (at 1.181837 1.195476 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 22 "+1.8V"))
    (pad "2" smd rect (at 0 0.9144) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 682 "+TXVDDR"))
  )
  (footprint "SOT23_3PIN_1" (layer "B.Cu")
    (tedit 0)
    (at 165.231615 23.267002 -90)
    (fp_text reference "Q993" (at 1.381125 -1.38115 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9398 1.143 270) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 852 "N86495698"))
    (pad "2" smd rect (at -0.9398 1.143 270) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "3" smd rect (at 0 -1.143 270) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 851 "N86495700"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 93.704605 91.450991 90)
    (fp_text reference "C231" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 585 "N25404871"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 96.304626 60.851001 90)
    (fp_text reference "C251" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 94.104605 78.750991 180)
    (fp_text reference "C232" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 584 "N25405001"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 65.504611 100.650998 180)
    (fp_text reference "C35" (at -1.5875 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 891 "PERP14"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 721 "GFXTP14_PERP14"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 87.204618 19.151008 -90)
    (fp_text reference "C363" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 85.404622 90.250993 180)
    (fp_text reference "C216" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "SMIND1005_0_5H_1" (layer "B.Cu")
    (tedit 0)
    (at 51.803622 60.966012 90)
    (fp_text reference "B121" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 761 "+VDDRHB"))
  )
  (footprint "GEOM0013_1" (layer "B.Cu")
    (tedit 0)
    (at 7.304626 68.95101 90)
    (fp_text reference "C861" (at -1.195476 1.181837 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144 90) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 22 "+1.8V"))
    (pad "2" smd rect (at 0 0.9144 90) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 94.804629 43.050986 45)
    (fp_text reference "R302" (at 0 2.694077 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 45) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 414 "CLKB0B"))
    (pad "2" smd rect (at 0 0.492608 45) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 55.004607 22.351002)
    (fp_text reference "C423" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -19.23238 52.9436 180)
    (fp_text reference "MR73" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 650 "VID_3"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 40.059628 49.391004 -90)
    (fp_text reference "C133" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1608_0_8H_1" (layer "B.Cu")
    (tedit 0)
    (at -32.795396 52.151018)
    (fp_text reference "ML2001" (at 2.539975 3.175025 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 41 "A_DAC2_R"))
    (pad "2" smd rect (at 0 0.7874) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 42 "A_R_DAC2_F"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 41.009943 59.645161 180)
    (fp_text reference "C179" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1608_1" (layer "B.Cu")
    (tedit 0)
    (at 34.404622 6.251009 90)
    (fp_text reference "C479" (at -1.905025 1.904975 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 90) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.7874 90) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 30.704604 47.351003 -90)
    (fp_text reference "C155" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "GEOM0013_1" (layer "B.Cu")
    (tedit 0)
    (at 54.584618 37.691002 135)
    (fp_text reference "C958" (at -1.681014 -0.009644 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144 135) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.9144 135) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -29.280391 46.351005 180)
    (fp_text reference "R2029" (at -2.2225 -2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 705 "A_DAC2_BB"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 42.504606 100.650998 180)
    (fp_text reference "C24" (at -1.5875 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 883 "PERN8"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 635 "GFXTN8_PERN8"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 53.804609 12.550996 -90)
    (fp_text reference "C431" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 330 "N48027790"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 45.404626 73.951 90)
    (fp_text reference "R294" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 719 "MVREFS_A"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 21.504623 53.651015 -90)
    (fp_text reference "C97" (at 1.27 -1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 680 "+VDDR_DVP"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "TP089X043_1" (layer "B.Cu")
    (tedit 0)
    (at 30.104606 52.750992)
    (fp_text reference "TP82" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 0.5588 0.5588) (drill 0.250012) (layers *.Cu *.Mask)
      (net 828 "DVPDATA_22"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -33.195395 84.951004 180)
    (fp_text reference "R1007" (at -2.2225 -2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 765 "DDC1CLK"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "+3.3V"))
  )
  (footprint "SMIND1005_0_5H_1" (layer "B.Cu")
    (tedit 0)
    (at 24.364612 12.585997 -90)
    (fp_text reference "B501" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 202 "N48569853"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 95.704601 46.751004 -90)
    (fp_text reference "C304" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "GEOM0013_1" (layer "B.Cu")
    (tedit 0)
    (at 5.95962 88.363011)
    (fp_text reference "C851" (at 1.181837 1.195476 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 27 "+1.1V"))
    (pad "2" smd rect (at 0 0.9144) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 25.104616 73.851 -135)
    (fp_text reference "C1022" (at 0.224506 -3.367596 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 225) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 632 "+AVDD"))
    (pad "2" smd rect (at 0 0.492608 225) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 631 "GND_AVSSQ"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 94.619615 61.545996 45)
    (fp_text reference "R251" (at 0 2.694077 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 45) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 481 "CLKA1"))
    (pad "2" smd rect (at 0 0.492608 45) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 55.804605 9.251003 90)
    (fp_text reference "C404" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 34.804622 51.450994)
    (fp_text reference "R44" (at 1.5875 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 821 "VREFG"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 41.009689 57.644911 180)
    (fp_text reference "C166" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 87.504618 23.550999 -90)
    (fp_text reference "C357" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 42.904605 21.351004 180)
    (fp_text reference "C458" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -11.005396 56.343593 180)
    (fp_text reference "MR77" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 710 "VID_7"))
  )
  (footprint "SMIND1005_0_5H_1" (layer "B.Cu")
    (tedit 0)
    (at 63.904614 12.650996 -90)
    (fp_text reference "B401" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 329 "N48027732"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 91.50461 92.351014 -90)
    (fp_text reference "C235" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 585 "N25404871"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 43.404604 9.151003)
    (fp_text reference "C467" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 39.004613 17.951011 90)
    (fp_text reference "C461" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1608_1" (layer "B.Cu")
    (tedit 0)
    (at 34.404622 54.150989)
    (fp_text reference "MC1139" (at 2.539975 3.175025 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.7874) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 33.604624 13.050995 -90)
    (fp_text reference "C481" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 274 "N48027825"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 92.744612 22.805992)
    (fp_text reference "R356" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 353 "RASB1B"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -38.603385 56.033002)
    (fp_text reference "MR79" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "HSYNC2"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 94.544609 77.361001 90)
    (fp_text reference "C237" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 586 "N25404815"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -35.936385 67.082002 180)
    (fp_text reference "R66" (at -1.5875 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "+3.3V"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 6 "VSYNC1"))
  )
  (footprint "CAP1608_1" (layer "B.Cu")
    (tedit 0)
    (at 101.504615 68.351011 180)
    (fp_text reference "C277" (at -1.904975 -1.905025 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 180) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.7874 180) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 44.204603 39.650993 180)
    (fp_text reference "C131" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 24.504617 63.350996 90)
    (fp_text reference "C64" (at -1.27 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 674 "+DPLL_VDDC"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 673 "GND_PVSS"))
  )
  (footprint "F_PAD_M120_1" (layer "B.Cu")
    (tedit 0)
    (at -18.537385 11.202002)
    (fp_text reference "FM6" (at -0.762501 -0.000013 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd circle (at 0 0) (size 1.020064 1.020064) (layers "B.Cu" "B.Paste" "B.Mask"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 50.704615 11.050999)
    (fp_text reference "R421" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 332 "N48027731"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 88.984625 43.45101 -90)
    (fp_text reference "C310" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -15.055375 52.9436 180)
    (fp_text reference "MR68" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 792 "PSYNC"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 39.804612 36.850998 -90)
    (fp_text reference "C594" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 738 "MVREFS_D"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -25.165388 22.231012 -90)
    (fp_text reference "MR59" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 595 "GPIO_9_R"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 38.014775 55.649487)
    (fp_text reference "C946" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1608_1" (layer "B.Cu")
    (tedit 0)
    (at 127.639615 8.916002 180)
    (fp_text reference "ER14" (at -1.904975 -1.905025 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 180) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 60 "+12V_EXT"))
    (pad "2" smd rect (at 0 0.7874 180) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 857 "N85769033"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -0.795383 66.55099 90)
    (fp_text reference "C868" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 8 "+5V"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "SOT23_3PIN_1" (layer "B.Cu")
    (tedit 0)
    (at -35.895389 92.251014 90)
    (fp_text reference "Q1001" (at -1.4732 1.289075 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9398 1.143 90) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "+3.3V"))
    (pad "2" smd rect (at -0.9398 1.143 90) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 766 "DDC1DATA"))
    (pad "3" smd rect (at 0 -1.143 90) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 844 "DDCDATA_DAC1_5V"))
  )
  (footprint "SMIND1005_0_5H_1" (layer "B.Cu")
    (tedit 0)
    (at 16.704607 67.851012 90)
    (fp_text reference "B2021" (at -2.54 2.2225 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 22 "+1.8V"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 694 "+VDD2DI"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 84.622023 40.094197 -90)
    (fp_text reference "C324" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 58.404625 55.850986 135)
    (fp_text reference "C972" (at -2.694077 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 135) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 135) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "TP089X043_1" (layer "B.Cu")
    (tedit 0)
    (at 27.814618 51.610989)
    (fp_text reference "TP75" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 0.5588 0.5588) (drill 0.250012) (layers *.Cu *.Mask)
      (net 786 "DVPDATA_15"))
  )
  (footprint "CAP1608_1" (layer "B.Cu")
    (tedit 0)
    (at 41.300341 63.676395 -90)
    (fp_text reference "MC1125" (at 3.175025 -2.539975 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 270) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 735 "+VDDC"))
    (pad "2" smd rect (at 0 0.7874 270) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -3.095379 28.950989 135)
    (fp_text reference "C571" (at -2.694077 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 135) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 135) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "GEOM0008_1" (layer "B.Cu")
    (tedit 0)
    (at 3.404608 50.450996 90)
    (fp_text reference "MB67" (at -1.195476 1.181837 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144 90) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 731 "+MPVDD"))
    (pad "2" smd rect (at 0 0.9144 90) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 17 "+VDDCI_LDO"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 159.389615 39.904002 180)
    (fp_text reference "AC79" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 945 "AICSN1"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1608_1" (layer "B.Cu")
    (tedit 0)
    (at 25.004616 23.351 -90)
    (fp_text reference "C526" (at 1.905025 -1.904975 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 270) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.7874 270) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "GEOM0008_1" (layer "B.Cu")
    (tedit 0)
    (at -32.680384 49.250999 -90)
    (fp_text reference "L2002" (at 1.27033 -1.111516 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144 270) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 39 "A_DAC2_G"))
    (pad "2" smd rect (at 0 0.9144 270) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 40 "A_G_DAC2_F"))
  )
  (footprint "CAP1608_1" (layer "B.Cu")
    (tedit 0)
    (at 59.328804 49.275205 45)
    (fp_text reference "MC959" (at -0.224542 3.367596 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 45) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.7874 45) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 94.104605 38.750994 180)
    (fp_text reference "C332" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 457 "N49337896"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "SMIND1005_0_5H_1" (layer "B.Cu")
    (tedit 0)
    (at 24.604617 72.051004 135)
    (fp_text reference "B2020" (at -3.367596 -0.224506 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 135) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 22 "+1.8V"))
    (pad "2" smd rect (at 0 0.492608 315) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 781 "+A2VDDQ"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 52.594604 63.361004 -90)
    (fp_text reference "C988" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -0.180373 24.810992 -135)
    (fp_text reference "C573" (at 0 -2.694077 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 225) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 225) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 39.384546 46.538304)
    (fp_text reference "C152" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 91.669608 24.050998)
    (fp_text reference "R353" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 408 "CKEB1"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 50.164611 58.505997 -90)
    (fp_text reference "C143" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 96.604625 58.651005 90)
    (fp_text reference "C261" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "+MVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 0.534611 92.865999 90)
    (fp_text reference "C39" (at -1.27 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "+3.3V"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 95.339603 76.57101 90)
    (fp_text reference "R222" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 586 "N25404815"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
  )
)
