(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "1.8V_REG")
  (net 2 "LVDDR")
  (net 3 "VDD_CORE")
  (net 4 "MPVDD")
  (net 5 "N16909622")
  (net 6 "N18849793")
  (net 7 "N18850036")
  (net 8 "N18859523")
  (net 9 "N18859284")
  (net 10 "N18866844")
  (net 11 "N18866342")
  (net 12 "N18875755")
  (net 13 "N18875830")
  (net 14 "N22176053")
  (net 15 "AGND")
  (net 16 "+3VRUN")
  (net 17 "+5VRUN")
  (net 18 "N22665126")
  (net 19 "N22665706")
  (net 20 "VREF_22665604")
  (net 21 "N22665484")
  (net 22 "N22672706")
  (net 23 "N22673014")
  (net 24 "VREF")
  (net 25 "N22672632")
  (net 26 "VDDRHA1")
  (net 27 "N16910486")
  (net 28 "VDDRHA2")
  (net 29 "N16909667")
  (net 30 "VDDRHB1")
  (net 31 "N16910998")
  (net 32 "LPVDD")
  (net 33 "N22176268")
  (net 34 "VDDRHB2")
  (net 35 "N16909550")
  (net 36 "DPLL_PVDD")
  (net 37 "N22176582")
  (net 38 "PCIE_PVDD")
  (net 39 "VDD2DI")
  (net 40 "N22176225")
  (net 41 "VDD1DI")
  (net 42 "N22175888")
  (net 43 "A2VDD")
  (net 44 "DPLL_VDDC")
  (net 45 "N22175956")
  (net 46 "AVDD")
  (net 47 "N22175870")
  (net 48 "DPA_VDDR")
  (net 49 "N22175859")
  (net 50 "DPA_PVDD")
  (net 51 "N22175966")
  (net 52 "N16909654")
  (net 53 "N22276438")
  (net 54 "PCIE_TXN15")
  (net 55 "N22276387")
  (net 56 "PCIE_TXP15")
  (net 57 "N22276563")
  (net 58 "PCIE_TXN14")
  (net 59 "N22276557")
  (net 60 "PCIE_TXP14")
  (net 61 "N22276551")
  (net 62 "PCIE_TXN13")
  (net 63 "N22276545")
  (net 64 "PCIE_TXP13")
  (net 65 "N22276539")
  (net 66 "PCIE_TXN12")
  (net 67 "N22276533")
  (net 68 "PCIE_TXP12")
  (net 69 "N22276527")
  (net 70 "PCIE_TXN11")
  (net 71 "N22276496")
  (net 72 "PCIE_TXP11")
  (net 73 "N22276444")
  (net 74 "PCIE_TXN10")
  (net 75 "N22276440")
  (net 76 "PCIE_TXP10")
  (net 77 "N22276389")
  (net 78 "PCIE_TXN9")
  (net 79 "N22276565")
  (net 80 "PCIE_TXP9")
  (net 81 "N22276559")
  (net 82 "PCIE_TXN8")
  (net 83 "N22276553")
  (net 84 "PCIE_TXP8")
  (net 85 "N22276547")
  (net 86 "PCIE_TXN7")
  (net 87 "N22276541")
  (net 88 "PCIE_TXP7")
  (net 89 "N22276535")
  (net 90 "PCIE_TXN6")
  (net 91 "N22276529")
  (net 92 "PCIE_TXP6")
  (net 93 "N22276498")
  (net 94 "PCIE_TXN5")
  (net 95 "N22276446")
  (net 96 "PCIE_TXP5")
  (net 97 "N22276442")
  (net 98 "PCIE_TXN4")
  (net 99 "N22276391")
  (net 100 "PCIE_TXP4")
  (net 101 "N22276385")
  (net 102 "PCIE_TXN3")
  (net 103 "N22276561")
  (net 104 "PCIE_TXP3")
  (net 105 "N22276555")
  (net 106 "PCIE_TXN2")
  (net 107 "N22276549")
  (net 108 "PCIE_TXP2")
  (net 109 "N22276543")
  (net 110 "PCIE_TXN1")
  (net 111 "N22276537")
  (net 112 "PCIE_TXP1")
  (net 113 "N22276531")
  (net 114 "PCIE_TXN0")
  (net 115 "N22276525")
  (net 116 "PCIE_TXP0")
  (net 117 "N22176231")
  (net 118 "N22176381")
  (net 119 "N22175861")
  (net 120 "VDDR3")
  (net 121 "N16912873")
  (net 122 "N16919383")
  (net 123 "N16919381")
  (net 124 "DPB_PVDD")
  (net 125 "N22175699")
  (net 126 "N16919174")
  (net 127 "DPB_VDDR")
  (net 128 "N22176186")
  (net 129 "N16919368")
  (net 130 "N22625904")
  (net 131 "N22665594")
  (net 132 "N22672648")
  (net 133 "PCIE_VDDC")
  (net 134 "N16910916")
  (net 135 "N22665740")
  (net 136 "N22673140")
  (net 137 "N22665412")
  (net 138 "N22665400")
  (net 139 "N22665482")
  (net 140 "N22672636")
  (net 141 "N22672640")
  (net 142 "G_PWR_SRC")
  (net 143 "N22672644")
  (net 144 "N22176881")
  (net 145 "N22176083")
  (net 146 "D+")
  (net 147 "D-")
  (net 148 "+BBP")
  (net 149 "N22665296")
  (net 150 "N18850055")
  (net 151 "N18859640")
  (net 152 "N18859449")
  (net 153 "N18876007")
  (net 154 "N18876029")
  (net 155 "N18850604")
  (net 156 "N18866671")
  (net 157 "N18866513")
  (net 158 "N18876394")
  (net 159 "N18850123")
  (net 160 "N18859575")
  (net 161 "N18867037")
  (net 162 "DPA0P")
  (net 163 "DVI_CLK-")
  (net 164 "DPA1P")
  (net 165 "DVI_TX0-")
  (net 166 "DPA1N")
  (net 167 "DVI_TX0+")
  (net 168 "DPB0P")
  (net 169 "DVIB_CLK-")
  (net 170 "DPB1P")
  (net 171 "DVIB_TX0-")
  (net 172 "DPA0N")
  (net 173 "DVI_CLK+")
  (net 174 "DPA2P")
  (net 175 "DVI_TX1-")
  (net 176 "DPA2N")
  (net 177 "DVI_TX1+")
  (net 178 "DPA3P")
  (net 179 "DVI_TX2-")
  (net 180 "DPA3N")
  (net 181 "DVI_TX2+")
  (net 182 "DPB0N")
  (net 183 "DVIB_CLK+")
  (net 184 "DPB1N")
  (net 185 "DVIB_TX0+")
  (net 186 "DPB2P")
  (net 187 "DVIB_TX1-")
  (net 188 "DPB2N")
  (net 189 "DVIB_TX1+")
  (net 190 "DPB3P")
  (net 191 "DVIB_TX2-")
  (net 192 "DPB3N")
  (net 193 "DVIB_TX2+")
  (net 194 "N22274400")
  (net 195 "DVI_DETECT")
  (net 196 "N22540247")
  (net 197 "N22538866")
  (net 198 "N22794094")
  (net 199 "N22798927")
  (net 200 "N22276906")
  (net 201 "I2C_CLK")
  (net 202 "I2C_DAT")
  (net 203 "BL_ENA")
  (net 204 "FPVCC")
  (net 205 "TXCLK_L+")
  (net 206 "TXCLK_L-")
  (net 207 "TXOUT_L0+")
  (net 208 "TXOUT_L0-")
  (net 209 "TXOUT_L1+")
  (net 210 "TXOUT_L1-")
  (net 211 "TXOUT_L2+")
  (net 212 "TXOUT_L2-")
  (net 213 "TXOUT_L3+")
  (net 214 "TXOUT_L3-")
  (net 215 "BL_BRIGHT")
  (net 216 "TXCLK_U+")
  (net 217 "TXCLK_U-")
  (net 218 "TXOUT_U0+")
  (net 219 "TXOUT_U0-")
  (net 220 "TXOUT_U1+")
  (net 221 "TXOUT_U1-")
  (net 222 "TXOUT_U2+")
  (net 223 "TXOUT_U2-")
  (net 224 "TXOUT_U3+")
  (net 225 "TXOUT_U3-")
  (net 226 "PCIE_RST#")
  (net 227 "PCIE_RXN0")
  (net 228 "PCIE_RXN1")
  (net 229 "PCIE_RXN10")
  (net 230 "PCIE_RXN11")
  (net 231 "PCIE_RXN12")
  (net 232 "PCIE_RXN13")
  (net 233 "PCIE_RXN14")
  (net 234 "PCIE_RXN15")
  (net 235 "PCIE_RXN2")
  (net 236 "PCIE_RXN3")
  (net 237 "PCIE_RXN4")
  (net 238 "PCIE_RXN5")
  (net 239 "PCIE_RXN6")
  (net 240 "PCIE_RXN7")
  (net 241 "PCIE_RXN8")
  (net 242 "PCIE_RXN9")
  (net 243 "PCIE_RXP0")
  (net 244 "PCIE_RXP1")
  (net 245 "PCIE_RXP10")
  (net 246 "PCIE_RXP11")
  (net 247 "PCIE_RXP12")
  (net 248 "PCIE_RXP13")
  (net 249 "PCIE_RXP14")
  (net 250 "PCIE_RXP15")
  (net 251 "PCIE_RXP2")
  (net 252 "PCIE_RXP3")
  (net 253 "PCIE_RXP4")
  (net 254 "PCIE_RXP5")
  (net 255 "PCIE_RXP6")
  (net 256 "PCIE_RXP7")
  (net 257 "PCIE_RXP8")
  (net 258 "PCIE_RXP9")
  (net 259 "N22275059")
  (net 260 "PCIE_REFCLKP")
  (net 261 "PCIE_REFCLKN")
  (net 262 "CLK_REQB*")
  (net 263 "N22778501")
  (net 264 "N22778505")
  (net 265 "N22274460")
  (net 266 "N22275940")
  (net 267 "AC_BAT")
  (net 268 "N22274456")
  (net 269 "N22275399")
  (net 270 "N22276217")
  (net 271 "N22276768")
  (net 272 "N22774274")
  (net 273 "N22628117")
  (net 274 "SMB_CLK")
  (net 275 "SMB_DAT")
  (net 276 "THERM#")
  (net 277 "TV_COMP_B_PB")
  (net 278 "TV_CR_PR")
  (net 279 "TV_Y_G")
  (net 280 "VGA_BLU")
  (net 281 "DDC1CLK")
  (net 282 "DDC1DATA")
  (net 283 "VGA_GRN")
  (net 284 "HSYNC")
  (net 285 "VGA_RED")
  (net 286 "VSYNC")
  (net 287 "N16912894")
  (net 288 "N16909921")
  (net 289 "MB_THERM#")
  (net 290 "PBAT_SMBCLK")
  (net 291 "PBAT_SMBDAT")
  (net 292 "BB_ENA")
  (net 293 "N22672692")
  (net 294 "POW_SW0")
  (net 295 "N22672726")
  (net 296 "POW_SW1")
  (net 297 "N22316530")
  (net 298 "N22316558")
  (net 299 "CTFB")
  (net 300 "N22177921")
  (net 301 "N22665692")
  (net 302 "N22672940")
  (net 303 "N22665180")
  (net 304 "N22672861")
  (net 305 "N2080875267")
  (net 306 "OPT_BL_ENA")
  (net 307 "DDC2CLK")
  (net 308 "DDC2DATA")
  (net 309 "DDC4CLK")
  (net 310 "DDC4DATA")
  (net 311 "N22471791")
  (net 312 "VHAD0")
  (net 313 "GPIO0")
  (net 314 "GPIO1")
  (net 315 "GPIO2")
  (net 316 "GPIO3")
  (net 317 "GPIO5")
  (net 318 "GPIO9")
  (net 319 "GPIO11")
  (net 320 "GPIO12")
  (net 321 "GPIO13")
  (net 322 "GPIO8")
  (net 323 "GPIO22")
  (net 324 "VID_0")
  (net 325 "VID_1")
  (net 326 "VID_2")
  (net 327 "VID_3")
  (net 328 "VID_4")
  (net 329 "VID_5")
  (net 330 "VID_6")
  (net 331 "VID_7")
  (net 332 "DVALID")
  (net 333 "PSYNC")
  (net 334 "DDC3DATA")
  (net 335 "DDC3CLK")
  (net 336 "BLON_PWM")
  (net 337 "N22176754")
  (net 338 "DVI_HPD2")
  (net 339 "DVI_HPD3")
  (net 340 "N22625856")
  (net 341 "RUNPWROK")
  (net 342 "OTEMP#")
  (net 343 "THERM_SCLK")
  (net 344 "N21377273")
  (net 345 "THERM_SDAT")
  (net 346 "N21377265")
  (net 347 "N21360761")
  (net 348 "N17821681")
  (net 349 "N17821689")
  (net 350 "MEM_ID0")
  (net 351 "MEM_ID1")
  (net 352 "MEM_ID2")
  (net 353 "MEM_ID3")
  (net 354 "RUNPWROK_1")
  (net 355 "N22175845")
  (net 356 "VIN_22665782")
  (net 357 "VIN")
  (net 358 "N16919725")
  (net 359 "N16919341")
  (net 360 "N2080875268")
  (net 361 "N22176800")
  (net 362 "N16920644")
  (net 363 "N16919162")
  (net 364 "CLKA0#")
  (net 365 "CLKA0")
  (net 366 "CLKB0#")
  (net 367 "CLKB0")
  (net 368 "CLKA1#")
  (net 369 "CLKA1")
  (net 370 "CLKB1#")
  (net 371 "CLKB1")
  (net 372 "SCLK")
  (net 373 "CASA#0")
  (net 374 "CASA#1")
  (net 375 "CKEA0")
  (net 376 "CKEA1")
  (net 377 "CSA0_0#")
  (net 378 "CSA1_0#")
  (net 379 "MDA0")
  (net 380 "MDA1")
  (net 381 "MDA10")
  (net 382 "MDA11")
  (net 383 "MDA12")
  (net 384 "MDA13")
  (net 385 "MDA14")
  (net 386 "MDA15")
  (net 387 "MDA16")
  (net 388 "MDA17")
  (net 389 "MDA18")
  (net 390 "MDA19")
  (net 391 "MDA2")
  (net 392 "MDA20")
  (net 393 "MDA21")
  (net 394 "MDA22")
  (net 395 "MDA23")
  (net 396 "MDA24")
  (net 397 "MDA25")
  (net 398 "MDA26")
  (net 399 "MDA27")
  (net 400 "MDA28")
  (net 401 "MDA29")
  (net 402 "MDA3")
  (net 403 "MDA30")
  (net 404 "MDA31")
  (net 405 "MDA32")
  (net 406 "MDA33")
  (net 407 "MDA34")
  (net 408 "MDA35")
  (net 409 "MDA36")
  (net 410 "MDA37")
  (net 411 "MDA38")
  (net 412 "MDA39")
  (net 413 "MDA4")
  (net 414 "MDA40")
  (net 415 "MDA41")
  (net 416 "MDA42")
  (net 417 "MDA43")
  (net 418 "MDA44")
  (net 419 "MDA45")
  (net 420 "MDA46")
  (net 421 "MDA47")
  (net 422 "MDA48")
  (net 423 "MDA49")
  (net 424 "MDA5")
  (net 425 "MDA50")
  (net 426 "MDA51")
  (net 427 "MDA52")
  (net 428 "MDA53")
  (net 429 "MDA54")
  (net 430 "MDA55")
  (net 431 "MDA56")
  (net 432 "MDA57")
  (net 433 "MDA58")
  (net 434 "MDA59")
  (net 435 "MDA6")
  (net 436 "MDA60")
  (net 437 "MDA61")
  (net 438 "MDA62")
  (net 439 "MDA63")
  (net 440 "MDA7")
  (net 441 "MDA8")
  (net 442 "MDA9")
  (net 443 "DQMA#0")
  (net 444 "DQMA#1")
  (net 445 "DQMA#2")
  (net 446 "DQMA#3")
  (net 447 "DQMA#4")
  (net 448 "DQMA#5")
  (net 449 "DQMA#6")
  (net 450 "DQMA#7")
  (net 451 "MAA0")
  (net 452 "MAA1")
  (net 453 "MAA10")
  (net 454 "MAA11")
  (net 455 "MAA2")
  (net 456 "MAA3")
  (net 457 "MAA4")
  (net 458 "MAA5")
  (net 459 "MAA6")
  (net 460 "MAA7")
  (net 461 "MAA8")
  (net 462 "MAA9")
  (net 463 "MAA12")
  (net 464 "A_BA0")
  (net 465 "A_BA1")
  (net 466 "A_BA2")
  (net 467 "ODTA0")
  (net 468 "ODTA1")
  (net 469 "QSA0")
  (net 470 "QSA#0")
  (net 471 "QSA1")
  (net 472 "QSA#1")
  (net 473 "QSA2")
  (net 474 "QSA#2")
  (net 475 "QSA3")
  (net 476 "QSA#3")
  (net 477 "QSA4")
  (net 478 "QSA#4")
  (net 479 "QSA5")
  (net 480 "QSA#5")
  (net 481 "QSA6")
  (net 482 "QSA#6")
  (net 483 "QSA7")
  (net 484 "QSA#7")
  (net 485 "RASA#0")
  (net 486 "RASA#1")
  (net 487 "WEA#0")
  (net 488 "WEA#1")
  (net 489 "CASB#0")
  (net 490 "CASB#1")
  (net 491 "CKEB0")
  (net 492 "CKEB1")
  (net 493 "CSB0_0#")
  (net 494 "CSB1_0#")
  (net 495 "MDB0")
  (net 496 "MDB1")
  (net 497 "MDB10")
  (net 498 "MDB11")
  (net 499 "MDB12")
  (net 500 "MDB13")
  (net 501 "MDB14")
  (net 502 "MDB15")
  (net 503 "MDB16")
  (net 504 "MDB17")
  (net 505 "MDB18")
  (net 506 "MDB19")
  (net 507 "MDB2")
  (net 508 "MDB20")
  (net 509 "MDB21")
  (net 510 "MDB22")
  (net 511 "MDB23")
  (net 512 "MDB24")
  (net 513 "MDB25")
  (net 514 "MDB26")
  (net 515 "MDB27")
  (net 516 "MDB28")
  (net 517 "MDB29")
  (net 518 "MDB3")
  (net 519 "MDB30")
  (net 520 "MDB31")
  (net 521 "MDB32")
  (net 522 "MDB33")
  (net 523 "MDB34")
  (net 524 "MDB35")
  (net 525 "MDB36")
  (net 526 "MDB37")
  (net 527 "MDB38")
  (net 528 "MDB39")
  (net 529 "MDB4")
  (net 530 "MDB40")
  (net 531 "MDB41")
  (net 532 "MDB42")
  (net 533 "MDB43")
  (net 534 "MDB44")
  (net 535 "MDB45")
  (net 536 "MDB46")
  (net 537 "MDB47")
  (net 538 "MDB48")
  (net 539 "MDB49")
  (net 540 "MDB5")
  (net 541 "MDB50")
  (net 542 "MDB51")
  (net 543 "MDB52")
  (net 544 "MDB53")
  (net 545 "MDB54")
  (net 546 "MDB55")
  (net 547 "MDB56")
  (net 548 "MDB57")
  (net 549 "MDB58")
  (net 550 "MDB59")
  (net 551 "MDB6")
  (net 552 "MDB60")
  (net 553 "MDB61")
  (net 554 "MDB62")
  (net 555 "MDB63")
  (net 556 "MDB7")
  (net 557 "MDB8")
  (net 558 "MDB9")
  (net 559 "DQMB#0")
  (net 560 "DQMB#1")
  (net 561 "DQMB#2")
  (net 562 "DQMB#3")
  (net 563 "DQMB#4")
  (net 564 "DQMB#5")
  (net 565 "DQMB#6")
  (net 566 "DQMB#7")
  (net 567 "MAB0")
  (net 568 "MAB1")
  (net 569 "MAB10")
  (net 570 "MAB11")
  (net 571 "MAB2")
  (net 572 "MAB3")
  (net 573 "MAB4")
  (net 574 "MAB5")
  (net 575 "MAB6")
  (net 576 "MAB7")
  (net 577 "MAB8")
  (net 578 "MAB9")
  (net 579 "MAB12")
  (net 580 "B_BA0")
  (net 581 "B_BA1")
  (net 582 "B_BA2")
  (net 583 "ODTB0")
  (net 584 "ODTB1")
  (net 585 "QSB0")
  (net 586 "QSB#0")
  (net 587 "QSB1")
  (net 588 "QSB#1")
  (net 589 "QSB2")
  (net 590 "QSB#2")
  (net 591 "QSB3")
  (net 592 "QSB#3")
  (net 593 "QSB4")
  (net 594 "QSB#4")
  (net 595 "QSB5")
  (net 596 "QSB#5")
  (net 597 "QSB6")
  (net 598 "QSB#6")
  (net 599 "QSB7")
  (net 600 "QSB#7")
  (net 601 "RASB#0")
  (net 602 "RASB#1")
  (net 603 "WEB#0")
  (net 604 "WEB#1")
  (net 605 "N22625885")
  (net 606 "N22625842")
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -51.797999 28.009995 -90)
    (fp_text reference "R149" (at 1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 327 "VID_3"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "+3VRUN"))
  )
  (footprint "lib:GEOM0009_1" (layer "F.Cu")
    (tedit 0)
    (at -25.498001 42.609991 -90)
    (fp_text reference "U1" (at 0 0.635 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "A2" smd circle (at -12.8 -13.599998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "A3" smd circle (at -12.000001 -13.599998 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 367 "CLKB0"))
    (pad "A4" smd circle (at -11.200003 -13.599998 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "A5" smd circle (at -10.400005 -13.199999 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 517 "MDB29"))
    (pad "A6" smd circle (at -9.600006 -13.599998 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 592 "QSB#3"))
    (pad "A7" smd circle (at -8.800008 -13.199999 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 515 "MDB27"))
    (pad "A8" smd circle (at -8.000009 -13.599998 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "A9" smd circle (at -7.200011 -13.199999 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 501 "MDB14"))
    (pad "A10" smd circle (at -6.400013 -13.599998 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 588 "QSB#1"))
    (pad "A11" smd circle (at -5.599989 -13.199999 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "A12" smd circle (at -4.79999 -13.599998 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "A13" smd circle (at -3.999992 -13.199999 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 129 "N16919368"))
    (pad "A14" smd circle (at -3.199994 -13.599998 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "MPVDD"))
    (pad "A15" smd circle (at -2.399995 -13.199999 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 430 "MDA55"))
    (pad "A16" smd circle (at -1.599997 -13.599998 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "A17" smd circle (at -0.799998 -13.199999 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 482 "QSA#6"))
    (pad "A18" smd circle (at 0 -13.599998 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "A19" smd circle (at 0.799998 -13.199999 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 425 "MDA50"))
    (pad "A20" smd circle (at 1.599997 -13.599998 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "A21" smd circle (at 2.399995 -13.199999 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "A22" smd circle (at 3.199994 -13.599998 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 478 "QSA#4"))
    (pad "A23" smd circle (at 3.999992 -13.199999 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 408 "MDA35"))
    (pad "A24" smd circle (at 4.79999 -13.599998 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "A25" smd circle (at 5.599989 -13.199999 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "VDDRHA1"))
    (pad "A26" smd circle (at 6.399987 -13.599998 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 369 "CLKA1"))
    (pad "A27" smd circle (at 7.200011 -13.199999 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 454 "MAA11"))
    (pad "A28" smd circle (at 8.000009 -13.599998 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "A29" smd circle (at 8.800008 -13.199999 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "A30" smd circle (at 9.600006 -13.599998 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 377 "CSA0_0#"))
    (pad "A31" smd circle (at 10.400005 -13.199999 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 485 "RASA#0"))
    (pad "A32" smd circle (at 11.200003 -13.599998 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "VDDRHA2"))
    (pad "A33" smd circle (at 12.000001 -13.599998 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 365 "CLKA0"))
    (pad "A34" smd circle (at 12.8 -13.599998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "A35" smd circle (at 13.599998 -13.599998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AA1" smd circle (at -13.199999 2.399995 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 546 "MDB55"))
    (pad "AA2" smd circle (at -12.400001 2.399995 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 545 "MDB54"))
    (pad "AA3" smd circle (at -11.600002 2.399995 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AA4" smd circle (at -10.800004 2.399995 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AA5" smd circle (at -10.000005 2.399995 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 363 "N16919162"))
    (pad "AA6" smd circle (at -9.200007 2.399995 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AA7" smd circle (at -8.400009 2.399995 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 359 "N16919341"))
    (pad "AA8" smd circle (at -7.60001 2.399995 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 358 "N16919725"))
    (pad "AA9" smd circle (at -6.800012 2.399995 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AA10" smd circle (at -6.000013 2.399995 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AA11" smd circle (at -5.19999 2.399995 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 52 "N16909654"))
    (pad "AA13" smd circle (at -3.999992 1.999996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AA14" smd circle (at -2.999994 1.999996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AA15" smd circle (at -1.999996 1.999996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "VDD_CORE"))
    (pad "AA17" smd circle (at -0.999998 1.999996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AA18" smd circle (at 0 1.999996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "VDD_CORE"))
    (pad "AA19" smd circle (at 0.999998 1.999996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AA21" smd circle (at 1.999996 1.999996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "VDD_CORE"))
    (pad "AA22" smd circle (at 2.999994 1.999996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AA23" smd circle (at 3.999992 1.999996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "VDD_CORE"))
    (pad "AA25" smd circle (at 5.19999 2.399995 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 133 "PCIE_VDDC"))
    (pad "AA26" smd circle (at 5.999988 2.399995 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 133 "PCIE_VDDC"))
    (pad "AA27" smd circle (at 6.799986 2.399995 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 82 "PCIE_TXN8"))
    (pad "AA28" smd circle (at 7.60001 2.399995 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 84 "PCIE_TXP8"))
    (pad "AA29" smd circle (at 8.400009 2.399995 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AA30" smd circle (at 9.200007 2.399995 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 86 "PCIE_TXN7"))
    (pad "AA31" smd circle (at 10.000005 2.399995 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 88 "PCIE_TXP7"))
    (pad "AA32" smd circle (at 10.800004 2.399995 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AA33" smd circle (at 11.600002 2.399995 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 241 "PCIE_RXN8"))
    (pad "AA34" smd circle (at 12.400001 2.399995 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 242 "PCIE_RXN9"))
    (pad "AA35" smd circle (at 13.199999 2.399995 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 258 "PCIE_RXP9"))
    (pad "AB1" smd circle (at -13.599998 3.199994 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AB2" smd circle (at -12.8 3.199994 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 294 "POW_SW0"))
    (pad "AB3" smd circle (at -11.600002 3.199994 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 338 "DVI_HPD2"))
    (pad "AB4" smd circle (at -10.800004 3.599993 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AB5" smd circle (at -10.000005 3.599993 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AB6" smd circle (at -9.200007 3.599993 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AB7" smd circle (at -8.400009 3.599993 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AB8" smd circle (at -7.60001 3.599993 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AB9" smd circle (at -6.800012 3.599993 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AB10" smd circle (at -6.000013 3.599993 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AB11" smd circle (at -5.19999 3.599993 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 52 "N16909654"))
    (pad "AB13" smd circle (at -3.999992 2.999994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AB14" smd circle (at -2.999994 2.999994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "VDD_CORE"))
    (pad "AB15" smd circle (at -1.999996 2.999994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AB17" smd circle (at -0.999998 2.999994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "VDD_CORE"))
    (pad "AB18" smd circle (at 0 2.999994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AB19" smd circle (at 0.999998 2.999994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "VDD_CORE"))
    (pad "AB21" smd circle (at 1.999996 2.999994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AB22" smd circle (at 2.999994 2.999994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "VDD_CORE"))
    (pad "AB23" smd circle (at 3.999992 2.999994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AB25" smd circle (at 5.19999 3.599993 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 133 "PCIE_VDDC"))
    (pad "AB26" smd circle (at 5.999988 3.599993 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 133 "PCIE_VDDC"))
    (pad "AB27" smd circle (at 6.799986 3.599993 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 90 "PCIE_TXN6"))
    (pad "AB28" smd circle (at 7.60001 3.599993 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 92 "PCIE_TXP6"))
    (pad "AB29" smd circle (at 8.400009 3.599993 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AB30" smd circle (at 9.200007 3.599993 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 94 "PCIE_TXN5"))
    (pad "AB31" smd circle (at 10.000005 3.599993 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 96 "PCIE_TXP5"))
    (pad "AB32" smd circle (at 10.800004 3.599993 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AB33" smd circle (at 11.600002 3.199994 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 257 "PCIE_RXP8"))
    (pad "AB34" smd circle (at 12.8 3.199994 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AB35" smd circle (at 13.599998 3.199994 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AC1" smd circle (at -13.199999 3.999992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 321 "GPIO13"))
    (pad "AC2" smd circle (at -12.400001 3.999992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 320 "GPIO12"))
    (pad "AC3" smd circle (at -11.600002 3.999992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 319 "GPIO11"))
    (pad "AC13" smd circle (at -3.999992 3.999992 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "VDD_CORE"))
    (pad "AC14" smd circle (at -2.999994 3.999992 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AC15" smd circle (at -1.999996 3.999992 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "VDD_CORE"))
    (pad "AC17" smd circle (at -0.999998 3.999992 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AC18" smd circle (at 0 3.999992 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "VDD_CORE"))
    (pad "AC19" smd circle (at 0.999998 3.999992 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AC21" smd circle (at 1.999996 3.999992 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "VDD_CORE"))
    (pad "AC22" smd circle (at 2.999994 3.999992 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AC23" smd circle (at 3.999992 3.999992 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "VDD_CORE"))
    (pad "AC33" smd circle (at 11.600002 3.999992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AC34" smd circle (at 12.400001 3.999992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 240 "PCIE_RXN7"))
    (pad "AC35" smd circle (at 13.199999 3.999992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 256 "PCIE_RXP7"))
    (pad "AD1" smd circle (at -13.599998 4.79999 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 322 "GPIO8"))
    (pad "AD2" smd circle (at -12.8 4.79999 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 306 "OPT_BL_ENA"))
    (pad "AD3" smd circle (at -12.000001 4.79999 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AD4" smd circle (at -10.800004 4.79999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 372 "SCLK"))
    (pad "AD5" smd circle (at -10.000005 4.79999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 318 "GPIO9"))
    (pad "AD6" smd circle (at -9.200007 4.79999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AD7" smd circle (at -8.400009 4.79999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 262 "CLK_REQB*"))
    (pad "AD8" smd circle (at -7.60001 4.79999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 323 "GPIO22"))
    (pad "AD9" smd circle (at -6.800012 4.79999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 292 "BB_ENA"))
    (pad "AD10" smd circle (at -6.000013 4.79999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 52 "N16909654"))
    (pad "AD12" smd circle (at -4.79999 4.795012 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "N22176053"))
    (pad "AD24" smd circle (at 4.79999 4.79999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AD26" smd circle (at 5.999988 4.79999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 133 "PCIE_VDDC"))
    (pad "AD27" smd circle (at 6.799986 4.79999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 98 "PCIE_TXN4"))
    (pad "AD28" smd circle (at 7.60001 4.79999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 100 "PCIE_TXP4"))
    (pad "AD29" smd circle (at 8.400009 4.79999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AD30" smd circle (at 9.200007 4.79999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 102 "PCIE_TXN3"))
    (pad "AD31" smd circle (at 10.000005 4.79999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 104 "PCIE_TXP3"))
    (pad "AD32" smd circle (at 10.800004 4.79999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AD33" smd circle (at 12.000001 4.79999 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AD34" smd circle (at 12.8 4.79999 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 239 "PCIE_RXN6"))
    (pad "AD35" smd circle (at 13.599998 4.79999 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 255 "PCIE_RXP6"))
    (pad "AE1" smd circle (at -13.199999 5.599989 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 317 "GPIO5"))
    (pad "AE2" smd circle (at -12.400001 5.599989 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AE3" smd circle (at -11.600002 5.599989 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 316 "GPIO3"))
    (pad "AE14" smd circle (at -3.599993 5.19999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 120 "VDDR3"))
    (pad "AE15" smd circle (at -2.399995 5.19999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 120 "VDDR3"))
    (pad "AE17" smd circle (at -1.199998 5.19999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 120 "VDDR3"))
    (pad "AE18" smd circle (at 0 5.19999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "VDD_CORE"))
    (pad "AE19" smd circle (at 1.199998 5.19999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "VDD_CORE"))
    (pad "AE21" smd circle (at 2.399995 5.19999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "VDD_CORE"))
    (pad "AE22" smd circle (at 3.599993 5.19999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "VDD_CORE"))
    (pad "AE33" smd circle (at 11.600002 5.599989 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 237 "PCIE_RXN4"))
    (pad "AE34" smd circle (at 12.400001 5.599989 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 238 "PCIE_RXN5"))
    (pad "AE35" smd circle (at 13.199999 5.599989 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 254 "PCIE_RXP5"))
    (pad "AF1" smd circle (at -13.599998 6.400013 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 315 "GPIO2"))
    (pad "AF2" smd circle (at -12.8 6.400013 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 314 "GPIO1"))
    (pad "AF3" smd circle (at -11.600002 6.400013 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AF4" smd circle (at -10.800004 5.999988 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 339 "DVI_HPD3"))
    (pad "AF5" smd circle (at -10.000005 5.999988 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 342 "OTEMP#"))
    (pad "AF6" smd circle (at -9.200007 5.999988 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AF7" smd circle (at -8.400009 5.999988 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AF8" smd circle (at -7.60001 5.999988 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AF9" smd circle (at -6.800012 5.999988 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AF10" smd circle (at -6.000013 5.999988 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 52 "N16909654"))
    (pad "AF12" smd circle (at -4.79999 5.999988 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 120 "VDDR3"))
    (pad "AF14" smd circle (at -3.599993 5.999988 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AF15" smd circle (at -2.399995 5.999988 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AF17" smd circle (at -1.199998 5.999988 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AF18" smd circle (at 0 5.999988 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AF19" smd circle (at 1.199998 5.999988 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AF21" smd circle (at 2.399995 5.999988 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AF22" smd circle (at 3.599993 5.999988 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AF24" smd circle (at 4.79999 5.999988 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AF26" smd circle (at 5.999988 5.999988 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 133 "PCIE_VDDC"))
    (pad "AF27" smd circle (at 6.799986 5.999988 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 106 "PCIE_TXN2"))
    (pad "AF28" smd circle (at 7.60001 5.999988 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 108 "PCIE_TXP2"))
    (pad "AF29" smd circle (at 8.400009 5.999988 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AF30" smd circle (at 9.200007 5.999988 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 110 "PCIE_TXN1"))
    (pad "AF31" smd circle (at 10.000005 5.999988 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 112 "PCIE_TXP1"))
    (pad "AF32" smd circle (at 10.800004 5.999988 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AF33" smd circle (at 11.600002 6.400013 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 253 "PCIE_RXP4"))
    (pad "AF34" smd circle (at 12.8 6.400013 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AF35" smd circle (at 13.599998 6.400013 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AG1" smd circle (at -13.199999 7.200011 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AG2" smd circle (at -12.400001 7.200011 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 313 "GPIO0"))
    (pad "AG3" smd circle (at -11.600002 7.200011 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 296 "POW_SW1"))
    (pad "AG4" smd circle (at -10.800004 7.200011 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 300 "N22177921"))
    (pad "AG5" smd circle (at -10.000005 7.200011 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AG6" smd circle (at -9.200007 7.200011 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 195 "DVI_DETECT"))
    (pad "AG7" smd circle (at -8.400009 7.200011 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 336 "BLON_PWM"))
    (pad "AG9" smd circle (at -7.200011 7.220001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AG10" smd circle (at -6.000013 6.800012 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AG12" smd circle (at -4.79999 6.800012 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AG14" smd circle (at -3.599993 6.800012 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 309 "DDC4CLK"))
    (pad "AG15" smd circle (at -2.399995 6.800012 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 355 "N22175845"))
    (pad "AG17" smd circle (at -1.199998 6.800012 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 125 "N22175699"))
    (pad "AG18" smd circle (at 0 6.800012 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AG19" smd circle (at 1.199998 6.800012 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 44 "DPLL_VDDC"))
    (pad "AG21" smd circle (at 2.399995 6.800012 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AG22" smd circle (at 3.599993 6.800012 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 40 "N22176225"))
    (pad "AG24" smd circle (at 4.79999 6.800012 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 222 "TXOUT_U2+"))
    (pad "AG26" smd circle (at 5.999988 6.800012 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 305 "N2080875267"))
    (pad "AG27" smd circle (at 7.220001 7.200011 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AG29" smd circle (at 8.400009 7.200011 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AG30" smd circle (at 9.200007 7.200011 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 114 "PCIE_TXN0"))
    (pad "AG31" smd circle (at 10.000005 7.200011 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 116 "PCIE_TXP0"))
    (pad "AG32" smd circle (at 10.800004 7.200011 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AG33" smd circle (at 11.600002 7.200011 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AG34" smd circle (at 12.400001 7.200011 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 236 "PCIE_RXN3"))
    (pad "AG35" smd circle (at 13.199999 7.200011 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 252 "PCIE_RXP3"))
    (pad "AH1" smd circle (at -13.599998 8.000009 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AH2" smd circle (at -12.8 8.000009 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AH3" smd circle (at -12.000001 8.000009 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AH10" smd circle (at -6.000013 7.60001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 331 "VID_7"))
    (pad "AH12" smd circle (at -4.79999 7.60001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 327 "VID_3"))
    (pad "AH14" smd circle (at -3.599993 7.60001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 310 "DDC4DATA"))
    (pad "AH15" smd circle (at -2.399995 7.60001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 307 "DDC2CLK"))
    (pad "AH17" smd circle (at -1.199998 7.60001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 124 "DPB_PVDD"))
    (pad "AH18" smd circle (at 0 7.60001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AH19" smd circle (at 1.199998 7.60001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 311 "N22471791"))
    (pad "AH21" smd circle (at 2.399995 7.60001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AH22" smd circle (at 3.599993 7.60001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "VDD2DI"))
    (pad "AH24" smd circle (at 4.79999 7.60001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 223 "TXOUT_U2-"))
    (pad "AH26" smd circle (at 5.999988 7.60001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "LVDDR"))
    (pad "AH33" smd circle (at 12.000001 8.000009 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AH34" smd circle (at 12.8 8.000009 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 235 "PCIE_RXN2"))
    (pad "AH35" smd circle (at 13.599998 8.000009 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 251 "PCIE_RXP2"))
    (pad "AJ1" smd circle (at -13.199999 8.800008 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AJ2" smd circle (at -12.400001 8.800008 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AJ3" smd circle (at -11.600002 8.800008 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AJ4" smd circle (at -10.800004 8.400009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 335 "DDC3CLK"))
    (pad "AJ5" smd circle (at -10.000005 8.400009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 334 "DDC3DATA"))
    (pad "AJ6" smd circle (at -9.200007 8.400009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 204 "FPVCC"))
    (pad "AJ7" smd circle (at -8.400009 8.400009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 332 "DVALID"))
    (pad "AJ9" smd circle (at -7.200011 8.400009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AJ10" smd circle (at -6.000013 8.400009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 330 "VID_6"))
    (pad "AJ12" smd circle (at -4.79999 8.400009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 326 "VID_2"))
    (pad "AJ14" smd circle (at -3.599993 8.400009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AJ15" smd circle (at -2.399995 8.400009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 308 "DDC2DATA"))
    (pad "AJ17" smd circle (at -1.199998 8.400009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AJ18" smd circle (at 0 8.400009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AJ19" smd circle (at 1.199998 8.400009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AJ21" smd circle (at 2.399995 8.400009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 361 "N22176800"))
    (pad "AJ22" smd circle (at 3.599993 8.400009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AJ24" smd circle (at 4.79999 8.400009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AJ26" smd circle (at 5.999988 8.400009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "LVDDR"))
    (pad "AJ27" smd circle (at 7.200011 8.400009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 360 "N2080875268"))
    (pad "AJ29" smd circle (at 8.400009 8.400009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AJ30" smd circle (at 9.200007 8.400009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 261 "PCIE_REFCLKN"))
    (pad "AJ31" smd circle (at 10.000005 8.400009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 260 "PCIE_REFCLKP"))
    (pad "AJ32" smd circle (at 10.800004 8.400009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AJ33" smd circle (at 11.600002 8.800008 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 227 "PCIE_RXN0"))
    (pad "AJ34" smd circle (at 12.400001 8.800008 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 228 "PCIE_RXN1"))
    (pad "AJ35" smd circle (at 13.199999 8.800008 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 244 "PCIE_RXP1"))
    (pad "AK1" smd circle (at -13.599998 9.600006 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AK2" smd circle (at -12.8 9.600006 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AK3" smd circle (at -11.600002 9.600006 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AK4" smd circle (at -10.800004 9.600006 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 147 "D-"))
    (pad "AK6" smd circle (at -9.600006 9.625 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 202 "I2C_DAT"))
    (pad "AK7" smd circle (at -8.400009 9.200007 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AK9" smd circle (at -7.200011 9.200007 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AK10" smd circle (at -6.000013 9.200007 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AK12" smd circle (at -4.79999 9.200007 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AK14" smd circle (at -3.599993 9.200007 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AK15" smd circle (at -2.399995 9.200007 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AK17" smd circle (at -1.199998 9.200007 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 277 "TV_COMP_B_PB"))
    (pad "AK18" smd circle (at 0 9.200007 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 279 "TV_Y_G"))
    (pad "AK19" smd circle (at 1.199998 9.200007 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 278 "TV_CR_PR"))
    (pad "AK21" smd circle (at 2.399995 9.200007 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 119 "N22175861"))
    (pad "AK22" smd circle (at 3.599993 9.200007 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "N22176268"))
    (pad "AK24" smd circle (at 4.79999 9.200007 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 216 "TXCLK_U+"))
    (pad "AK26" smd circle (at 5.999988 9.200007 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 224 "TXOUT_U3+"))
    (pad "AK27" smd circle (at 7.200011 9.200007 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 117 "N22176231"))
    (pad "AK29" smd circle (at 8.400009 9.200007 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AK30" smd circle (at 9.619996 9.600006 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AK32" smd circle (at 10.800004 9.600006 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AK33" smd circle (at 11.600002 9.600006 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 243 "PCIE_RXP0"))
    (pad "AK34" smd circle (at 12.8 9.600006 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AK35" smd circle (at 13.599998 9.600006 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AL1" smd circle (at -13.199999 10.400005 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 352 "MEM_ID2"))
    (pad "AL2" smd circle (at -12.400001 10.400005 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 353 "MEM_ID3"))
    (pad "AL3" smd circle (at -11.600002 10.400005 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AL7" smd circle (at -8.400009 10.000005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AL9" smd circle (at -7.200011 10.000005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AL10" smd circle (at -6.000013 10.000005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 329 "VID_5"))
    (pad "AL12" smd circle (at -4.79999 10.000005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 325 "VID_1"))
    (pad "AL14" smd circle (at -3.599993 10.000005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 51 "N22175966"))
    (pad "AL15" smd circle (at -2.399995 10.000005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AL17" smd circle (at -1.199998 10.000005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AL18" smd circle (at 0 10.000005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AL19" smd circle (at 1.199998 10.000005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AL21" smd circle (at 2.399995 10.000005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 118 "N22176381"))
    (pad "AL22" smd circle (at 3.599993 10.000005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "LPVDD"))
    (pad "AL24" smd circle (at 4.79999 10.000005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 217 "TXCLK_U-"))
    (pad "AL26" smd circle (at 5.999988 10.000005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 225 "TXOUT_U3-"))
    (pad "AL27" smd circle (at 7.200011 10.000005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 117 "N22176231"))
    (pad "AL29" smd circle (at 8.400009 10.000005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 281 "DDC1CLK"))
    (pad "AL33" smd circle (at 11.600002 10.400005 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "N16909622"))
    (pad "AL34" smd circle (at 12.400001 10.400005 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AL35" smd circle (at 13.199999 10.400005 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AM1" smd circle (at -13.599998 11.200003 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AM2" smd circle (at -12.8 11.200003 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AM3" smd circle (at -12.000001 11.200003 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AM4" smd circle (at -10.800004 10.800004 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 146 "D+"))
    (pad "AM6" smd circle (at -9.600006 10.800004 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 201 "I2C_CLK"))
    (pad "AM7" smd circle (at -8.400009 10.800004 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 333 "PSYNC"))
    (pad "AM9" smd circle (at -7.200011 10.800004 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 312 "VHAD0"))
    (pad "AM10" smd circle (at -6.000013 10.800004 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 328 "VID_4"))
    (pad "AM12" smd circle (at -4.79999 10.800004 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 324 "VID_0"))
    (pad "AM14" smd circle (at -3.599993 10.800004 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 50 "DPA_PVDD"))
    (pad "AM15" smd circle (at -2.399995 10.800004 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AM17" smd circle (at -1.199998 10.800004 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AM18" smd circle (at 0 10.800004 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AM19" smd circle (at 1.199998 10.800004 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AM21" smd circle (at 2.399995 10.800004 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "A2VDD"))
    (pad "AM22" smd circle (at 3.599993 10.800004 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AM24" smd circle (at 4.79999 10.800004 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AM26" smd circle (at 5.999988 10.800004 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AM27" smd circle (at 7.200011 10.800004 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AM29" smd circle (at 8.400009 10.800004 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 282 "DDC1DATA"))
    (pad "AM30" smd circle (at 9.600006 10.800004 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 362 "N16920644"))
    (pad "AM32" smd circle (at 10.800004 10.800004 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 226 "PCIE_RST#"))
    (pad "AM33" smd circle (at 12.000001 11.200003 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "N16909622"))
    (pad "AM34" smd circle (at 12.8 11.200003 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AM35" smd circle (at 13.599998 11.200003 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "PCIE_PVDD"))
    (pad "AN1" smd circle (at -13.599998 12.000001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 120 "VDDR3"))
    (pad "AN2" smd circle (at -12.8 12.000001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AN3" smd circle (at -12.000001 12.000001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AN4" smd circle (at -11.200003 12.000001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AN5" smd circle (at -10.400005 11.600002 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AN6" smd circle (at -9.600006 11.600002 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AN7" smd circle (at -8.800008 11.600002 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AN8" smd circle (at -8.000009 12.000001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AN9" smd circle (at -7.200011 11.600002 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 162 "DPA0P"))
    (pad "AN10" smd circle (at -6.400013 11.600002 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 172 "DPA0N"))
    (pad "AN11" smd circle (at -5.599989 11.600002 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 49 "N22175859"))
    (pad "AN12" smd circle (at -4.79999 12.000001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 49 "N22175859"))
    (pad "AN13" smd circle (at -3.999992 11.600002 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 49 "N22175859"))
    (pad "AN14" smd circle (at -3.199994 11.600002 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 49 "N22175859"))
    (pad "AN15" smd circle (at -2.399995 11.600002 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 49 "N22175859"))
    (pad "AN16" smd circle (at -1.599997 12.000001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 128 "N22176186"))
    (pad "AN17" smd circle (at -0.799998 11.600002 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 128 "N22176186"))
    (pad "AN18" smd circle (at 0 11.600002 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 128 "N22176186"))
    (pad "AN19" smd circle (at 0.799998 11.600002 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 127 "DPB_VDDR"))
    (pad "AN20" smd circle (at 1.599997 12.000001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 127 "DPB_VDDR"))
    (pad "AN21" smd circle (at 2.399995 11.600002 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AN22" smd circle (at 3.199994 11.600002 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 208 "TXOUT_L0-"))
    (pad "AN23" smd circle (at 3.999992 11.600002 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 207 "TXOUT_L0+"))
    (pad "AN24" smd circle (at 4.79999 12.000001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AN25" smd circle (at 5.599989 11.600002 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AN26" smd circle (at 6.399987 11.600002 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 219 "TXOUT_U0-"))
    (pad "AN27" smd circle (at 7.200011 11.600002 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 218 "TXOUT_U0+"))
    (pad "AN28" smd circle (at 8.000009 12.000001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AN29" smd circle (at 8.800008 11.600002 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 284 "HSYNC"))
    (pad "AN30" smd circle (at 9.600006 11.600002 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 286 "VSYNC"))
    (pad "AN31" smd circle (at 10.400005 11.600002 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 337 "N22176754"))
    (pad "AN32" smd circle (at 11.200003 12.000001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AN33" smd circle (at 12.000001 12.000001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "N16909622"))
    (pad "AN34" smd circle (at 12.8 12.000001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "N16909622"))
    (pad "AN35" smd circle (at 13.599998 12.000001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "N16909622"))
    (pad "AP1" smd circle (at -13.599998 12.8 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 120 "VDDR3"))
    (pad "AP2" smd circle (at -12.8 12.8 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 120 "VDDR3"))
    (pad "AP3" smd circle (at -12.000001 12.8 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AP4" smd circle (at -11.200003 12.8 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AP5" smd circle (at -10.400005 12.400001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 345 "THERM_SDAT"))
    (pad "AP6" smd circle (at -9.600006 12.8 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 343 "THERM_SCLK"))
    (pad "AP7" smd circle (at -8.800008 12.400001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 350 "MEM_ID0"))
    (pad "AP8" smd circle (at -8.000009 12.8 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AP9" smd circle (at -7.200011 12.400001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AP10" smd circle (at -6.400013 12.8 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 166 "DPA1N"))
    (pad "AP11" smd circle (at -5.599989 12.400001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 176 "DPA2N"))
    (pad "AP12" smd circle (at -4.79999 12.8 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 180 "DPA3N"))
    (pad "AP13" smd circle (at -3.999992 12.400001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AP14" smd circle (at -3.199994 12.8 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 182 "DPB0N"))
    (pad "AP15" smd circle (at -2.399995 12.400001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 184 "DPB1N"))
    (pad "AP16" smd circle (at -1.599997 12.8 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 188 "DPB2N"))
    (pad "AP17" smd circle (at -0.799998 12.400001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 192 "DPB3N"))
    (pad "AP18" smd circle (at 0 12.8 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 128 "N22176186"))
    (pad "AP19" smd circle (at 0.799998 12.400001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 48 "DPA_VDDR"))
    (pad "AP20" smd circle (at 1.599997 12.8 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "N22176582"))
    (pad "AP21" smd circle (at 2.399995 12.400001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AP22" smd circle (at 3.199994 12.8 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 206 "TXCLK_L-"))
    (pad "AP23" smd circle (at 3.999992 12.400001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 209 "TXOUT_L1+"))
    (pad "AP24" smd circle (at 4.79999 12.8 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 211 "TXOUT_L2+"))
    (pad "AP25" smd circle (at 5.599989 12.400001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 213 "TXOUT_L3+"))
    (pad "AP26" smd circle (at 6.399987 12.8 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AP27" smd circle (at 7.200011 12.400001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 220 "TXOUT_U1+"))
    (pad "AP28" smd circle (at 8.000009 12.8 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "N22175888"))
    (pad "AP29" smd circle (at 8.800008 12.400001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AP30" smd circle (at 9.600006 12.8 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AP31" smd circle (at 10.400005 12.400001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AP32" smd circle (at 11.200003 12.8 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 47 "N22175870"))
    (pad "AP33" smd circle (at 12.000001 12.8 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 145 "N22176083"))
    (pad "AP34" smd circle (at 12.8 12.8 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "N16909622"))
    (pad "AP35" smd circle (at 13.599998 12.8 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "N16909622"))
    (pad "AR1" smd circle (at -13.599998 13.599998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AR2" smd circle (at -12.8 13.599998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 120 "VDDR3"))
    (pad "AR3" smd circle (at -12.000001 13.599998 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AR4" smd circle (at -11.200003 13.599998 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AR5" smd circle (at -10.400005 13.199999 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AR6" smd circle (at -9.600006 13.599998 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AR7" smd circle (at -8.800008 13.199999 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 351 "MEM_ID1"))
    (pad "AR8" smd circle (at -8.000009 13.599998 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AR9" smd circle (at -7.200011 13.199999 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AR10" smd circle (at -6.400013 13.599998 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 164 "DPA1P"))
    (pad "AR11" smd circle (at -5.599989 13.199999 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 174 "DPA2P"))
    (pad "AR12" smd circle (at -4.79999 13.599998 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 178 "DPA3P"))
    (pad "AR13" smd circle (at -3.999992 13.199999 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "AR14" smd circle (at -3.199994 13.599998 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 168 "DPB0P"))
    (pad "AR15" smd circle (at -2.399995 13.199999 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 170 "DPB1P"))
    (pad "AR16" smd circle (at -1.599997 13.599998 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 186 "DPB2P"))
    (pad "AR17" smd circle (at -0.799998 13.199999 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 190 "DPB3P"))
    (pad "AR18" smd circle (at 0 13.599998 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 128 "N22176186"))
    (pad "AR19" smd circle (at 0.799998 13.199999 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 48 "DPA_VDDR"))
    (pad "AR20" smd circle (at 1.599997 13.599998 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "DPLL_PVDD"))
    (pad "AR21" smd circle (at 2.399995 13.199999 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AR22" smd circle (at 3.199994 13.599998 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 205 "TXCLK_L+"))
    (pad "AR23" smd circle (at 3.999992 13.199999 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 210 "TXOUT_L1-"))
    (pad "AR24" smd circle (at 4.79999 13.599998 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 212 "TXOUT_L2-"))
    (pad "AR25" smd circle (at 5.599989 13.199999 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 214 "TXOUT_L3-"))
    (pad "AR26" smd circle (at 6.399987 13.599998 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "AR27" smd circle (at 7.200011 13.199999 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 221 "TXOUT_U1-"))
    (pad "AR28" smd circle (at 8.000009 13.599998 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "VDD1DI"))
    (pad "AR29" smd circle (at 8.800008 13.199999 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 280 "VGA_BLU"))
    (pad "AR30" smd circle (at 9.600006 13.599998 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 283 "VGA_GRN"))
    (pad "AR31" smd circle (at 10.400005 13.199999 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 285 "VGA_RED"))
    (pad "AR32" smd circle (at 11.200003 13.599998 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 46 "AVDD"))
    (pad "AR33" smd circle (at 12.000001 13.599998 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 144 "N22176881"))
    (pad "AR34" smd circle (at 12.8 13.599998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "N16909622"))
    (pad "AR35" smd circle (at 13.599998 13.599998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "B1" smd circle (at -13.599998 -12.8 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "B2" smd circle (at -12.8 -12.8 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "VDDRHB1"))
    (pad "B3" smd circle (at -12.000001 -12.8 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 366 "CLKB0#"))
    (pad "B4" smd circle (at -11.200003 -12.8 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 520 "MDB31"))
    (pad "B5" smd circle (at -10.400005 -12.400001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 516 "MDB28"))
    (pad "B6" smd circle (at -9.600006 -12.8 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 591 "QSB3"))
    (pad "B7" smd circle (at -8.800008 -12.400001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 514 "MDB26"))
    (pad "B8" smd circle (at -8.000009 -12.8 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 502 "MDB15"))
    (pad "B9" smd circle (at -7.200011 -12.400001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 500 "MDB13"))
    (pad "B10" smd circle (at -6.400013 -12.8 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 587 "QSB1"))
    (pad "B11" smd circle (at -5.599989 -12.400001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 498 "MDB11"))
    (pad "B12" smd circle (at -4.79999 -12.8 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 497 "MDB10"))
    (pad "B13" smd circle (at -3.999992 -12.400001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 557 "MDB8"))
    (pad "B14" smd circle (at -3.199994 -12.8 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 123 "N16919381"))
    (pad "B15" smd circle (at -2.399995 -12.400001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "N22175956"))
    (pad "B16" smd circle (at -1.599997 -12.8 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 428 "MDA53"))
    (pad "B17" smd circle (at -0.799998 -12.400001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 481 "QSA6"))
    (pad "B18" smd circle (at 0 -12.8 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 426 "MDA51"))
    (pad "B19" smd circle (at 0.799998 -12.400001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 423 "MDA49"))
    (pad "B20" smd circle (at 1.599997 -12.8 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 412 "MDA39"))
    (pad "B21" smd circle (at 2.399995 -12.400001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 410 "MDA37"))
    (pad "B22" smd circle (at 3.199994 -12.8 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 477 "QSA4"))
    (pad "B23" smd circle (at 3.999992 -12.400001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 407 "MDA34"))
    (pad "B24" smd circle (at 4.79999 -12.8 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 406 "MDA33"))
    (pad "B25" smd circle (at 5.599989 -12.400001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "N16910486"))
    (pad "B26" smd circle (at 6.399987 -12.8 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 368 "CLKA1#"))
    (pad "B27" smd circle (at 7.200011 -12.400001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 455 "MAA2"))
    (pad "B28" smd circle (at 8.000009 -12.8 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 452 "MAA1"))
    (pad "B29" smd circle (at 8.800008 -12.400001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 465 "A_BA1"))
    (pad "B30" smd circle (at 9.600006 -12.8 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "B31" smd circle (at 10.400005 -12.400001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 375 "CKEA0"))
    (pad "B32" smd circle (at 11.200003 -12.8 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "N16909667"))
    (pad "B33" smd circle (at 12.000001 -12.8 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 364 "CLKA0#"))
    (pad "B34" smd circle (at 12.8 -12.8 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 404 "MDA31"))
    (pad "B35" smd circle (at 13.599998 -12.8 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "C1" smd circle (at -13.599998 -12.000001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 489 "CASB#0"))
    (pad "C2" smd circle (at -12.8 -12.000001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "N16910998"))
    (pad "C3" smd circle (at -12.000001 -12.000001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "C4" smd circle (at -11.200003 -12.000001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 519 "MDB30"))
    (pad "C5" smd circle (at -10.400005 -11.600002 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "C6" smd circle (at -9.600006 -11.600002 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 562 "DQMB#3"))
    (pad "C7" smd circle (at -8.800008 -11.600002 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 513 "MDB25"))
    (pad "C8" smd circle (at -8.000009 -12.000001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 512 "MDB24"))
    (pad "C9" smd circle (at -7.200011 -11.600002 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 499 "MDB12"))
    (pad "C10" smd circle (at -6.400013 -11.600002 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 560 "DQMB#1"))
    (pad "C11" smd circle (at -5.599989 -11.600002 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "C12" smd circle (at -4.79999 -12.000001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 558 "MDB9"))
    (pad "C13" smd circle (at -3.999992 -11.600002 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "C14" smd circle (at -3.199994 -11.600002 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "C15" smd circle (at -2.399995 -11.600002 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 429 "MDA54"))
    (pad "C16" smd circle (at -1.599997 -12.000001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 427 "MDA52"))
    (pad "C17" smd circle (at -0.799998 -11.600002 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 449 "DQMA#6"))
    (pad "C18" smd circle (at 0 -11.600002 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "C19" smd circle (at 0.799998 -11.600002 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 422 "MDA48"))
    (pad "C20" smd circle (at 1.599997 -12.000001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 411 "MDA38"))
    (pad "C21" smd circle (at 2.399995 -11.600002 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 409 "MDA36"))
    (pad "C22" smd circle (at 3.199994 -11.600002 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 447 "DQMA#4"))
    (pad "C23" smd circle (at 3.999992 -11.600002 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "C24" smd circle (at 4.79999 -12.000001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 405 "MDA32"))
    (pad "C25" smd circle (at 5.599989 -11.600002 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 468 "ODTA1"))
    (pad "C26" smd circle (at 6.399987 -11.600002 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "C27" smd circle (at 7.200011 -11.600002 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 451 "MAA0"))
    (pad "C28" smd circle (at 8.000009 -12.000001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 464 "A_BA0"))
    (pad "C29" smd circle (at 8.800008 -11.600002 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 487 "WEA#0"))
    (pad "C30" smd circle (at 9.600006 -11.600002 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 462 "MAA9"))
    (pad "C31" smd circle (at 10.400005 -11.600002 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 467 "ODTA0"))
    (pad "C32" smd circle (at 11.200003 -12.000001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 373 "CASA#0"))
    (pad "C33" smd circle (at 12.000001 -12.000001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "C34" smd circle (at 12.8 -12.000001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 401 "MDA29"))
    (pad "C35" smd circle (at 13.599998 -12.000001 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 403 "MDA30"))
    (pad "D1" smd circle (at -13.599998 -11.200003 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "D2" smd circle (at -12.8 -11.200003 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 583 "ODTB0"))
    (pad "D3" smd circle (at -12.000001 -11.200003 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 601 "RASB#0"))
    (pad "D4" smd circle (at -10.800004 -10.800004 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "D6" smd circle (at -9.600006 -10.800004 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 511 "MDB23"))
    (pad "D7" smd circle (at -8.400009 -10.800004 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "D9" smd circle (at -7.200011 -10.800004 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 506 "MDB19"))
    (pad "D10" smd circle (at -6.000013 -10.800004 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 556 "MDB7"))
    (pad "D12" smd circle (at -4.79999 -10.800004 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 559 "DQMB#0"))
    (pad "D14" smd circle (at -3.599993 -10.800004 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 518 "MDB3"))
    (pad "D15" smd circle (at -2.399995 -10.800004 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 439 "MDA63"))
    (pad "D17" smd circle (at -1.199998 -10.800004 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 483 "QSA7"))
    (pad "D18" smd circle (at 0 -10.800004 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 434 "MDA59"))
    (pad "D19" smd circle (at 1.199998 -10.800004 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 421 "MDA47"))
    (pad "D21" smd circle (at 2.399995 -10.800004 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 417 "MDA43"))
    (pad "D22" smd circle (at 3.599993 -10.800004 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 488 "WEA#1"))
    (pad "D24" smd circle (at 4.79999 -10.800004 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 486 "RASA#1"))
    (pad "D26" smd circle (at 5.999988 -10.800004 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 466 "A_BA2"))
    (pad "D27" smd circle (at 7.200011 -10.800004 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 459 "MAA6"))
    (pad "D29" smd circle (at 8.400009 -10.800004 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "D30" smd circle (at 9.600006 -10.800004 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 394 "MDA22"))
    (pad "D32" smd circle (at 10.800004 -10.800004 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 395 "MDA23"))
    (pad "D33" smd circle (at 12.000001 -11.200003 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "D34" smd circle (at 12.8 -11.200003 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 400 "MDA28"))
    (pad "D35" smd circle (at 13.599998 -11.200003 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "E1" smd circle (at -13.199999 -10.400005 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 493 "CSB0_0#"))
    (pad "E2" smd circle (at -12.400001 -10.400005 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "E3" smd circle (at -11.600002 -10.400005 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 491 "CKEB0"))
    (pad "E7" smd circle (at -8.400009 -10.000005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 561 "DQMB#2"))
    (pad "E9" smd circle (at -7.200011 -10.000005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 590 "QSB#2"))
    (pad "E10" smd circle (at -6.000013 -10.000005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "E12" smd circle (at -4.79999 -10.000005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "E14" smd circle (at -3.599993 -10.000005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 507 "MDB2"))
    (pad "E15" smd circle (at -2.399995 -10.000005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 438 "MDA62"))
    (pad "E17" smd circle (at -1.199998 -10.000005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 484 "QSA#7"))
    (pad "E18" smd circle (at 0 -10.000005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 433 "MDA58"))
    (pad "E19" smd circle (at 1.199998 -10.000005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "E21" smd circle (at 2.399995 -10.000005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 480 "QSA#5"))
    (pad "E22" smd circle (at 3.599993 -10.000005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "E24" smd circle (at 4.79999 -10.000005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "E26" smd circle (at 5.999988 -10.000005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 453 "MAA10"))
    (pad "E27" smd circle (at 7.200011 -10.000005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 458 "MAA5"))
    (pad "E29" smd circle (at 8.400009 -10.000005 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 461 "MAA8"))
    (pad "E33" smd circle (at 11.600002 -10.400005 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 446 "DQMA#3"))
    (pad "E34" smd circle (at 12.400001 -10.400005 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 475 "QSA3"))
    (pad "E35" smd circle (at 13.199999 -10.400005 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 476 "QSA#3"))
    (pad "F1" smd circle (at -13.599998 -9.600006 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 582 "B_BA2"))
    (pad "F2" smd circle (at -12.8 -9.600006 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 603 "WEB#0"))
    (pad "F3" smd circle (at -11.600002 -9.600006 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 577 "MAB8"))
    (pad "F4" smd circle (at -10.800004 -9.600006 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 578 "MAB9"))
    (pad "F6" smd circle (at -9.619996 -9.600006 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 510 "MDB22"))
    (pad "F7" smd circle (at -8.400009 -9.200007 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "F9" smd circle (at -7.200011 -9.200007 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 589 "QSB2"))
    (pad "F10" smd circle (at -6.000013 -9.200007 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 505 "MDB18"))
    (pad "F12" smd circle (at -4.79999 -9.200007 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 551 "MDB6"))
    (pad "F14" smd circle (at -3.599993 -9.200007 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "F15" smd circle (at -2.399995 -9.200007 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "F17" smd circle (at -1.199998 -9.200007 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "F18" smd circle (at 0 -9.200007 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 432 "MDA57"))
    (pad "F19" smd circle (at 1.199998 -9.200007 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 420 "MDA46"))
    (pad "F21" smd circle (at 2.399995 -9.200007 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 479 "QSA5"))
    (pad "F22" smd circle (at 3.599993 -9.200007 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 416 "MDA42"))
    (pad "F24" smd circle (at 4.79999 -9.200007 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 376 "CKEA1"))
    (pad "F26" smd circle (at 5.999988 -9.200007 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "F27" smd circle (at 7.200011 -9.200007 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 457 "MAA4"))
    (pad "F29" smd circle (at 8.400009 -9.200007 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 392 "MDA20"))
    (pad "F30" smd circle (at 9.600006 -9.619996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "F32" smd circle (at 10.800004 -9.600006 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 393 "MDA21"))
    (pad "F33" smd circle (at 11.600002 -9.600006 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "F34" smd circle (at 12.8 -9.600006 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 399 "MDA27"))
    (pad "F35" smd circle (at 13.599998 -9.600006 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "G1" smd circle (at -13.199999 -8.800008 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "G2" smd circle (at -12.400001 -8.800008 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 580 "B_BA0"))
    (pad "G3" smd circle (at -11.600002 -8.800008 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 581 "B_BA1"))
    (pad "G4" smd circle (at -10.800004 -8.400009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "G5" smd circle (at -10.000005 -8.400009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 575 "MAB6"))
    (pad "G6" smd circle (at -9.200007 -8.400009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 509 "MDB21"))
    (pad "G7" smd circle (at -8.400009 -8.400009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 508 "MDB20"))
    (pad "G9" smd circle (at -7.200011 -8.400009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "G10" smd circle (at -6.000013 -8.400009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "G12" smd circle (at -4.79999 -8.400009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 540 "MDB5"))
    (pad "G14" smd circle (at -3.599993 -8.400009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 496 "MDB1"))
    (pad "G15" smd circle (at -2.399995 -8.400009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 437 "MDA61"))
    (pad "G17" smd circle (at -1.199998 -8.400009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 450 "DQMA#7"))
    (pad "G18" smd circle (at 0 -8.400009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "G19" smd circle (at 1.199998 -8.400009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 419 "MDA45"))
    (pad "G21" smd circle (at 2.399995 -8.400009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "G22" smd circle (at 3.599993 -8.400009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "G24" smd circle (at 4.79999 -8.400009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 378 "CSA1_0#"))
    (pad "G26" smd circle (at 5.999988 -8.400009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 456 "MAA3"))
    (pad "G27" smd circle (at 7.200011 -8.400009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 463 "MAA12"))
    (pad "G29" smd circle (at 8.400009 -8.400009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "G30" smd circle (at 9.200007 -8.400009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 445 "DQMA#2"))
    (pad "G31" smd circle (at 10.000005 -8.400009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 473 "QSA2"))
    (pad "G32" smd circle (at 10.800004 -8.400009 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 474 "QSA#2"))
    (pad "G33" smd circle (at 11.600002 -8.800008 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 396 "MDA24"))
    (pad "G34" smd circle (at 12.400001 -8.800008 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 397 "MDA25"))
    (pad "G35" smd circle (at 13.199999 -8.800008 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 398 "MDA26"))
    (pad "H1" smd circle (at -13.599998 -8.000009 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "H2" smd circle (at -12.8 -8.000009 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 567 "MAB0"))
    (pad "H3" smd circle (at -12.000001 -8.000009 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 568 "MAB1"))
    (pad "H10" smd circle (at -6.000013 -7.60001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 504 "MDB17"))
    (pad "H12" smd circle (at -4.79999 -7.60001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 529 "MDB4"))
    (pad "H14" smd circle (at -3.599993 -7.60001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 586 "QSB#0"))
    (pad "H15" smd circle (at -2.399995 -7.60001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 495 "MDB0"))
    (pad "H17" smd circle (at -1.199998 -7.60001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "H18" smd circle (at 0 -7.60001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 431 "MDA56"))
    (pad "H19" smd circle (at 1.199998 -7.60001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "H21" smd circle (at 2.399995 -7.60001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 448 "DQMA#5"))
    (pad "H22" smd circle (at 3.599993 -7.60001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 415 "MDA41"))
    (pad "H24" smd circle (at 4.79999 -7.60001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "H26" smd circle (at 5.999988 -7.60001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 374 "CASA#1"))
    (pad "H33" smd circle (at 12.000001 -8.000009 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 385 "MDA14"))
    (pad "H34" smd circle (at 12.8 -8.000009 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 386 "MDA15"))
    (pad "H35" smd circle (at 13.599998 -8.000009 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "J1" smd circle (at -13.199999 -7.200011 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 569 "MAB10"))
    (pad "J2" smd circle (at -12.400001 -7.200011 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 570 "MAB11"))
    (pad "J3" smd circle (at -11.600002 -7.200011 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 571 "MAB2"))
    (pad "J4" smd circle (at -10.800004 -7.200011 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 573 "MAB4"))
    (pad "J5" smd circle (at -10.000005 -7.200011 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 572 "MAB3"))
    (pad "J6" smd circle (at -9.200007 -7.200011 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 574 "MAB5"))
    (pad "J7" smd circle (at -8.400009 -7.200011 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 579 "MAB12"))
    (pad "J9" smd circle (at -7.220001 -7.200011 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 576 "MAB7"))
    (pad "J10" smd circle (at -6.000013 -6.800012 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 503 "MDB16"))
    (pad "J12" smd circle (at -4.79999 -6.800012 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "J14" smd circle (at -3.599993 -6.800012 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 585 "QSB0"))
    (pad "J15" smd circle (at -2.399995 -6.800012 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "J17" smd circle (at -1.199998 -6.800012 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 436 "MDA60"))
    (pad "J18" smd circle (at 0 -6.800012 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "J19" smd circle (at 1.199998 -6.800012 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 418 "MDA44"))
    (pad "J21" smd circle (at 2.399995 -6.800012 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "J22" smd circle (at 3.599993 -6.800012 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 414 "MDA40"))
    (pad "J24" smd circle (at 4.79999 -6.800012 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "J26" smd circle (at 5.999988 -6.800012 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "J27" smd circle (at 7.200011 -7.220001 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 460 "MAA7"))
    (pad "J29" smd circle (at 8.400009 -7.200011 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 388 "MDA17"))
    (pad "J30" smd circle (at 9.200007 -7.200011 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 389 "MDA18"))
    (pad "J31" smd circle (at 10.000005 -7.200011 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 390 "MDA19"))
    (pad "J32" smd circle (at 10.800004 -7.200011 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "J33" smd circle (at 11.600002 -7.200011 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 383 "MDA12"))
    (pad "J34" smd circle (at 12.400001 -7.200011 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 384 "MDA13"))
    (pad "J35" smd circle (at 13.199999 -7.200011 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "K1" smd circle (at -13.599998 -6.400013 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 371 "CLKB1"))
    (pad "K2" smd circle (at -12.8 -6.400013 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 370 "CLKB1#"))
    (pad "K3" smd circle (at -11.600002 -6.400013 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "K4" smd circle (at -10.800004 -5.999988 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 490 "CASB#1"))
    (pad "K5" smd circle (at -10.000005 -5.999988 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 584 "ODTB1"))
    (pad "K6" smd circle (at -9.200007 -5.999988 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "K7" smd circle (at -8.400009 -5.999988 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 602 "RASB#1"))
    (pad "K8" smd circle (at -7.60001 -5.999988 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 492 "CKEB1"))
    (pad "K9" smd circle (at -6.800012 -5.999988 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "K10" smd circle (at -6.000013 -5.999988 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "K12" smd circle (at -4.79999 -5.999988 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "K14" smd circle (at -3.599993 -5.999988 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "K15" smd circle (at -2.399995 -5.999988 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "K17" smd circle (at -1.199998 -5.999988 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "K18" smd circle (at 0 -5.999988 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "K19" smd circle (at 1.199998 -5.999988 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "K21" smd circle (at 2.399995 -5.999988 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "K22" smd circle (at 3.599993 -5.999988 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "K24" smd circle (at 4.79999 -5.999988 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "K26" smd circle (at 5.999988 -5.999988 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "K27" smd circle (at 6.799986 -5.999988 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 387 "MDA16"))
    (pad "K28" smd circle (at 7.60001 -5.999988 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "K29" smd circle (at 8.400009 -5.999988 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 424 "MDA5"))
    (pad "K30" smd circle (at 9.200007 -5.999988 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "K31" smd circle (at 10.000005 -5.999988 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 435 "MDA6"))
    (pad "K32" smd circle (at 10.800004 -5.999988 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 440 "MDA7"))
    (pad "K33" smd circle (at 11.600002 -6.400013 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 444 "DQMA#1"))
    (pad "K34" smd circle (at 12.8 -6.400013 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 471 "QSA1"))
    (pad "K35" smd circle (at 13.599998 -6.400013 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 472 "QSA#1"))
    (pad "L1" smd circle (at -13.199999 -5.599989 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "VDDRHB2"))
    (pad "L2" smd circle (at -12.400001 -5.599989 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "N16909550"))
    (pad "L3" smd circle (at -11.600002 -5.599989 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 494 "CSB1_0#"))
    (pad "L14" smd circle (at -3.599993 -5.19999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "L15" smd circle (at -2.399995 -5.19999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "L17" smd circle (at -1.199998 -5.19999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "L18" smd circle (at 0 -5.19999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "L19" smd circle (at 1.199998 -5.19999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "L21" smd circle (at 2.399995 -5.19999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "L22" smd circle (at 3.599993 -5.19999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "L33" smd circle (at 11.600002 -5.599989 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "L34" smd circle (at 12.400001 -5.599989 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 381 "MDA10"))
    (pad "L35" smd circle (at 13.199999 -5.599989 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 382 "MDA11"))
    (pad "M1" smd circle (at -13.599998 -4.79999 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "M2" smd circle (at -12.8 -4.79999 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 522 "MDB33"))
    (pad "M3" smd circle (at -12.000001 -4.79999 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 521 "MDB32"))
    (pad "M4" smd circle (at -10.800004 -4.79999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "M5" smd circle (at -10.000005 -4.79999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "M6" smd circle (at -9.200007 -4.79999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 604 "WEB#1"))
    (pad "M7" smd circle (at -8.400009 -4.79999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 531 "MDB41"))
    (pad "M8" smd circle (at -7.60001 -4.79999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 530 "MDB40"))
    (pad "M9" smd circle (at -6.800012 -4.79999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "M10" smd circle (at -6.000013 -4.79999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "M12" smd circle (at -4.79999 -4.79999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 134 "N16910916"))
    (pad "M24" smd circle (at 4.79999 -4.795012 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 134 "N16910916"))
    (pad "M26" smd circle (at 5.999988 -4.79999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "M27" smd circle (at 6.799986 -4.79999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 413 "MDA4"))
    (pad "M28" smd circle (at 7.60001 -4.79999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "M29" smd circle (at 8.400009 -4.79999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 443 "DQMA#0"))
    (pad "M30" smd circle (at 9.200007 -4.79999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 469 "QSA0"))
    (pad "M31" smd circle (at 10.000005 -4.79999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 470 "QSA#0"))
    (pad "M32" smd circle (at 10.800004 -4.79999 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "M33" smd circle (at 12.000001 -4.79999 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 441 "MDA8"))
    (pad "M34" smd circle (at 12.8 -4.79999 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 442 "MDA9"))
    (pad "M35" smd circle (at 13.599998 -4.79999 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "N1" smd circle (at -13.199999 -3.999992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 524 "MDB35"))
    (pad "N2" smd circle (at -12.400001 -3.999992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 523 "MDB34"))
    (pad "N3" smd circle (at -11.600002 -3.999992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "N13" smd circle (at -3.999992 -3.999992 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "VDD_CORE"))
    (pad "N14" smd circle (at -2.999994 -3.999992 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "N15" smd circle (at -1.999996 -3.999992 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "VDD_CORE"))
    (pad "N17" smd circle (at -0.999998 -3.999992 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "N18" smd circle (at 0 -3.999992 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "VDD_CORE"))
    (pad "N19" smd circle (at 0.999998 -3.999992 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "N21" smd circle (at 1.999996 -3.999992 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "VDD_CORE"))
    (pad "N22" smd circle (at 2.999994 -3.999992 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "N23" smd circle (at 3.999992 -3.999992 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "VDD_CORE"))
    (pad "N33" smd circle (at 11.600002 -3.999992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "N34" smd circle (at 12.400001 -3.999992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 126 "N16919174"))
    (pad "N35" smd circle (at 13.199999 -3.999992 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 122 "N16919383"))
    (pad "P1" smd circle (at -13.599998 -3.199994 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 594 "QSB#4"))
    (pad "P2" smd circle (at -12.8 -3.199994 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 593 "QSB4"))
    (pad "P3" smd circle (at -11.600002 -3.199994 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 563 "DQMB#4"))
    (pad "P4" smd circle (at -10.800004 -3.599993 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 533 "MDB43"))
    (pad "P5" smd circle (at -10.000005 -3.599993 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 532 "MDB42"))
    (pad "P6" smd circle (at -9.200007 -3.599993 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "P7" smd circle (at -8.400009 -3.599993 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 596 "QSB#5"))
    (pad "P8" smd circle (at -7.60001 -3.599993 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 595 "QSB5"))
    (pad "P9" smd circle (at -6.800012 -3.599993 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "P10" smd circle (at -6.000013 -3.599993 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "P11" smd circle (at -5.19999 -3.599993 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 134 "N16910916"))
    (pad "P13" smd circle (at -3.999992 -2.999994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "P14" smd circle (at -2.999994 -2.999994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "VDD_CORE"))
    (pad "P15" smd circle (at -1.999996 -2.999994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "P17" smd circle (at -0.999998 -2.999994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "VDD_CORE"))
    (pad "P18" smd circle (at 0 -2.999994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "P19" smd circle (at 0.999998 -2.999994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "VDD_CORE"))
    (pad "P21" smd circle (at 1.999996 -2.999994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "P22" smd circle (at 2.999994 -2.999994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "VDD_CORE"))
    (pad "P23" smd circle (at 3.999992 -2.999994 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "P25" smd circle (at 5.19999 -3.599993 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 134 "N16910916"))
    (pad "P26" smd circle (at 5.999988 -3.599993 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "P27" smd circle (at 6.799986 -3.599993 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 379 "MDA0"))
    (pad "P28" smd circle (at 7.60001 -3.599993 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 380 "MDA1"))
    (pad "P29" smd circle (at 8.400009 -3.599993 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "P30" smd circle (at 9.200007 -3.599993 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "P31" smd circle (at 10.000005 -3.599993 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 391 "MDA2"))
    (pad "P32" smd circle (at 10.800004 -3.599993 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 402 "MDA3"))
    (pad "P33" smd circle (at 11.600002 -3.199994 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "P34" smd circle (at 12.8 -3.199994 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "P35" smd circle (at 13.599998 -3.199994 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "R1" smd circle (at -13.199999 -2.399995 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "R2" smd circle (at -12.400001 -2.399995 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 526 "MDB37"))
    (pad "R3" smd circle (at -11.600002 -2.399995 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 525 "MDB36"))
    (pad "R4" smd circle (at -10.800004 -2.399995 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 564 "DQMB#5"))
    (pad "R5" smd circle (at -10.000005 -2.399995 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "R6" smd circle (at -9.200007 -2.399995 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 536 "MDB46"))
    (pad "R7" smd circle (at -8.400009 -2.399995 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "R8" smd circle (at -7.60001 -2.399995 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 535 "MDB45"))
    (pad "R9" smd circle (at -6.800012 -2.399995 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 534 "MDB44"))
    (pad "R10" smd circle (at -6.000013 -2.399995 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "R11" smd circle (at -5.19999 -2.399995 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 52 "N16909654"))
    (pad "R13" smd circle (at -3.999992 -1.999996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "VDD_CORE"))
    (pad "R14" smd circle (at -2.999994 -1.999996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "R15" smd circle (at -1.999996 -1.999996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "VDD_CORE"))
    (pad "R17" smd circle (at -0.999998 -1.999996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "R18" smd circle (at 0 -1.999996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "VDD_CORE"))
    (pad "R19" smd circle (at 0.999998 -1.999996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "R21" smd circle (at 1.999996 -1.999996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "VDD_CORE"))
    (pad "R22" smd circle (at 2.999994 -1.999996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "R23" smd circle (at 3.999992 -1.999996 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "VDD_CORE"))
    (pad "R25" smd circle (at 5.19999 -2.399995 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 52 "N16909654"))
    (pad "R26" smd circle (at 5.999988 -2.399995 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 133 "PCIE_VDDC"))
    (pad "R27" smd circle (at 6.799986 -2.399995 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "R28" smd circle (at 7.60001 -2.399995 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "R29" smd circle (at 8.400009 -2.399995 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "R30" smd circle (at 9.200007 -2.399995 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 54 "PCIE_TXN15"))
    (pad "R31" smd circle (at 10.000005 -2.399995 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 56 "PCIE_TXP15"))
    (pad "R32" smd circle (at 10.800004 -2.399995 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "R33" smd circle (at 11.600002 -2.399995 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "R34" smd circle (at 12.400001 -2.399995 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 234 "PCIE_RXN15"))
    (pad "R35" smd circle (at 13.199999 -2.399995 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 250 "PCIE_RXP15"))
    (pad "T1" smd circle (at -13.599998 -1.599997 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "T2" smd circle (at -12.8 -1.599997 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 528 "MDB39"))
    (pad "T3" smd circle (at -12.000001 -1.599997 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 527 "MDB38"))
    (pad "T33" smd circle (at 12.000001 -1.599997 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "T34" smd circle (at 12.8 -1.599997 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 233 "PCIE_RXN14"))
    (pad "T35" smd circle (at 13.599998 -1.599997 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 249 "PCIE_RXP14"))
    (pad "U1" smd circle (at -13.199999 -0.799998 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 541 "MDB50"))
    (pad "U2" smd circle (at -12.400001 -0.799998 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 539 "MDB49"))
    (pad "U3" smd circle (at -11.600002 -0.799998 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 538 "MDB48"))
    (pad "U4" smd circle (at -10.800004 -1.199998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 537 "MDB47"))
    (pad "U5" smd circle (at -10.000005 -1.199998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "U6" smd circle (at -9.200007 -1.199998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 549 "MDB58"))
    (pad "U7" smd circle (at -8.400009 -1.199998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 548 "MDB57"))
    (pad "U8" smd circle (at -7.60001 -1.199998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "U9" smd circle (at -6.800012 -1.199998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 547 "MDB56"))
    (pad "U10" smd circle (at -6.000013 -1.199998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "U11" smd circle (at -5.19999 -1.199998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 52 "N16909654"))
    (pad "U13" smd circle (at -3.999992 -0.999998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 148 "+BBP"))
    (pad "U14" smd circle (at -2.999994 -0.999998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "VDD_CORE"))
    (pad "U15" smd circle (at -1.999996 -0.999998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "U17" smd circle (at -0.999998 -0.999998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "VDD_CORE"))
    (pad "U18" smd circle (at 0 -0.999998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "U19" smd circle (at 0.999998 -0.999998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "VDD_CORE"))
    (pad "U21" smd circle (at 1.999996 -0.999998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "U22" smd circle (at 2.999994 -0.999998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "VDD_CORE"))
    (pad "U23" smd circle (at 3.999992 -0.999998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "U25" smd circle (at 5.19999 -1.199998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 52 "N16909654"))
    (pad "U26" smd circle (at 5.999988 -1.199998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 133 "PCIE_VDDC"))
    (pad "U27" smd circle (at 6.799986 -1.199998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 58 "PCIE_TXN14"))
    (pad "U28" smd circle (at 7.60001 -1.199998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "PCIE_TXP14"))
    (pad "U29" smd circle (at 8.400009 -1.199998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "U30" smd circle (at 9.200007 -1.199998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 62 "PCIE_TXN13"))
    (pad "U31" smd circle (at 10.000005 -1.199998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 64 "PCIE_TXP13"))
    (pad "U32" smd circle (at 10.800004 -1.199998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "U33" smd circle (at 11.600002 -0.799998 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 231 "PCIE_RXN12"))
    (pad "U34" smd circle (at 12.400001 -0.799998 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 232 "PCIE_RXN13"))
    (pad "U35" smd circle (at 13.199999 -0.799998 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 248 "PCIE_RXP13"))
    (pad "V1" smd circle (at -13.599998 0 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "V2" smd circle (at -12.8 0 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 542 "MDB51"))
    (pad "V3" smd circle (at -11.600002 0 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "V4" smd circle (at -10.800004 0 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 550 "MDB59"))
    (pad "V5" smd circle (at -10.000005 0 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 600 "QSB#7"))
    (pad "V6" smd circle (at -9.200007 0 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 599 "QSB7"))
    (pad "V7" smd circle (at -8.400009 0 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "V8" smd circle (at -7.60001 0 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 566 "DQMB#7"))
    (pad "V9" smd circle (at -6.800012 0 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "V10" smd circle (at -6.000013 0 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "V11" smd circle (at -5.19999 0 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "V13" smd circle (at -3.999992 0 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 148 "+BBP"))
    (pad "V14" smd circle (at -2.999994 0 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "V15" smd circle (at -1.999996 0 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "VDD_CORE"))
    (pad "V17" smd circle (at -0.999998 0 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "V18" smd circle (at 0 0 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "VDD_CORE"))
    (pad "V19" smd circle (at 0.999998 0 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "V21" smd circle (at 1.999996 0 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "VDD_CORE"))
    (pad "V22" smd circle (at 2.999994 0 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "V23" smd circle (at 3.999992 0 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "VDD_CORE"))
    (pad "V25" smd circle (at 5.19999 0 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 133 "PCIE_VDDC"))
    (pad "V26" smd circle (at 5.999988 0 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 133 "PCIE_VDDC"))
    (pad "V27" smd circle (at 6.799986 0 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 66 "PCIE_TXN12"))
    (pad "V28" smd circle (at 7.60001 0 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 68 "PCIE_TXP12"))
    (pad "V29" smd circle (at 8.400009 0 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "V30" smd circle (at 9.200007 0 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "PCIE_TXN11"))
    (pad "V31" smd circle (at 10.000005 0 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 72 "PCIE_TXP11"))
    (pad "V32" smd circle (at 10.800004 0 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "V33" smd circle (at 11.600002 0 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 247 "PCIE_RXP12"))
    (pad "V34" smd circle (at 12.8 0 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "V35" smd circle (at 13.599998 0 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "W1" smd circle (at -13.199999 0.799998 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 598 "QSB#6"))
    (pad "W2" smd circle (at -12.400001 0.799998 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 597 "QSB6"))
    (pad "W3" smd circle (at -11.600002 0.799998 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 565 "DQMB#6"))
    (pad "W4" smd circle (at -10.800004 1.199998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 555 "MDB63"))
    (pad "W5" smd circle (at -10.000005 1.199998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "W6" smd circle (at -9.200007 1.199998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 554 "MDB62"))
    (pad "W7" smd circle (at -8.400009 1.199998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 553 "MDB61"))
    (pad "W8" smd circle (at -7.60001 1.199998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "W9" smd circle (at -6.800012 1.199998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 552 "MDB60"))
    (pad "W10" smd circle (at -6.000013 1.199998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "W11" smd circle (at -5.19999 1.199998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "VDD_CORE"))
    (pad "W13" smd circle (at -3.999992 0.999998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "W14" smd circle (at -2.999994 0.999998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "VDD_CORE"))
    (pad "W15" smd circle (at -1.999996 0.999998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "W17" smd circle (at -0.999998 0.999998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "VDD_CORE"))
    (pad "W18" smd circle (at 0 0.999998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "W19" smd circle (at 0.999998 0.999998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "VDD_CORE"))
    (pad "W21" smd circle (at 1.999996 0.999998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "W22" smd circle (at 2.999994 0.999998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "VDD_CORE"))
    (pad "W23" smd circle (at 3.999992 0.999998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "W25" smd circle (at 5.19999 1.199998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 133 "PCIE_VDDC"))
    (pad "W26" smd circle (at 5.999988 1.199998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 133 "PCIE_VDDC"))
    (pad "W27" smd circle (at 6.799986 1.199998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 74 "PCIE_TXN10"))
    (pad "W28" smd circle (at 7.60001 1.199998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 76 "PCIE_TXP10"))
    (pad "W29" smd circle (at 8.400009 1.199998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "W30" smd circle (at 9.200007 1.199998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 78 "PCIE_TXN9"))
    (pad "W31" smd circle (at 10.000005 1.199998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 80 "PCIE_TXP9"))
    (pad "W32" smd circle (at 10.800004 1.199998 270) (size 0.500024 0.500024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "W33" smd circle (at 11.600002 0.799998 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "W34" smd circle (at 12.400001 0.799998 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 230 "PCIE_RXN11"))
    (pad "W35" smd circle (at 13.199999 0.799998 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 246 "PCIE_RXP11"))
    (pad "Y1" smd circle (at -13.599998 1.599997 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "Y2" smd circle (at -12.8 1.599997 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 544 "MDB53"))
    (pad "Y3" smd circle (at -12.000001 1.599997 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 543 "MDB52"))
    (pad "Y33" smd circle (at 12.000001 1.599997 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "Y34" smd circle (at 12.8 1.599997 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 229 "PCIE_RXN10"))
    (pad "Y35" smd circle (at 13.599998 1.599997 270) (size 0.3302 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 245 "PCIE_RXP10"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at 8.702007 24.610002 180)
    (fp_text reference "R638" (at -1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 368 "CLKA1#"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 160 "N18859575"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -23.698004 9.559994 90)
    (fp_text reference "C574" (at -1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 153 "N18876007"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -51.298 6.509987 90)
    (fp_text reference "R129" (at -1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 291 "PBAT_SMBDAT"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 346 "N21377265"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -46.898009 2.309996)
    (fp_text reference "R1037" (at 2.2225 2.54 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 300 "N22177921"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -45.998011 9.410007 -90)
    (fp_text reference "C333" (at 1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "+3VRUN"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAPT7343_2_0H_1" (layer "F.Cu")
    (tedit 0)
    (at 13.101998 62.410003 -90)
    (fp_text reference "C418" (at 2.029993 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -3.048 270) (size 2.921 2.413) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 3.298012 270) (size 2.921 2.413) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -51.797999 63.71 -90)
    (fp_text reference "R199" (at 1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 203 "BL_ENA"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 336 "BLON_PWM"))
  )
  (footprint "lib:CAPT7343_2_8H_1" (layer "F.Cu")
    (tedit 0)
    (at 8.802007 4.609991)
    (fp_text reference "C437" (at 1.905 2.029993 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -3.048) (size 2.921 2.413) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "VDD_CORE"))
    (pad "2" smd rect (at 0 3.298012) (size 2.921 2.413) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -40.197997 7.509985 90)
    (fp_text reference "C148" (at -1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -43.69799 36.310004 -90)
    (fp_text reference "C617" (at 1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 174 "DPA2P"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 175 "DVI_TX1-"))
  )
  (footprint "lib:TP055PRI_1" (layer "F.Cu")
    (tedit 0)
    (at -28.048008 59.010009)
    (fp_text reference "TP4" (at -0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd circle (at 0 0) (size 0.550012 0.550012) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 240 "PCIE_RXN7"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -23.698004 17.860003 -90)
    (fp_text reference "C124" (at 1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
  )
  (footprint "lib:GEOM0001_1" (layer "F.Cu")
    (tedit 0)
    (at -42.097993 58.109986)
    (fp_text reference "L38" (at 1.323232 1.058608 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144) (size 1.27 1.219987) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "N16909622"))
    (pad "2" smd rect (at 0 0.9144) (size 1.27 1.219987) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
  )
  (footprint "lib:RES1608_0_8H_1" (layer "F.Cu")
    (tedit 0)
    (at 3.401992 57.209988 -90)
    (fp_text reference "B44" (at 1.270025 -1.587475 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 270) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "N18849793"))
    (pad "2" smd rect (at 0 0.7874 270) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -51.797999 64.609998 -90)
    (fp_text reference "R198" (at 1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 215 "BL_BRIGHT"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 336 "BLON_PWM"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -48.698005 40.309996 -90)
    (fp_text reference "R1010" (at 2.54 -2.2225 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 169 "DVIB_CLK-"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 298 "N22316558"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -48.698005 41.309994 -90)
    (fp_text reference "R1011" (at 2.54 -2.2225 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 183 "DVIB_CLK+"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 298 "N22316558"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -6.998012 15.909994 -90)
    (fp_text reference "C123" (at 1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -34.798008 3.109994 -90)
    (fp_text reference "R655" (at 1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 288 "N16909921"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "+5VRUN"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -48.298006 67.560005 -90)
    (fp_text reference "R1030" (at 2.54 -2.2225 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "+5VRUN"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 310 "DDC4DATA"))
  )
  (footprint "lib:RES1608_0_8H_1" (layer "F.Cu")
    (tedit 0)
    (at -7.372993 14.709996 90)
    (fp_text reference "B48" (at -1.270025 1.587475 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 90) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "N18866844"))
    (pad "2" smd rect (at 0 0.7874 90) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
  )
  (footprint "lib:GEOM0010_1" (layer "F.Cu")
    (tedit 0)
    (at -38.098001 66.309995 90)
    (fp_text reference "U19" (at -1.2573 1.5875 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd oval (at -1.905 2.8448 90) (size 0.639978 1.579982) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "2" smd oval (at -0.635 2.8448 90) (size 0.639978 1.579982) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 149 "N22665296"))
    (pad "3" smd oval (at 0.635 2.8448 90) (size 0.639978 1.579982) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 133 "PCIE_VDDC"))
    (pad "4" smd oval (at 1.905 2.8448 90) (size 0.639978 1.579982) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 133 "PCIE_VDDC"))
    (pad "5" smd oval (at 1.905 -2.8702 90) (size 0.639978 1.579982) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "6" smd oval (at 0.635 -2.8702 90) (size 0.639978 1.579982) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "+5VRUN"))
    (pad "7" smd oval (at -0.635 -2.8702 90) (size 0.639978 1.579982) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "8" smd oval (at -1.905 -2.8702 90) (size 0.639978 1.579982) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 354 "RUNPWROK_1"))
    (pad "9" smd rect (at 0 0 90) (size 4.099992 2.799994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
  )
  (footprint "lib:TP055PRI_1" (layer "F.Cu")
    (tedit 0)
    (at -28.848007 59.010009)
    (fp_text reference "TP3" (at -0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd circle (at 0 0) (size 0.550012 0.550012) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 256 "PCIE_RXP7"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -41.897993 2.809995)
    (fp_text reference "R1072" (at 2.2225 2.54 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 267 "AC_BAT"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 342 "OTEMP#"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -40.497996 14.109998 90)
    (fp_text reference "C146" (at -1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -6.998012 8.359996 90)
    (fp_text reference "R50" (at -1.27 1.5875 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 156 "N18866671"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1608_0_89H_1" (layer "F.Cu")
    (tedit 0)
    (at -44.598013 57.109988 -90)
    (fp_text reference "C401" (at 1.905025 -1.904975 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 270) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "N16909622"))
    (pad "2" smd rect (at 0 0.7874 270) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP3216_1" (layer "F.Cu")
    (tedit 0)
    (at 8.451995 21.28499 -60)
    (fp_text reference "C430" (at 2.26552 -0.607035 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -1.4478 300) (size 1.799996 1.399997) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 142 "G_PWR_SRC"))
    (pad "2" smd rect (at 0 1.4478 300) (size 1.799996 1.399997) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP3216_1" (layer "F.Cu")
    (tedit 0)
    (at 15.101994 17.509991 90)
    (fp_text reference "C432" (at -1.65848 1.658468 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -1.4478 90) (size 1.799996 1.399997) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 142 "G_PWR_SRC"))
    (pad "2" smd rect (at 0 1.4478 90) (size 1.799996 1.399997) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -43.69799 39.309998 -90)
    (fp_text reference "C620" (at 1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 180 "DPA3N"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 181 "DVI_TX2+"))
  )
  (footprint "lib:CAP1608_0_89H_1" (layer "F.Cu")
    (tedit 0)
    (at 13.201998 24.610002 -90)
    (fp_text reference "C95" (at 1.270025 -1.587475 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 270) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.7874 270) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -6.998012 10.059993 -90)
    (fp_text reference "C122" (at 1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
  )
  (footprint "lib:CAP1608_0_89H_1" (layer "F.Cu")
    (tedit 0)
    (at -25.498001 2.309996 180)
    (fp_text reference "C142" (at -1.904975 -1.905025 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 180) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.7874 180) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -45.198012 28.609994 180)
    (fp_text reference "C49" (at -1.5875 -1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 120 "VDDR3"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1608_0_8H_1" (layer "F.Cu")
    (tedit 0)
    (at 4.101991 41.109994)
    (fp_text reference "B46" (at 1.587475 1.270025 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "N18859523"))
    (pad "2" smd rect (at 0 0.7874) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
  )
  (footprint "lib:CAPT7343_2_8H_1" (layer "F.Cu")
    (tedit 0)
    (at 14.401996 4.544002)
    (fp_text reference "C436" (at 1.905 2.029993 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -3.048) (size 2.921 2.413) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "VDD_CORE"))
    (pad "2" smd rect (at 0 3.298012) (size 2.921 2.413) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:BGA080_11X13-84_1" (layer "F.Cu")
    (tedit 0)
    (at -15.397996 12.310001 180)
    (fp_text reference "U6" (at -1.27 -0.635 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "A1" smd circle (at -3.199994 -5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "A2" smd circle (at -2.399995 -5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "A3" smd circle (at -1.599997 -5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "A7" smd circle (at 1.599997 -5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "A8" smd circle (at 2.399995 -5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 586 "QSB#0"))
    (pad "A9" smd circle (at 3.199994 -5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "B1" smd circle (at -3.199994 -4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 507 "MDB2"))
    (pad "B2" smd circle (at -2.399995 -4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "B3" smd circle (at -1.599997 -4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 559 "DQMB#0"))
    (pad "B7" smd circle (at 1.599997 -4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 585 "QSB0"))
    (pad "B8" smd circle (at 2.399995 -4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "B9" smd circle (at 3.199994 -4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 540 "MDB5"))
    (pad "C1" smd circle (at -3.199994 -3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "C2" smd circle (at -2.399995 -3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 496 "MDB1"))
    (pad "C3" smd circle (at -1.599997 -3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "C7" smd circle (at 1.599997 -3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "C8" smd circle (at 2.399995 -3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 529 "MDB4"))
    (pad "C9" smd circle (at 3.199994 -3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "D1" smd circle (at -3.199994 -3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 518 "MDB3"))
    (pad "D2" smd circle (at -2.399995 -3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "D3" smd circle (at -1.599997 -3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 495 "MDB0"))
    (pad "D7" smd circle (at 1.599997 -3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 556 "MDB7"))
    (pad "D8" smd circle (at 2.399995 -3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "D9" smd circle (at 3.199994 -3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 551 "MDB6"))
    (pad "E1" smd circle (at -3.199994 -2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "E2" smd circle (at -2.399995 -2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "E3" smd circle (at -1.599997 -2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "E7" smd circle (at 1.599997 -2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "E8" smd circle (at 2.399995 -2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 588 "QSB#1"))
    (pad "E9" smd circle (at 3.199994 -2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "F1" smd circle (at -3.199994 -1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 498 "MDB11"))
    (pad "F2" smd circle (at -2.399995 -1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "F3" smd circle (at -1.599997 -1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 560 "DQMB#1"))
    (pad "F7" smd circle (at 1.599997 -1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 587 "QSB1"))
    (pad "F8" smd circle (at 2.399995 -1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "F9" smd circle (at 3.199994 -1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 499 "MDB12"))
    (pad "G1" smd circle (at -3.199994 -0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "G2" smd circle (at -2.399995 -0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 497 "MDB10"))
    (pad "G3" smd circle (at -1.599997 -0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "G7" smd circle (at 1.599997 -0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "G8" smd circle (at 2.399995 -0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 501 "MDB14"))
    (pad "G9" smd circle (at 3.199994 -0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "H1" smd circle (at -3.199994 0 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 557 "MDB8"))
    (pad "H2" smd circle (at -2.399995 0 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "H3" smd circle (at -1.599997 0 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 558 "MDB9"))
    (pad "H7" smd circle (at 1.599997 0 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 500 "MDB13"))
    (pad "H8" smd circle (at 2.399995 0 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "H9" smd circle (at 3.199994 0 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 502 "MDB15"))
    (pad "J1" smd circle (at -3.199994 0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "N18866844"))
    (pad "J2" smd circle (at -2.399995 0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 156 "N18866671"))
    (pad "J3" smd circle (at -1.599997 0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "J7" smd circle (at 1.599997 0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "J8" smd circle (at 2.399995 0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 367 "CLKB0"))
    (pad "J9" smd circle (at 3.199994 0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "K2" smd circle (at -2.399995 1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 491 "CKEB0"))
    (pad "K3" smd circle (at -1.599997 1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 603 "WEB#0"))
    (pad "K7" smd circle (at 1.599997 1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 601 "RASB#0"))
    (pad "K8" smd circle (at 2.399995 1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 366 "CLKB0#"))
    (pad "K9" smd circle (at 3.199994 1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 583 "ODTB0"))
    (pad "L1" smd circle (at -3.199994 2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 582 "B_BA2"))
    (pad "L2" smd circle (at -2.399995 2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 580 "B_BA0"))
    (pad "L3" smd circle (at -1.599997 2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 581 "B_BA1"))
    (pad "L7" smd circle (at 1.599997 2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 489 "CASB#0"))
    (pad "L8" smd circle (at 2.399995 2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 493 "CSB0_0#"))
    (pad "M2" smd circle (at -2.399995 3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 569 "MAB10"))
    (pad "M3" smd circle (at -1.599997 3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 568 "MAB1"))
    (pad "M7" smd circle (at 1.599997 3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 571 "MAB2"))
    (pad "M8" smd circle (at 2.399995 3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 567 "MAB0"))
    (pad "M9" smd circle (at 3.199994 3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "N1" smd circle (at -3.199994 3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "N2" smd circle (at -2.399995 3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 572 "MAB3"))
    (pad "N3" smd circle (at -1.599997 3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 574 "MAB5"))
    (pad "N7" smd circle (at 1.599997 3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 575 "MAB6"))
    (pad "N8" smd circle (at 2.399995 3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 573 "MAB4"))
    (pad "P2" smd circle (at -2.399995 4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 576 "MAB7"))
    (pad "P3" smd circle (at -1.599997 4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 578 "MAB9"))
    (pad "P7" smd circle (at 1.599997 4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 570 "MAB11"))
    (pad "P8" smd circle (at 2.399995 4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 577 "MAB8"))
    (pad "P9" smd circle (at 3.199994 4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "R1" smd circle (at -3.199994 5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "R2" smd circle (at -2.399995 5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 579 "MAB12"))
    (pad "R3" smd circle (at -1.599997 5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "R7" smd circle (at 1.599997 5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "R8" smd circle (at 2.399995 5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
  )
  (footprint "lib:NET_SHORT_1" (layer "F.Cu")
    (tedit 0)
    (at -32.698012 45.609985 -45)
    (fp_text reference "NS17" (at -0.893248 0.893248 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0 315) (size 0.500024 0.500024) (drill 0.250012) (layers *.Cu *.Mask)
      (net 15 "AGND"))
    (pad "2" smd circle (at 0.2 0 315) (size 0.127 0.127) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 40 "N22176225"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -47.198008 59.310009)
    (fp_text reference "C328" (at 1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 145 "N22176083"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -46.29801 43.30999 -90)
    (fp_text reference "C622" (at 1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 184 "DPB1N"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 185 "DVIB_TX0+"))
  )
  (footprint "lib:NET_SHORT_1" (layer "F.Cu")
    (tedit 0)
    (at -37.698002 39.409998)
    (fp_text reference "NS14" (at -1.263244 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 0.500024 0.500024) (drill 0.250012) (layers *.Cu *.Mask)
      (net 15 "AGND"))
    (pad "2" smd circle (at 0.2 0) (size 0.127 0.127) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 49 "N22175859"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -51.298 8.510009 90)
    (fp_text reference "R122" (at -1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "+3VRUN"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 346 "N21377265"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -46.09801 32.309987 -90)
    (fp_text reference "R1002" (at 2.54 -2.2225 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 163 "DVI_CLK-"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 297 "N22316530"))
  )
  (footprint "lib:CAP3216_1" (layer "F.Cu")
    (tedit 0)
    (at 15.101994 20.009986 90)
    (fp_text reference "C431" (at -1.65848 1.658468 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -1.4478 90) (size 1.799996 1.399997) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 142 "G_PWR_SRC"))
    (pad "2" smd rect (at 0 1.4478 90) (size 1.799996 1.399997) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1608_0_89H_1" (layer "F.Cu")
    (tedit 0)
    (at -6.948 12.685007 180)
    (fp_text reference "C82" (at -1.587475 -1.270025 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 180) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "N18866844"))
    (pad "2" smd rect (at 0 0.7874 180) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at 11.002002 24.610002)
    (fp_text reference "C98" (at 1.5875 1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -51.298 5.509989 -90)
    (fp_text reference "R131" (at 1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 348 "N17821681"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 342 "OTEMP#"))
  )
  (footprint "lib:GEOM0006_1" (layer "F.Cu")
    (tedit 0)
    (at -0.698 7.009986 -90)
    (fp_text reference "L41" (at 0 0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 4.89999 0 270) (size 3.799992 4.599991) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "N22672706"))
    (pad "2" smd rect (at -4.89999 0 270) (size 3.799992 4.599991) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "VDD_CORE"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -23.698004 16.560005 90)
    (fp_text reference "C143" (at -1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -46.09801 37.310002 -90)
    (fp_text reference "R1007" (at 2.54 -2.2225 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 177 "DVI_TX1+"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 297 "N22316530"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -44.698013 30.50999 -90)
    (fp_text reference "R6" (at 0.635 -1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "+3VRUN"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 202 "I2C_DAT"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -46.09801 34.310008 -90)
    (fp_text reference "R1004" (at 2.54 -2.2225 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 165 "DVI_TX0-"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 297 "N22316530"))
  )
  (footprint "lib:SO8_1_78H_1" (layer "F.Cu")
    (tedit 0)
    (at -45.098012 14.509997)
    (fp_text reference "U15" (at 1.5875 1.2573 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd oval (at -1.905 2.8448) (size 0.639978 1.579982) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 323 "GPIO22"))
    (pad "2" smd oval (at -0.635 2.8448) (size 0.639978 1.579982) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 322 "GPIO8"))
    (pad "3" smd oval (at 0.635 2.8448) (size 0.639978 1.579982) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 347 "N21360761"))
    (pad "4" smd oval (at 1.905 2.8448) (size 0.639978 1.579982) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "5" smd oval (at 1.905 -2.8702) (size 0.639978 1.579982) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 318 "GPIO9"))
    (pad "6" smd oval (at 0.635 -2.8702) (size 0.639978 1.579982) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 372 "SCLK"))
    (pad "7" smd oval (at -0.635 -2.8702) (size 0.639978 1.579982) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "+3VRUN"))
    (pad "8" smd oval (at -1.905 -2.8702) (size 0.639978 1.579982) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "+3VRUN"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -23.698004 6.56 -90)
    (fp_text reference "R646" (at 1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 153 "N18876007"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at 0.352011 41.109994 180)
    (fp_text reference "C581" (at -1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -48.798005 3.609993 -90)
    (fp_text reference "R729" (at 1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 299 "CTFB"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 289 "MB_THERM#"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at 8.302008 57.409987)
    (fp_text reference "C576" (at 1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "N18849793"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -8.598009 38.909999)
    (fp_text reference "C289" (at 1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "MPVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "N22175956"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -51.797999 26.009999 -90)
    (fp_text reference "R153" (at 1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 331 "VID_7"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "+3VRUN"))
  )
  (footprint "lib:TP055PRI_1" (layer "F.Cu")
    (tedit 0)
    (at -21.898008 59.010009)
    (fp_text reference "TP6" (at -0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd circle (at 0 0) (size 0.550012 0.550012) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 234 "PCIE_RXN15"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -51.298 3.509993 90)
    (fp_text reference "R132" (at -1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "+3VRUN"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 348 "N17821681"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -43.69799 37.310002 -90)
    (fp_text reference "C618" (at 1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 176 "DPA2N"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 177 "DVI_TX1+"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -48.698005 47.310007 -90)
    (fp_text reference "R1017" (at 2.54 -2.2225 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 193 "DVIB_TX2+"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 298 "N22316558"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -42.697992 50.110002)
    (fp_text reference "C396" (at 1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "VDD1DI"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "N22175888"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -52.597997 40.909995 180)
    (fp_text reference "R1001" (at -2.2225 -2.54 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "+5VRUN"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:SOT23_3PIN_1_1H_1" (layer "F.Cu")
    (tedit 0)
    (at -51.797999 43.709989 -90)
    (fp_text reference "Q30" (at 1.227671 -1.534586 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.9398 1.143 270) (size 0.640004 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "+5VRUN"))
    (pad "2" smd rect (at 0.9398 1.143 270) (size 0.640004 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "3" smd rect (at 0 -1.143 270) (size 0.640004 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 298 "N22316558"))
  )
  (footprint "lib:SOT23_3PIN_1_1H_1" (layer "F.Cu")
    (tedit 0)
    (at -49.298004 37.210002 -90)
    (fp_text reference "Q29" (at 1.227671 -1.534586 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.9398 1.143 270) (size 0.640004 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "+5VRUN"))
    (pad "2" smd rect (at 0.9398 1.143 270) (size 0.640004 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "3" smd rect (at 0 -1.143 270) (size 0.640004 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 297 "N22316530"))
  )
  (footprint "lib:GEOM0008_1" (layer "F.Cu")
    (tedit 0)
    (at 7.376991 15.934988 -150)
    (fp_text reference "Q23" (at -0.738571 -1.895758 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -1.905025 3.174975 210) (size 0.759993 1.599997) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "N22672706"))
    (pad "2" smd rect (at -0.635 3.174975 210) (size 0.759993 1.599997) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "N22672706"))
    (pad "3" smd rect (at 0.634975 3.175 210) (size 0.759993 1.599997) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "N22672706"))
    (pad "4" smd rect (at 1.905 3.174975 210) (size 0.759993 1.599997) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 302 "N22672940"))
    (pad "5" smd rect (at 1.905025 -3.169996 210) (size 0.759993 1.599997) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 142 "G_PWR_SRC"))
    (pad "6" smd rect (at 0.634975 -3.169996 210) (size 0.759993 1.599997) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 142 "G_PWR_SRC"))
    (pad "7" smd rect (at -0.634975 -3.170022 210) (size 0.759993 1.599997) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 142 "G_PWR_SRC"))
    (pad "8" smd rect (at -1.905025 -3.169996 210) (size 0.759993 1.599997) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 142 "G_PWR_SRC"))
    (pad "9" smd rect (at 0 0 210) (size 5.550002 3.474999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 142 "G_PWR_SRC"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -51.797999 62.810002 -90)
    (fp_text reference "R200" (at 1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 203 "BL_ENA"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 306 "OPT_BL_ENA"))
  )
  (footprint "lib:CAP1608_0_89H_1" (layer "F.Cu")
    (tedit 0)
    (at -40.697996 9.110008 -90)
    (fp_text reference "C141" (at 1.905025 -1.904975 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 270) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.7874 270) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:XTAL_TXC_6P_1" (layer "F.Cu")
    (tedit 0)
    (at -50.698001 57.409987 90)
    (fp_text reference "Y1" (at 0 -0.635 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -2.950007 1.27 90) (size 1.699997 1.399997) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 145 "N22176083"))
    (pad "2" smd rect (at 2.950007 1.27 90) (size 1.699997 1.399997) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "3" smd rect (at 2.950007 -1.27 90) (size 1.699997 1.399997) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 144 "N22176881"))
    (pad "4" smd rect (at -2.950007 -1.27 90) (size 1.699997 1.399997) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:BGA080_11X13-84_1" (layer "F.Cu")
    (tedit 0)
    (at -31.998013 12.310001 180)
    (fp_text reference "U24" (at -1.5875 -1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "A1" smd circle (at -3.199994 -5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "A2" smd circle (at -2.399995 -5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "A3" smd circle (at -1.599997 -5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "A7" smd circle (at 1.599997 -5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "A8" smd circle (at 2.399995 -5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 598 "QSB#6"))
    (pad "A9" smd circle (at 3.199994 -5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "B1" smd circle (at -3.199994 -4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 543 "MDB52"))
    (pad "B2" smd circle (at -2.399995 -4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "B3" smd circle (at -1.599997 -4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 565 "DQMB#6"))
    (pad "B7" smd circle (at 1.599997 -4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 597 "QSB6"))
    (pad "B8" smd circle (at 2.399995 -4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "B9" smd circle (at 3.199994 -4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 539 "MDB49"))
    (pad "C1" smd circle (at -3.199994 -3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "C2" smd circle (at -2.399995 -3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 545 "MDB54"))
    (pad "C3" smd circle (at -1.599997 -3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "C7" smd circle (at 1.599997 -3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "C8" smd circle (at 2.399995 -3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 542 "MDB51"))
    (pad "C9" smd circle (at 3.199994 -3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "D1" smd circle (at -3.199994 -3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 546 "MDB55"))
    (pad "D2" smd circle (at -2.399995 -3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "D3" smd circle (at -1.599997 -3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 544 "MDB53"))
    (pad "D7" smd circle (at 1.599997 -3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 541 "MDB50"))
    (pad "D8" smd circle (at 2.399995 -3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "D9" smd circle (at 3.199994 -3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 538 "MDB48"))
    (pad "E1" smd circle (at -3.199994 -2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "E2" smd circle (at -2.399995 -2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "E3" smd circle (at -1.599997 -2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "E7" smd circle (at 1.599997 -2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "E8" smd circle (at 2.399995 -2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 594 "QSB#4"))
    (pad "E9" smd circle (at 3.199994 -2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "F1" smd circle (at -3.199994 -1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 524 "MDB35"))
    (pad "F2" smd circle (at -2.399995 -1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "F3" smd circle (at -1.599997 -1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 563 "DQMB#4"))
    (pad "F7" smd circle (at 1.599997 -1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 593 "QSB4"))
    (pad "F8" smd circle (at 2.399995 -1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "F9" smd circle (at 3.199994 -1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 526 "MDB37"))
    (pad "G1" smd circle (at -3.199994 -0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "G2" smd circle (at -2.399995 -0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 523 "MDB34"))
    (pad "G3" smd circle (at -1.599997 -0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "G7" smd circle (at 1.599997 -0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "G8" smd circle (at 2.399995 -0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 525 "MDB36"))
    (pad "G9" smd circle (at 3.199994 -0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "H1" smd circle (at -3.199994 0 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 521 "MDB32"))
    (pad "H2" smd circle (at -2.399995 0 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "H3" smd circle (at -1.599997 0 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 522 "MDB33"))
    (pad "H7" smd circle (at 1.599997 0 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 527 "MDB38"))
    (pad "H8" smd circle (at 2.399995 0 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "H9" smd circle (at 3.199994 0 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 528 "MDB39"))
    (pad "J1" smd circle (at -3.199994 0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "N18875755"))
    (pad "J2" smd circle (at -2.399995 0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 153 "N18876007"))
    (pad "J3" smd circle (at -1.599997 0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "J7" smd circle (at 1.599997 0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "J8" smd circle (at 2.399995 0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 371 "CLKB1"))
    (pad "J9" smd circle (at 3.199994 0.799998 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "K2" smd circle (at -2.399995 1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 492 "CKEB1"))
    (pad "K3" smd circle (at -1.599997 1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 604 "WEB#1"))
    (pad "K7" smd circle (at 1.599997 1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 602 "RASB#1"))
    (pad "K8" smd circle (at 2.399995 1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 370 "CLKB1#"))
    (pad "K9" smd circle (at 3.199994 1.599997 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 584 "ODTB1"))
    (pad "L1" smd circle (at -3.199994 2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 582 "B_BA2"))
    (pad "L2" smd circle (at -2.399995 2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 580 "B_BA0"))
    (pad "L3" smd circle (at -1.599997 2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 581 "B_BA1"))
    (pad "L7" smd circle (at 1.599997 2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 490 "CASB#1"))
    (pad "L8" smd circle (at 2.399995 2.399995 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 494 "CSB1_0#"))
    (pad "M2" smd circle (at -2.399995 3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 569 "MAB10"))
    (pad "M3" smd circle (at -1.599997 3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 568 "MAB1"))
    (pad "M7" smd circle (at 1.599997 3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 571 "MAB2"))
    (pad "M8" smd circle (at 2.399995 3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 567 "MAB0"))
    (pad "M9" smd circle (at 3.199994 3.199994 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "N1" smd circle (at -3.199994 3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "N2" smd circle (at -2.399995 3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 572 "MAB3"))
    (pad "N3" smd circle (at -1.599997 3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 574 "MAB5"))
    (pad "N7" smd circle (at 1.599997 3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 575 "MAB6"))
    (pad "N8" smd circle (at 2.399995 3.999992 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 573 "MAB4"))
    (pad "P2" smd circle (at -2.399995 4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 576 "MAB7"))
    (pad "P3" smd circle (at -1.599997 4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 578 "MAB9"))
    (pad "P7" smd circle (at 1.599997 4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 570 "MAB11"))
    (pad "P8" smd circle (at 2.399995 4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 577 "MAB8"))
    (pad "P9" smd circle (at 3.199994 4.79999 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "R1" smd circle (at -3.199994 5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "R2" smd circle (at -2.399995 5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 579 "MAB12"))
    (pad "R3" smd circle (at -1.599997 5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "R7" smd circle (at 1.599997 5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "R8" smd circle (at 2.399995 5.599989 180) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
  )
  (footprint "lib:CAP1608_0_89H_1" (layer "F.Cu")
    (tedit 0)
    (at 15.901993 48.610005 180)
    (fp_text reference "C73" (at -1.587475 -1.270025 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 180) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.7874 180) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:NET_SHORT_1" (layer "F.Cu")
    (tedit 0)
    (at -35.098007 38.41 -135)
    (fp_text reference "NS1" (at 0.668742 0.668742 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0 225) (size 0.500024 0.500024) (drill 0.250012) (layers *.Cu *.Mask)
      (net 15 "AGND"))
    (pad "2" smd circle (at 0.2 0 225) (size 0.127 0.127) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 51 "N22175966"))
  )
  (footprint "lib:TP055PRI_1" (layer "F.Cu")
    (tedit 0)
    (at -35.698006 59.010009)
    (fp_text reference "TP1" (at -0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd circle (at 0 0) (size 0.550012 0.550012) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 243 "PCIE_RXP0"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -23.698004 19.06 -90)
    (fp_text reference "C144" (at 1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -47.198008 57.109988 180)
    (fp_text reference "R999" (at -1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 145 "N22176083"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 144 "N22176881"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at 7.30201 41.109994)
    (fp_text reference "C546" (at 1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "N18859523"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -47.198008 55.060005 180)
    (fp_text reference "C327" (at -1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 144 "N22176881"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -26.997998 2.709995)
    (fp_text reference "C145" (at 1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -36.998003 3.109994 -90)
    (fp_text reference "R657" (at 1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 292 "BB_ENA"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_BGA_1" (layer "F.Cu")
    (tedit 0)
    (at -42.197993 43.009991 135)
    (fp_text reference "C631" (at -2.694077 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 135) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 127 "DPB_VDDR"))
    (pad "2" smd rect (at 0 0.492608 315) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 128 "N22176186"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at 13.35201 41.009995 180)
    (fp_text reference "R640" (at -1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 151 "N18859640"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -7.698011 38.909999)
    (fp_text reference "C288" (at 1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "MPVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "N22175956"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at 1.501996 24.610002 180)
    (fp_text reference "C97" (at -1.5875 -1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1608_0_89H_1" (layer "F.Cu")
    (tedit 0)
    (at 5.001989 24.510002 90)
    (fp_text reference "C104" (at -1.905025 1.904975 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 90) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.7874 90) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -51.897999 37.210002)
    (fp_text reference "R1000" (at 2.2225 2.54 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "+5VRUN"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1608_0_89H_1" (layer "F.Cu")
    (tedit 0)
    (at 15.901993 53.409995 180)
    (fp_text reference "C72" (at -1.587475 -1.270025 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 180) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.7874 180) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1608_0_89H_1" (layer "F.Cu")
    (tedit 0)
    (at -11.598003 3.009994 -90)
    (fp_text reference "C118" (at 1.905025 -1.904975 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 270) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.7874 270) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:TP055PRI_1" (layer "F.Cu")
    (tedit 0)
    (at -22.698006 59.010009)
    (fp_text reference "TP5" (at -0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd circle (at 0 0) (size 0.550012 0.550012) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 250 "PCIE_RXP15"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at 11.302002 57.409987)
    (fp_text reference "R42" (at 1.5875 1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 150 "N18850055"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -6.998012 9.210007 90)
    (fp_text reference "C590" (at -1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 156 "N18866671"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -36.647991 62.010003 90)
    (fp_text reference "C263" (at -1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "PCIE_PVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -23.698004 11.059991 -90)
    (fp_text reference "C147" (at 1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -46.29801 44.709987 -90)
    (fp_text reference "C623" (at 1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 186 "DPB2P"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 187 "DVIB_TX1-"))
  )
  (footprint "lib:BGA080_11X13-84_1" (layer "F.Cu")
    (tedit 0)
    (at 7.10201 49.410003 90)
    (fp_text reference "U4" (at -0.635 1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "A1" smd circle (at -3.199994 -5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "A2" smd circle (at -2.399995 -5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "A3" smd circle (at -1.599997 -5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "A7" smd circle (at 1.599997 -5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "A8" smd circle (at 2.399995 -5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 470 "QSA#0"))
    (pad "A9" smd circle (at 3.199994 -5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "B1" smd circle (at -3.199994 -4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 379 "MDA0"))
    (pad "B2" smd circle (at -2.399995 -4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "B3" smd circle (at -1.599997 -4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 443 "DQMA#0"))
    (pad "B7" smd circle (at 1.599997 -4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 469 "QSA0"))
    (pad "B8" smd circle (at 2.399995 -4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "B9" smd circle (at 3.199994 -4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 440 "MDA7"))
    (pad "C1" smd circle (at -3.199994 -3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "C2" smd circle (at -2.399995 -3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 380 "MDA1"))
    (pad "C3" smd circle (at -1.599997 -3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "C7" smd circle (at 1.599997 -3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "C8" smd circle (at 2.399995 -3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 435 "MDA6"))
    (pad "C9" smd circle (at 3.199994 -3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "D1" smd circle (at -3.199994 -3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 391 "MDA2"))
    (pad "D2" smd circle (at -2.399995 -3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "D3" smd circle (at -1.599997 -3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 402 "MDA3"))
    (pad "D7" smd circle (at 1.599997 -3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 413 "MDA4"))
    (pad "D8" smd circle (at 2.399995 -3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "D9" smd circle (at 3.199994 -3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 424 "MDA5"))
    (pad "E1" smd circle (at -3.199994 -2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "E2" smd circle (at -2.399995 -2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "E3" smd circle (at -1.599997 -2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "E7" smd circle (at 1.599997 -2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "E8" smd circle (at 2.399995 -2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 476 "QSA#3"))
    (pad "E9" smd circle (at 3.199994 -2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "F1" smd circle (at -3.199994 -1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 399 "MDA27"))
    (pad "F2" smd circle (at -2.399995 -1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "F3" smd circle (at -1.599997 -1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 446 "DQMA#3"))
    (pad "F7" smd circle (at 1.599997 -1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 475 "QSA3"))
    (pad "F8" smd circle (at 2.399995 -1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "F9" smd circle (at 3.199994 -1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 400 "MDA28"))
    (pad "G1" smd circle (at -3.199994 -0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "G2" smd circle (at -2.399995 -0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 396 "MDA24"))
    (pad "G3" smd circle (at -1.599997 -0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "G7" smd circle (at 1.599997 -0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "G8" smd circle (at 2.399995 -0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 403 "MDA30"))
    (pad "G9" smd circle (at 3.199994 -0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "H1" smd circle (at -3.199994 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 397 "MDA25"))
    (pad "H2" smd circle (at -2.399995 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "H3" smd circle (at -1.599997 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 398 "MDA26"))
    (pad "H7" smd circle (at 1.599997 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 401 "MDA29"))
    (pad "H8" smd circle (at 2.399995 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "H9" smd circle (at 3.199994 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 404 "MDA31"))
    (pad "J1" smd circle (at -3.199994 0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "N18849793"))
    (pad "J2" smd circle (at -2.399995 0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 150 "N18850055"))
    (pad "J3" smd circle (at -1.599997 0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "J7" smd circle (at 1.599997 0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "J8" smd circle (at 2.399995 0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 365 "CLKA0"))
    (pad "J9" smd circle (at 3.199994 0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "K2" smd circle (at -2.399995 1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 375 "CKEA0"))
    (pad "K3" smd circle (at -1.599997 1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 487 "WEA#0"))
    (pad "K7" smd circle (at 1.599997 1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 485 "RASA#0"))
    (pad "K8" smd circle (at 2.399995 1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 364 "CLKA0#"))
    (pad "K9" smd circle (at 3.199994 1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 467 "ODTA0"))
    (pad "L1" smd circle (at -3.199994 2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 466 "A_BA2"))
    (pad "L2" smd circle (at -2.399995 2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 464 "A_BA0"))
    (pad "L3" smd circle (at -1.599997 2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 465 "A_BA1"))
    (pad "L7" smd circle (at 1.599997 2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 373 "CASA#0"))
    (pad "L8" smd circle (at 2.399995 2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 377 "CSA0_0#"))
    (pad "M2" smd circle (at -2.399995 3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 453 "MAA10"))
    (pad "M3" smd circle (at -1.599997 3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 452 "MAA1"))
    (pad "M7" smd circle (at 1.599997 3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 455 "MAA2"))
    (pad "M8" smd circle (at 2.399995 3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 451 "MAA0"))
    (pad "M9" smd circle (at 3.199994 3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "N1" smd circle (at -3.199994 3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "N2" smd circle (at -2.399995 3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 456 "MAA3"))
    (pad "N3" smd circle (at -1.599997 3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 458 "MAA5"))
    (pad "N7" smd circle (at 1.599997 3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 459 "MAA6"))
    (pad "N8" smd circle (at 2.399995 3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 457 "MAA4"))
    (pad "P2" smd circle (at -2.399995 4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 460 "MAA7"))
    (pad "P3" smd circle (at -1.599997 4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 462 "MAA9"))
    (pad "P7" smd circle (at 1.599997 4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 454 "MAA11"))
    (pad "P8" smd circle (at 2.399995 4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 461 "MAA8"))
    (pad "P9" smd circle (at 3.199994 4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "R1" smd circle (at -3.199994 5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "R2" smd circle (at -2.399995 5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 463 "MAA12"))
    (pad "R3" smd circle (at -1.599997 5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "R7" smd circle (at 1.599997 5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "R8" smd circle (at 2.399995 5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
  )
  (footprint "lib:NET_SHORT_1" (layer "F.Cu")
    (tedit 0)
    (at -39.797998 45.009987)
    (fp_text reference "NS4" (at -0.945744 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 0.500024 0.500024) (drill 0.250012) (layers *.Cu *.Mask)
      (net 15 "AGND"))
    (pad "2" smd circle (at 0.2 0) (size 0.127 0.127) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "N22176582"))
  )
  (footprint "lib:RES1005_BGA_1" (layer "F.Cu")
    (tedit 0)
    (at -52.797997 70.409987 180)
    (fp_text reference "R1071" (at -2.2225 -2.54 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 198 "N22794094"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:NET_SHORT_1" (layer "F.Cu")
    (tedit 0)
    (at -35.098007 46.810008 45)
    (fp_text reference "NS2" (at -0.668742 -0.668742 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0 45) (size 0.500024 0.500024) (drill 0.250012) (layers *.Cu *.Mask)
      (net 15 "AGND"))
    (pad "2" smd circle (at 0.2 0 45) (size 0.127 0.127) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "N22176268"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -43.69799 33.31001 -90)
    (fp_text reference "C616" (at 1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 172 "DPA0N"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 173 "DVI_CLK+"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -48.098006 71.110011 90)
    (fp_text reference "R1032" (at -2.54 2.2225 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 339 "DVI_HPD3"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 271 "N22276768"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -23.698004 12.610001 90)
    (fp_text reference "C569" (at -1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "N18875755"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -48.798005 2.709995 90)
    (fp_text reference "R1036" (at -2.54 2.2225 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "+3VRUN"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 299 "CTFB"))
  )
  (footprint "lib:NET_SHORT_1" (layer "F.Cu")
    (tedit 0)
    (at -9.798007 39.809997)
    (fp_text reference "NS7" (at -0.945744 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 0.500024 0.500024) (drill 0.250012) (layers *.Cu *.Mask)
      (net 15 "AGND"))
    (pad "2" smd circle (at 0.2 0) (size 0.127 0.127) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "N22175956"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -46.09801 35.310006 -90)
    (fp_text reference "R1005" (at 2.54 -2.2225 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 167 "DVI_TX0+"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 297 "N22316530"))
  )
  (footprint "lib:CAP1005_BGA_1" (layer "F.Cu")
    (tedit 0)
    (at -43.59799 50.110002)
    (fp_text reference "C268" (at 1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "VDD1DI"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "N22175888"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -46.29801 40.309996 -90)
    (fp_text reference "C613" (at 1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 168 "DPB0P"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 169 "DVIB_CLK-"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -19.698012 24.810002 90)
    (fp_text reference "C258" (at -1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "VDDRHB2"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "N16909550"))
  )
  (footprint "lib:RES1005_BGA_1" (layer "F.Cu")
    (tedit 0)
    (at -51.948011 70.409987 180)
    (fp_text reference "R1035" (at -2.2225 -2.54 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 196 "N22540247"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 335 "DDC3CLK"))
  )
  (footprint "lib:NET_SHORT_1" (layer "F.Cu")
    (tedit 0)
    (at -8.212996 50.080004 90)
    (fp_text reference "NS9" (at 0 -0.945744 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0 90) (size 0.500024 0.500024) (drill 0.250012) (layers *.Cu *.Mask)
      (net 15 "AGND"))
    (pad "2" smd circle (at 0.2 0 90) (size 0.127 0.127) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "N16910486"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -46.29801 47.710007 -90)
    (fp_text reference "C626" (at 1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 192 "DPB3N"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 193 "DVIB_TX2+"))
  )
  (footprint "lib:GEOM0004_1" (layer "F.Cu")
    (tedit 0)
    (at -40.097997 60.710006 90)
    (fp_text reference "C424" (at -1.190929 1.19093 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144 90) (size 1.27 1.219987) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.9144 90) (size 1.27 1.219987) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -46.29801 46.710009 -90)
    (fp_text reference "C625" (at 1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 190 "DPB3P"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 191 "DVIB_TX2-"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at 8.351995 41.109994 180)
    (fp_text reference "C99" (at -1.5875 -1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
  )
  (footprint "lib:CAP1608_0_89H_1" (layer "F.Cu")
    (tedit 0)
    (at 6.301986 57.209988 90)
    (fp_text reference "C577" (at -1.905025 1.904975 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 90) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "N18849793"))
    (pad "2" smd rect (at 0 0.7874 90) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -34.998007 70.209987)
    (fp_text reference "R212" (at 1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "+3VRUN"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 282 "DDC1DATA"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at 2.501994 24.610002)
    (fp_text reference "C100" (at 1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
  )
  (footprint "lib:GEOM0008_1" (layer "F.Cu")
    (tedit 0)
    (at 2.101995 18.409989 30)
    (fp_text reference "Q25" (at 0.738571 1.895758 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -1.905025 3.174975 30) (size 0.759993 1.599997) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "2" smd rect (at -0.635 3.174975 30) (size 0.759993 1.599997) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "3" smd rect (at 0.634975 3.175 30) (size 0.759993 1.599997) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "4" smd rect (at 1.905 3.174975 30) (size 0.759993 1.599997) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 304 "N22672861"))
    (pad "5" smd rect (at 1.905025 -3.169996 30) (size 0.759993 1.599997) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "N22672706"))
    (pad "6" smd rect (at 0.634975 -3.169996 30) (size 0.759993 1.599997) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "N22672706"))
    (pad "7" smd rect (at -0.634975 -3.170022 30) (size 0.759993 1.599997) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "N22672706"))
    (pad "8" smd rect (at -1.905025 -3.169996 30) (size 0.759993 1.599997) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "N22672706"))
    (pad "9" smd rect (at 0 0 30) (size 5.550002 3.474999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "N22672706"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -43.69799 35.310006 -90)
    (fp_text reference "C612" (at 1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 166 "DPA1N"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 167 "DVI_TX0+"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -6.998012 10.910004 90)
    (fp_text reference "C81" (at -1.27 1.5875 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "N18866844"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -46.09801 33.31001 -90)
    (fp_text reference "R1003" (at 2.54 -2.2225 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 173 "DVI_CLK+"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 297 "N22316530"))
  )
  (footprint "lib:CAP1608_0_89H_1" (layer "F.Cu")
    (tedit 0)
    (at -23.698004 13.909998 90)
    (fp_text reference "C570" (at -1.905025 1.904975 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 90) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "N18875755"))
    (pad "2" smd rect (at 0 0.7874 90) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -46.29801 42.309992 -90)
    (fp_text reference "C614" (at 1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 170 "DPB1P"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 171 "DVIB_TX0-"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -48.698005 45.309986 -90)
    (fp_text reference "R1015" (at 2.54 -2.2225 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 189 "DVIB_TX1+"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 298 "N22316558"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -51.797999 18.00999 -90)
    (fp_text reference "R142" (at 1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 320 "GPIO12"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "+3VRUN"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -6.998012 7.509985 -90)
    (fp_text reference "R48" (at 1.27 -1.5875 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 156 "N18866671"))
  )
  (footprint "lib:GEOM0007_1" (layer "F.Cu")
    (tedit 0)
    (at 0.001999 77.409998)
    (fp_text reference "MPCIE1" (at -25.109983 -1.399972 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "A1" smd rect (at 6.920001 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 142 "G_PWR_SRC"))
    (pad "A2" smd rect (at 6.420002 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 142 "G_PWR_SRC"))
    (pad "A3" smd rect (at 5.920003 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 142 "G_PWR_SRC"))
    (pad "A4" smd rect (at 5.420004 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 142 "G_PWR_SRC"))
    (pad "A5" smd rect (at 4.920005 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 142 "G_PWR_SRC"))
    (pad "A6" smd rect (at 4.420006 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 142 "G_PWR_SRC"))
    (pad "A7" smd rect (at 3.920007 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 142 "G_PWR_SRC"))
    (pad "A8" smd rect (at 3.420008 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 142 "G_PWR_SRC"))
    (pad "A9" smd rect (at 2.920009 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "A10" smd rect (at 2.42001 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "A11" smd rect (at 1.920011 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "A12" smd rect (at 1.420012 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "A19" smd rect (at -2.080006 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 53 "N22276438"))
    (pad "A20" smd rect (at -2.580005 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 55 "N22276387"))
    (pad "A21" smd rect (at -3.080004 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "A22" smd rect (at -3.580003 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 57 "N22276563"))
    (pad "A23" smd rect (at -4.080002 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 59 "N22276557"))
    (pad "A24" smd rect (at -4.580001 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "A25" smd rect (at -5.08 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "N22276551"))
    (pad "A26" smd rect (at -5.579999 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 63 "N22276545"))
    (pad "A27" smd rect (at -6.079998 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "A28" smd rect (at -6.579997 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 65 "N22276539"))
    (pad "A29" smd rect (at -7.079996 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 67 "N22276533"))
    (pad "A30" smd rect (at -7.579995 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "A31" smd rect (at -8.079994 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 69 "N22276527"))
    (pad "A32" smd rect (at -8.579993 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 71 "N22276496"))
    (pad "A33" smd rect (at -9.079992 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "A34" smd rect (at -9.579991 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 73 "N22276444"))
    (pad "A35" smd rect (at -10.07999 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 75 "N22276440"))
    (pad "A36" smd rect (at -10.579989 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "A37" smd rect (at -11.079988 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 77 "N22276389"))
    (pad "A38" smd rect (at -11.579987 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 79 "N22276565"))
    (pad "A39" smd rect (at -12.080011 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "A40" smd rect (at -12.58001 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 81 "N22276559"))
    (pad "A41" smd rect (at -13.080009 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 83 "N22276553"))
    (pad "A42" smd rect (at -13.580008 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "A43" smd rect (at -14.080007 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 85 "N22276547"))
    (pad "A44" smd rect (at -14.580006 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 87 "N22276541"))
    (pad "A45" smd rect (at -15.080005 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "A46" smd rect (at -15.580004 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 89 "N22276535"))
    (pad "A47" smd rect (at -16.080003 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 91 "N22276529"))
    (pad "A48" smd rect (at -16.580002 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "A49" smd rect (at -17.080001 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 93 "N22276498"))
    (pad "A50" smd rect (at -17.58 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 95 "N22276446"))
    (pad "A51" smd rect (at -18.079999 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "A52" smd rect (at -18.579998 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 97 "N22276442"))
    (pad "A53" smd rect (at -19.079997 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 99 "N22276391"))
    (pad "A54" smd rect (at -19.579996 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "A55" smd rect (at -20.079995 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 101 "N22276385"))
    (pad "A56" smd rect (at -20.579994 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 103 "N22276561"))
    (pad "A57" smd rect (at -21.079993 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "A58" smd rect (at -21.579992 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 105 "N22276555"))
    (pad "A59" smd rect (at -22.079991 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 107 "N22276549"))
    (pad "A60" smd rect (at -22.57999 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "A61" smd rect (at -23.079989 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 109 "N22276543"))
    (pad "A62" smd rect (at -23.579988 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 111 "N22276537"))
    (pad "A63" smd rect (at -24.079987 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "A64" smd rect (at -24.580012 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 113 "N22276531"))
    (pad "A65" smd rect (at -25.080011 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 115 "N22276525"))
    (pad "A66" smd rect (at -25.58001 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "A67" smd rect (at -26.080009 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 261 "PCIE_REFCLKN"))
    (pad "A68" smd rect (at -26.580008 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 260 "PCIE_REFCLKP"))
    (pad "A69" smd rect (at -27.080007 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 262 "CLK_REQB*"))
    (pad "A70" smd rect (at -27.580006 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 226 "PCIE_RST#"))
    (pad "A71" smd rect (at -28.080005 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "A72" smd rect (at -28.580004 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "A73" smd rect (at -29.080003 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 275 "SMB_DAT"))
    (pad "A74" smd rect (at -29.580002 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 274 "SMB_CLK"))
    (pad "A75" smd rect (at -30.080001 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 276 "THERM#"))
    (pad "A76" smd rect (at -30.58 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 284 "HSYNC"))
    (pad "A77" smd rect (at -31.079999 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 286 "VSYNC"))
    (pad "A78" smd rect (at -31.579998 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 281 "DDC1CLK"))
    (pad "A79" smd rect (at -32.079997 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 282 "DDC1DATA"))
    (pad "A80" smd rect (at -32.579996 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 263 "N22778501"))
    (pad "A81" smd rect (at -33.079995 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 264 "N22778505"))
    (pad "A82" smd rect (at -33.579994 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "A83" smd rect (at -34.079993 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 265 "N22274460"))
    (pad "A84" smd rect (at -34.579992 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 266 "N22275940"))
    (pad "A85" smd rect (at -35.079991 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 267 "AC_BAT"))
    (pad "A86" smd rect (at -35.57999 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 268 "N22274456"))
    (pad "A87" smd rect (at -36.079989 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 269 "N22275399"))
    (pad "A88" smd rect (at -36.580013 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "A89" smd rect (at -37.080012 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "A90" smd rect (at -37.580011 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "A91" smd rect (at -38.08001 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "A92" smd rect (at -38.580009 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "A93" smd rect (at -39.080008 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "A94" smd rect (at -39.580007 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "A95" smd rect (at -40.080006 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 169 "DVIB_CLK-"))
    (pad "A96" smd rect (at -40.580005 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 183 "DVIB_CLK+"))
    (pad "A97" smd rect (at -41.080004 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 270 "N22276217"))
    (pad "A98" smd rect (at -41.580003 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 271 "N22276768"))
    (pad "A99" smd rect (at -42.080002 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 272 "N22774274"))
    (pad "A100" smd rect (at -42.580001 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "A101" smd rect (at -43.08 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 191 "DVIB_TX2-"))
    (pad "A102" smd rect (at -43.579999 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 193 "DVIB_TX2+"))
    (pad "A103" smd rect (at -44.079998 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "A104" smd rect (at -44.579997 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 187 "DVIB_TX1-"))
    (pad "A105" smd rect (at -45.079996 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 189 "DVIB_TX1+"))
    (pad "A106" smd rect (at -45.579995 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "A107" smd rect (at -46.079994 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 171 "DVIB_TX0-"))
    (pad "A108" smd rect (at -46.579993 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 185 "DVIB_TX0+"))
    (pad "A109" smd rect (at -47.079992 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 195 "DVI_DETECT"))
    (pad "A110" smd rect (at -47.579991 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 163 "DVI_CLK-"))
    (pad "A111" smd rect (at -48.07999 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 173 "DVI_CLK+"))
    (pad "A112" smd rect (at -48.579989 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "A113" smd rect (at -49.080014 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 179 "DVI_TX2-"))
    (pad "A114" smd rect (at -49.580013 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 181 "DVI_TX2+"))
    (pad "A115" smd rect (at -50.080012 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "A116" smd rect (at -50.580011 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 175 "DVI_TX1-"))
    (pad "A117" smd rect (at -51.08001 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 177 "DVI_TX1+"))
    (pad "A118" smd rect (at -51.580009 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "A119" smd rect (at -52.080008 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 165 "DVI_TX0-"))
    (pad "A120" smd rect (at -52.580007 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 167 "DVI_TX0+"))
    (pad "A121" smd rect (at -53.080006 -1.399997) (size 0.329997 2.299995) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "B1" smd rect (at 6.669989 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 194 "N22274400"))
    (pad "B2" smd rect (at 6.16999 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 194 "N22274400"))
    (pad "B3" smd rect (at 5.669991 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 194 "N22274400"))
    (pad "B4" smd rect (at 5.169992 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 194 "N22274400"))
    (pad "B5" smd rect (at 4.669993 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 194 "N22274400"))
    (pad "B6" smd rect (at 4.169994 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 194 "N22274400"))
    (pad "B7" smd rect (at 3.669995 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 194 "N22274400"))
    (pad "B8" smd rect (at 3.169996 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 273 "N22628117"))
    (pad "B9" smd rect (at 2.669997 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "+5VRUN"))
    (pad "B10" smd rect (at 2.169998 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "B11" smd rect (at 1.669999 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "B12" smd rect (at 1.17 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "B19" smd rect (at -2.329993 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "B20" smd rect (at -2.829992 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 234 "PCIE_RXN15"))
    (pad "B21" smd rect (at -3.329991 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 250 "PCIE_RXP15"))
    (pad "B22" smd rect (at -3.82999 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "B23" smd rect (at -4.329989 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 233 "PCIE_RXN14"))
    (pad "B24" smd rect (at -4.829988 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 249 "PCIE_RXP14"))
    (pad "B25" smd rect (at -5.330012 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "B26" smd rect (at -5.830011 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 232 "PCIE_RXN13"))
    (pad "B27" smd rect (at -6.33001 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 248 "PCIE_RXP13"))
    (pad "B28" smd rect (at -6.830009 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "B29" smd rect (at -7.330008 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 231 "PCIE_RXN12"))
    (pad "B30" smd rect (at -7.830007 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 247 "PCIE_RXP12"))
    (pad "B31" smd rect (at -8.330006 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "B32" smd rect (at -8.830005 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 230 "PCIE_RXN11"))
    (pad "B33" smd rect (at -9.330004 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 246 "PCIE_RXP11"))
    (pad "B34" smd rect (at -9.830003 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "B35" smd rect (at -10.330002 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 229 "PCIE_RXN10"))
    (pad "B36" smd rect (at -10.830001 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 245 "PCIE_RXP10"))
    (pad "B37" smd rect (at -11.33 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "B38" smd rect (at -11.829999 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 242 "PCIE_RXN9"))
    (pad "B39" smd rect (at -12.329998 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 258 "PCIE_RXP9"))
    (pad "B40" smd rect (at -12.829997 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "B41" smd rect (at -13.329996 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 241 "PCIE_RXN8"))
    (pad "B42" smd rect (at -13.829995 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 257 "PCIE_RXP8"))
    (pad "B43" smd rect (at -14.329994 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "B44" smd rect (at -14.829993 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 240 "PCIE_RXN7"))
    (pad "B45" smd rect (at -15.329992 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 256 "PCIE_RXP7"))
    (pad "B46" smd rect (at -15.829991 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "B47" smd rect (at -16.32999 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 239 "PCIE_RXN6"))
    (pad "B48" smd rect (at -16.829989 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 255 "PCIE_RXP6"))
    (pad "B49" smd rect (at -17.329988 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "B50" smd rect (at -17.829987 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 238 "PCIE_RXN5"))
    (pad "B51" smd rect (at -18.330012 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 254 "PCIE_RXP5"))
    (pad "B52" smd rect (at -18.830011 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "B53" smd rect (at -19.33001 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 237 "PCIE_RXN4"))
    (pad "B54" smd rect (at -19.830009 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 253 "PCIE_RXP4"))
    (pad "B55" smd rect (at -20.330008 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "B56" smd rect (at -20.830007 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 236 "PCIE_RXN3"))
    (pad "B57" smd rect (at -21.330006 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 252 "PCIE_RXP3"))
    (pad "B58" smd rect (at -21.830005 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "B59" smd rect (at -22.330004 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 235 "PCIE_RXN2"))
    (pad "B60" smd rect (at -22.830003 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 251 "PCIE_RXP2"))
    (pad "B61" smd rect (at -23.330002 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "B62" smd rect (at -23.830001 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 228 "PCIE_RXN1"))
    (pad "B63" smd rect (at -24.33 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 244 "PCIE_RXP1"))
    (pad "B64" smd rect (at -24.829999 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "B65" smd rect (at -25.329998 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 227 "PCIE_RXN0"))
    (pad "B66" smd rect (at -25.829997 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 243 "PCIE_RXP0"))
    (pad "B67" smd rect (at -26.329996 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 259 "N22275059"))
    (pad "B68" smd rect (at -26.829995 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 278 "TV_CR_PR"))
    (pad "B69" smd rect (at -27.329994 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "B70" smd rect (at -27.829993 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 279 "TV_Y_G"))
    (pad "B71" smd rect (at -28.329992 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "B72" smd rect (at -28.829991 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 277 "TV_COMP_B_PB"))
    (pad "B73" smd rect (at -29.32999 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 199 "N22798927"))
    (pad "B74" smd rect (at -29.829989 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 285 "VGA_RED"))
    (pad "B75" smd rect (at -30.330013 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "B76" smd rect (at -30.830012 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 283 "VGA_GRN"))
    (pad "B77" smd rect (at -31.330011 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "B78" smd rect (at -31.83001 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 280 "VGA_BLU"))
    (pad "B79" smd rect (at -32.330009 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "B80" smd rect (at -32.830008 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 217 "TXCLK_U-"))
    (pad "B81" smd rect (at -33.330007 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 216 "TXCLK_U+"))
    (pad "B82" smd rect (at -33.830006 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "B83" smd rect (at -34.330005 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 225 "TXOUT_U3-"))
    (pad "B84" smd rect (at -34.830004 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 224 "TXOUT_U3+"))
    (pad "B85" smd rect (at -35.330003 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 200 "N22276906"))
    (pad "B86" smd rect (at -35.830002 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 223 "TXOUT_U2-"))
    (pad "B87" smd rect (at -36.330001 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 222 "TXOUT_U2+"))
    (pad "B88" smd rect (at -36.83 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "B89" smd rect (at -37.329999 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 221 "TXOUT_U1-"))
    (pad "B90" smd rect (at -37.829998 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 220 "TXOUT_U1+"))
    (pad "B91" smd rect (at -38.329997 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "B92" smd rect (at -38.829996 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 219 "TXOUT_U0-"))
    (pad "B93" smd rect (at -39.329995 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 218 "TXOUT_U0+"))
    (pad "B94" smd rect (at -39.829994 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "B95" smd rect (at -40.329993 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 206 "TXCLK_L-"))
    (pad "B96" smd rect (at -40.829992 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 205 "TXCLK_L+"))
    (pad "B97" smd rect (at -41.329991 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "B98" smd rect (at -41.82999 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 214 "TXOUT_L3-"))
    (pad "B99" smd rect (at -42.329989 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 213 "TXOUT_L3+"))
    (pad "B100" smd rect (at -42.830013 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 198 "N22794094"))
    (pad "B101" smd rect (at -43.330012 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 212 "TXOUT_L2-"))
    (pad "B102" smd rect (at -43.830011 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 211 "TXOUT_L2+"))
    (pad "B103" smd rect (at -44.33001 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "B104" smd rect (at -44.830009 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 210 "TXOUT_L1-"))
    (pad "B105" smd rect (at -45.330008 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 209 "TXOUT_L1+"))
    (pad "B106" smd rect (at -45.830007 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "B107" smd rect (at -46.330006 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 208 "TXOUT_L0-"))
    (pad "B108" smd rect (at -46.830005 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 207 "TXOUT_L0+"))
    (pad "B109" smd rect (at -47.330004 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "B110" smd rect (at -47.830003 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 202 "I2C_DAT"))
    (pad "B111" smd rect (at -48.330002 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 201 "I2C_CLK"))
    (pad "B112" smd rect (at -48.830001 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 204 "FPVCC"))
    (pad "B113" smd rect (at -49.33 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 215 "BL_BRIGHT"))
    (pad "B114" smd rect (at -49.829999 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 203 "BL_ENA"))
    (pad "B115" smd rect (at -50.329998 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 197 "N22538866"))
    (pad "B116" smd rect (at -50.829997 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 196 "N22540247"))
    (pad "B117" smd rect (at -51.329996 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "B118" smd rect (at -51.829995 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "B119" smd rect (at -52.329994 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "+3VRUN"))
    (pad "B120" smd rect (at -52.829993 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "+3VRUN"))
    (pad "B121" smd rect (at -53.329992 -1.399997) (size 0.329997 2.299995) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "+3VRUN"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -23.698004 8.059997 90)
    (fp_text reference "R648" (at -1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 153 "N18876007"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -6.998012 5.909989 90)
    (fp_text reference "C120" (at -1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -46.698009 53.409995 -90)
    (fp_text reference "R209" (at 1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 285 "VGA_RED"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -48.298006 65.860008 90)
    (fp_text reference "R1024" (at -2.54 2.2225 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 308 "DDC2DATA"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "+3VRUN"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -39.897997 59.510008 90)
    (fp_text reference "C400" (at -1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "N16909622"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at 11.302002 41.160007)
    (fp_text reference "C551" (at 1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 151 "N18859640"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -41.897993 5.20999)
    (fp_text reference "R1065" (at 2.2225 2.54 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 267 "AC_BAT"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -0.797999 70.609986 180)
    (fp_text reference "C353" (at -1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 142 "G_PWR_SRC"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -48.698005 46.310009 -90)
    (fp_text reference "R1016" (at 2.54 -2.2225 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 191 "DVIB_TX2-"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 298 "N22316558"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at 10.102004 24.610002 180)
    (fp_text reference "C589" (at -1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 160 "N18859575"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1608_0_89H_1" (layer "F.Cu")
    (tedit 0)
    (at 15.701993 35.710005 180)
    (fp_text reference "C96" (at -1.587475 -1.270025 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 180) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.7874 180) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -51.797999 21.010009 -90)
    (fp_text reference "R135" (at 1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 315 "GPIO2"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "+3VRUN"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -46.29801 41.309994 -90)
    (fp_text reference "C621" (at 1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 182 "DPB0N"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 183 "DVIB_CLK+"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -46.698009 52.409997 -90)
    (fp_text reference "R208" (at 1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 283 "VGA_GRN"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:SMIND1005_0_5H_1" (layer "F.Cu")
    (tedit 0)
    (at -39.097999 62.010003 90)
    (fp_text reference "L16" (at -1.27 1.5875 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "PCIE_PVDD"))
  )
  (footprint "lib:SOT23_3PIN_1_1H_1" (layer "F.Cu")
    (tedit 0)
    (at -44.397988 2.809995 -90)
    (fp_text reference "Q31" (at 1.227671 -1.534586 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.9398 1.143 270) (size 0.640004 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 300 "N22177921"))
    (pad "2" smd rect (at 0.9398 1.143 270) (size 0.640004 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "3" smd rect (at 0 -1.143 270) (size 0.640004 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 299 "CTFB"))
  )
  (footprint "lib:RES1005_BGA_1" (layer "F.Cu")
    (tedit 0)
    (at -48.298006 69.309989 -90)
    (fp_text reference "R1070" (at 2.54 -2.2225 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 310 "DDC4DATA"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 339 "DVI_HPD3"))
  )
  (footprint "lib:RES1608_0_8H_1" (layer "F.Cu")
    (tedit 0)
    (at -23.698004 15.309995 90)
    (fp_text reference "B50" (at -1.270025 1.587475 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 90) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "N18875755"))
    (pad "2" smd rect (at 0 0.7874 90) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -6.998012 16.909992 -90)
    (fp_text reference "C125" (at 1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
  )
  (footprint "lib:SMIND1005_0_5H_1" (layer "F.Cu")
    (tedit 0)
    (at -21.198009 25.210001)
    (fp_text reference "L13" (at 1.5875 1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "VDDRHB2"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -51.797999 27.009997 -90)
    (fp_text reference "R151" (at 1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 329 "VID_5"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "+3VRUN"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -46.698009 51.409999 -90)
    (fp_text reference "R207" (at 1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 280 "VGA_BLU"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1608_0_89H_1" (layer "F.Cu")
    (tedit 0)
    (at -6.097989 44.109988)
    (fp_text reference "C5" (at 1.269975 0.635025 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.7874) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:NET_SHORT_1" (layer "F.Cu")
    (tedit 0)
    (at -18.421002 25.334004 180)
    (fp_text reference "NS12" (at 1.263244 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0 180) (size 0.500024 0.500024) (drill 0.250012) (layers *.Cu *.Mask)
      (net 15 "AGND"))
    (pad "2" smd circle (at 0.2 0 180) (size 0.127 0.127) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "N16909550"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at 12.351987 41.109994)
    (fp_text reference "R642" (at 1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 151 "N18859640"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1608_0_89H_1" (layer "F.Cu")
    (tedit 0)
    (at -36.898003 60.710006 90)
    (fp_text reference "C264" (at -1.905025 1.904975 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 90) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "PCIE_PVDD"))
    (pad "2" smd rect (at 0 0.7874 90) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -31.697988 70.070008 180)
    (fp_text reference "R1066" (at -2.2225 -2.54 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 199 "N22798927"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at 10.402004 57.409987)
    (fp_text reference "C53" (at 1.5875 1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 150 "N18850055"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:NET_SHORT_1" (layer "F.Cu")
    (tedit 0)
    (at -37.698002 42.609991)
    (fp_text reference "NS15" (at -1.263244 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 0.500024 0.500024) (drill 0.250012) (layers *.Cu *.Mask)
      (net 15 "AGND"))
    (pad "2" smd circle (at 0.2 0) (size 0.127 0.127) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 128 "N22176186"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -48.698005 43.30999 -90)
    (fp_text reference "R1013" (at 2.54 -2.2225 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 185 "DVIB_TX0+"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 298 "N22316558"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at 0.201999 57.409987)
    (fp_text reference "C74" (at 1.5875 1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -36.698004 59.710008 90)
    (fp_text reference "C265" (at -1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "PCIE_PVDD"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:SMIND1005_0_5H_1" (layer "F.Cu")
    (tedit 0)
    (at -44.498014 50.110002 180)
    (fp_text reference "L36" (at -1.5875 -1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "VDD1DI"))
  )
  (footprint "lib:CAP1608_0_89H_1" (layer "F.Cu")
    (tedit 0)
    (at -6.297988 40.960007 -90)
    (fp_text reference "C287" (at 1.905025 -1.904975 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 270) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "MPVDD"))
    (pad "2" smd rect (at 0 0.7874 270) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "N22175956"))
  )
  (footprint "lib:GEOM0005_1" (layer "F.Cu")
    (tedit 0)
    (at 13.201998 68.309991 90)
    (fp_text reference "L40" (at -1.27 1.5875 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -2.8702 90) (size 3.429 1.6764) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "N22665126"))
    (pad "2" smd rect (at 0 2.8702 90) (size 3.429 1.6764) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -48.698005 42.309992 -90)
    (fp_text reference "R1012" (at 2.54 -2.2225 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 171 "DVIB_TX0-"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 298 "N22316558"))
  )
  (footprint "lib:DIO_SMA_1" (layer "F.Cu")
    (tedit 0)
    (at 6.802011 68.60999)
    (fp_text reference "D2" (at 1.27 0.635 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -2.129993 90) (size 1.27 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "N22665126"))
    (pad "2" smd rect (at 0 2.129993 90) (size 1.27 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:NET_SHORT_1" (layer "F.Cu")
    (tedit 0)
    (at -5.802993 57.374986 180)
    (fp_text reference "NS10" (at 1.263244 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0 180) (size 0.500024 0.500024) (drill 0.250012) (layers *.Cu *.Mask)
      (net 15 "AGND"))
    (pad "2" smd circle (at 0.2 0 180) (size 0.127 0.127) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "N16909667"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -51.298 7.509985 90)
    (fp_text reference "R126" (at -1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 345 "THERM_SDAT"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 346 "N21377265"))
  )
  (footprint "lib:BGA080_11X13-84_1" (layer "F.Cu")
    (tedit 0)
    (at 7.10201 32.809986 90)
    (fp_text reference "U22" (at -1.27 1.5875 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "A1" smd circle (at -3.199994 -5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "A2" smd circle (at -2.399995 -5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "A3" smd circle (at -1.599997 -5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "A7" smd circle (at 1.599997 -5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "A8" smd circle (at 2.399995 -5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 482 "QSA#6"))
    (pad "A9" smd circle (at 3.199994 -5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "B1" smd circle (at -3.199994 -4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 423 "MDA49"))
    (pad "B2" smd circle (at -2.399995 -4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "B3" smd circle (at -1.599997 -4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 449 "DQMA#6"))
    (pad "B7" smd circle (at 1.599997 -4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 481 "QSA6"))
    (pad "B8" smd circle (at 2.399995 -4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "B9" smd circle (at 3.199994 -4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 427 "MDA52"))
    (pad "C1" smd circle (at -3.199994 -3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "C2" smd circle (at -2.399995 -3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 425 "MDA50"))
    (pad "C3" smd circle (at -1.599997 -3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "C7" smd circle (at 1.599997 -3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "C8" smd circle (at 2.399995 -3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 430 "MDA55"))
    (pad "C9" smd circle (at 3.199994 -3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "D1" smd circle (at -3.199994 -3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 426 "MDA51"))
    (pad "D2" smd circle (at -2.399995 -3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "D3" smd circle (at -1.599997 -3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 422 "MDA48"))
    (pad "D7" smd circle (at 1.599997 -3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 429 "MDA54"))
    (pad "D8" smd circle (at 2.399995 -3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "D9" smd circle (at 3.199994 -3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 428 "MDA53"))
    (pad "E1" smd circle (at -3.199994 -2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "E2" smd circle (at -2.399995 -2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "E3" smd circle (at -1.599997 -2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "E7" smd circle (at 1.599997 -2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "E8" smd circle (at 2.399995 -2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 478 "QSA#4"))
    (pad "E9" smd circle (at 3.199994 -2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "F1" smd circle (at -3.199994 -1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 408 "MDA35"))
    (pad "F2" smd circle (at -2.399995 -1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "F3" smd circle (at -1.599997 -1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 447 "DQMA#4"))
    (pad "F7" smd circle (at 1.599997 -1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 477 "QSA4"))
    (pad "F8" smd circle (at 2.399995 -1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "F9" smd circle (at 3.199994 -1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 409 "MDA36"))
    (pad "G1" smd circle (at -3.199994 -0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "G2" smd circle (at -2.399995 -0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 407 "MDA34"))
    (pad "G3" smd circle (at -1.599997 -0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "G7" smd circle (at 1.599997 -0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "G8" smd circle (at 2.399995 -0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 410 "MDA37"))
    (pad "G9" smd circle (at 3.199994 -0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "H1" smd circle (at -3.199994 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 406 "MDA33"))
    (pad "H2" smd circle (at -2.399995 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "H3" smd circle (at -1.599997 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 405 "MDA32"))
    (pad "H7" smd circle (at 1.599997 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 412 "MDA39"))
    (pad "H8" smd circle (at 2.399995 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "H9" smd circle (at 3.199994 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 411 "MDA38"))
    (pad "J1" smd circle (at -3.199994 0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "N18859523"))
    (pad "J2" smd circle (at -2.399995 0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 151 "N18859640"))
    (pad "J3" smd circle (at -1.599997 0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "J7" smd circle (at 1.599997 0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "J8" smd circle (at 2.399995 0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 369 "CLKA1"))
    (pad "J9" smd circle (at 3.199994 0.799998 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "K2" smd circle (at -2.399995 1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 376 "CKEA1"))
    (pad "K3" smd circle (at -1.599997 1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 488 "WEA#1"))
    (pad "K7" smd circle (at 1.599997 1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 486 "RASA#1"))
    (pad "K8" smd circle (at 2.399995 1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 368 "CLKA1#"))
    (pad "K9" smd circle (at 3.199994 1.599997 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 468 "ODTA1"))
    (pad "L1" smd circle (at -3.199994 2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 466 "A_BA2"))
    (pad "L2" smd circle (at -2.399995 2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 464 "A_BA0"))
    (pad "L3" smd circle (at -1.599997 2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 465 "A_BA1"))
    (pad "L7" smd circle (at 1.599997 2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 374 "CASA#1"))
    (pad "L8" smd circle (at 2.399995 2.399995 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 378 "CSA1_0#"))
    (pad "M2" smd circle (at -2.399995 3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 453 "MAA10"))
    (pad "M3" smd circle (at -1.599997 3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 452 "MAA1"))
    (pad "M7" smd circle (at 1.599997 3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 455 "MAA2"))
    (pad "M8" smd circle (at 2.399995 3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 451 "MAA0"))
    (pad "M9" smd circle (at 3.199994 3.199994 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "N1" smd circle (at -3.199994 3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "N2" smd circle (at -2.399995 3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 456 "MAA3"))
    (pad "N3" smd circle (at -1.599997 3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 458 "MAA5"))
    (pad "N7" smd circle (at 1.599997 3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 459 "MAA6"))
    (pad "N8" smd circle (at 2.399995 3.999992 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 457 "MAA4"))
    (pad "P2" smd circle (at -2.399995 4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 460 "MAA7"))
    (pad "P3" smd circle (at -1.599997 4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 462 "MAA9"))
    (pad "P7" smd circle (at 1.599997 4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 454 "MAA11"))
    (pad "P8" smd circle (at 2.399995 4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 461 "MAA8"))
    (pad "P9" smd circle (at 3.199994 4.79999 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "R1" smd circle (at -3.199994 5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "R2" smd circle (at -2.399995 5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 463 "MAA12"))
    (pad "R3" smd circle (at -1.599997 5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "R7" smd circle (at 1.599997 5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "R8" smd circle (at 2.399995 5.599989 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
  )
  (footprint "lib:P-TDSON-8_1_2H_1" (layer "F.Cu")
    (tedit 0)
    (at 2.201995 68.409991 180)
    (fp_text reference "Q21" (at -1.5875 -1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -1.905 2.869997 180) (size 0.759993 1.599997) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "N22665126"))
    (pad "2" smd rect (at -0.635 2.869997 180) (size 0.759993 1.599997) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "N22665126"))
    (pad "3" smd rect (at 0.635 2.869997 180) (size 0.759993 1.599997) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "N22665126"))
    (pad "4" smd rect (at 1.905 2.869997 180) (size 0.759993 1.599997) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 301 "N22665692"))
    (pad "5" smd rect (at 1.905 -2.869997 180) (size 0.759993 1.599997) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 142 "G_PWR_SRC"))
    (pad "6" smd rect (at 0.635 -2.869997 180) (size 0.759993 1.599997) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 142 "G_PWR_SRC"))
    (pad "7" smd rect (at -0.635 -2.869997 180) (size 0.759993 1.599997) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 142 "G_PWR_SRC"))
    (pad "8" smd rect (at -1.905 -2.869997 180) (size 0.759993 1.599997) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 142 "G_PWR_SRC"))
    (pad "9" smd rect (at 0 0 180) (size 5.299989 2.799994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 142 "G_PWR_SRC"))
  )
  (footprint "lib:CAP1005_BGA_1" (layer "F.Cu")
    (tedit 0)
    (at -42.497992 44.509988 -90)
    (fp_text reference "C295" (at 1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 48 "DPA_VDDR"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 49 "N22175859"))
  )
  (footprint "lib:GEOM0001_1" (layer "F.Cu")
    (tedit 0)
    (at -5.532991 39.12501 -90)
    (fp_text reference "L27" (at 1.058608 -1.323232 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144 270) (size 1.27 1.219987) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "VDD_CORE"))
    (pad "2" smd rect (at 0 0.9144 270) (size 1.27 1.219987) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "MPVDD"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -28.997994 70.909986 180)
    (fp_text reference "R203" (at -1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 259 "N22275059"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -39.897997 58.410011 90)
    (fp_text reference "C402" (at -1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "N16909622"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -1.217988 41.129984)
    (fp_text reference "C102" (at 1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -40.497996 11.210003 90)
    (fp_text reference "C573" (at -1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 158 "N18876394"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:NET_SHORT_1" (layer "F.Cu")
    (tedit 0)
    (at -41.597994 51.309999 90)
    (fp_text reference "NS16" (at 0 -1.263244 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0 90) (size 0.500024 0.500024) (drill 0.250012) (layers *.Cu *.Mask)
      (net 15 "AGND"))
    (pad "2" smd circle (at 0.2 0 90) (size 0.127 0.127) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "N22175888"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -43.69799 55.109992)
    (fp_text reference "C291" (at 1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 46 "AVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 47 "N22175870"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -46.29801 45.710011 -90)
    (fp_text reference "C624" (at 1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 188 "DPB2N"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 189 "DVIB_TX1+"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -19.698012 25.71 90)
    (fp_text reference "C259" (at -1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "VDDRHB2"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "N16909550"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -43.69799 38.31 -90)
    (fp_text reference "C619" (at 1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 178 "DPA3P"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 179 "DVI_TX2-"))
  )
  (footprint "lib:DIO_SMA_1" (layer "F.Cu")
    (tedit 0)
    (at -4.497992 15.809994)
    (fp_text reference "D4" (at 1.27 0.635 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -2.129993 90) (size 1.27 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "N22672706"))
    (pad "2" smd rect (at 0 2.129993 90) (size 1.27 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -48.298006 68.409991 -90)
    (fp_text reference "R1029" (at 2.54 -2.2225 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "+5VRUN"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 309 "DDC4CLK"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -43.69799 32.309987 -90)
    (fp_text reference "C610" (at 1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 162 "DPA0P"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 163 "DVI_CLK-"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -51.797999 23.010005 -90)
    (fp_text reference "R133" (at 1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 313 "GPIO0"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "+3VRUN"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at 1.201997 57.409987 180)
    (fp_text reference "C580" (at -1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -52.097998 67.060006 90)
    (fp_text reference "R216" (at -1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 335 "DDC3CLK"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "+5VRUN"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -41.797994 30.80999 -90)
    (fp_text reference "R114" (at 1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 312 "VHAD0"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "+3VRUN"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -43.69799 34.310008 -90)
    (fp_text reference "C611" (at 1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 164 "DPA1P"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 165 "DVI_TX0-"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -42.697992 55.109992)
    (fp_text reference "C292" (at 1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 46 "AVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 47 "N22175870"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -51.797999 22.010007 -90)
    (fp_text reference "R134" (at 1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 314 "GPIO1"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "+3VRUN"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -30.097992 3.109994 90)
    (fp_text reference "C405" (at -1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 148 "+BBP"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1608_0_89H_1" (layer "F.Cu")
    (tedit 0)
    (at -18.997988 3.009994 -90)
    (fp_text reference "C119" (at 1.905025 -1.904975 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 270) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.7874 270) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1608_0_89H_1" (layer "F.Cu")
    (tedit 0)
    (at 15.701993 28.909993)
    (fp_text reference "C103" (at 1.904975 1.905025 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.7874) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at 2.852006 41.060007 180)
    (fp_text reference "C101" (at -1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at 7.802009 24.610002 180)
    (fp_text reference "R639" (at -1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 369 "CLKA1"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 160 "N18859575"))
  )
  (footprint "lib:GEOM0003_1" (layer "F.Cu")
    (tedit 0)
    (at -7.285591 2.024297)
    (fp_text reference "C438" (at 1.19093 1.190929 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144) (size 1.27 1.219987) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "VDD_CORE"))
    (pad "2" smd rect (at 0 0.9144) (size 1.27 1.219987) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_BGA_1" (layer "F.Cu")
    (tedit 0)
    (at -51.098 70.409987 180)
    (fp_text reference "R1034" (at -2.2225 -2.54 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 197 "N22538866"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 334 "DDC3DATA"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -51.298 4.509991 -90)
    (fp_text reference "R221" (at 1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 348 "N17821681"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 289 "MB_THERM#"))
  )
  (footprint "lib:TP055PRI_1" (layer "F.Cu")
    (tedit 0)
    (at -34.898007 59.010009)
    (fp_text reference "TP2" (at -0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd circle (at 0 0) (size 0.550012 0.550012) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 227 "PCIE_RXN0"))
  )
  (footprint "lib:P-TDSON-8_1_2H_1" (layer "F.Cu")
    (tedit 0)
    (at 3.901991 61.710004 -90)
    (fp_text reference "Q22" (at 1.27 -1.5875 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -1.905 2.869997 270) (size 0.759993 1.599997) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "2" smd rect (at -0.635 2.869997 270) (size 0.759993 1.599997) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "3" smd rect (at 0.635 2.869997 270) (size 0.759993 1.599997) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "4" smd rect (at 1.905 2.869997 270) (size 0.759993 1.599997) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 303 "N22665180"))
    (pad "5" smd rect (at 1.905 -2.869997 270) (size 0.759993 1.599997) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "N22665126"))
    (pad "6" smd rect (at 0.635 -2.869997 270) (size 0.759993 1.599997) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "N22665126"))
    (pad "7" smd rect (at -0.635 -2.869997 270) (size 0.759993 1.599997) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "N22665126"))
    (pad "8" smd rect (at -1.905 -2.869997 270) (size 0.759993 1.599997) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "N22665126"))
    (pad "9" smd rect (at 0 0 270) (size 5.299989 2.799994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "N22665126"))
  )
  (footprint "lib:SMIND1005_0_5H_1" (layer "F.Cu")
    (tedit 0)
    (at -32.298013 3.109994 90)
    (fp_text reference "L39" (at -1.27 1.5875 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "VDD_CORE"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 148 "+BBP"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -44.197989 28.609994 180)
    (fp_text reference "C48" (at -1.5875 -1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 120 "VDDR3"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at 9.202006 57.409987)
    (fp_text reference "C583" (at 1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -0.797999 57.409987 180)
    (fp_text reference "C579" (at -1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
  )
  (footprint "lib:NET_SHORT_1" (layer "F.Cu")
    (tedit 0)
    (at -13.497999 27.309997 180)
    (fp_text reference "NS11" (at 1.263244 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0 180) (size 0.500024 0.500024) (drill 0.250012) (layers *.Cu *.Mask)
      (net 15 "AGND"))
    (pad "2" smd circle (at 0.2 0 180) (size 0.127 0.127) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "N16910998"))
  )
  (footprint "lib:GEOM0002_1" (layer "F.Cu")
    (tedit 0)
    (at -2.097997 70.609986 180)
    (fp_text reference "C416" (at -1.19093 -1.190929 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144 180) (size 1.27 1.219987) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 142 "G_PWR_SRC"))
    (pad "2" smd rect (at 0 0.9144 180) (size 1.27 1.219987) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -46.09801 38.31 -90)
    (fp_text reference "R1008" (at 2.54 -2.2225 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 179 "DVI_TX2-"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 297 "N22316530"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at 1.601996 41.109994 180)
    (fp_text reference "C75" (at -1.5875 -1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -40.497996 12.210001 -90)
    (fp_text reference "R645" (at 1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 371 "CLKB1"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 158 "N18876394"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -51.797999 24.010003 -90)
    (fp_text reference "R226" (at 1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 353 "MEM_ID3"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "+3VRUN"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -48.698005 44.309988 -90)
    (fp_text reference "R1014" (at 2.54 -2.2225 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 187 "DVIB_TX1-"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 298 "N22316558"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -46.09801 39.309998 -90)
    (fp_text reference "R1009" (at 2.54 -2.2225 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 181 "DVI_TX2+"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 297 "N22316530"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -48.298006 66.709994 90)
    (fp_text reference "R1023" (at -2.54 2.2225 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 307 "DDC2CLK"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "+3VRUN"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -46.09801 36.310004 -90)
    (fp_text reference "R1006" (at 2.54 -2.2225 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 175 "DVI_TX1-"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 297 "N22316530"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at 12.302 57.409987)
    (fp_text reference "R40" (at 1.5875 1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 150 "N18850055"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -51.797999 19.009988 -90)
    (fp_text reference "R141" (at 1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 319 "GPIO11"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "+3VRUN"))
  )
  (footprint "lib:CAP1608_0_89H_1" (layer "F.Cu")
    (tedit 0)
    (at 5.452001 41.109994)
    (fp_text reference "C547" (at 1.904975 1.905025 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "N18859523"))
    (pad "2" smd rect (at 0 0.7874) (size 0.899998 0.959993) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at -43.097991 66.809994 -90)
    (fp_text reference "C427" (at 1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "+5VRUN"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -52.097998 66.209995 90)
    (fp_text reference "R215" (at -1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 334 "DDC3DATA"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "+5VRUN"))
  )
  (footprint "lib:NET_SHORT_1" (layer "F.Cu")
    (tedit 0)
    (at -32.698012 42.109992 45)
    (fp_text reference "NS13" (at -0.893248 -0.893248 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0 45) (size 0.500024 0.500024) (drill 0.250012) (layers *.Cu *.Mask)
      (net 15 "AGND"))
    (pad "2" smd circle (at 0.2 0 45) (size 0.127 0.127) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 125 "N22175699"))
  )
  (footprint "lib:CAP1005_1" (layer "F.Cu")
    (tedit 0)
    (at 13.901997 56.909988 -90)
    (fp_text reference "C76" (at 1.27 -1.5875 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V_REG"))
  )
  (footprint "lib:RES1005_1" (layer "F.Cu")
    (tedit 0)
    (at -40.497996 13.11 -90)
    (fp_text reference "R644" (at 1.905 -1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 370 "CLKB1#"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 158 "N18876394"))
  )
  (footprint "lib:SO_08_MICRO_8_1" (layer "F.Cu")
    (tedit 0)
    (at -46.598009 5.960001 90)
    (fp_text reference "U14" (at -1.27 1.586509 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd oval (at -0.976097 2.184908 90) (size 0.410007 1.444981) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "+3VRUN"))
    (pad "2" smd oval (at -0.325907 2.184908 90) (size 0.410007 1.444981) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 146 "D+"))
    (pad "3" smd oval (at 0.324104 2.184908 90) (size 0.410007 1.444981) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 147 "D-"))
    (pad "4" smd oval (at 0.97409 2.184908 90) (size 0.410007 1.444981) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 349 "N17821689"))
    (pad "5" smd oval (at 0.97409 -2.184908 90) (size 0.410007 1.444981) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "AGND"))
    (pad "6" smd oval (at 0.324104 -2.184908 90) (size 0.410007 1.444981) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 348 "N17821681"))
    (pad "7" smd oval (at -0.325907 -2.184908 90) (size 0.410007 1.444981) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 346 "N21377265"))
    (pad "8" smd oval (at -0.976097 -2.184908 90) (size 0.410007 1.444981) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 344 "N21377273"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 8.102008 62.010003 180)
    (fp_text reference "C1111" (at -2.2225 -2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 138 "N22665400"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -13.897999 25.41 -45)
    (fp_text reference "C252" (at 2.694077 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 315) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 30 "VDDRHB1"))
    (pad "2" smd rect (at 0 0.492608 315) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 31 "N16910998"))
  )
  (footprint "lib:CAP1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -44.698013 48.810004)
    (fp_text reference "C256" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 32 "LPVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 33 "N22176268"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -52.897997 56.00999)
    (fp_text reference "R217" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 275 "SMB_DAT"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 291 "PBAT_SMBDAT"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -20.69801 37.110002 180)
    (fp_text reference "C55" (at -1.5875 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 134 "N16910916"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 16.201992 58.81001 90)
    (fp_text reference "C1108" (at -2.54 2.2225 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 131 "N22665594"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1608_0_8H_1" (layer "B.Cu")
    (tedit 0)
    (at -23.698004 15.309995 -90)
    (fp_text reference "B49" (at 1.270025 -1.587475 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 270) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 11 "N18866342"))
    (pad "2" smd rect (at 0 0.7874 270) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 15.501993 2.409996)
    (fp_text reference "R1110" (at 2.2225 2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 132 "N22672648"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 17 "+5VRUN"))
  )
  (footprint "lib:SOT23_3PIN_1" (layer "B.Cu")
    (tedit 0)
    (at -50.398002 54.009994 -90)
    (fp_text reference "Q16" (at 1.227671 -1.534586 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9398 1.143 270) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "+3VRUN"))
    (pad "2" smd rect (at -0.9398 1.143 270) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 290 "PBAT_SMBCLK"))
    (pad "3" smd rect (at 0 -1.143 270) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 274 "SMB_CLK"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -46.898009 7.309986 -90)
    (fp_text reference "C1027" (at 2.54 -2.2225 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "+3VRUN"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -51.797999 25.010001 -90)
    (fp_text reference "R140" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 318 "GPIO9"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "+3VRUN"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -10.647992 68.50999 180)
    (fp_text reference "C370" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 77 "N22276389"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 78 "PCIE_TXN9"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -42.897991 45.109986)
    (fp_text reference "C262" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 36 "DPLL_PVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 37 "N22176582"))
  )
  (footprint "lib:SOT23_3PIN_1" (layer "B.Cu")
    (tedit 0)
    (at -50.498002 61.210005 -90)
    (fp_text reference "Q15" (at 1.227671 -1.534586 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9398 1.143 270) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "+3VRUN"))
    (pad "2" smd rect (at -0.9398 1.143 270) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 289 "MB_THERM#"))
    (pad "3" smd rect (at 0 -1.143 270) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 276 "THERM#"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -7.398012 56.20999)
    (fp_text reference "C249" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 28 "VDDRHA2"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 29 "N16909667"))
  )
  (footprint "lib:CAP3225_1_1H_1" (layer "B.Cu")
    (tedit 0)
    (at 7.30201 69.909988 180)
    (fp_text reference "C413" (at -1.658468 -1.65848 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -1.4478 180) (size 2.799994 1.399997) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 142 "G_PWR_SRC"))
    (pad "2" smd rect (at 0 1.4478 180) (size 2.799994 1.399997) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -4.497992 68.50999 180)
    (fp_text reference "C362" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "N22276551"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 62 "PCIE_TXN13"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -51.148013 34.359995 180)
    (fp_text reference "R25" (at -1.5875 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 287 "N16912894"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 17 "+5VRUN"))
  )
  (footprint "lib:SMIND1005_0_5H_1" (layer "B.Cu")
    (tedit 0)
    (at -43.897989 52.109998 90)
    (fp_text reference "L35" (at -1.27 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 117 "N22176231"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 6.001987 57.409987)
    (fp_text reference "R45" (at 1.5875 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 365 "CLKA0"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 159 "N18850123"))
  )
  (footprint "lib:SMIND1005_0_5H_1" (layer "B.Cu")
    (tedit 0)
    (at -49.698003 50.410001 180)
    (fp_text reference "L14" (at -1.5875 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 36 "DPLL_PVDD"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -15.297996 71.359997 180)
    (fp_text reference "C376" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 89 "N22276535"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 90 "PCIE_TXN6"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -49.298004 64.309999 180)
    (fp_text reference "R214" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 17 "+5VRUN"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 275 "SMB_DAT"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -6.748 11.010004 -90)
    (fp_text reference "C121" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
  )
  (footprint "lib:SOT23_3PIN_1" (layer "B.Cu")
    (tedit 0)
    (at 13.401998 67.509992 90)
    (fp_text reference "D5" (at -0.635 1.270025 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9398 1.143 90) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 17 "+5VRUN"))
    (pad "2" smd rect (at -0.9398 1.143 90) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "3" smd rect (at 0 -1.143 90) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 19 "N22665706"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -44.598013 29.109993 -90)
    (fp_text reference "R5" (at 0.635 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "+3VRUN"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 201 "I2C_CLK"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 13.201998 41.109994)
    (fp_text reference "R41" (at 1.5875 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 155 "N18850604"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -17.797991 68.50999 180)
    (fp_text reference "C379" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 95 "N22276446"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 96 "PCIE_TXP5"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 6.001987 4.109992 90)
    (fp_text reference "R1117" (at -2.54 2.2225 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "VDD_CORE"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 141 "N22672640"))
  )
  (footprint "lib:CAP1608_0_89H_1" (layer "B.Cu")
    (tedit 0)
    (at 15.960997 47.748005)
    (fp_text reference "C80" (at 1.587475 1.270025 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.7874) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -23.798004 69.109989 180)
    (fp_text reference "C386" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 109 "N22276543"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 110 "PCIE_TXN1"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 1.601996 41.109994)
    (fp_text reference "C83" (at 1.5875 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
  )
  (footprint "lib:RES1608_0_8H_1" (layer "B.Cu")
    (tedit 0)
    (at 4.101991 41.109994 180)
    (fp_text reference "B45" (at -1.587475 -1.270025 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 180) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "N18850036"))
    (pad "2" smd rect (at 0 0.7874 180) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
  )
  (footprint "lib:CAP1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -24.498003 41.109994 180)
    (fp_text reference "C26" (at -1.5875 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "VDD_CORE"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -50.398002 64.309999 180)
    (fp_text reference "R210" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 17 "+5VRUN"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 274 "SMB_CLK"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -51.398 64.309999 180)
    (fp_text reference "R201" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 17 "+5VRUN"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 276 "THERM#"))
  )
  (footprint "lib:SMIND1005_0_5H_1" (layer "B.Cu")
    (tedit 0)
    (at -15.297996 26.309999 180)
    (fp_text reference "L10" (at -1.5875 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 30 "VDDRHB1"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -41.997993 45.109986)
    (fp_text reference "C260" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 36 "DPLL_PVDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 37 "N22176582"))
  )
  (footprint "lib:CAP1608_0_89H_1" (layer "B.Cu")
    (tedit 0)
    (at -49.247991 46.310009 180)
    (fp_text reference "C294" (at -1.904975 -1.905025 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 180) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 48 "DPA_VDDR"))
    (pad "2" smd rect (at 0 0.7874 180) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 49 "N22175859"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 5.101989 57.409987 180)
    (fp_text reference "C578" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 159 "N18850123"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:BGA080_11X13-84_1" (layer "B.Cu")
    (tedit 0)
    (at 7.10201 32.809986 90)
    (fp_text reference "U23" (at -1.27 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "A1" smd circle (at 3.199994 -5.599989 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "A2" smd circle (at 2.399995 -5.599989 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "A3" smd circle (at 1.599997 -5.599989 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "A7" smd circle (at -1.599997 -5.599989 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "A8" smd circle (at -2.399995 -5.599989 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 480 "QSA#5"))
    (pad "A9" smd circle (at -3.199994 -5.599989 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "B1" smd circle (at 3.199994 -4.79999 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 421 "MDA47"))
    (pad "B2" smd circle (at 2.399995 -4.79999 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "B3" smd circle (at 1.599997 -4.79999 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 448 "DQMA#5"))
    (pad "B7" smd circle (at -1.599997 -4.79999 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 479 "QSA5"))
    (pad "B8" smd circle (at -2.399995 -4.79999 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "B9" smd circle (at -3.199994 -4.79999 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 416 "MDA42"))
    (pad "C1" smd circle (at 3.199994 -3.999992 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "C2" smd circle (at 2.399995 -3.999992 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 420 "MDA46"))
    (pad "C3" smd circle (at 1.599997 -3.999992 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "C7" smd circle (at -1.599997 -3.999992 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "C8" smd circle (at -2.399995 -3.999992 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 417 "MDA43"))
    (pad "C9" smd circle (at -3.199994 -3.999992 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "D1" smd circle (at 3.199994 -3.199994 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 418 "MDA44"))
    (pad "D2" smd circle (at 2.399995 -3.199994 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "D3" smd circle (at 1.599997 -3.199994 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 419 "MDA45"))
    (pad "D7" smd circle (at -1.599997 -3.199994 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 414 "MDA40"))
    (pad "D8" smd circle (at -2.399995 -3.199994 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "D9" smd circle (at -3.199994 -3.199994 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 415 "MDA41"))
    (pad "E1" smd circle (at 3.199994 -2.399995 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "E2" smd circle (at 2.399995 -2.399995 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "E3" smd circle (at 1.599997 -2.399995 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "E7" smd circle (at -1.599997 -2.399995 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "E8" smd circle (at -2.399995 -2.399995 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 484 "QSA#7"))
    (pad "E9" smd circle (at -3.199994 -2.399995 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "F1" smd circle (at 3.199994 -1.599997 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 438 "MDA62"))
    (pad "F2" smd circle (at 2.399995 -1.599997 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "F3" smd circle (at 1.599997 -1.599997 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 450 "DQMA#7"))
    (pad "F7" smd circle (at -1.599997 -1.599997 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 483 "QSA7"))
    (pad "F8" smd circle (at -2.399995 -1.599997 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "F9" smd circle (at -3.199994 -1.599997 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 434 "MDA59"))
    (pad "G1" smd circle (at 3.199994 -0.799998 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "G2" smd circle (at 2.399995 -0.799998 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 439 "MDA63"))
    (pad "G3" smd circle (at 1.599997 -0.799998 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "G7" smd circle (at -1.599997 -0.799998 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "G8" smd circle (at -2.399995 -0.799998 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 433 "MDA58"))
    (pad "G9" smd circle (at -3.199994 -0.799998 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "H1" smd circle (at 3.199994 0 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 436 "MDA60"))
    (pad "H2" smd circle (at 2.399995 0 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "H3" smd circle (at 1.599997 0 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 437 "MDA61"))
    (pad "H7" smd circle (at -1.599997 0 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 432 "MDA57"))
    (pad "H8" smd circle (at -2.399995 0 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "H9" smd circle (at -3.199994 0 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 431 "MDA56"))
    (pad "J1" smd circle (at 3.199994 0.799998 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "N18859284"))
    (pad "J2" smd circle (at 2.399995 0.799998 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 152 "N18859449"))
    (pad "J3" smd circle (at 1.599997 0.799998 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "J7" smd circle (at -1.599997 0.799998 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "J8" smd circle (at -2.399995 0.799998 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 369 "CLKA1"))
    (pad "J9" smd circle (at -3.199994 0.799998 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "K2" smd circle (at 2.399995 1.599997 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 376 "CKEA1"))
    (pad "K3" smd circle (at 1.599997 1.599997 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 488 "WEA#1"))
    (pad "K7" smd circle (at -1.599997 1.599997 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 486 "RASA#1"))
    (pad "K8" smd circle (at -2.399995 1.599997 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 368 "CLKA1#"))
    (pad "K9" smd circle (at -3.199994 1.599997 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 468 "ODTA1"))
    (pad "L1" smd circle (at 3.199994 2.399995 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 466 "A_BA2"))
    (pad "L2" smd circle (at 2.399995 2.399995 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 464 "A_BA0"))
    (pad "L3" smd circle (at 1.599997 2.399995 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 465 "A_BA1"))
    (pad "L7" smd circle (at -1.599997 2.399995 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 374 "CASA#1"))
    (pad "L8" smd circle (at -2.399995 2.399995 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 378 "CSA1_0#"))
    (pad "M2" smd circle (at 2.399995 3.199994 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 453 "MAA10"))
    (pad "M3" smd circle (at 1.599997 3.199994 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 452 "MAA1"))
    (pad "M7" smd circle (at -1.599997 3.199994 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 455 "MAA2"))
    (pad "M8" smd circle (at -2.399995 3.199994 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 451 "MAA0"))
    (pad "M9" smd circle (at -3.199994 3.199994 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "N1" smd circle (at 3.199994 3.999992 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "N2" smd circle (at 2.399995 3.999992 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 456 "MAA3"))
    (pad "N3" smd circle (at 1.599997 3.999992 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 458 "MAA5"))
    (pad "N7" smd circle (at -1.599997 3.999992 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 459 "MAA6"))
    (pad "N8" smd circle (at -2.399995 3.999992 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 457 "MAA4"))
    (pad "P2" smd circle (at 2.399995 4.79999 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 460 "MAA7"))
    (pad "P3" smd circle (at 1.599997 4.79999 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 462 "MAA9"))
    (pad "P7" smd circle (at -1.599997 4.79999 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 454 "MAA11"))
    (pad "P8" smd circle (at -2.399995 4.79999 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 461 "MAA8"))
    (pad "P9" smd circle (at -3.199994 4.79999 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "R1" smd circle (at 3.199994 5.599989 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "R2" smd circle (at 2.399995 5.599989 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 463 "MAA12"))
    (pad "R3" smd circle (at 1.599997 5.599989 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "R7" smd circle (at -1.599997 5.599989 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "R8" smd circle (at -2.399995 5.599989 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask"))
  )
  (footprint "lib:CAP1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -22.498007 45.109986 180)
    (fp_text reference "C38" (at -1.5875 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "VDD_CORE"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1608_0_89H_1" (layer "B.Cu")
    (tedit 0)
    (at -29.897992 43.30999 180)
    (fp_text reference "C42" (at -1.587475 -1.270025 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 180) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "VDD_CORE"))
    (pad "2" smd rect (at 0 0.7874 180) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -16.848005 68.50999 180)
    (fp_text reference "C378" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 93 "N22276498"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 94 "PCIE_TXN5"))
  )
  (footprint "lib:CAP1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -26.497999 43.10999 180)
    (fp_text reference "C21" (at -1.5875 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "VDD_CORE"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -7.247999 71.359997 180)
    (fp_text reference "C365" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 67 "N22276533"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 68 "PCIE_TXP12"))
  )
  (footprint "lib:CAP1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -26.497999 41.109994 180)
    (fp_text reference "C29" (at -1.5875 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "VDD_CORE"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -31.172996 44.984993 90)
    (fp_text reference "C283" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 44 "DPLL_VDDC"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -51.298 7.509985 90)
    (fp_text reference "R128" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 290 "PBAT_SMBCLK"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 344 "N21377273"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -24.298003 49.110004)
    (fp_text reference "C270" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 133 "PCIE_VDDC"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1608_0_89H_1" (layer "B.Cu")
    (tedit 0)
    (at -43.097991 34.710007)
    (fp_text reference "C297" (at 1.904975 1.905025 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 50 "DPA_PVDD"))
    (pad "2" smd rect (at 0 0.7874) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 51 "N22175966"))
  )
  (footprint "lib:CAP1608_0_89H_1" (layer "B.Cu")
    (tedit 0)
    (at -23.698004 14.009998 -90)
    (fp_text reference "C87" (at 1.270025 -1.587475 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 270) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 11 "N18866342"))
    (pad "2" smd rect (at 0 0.7874 270) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -49.398004 30.40999)
    (fp_text reference "R224" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 351 "MEM_ID1"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "+3VRUN"))
  )
  (footprint "lib:RES1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -34.498008 54.109994)
    (fp_text reference "R11" (at 1.5875 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 337 "N22176754"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1608_0_8H_1" (layer "B.Cu")
    (tedit 0)
    (at 4.901989 24.210003 180)
    (fp_text reference "B47" (at -1.587475 -1.270025 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 180) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "N18859284"))
    (pad "2" smd rect (at 0 0.7874 180) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -34.998007 70.309987)
    (fp_text reference "R211" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "+3VRUN"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 281 "DDC1CLK"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -3.297994 71.359997 180)
    (fp_text reference "C360" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 57 "N22276563"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 58 "PCIE_TXN14"))
  )
  (footprint "lib:CAP1608_0_89H_1" (layer "B.Cu")
    (tedit 0)
    (at -48.498006 41.160007 180)
    (fp_text reference "C615" (at -1.904975 -1.905025 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 180) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 124 "DPB_PVDD"))
    (pad "2" smd rect (at 0 0.7874 180) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 125 "N22175699"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -46.698009 16.309993 -90)
    (fp_text reference "C1025" (at 2.54 -2.2225 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "+3VRUN"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:SMIND1005_0_5H_1" (layer "B.Cu")
    (tedit 0)
    (at -48.998005 43.20999 90)
    (fp_text reference "L43" (at -1.27 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 127 "DPB_VDDR"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 133 "PCIE_VDDC"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -46.898009 6.309988 90)
    (fp_text reference "C326" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "+3VRUN"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -7.598011 68.50999 180)
    (fp_text reference "C366" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 69 "N22276527"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 70 "PCIE_TXN11"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -45.998011 17.409991 90)
    (fp_text reference "R158" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "+3VRUN"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 347 "N21360761"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 11.002002 1.409998 180)
    (fp_text reference "R1111" (at -2.2225 -2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 24 "VREF"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 25 "N22672632"))
  )
  (footprint "lib:CAP1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -28.497995 43.10999 180)
    (fp_text reference "C24" (at -1.5875 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "VDD_CORE"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -51.697999 69.560001 180)
    (fp_text reference "C391" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "+3VRUN"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -28.097996 33.759996 180)
    (fp_text reference "R36" (at -1.5875 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 359 "N16919341"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -18.366011 43.127008)
    (fp_text reference "C6" (at 1.27 0.635 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 10.002004 67.309993 -90)
    (fp_text reference "C1100" (at 2.54 -2.2225 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 17 "+5VRUN"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -8.09801 38.909999 180)
    (fp_text reference "R38" (at -1.5875 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 129 "N16919368"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 9.602005 4.309992 180)
    (fp_text reference "C1121" (at -2.2225 -2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 143 "N22672644"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 141 "N22672640"))
  )
  (footprint "lib:CAP1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -19.377998 36.600986 180)
    (fp_text reference "C9" (at -1.27 -0.635 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:GEOM0002_1" (layer "B.Cu")
    (tedit 0)
    (at 9.902005 70.409987 180)
    (fp_text reference "C352" (at -1.19093 -1.190929 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144 180) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 142 "G_PWR_SRC"))
    (pad "2" smd rect (at 0 0.9144 180) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -16.993014 38.41099)
    (fp_text reference "R29" (at 1.5875 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 123 "N16919381"))
  )
  (footprint "lib:CAP1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -23.498005 43.10999)
    (fp_text reference "C31" (at 1.5875 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "VDD_CORE"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -19.518003 55.849995 90)
    (fp_text reference "R28" (at -1.27 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 122 "N16919383"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -27.897996 49.110004)
    (fp_text reference "C277" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 133 "PCIE_VDDC"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -6.748 11.910002 90)
    (fp_text reference "C79" (at -1.27 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 161 "N18867037"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -40.197997 10.810004 90)
    (fp_text reference "C153" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
  )
  (footprint "lib:CAP1608_0_89H_1" (layer "B.Cu")
    (tedit 0)
    (at -46.247997 47.810006)
    (fp_text reference "C635" (at 1.904975 1.905025 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 39 "VDD2DI"))
    (pad "2" smd rect (at 0 0.7874) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 40 "N22176225"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -23.698004 16.560005 90)
    (fp_text reference "C154" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
  )
  (footprint "lib:RES1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -33.298011 43.809989 90)
    (fp_text reference "R21" (at -1.27 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 361 "N22176800"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -35.047994 40.160009 -90)
    (fp_text reference "R206" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 277 "TV_COMP_B_PB"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 14.401996 58.309985)
    (fp_text reference "C1105" (at 2.2225 2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 21 "N22665484"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -48.398006 68.70999 90)
    (fp_text reference "R1027" (at -2.54 2.2225 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 310 "DDC4DATA"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 268 "N22274456"))
  )
  (footprint "lib:CAP1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -30.297991 38.709999 90)
    (fp_text reference "C35" (at -1.27 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 120 "VDDR3"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 9.002006 59.910008)
    (fp_text reference "C1107" (at 2.2225 2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 139 "N22665482"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -13.497999 26.209999 -45)
    (fp_text reference "C253" (at 2.694077 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 315) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 30 "VDDRHB1"))
    (pad "2" smd rect (at 0 0.492608 315) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 31 "N16910998"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 12.801999 1.409998 180)
    (fp_text reference "C1118" (at -2.2225 -2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 25 "N22672632"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -1.197999 41.109994 180)
    (fp_text reference "C85" (at -1.5875 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 6.702011 41.109994 180)
    (fp_text reference "C587" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "N18850036"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1608_0_89H_1" (layer "B.Cu")
    (tedit 0)
    (at -27.34801 47.159995 90)
    (fp_text reference "C23" (at -1.270025 1.587475 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 90) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "VDD_CORE"))
    (pad "2" smd rect (at 0 0.7874 90) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:GEOM0002_1" (layer "B.Cu")
    (tedit 0)
    (at 8.702007 20.71001 -60)
    (fp_text reference "C433" (at 1.62684 -0.435911 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144 300) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 142 "G_PWR_SRC"))
    (pad "2" smd rect (at 0 0.9144 300) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -51.997999 40.060009 -90)
    (fp_text reference "C60" (at 1.27 -1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 121 "N16912873"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:SOT23_3PIN_1" (layer "B.Cu")
    (tedit 0)
    (at 6.802011 9.610007 90)
    (fp_text reference "D6" (at -0.635 1.270025 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9398 1.143 90) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 17 "+5VRUN"))
    (pad "2" smd rect (at -0.9398 1.143 90) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "3" smd rect (at 0 -1.143 90) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 23 "N22673014"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 7.602009 3.809993 180)
    (fp_text reference "C1124" (at -2.2225 -2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 143 "N22672644"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 12.251987 41.109994 180)
    (fp_text reference "R43" (at -1.5875 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 155 "N18850604"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:SOT23_3PIN_1_1H_1" (layer "B.Cu")
    (tedit 0)
    (at -37.098003 2.309996)
    (fp_text reference "Q20" (at 1.534586 1.227671 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9398 1.143) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 292 "BB_ENA"))
    (pad "2" smd rect (at -0.9398 1.143) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "3" smd rect (at 0 -1.143) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 288 "N16909921"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -24.74799 69.109989 180)
    (fp_text reference "C387" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 111 "N22276537"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 112 "PCIE_TXP1"))
  )
  (footprint "lib:SMIND1005_0_5H_1" (layer "B.Cu")
    (tedit 0)
    (at -44.197989 37.510002)
    (fp_text reference "L32" (at 1.5875 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 50 "DPA_PVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
  )
  (footprint "lib:SMIND1005_0_5H_1" (layer "B.Cu")
    (tedit 0)
    (at -6.498013 56.20999 180)
    (fp_text reference "L9" (at -1.27 -0.635 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 28 "VDDRHA2"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 10.102004 24.610002 180)
    (fp_text reference "C552" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 152 "N18859449"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -26.697998 49.110004)
    (fp_text reference "C276" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 133 "PCIE_VDDC"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 2.852006 41.109994)
    (fp_text reference "C107" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
  )
  (footprint "lib:CAP1608_0_89H_1" (layer "B.Cu")
    (tedit 0)
    (at -45.798011 34.110008)
    (fp_text reference "C632" (at 1.904975 1.905025 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 120 "VDDR3"))
    (pad "2" smd rect (at 0 0.7874) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -42.397992 52.509997)
    (fp_text reference "C394" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 117 "N22176231"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 5.501988 62.510002 -90)
    (fp_text reference "R1104" (at 2.54 -2.2225 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 137 "N22665412"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
  )
  (footprint "lib:CAP1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -23.498005 45.109986)
    (fp_text reference "C39" (at 1.5875 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "VDD_CORE"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1608_2012_1" (layer "B.Cu")
    (tedit 0)
    (at -45.947998 37.510002)
    (fp_text reference "R654" (at 1.19093 1.190929 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "+3VRUN"))
    (pad "2" smd rect (at 0 0.9144) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 120 "VDDR3"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 15.901993 60.510006 180)
    (fp_text reference "C1104" (at -2.2225 -2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 135 "N22665740"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -27.497997 45.109986)
    (fp_text reference "C44" (at 1.5875 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "VDD_CORE"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 5.501988 61.510004 90)
    (fp_text reference "R1106" (at -2.54 2.2225 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 138 "N22665400"))
  )
  (footprint "lib:CAP1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -23.398005 26.909997 90)
    (fp_text reference "C15" (at -1.27 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -18.764994 58.262995)
    (fp_text reference "R30" (at 1.5875 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 126 "N16919174"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 14.001996 8.310009 -90)
    (fp_text reference "C1123" (at 2.54 -2.2225 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 17 "+5VRUN"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:NET_SHORT_1" (layer "B.Cu")
    (tedit 0)
    (at -36.87301 41.009995 90)
    (fp_text reference "NS5" (at 0 -0.945744 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0 90) (size 0.500024 0.500024) (drill 0.250012) (layers *.Cu *.Mask)
      (net 15 "AGND"))
    (pad "2" smd circle (at -0.2 0 90) (size 0.127 0.127) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 119 "N22175861"))
  )
  (footprint "lib:RES1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -8.498009 37.410002 90)
    (fp_text reference "R34" (at -1.27 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 129 "N16919368"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 11.702001 58.309985)
    (fp_text reference "R1102" (at 2.2225 2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 20 "VREF_22665604"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 21 "N22665484"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -41.797994 3.109994 90)
    (fp_text reference "R1042" (at -2.54 2.2225 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 341 "RUNPWROK"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 354 "RUNPWROK_1"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 16.801991 60.510006 180)
    (fp_text reference "R1100" (at -2.2225 -2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 356 "VIN_22665782"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 142 "G_PWR_SRC"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -9.298008 71.359997 180)
    (fp_text reference "C368" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 73 "N22276444"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 74 "PCIE_TXN10"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 3.601992 24.610002 180)
    (fp_text reference "C105" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 9.202006 62.110003 180)
    (fp_text reference "C1106" (at -2.2225 -2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 137 "N22665412"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 138 "N22665400"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -51.797999 26.009999 -90)
    (fp_text reference "R152" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 330 "VID_6"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "+3VRUN"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 8.602007 6.709987)
    (fp_text reference "C1116" (at 2.2225 2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 22 "N22672706"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 23 "N22673014"))
  )
  (footprint "lib:RES1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -25.448014 34.759994 180)
    (fp_text reference "R35" (at -1.5875 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 358 "N16919725"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -8.498009 68.50999 180)
    (fp_text reference "C367" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 71 "N22276496"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 72 "PCIE_TXP11"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -50.398002 30.40999)
    (fp_text reference "R154" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 332 "DVALID"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "+3VRUN"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -48.247993 70.909986 90)
    (fp_text reference "R1069" (at -2.54 2.2225 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 309 "DDC4CLK"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 272 "N22774274"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -6.748 15.309995 90)
    (fp_text reference "C128" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1608_0_89H_1" (layer "B.Cu")
    (tedit 0)
    (at -40.697996 13.209999 -90)
    (fp_text reference "C572" (at 1.905025 -1.904975 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 270) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 13 "N18875830"))
    (pad "2" smd rect (at 0 0.7874 270) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 13.701997 1.409998 180)
    (fp_text reference "R1115" (at -2.2225 -2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 25 "N22672632"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1608_0_89H_1" (layer "B.Cu")
    (tedit 0)
    (at -22.098008 39.009999 90)
    (fp_text reference "C28" (at -1.270025 1.587475 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 90) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "VDD_CORE"))
    (pad "2" smd rect (at 0 0.7874 90) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -26.997998 2.709995)
    (fp_text reference "C152" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
  )
  (footprint "lib:QFN065-16_4X4_1" (layer "B.Cu")
    (tedit 0)
    (at 12.701999 62.210003)
    (fp_text reference "U26" (at -0.9525 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd oval (at 1.999996 -0.975004 270) (size 0.379984 0.810006) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 135 "N22665740"))
    (pad "2" smd oval (at 1.999996 -0.324993 270) (size 0.379984 0.810006) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 356 "VIN_22665782"))
    (pad "3" smd oval (at 1.999996 0.324993 270) (size 0.379984 0.810006) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 354 "RUNPWROK_1"))
    (pad "4" smd oval (at 1.999996 0.975004 270) (size 0.379984 0.810006) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "5" smd oval (at 0.975004 1.999996 180) (size 0.379984 0.810006) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 17 "+5VRUN"))
    (pad "6" smd oval (at 0.324993 1.999996 180) (size 0.379984 0.810006) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "7" smd oval (at -0.324993 1.999996 180) (size 0.379984 0.810006) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 303 "N22665180"))
    (pad "8" smd oval (at -0.975004 1.999996 180) (size 0.379984 0.810006) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 19 "N22665706"))
    (pad "9" smd oval (at -1.999996 0.975004 90) (size 0.379984 0.810006) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 301 "N22665692"))
    (pad "10" smd oval (at -1.999996 0.324993 90) (size 0.379984 0.810006) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 18 "N22665126"))
    (pad "11" smd oval (at -1.999996 -0.324993 90) (size 0.379984 0.810006) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 137 "N22665412"))
    (pad "12" smd oval (at -1.999996 -0.975004 90) (size 0.379984 0.810006) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 138 "N22665400"))
    (pad "13" smd oval (at -0.975004 -1.999996) (size 0.379984 0.810006) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 139 "N22665482"))
    (pad "14" smd oval (at -0.324993 -1.999996) (size 0.379984 0.810006) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 20 "VREF_22665604"))
    (pad "15" smd oval (at 0.324993 -1.999996) (size 0.379984 0.810006) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 21 "N22665484"))
    (pad "16" smd oval (at 0.975004 -1.999996) (size 0.379984 0.810006) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 131 "N22665594"))
    (pad "17" thru_hole circle (at 0 0) (size 0.550012 0.550012) (drill 0.250012) (layers *.Cu *.Mask)
      (net 15 "AGND"))
    (pad "18" thru_hole circle (at 0 -0.750011 270) (size 0.550012 0.550012) (drill 0.250012) (layers *.Cu *.Mask)
      (net 15 "AGND"))
    (pad "19" thru_hole circle (at -0.750011 0 270) (size 0.550012 0.550012) (drill 0.250012) (layers *.Cu *.Mask)
      (net 15 "AGND"))
    (pad "20" thru_hole circle (at 0 0.750011 270) (size 0.550012 0.550012) (drill 0.250012) (layers *.Cu *.Mask)
      (net 15 "AGND"))
    (pad "21" thru_hole circle (at 0.750011 0 270) (size 0.550012 0.550012) (drill 0.250012) (layers *.Cu *.Mask)
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -33.59801 48.010006 180)
    (fp_text reference "C240" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "LVDDR"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 12.251987 24.610002 180)
    (fp_text reference "R641" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 152 "N18859449"))
  )
  (footprint "lib:CAP1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -30.99799 43.20999 180)
    (fp_text reference "C282" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 44 "DPLL_VDDC"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -10.247993 71.359997 180)
    (fp_text reference "C369" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 75 "N22276440"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 76 "PCIE_TXP10"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 12.601999 58.309985)
    (fp_text reference "C1103" (at 2.2225 2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 20 "VREF_22665604"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:BGA080_11X13-84_1" (layer "B.Cu")
    (tedit 0)
    (at 7.10201 49.410003 90)
    (fp_text reference "U5" (at -0.635 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "A1" smd circle (at 3.199994 -5.599989 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "A2" smd circle (at 2.399995 -5.599989 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "A3" smd circle (at 1.599997 -5.599989 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "A7" smd circle (at -1.599997 -5.599989 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "A8" smd circle (at -2.399995 -5.599989 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 474 "QSA#2"))
    (pad "A9" smd circle (at -3.199994 -5.599989 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "B1" smd circle (at 3.199994 -4.79999 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 395 "MDA23"))
    (pad "B2" smd circle (at 2.399995 -4.79999 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "B3" smd circle (at 1.599997 -4.79999 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 445 "DQMA#2"))
    (pad "B7" smd circle (at -1.599997 -4.79999 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 473 "QSA2"))
    (pad "B8" smd circle (at -2.399995 -4.79999 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "B9" smd circle (at -3.199994 -4.79999 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 389 "MDA18"))
    (pad "C1" smd circle (at 3.199994 -3.999992 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "C2" smd circle (at 2.399995 -3.999992 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 393 "MDA21"))
    (pad "C3" smd circle (at 1.599997 -3.999992 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "C7" smd circle (at -1.599997 -3.999992 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "C8" smd circle (at -2.399995 -3.999992 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 390 "MDA19"))
    (pad "C9" smd circle (at -3.199994 -3.999992 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "D1" smd circle (at 3.199994 -3.199994 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 394 "MDA22"))
    (pad "D2" smd circle (at 2.399995 -3.199994 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "D3" smd circle (at 1.599997 -3.199994 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 392 "MDA20"))
    (pad "D7" smd circle (at -1.599997 -3.199994 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 387 "MDA16"))
    (pad "D8" smd circle (at -2.399995 -3.199994 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "D9" smd circle (at -3.199994 -3.199994 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 388 "MDA17"))
    (pad "E1" smd circle (at 3.199994 -2.399995 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "E2" smd circle (at 2.399995 -2.399995 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "E3" smd circle (at 1.599997 -2.399995 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "E7" smd circle (at -1.599997 -2.399995 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "E8" smd circle (at -2.399995 -2.399995 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 472 "QSA#1"))
    (pad "E9" smd circle (at -3.199994 -2.399995 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "F1" smd circle (at 3.199994 -1.599997 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 384 "MDA13"))
    (pad "F2" smd circle (at 2.399995 -1.599997 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "F3" smd circle (at 1.599997 -1.599997 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 444 "DQMA#1"))
    (pad "F7" smd circle (at -1.599997 -1.599997 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 471 "QSA1"))
    (pad "F8" smd circle (at -2.399995 -1.599997 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "F9" smd circle (at -3.199994 -1.599997 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 381 "MDA10"))
    (pad "G1" smd circle (at 3.199994 -0.799998 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "G2" smd circle (at 2.399995 -0.799998 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 386 "MDA15"))
    (pad "G3" smd circle (at 1.599997 -0.799998 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "G7" smd circle (at -1.599997 -0.799998 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "G8" smd circle (at -2.399995 -0.799998 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 382 "MDA11"))
    (pad "G9" smd circle (at -3.199994 -0.799998 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "H1" smd circle (at 3.199994 0 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 385 "MDA14"))
    (pad "H2" smd circle (at 2.399995 0 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "H3" smd circle (at 1.599997 0 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 383 "MDA12"))
    (pad "H7" smd circle (at -1.599997 0 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 442 "MDA9"))
    (pad "H8" smd circle (at -2.399995 0 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "H9" smd circle (at -3.199994 0 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 441 "MDA8"))
    (pad "J1" smd circle (at 3.199994 0.799998 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "N18850036"))
    (pad "J2" smd circle (at 2.399995 0.799998 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 155 "N18850604"))
    (pad "J3" smd circle (at 1.599997 0.799998 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "J7" smd circle (at -1.599997 0.799998 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "J8" smd circle (at -2.399995 0.799998 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 365 "CLKA0"))
    (pad "J9" smd circle (at -3.199994 0.799998 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "K2" smd circle (at 2.399995 1.599997 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 375 "CKEA0"))
    (pad "K3" smd circle (at 1.599997 1.599997 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 487 "WEA#0"))
    (pad "K7" smd circle (at -1.599997 1.599997 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 485 "RASA#0"))
    (pad "K8" smd circle (at -2.399995 1.599997 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 364 "CLKA0#"))
    (pad "K9" smd circle (at -3.199994 1.599997 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 467 "ODTA0"))
    (pad "L1" smd circle (at 3.199994 2.399995 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 466 "A_BA2"))
    (pad "L2" smd circle (at 2.399995 2.399995 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 464 "A_BA0"))
    (pad "L3" smd circle (at 1.599997 2.399995 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 465 "A_BA1"))
    (pad "L7" smd circle (at -1.599997 2.399995 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 373 "CASA#0"))
    (pad "L8" smd circle (at -2.399995 2.399995 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 377 "CSA0_0#"))
    (pad "M2" smd circle (at 2.399995 3.199994 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 453 "MAA10"))
    (pad "M3" smd circle (at 1.599997 3.199994 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 452 "MAA1"))
    (pad "M7" smd circle (at -1.599997 3.199994 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 455 "MAA2"))
    (pad "M8" smd circle (at -2.399995 3.199994 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 451 "MAA0"))
    (pad "M9" smd circle (at -3.199994 3.199994 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "N1" smd circle (at 3.199994 3.999992 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "N2" smd circle (at 2.399995 3.999992 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 456 "MAA3"))
    (pad "N3" smd circle (at 1.599997 3.999992 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 458 "MAA5"))
    (pad "N7" smd circle (at -1.599997 3.999992 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 459 "MAA6"))
    (pad "N8" smd circle (at -2.399995 3.999992 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 457 "MAA4"))
    (pad "P2" smd circle (at 2.399995 4.79999 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 460 "MAA7"))
    (pad "P3" smd circle (at 1.599997 4.79999 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 462 "MAA9"))
    (pad "P7" smd circle (at -1.599997 4.79999 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 454 "MAA11"))
    (pad "P8" smd circle (at -2.399995 4.79999 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 461 "MAA8"))
    (pad "P9" smd circle (at -3.199994 4.79999 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "R1" smd circle (at 3.199994 5.599989 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "R2" smd circle (at 2.399995 5.599989 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 463 "MAA12"))
    (pad "R3" smd circle (at 1.599997 5.599989 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "R7" smd circle (at -1.599997 5.599989 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "R8" smd circle (at -2.399995 5.599989 90) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -40.797996 16.309993 90)
    (fp_text reference "C155" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
  )
  (footprint "lib:CAP1608_0_89H_1" (layer "B.Cu")
    (tedit 0)
    (at 15.901993 51.409999 180)
    (fp_text reference "C582" (at -1.904975 -1.905025 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 180) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.7874 180) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:SOT23_3PIN_1" (layer "B.Cu")
    (tedit 0)
    (at -50.398002 57.609987 90)
    (fp_text reference "Q17" (at -1.227671 1.534586 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9398 1.143 90) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "+3VRUN"))
    (pad "2" smd rect (at -0.9398 1.143 90) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 291 "PBAT_SMBDAT"))
    (pad "3" smd rect (at 0 -1.143 90) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 275 "SMB_DAT"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 7.602009 6.709987)
    (fp_text reference "C1115" (at 2.2225 2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 22 "N22672706"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 23 "N22673014"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -27.34801 69.709988 180)
    (fp_text reference "C389" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 115 "N22276525"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 116 "PCIE_TXP0"))
  )
  (footprint "lib:CAP1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -24.498003 43.10999 180)
    (fp_text reference "C19" (at -1.5875 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "VDD_CORE"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -39.297999 4.709991 180)
    (fp_text reference "C151" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -6.748 6.609987 -90)
    (fp_text reference "C129" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
  )
  (footprint "lib:CAP1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -41.997993 41.309994 180)
    (fp_text reference "C397" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 118 "N22176381"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 119 "N22175861"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -1.197999 69.309989 180)
    (fp_text reference "C357" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 53 "N22276438"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 54 "PCIE_TXN15"))
  )
  (footprint "lib:CAP1608_0_89H_1" (layer "B.Cu")
    (tedit 0)
    (at -45.998011 40.809995 180)
    (fp_text reference "C399" (at -1.904975 -1.905025 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 180) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 44 "DPLL_VDDC"))
    (pad "2" smd rect (at 0 0.7874 180) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:SMIND1005_0_5H_1" (layer "B.Cu")
    (tedit 0)
    (at -46.798009 45.209986)
    (fp_text reference "L42" (at 1.5875 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 124 "DPB_PVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
  )
  (footprint "lib:CAP1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -42.897991 43.20999 180)
    (fp_text reference "C273" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 43 "A2VDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -43.79799 5.609989 180)
    (fp_text reference "C359" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "+3VRUN"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -41.997993 43.20999 180)
    (fp_text reference "C274" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 43 "A2VDD"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:SOT23_3PIN_1" (layer "B.Cu")
    (tedit 0)
    (at -33.39801 2.309996 180)
    (fp_text reference "Q18" (at -1.534586 -1.227671 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9398 1.143 180) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 288 "N16909921"))
    (pad "2" smd rect (at -0.9398 1.143 180) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "VDD_CORE"))
    (pad "3" smd rect (at 0 -1.143 180) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 148 "+BBP"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -51.398 30.40999)
    (fp_text reference "R146" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 324 "VID_0"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "+3VRUN"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 16.101992 7.610011)
    (fp_text reference "R1109" (at 2.2225 2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 357 "VIN"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 142 "G_PWR_SRC"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -10.698005 2.509995)
    (fp_text reference "R723" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 296 "POW_SW1"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "+3VRUN"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -49.798003 40.809995 180)
    (fp_text reference "C628" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 124 "DPB_PVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 125 "N22175699"))
  )
  (footprint "lib:CAP1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -18.348002 41.409994 90)
    (fp_text reference "C10" (at -1.27 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -18.848001 39.960009 90)
    (fp_text reference "C8" (at -0.635 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -14.64801 68.50999 180)
    (fp_text reference "C375" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 87 "N22276541"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 88 "PCIE_TXP7"))
  )
  (footprint "lib:CAP1608_0_89H_1" (layer "B.Cu")
    (tedit 0)
    (at -6.798013 8.810008 180)
    (fp_text reference "C126" (at -1.904975 -1.905025 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 180) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.7874 180) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -8.998008 38.909999 180)
    (fp_text reference "C64" (at -1.5875 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 129 "N16919368"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:GEOM0003_1" (layer "B.Cu")
    (tedit 0)
    (at 16.401992 67.309993)
    (fp_text reference "C419" (at 1.19093 1.190929 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.9144) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP3225_1_1H_1" (layer "B.Cu")
    (tedit 0)
    (at 3.801991 69.909988 180)
    (fp_text reference "C414" (at -1.658468 -1.65848 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -1.4478 180) (size 2.799994 1.399997) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 142 "G_PWR_SRC"))
    (pad "2" smd rect (at 0 1.4478 180) (size 2.799994 1.399997) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:SOT23_3PIN_1_1H_1" (layer "B.Cu")
    (tedit 0)
    (at 2.501994 5.660002 90)
    (fp_text reference "Q28" (at -1.227671 1.534586 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9398 1.143 90) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 296 "POW_SW1"))
    (pad "2" smd rect (at -0.9398 1.143 90) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "3" smd rect (at 0 -1.143 90) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 295 "N22672726"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -51.797999 27.009997 -90)
    (fp_text reference "R150" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 328 "VID_4"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "+3VRUN"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -16.248007 71.359997 180)
    (fp_text reference "C377" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 91 "N22276529"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 92 "PCIE_TXP6"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -32.098013 35.410006 90)
    (fp_text reference "R4" (at -0.635 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 336 "BLON_PWM"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -41.997993 39.309998)
    (fp_text reference "R20" (at 1.5875 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 14 "N22176053"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 6.902011 57.409987)
    (fp_text reference "R44" (at 1.5875 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 364 "CLKA0#"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 159 "N18850123"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -8.29801 56.20999)
    (fp_text reference "C250" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 28 "VDDRHA2"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 29 "N16909667"))
  )
  (footprint "lib:CAP1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -20.820997 47.850011)
    (fp_text reference "C57" (at 1.5875 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 134 "N16910916"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1608_0_89H_1" (layer "B.Cu")
    (tedit 0)
    (at -50.998001 46.359997)
    (fp_text reference "C630" (at 1.904975 1.905025 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 127 "DPB_VDDR"))
    (pad "2" smd rect (at 0 0.7874) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 128 "N22176186"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -20.99801 55.209992 180)
    (fp_text reference "C61" (at -1.5875 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 122 "N16919383"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -12.298002 71.359997 180)
    (fp_text reference "C372" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 81 "N22276559"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 82 "PCIE_TXN8"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -8.09801 48.810004)
    (fp_text reference "C243" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 26 "VDDRHA1"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 27 "N16910486"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -51.797999 17.009992 -90)
    (fp_text reference "R143" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 321 "GPIO13"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "+3VRUN"))
  )
  (footprint "lib:CAP1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -22.498007 43.10999 180)
    (fp_text reference "C32" (at -1.5875 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "VDD_CORE"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -22.647994 71.359997 180)
    (fp_text reference "C385" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 107 "N22276549"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 108 "PCIE_TXP2"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -51.298 4.509991 -90)
    (fp_text reference "R220" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 349 "N17821689"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 289 "MB_THERM#"))
  )
  (footprint "lib:CAP1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -18.848001 39.109998 90)
    (fp_text reference "C7" (at -0.635 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -51.248013 67.509992 -90)
    (fp_text reference "R1067" (at 2.54 -2.2225 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 307 "DDC2CLK"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 263 "N22778501"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -51.797999 20.009986 -90)
    (fp_text reference "R1031" (at 2.54 -2.2225 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 338 "DVI_HPD2"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 270 "N22276217"))
  )
  (footprint "lib:SOT23_5PIN_1" (layer "B.Cu")
    (tedit 0)
    (at -45.198012 9.310007 90)
    (fp_text reference "U29" (at -1.227671 1.534586 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9398 1.143 90) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 606 "N22625842"))
    (pad "2" smd rect (at 0 1.143 90) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 299 "CTFB"))
    (pad "3" smd rect (at -0.9398 1.143 90) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "4" smd rect (at -0.9398 -1.143 90) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 605 "N22625885"))
    (pad "5" smd rect (at 0.9398 -1.143 90) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "+3VRUN"))
  )
  (footprint "lib:CAP1608_0_89H_1" (layer "B.Cu")
    (tedit 0)
    (at -20.89801 45.035006)
    (fp_text reference "C54" (at 1.587475 1.270025 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 134 "N16910916"))
    (pad "2" smd rect (at 0 0.7874) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1608_0_89H_1" (layer "B.Cu")
    (tedit 0)
    (at -44.498014 50.610001 -90)
    (fp_text reference "C239" (at 1.905025 -1.904975 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 270) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "LVDDR"))
    (pad "2" smd rect (at 0 0.7874 270) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:SMIND1005_0_5H_1" (layer "B.Cu")
    (tedit 0)
    (at -43.49799 58.109986 90)
    (fp_text reference "L28" (at -1.27 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 46 "AVDD"))
  )
  (footprint "lib:CAP1608_0_89H_1" (layer "B.Cu")
    (tedit 0)
    (at -50.948013 71.059998 90)
    (fp_text reference "C390" (at -1.905025 1.904975 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 90) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "+3VRUN"))
    (pad "2" smd rect (at 0 0.7874 90) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -23.698004 12.81 -90)
    (fp_text reference "C86" (at 1.27 -1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 11 "N18866342"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:SMIND1005_0_5H_1" (layer "B.Cu")
    (tedit 0)
    (at -42.497992 37.910001 90)
    (fp_text reference "L34" (at -1.27 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 52 "N16909654"))
  )
  (footprint "lib:CAP1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -34.098009 45.609985)
    (fp_text reference "C266" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 39 "VDD2DI"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 40 "N22176225"))
  )
  (footprint "lib:SOT23_3PIN_1_1H_1" (layer "B.Cu")
    (tedit 0)
    (at -51.498 37.610001)
    (fp_text reference "Q2" (at 1.270025 0.635 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9398 1.143) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 121 "N16912873"))
    (pad "2" smd rect (at -0.9398 1.143) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "3" smd rect (at 0 -1.143) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 287 "N16912894"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -19.971012 57.741)
    (fp_text reference "R33" (at 1.5875 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 126 "N16919174"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -51.797999 23.010005 -90)
    (fp_text reference "R225" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 352 "MEM_ID2"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "+3VRUN"))
  )
  (footprint "lib:SMIND1005_0_5H_1" (layer "B.Cu")
    (tedit 0)
    (at -48.698005 50.410001)
    (fp_text reference "L11" (at 1.5875 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 32 "LPVDD"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -51.797999 24.010003 -90)
    (fp_text reference "R145" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 323 "GPIO22"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "+3VRUN"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 10.702003 58.309985)
    (fp_text reference "R1105" (at 2.2225 2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 20 "VREF_22665604"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 139 "N22665482"))
  )
  (footprint "lib:GEOM0008_1" (layer "B.Cu")
    (tedit 0)
    (at 1.901995 18.309989 30)
    (fp_text reference "Q26" (at 0.738571 1.895758 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 1.905025 3.174975 30) (size 0.759993 1.599997) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "2" smd rect (at 0.635 3.174975 30) (size 0.759993 1.599997) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "3" smd rect (at -0.634975 3.175 30) (size 0.759993 1.599997) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "4" smd rect (at -1.905 3.174975 30) (size 0.759993 1.599997) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 304 "N22672861"))
    (pad "5" smd rect (at -1.905025 -3.169996 30) (size 0.759993 1.599997) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 22 "N22672706"))
    (pad "6" smd rect (at -0.634975 -3.169996 30) (size 0.759993 1.599997) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 22 "N22672706"))
    (pad "7" smd rect (at 0.634975 -3.170022 30) (size 0.759993 1.599997) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 22 "N22672706"))
    (pad "8" smd rect (at 1.905025 -3.169996 30) (size 0.759993 1.599997) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 22 "N22672706"))
    (pad "9" smd rect (at 0 0 30) (size 5.550002 3.474999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 22 "N22672706"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -46.998009 14.709996)
    (fp_text reference "C1026" (at 2.2225 2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 130 "N22625904"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 10.102004 8.910008)
    (fp_text reference "C1114" (at 2.2225 2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 17 "+5VRUN"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -19.248001 71.359997 180)
    (fp_text reference "C381" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 99 "N22276391"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 100 "PCIE_TXP4"))
  )
  (footprint "lib:CAP1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -15.997994 55.80999 -90)
    (fp_text reference "C14" (at 1.27 -1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:GEOM0008_1" (layer "B.Cu")
    (tedit 0)
    (at 6.902011 15.360008 -150)
    (fp_text reference "Q24" (at -0.738571 -1.895758 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 1.905025 3.174975 210) (size 0.759993 1.599997) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 22 "N22672706"))
    (pad "2" smd rect (at 0.635 3.174975 210) (size 0.759993 1.599997) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 22 "N22672706"))
    (pad "3" smd rect (at -0.634975 3.175 210) (size 0.759993 1.599997) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 22 "N22672706"))
    (pad "4" smd rect (at -1.905 3.174975 210) (size 0.759993 1.599997) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 302 "N22672940"))
    (pad "5" smd rect (at -1.905025 -3.169996 210) (size 0.759993 1.599997) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 142 "G_PWR_SRC"))
    (pad "6" smd rect (at -0.634975 -3.169996 210) (size 0.759993 1.599997) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 142 "G_PWR_SRC"))
    (pad "7" smd rect (at 0.634975 -3.170022 210) (size 0.759993 1.599997) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 142 "G_PWR_SRC"))
    (pad "8" smd rect (at 1.905025 -3.169996 210) (size 0.759993 1.599997) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 142 "G_PWR_SRC"))
    (pad "9" smd rect (at 0 0 210) (size 5.550002 3.474999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 142 "G_PWR_SRC"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -11.547991 68.50999 180)
    (fp_text reference "C371" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 79 "N22276565"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 80 "PCIE_TXP9"))
  )
  (footprint "lib:SOT23_5PIN_1" (layer "B.Cu")
    (tedit 0)
    (at -44.498014 13.309999 180)
    (fp_text reference "U28" (at -1.534586 -1.227671 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9398 1.143 180) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 130 "N22625904"))
    (pad "2" smd rect (at 0 1.143 180) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 605 "N22625885"))
    (pad "3" smd rect (at -0.9398 1.143 180) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "4" smd rect (at -0.9398 -1.143 180) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 606 "N22625842"))
    (pad "5" smd rect (at 0.9398 -1.143 180) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "+3VRUN"))
  )
  (footprint "lib:CAP1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -24.398003 36.110004 180)
    (fp_text reference "C301" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 52 "N16909654"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1608_0_89H_1" (layer "B.Cu")
    (tedit 0)
    (at -4.797991 55.209992 180)
    (fp_text reference "C3" (at -1.269975 -0.635025 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 180) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.7874 180) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1608_0_89H_1" (layer "B.Cu")
    (tedit 0)
    (at -37.898001 67.109993 180)
    (fp_text reference "C425" (at -1.904975 -1.905025 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 180) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 133 "PCIE_VDDC"))
    (pad "2" smd rect (at 0 0.7874 180) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1608_0_8H_1" (layer "B.Cu")
    (tedit 0)
    (at -40.697996 14.609997 90)
    (fp_text reference "B51" (at -1.270025 1.587475 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 90) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 13 "N18875830"))
    (pad "2" smd rect (at 0 0.7874 90) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 15.701993 54.109994 180)
    (fp_text reference "C585" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 6.502011 1.409998)
    (fp_text reference "R1116" (at 2.2225 2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 140 "N22672636"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 293 "N22672692"))
  )
  (footprint "lib:RES1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -32.747999 50.459988)
    (fp_text reference "R2" (at 1.27 0.635 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 360 "N2080875268"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -25.498001 49.110004)
    (fp_text reference "C275" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 133 "PCIE_VDDC"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -28.497995 45.109986 180)
    (fp_text reference "C45" (at -1.5875 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "VDD_CORE"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1608_0_89H_1" (layer "B.Cu")
    (tedit 0)
    (at -49.298004 48.559992 90)
    (fp_text reference "C261" (at -1.905025 1.904975 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 90) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 36 "DPLL_PVDD"))
    (pad "2" smd rect (at 0 0.7874 90) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 37 "N22176582"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 8.302008 1.409998)
    (fp_text reference "R1119" (at 2.2225 2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 140 "N22672636"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1608_0_89H_1" (layer "B.Cu")
    (tedit 0)
    (at -29.897992 40.509996)
    (fp_text reference "C37" (at 1.587475 1.270025 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "VDD_CORE"))
    (pad "2" smd rect (at 0 0.7874) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 1.201997 70.609986 -90)
    (fp_text reference "C355" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 17 "+5VRUN"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -13.248013 71.359997 180)
    (fp_text reference "C373" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 83 "N22276553"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 84 "PCIE_TXP8"))
  )
  (footprint "lib:RES1608_0_8H_1" (layer "B.Cu")
    (tedit 0)
    (at -20.89801 41.809993 180)
    (fp_text reference "L1" (at -1.269975 -0.635025 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 180) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 134 "N16910916"))
    (pad "2" smd rect (at 0 0.7874 180) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "VDD_CORE"))
  )
  (footprint "lib:CAP1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -19.418003 47.437998 90)
    (fp_text reference "C12" (at -1.27 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -6.748 16.609993 -90)
    (fp_text reference "C132" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
  )
  (footprint "lib:CAP1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -33.198011 42.709991 90)
    (fp_text reference "C627" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 124 "DPB_PVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 125 "N22175699"))
  )
  (footprint "lib:CAP1608_0_89H_1" (layer "B.Cu")
    (tedit 0)
    (at -29.497993 25.010001 -90)
    (fp_text reference "C4" (at 0.635025 -1.269975 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 270) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.7874 270) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -21.909006 49.123009)
    (fp_text reference "C56" (at 1.5875 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 134 "N16910916"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -31.898013 66.309995 180)
    (fp_text reference "C453" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 149 "N22665296"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 133 "PCIE_VDDC"))
  )
  (footprint "lib:CAP1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -22.998006 41.609993 -90)
    (fp_text reference "C25" (at 1.27 -1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "VDD_CORE"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -41.797994 2.009996 90)
    (fp_text reference "R1043" (at -2.54 2.2225 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 354 "RUNPWROK_1"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 14.301996 65.309997 -90)
    (fp_text reference "C1109" (at 2.54 -2.2225 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 17 "+5VRUN"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -42.897991 39.309998 180)
    (fp_text reference "R18" (at -1.5875 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 14 "N22176053"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -52.897997 59.610008 180)
    (fp_text reference "R202" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 276 "THERM#"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 289 "MB_THERM#"))
  )
  (footprint "lib:CAP1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -30.297991 37.910001 90)
    (fp_text reference "C34" (at -1.27 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 120 "VDDR3"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -51.797999 28.860006 -90)
    (fp_text reference "R147" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 325 "VID_1"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "+3VRUN"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 8.602007 3.809993 180)
    (fp_text reference "C1125" (at -2.2225 -2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 141 "N22672640"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 2.601994 24.610002)
    (fp_text reference "C106" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
  )
  (footprint "lib:CAP1608_0_89H_1" (layer "B.Cu")
    (tedit 0)
    (at -31.197989 48.010006 -45)
    (fp_text reference "C271" (at 2.694077 0.000035 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 315) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 133 "PCIE_VDDC"))
    (pad "2" smd rect (at 0 0.7874 315) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 8.702007 24.610002)
    (fp_text reference "C108" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -13.697999 68.50999 180)
    (fp_text reference "C374" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 85 "N22276547"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 86 "PCIE_TXN7"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -18.29799 71.359997 180)
    (fp_text reference "C380" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 97 "N22276442"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 98 "PCIE_TXN4"))
  )
  (footprint "lib:CAP1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -21.947995 36.359991)
    (fp_text reference "C13" (at 1.5875 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -48.398006 69.509988 90)
    (fp_text reference "R1028" (at -2.54 2.2225 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 309 "DDC4CLK"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 269 "N22275399"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -16.191009 38.407003 180)
    (fp_text reference "R31" (at -1.5875 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 123 "N16919381"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 13.501997 58.309985)
    (fp_text reference "R1107" (at 2.2225 2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 21 "N22665484"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -42.897991 41.309994 180)
    (fp_text reference "C398" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 118 "N22176381"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 119 "N22175861"))
  )
  (footprint "lib:CAP1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -27.497997 43.10999)
    (fp_text reference "C22" (at 1.5875 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "VDD_CORE"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -20.347998 68.50999 180)
    (fp_text reference "C382" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 101 "N22276385"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 102 "PCIE_TXN3"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -39.548011 7.159999)
    (fp_text reference "R647" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 154 "N18876029"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -51.298 6.509987 90)
    (fp_text reference "R125" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 343 "THERM_SCLK"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 344 "N21377273"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 9.202006 1.409998)
    (fp_text reference "C1119" (at 2.2225 2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 140 "N22672636"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -30.89799 50.659988 90)
    (fp_text reference "R1" (at -0.635 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 305 "N2080875267"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 133 "PCIE_VDDC"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -21.698008 71.359997 180)
    (fp_text reference "C384" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 105 "N22276555"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 106 "PCIE_TXN2"))
  )
  (footprint "lib:CAP1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -25.498001 41.109994)
    (fp_text reference "C27" (at 1.5875 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "VDD_CORE"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1608_0_89H_1" (layer "B.Cu")
    (tedit 0)
    (at -36.198005 67.109993 180)
    (fp_text reference "C1112" (at -2.222475 -2.540025 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 180) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 133 "PCIE_VDDC"))
    (pad "2" smd rect (at 0 0.7874 180) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -50.598001 69.560001 180)
    (fp_text reference "C392" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "+3VRUN"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1608_0_89H_1" (layer "B.Cu")
    (tedit 0)
    (at 6.301986 24.210003 180)
    (fp_text reference "C549" (at -1.904975 -1.905025 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 180) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "N18859284"))
    (pad "2" smd rect (at 0 0.7874 180) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 0.352011 41.109994)
    (fp_text reference "C584" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
  )
  (footprint "lib:SOT23_1_15H_1" (layer "B.Cu")
    (tedit 0)
    (at -29.597993 2.309996 180)
    (fp_text reference "Q19" (at -1.534586 -1.227671 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 1.016 1.143 180) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 288 "N16909921"))
    (pad "2" smd rect (at -1.016 1.143 180) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "3" smd rect (at 0 -1.143 180) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 148 "+BBP"))
  )
  (footprint "lib:CAP1608_0_89H_1" (layer "B.Cu")
    (tedit 0)
    (at -25.498001 2.309996 180)
    (fp_text reference "C149" (at -1.904975 -1.905025 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 180) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.7874 180) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -35.047994 42.660004 -90)
    (fp_text reference "R204" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 278 "TV_CR_PR"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -41.797994 4.109992 90)
    (fp_text reference "R1041" (at -2.54 2.2225 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 341 "RUNPWROK"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 340 "N22625856"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 1.201997 71.61001 -90)
    (fp_text reference "C356" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 17 "+5VRUN"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:GEOM0002_1" (layer "B.Cu")
    (tedit 0)
    (at 11.902001 70.409987 180)
    (fp_text reference "C354" (at -1.19093 -1.190929 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144 180) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 142 "G_PWR_SRC"))
    (pad "2" smd rect (at 0 0.9144 180) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 9.902005 59.910008)
    (fp_text reference "R1108" (at 2.2225 2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 139 "N22665482"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -38.698 70.309987)
    (fp_text reference "R157" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 284 "HSYNC"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "+3VRUN"))
  )
  (footprint "lib:RES1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -51.248013 66.609994 -90)
    (fp_text reference "R1068" (at 2.54 -2.2225 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 308 "DDC2DATA"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 264 "N22778505"))
  )
  (footprint "lib:SOT23_1_15H_1" (layer "B.Cu")
    (tedit 0)
    (at -48.398006 37.610001 180)
    (fp_text reference "Q1" (at -1.270025 -0.635 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 1.016 1.143 180) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 287 "N16912894"))
    (pad "2" smd rect (at -1.016 1.143 180) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "+3VRUN"))
    (pad "3" smd rect (at 0 -1.143 180) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 120 "VDDR3"))
  )
  (footprint "lib:CAP1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -25.498001 45.109986)
    (fp_text reference "C41" (at 1.5875 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "VDD_CORE"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -11.698003 2.509995)
    (fp_text reference "R722" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 294 "POW_SW0"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "+3VRUN"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 7.40201 1.409998)
    (fp_text reference "R1118" (at 2.2225 2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 140 "N22672636"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 295 "N22672726"))
  )
  (footprint "lib:NET_SHORT_1" (layer "B.Cu")
    (tedit 0)
    (at -44.798013 55.609991 180)
    (fp_text reference "NS3" (at 0.945744 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0 180) (size 0.500024 0.500024) (drill 0.250012) (layers *.Cu *.Mask)
      (net 15 "AGND"))
    (pad "2" smd circle (at -0.2 0 180) (size 0.127 0.127) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 47 "N22175870"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 10.702003 65.409997 90)
    (fp_text reference "C1102" (at -2.54 2.2225 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 18 "N22665126"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 19 "N22665706"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -23.798004 6.309988 90)
    (fp_text reference "R49" (at -1.27 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 157 "N18866513"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -47.398008 30.40999)
    (fp_text reference "R155" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 333 "PSYNC"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "+3VRUN"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -6.748 12.91 90)
    (fp_text reference "R52" (at -1.27 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 366 "CLKB0#"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 161 "N18867037"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 9.202006 8.910008)
    (fp_text reference "C1113" (at 2.2225 2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 17 "+5VRUN"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -18.997988 46.21001 90)
    (fp_text reference "C11" (at -1.27 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:SOT23_3PIN_1_1H_1" (layer "B.Cu")
    (tedit 0)
    (at 2.501994 2.109996 90)
    (fp_text reference "Q27" (at -1.227671 1.534586 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9398 1.143 90) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 294 "POW_SW0"))
    (pad "2" smd rect (at -0.9398 1.143 90) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "3" smd rect (at 0 -1.143 90) (size 0.640004 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 293 "N22672692"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 15.701993 57.309987 180)
    (fp_text reference "R1101" (at -2.2225 -2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 131 "N22665594"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 17 "+5VRUN"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -51.997999 41.009995 90)
    (fp_text reference "R26" (at -1.27 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 341 "RUNPWROK"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 121 "N16912873"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -40.197997 11.910002 -90)
    (fp_text reference "C571" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 13 "N18875830"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -21.298009 68.50999 180)
    (fp_text reference "C383" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 103 "N22276561"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 104 "PCIE_TXP3"))
  )
  (footprint "lib:CAP1608_0_89H_1" (layer "B.Cu")
    (tedit 0)
    (at -47.598007 51.11)
    (fp_text reference "C255" (at 1.904975 1.905025 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 32 "LPVDD"))
    (pad "2" smd rect (at 0 0.7874) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 33 "N22176268"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 8.351995 41.109994 180)
    (fp_text reference "C84" (at -1.5875 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
  )
  (footprint "lib:CAP1608_0_89H_1" (layer "B.Cu")
    (tedit 0)
    (at -19.498013 3.009994 90)
    (fp_text reference "C127" (at -1.905025 1.904975 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 90) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.7874 90) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -44.698013 2.409996 180)
    (fp_text reference "R1040" (at -2.2225 -2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 340 "N22625856"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "+3VRUN"))
  )
  (footprint "lib:RES1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -52.74801 70.209987 180)
    (fp_text reference "R1120" (at -2.2225 -2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 198 "N22794094"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 339 "DVI_HPD3"))
  )
  (footprint "lib:GEOM0001_1" (layer "B.Cu")
    (tedit 0)
    (at -46.39801 54.209994 180)
    (fp_text reference "B10" (at -1.323232 -1.058608 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.9144 180) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.9144 180) (size 1.27 1.219987) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "LVDDR"))
  )
  (footprint "lib:CAP1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -26.497999 45.109986 180)
    (fp_text reference "C43" (at -1.5875 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "VDD_CORE"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -51.797999 28.009995 -90)
    (fp_text reference "R148" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 326 "VID_2"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "+3VRUN"))
  )
  (footprint "lib:QFN065-16_4X4_1" (layer "B.Cu")
    (tedit 0)
    (at 12.701999 5.10999)
    (fp_text reference "U27" (at -0.9525 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd oval (at 1.999996 -0.975004 270) (size 0.379984 0.810006) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 136 "N22673140"))
    (pad "2" smd oval (at 1.999996 -0.324993 270) (size 0.379984 0.810006) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 357 "VIN"))
    (pad "3" smd oval (at 1.999996 0.324993 270) (size 0.379984 0.810006) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 354 "RUNPWROK_1"))
    (pad "4" smd oval (at 1.999996 0.975004 270) (size 0.379984 0.810006) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "5" smd oval (at 0.975004 1.999996 180) (size 0.379984 0.810006) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 17 "+5VRUN"))
    (pad "6" smd oval (at 0.324993 1.999996 180) (size 0.379984 0.810006) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "7" smd oval (at -0.324993 1.999996 180) (size 0.379984 0.810006) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 304 "N22672861"))
    (pad "8" smd oval (at -0.975004 1.999996 180) (size 0.379984 0.810006) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 23 "N22673014"))
    (pad "9" smd oval (at -1.999996 0.975004 90) (size 0.379984 0.810006) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 302 "N22672940"))
    (pad "10" smd oval (at -1.999996 0.324993 90) (size 0.379984 0.810006) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 22 "N22672706"))
    (pad "11" smd oval (at -1.999996 -0.324993 90) (size 0.379984 0.810006) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 143 "N22672644"))
    (pad "12" smd oval (at -1.999996 -0.975004 90) (size 0.379984 0.810006) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 141 "N22672640"))
    (pad "13" smd oval (at -0.975004 -1.999996) (size 0.379984 0.810006) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 140 "N22672636"))
    (pad "14" smd oval (at -0.324993 -1.999996) (size 0.379984 0.810006) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 24 "VREF"))
    (pad "15" smd oval (at 0.324993 -1.999996) (size 0.379984 0.810006) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 25 "N22672632"))
    (pad "16" smd oval (at 0.975004 -1.999996) (size 0.379984 0.810006) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 132 "N22672648"))
    (pad "17" thru_hole circle (at 0 0) (size 0.550012 0.550012) (drill 0.250012) (layers *.Cu *.Mask)
      (net 15 "AGND"))
    (pad "18" thru_hole circle (at 0 -0.750011 270) (size 0.550012 0.550012) (drill 0.250012) (layers *.Cu *.Mask)
      (net 15 "AGND"))
    (pad "19" thru_hole circle (at -0.750011 0 270) (size 0.550012 0.550012) (drill 0.250012) (layers *.Cu *.Mask)
      (net 15 "AGND"))
    (pad "20" thru_hole circle (at 0 0.750011 270) (size 0.550012 0.550012) (drill 0.250012) (layers *.Cu *.Mask)
      (net 15 "AGND"))
    (pad "21" thru_hole circle (at 0.750011 0 270) (size 0.550012 0.550012) (drill 0.250012) (layers *.Cu *.Mask)
      (net 15 "AGND"))
  )
  (footprint "lib:SMIND1005_0_5H_1" (layer "B.Cu")
    (tedit 0)
    (at -48.798005 44.409988 90)
    (fp_text reference "L30" (at -1.27 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 48 "DPA_VDDR"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 133 "PCIE_VDDC"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -23.698004 19.06 90)
    (fp_text reference "C133" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -2.148009 69.309989 180)
    (fp_text reference "C358" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 55 "N22276387"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 56 "PCIE_TXP15"))
  )
  (footprint "lib:CAP1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -41.997993 35.010007)
    (fp_text reference "C298" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 50 "DPA_PVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 51 "N22175966"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 13.701997 24.610002)
    (fp_text reference "C109" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
  )
  (footprint "lib:CAP1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -27.497997 41.109994)
    (fp_text reference "C30" (at 1.5875 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "VDD_CORE"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -23.698004 17.80999 90)
    (fp_text reference "C130" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -51.797999 22.010007 -90)
    (fp_text reference "R136" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 316 "GPIO3"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "+3VRUN"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 1.601996 24.610002)
    (fp_text reference "C110" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 16.501991 4.009992 180)
    (fp_text reference "C1120" (at -2.2225 -2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 136 "N22673140"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -51.298 3.509993 90)
    (fp_text reference "R222" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "+3VRUN"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 349 "N17821689"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -23.698004 10.910004 -90)
    (fp_text reference "C131" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
  )
  (footprint "lib:SMIND1005_0_5H_1" (layer "B.Cu")
    (tedit 0)
    (at -7.098012 48.910004 180)
    (fp_text reference "L6" (at -1.27 -0.635 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 26 "VDDRHA1"))
  )
  (footprint "lib:CAP1608_0_89H_1" (layer "B.Cu")
    (tedit 0)
    (at 5.452001 41.109994 180)
    (fp_text reference "C588" (at -1.904975 -1.905025 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 180) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "N18850036"))
    (pad "2" smd rect (at 0 0.7874 180) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1608_0_89H_1" (layer "B.Cu")
    (tedit 0)
    (at -29.123013 35.534999 -90)
    (fp_text reference "C299" (at 1.905025 -1.904975 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 270) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 52 "N16909654"))
    (pad "2" smd rect (at 0 0.7874 270) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -30.89799 66.309995)
    (fp_text reference "R701" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 133 "PCIE_VDDC"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 149 "N22665296"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -48.198006 46.11001 180)
    (fp_text reference "C293" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 48 "DPA_VDDR"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 49 "N22175859"))
  )
  (footprint "lib:CAP1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -16.897993 26.909997 90)
    (fp_text reference "C16" (at -1.27 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:BGA080_11X13-84_1" (layer "B.Cu")
    (tedit 0)
    (at -15.397996 12.310001 180)
    (fp_text reference "U7" (at -1.27 -0.635 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "A1" smd circle (at 3.199994 -5.599989 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "A2" smd circle (at 2.399995 -5.599989 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "A3" smd circle (at 1.599997 -5.599989 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "A7" smd circle (at -1.599997 -5.599989 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "A8" smd circle (at -2.399995 -5.599989 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 590 "QSB#2"))
    (pad "A9" smd circle (at -3.199994 -5.599989 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "B1" smd circle (at 3.199994 -4.79999 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 510 "MDB22"))
    (pad "B2" smd circle (at 2.399995 -4.79999 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "B3" smd circle (at 1.599997 -4.79999 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 561 "DQMB#2"))
    (pad "B7" smd circle (at -1.599997 -4.79999 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 589 "QSB2"))
    (pad "B8" smd circle (at -2.399995 -4.79999 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "B9" smd circle (at -3.199994 -4.79999 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 504 "MDB17"))
    (pad "C1" smd circle (at 3.199994 -3.999992 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "C2" smd circle (at 2.399995 -3.999992 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 511 "MDB23"))
    (pad "C3" smd circle (at 1.599997 -3.999992 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "C7" smd circle (at -1.599997 -3.999992 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "C8" smd circle (at -2.399995 -3.999992 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 503 "MDB16"))
    (pad "C9" smd circle (at -3.199994 -3.999992 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "D1" smd circle (at 3.199994 -3.199994 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 508 "MDB20"))
    (pad "D2" smd circle (at 2.399995 -3.199994 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "D3" smd circle (at 1.599997 -3.199994 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 509 "MDB21"))
    (pad "D7" smd circle (at -1.599997 -3.199994 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 505 "MDB18"))
    (pad "D8" smd circle (at -2.399995 -3.199994 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "D9" smd circle (at -3.199994 -3.199994 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 506 "MDB19"))
    (pad "E1" smd circle (at 3.199994 -2.399995 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "E2" smd circle (at 2.399995 -2.399995 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "E3" smd circle (at 1.599997 -2.399995 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "E7" smd circle (at -1.599997 -2.399995 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "E8" smd circle (at -2.399995 -2.399995 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 592 "QSB#3"))
    (pad "E9" smd circle (at -3.199994 -2.399995 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "F1" smd circle (at 3.199994 -1.599997 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 515 "MDB27"))
    (pad "F2" smd circle (at 2.399995 -1.599997 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "F3" smd circle (at 1.599997 -1.599997 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 562 "DQMB#3"))
    (pad "F7" smd circle (at -1.599997 -1.599997 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 591 "QSB3"))
    (pad "F8" smd circle (at -2.399995 -1.599997 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "F9" smd circle (at -3.199994 -1.599997 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 520 "MDB31"))
    (pad "G1" smd circle (at 3.199994 -0.799998 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "G2" smd circle (at 2.399995 -0.799998 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 514 "MDB26"))
    (pad "G3" smd circle (at 1.599997 -0.799998 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "G7" smd circle (at -1.599997 -0.799998 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "G8" smd circle (at -2.399995 -0.799998 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 519 "MDB30"))
    (pad "G9" smd circle (at -3.199994 -0.799998 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "H1" smd circle (at 3.199994 0 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 512 "MDB24"))
    (pad "H2" smd circle (at 2.399995 0 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "H3" smd circle (at 1.599997 0 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 513 "MDB25"))
    (pad "H7" smd circle (at -1.599997 0 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 516 "MDB28"))
    (pad "H8" smd circle (at -2.399995 0 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "H9" smd circle (at -3.199994 0 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 517 "MDB29"))
    (pad "J1" smd circle (at 3.199994 0.799998 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 11 "N18866342"))
    (pad "J2" smd circle (at 2.399995 0.799998 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 157 "N18866513"))
    (pad "J3" smd circle (at 1.599997 0.799998 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "J7" smd circle (at -1.599997 0.799998 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "J8" smd circle (at -2.399995 0.799998 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 367 "CLKB0"))
    (pad "J9" smd circle (at -3.199994 0.799998 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "K2" smd circle (at 2.399995 1.599997 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 491 "CKEB0"))
    (pad "K3" smd circle (at 1.599997 1.599997 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 603 "WEB#0"))
    (pad "K7" smd circle (at -1.599997 1.599997 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 601 "RASB#0"))
    (pad "K8" smd circle (at -2.399995 1.599997 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 366 "CLKB0#"))
    (pad "K9" smd circle (at -3.199994 1.599997 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 583 "ODTB0"))
    (pad "L1" smd circle (at 3.199994 2.399995 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 582 "B_BA2"))
    (pad "L2" smd circle (at 2.399995 2.399995 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 580 "B_BA0"))
    (pad "L3" smd circle (at 1.599997 2.399995 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 581 "B_BA1"))
    (pad "L7" smd circle (at -1.599997 2.399995 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 489 "CASB#0"))
    (pad "L8" smd circle (at -2.399995 2.399995 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 493 "CSB0_0#"))
    (pad "M2" smd circle (at 2.399995 3.199994 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 569 "MAB10"))
    (pad "M3" smd circle (at 1.599997 3.199994 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 568 "MAB1"))
    (pad "M7" smd circle (at -1.599997 3.199994 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 571 "MAB2"))
    (pad "M8" smd circle (at -2.399995 3.199994 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 567 "MAB0"))
    (pad "M9" smd circle (at -3.199994 3.199994 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "N1" smd circle (at 3.199994 3.999992 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "N2" smd circle (at 2.399995 3.999992 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 572 "MAB3"))
    (pad "N3" smd circle (at 1.599997 3.999992 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 574 "MAB5"))
    (pad "N7" smd circle (at -1.599997 3.999992 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 575 "MAB6"))
    (pad "N8" smd circle (at -2.399995 3.999992 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 573 "MAB4"))
    (pad "P2" smd circle (at 2.399995 4.79999 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 576 "MAB7"))
    (pad "P3" smd circle (at 1.599997 4.79999 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 578 "MAB9"))
    (pad "P7" smd circle (at -1.599997 4.79999 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 570 "MAB11"))
    (pad "P8" smd circle (at -2.399995 4.79999 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 577 "MAB8"))
    (pad "P9" smd circle (at -3.199994 4.79999 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "R1" smd circle (at 3.199994 5.599989 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "R2" smd circle (at 2.399995 5.599989 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 579 "MAB12"))
    (pad "R3" smd circle (at 1.599997 5.599989 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "R7" smd circle (at -1.599997 5.599989 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "R8" smd circle (at -2.399995 5.599989 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 6.001987 6.46 90)
    (fp_text reference "R1113" (at -2.54 2.2225 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 22 "N22672706"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 143 "N22672644"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -48.398006 30.40999)
    (fp_text reference "R223" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 350 "MEM_ID0"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "+3VRUN"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -23.647992 3.809993 180)
    (fp_text reference "C591" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 157 "N18866513"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 14.601995 1.409998 180)
    (fp_text reference "C1122" (at -2.2225 -2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 132 "N22672648"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -4.248005 71.359997 180)
    (fp_text reference "C361" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 59 "N22276557"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 60 "PCIE_TXP14"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 11.302002 41.109994 180)
    (fp_text reference "C586" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 155 "N18850604"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1608_0_89H_1" (layer "B.Cu")
    (tedit 0)
    (at -39.597998 67.109993 180)
    (fp_text reference "C426" (at -1.904975 -1.905025 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 180) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 133 "PCIE_VDDC"))
    (pad "2" smd rect (at 0 0.7874 180) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -6.297988 71.359997 180)
    (fp_text reference "C364" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 65 "N22276539"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 66 "PCIE_TXN12"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -46.947996 12.410001 180)
    (fp_text reference "R1038" (at -2.2225 -2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 130 "N22625904"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "+3VRUN"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -51.298 5.509989 -90)
    (fp_text reference "R130" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 349 "N17821689"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 342 "OTEMP#"))
  )
  (footprint "lib:CAP1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -31.667991 36.810003 180)
    (fp_text reference "C1" (at -1.27 -0.635 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 14 "N22176053"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 5.501988 63.410001 90)
    (fp_text reference "R1103" (at -2.54 2.2225 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 18 "N22665126"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 137 "N22665412"))
  )
  (footprint "lib:CAP1608_0_89H_1" (layer "B.Cu")
    (tedit 0)
    (at -23.698004 47.159995 -90)
    (fp_text reference "C18" (at 1.270025 -1.587475 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 270) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "VDD_CORE"))
    (pad "2" smd rect (at 0 0.7874 270) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -25.498001 39.109998)
    (fp_text reference "C58" (at 1.5875 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 148 "+BBP"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -52.897997 53.509995 180)
    (fp_text reference "R213" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 274 "SMB_CLK"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 290 "PBAT_SMBCLK"))
  )
  (footprint "lib:CAP1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -24.498003 45.109986 180)
    (fp_text reference "C40" (at -1.5875 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "VDD_CORE"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -42.397992 54.609993)
    (fp_text reference "C395" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 117 "N22176231"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -51.298 8.510009 90)
    (fp_text reference "R121" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "+3VRUN"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 344 "N21377273"))
  )
  (footprint "lib:CAP1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -19.398013 48.859992 90)
    (fp_text reference "C17" (at -1.27 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -6.748 13.909998 90)
    (fp_text reference "R53" (at -1.27 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 367 "CLKB0"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 161 "N18867037"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 11.902001 1.409998 180)
    (fp_text reference "C1117" (at -2.2225 -2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 24 "VREF"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 7.802009 24.610002 180)
    (fp_text reference "C548" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "N18859284"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -23.098006 49.110004)
    (fp_text reference "C300" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 52 "N16909654"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -37.698002 70.309987)
    (fp_text reference "R156" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 286 "VSYNC"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "+3VRUN"))
  )
  (footprint "lib:CAP1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -28.497995 41.109994 180)
    (fp_text reference "C46" (at -1.5875 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "VDD_CORE"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -28.948007 33.759996)
    (fp_text reference "R37" (at 1.5875 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 363 "N16919162"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 10.002004 66.309995 -90)
    (fp_text reference "C1101" (at 2.54 -2.2225 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 17 "+5VRUN"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -23.698004 8.059997 -90)
    (fp_text reference "R51" (at 1.27 -1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 157 "N18866513"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 11.002002 24.610002 180)
    (fp_text reference "R643" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 152 "N18859449"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -40.197997 9.710006 -90)
    (fp_text reference "C575" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 154 "N18876029"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -21.290008 57.754005)
    (fp_text reference "C63" (at 1.5875 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 126 "N16919174"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1608_0_89H_1" (layer "B.Cu")
    (tedit 0)
    (at -44.698013 43.20999 -90)
    (fp_text reference "C272" (at 1.905025 -1.904975 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 270) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 43 "A2VDD"))
    (pad "2" smd rect (at 0 0.7874 270) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -19.52801 54.660005 -90)
    (fp_text reference "R27" (at 1.27 -1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 122 "N16919383"))
  )
  (footprint "lib:CAP1608_0_89H_1" (layer "B.Cu")
    (tedit 0)
    (at -43.39799 56.709989 -90)
    (fp_text reference "C290" (at 1.905025 -1.904975 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 270) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 46 "AVDD"))
    (pad "2" smd rect (at 0 0.7874 270) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 47 "N22175870"))
  )
  (footprint "lib:CAP1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -24.498003 39.109998)
    (fp_text reference "C59" (at 1.5875 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 148 "+BBP"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:SMIND1005_0_5H_1" (layer "B.Cu")
    (tedit 0)
    (at -30.497991 46.359997 -90)
    (fp_text reference "L24" (at 1.27 -1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 133 "PCIE_VDDC"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 44 "DPLL_VDDC"))
  )
  (footprint "lib:CAP1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -42.497992 49.010004)
    (fp_text reference "C254" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 32 "LPVDD"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 33 "N22176268"))
  )
  (footprint "lib:RES1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -32.567989 41.309994 -90)
    (fp_text reference "R1064" (at 2.54 -2.2225 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 311 "N22471791"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1608_0_89H_1" (layer "B.Cu")
    (tedit 0)
    (at -43.69799 54.409993)
    (fp_text reference "C393" (at 1.904975 1.905025 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 117 "N22176231"))
    (pad "2" smd rect (at 0 0.7874) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:SMIND1005_0_5H_1" (layer "B.Cu")
    (tedit 0)
    (at -43.79799 40.809995)
    (fp_text reference "L37" (at 1.5875 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 118 "N22176381"))
  )
  (footprint "lib:CAP1608_0_89H_1" (layer "B.Cu")
    (tedit 0)
    (at -6.898013 35.210006 180)
    (fp_text reference "C2" (at -1.269975 -0.635025 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874 180) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.7874 180) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -5.39799 68.50999 180)
    (fp_text reference "C363" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 63 "N22276545"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 64 "PCIE_TXP13"))
  )
  (footprint "lib:SMIND1005_0_5H_1" (layer "B.Cu")
    (tedit 0)
    (at -45.098012 45.609985 90)
    (fp_text reference "L19" (at -1.27 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 39 "VDD2DI"))
  )
  (footprint "lib:RES1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -32.448 40.160009 90)
    (fp_text reference "R1063" (at -2.54 2.2225 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 355 "N22175845"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -48.398006 66.960006 90)
    (fp_text reference "R1025" (at -2.54 2.2225 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 308 "DDC2DATA"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 265 "N22274460"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -29.897992 66.309995 180)
    (fp_text reference "R700" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 149 "N22665296"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 6.001987 5.609989 -90)
    (fp_text reference "R1114" (at 2.54 -2.2225 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 143 "N22672644"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "VDD_CORE"))
  )
  (footprint "lib:CAP1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -35.098007 45.609985)
    (fp_text reference "C267" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 39 "VDD2DI"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 40 "N22176225"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -43.997989 17.409991 -90)
    (fp_text reference "R159" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 347 "N21360761"))
  )
  (footprint "lib:CAP1608_0_89H_1" (layer "B.Cu")
    (tedit 0)
    (at -40.097997 18.209989)
    (fp_text reference "C150" (at 1.904975 1.905025 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.7874) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "2" smd rect (at 0 0.7874) (size 0.899998 0.959993) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -51.797999 18.00999 -90)
    (fp_text reference "R144" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 322 "GPIO8"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "+3VRUN"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at 7.10201 61.910004 180)
    (fp_text reference "C1110" (at -2.2225 -2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 137 "N22665412"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -25.498001 43.10999)
    (fp_text reference "C20" (at 1.5875 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "VDD_CORE"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -35.047994 41.409994 -90)
    (fp_text reference "R205" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 279 "TV_Y_G"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -33.998009 50.310001)
    (fp_text reference "C241" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "LVDDR"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at 10.102004 1.409998)
    (fp_text reference "R1112" (at 2.2225 2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 24 "VREF"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 140 "N22672636"))
  )
  (footprint "lib:SOT353_1_1H_1" (layer "B.Cu")
    (tedit 0)
    (at -41.597994 6.109988 90)
    (fp_text reference "U30" (at -0.85833 1.072941 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd oval (at 0.649986 0.950011 90) (size 0.300025 0.610006) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 606 "N22625842"))
    (pad "2" smd oval (at 0 0.950011 90) (size 0.300025 0.610006) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 340 "N22625856"))
    (pad "3" smd oval (at -0.650011 0.950011 90) (size 0.300025 0.610006) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "4" smd oval (at -0.650011 -0.950011 90) (size 0.300025 0.610006) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 341 "RUNPWROK"))
    (pad "5" smd oval (at 0.649986 -0.950011 90) (size 0.300025 0.610006) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "+3VRUN"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -48.398006 67.809992 90)
    (fp_text reference "R1026" (at -2.54 2.2225 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 307 "DDC2CLK"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 266 "N22275940"))
  )
  (footprint "lib:BGA080_11X13-84_1" (layer "B.Cu")
    (tedit 0)
    (at -31.998013 12.310001 180)
    (fp_text reference "U25" (at -1.5875 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "A1" smd circle (at 3.199994 -5.599989 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "A2" smd circle (at 2.399995 -5.599989 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "A3" smd circle (at 1.599997 -5.599989 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "A7" smd circle (at -1.599997 -5.599989 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "A8" smd circle (at -2.399995 -5.599989 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 600 "QSB#7"))
    (pad "A9" smd circle (at -3.199994 -5.599989 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "B1" smd circle (at 3.199994 -4.79999 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 554 "MDB62"))
    (pad "B2" smd circle (at 2.399995 -4.79999 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "B3" smd circle (at 1.599997 -4.79999 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 566 "DQMB#7"))
    (pad "B7" smd circle (at -1.599997 -4.79999 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 599 "QSB7"))
    (pad "B8" smd circle (at -2.399995 -4.79999 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "B9" smd circle (at -3.199994 -4.79999 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 550 "MDB59"))
    (pad "C1" smd circle (at 3.199994 -3.999992 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "C2" smd circle (at 2.399995 -3.999992 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 555 "MDB63"))
    (pad "C3" smd circle (at 1.599997 -3.999992 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "C7" smd circle (at -1.599997 -3.999992 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "C8" smd circle (at -2.399995 -3.999992 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 548 "MDB57"))
    (pad "C9" smd circle (at -3.199994 -3.999992 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "D1" smd circle (at 3.199994 -3.199994 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 553 "MDB61"))
    (pad "D2" smd circle (at 2.399995 -3.199994 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "D3" smd circle (at 1.599997 -3.199994 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 552 "MDB60"))
    (pad "D7" smd circle (at -1.599997 -3.199994 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 547 "MDB56"))
    (pad "D8" smd circle (at -2.399995 -3.199994 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "D9" smd circle (at -3.199994 -3.199994 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 549 "MDB58"))
    (pad "E1" smd circle (at 3.199994 -2.399995 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "E2" smd circle (at 2.399995 -2.399995 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "E3" smd circle (at 1.599997 -2.399995 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "E7" smd circle (at -1.599997 -2.399995 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "E8" smd circle (at -2.399995 -2.399995 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 596 "QSB#5"))
    (pad "E9" smd circle (at -3.199994 -2.399995 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "F1" smd circle (at 3.199994 -1.599997 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 536 "MDB46"))
    (pad "F2" smd circle (at 2.399995 -1.599997 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "F3" smd circle (at 1.599997 -1.599997 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 564 "DQMB#5"))
    (pad "F7" smd circle (at -1.599997 -1.599997 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 595 "QSB5"))
    (pad "F8" smd circle (at -2.399995 -1.599997 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "F9" smd circle (at -3.199994 -1.599997 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 533 "MDB43"))
    (pad "G1" smd circle (at 3.199994 -0.799998 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "G2" smd circle (at 2.399995 -0.799998 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 535 "MDB45"))
    (pad "G3" smd circle (at 1.599997 -0.799998 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "G7" smd circle (at -1.599997 -0.799998 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "G8" smd circle (at -2.399995 -0.799998 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 532 "MDB42"))
    (pad "G9" smd circle (at -3.199994 -0.799998 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "H1" smd circle (at 3.199994 0 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 534 "MDB44"))
    (pad "H2" smd circle (at 2.399995 0 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "H3" smd circle (at 1.599997 0 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 537 "MDB47"))
    (pad "H7" smd circle (at -1.599997 0 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 531 "MDB41"))
    (pad "H8" smd circle (at -2.399995 0 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "H9" smd circle (at -3.199994 0 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 530 "MDB40"))
    (pad "J1" smd circle (at 3.199994 0.799998 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 13 "N18875830"))
    (pad "J2" smd circle (at 2.399995 0.799998 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 154 "N18876029"))
    (pad "J3" smd circle (at 1.599997 0.799998 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "J7" smd circle (at -1.599997 0.799998 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "J8" smd circle (at -2.399995 0.799998 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 371 "CLKB1"))
    (pad "J9" smd circle (at -3.199994 0.799998 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "K2" smd circle (at 2.399995 1.599997 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 492 "CKEB1"))
    (pad "K3" smd circle (at 1.599997 1.599997 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 604 "WEB#1"))
    (pad "K7" smd circle (at -1.599997 1.599997 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 602 "RASB#1"))
    (pad "K8" smd circle (at -2.399995 1.599997 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 370 "CLKB1#"))
    (pad "K9" smd circle (at -3.199994 1.599997 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 584 "ODTB1"))
    (pad "L1" smd circle (at 3.199994 2.399995 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 582 "B_BA2"))
    (pad "L2" smd circle (at 2.399995 2.399995 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 580 "B_BA0"))
    (pad "L3" smd circle (at 1.599997 2.399995 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 581 "B_BA1"))
    (pad "L7" smd circle (at -1.599997 2.399995 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 490 "CASB#1"))
    (pad "L8" smd circle (at -2.399995 2.399995 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 494 "CSB1_0#"))
    (pad "M2" smd circle (at 2.399995 3.199994 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 569 "MAB10"))
    (pad "M3" smd circle (at 1.599997 3.199994 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 568 "MAB1"))
    (pad "M7" smd circle (at -1.599997 3.199994 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 571 "MAB2"))
    (pad "M8" smd circle (at -2.399995 3.199994 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 567 "MAB0"))
    (pad "M9" smd circle (at -3.199994 3.199994 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "N1" smd circle (at 3.199994 3.999992 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "N2" smd circle (at 2.399995 3.999992 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 572 "MAB3"))
    (pad "N3" smd circle (at 1.599997 3.999992 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 574 "MAB5"))
    (pad "N7" smd circle (at -1.599997 3.999992 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 575 "MAB6"))
    (pad "N8" smd circle (at -2.399995 3.999992 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 573 "MAB4"))
    (pad "P2" smd circle (at 2.399995 4.79999 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 576 "MAB7"))
    (pad "P3" smd circle (at 1.599997 4.79999 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 578 "MAB9"))
    (pad "P7" smd circle (at -1.599997 4.79999 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 570 "MAB11"))
    (pad "P8" smd circle (at -2.399995 4.79999 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 577 "MAB8"))
    (pad "P9" smd circle (at -3.199994 4.79999 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "R1" smd circle (at 3.199994 5.599989 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
    (pad "R2" smd circle (at 2.399995 5.599989 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 579 "MAB12"))
    (pad "R3" smd circle (at 1.599997 5.599989 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "R7" smd circle (at -1.599997 5.599989 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "R8" smd circle (at -2.399995 5.599989 180) (size 0.3556 0.3556) (layers "B.Cu" "B.Paste" "B.Mask"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -43.69799 2.409996 180)
    (fp_text reference "R1039" (at -2.2225 -2.54 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 340 "N22625856"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 273 "N22628117"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -51.797999 19.009988 -90)
    (fp_text reference "R138" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 317 "GPIO5"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "+3VRUN"))
  )
  (footprint "lib:RES1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -34.998007 55.709991 90)
    (fp_text reference "R32" (at -1.27 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 362 "N16920644"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:SMIND1005_0_5H_1" (layer "B.Cu")
    (tedit 0)
    (at -45.098012 44.609987 90)
    (fp_text reference "L21" (at -1.27 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 120 "VDDR3"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 43 "A2VDD"))
  )
  (footprint "lib:CAP1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -42.497992 36.810003 90)
    (fp_text reference "C296" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 50 "DPA_PVDD"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 51 "N22175966"))
  )
  (footprint "lib:CAP1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -51.198 44.409988 -90)
    (fp_text reference "C629" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 127 "DPB_VDDR"))
    (pad "2" smd rect (at 0 0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 128 "N22176186"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -44.698013 5.609989 180)
    (fp_text reference "C329" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 146 "D+"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 147 "D-"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -35.998005 70.309987 180)
    (fp_text reference "R652" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 200 "N22276906"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -23.698004 11.910002 -90)
    (fp_text reference "C156" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "1.8V_REG"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -9.071008 48.802003)
    (fp_text reference "C244" (at 1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 26 "VDDRHA1"))
    (pad "2" smd rect (at 0 0.492608) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 27 "N16910486"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -26.397999 69.709988 180)
    (fp_text reference "C388" (at -1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 113 "N22276531"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 114 "PCIE_TXN0"))
  )
  (footprint "lib:CAP1005_1" (layer "B.Cu")
    (tedit 0)
    (at -15.367008 38.404996 180)
    (fp_text reference "C62" (at -1.5875 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 123 "N16919381"))
    (pad "2" smd rect (at 0 0.492608 180) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_1" (layer "B.Cu")
    (tedit 0)
    (at -40.197997 8.710008 -90)
    (fp_text reference "R649" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 154 "N18876029"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
  )
  (footprint "lib:RES1005_BGA_1" (layer "B.Cu")
    (tedit 0)
    (at -30.89799 33.610009 90)
    (fp_text reference "R10" (at -1.27 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 -0.492608 90) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "AGND"))
    (pad "2" smd rect (at 0 0.492608 270) (size 0.550012 0.599999) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 306 "OPT_BL_ENA"))
  )
)
