(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "INPUT_PEX6_IN1")
  (net 3 "SNN_INPUT_PEX6_DT1*")
  (net 4 "INPUT_PEX6_IN2")
  (net 5 "SNN_INPUT_PEX6_DT2*")
  (net 6 "PS1_1V15_PH")
  (net 7 "1V15")
  (net 8 "PS5_NVVDD_PHASE1")
  (net 9 "NVVDD")
  (net 10 "PS5_NVVDD_PHASE3")
  (net 11 "PS5_NVVDD_PHASE4")
  (net 12 "PS5_NVVDD_PHASE5")
  (net 13 "PS5_NVVDD_PHASE6")
  (net 14 "PS5_NVVDD_PHASE2")
  (net 15 "FBF_CMD<9>")
  (net 16 "FBF_CMD<25>")
  (net 17 "FBF_CMD<19>")
  (net 18 "FBF_CMD<27>")
  (net 19 "FBF_CMD<28>")
  (net 20 "FBF_CMD<26>")
  (net 21 "FBF_CMD<18>")
  (net 22 "FBF_CMD<21>")
  (net 23 "FBF_CMD<12>")
  (net 24 "FBF_CMD<23>")
  (net 25 "FBF_CMD<20>")
  (net 26 "FBF_CMD<24>")
  (net 27 "FBF_CMD<11>")
  (net 28 "FBF_CMD<15>")
  (net 29 "FBF_CMD<14>")
  (net 30 "FBF_CMD<16>")
  (net 31 "FBF_CMD<7>")
  (net 32 "FBF1_CLK0")
  (net 33 "FBF1_CLK0*")
  (net 34 "FBF_CMD<17>")
  (net 35 "FBVDDQ")
  (net 36 "FBF_CMD<8>")
  (net 37 "FBF_CMD<10>")
  (net 38 "SNN_FBF_NC04")
  (net 39 "FBF_CMD<13>")
  (net 40 "FBF_SEN2")
  (net 41 "FBF_VREF3")
  (net 42 "FBF_VREF4")
  (net 43 "FBF_CMD<6>")
  (net 44 "FBF_ZQ2")
  (net 45 "FBF_D<61>")
  (net 46 "FBF_D<63>")
  (net 47 "FBF_D<59>")
  (net 48 "FBF_D<60>")
  (net 49 "FBF_D<56>")
  (net 50 "FBF_D<58>")
  (net 51 "FBF_D<57>")
  (net 52 "FBF_D<62>")
  (net 53 "FBF_DQM7")
  (net 54 "FBF_DQS_RN7")
  (net 55 "FBF_DQS_WP7")
  (net 56 "FBF_D<32>")
  (net 57 "FBF_D<33>")
  (net 58 "FBF_D<35>")
  (net 59 "FBF_D<34>")
  (net 60 "FBF_D<37>")
  (net 61 "FBF_D<39>")
  (net 62 "FBF_D<36>")
  (net 63 "FBF_D<38>")
  (net 64 "FBF_DQM4")
  (net 65 "FBF_DQS_RN4")
  (net 66 "FBF_DQS_WP4")
  (net 67 "FBF_D<54>")
  (net 68 "FBF_D<55>")
  (net 69 "FBF_D<48>")
  (net 70 "FBF_D<53>")
  (net 71 "FBF_D<49>")
  (net 72 "FBF_D<52>")
  (net 73 "FBF_D<51>")
  (net 74 "FBF_D<50>")
  (net 75 "FBF_DQM6")
  (net 76 "FBF_DQS_RN6")
  (net 77 "FBF_DQS_WP6")
  (net 78 "FBF_D<45>")
  (net 79 "FBF_D<47>")
  (net 80 "FBF_D<46>")
  (net 81 "FBF_D<44>")
  (net 82 "FBF_D<40>")
  (net 83 "FBF_D<43>")
  (net 84 "FBF_D<42>")
  (net 85 "FBF_D<41>")
  (net 86 "FBF_DQM5")
  (net 87 "FBF_DQS_RN5")
  (net 88 "FBF_DQS_WP5")
  (net 89 "FBG_CMD<19>")
  (net 90 "FBG_CMD<21>")
  (net 91 "FBG_CMD<9>")
  (net 92 "FBG_CMD<20>")
  (net 93 "FBG_CMD<12>")
  (net 94 "FBG_CMD<5>")
  (net 95 "FBG_CMD<4>")
  (net 96 "FBG_CMD<3>")
  (net 97 "FBG_CMD<0>")
  (net 98 "FBG_CMD<2>")
  (net 99 "FBG_CMD<1>")
  (net 100 "FBG_CMD<18>")
  (net 101 "FBG_CMD<15>")
  (net 102 "FBG_CMD<11>")
  (net 103 "FBG_CMD<8>")
  (net 104 "FBG_CMD<17>")
  (net 105 "FBG_CMD<6>")
  (net 106 "FBG0_CLK0")
  (net 107 "FBG0_CLK0*")
  (net 108 "FBG_CMD<16>")
  (net 109 "FBG_CMD<14>")
  (net 110 "FBG_CMD<10>")
  (net 111 "SNN_FBG_NC01")
  (net 112 "FBG_CMD<13>")
  (net 113 "FBG_SEN1")
  (net 114 "FBG_VREF1")
  (net 115 "FBG_VREF2")
  (net 116 "FBG_CMD<7>")
  (net 117 "FBG_ZQ1")
  (net 118 "FBG_D<26>")
  (net 119 "FBG_D<24>")
  (net 120 "FBG_D<25>")
  (net 121 "FBG_D<27>")
  (net 122 "FBG_D<29>")
  (net 123 "FBG_D<28>")
  (net 124 "FBG_D<30>")
  (net 125 "FBG_D<31>")
  (net 126 "FBG_DQM3")
  (net 127 "FBG_DQS_RN3")
  (net 128 "FBG_DQS_WP3")
  (net 129 "FBG_D<1>")
  (net 130 "FBG_D<3>")
  (net 131 "FBG_D<0>")
  (net 132 "FBG_D<2>")
  (net 133 "FBG_D<7>")
  (net 134 "FBG_D<6>")
  (net 135 "FBG_D<4>")
  (net 136 "FBG_D<5>")
  (net 137 "FBG_DQM0")
  (net 138 "FBG_DQS_RN0")
  (net 139 "FBG_DQS_WP0")
  (net 140 "FBG_D<8>")
  (net 141 "FBG_D<10>")
  (net 142 "FBG_D<11>")
  (net 143 "FBG_D<9>")
  (net 144 "FBG_D<15>")
  (net 145 "FBG_D<12>")
  (net 146 "FBG_D<14>")
  (net 147 "FBG_D<13>")
  (net 148 "FBG_DQM1")
  (net 149 "FBG_DQS_RN1")
  (net 150 "FBG_DQS_WP1")
  (net 151 "FBG_D<21>")
  (net 152 "FBG_D<17>")
  (net 153 "FBG_D<22>")
  (net 154 "FBG_D<16>")
  (net 155 "FBG_D<19>")
  (net 156 "FBG_D<18>")
  (net 157 "FBG_D<23>")
  (net 158 "FBG_D<20>")
  (net 159 "FBG_DQM2")
  (net 160 "FBG_DQS_RN2")
  (net 161 "FBG_DQS_WP2")
  (net 162 "FBG_CMD<25>")
  (net 163 "FBG_CMD<27>")
  (net 164 "FBG_CMD<28>")
  (net 165 "FBG_CMD<26>")
  (net 166 "FBG_CMD<23>")
  (net 167 "FBG_CMD<24>")
  (net 168 "FBG1_CLK0")
  (net 169 "FBG1_CLK0*")
  (net 170 "SNN_FBG_NC04")
  (net 171 "FBG_SEN2")
  (net 172 "FBG_VREF3")
  (net 173 "FBG_VREF4")
  (net 174 "FBG_ZQ2")
  (net 175 "FBG_D<58>")
  (net 176 "FBG_D<63>")
  (net 177 "FBG_D<57>")
  (net 178 "FBG_D<62>")
  (net 179 "FBG_D<60>")
  (net 180 "FBG_D<56>")
  (net 181 "FBG_D<59>")
  (net 182 "FBG_D<61>")
  (net 183 "FBG_DQM7")
  (net 184 "FBG_DQS_RN7")
  (net 185 "FBG_DQS_WP7")
  (net 186 "FBG_D<51>")
  (net 187 "FBG_D<48>")
  (net 188 "FBG_D<50>")
  (net 189 "FBG_D<49>")
  (net 190 "FBG_D<53>")
  (net 191 "FBG_D<54>")
  (net 192 "FBG_D<52>")
  (net 193 "FBG_D<55>")
  (net 194 "FBG_DQM6")
  (net 195 "FBG_DQS_RN6")
  (net 196 "FBG_DQS_WP6")
  (net 197 "FBG_D<37>")
  (net 198 "FBG_D<39>")
  (net 199 "FBG_D<33>")
  (net 200 "FBG_D<36>")
  (net 201 "FBG_D<32>")
  (net 202 "FBG_D<34>")
  (net 203 "FBG_D<35>")
  (net 204 "FBG_D<38>")
  (net 205 "FBG_DQM4")
  (net 206 "FBG_DQS_RN4")
  (net 207 "FBG_DQS_WP4")
  (net 208 "FBG_D<46>")
  (net 209 "FBG_D<45>")
  (net 210 "FBG_D<44>")
  (net 211 "FBG_D<47>")
  (net 212 "FBG_D<40>")
  (net 213 "FBG_D<43>")
  (net 214 "FBG_D<41>")
  (net 215 "FBG_D<42>")
  (net 216 "FBG_DQM5")
  (net 217 "FBG_DQS_RN5")
  (net 218 "FBG_DQS_WP5")
  (net 219 "FBF_CMD<5>")
  (net 220 "FBF_CMD<4>")
  (net 221 "FBF_CMD<3>")
  (net 222 "FBF_CMD<0>")
  (net 223 "FBF_CMD<2>")
  (net 224 "FBF_CMD<1>")
  (net 225 "FBF0_CLK0")
  (net 226 "FBF0_CLK0*")
  (net 227 "SNN_FBF_NC01")
  (net 228 "FBF_SEN1")
  (net 229 "FBF_VREF1")
  (net 230 "FBF_VREF2")
  (net 231 "FBF_ZQ1")
  (net 232 "FBF_D<24>")
  (net 233 "FBF_D<27>")
  (net 234 "FBF_D<26>")
  (net 235 "FBF_D<25>")
  (net 236 "FBF_D<31>")
  (net 237 "FBF_D<29>")
  (net 238 "FBF_D<30>")
  (net 239 "FBF_D<28>")
  (net 240 "FBF_DQM3")
  (net 241 "FBF_DQS_RN3")
  (net 242 "FBF_DQS_WP3")
  (net 243 "FBF_D<0>")
  (net 244 "FBF_D<2>")
  (net 245 "FBF_D<3>")
  (net 246 "FBF_D<1>")
  (net 247 "FBF_D<5>")
  (net 248 "FBF_D<4>")
  (net 249 "FBF_D<6>")
  (net 250 "FBF_D<7>")
  (net 251 "FBF_DQM0")
  (net 252 "FBF_DQS_RN0")
  (net 253 "FBF_DQS_WP0")
  (net 254 "FBF_D<18>")
  (net 255 "FBF_D<20>")
  (net 256 "FBF_D<17>")
  (net 257 "FBF_D<16>")
  (net 258 "FBF_D<19>")
  (net 259 "FBF_D<21>")
  (net 260 "FBF_D<23>")
  (net 261 "FBF_D<22>")
  (net 262 "FBF_DQM2")
  (net 263 "FBF_DQS_RN2")
  (net 264 "FBF_DQS_WP2")
  (net 265 "FBF_D<14>")
  (net 266 "FBF_D<15>")
  (net 267 "FBF_D<12>")
  (net 268 "FBF_D<13>")
  (net 269 "FBF_D<10>")
  (net 270 "FBF_D<9>")
  (net 271 "FBF_D<11>")
  (net 272 "FBF_D<8>")
  (net 273 "FBF_DQM1")
  (net 274 "FBF_DQS_RN1")
  (net 275 "FBF_DQS_WP1")
  (net 276 "FBE_CMD<9>")
  (net 277 "FBE_CMD<25>")
  (net 278 "FBE_CMD<19>")
  (net 279 "FBE_CMD<27>")
  (net 280 "FBE_CMD<28>")
  (net 281 "FBE_CMD<26>")
  (net 282 "FBE_CMD<18>")
  (net 283 "FBE_CMD<21>")
  (net 284 "FBE_CMD<12>")
  (net 285 "FBE_CMD<23>")
  (net 286 "FBE_CMD<20>")
  (net 287 "FBE_CMD<24>")
  (net 288 "FBE_CMD<11>")
  (net 289 "FBE_CMD<15>")
  (net 290 "FBE_CMD<14>")
  (net 291 "FBE_CMD<16>")
  (net 292 "FBE_CMD<7>")
  (net 293 "FBE1_CLK0")
  (net 294 "FBE1_CLK0*")
  (net 295 "FBE_CMD<17>")
  (net 296 "FBE_CMD<8>")
  (net 297 "FBE_CMD<10>")
  (net 298 "SNN_FBE_NC04")
  (net 299 "FBE_CMD<13>")
  (net 300 "FBE_SEN2")
  (net 301 "FBE_VREF3")
  (net 302 "FBE_VREF4")
  (net 303 "FBE_CMD<6>")
  (net 304 "FBE_ZQ2")
  (net 305 "FBE_D<62>")
  (net 306 "FBE_D<63>")
  (net 307 "FBE_D<60>")
  (net 308 "FBE_D<61>")
  (net 309 "FBE_D<59>")
  (net 310 "FBE_D<58>")
  (net 311 "FBE_D<56>")
  (net 312 "FBE_D<57>")
  (net 313 "FBE_DQM7")
  (net 314 "FBE_DQS_RN7")
  (net 315 "FBE_DQS_WP7")
  (net 316 "FBE_D<35>")
  (net 317 "FBE_D<32>")
  (net 318 "FBE_D<34>")
  (net 319 "FBE_D<33>")
  (net 320 "FBE_D<38>")
  (net 321 "FBE_D<39>")
  (net 322 "FBE_D<36>")
  (net 323 "FBE_D<37>")
  (net 324 "FBE_DQM4")
  (net 325 "FBE_DQS_RN4")
  (net 326 "FBE_DQS_WP4")
  (net 327 "FBE_D<49>")
  (net 328 "FBE_D<48>")
  (net 329 "FBE_D<50>")
  (net 330 "FBE_D<51>")
  (net 331 "FBE_D<53>")
  (net 332 "FBE_D<55>")
  (net 333 "FBE_D<54>")
  (net 334 "FBE_D<52>")
  (net 335 "FBE_DQM6")
  (net 336 "FBE_DQS_RN6")
  (net 337 "FBE_DQS_WP6")
  (net 338 "FBE_D<45>")
  (net 339 "FBE_D<47>")
  (net 340 "FBE_D<44>")
  (net 341 "FBE_D<46>")
  (net 342 "FBE_D<42>")
  (net 343 "FBE_D<40>")
  (net 344 "FBE_D<43>")
  (net 345 "FBE_D<41>")
  (net 346 "FBE_DQM5")
  (net 347 "FBE_DQS_RN5")
  (net 348 "FBE_DQS_WP5")
  (net 349 "FBE_CMD<5>")
  (net 350 "FBE_CMD<4>")
  (net 351 "FBE_CMD<3>")
  (net 352 "FBE_CMD<0>")
  (net 353 "FBE_CMD<2>")
  (net 354 "FBE_CMD<1>")
  (net 355 "FBE0_CLK0")
  (net 356 "FBE0_CLK0*")
  (net 357 "SNN_FBE_NC01")
  (net 358 "FBE_SEN1")
  (net 359 "FBE_VREF1")
  (net 360 "FBE_VREF2")
  (net 361 "FBE_ZQ1")
  (net 362 "FBE_D<17>")
  (net 363 "FBE_D<18>")
  (net 364 "FBE_D<16>")
  (net 365 "FBE_D<19>")
  (net 366 "FBE_D<21>")
  (net 367 "FBE_D<23>")
  (net 368 "FBE_D<22>")
  (net 369 "FBE_D<20>")
  (net 370 "FBE_DQM2")
  (net 371 "FBE_DQS_RN2")
  (net 372 "FBE_DQS_WP2")
  (net 373 "FBE_D<3>")
  (net 374 "FBE_D<4>")
  (net 375 "FBE_D<1>")
  (net 376 "FBE_D<2>")
  (net 377 "FBE_D<0>")
  (net 378 "FBE_D<5>")
  (net 379 "FBE_D<7>")
  (net 380 "FBE_D<6>")
  (net 381 "FBE_DQM0")
  (net 382 "FBE_DQS_RN0")
  (net 383 "FBE_DQS_WP0")
  (net 384 "FBE_D<10>")
  (net 385 "FBE_D<11>")
  (net 386 "FBE_D<8>")
  (net 387 "FBE_D<9>")
  (net 388 "FBE_D<12>")
  (net 389 "FBE_D<13>")
  (net 390 "FBE_D<15>")
  (net 391 "FBE_D<14>")
  (net 392 "FBE_DQM1")
  (net 393 "FBE_DQS_RN1")
  (net 394 "FBE_DQS_WP1")
  (net 395 "FBE_D<25>")
  (net 396 "FBE_D<27>")
  (net 397 "FBE_D<26>")
  (net 398 "FBE_D<24>")
  (net 399 "FBE_D<28>")
  (net 400 "FBE_D<31>")
  (net 401 "FBE_D<30>")
  (net 402 "FBE_D<29>")
  (net 403 "FBE_DQM3")
  (net 404 "FBE_DQS_RN3")
  (net 405 "FBE_DQS_WP3")
  (net 406 "FBD_CMD<9>")
  (net 407 "FBD_CMD<25>")
  (net 408 "FBD_CMD<19>")
  (net 409 "FBD_CMD<27>")
  (net 410 "FBD_CMD<28>")
  (net 411 "FBD_CMD<26>")
  (net 412 "FBD_CMD<18>")
  (net 413 "FBD_CMD<21>")
  (net 414 "FBD_CMD<12>")
  (net 415 "FBD_CMD<23>")
  (net 416 "FBD_CMD<20>")
  (net 417 "FBD_CMD<24>")
  (net 418 "FBD_CMD<11>")
  (net 419 "FBD_CMD<15>")
  (net 420 "FBD_CMD<14>")
  (net 421 "FBD_CMD<16>")
  (net 422 "FBD_CMD<7>")
  (net 423 "FBD1_CLK0")
  (net 424 "FBD1_CLK0*")
  (net 425 "FBD_CMD<17>")
  (net 426 "FBD_CMD<8>")
  (net 427 "FBD_CMD<10>")
  (net 428 "SNN_FBD_NC04")
  (net 429 "FBD_CMD<13>")
  (net 430 "FBD_SEN2")
  (net 431 "FBD_VREF3")
  (net 432 "FBD_VREF4")
  (net 433 "FBD_CMD<6>")
  (net 434 "FBD_ZQ2")
  (net 435 "FBD_D<63>")
  (net 436 "FBD_D<58>")
  (net 437 "FBD_D<60>")
  (net 438 "FBD_D<59>")
  (net 439 "FBD_D<56>")
  (net 440 "FBD_D<61>")
  (net 441 "FBD_D<57>")
  (net 442 "FBD_D<62>")
  (net 443 "FBD_DQM7")
  (net 444 "FBD_DQS_RN7")
  (net 445 "FBD_DQS_WP7")
  (net 446 "FBD_D<34>")
  (net 447 "FBD_D<35>")
  (net 448 "FBD_D<32>")
  (net 449 "FBD_D<33>")
  (net 450 "FBD_D<39>")
  (net 451 "FBD_D<38>")
  (net 452 "FBD_D<36>")
  (net 453 "FBD_D<37>")
  (net 454 "FBD_DQM4")
  (net 455 "FBD_DQS_RN4")
  (net 456 "FBD_DQS_WP4")
  (net 457 "FBD_D<42>")
  (net 458 "FBD_D<43>")
  (net 459 "FBD_D<41>")
  (net 460 "FBD_D<40>")
  (net 461 "FBD_D<44>")
  (net 462 "FBD_D<47>")
  (net 463 "FBD_D<46>")
  (net 464 "FBD_D<45>")
  (net 465 "FBD_DQM5")
  (net 466 "FBD_DQS_RN5")
  (net 467 "FBD_DQS_WP5")
  (net 468 "FBD_D<54>")
  (net 469 "FBD_D<50>")
  (net 470 "FBD_D<48>")
  (net 471 "FBD_D<51>")
  (net 472 "FBD_D<53>")
  (net 473 "FBD_D<52>")
  (net 474 "FBD_D<55>")
  (net 475 "FBD_D<49>")
  (net 476 "FBD_DQM6")
  (net 477 "FBD_DQS_RN6")
  (net 478 "FBD_DQS_WP6")
  (net 479 "FBD_CMD<5>")
  (net 480 "FBD_CMD<4>")
  (net 481 "FBD_CMD<3>")
  (net 482 "FBD_CMD<0>")
  (net 483 "FBD_CMD<2>")
  (net 484 "FBD_CMD<1>")
  (net 485 "FBD0_CLK0")
  (net 486 "FBD0_CLK0*")
  (net 487 "SNN_FBD_NC01")
  (net 488 "FBD_SEN1")
  (net 489 "FBD_VREF1")
  (net 490 "FBD_VREF2")
  (net 491 "FBD_ZQ1")
  (net 492 "FBD_D<16>")
  (net 493 "FBD_D<18>")
  (net 494 "FBD_D<17>")
  (net 495 "FBD_D<19>")
  (net 496 "FBD_D<22>")
  (net 497 "FBD_D<23>")
  (net 498 "FBD_D<21>")
  (net 499 "FBD_D<20>")
  (net 500 "FBD_DQM2")
  (net 501 "FBD_DQS_RN2")
  (net 502 "FBD_DQS_WP2")
  (net 503 "FBD_D<3>")
  (net 504 "FBD_D<2>")
  (net 505 "FBD_D<1>")
  (net 506 "FBD_D<0>")
  (net 507 "FBD_D<6>")
  (net 508 "FBD_D<7>")
  (net 509 "FBD_D<4>")
  (net 510 "FBD_D<5>")
  (net 511 "FBD_DQM0")
  (net 512 "FBD_DQS_RN0")
  (net 513 "FBD_DQS_WP0")
  (net 514 "FBD_D<25>")
  (net 515 "FBD_D<24>")
  (net 516 "FBD_D<27>")
  (net 517 "FBD_D<26>")
  (net 518 "FBD_D<28>")
  (net 519 "FBD_D<30>")
  (net 520 "FBD_D<29>")
  (net 521 "FBD_D<31>")
  (net 522 "FBD_DQM3")
  (net 523 "FBD_DQS_RN3")
  (net 524 "FBD_DQS_WP3")
  (net 525 "FBD_D<9>")
  (net 526 "FBD_D<8>")
  (net 527 "FBD_D<11>")
  (net 528 "FBD_D<10>")
  (net 529 "FBD_D<14>")
  (net 530 "FBD_D<15>")
  (net 531 "FBD_D<12>")
  (net 532 "FBD_D<13>")
  (net 533 "FBD_DQM1")
  (net 534 "FBD_DQS_RN1")
  (net 535 "FBD_DQS_WP1")
  (net 536 "FBC_CMD<9>")
  (net 537 "FBC_CMD<25>")
  (net 538 "FBC_CMD<19>")
  (net 539 "FBC_CMD<27>")
  (net 540 "FBC_CMD<28>")
  (net 541 "FBC_CMD<26>")
  (net 542 "FBC_CMD<18>")
  (net 543 "FBC_CMD<21>")
  (net 544 "FBC_CMD<12>")
  (net 545 "FBC_CMD<23>")
  (net 546 "FBC_CMD<20>")
  (net 547 "FBC_CMD<24>")
  (net 548 "FBC_CMD<11>")
  (net 549 "FBC_CMD<15>")
  (net 550 "FBC_CMD<14>")
  (net 551 "FBC_CMD<16>")
  (net 552 "FBC_CMD<7>")
  (net 553 "FBC1_CLK0")
  (net 554 "FBC1_CLK0*")
  (net 555 "FBC_CMD<17>")
  (net 556 "FBC_CMD<8>")
  (net 557 "FBC_CMD<10>")
  (net 558 "SNN_FBC_NC04")
  (net 559 "FBC_CMD<13>")
  (net 560 "FBC_SEN2")
  (net 561 "FBC_VREF3")
  (net 562 "FBC_VREF4")
  (net 563 "FBC_CMD<6>")
  (net 564 "FBC_ZQ2")
  (net 565 "FBC_D<63>")
  (net 566 "FBC_D<61>")
  (net 567 "FBC_D<62>")
  (net 568 "FBC_D<60>")
  (net 569 "FBC_D<57>")
  (net 570 "FBC_D<56>")
  (net 571 "FBC_D<59>")
  (net 572 "FBC_D<58>")
  (net 573 "FBC_DQM7")
  (net 574 "FBC_DQS_RN7")
  (net 575 "FBC_DQS_WP7")
  (net 576 "FBC_D<34>")
  (net 577 "FBC_D<33>")
  (net 578 "FBC_D<35>")
  (net 579 "FBC_D<32>")
  (net 580 "FBC_D<37>")
  (net 581 "FBC_D<36>")
  (net 582 "FBC_D<38>")
  (net 583 "FBC_D<39>")
  (net 584 "FBC_DQM4")
  (net 585 "FBC_DQS_RN4")
  (net 586 "FBC_DQS_WP4")
  (net 587 "FBC_D<49>")
  (net 588 "FBC_D<48>")
  (net 589 "FBC_D<52>")
  (net 590 "FBC_D<51>")
  (net 591 "FBC_D<50>")
  (net 592 "FBC_D<55>")
  (net 593 "FBC_D<53>")
  (net 594 "FBC_D<54>")
  (net 595 "FBC_DQM6")
  (net 596 "FBC_DQS_RN6")
  (net 597 "FBC_DQS_WP6")
  (net 598 "FBC_D<46>")
  (net 599 "FBC_D<45>")
  (net 600 "FBC_D<44>")
  (net 601 "FBC_D<41>")
  (net 602 "FBC_D<42>")
  (net 603 "FBC_D<40>")
  (net 604 "FBC_D<47>")
  (net 605 "FBC_D<43>")
  (net 606 "FBC_DQM5")
  (net 607 "FBC_DQS_RN5")
  (net 608 "FBC_DQS_WP5")
  (net 609 "FBC_CMD<5>")
  (net 610 "FBC_CMD<4>")
  (net 611 "FBC_CMD<3>")
  (net 612 "FBC_CMD<0>")
  (net 613 "FBC_CMD<2>")
  (net 614 "FBC_CMD<1>")
  (net 615 "FBC0_CLK0")
  (net 616 "FBC0_CLK0*")
  (net 617 "SNN_FBC_NC01")
  (net 618 "FBC_SEN1")
  (net 619 "FBC_VREF1")
  (net 620 "FBC_VREF2")
  (net 621 "FBC_ZQ1")
  (net 622 "FBC_D<18>")
  (net 623 "FBC_D<17>")
  (net 624 "FBC_D<16>")
  (net 625 "FBC_D<23>")
  (net 626 "FBC_D<21>")
  (net 627 "FBC_D<20>")
  (net 628 "FBC_D<22>")
  (net 629 "FBC_D<19>")
  (net 630 "FBC_DQM2")
  (net 631 "FBC_DQS_RN2")
  (net 632 "FBC_DQS_WP2")
  (net 633 "FBC_D<6>")
  (net 634 "FBC_D<7>")
  (net 635 "FBC_D<0>")
  (net 636 "FBC_D<4>")
  (net 637 "FBC_D<1>")
  (net 638 "FBC_D<3>")
  (net 639 "FBC_D<5>")
  (net 640 "FBC_D<2>")
  (net 641 "FBC_DQM0")
  (net 642 "FBC_DQS_RN0")
  (net 643 "FBC_DQS_WP0")
  (net 644 "FBC_D<12>")
  (net 645 "FBC_D<8>")
  (net 646 "FBC_D<10>")
  (net 647 "FBC_D<9>")
  (net 648 "FBC_D<11>")
  (net 649 "FBC_D<14>")
  (net 650 "FBC_D<15>")
  (net 651 "FBC_D<13>")
  (net 652 "FBC_DQM1")
  (net 653 "FBC_DQS_RN1")
  (net 654 "FBC_DQS_WP1")
  (net 655 "FBC_D<25>")
  (net 656 "FBC_D<24>")
  (net 657 "FBC_D<28>")
  (net 658 "FBC_D<26>")
  (net 659 "FBC_D<30>")
  (net 660 "FBC_D<29>")
  (net 661 "FBC_D<31>")
  (net 662 "FBC_D<27>")
  (net 663 "FBC_DQM3")
  (net 664 "FBC_DQS_RN3")
  (net 665 "FBC_DQS_WP3")
  (net 666 "FBB_CMD<9>")
  (net 667 "FBB_CMD<25>")
  (net 668 "FBB_CMD<19>")
  (net 669 "FBB_CMD<27>")
  (net 670 "FBB_CMD<28>")
  (net 671 "FBB_CMD<26>")
  (net 672 "FBB_CMD<18>")
  (net 673 "FBB_CMD<21>")
  (net 674 "FBB_CMD<12>")
  (net 675 "FBB_CMD<23>")
  (net 676 "FBB_CMD<20>")
  (net 677 "FBB_CMD<24>")
  (net 678 "FBB_CMD<11>")
  (net 679 "FBB_CMD<15>")
  (net 680 "FBB_CMD<14>")
  (net 681 "FBB_CMD<16>")
  (net 682 "FBB_CMD<7>")
  (net 683 "FBB1_CLK0")
  (net 684 "FBB1_CLK0*")
  (net 685 "FBB_CMD<17>")
  (net 686 "FBB_CMD<8>")
  (net 687 "FBB_CMD<10>")
  (net 688 "SNN_FBB_NC04")
  (net 689 "FBB_CMD<13>")
  (net 690 "FBB_SEN2")
  (net 691 "FBB_VREF3")
  (net 692 "FBB_VREF4")
  (net 693 "FBB_CMD<6>")
  (net 694 "FBB_ZQ2")
  (net 695 "FBB_D<62>")
  (net 696 "FBB_D<63>")
  (net 697 "FBB_D<61>")
  (net 698 "FBB_D<60>")
  (net 699 "FBB_D<58>")
  (net 700 "FBB_D<56>")
  (net 701 "FBB_D<59>")
  (net 702 "FBB_D<57>")
  (net 703 "FBB_DQM7")
  (net 704 "FBB_DQS_RN7")
  (net 705 "FBB_DQS_WP7")
  (net 706 "FBB_D<32>")
  (net 707 "FBB_D<33>")
  (net 708 "FBB_D<35>")
  (net 709 "FBB_D<34>")
  (net 710 "FBB_D<38>")
  (net 711 "FBB_D<39>")
  (net 712 "FBB_D<36>")
  (net 713 "FBB_D<37>")
  (net 714 "FBB_DQM4")
  (net 715 "FBB_DQS_RN4")
  (net 716 "FBB_DQS_WP4")
  (net 717 "FBB_D<40>")
  (net 718 "FBB_D<42>")
  (net 719 "FBB_D<41>")
  (net 720 "FBB_D<43>")
  (net 721 "FBB_D<45>")
  (net 722 "FBB_D<46>")
  (net 723 "FBB_D<44>")
  (net 724 "FBB_D<47>")
  (net 725 "FBB_DQM5")
  (net 726 "FBB_DQS_RN5")
  (net 727 "FBB_DQS_WP5")
  (net 728 "FBB_D<54>")
  (net 729 "FBB_D<55>")
  (net 730 "FBB_D<52>")
  (net 731 "FBB_D<53>")
  (net 732 "FBB_D<48>")
  (net 733 "FBB_D<51>")
  (net 734 "FBB_D<50>")
  (net 735 "FBB_D<49>")
  (net 736 "FBB_DQM6")
  (net 737 "FBB_DQS_RN6")
  (net 738 "FBB_DQS_WP6")
  (net 739 "FBB_CMD<5>")
  (net 740 "FBB_CMD<4>")
  (net 741 "FBB_CMD<3>")
  (net 742 "FBB_CMD<0>")
  (net 743 "FBB_CMD<2>")
  (net 744 "FBB_CMD<1>")
  (net 745 "FBB0_CLK0")
  (net 746 "FBB0_CLK0*")
  (net 747 "SNN_FBB_NC01")
  (net 748 "FBB_SEN1")
  (net 749 "FBB_VREF1")
  (net 750 "FBB_VREF2")
  (net 751 "FBB_ZQ1")
  (net 752 "FBB_D<16>")
  (net 753 "FBB_D<17>")
  (net 754 "FBB_D<18>")
  (net 755 "FBB_D<19>")
  (net 756 "FBB_D<20>")
  (net 757 "FBB_D<22>")
  (net 758 "FBB_D<21>")
  (net 759 "FBB_D<23>")
  (net 760 "FBB_DQM2")
  (net 761 "FBB_DQS_RN2")
  (net 762 "FBB_DQS_WP2")
  (net 763 "FBB_D<0>")
  (net 764 "FBB_D<6>")
  (net 765 "FBB_D<1>")
  (net 766 "FBB_D<5>")
  (net 767 "FBB_D<2>")
  (net 768 "FBB_D<4>")
  (net 769 "FBB_D<3>")
  (net 770 "FBB_D<7>")
  (net 771 "FBB_DQM0")
  (net 772 "FBB_DQS_RN0")
  (net 773 "FBB_DQS_WP0")
  (net 774 "FBB_D<25>")
  (net 775 "FBB_D<26>")
  (net 776 "FBB_D<28>")
  (net 777 "FBB_D<27>")
  (net 778 "FBB_D<24>")
  (net 779 "FBB_D<31>")
  (net 780 "FBB_D<29>")
  (net 781 "FBB_D<30>")
  (net 782 "FBB_DQM3")
  (net 783 "FBB_DQS_RN3")
  (net 784 "FBB_DQS_WP3")
  (net 785 "FBB_D<12>")
  (net 786 "FBB_D<8>")
  (net 787 "FBB_D<9>")
  (net 788 "FBB_D<10>")
  (net 789 "FBB_D<13>")
  (net 790 "FBB_D<14>")
  (net 791 "FBB_D<15>")
  (net 792 "FBB_D<11>")
  (net 793 "FBB_DQM1")
  (net 794 "FBB_DQS_RN1")
  (net 795 "FBB_DQS_WP1")
  (net 796 "FBA_CMD<25>")
  (net 797 "FBA_CMD<19>")
  (net 798 "FBA_CMD<27>")
  (net 799 "FBA_CMD<28>")
  (net 800 "FBA_CMD<26>")
  (net 801 "FBA_CMD<18>")
  (net 802 "FBA_CMD<21>")
  (net 803 "FBA_CMD<12>")
  (net 804 "FBA_CMD<23>")
  (net 805 "FBA_CMD<20>")
  (net 806 "FBA_CMD<9>")
  (net 807 "FBA_CMD<24>")
  (net 808 "FBA_CMD<11>")
  (net 809 "FBA_CMD<15>")
  (net 810 "FBA_CMD<14>")
  (net 811 "FBA_CMD<16>")
  (net 812 "FBA_CMD<7>")
  (net 813 "FBA1_CLK0")
  (net 814 "FBA1_CLK0*")
  (net 815 "FBA_CMD<17>")
  (net 816 "FBA_CMD<13>")
  (net 817 "FBA_CMD<8>")
  (net 818 "FBA_CMD<10>")
  (net 819 "SNN_FBA_NC04")
  (net 820 "FBA_SEN2")
  (net 821 "FBA_VREF3")
  (net 822 "FBA_VREF4")
  (net 823 "FBA_CMD<6>")
  (net 824 "FBA_ZQ2")
  (net 825 "FBA_D<48>")
  (net 826 "FBA_D<50>")
  (net 827 "FBA_D<53>")
  (net 828 "FBA_D<52>")
  (net 829 "FBA_D<49>")
  (net 830 "FBA_D<55>")
  (net 831 "FBA_D<51>")
  (net 832 "FBA_D<54>")
  (net 833 "FBA_DQM6")
  (net 834 "FBA_DQS_RN6")
  (net 835 "FBA_DQS_WP6")
  (net 836 "FBA_D<46>")
  (net 837 "FBA_D<44>")
  (net 838 "FBA_D<45>")
  (net 839 "FBA_D<47>")
  (net 840 "FBA_D<42>")
  (net 841 "FBA_D<41>")
  (net 842 "FBA_D<43>")
  (net 843 "FBA_D<40>")
  (net 844 "FBA_DQM5")
  (net 845 "FBA_DQS_RN5")
  (net 846 "FBA_DQS_WP5")
  (net 847 "FBA_D<35>")
  (net 848 "FBA_D<32>")
  (net 849 "FBA_D<34>")
  (net 850 "FBA_D<33>")
  (net 851 "FBA_D<38>")
  (net 852 "FBA_D<39>")
  (net 853 "FBA_D<36>")
  (net 854 "FBA_D<37>")
  (net 855 "FBA_DQM4")
  (net 856 "FBA_DQS_RN4")
  (net 857 "FBA_DQS_WP4")
  (net 858 "FBA_D<63>")
  (net 859 "FBA_D<62>")
  (net 860 "FBA_D<61>")
  (net 861 "FBA_D<60>")
  (net 862 "FBA_D<56>")
  (net 863 "FBA_D<59>")
  (net 864 "FBA_D<57>")
  (net 865 "FBA_D<58>")
  (net 866 "FBA_DQM7")
  (net 867 "FBA_DQS_RN7")
  (net 868 "FBA_DQS_WP7")
  (net 869 "FBA_CMD<5>")
  (net 870 "FBA_CMD<4>")
  (net 871 "FBA_CMD<3>")
  (net 872 "FBA_CMD<0>")
  (net 873 "FBA_CMD<2>")
  (net 874 "FBA_CMD<1>")
  (net 875 "FBA0_CLK0")
  (net 876 "FBA0_CLK0*")
  (net 877 "SNN_FBA_NC01")
  (net 878 "FBA_SEN1")
  (net 879 "FBA_VREF1")
  (net 880 "FBA_VREF2")
  (net 881 "FBA_ZQ1")
  (net 882 "FBA_D<28>")
  (net 883 "FBA_D<30>")
  (net 884 "FBA_D<27>")
  (net 885 "FBA_D<31>")
  (net 886 "FBA_D<25>")
  (net 887 "FBA_D<26>")
  (net 888 "FBA_D<29>")
  (net 889 "FBA_D<24>")
  (net 890 "FBA_DQM3")
  (net 891 "FBA_DQS_RN3")
  (net 892 "FBA_DQS_WP3")
  (net 893 "FBA_D<13>")
  (net 894 "FBA_D<12>")
  (net 895 "FBA_D<9>")
  (net 896 "FBA_D<8>")
  (net 897 "FBA_D<14>")
  (net 898 "FBA_D<11>")
  (net 899 "FBA_D<15>")
  (net 900 "FBA_D<10>")
  (net 901 "FBA_DQM1")
  (net 902 "FBA_DQS_RN1")
  (net 903 "FBA_DQS_WP1")
  (net 904 "FBA_D<0>")
  (net 905 "FBA_D<1>")
  (net 906 "FBA_D<3>")
  (net 907 "FBA_D<2>")
  (net 908 "FBA_D<4>")
  (net 909 "FBA_D<7>")
  (net 910 "FBA_D<5>")
  (net 911 "FBA_D<6>")
  (net 912 "FBA_DQM0")
  (net 913 "FBA_DQS_RN0")
  (net 914 "FBA_DQS_WP0")
  (net 915 "FBA_D<17>")
  (net 916 "FBA_D<16>")
  (net 917 "FBA_D<19>")
  (net 918 "FBA_D<18>")
  (net 919 "FBA_D<23>")
  (net 920 "FBA_D<22>")
  (net 921 "FBA_D<21>")
  (net 922 "FBA_D<20>")
  (net 923 "FBA_DQM2")
  (net 924 "FBA_DQS_RN2")
  (net 925 "FBA_DQS_WP2")
  (net 926 "PS5_NVVDD_CP")
  (net 927 "NET0001")
  (net 928 "PS5_NVVDD_VAMP_CSREF")
  (net 929 "PS5_NVVDD_VAMP_CSSUM")
  (net 930 "PS5_NVVDD_EN")
  (net 931 "PS5_NVVDD_FB")
  (net 932 "PS5_NVVDD_FBRTN")
  (net 933 "PS5_NVVDD_SET_ILIMFS")
  (net 934 "PS5_NVVDD_SET_IMON")
  (net 935 "PS5_NVVDD_IDES")
  (net 936 "PS5_NVVDD_SET_LSSET")
  (net 937 "SNN_PS5_NVVDD_PIN1")
  (net 938 "SNN_PS5_NVVDD_PIN3")
  (net 939 "SNN_PS5_NVVDD_PIN2")
  (net 940 "SNN_PS5_NVVDD_PIN4")
  (net 941 "PS5_NVVDD_DRV_OD1")
  (net 942 "PS5_NVVDD_DRV_ODN")
  (net 943 "NET0002")
  (net 944 "NET0003")
  (net 945 "PS5_NVVDD_PWM1")
  (net 946 "PS5_NVVDD_PWM2")
  (net 947 "PS5_NVVDD_PWM3")
  (net 948 "PS5_NVVDD_PWM4")
  (net 949 "PS5_NVVDD_PWM5")
  (net 950 "PS5_NVVDD_PWM6")
  (net 951 "PS5_NVVDD_PGOOD")
  (net 952 "NET0004")
  (net 953 "PS5_NVVDD_FS")
  (net 954 "PS5_NVVDD_ISEN1")
  (net 955 "PS5_NVVDD_ISEN2")
  (net 956 "PS5_NVVDD_ISEN3")
  (net 957 "PS5_NVVDD_ISEN4")
  (net 958 "PS5_NVVDD_ISEN5")
  (net 959 "PS5_NVVDD_ISEN6")
  (net 960 "PS5_NVVDD_SET_TRDET")
  (net 961 "NET0005")
  (net 962 "PS5_NVVDD_VCC")
  (net 963 "PS5_NVVDD_VCC_VCC3")
  (net 964 "PS5_NVVDD_VID0")
  (net 965 "PS5_NVVDD_VID1")
  (net 966 "PS5_NVVDD_VID2")
  (net 967 "PS5_NVVDD_VID3")
  (net 968 "PS5_NVVDD_VID4")
  (net 969 "SNN_PS5_NVVDD_VID5")
  (net 970 "PS5_NVVDD_VID6")
  (net 971 "SNN_PS5_NVVDD_VID7")
  (net 972 "SNN_PS5_NVVDD_VRHOT")
  (net 973 "GPIO9_THERM_ALERT*")
  (net 974 "THERM_DP")
  (net 975 "THERM_DN")
  (net 976 "I2C3_SCL_R")
  (net 977 "I2C3_SDA_R")
  (net 978 "THERM_SHDN*")
  (net 979 "THERM_VDD")
  (net 980 "NET0006")
  (net 981 "12V_PEX6_F1")
  (net 982 "PS5_NVVDD_UG1_R")
  (net 983 "12V_PEX6_F2")
  (net 984 "PS5_NVVDD_UG3_R")
  (net 985 "PS5_NVVDD_UG4_R")
  (net 986 "PS5_NVVDD_UG5_R")
  (net 987 "PS5_NVVDD_UG6_R")
  (net 988 "PS5_NVVDD_UG2_R")
  (net 989 "PS3_FBVDDQ_PHASE")
  (net 990 "PS3_FBVDDQ_LG_G")
  (net 991 "12V_F")
  (net 992 "PS3_FBVDDQ_UG_R")
  (net 993 "PS5_NVVDD_LG1_AC")
  (net 994 "PS5_NVVDD_LG2_AC")
  (net 995 "PS5_NVVDD_LG3_AC")
  (net 996 "PS5_NVVDD_LG4_AC")
  (net 997 "PS5_NVVDD_LG5_AC")
  (net 998 "PS5_NVVDD_LG6_AC")
  (net 999 "NVVDD_SENSE_R")
  (net 1000 "12V")
  (net 1001 "5V_INPUT")
  (net 1002 "PS5_NVVDD_BOOT4_RC")
  (net 1003 "PS5_NVVDD_BOOT3_RC")
  (net 1004 "PS5_NVVDD_BOOT5_RC")
  (net 1005 "PS5_NVVDD_BOOT6_RC")
  (net 1006 "PS5_NVVDD_BOOT1_RC")
  (net 1007 "PS5_NVVDD_BOOT2_RC")
  (net 1008 "ROM_CS*")
  (net 1009 "3V3")
  (net 1010 "STRAP0")
  (net 1011 "STRAP1")
  (net 1012 "STRAP2")
  (net 1013 "PS5_NVVDD_BOOT1")
  (net 1014 "PS5_NVVDD_UG1")
  (net 1015 "PS5_NVVDD_LG1")
  (net 1016 "12V_PH1")
  (net 1017 "PS5_NVVDD_BOOT2")
  (net 1018 "PS5_NVVDD_UG2")
  (net 1019 "PS5_NVVDD_LG2")
  (net 1020 "12V_PH2")
  (net 1021 "PS5_NVVDD_BOOT3")
  (net 1022 "PS5_NVVDD_UG3")
  (net 1023 "PS5_NVVDD_LG3")
  (net 1024 "PS5_NVVDD_DRV_PHASE3")
  (net 1025 "12V_PH3")
  (net 1026 "PS5_NVVDD_BOOT4")
  (net 1027 "PS5_NVVDD_UG4")
  (net 1028 "PS5_NVVDD_LG4")
  (net 1029 "PS5_NVVDD_DRV_PHASE4")
  (net 1030 "12V_PH4")
  (net 1031 "PS5_NVVDD_BOOT5")
  (net 1032 "PS5_NVVDD_UG5")
  (net 1033 "PS5_NVVDD_LG5")
  (net 1034 "12V_PH5")
  (net 1035 "PS5_NVVDD_BOOT6")
  (net 1036 "PS5_NVVDD_UG6")
  (net 1037 "PS5_NVVDD_LG6")
  (net 1038 "12V_PH6")
  (net 1039 "PS5_NVVDD_CP_RC")
  (net 1040 "PS3_FBVDDQ_BOOT")
  (net 1041 "NET0007")
  (net 1042 "NET0008")
  (net 1043 "PS5_NVVDD_VIN_PWM")
  (net 1044 "12V_PS3_R")
  (net 1045 "PS3_PVCC5_DRV")
  (net 1046 "PS3_VCC5")
  (net 1047 "PS1_PVCC5")
  (net 1048 "PS1_VCC5")
  (net 1049 "PS1_VCC12")
  (net 1050 "GPU_RST*")
  (net 1051 "GPU_RST_R*")
  (net 1052 "IFP_IOVDD_EN")
  (net 1053 "IFP_IOVDD")
  (net 1054 "PS3_FBVDDQ_CP_RC")
  (net 1055 "PS3_FBVDDQ_FB")
  (net 1056 "FB_CAL_PD_VDDQ")
  (net 1057 "PS3_FS_DIS")
  (net 1058 "XTAL_OUT")
  (net 1059 "XTAL_IN")
  (net 1060 "DRB_CLK")
  (net 1061 "DRB_D0")
  (net 1062 "DRB_D10")
  (net 1063 "DRB_D11")
  (net 1064 "DRB_D1")
  (net 1065 "DRB_D2")
  (net 1066 "DRB_D3")
  (net 1067 "DRB_D4")
  (net 1068 "DRB_D5")
  (net 1069 "DRB_D6")
  (net 1070 "DRB_D7")
  (net 1071 "DRB_D8")
  (net 1072 "DRB_D9")
  (net 1073 "DRB_CMD")
  (net 1074 "NVIO_EXT_REFCLKB_R")
  (net 1075 "GPIO14_RASTERSYNC2_R")
  (net 1076 "DRB_D13")
  (net 1077 "DRB_D14")
  (net 1078 "DRB_D12")
  (net 1079 "GPIO15_SWAPRDY")
  (net 1080 "DRA_CLK")
  (net 1081 "DRA_D0")
  (net 1082 "DRA_D10")
  (net 1083 "DRA_D11")
  (net 1084 "DRA_D1")
  (net 1085 "DRA_D2")
  (net 1086 "DRA_D3")
  (net 1087 "DRA_D4")
  (net 1088 "DRA_D5")
  (net 1089 "DRA_D6")
  (net 1090 "DRA_D7")
  (net 1091 "DRA_D8")
  (net 1092 "DRA_D9")
  (net 1093 "DRA_CMD")
  (net 1094 "NVIO_EXT_REFCLKA_R")
  (net 1095 "GPIO11_RASTERSYNC1_R")
  (net 1096 "DRA_D13")
  (net 1097 "DRA_D14")
  (net 1098 "DRA_D12")
  (net 1099 "PS5_NVVDD_RC1")
  (net 1100 "PS5_NVVDD_RC4")
  (net 1101 "PS5_NVVDD_RC3")
  (net 1102 "PS5_NVVDD_RC5")
  (net 1103 "PS5_NVVDD_RC6")
  (net 1104 "PS3_FBVDDQ_RC")
  (net 1105 "PS5_NVVDD_RC2")
  (net 1106 "PS1_1V15_PH_RC")
  (net 1107 "PS1_1V15_LG")
  (net 1108 "PS1_1V15_UG_R")
  (net 1109 "PS3_FBVDDQ_VSEN")
  (net 1110 "GV_TX0")
  (net 1111 "GPU_BUFCLK_LDT_IN")
  (net 1112 "SNN_SPARE_63")
  (net 1113 "I2CS_SDA")
  (net 1114 "GPU_HOT_RESET*")
  (net 1115 "JTAG_TDI_GPU")
  (net 1116 "SNN_SPARE_65")
  (net 1117 "SNN_FBA_DBI0")
  (net 1118 "SNN_SPARE_67")
  (net 1119 "SNN_SPARE_64")
  (net 1120 "PEX_REFCLK")
  (net 1121 "PEX_REFCLK*")
  (net 1122 "PEX_RX1")
  (net 1123 "PEX_RX1*")
  (net 1124 "PEX_RX2*")
  (net 1125 "PEX_RX0*")
  (net 1126 "PEX_TX11")
  (net 1127 "PEX_RX12")
  (net 1128 "PEX_RX11")
  (net 1129 "PEX_RX11*")
  (net 1130 "PEX_TX14")
  (net 1131 "PEX_RX14")
  (net 1132 "PEX_RX13")
  (net 1133 "PEX_RX13*")
  (net 1134 "PEX_TSTCLK_OUT*")
  (net 1135 "PEX_RX15")
  (net 1136 "PEX_RX15*")
  (net 1137 "PEX_RX3")
  (net 1138 "PEX_RX3*")
  (net 1139 "PEX_RX4*")
  (net 1140 "SNN_SPARE_71")
  (net 1141 "PEX_RX5")
  (net 1142 "PEX_RX5*")
  (net 1143 "PEX_RX6")
  (net 1144 "PEX_RX6*")
  (net 1145 "PEX_TX5")
  (net 1146 "PEX_RX8")
  (net 1147 "PEX_RX7")
  (net 1148 "PEX_RX7*")
  (net 1149 "PEX_TX8")
  (net 1150 "PEX_RX10")
  (net 1151 "PEX_RX9")
  (net 1152 "PEX_RX9*")
  (net 1153 "PEX_RX14*")
  (net 1154 "PEX_TX14*")
  (net 1155 "PEX_TX0")
  (net 1156 "PEX_TX0*")
  (net 1157 "PEX_TX1")
  (net 1158 "PEX_TX1*")
  (net 1159 "SNN_SPARE_68")
  (net 1160 "PEX_TX8*")
  (net 1161 "PEX_TX10")
  (net 1162 "PEX_TX10*")
  (net 1163 "PEX_TX12")
  (net 1164 "PEX_TX12*")
  (net 1165 "PEX_TX11*")
  (net 1166 "PEX_TX13")
  (net 1167 "PEX_TX13*")
  (net 1168 "PEX_TX15")
  (net 1169 "PEX_TX15*")
  (net 1170 "PEX_RX4")
  (net 1171 "GPU_PEX_PWR_GOOD*")
  (net 1172 "PEX_TX2")
  (net 1173 "PEX_TX2*")
  (net 1174 "SNN_SPARE_72")
  (net 1175 "JTAG_TDO_GPU")
  (net 1176 "PEX_TX4")
  (net 1177 "PEX_TX4*")
  (net 1178 "PEX_TX5*")
  (net 1179 "PEX_TX6*")
  (net 1180 "JTAG_TRST*")
  (net 1181 "PEX_TX6")
  (net 1182 "PEX_TX7")
  (net 1183 "PEX_TX7*")
  (net 1184 "PEX_TX9")
  (net 1185 "PEX_TX9*")
  (net 1186 "SNN_FBA0_CLK1")
  (net 1187 "SNN_FBA0_CLK1*")
  (net 1188 "SNN_FBA1_CLK1")
  (net 1189 "SNN_FBA1_CLK1*")
  (net 1190 "SNN_GPU_NC_15")
  (net 1191 "SNN_THERM_LD_STEP1")
  (net 1192 "FBAB_REFCLK*")
  (net 1193 "SNN_FBA_CMD<22>")
  (net 1194 "SNN_FBA_CMD<29>")
  (net 1195 "SNN_FBA_CMD<31>")
  (net 1196 "SNN_FBA_CMD<30>")
  (net 1197 "SNN_THERM_LD_STEP0")
  (net 1198 "SNN_FBA_DBI1")
  (net 1199 "SNN_SPARE_45")
  (net 1200 "SNN_FBA_DBI3")
  (net 1201 "SNN_FBA_DBI5")
  (net 1202 "SNN_FBA_DBI6")
  (net 1203 "PEX_TSTCLK_OUT")
  (net 1204 "SNN_FBA_DBI4")
  (net 1205 "SNN_FBA_DBI2")
  (net 1206 "SNN_GPU_NC_16")
  (net 1207 "SNN_SPARE_01")
  (net 1208 "GPU_TESTMODE")
  (net 1209 "SNN_SPARE_02")
  (net 1210 "SNN_FBB0_CLK1")
  (net 1211 "SNN_FBB0_CLK1*")
  (net 1212 "SNN_FBB_DBI3")
  (net 1213 "SNN_FBB1_CLK1")
  (net 1214 "SNN_FBB1_CLK1*")
  (net 1215 "SNN_FBB_CMD<22>")
  (net 1216 "SNN_FBB_CMD<29>")
  (net 1217 "SNN_FBB_CMD<31>")
  (net 1218 "SNN_FBB_CMD<30>")
  (net 1219 "SNN_FBA_CMD<32>")
  (net 1220 "SNN_FBB_DBI2")
  (net 1221 "SNN_FBB_DBI0")
  (net 1222 "SNN_FBB_DBI1")
  (net 1223 "SNN_FBB_DBI7")
  (net 1224 "SNN_FB_VREF0")
  (net 1225 "SNN_FBB_DBI6")
  (net 1226 "SNN_FBB_DBI4")
  (net 1227 "FBCD_REFCLK*")
  (net 1228 "FBCD_REFCLK")
  (net 1229 "SNN_FBC0_CLK1")
  (net 1230 "SNN_FBC0_CLK1*")
  (net 1231 "SNN_FBC1_CLK1")
  (net 1232 "SNN_FBC1_CLK1*")
  (net 1233 "SNN_FBC_CMD<22>")
  (net 1234 "SNN_FBC_CMD<32>")
  (net 1235 "SNN_FBC_CMD<29>")
  (net 1236 "SNN_FBC_CMD<31>")
  (net 1237 "SNN_FBC_CMD<30>")
  (net 1238 "SNN_FBB_CMD<32>")
  (net 1239 "SNN_FBC_DBI4")
  (net 1240 "SNN_FBC_DBI0")
  (net 1241 "SNN_FBC_DBI7")
  (net 1242 "SNN_FBC_DBI6")
  (net 1243 "SNN_GPU_NC_35")
  (net 1244 "SNN_GPU_NC_33")
  (net 1245 "SNN_FBC_DBI5")
  (net 1246 "SNN_FBC_DBI3")
  (net 1247 "FBC_DEBUG")
  (net 1248 "SNN_FBC_DBI1")
  (net 1249 "SNN_FBC_DBI2")
  (net 1250 "FB_CAL_PU_GND")
  (net 1251 "SNN_FBD0_CLK1")
  (net 1252 "SNN_FBD0_CLK1*")
  (net 1253 "SNN_GPU_NC_37")
  (net 1254 "SNN_FBD1_CLK1")
  (net 1255 "SNN_FBD1_CLK1*")
  (net 1256 "SNN_FBD_CMD<22>")
  (net 1257 "SNN_FBD_CMD<29>")
  (net 1258 "SNN_FBD_CMD<30>")
  (net 1259 "SNN_FBD_CMD<31>")
  (net 1260 "SNN_FBD_DBI1")
  (net 1261 "SNN_FBD_DBI0")
  (net 1262 "SNN_FBD_DBI5")
  (net 1263 "SNN_FBD_CMD<32>")
  (net 1264 "SNN_FBD_DBI6")
  (net 1265 "SNN_FBD_DBI4")
  (net 1266 "SNN_GPU_NC_34")
  (net 1267 "FBD_DEBUG")
  (net 1268 "SNN_FBD_DBI2")
  (net 1269 "SNN_FBE0_CLK1")
  (net 1270 "SNN_FBE0_CLK1*")
  (net 1271 "FBEF_REFCLK*")
  (net 1272 "FBEF_REFCLK")
  (net 1273 "SNN_FBE1_CLK1")
  (net 1274 "SNN_FBE1_CLK1*")
  (net 1275 "SNN_FBE_CMD<31>")
  (net 1276 "SNN_FBE_CMD<29>")
  (net 1277 "SNN_FBE_CMD<30>")
  (net 1278 "SNN_FBE_CMD<32>")
  (net 1279 "SNN_FBE_DBI1")
  (net 1280 "SNN_FBE_DBI4")
  (net 1281 "SNN_FBF_DBI0")
  (net 1282 "FBEFGH_MPLL_AVDD")
  (net 1283 "SNN_FBE_DBI5")
  (net 1284 "SNN_FBE_CMD<22>")
  (net 1285 "SNN_FBE_DBI0")
  (net 1286 "FBE_DEBUG")
  (net 1287 "SNN_FBD_DBI7")
  (net 1288 "SNN_FBE_DBI3")
  (net 1289 "SNN_FBE_DBI2")
  (net 1290 "SNN_FBF0_CLK1")
  (net 1291 "SNN_FBF1_CLK1*")
  (net 1292 "SNN_FBF1_CLK1")
  (net 1293 "SNN_FBF0_CLK1*")
  (net 1294 "SNN_FBF_CMD<22>")
  (net 1295 "SNN_FBF_CMD<29>")
  (net 1296 "SNN_FBF_CMD<32>")
  (net 1297 "SNN_FBF_CMD<30>")
  (net 1298 "SNN_GPU_NC_36")
  (net 1299 "SNN_FBF_DBI2")
  (net 1300 "SNN_FBF_CMD<31>")
  (net 1301 "SNN_FBE_DBI7")
  (net 1302 "SNN_FBF_DBI4")
  (net 1303 "SNN_GPU_NC_38")
  (net 1304 "SNN_FBE_DBI6")
  (net 1305 "SNN_FBF_DBI6")
  (net 1306 "FBF_DEBUG")
  (net 1307 "SNN_FBF_DBI5")
  (net 1308 "SNN_FBF_DBI1")
  (net 1309 "SNN_FBF_DBI3")
  (net 1310 "SNN_FBG0_CLK1*")
  (net 1311 "SNN_FBG0_CLK1")
  (net 1312 "SNN_FBG1_CLK1")
  (net 1313 "SNN_FBG1_CLK1*")
  (net 1314 "SNN_GPU_NC_12")
  (net 1315 "SNN_SPARE_11")
  (net 1316 "SNN_GPU_NC_17")
  (net 1317 "SNN_FBG_CMD<22>")
  (net 1318 "SNN_FBG_CMD<29>")
  (net 1319 "SNN_FBG_CMD<30>")
  (net 1320 "SNN_FBH_CMD<0>")
  (net 1321 "SNN_FBG_CMD<31>")
  (net 1322 "SNN_FBH_CMD<2>")
  (net 1323 "SNN_FBH_CMD<3>")
  (net 1324 "SNN_FBH_CMD<1>")
  (net 1325 "SNN_FBG_DBI2")
  (net 1326 "SNN_FBG_DBI5")
  (net 1327 "SNN_FBG_DBI3")
  (net 1328 "SNN_FBF_DBI7")
  (net 1329 "SNN_FBG_DBI1")
  (net 1330 "SNN_FBG_DBI7")
  (net 1331 "SNN_FBH0_CLK0*")
  (net 1332 "SNN_FBG_DBI0")
  (net 1333 "SNN_FBG_DBI4")
  (net 1334 "SNN_GPU_NC_9")
  (net 1335 "SNN_FBG_DBI6")
  (net 1336 "SNN_FBG_CMD<32>")
  (net 1337 "SNN_FBH0_CLK0")
  (net 1338 "SNN_FBH_D<11>")
  (net 1339 "SNN_FBH0_CLK1")
  (net 1340 "SNN_FBH0_CLK1*")
  (net 1341 "SNN_FBH_D<15>")
  (net 1342 "SNN_FBH_D<24>")
  (net 1343 "SNN_FBH1_CLK1")
  (net 1344 "SNN_FBH1_CLK1*")
  (net 1345 "SNN_FBH_CMD<6>")
  (net 1346 "SNN_FBH_CMD<16>")
  (net 1347 "SNN_FBH_CMD<20>")
  (net 1348 "SNN_FBH_CMD<17>")
  (net 1349 "SNN_FBH_CMD<22>")
  (net 1350 "SNN_FBH_D<49>")
  (net 1351 "SNN_FBH_CMD<23>")
  (net 1352 "SNN_FBH_CMD<21>")
  (net 1353 "SNN_FBH_CMD<25>")
  (net 1354 "SNN_FBH_CMD<27>")
  (net 1355 "SNN_FBH_D<48>")
  (net 1356 "SNN_FBH_CMD<7>")
  (net 1357 "SNN_FBH_CMD<28>")
  (net 1358 "SNN_FBH_CMD<29>")
  (net 1359 "SNN_FBH_CMD<26>")
  (net 1360 "SNN_FBH_CMD<30>")
  (net 1361 "SNN_FBH_CMD<31>")
  (net 1362 "SNN_FBH_DQS_RN6")
  (net 1363 "SNN_FBH_DQM6")
  (net 1364 "SNN_FBH_CMD<32>")
  (net 1365 "SNN_FBH_DQS_WP6")
  (net 1366 "SNN_FBH_D<55>")
  (net 1367 "SNN_FBH_CMD<5>")
  (net 1368 "SNN_FBH_D<16>")
  (net 1369 "SNN_FBH_D<45>")
  (net 1370 "SNN_FBH_CMD<19>")
  (net 1371 "SNN_FBH_CMD<8>")
  (net 1372 "SNN_FBH_CMD<11>")
  (net 1373 "SNN_FBH_CMD<10>")
  (net 1374 "SNN_FBH_CMD<13>")
  (net 1375 "SNN_FBH_CMD<12>")
  (net 1376 "SNN_FBH_CMD<15>")
  (net 1377 "SNN_FBH_CMD<18>")
  (net 1378 "SNN_FBH_DQS_RN0")
  (net 1379 "SNN_FBH_DQM3")
  (net 1380 "SNN_FBH_D<28>")
  (net 1381 "SNN_FBH_D<26>")
  (net 1382 "SNN_FBH1_CLK0")
  (net 1383 "SNN_FBH_D<29>")
  (net 1384 "SNN_FBH1_CLK0*")
  (net 1385 "SNN_FBH_CMD<14>")
  (net 1386 "SNN_FBH_D<4>")
  (net 1387 "SNN_FBH_DQM2")
  (net 1388 "SNN_FBH_D<6>")
  (net 1389 "SNN_FBH_D<5>")
  (net 1390 "SNN_FBH_DQS_RN2")
  (net 1391 "SNN_FBH_D<7>")
  (net 1392 "SNN_FBH_D<19>")
  (net 1393 "SNN_FBH_D<13>")
  (net 1394 "SNN_FBH_D<10>")
  (net 1395 "SNN_FBH_DQS_RN1")
  (net 1396 "SNN_FBH_D<12>")
  (net 1397 "SNN_FBH_D<0>")
  (net 1398 "SNN_FBH_DQM1")
  (net 1399 "SNN_FBH_D<14>")
  (net 1400 "SNN_FBH_CMD<24>")
  (net 1401 "SNN_FBH_D<41>")
  (net 1402 "SNN_FBH_D<52>")
  (net 1403 "SNN_FBH_D<53>")
  (net 1404 "SNN_FBH_D<51>")
  (net 1405 "SNN_FBH_D<50>")
  (net 1406 "SNN_FBH_DBI5")
  (net 1407 "SNN_FBH_D<43>")
  (net 1408 "SNN_FBH_DQS_WP0")
  (net 1409 "SNN_SPARE_26")
  (net 1410 "SNN_FBH_D<33>")
  (net 1411 "SNN_FBH_D<35>")
  (net 1412 "SNN_SPARE_25")
  (net 1413 "SNN_FBH_D<32>")
  (net 1414 "SNN_FBH_D<34>")
  (net 1415 "SNN_SPARE_66")
  (net 1416 "SNN_SPARE_47")
  (net 1417 "SNN_FBH_DQS_RN5")
  (net 1418 "SNN_FBH_DQS_WP2")
  (net 1419 "SNN_FBH_CMD<9>")
  (net 1420 "SNN_FBH_D<23>")
  (net 1421 "SNN_FBH_D<40>")
  (net 1422 "SNN_FBH_DBI2")
  (net 1423 "SNN_FBH_DQS_WP5")
  (net 1424 "SNN_FBH_D<46>")
  (net 1425 "SNN_FBH_DQM5")
  (net 1426 "GV_TX19")
  (net 1427 "SNN_FBH_D<58>")
  (net 1428 "GV_RX2")
  (net 1429 "SNN_FBH_DBI4")
  (net 1430 "SNN_FBH_D<61>")
  (net 1431 "SNN_FBH_DQS_WP7")
  (net 1432 "SNN_FBH_D<62>")
  (net 1433 "GV_RX2*")
  (net 1434 "SNN_FBH_CMD<4>")
  (net 1435 "SNN_FBH_D<2>")
  (net 1436 "SNN_FBH_D<25>")
  (net 1437 "SNN_GPU_NC_11")
  (net 1438 "SNN_FBH_DQS_RN3")
  (net 1439 "SNN_FBH_DQM0")
  (net 1440 "SNN_FBH_DQS_WP1")
  (net 1441 "SNN_FBH_D<54>")
  (net 1442 "SNN_SPARE_46")
  (net 1443 "SNN_FBH_D<21>")
  (net 1444 "SNN_FBH_D<63>")
  (net 1445 "SNN_FBH_DBI0")
  (net 1446 "SNN_FBH_D<30>")
  (net 1447 "SNN_FBH_D<17>")
  (net 1448 "SNN_FBH_D<9>")
  (net 1449 "SNN_FBH_D<44>")
  (net 1450 "SNN_FBH_DQS_WP4")
  (net 1451 "SNN_FBH_D<20>")
  (net 1452 "SNN_FBH_DQS_RN7")
  (net 1453 "SNN_FBH_D<1>")
  (net 1454 "SNN_FBH_DBI3")
  (net 1455 "SNN_FBH_D<18>")
  (net 1456 "SNN_FBH_D<8>")
  (net 1457 "SNN_FBH_D<47>")
  (net 1458 "SNN_SPARE_60")
  (net 1459 "SNN_FBH_D<22>")
  (net 1460 "SNN_FBH_D<60>")
  (net 1461 "SNN_FBD_DBI3")
  (net 1462 "SNN_FBB_DBI5")
  (net 1463 "SNN_FB_VREF1")
  (net 1464 "SNN_SPARE_69")
  (net 1465 "SNN_SPARE_59")
  (net 1466 "SNN_FBA_DBI7")
  (net 1467 "SNN_FBH_D<3>")
  (net 1468 "SNN_FBH_D<31>")
  (net 1469 "SNN_FBH_D<27>")
  (net 1470 "SNN_FBH_DQS_WP3")
  (net 1471 "SNN_FBH_DBI6")
  (net 1472 "SNN_FBH_DQS_RN4")
  (net 1473 "SNN_FBH_D<42>")
  (net 1474 "SNN_FBH_D<59>")
  (net 1475 "SNN_FBVDDQ_MSUR")
  (net 1476 "SNN_FBVDDQ_GND_MSUR")
  (net 1477 "FBVDDQ_SENSE")
  (net 1478 "FBB_DEBUG")
  (net 1479 "SNN_GPU_NC_19")
  (net 1480 "SNN_SPARE_48")
  (net 1481 "SNN_SPARE_49")
  (net 1482 "SNN_SPARE_51")
  (net 1483 "GV_TX1")
  (net 1484 "GV_PLLAVDD")
  (net 1485 "SNN_SPARE_29")
  (net 1486 "GV_RXCLK*")
  (net 1487 "GV_RX0*")
  (net 1488 "SNN_GPU_NC_20")
  (net 1489 "SNN_FBH_D<39>")
  (net 1490 "GV_RX0")
  (net 1491 "GV_RXCLK")
  (net 1492 "SNN_FBH_D<57>")
  (net 1493 "SNN_FBH_DQM7")
  (net 1494 "GV_TX18")
  (net 1495 "GV_RX3*")
  (net 1496 "GV_TX14*")
  (net 1497 "GV_TX14")
  (net 1498 "SNN_FBH_D<38>")
  (net 1499 "GV_TX4*")
  (net 1500 "GV_TX6")
  (net 1501 "GV_TX8")
  (net 1502 "GV_TX5*")
  (net 1503 "SNN_SPARE_62")
  (net 1504 "SNN_SPARE_50")
  (net 1505 "GV_TX9")
  (net 1506 "GV_TX12")
  (net 1507 "GV_RXCTL")
  (net 1508 "SNN_SPARE_61")
  (net 1509 "GV_TX11")
  (net 1510 "GV_TX11*")
  (net 1511 "GV_RX_RSET_VDD")
  (net 1512 "GV_TXCTL")
  (net 1513 "GV_TXCTL*")
  (net 1514 "GV_RX1*")
  (net 1515 "GV_RX1")
  (net 1516 "GV_TX15")
  (net 1517 "GV_TX19*")
  (net 1518 "GV_TX18*")
  (net 1519 "GV_TX16*")
  (net 1520 "GV_TX17")
  (net 1521 "GV_TX17*")
  (net 1522 "GV_TX_RSET_GND")
  (net 1523 "PEX_RX2")
  (net 1524 "GV_TX12*")
  (net 1525 "GV_RXCTL*")
  (net 1526 "GV_TX2")
  (net 1527 "GV_TX2*")
  (net 1528 "GV_TXCLK")
  (net 1529 "GV_TXCLK*")
  (net 1530 "GV_TX3*")
  (net 1531 "GV_TX5")
  (net 1532 "SNN_SPARE_70")
  (net 1533 "GV_TX6*")
  (net 1534 "GV_TX8*")
  (net 1535 "GV_TX4")
  (net 1536 "GV_TX7")
  (net 1537 "GV_TX7*")
  (net 1538 "GV_TX10")
  (net 1539 "GV_TX10*")
  (net 1540 "GV_TX13")
  (net 1541 "GV_TX16")
  (net 1542 "GV_TX3")
  (net 1543 "SNN_SPARE_52")
  (net 1544 "FBGH_REFCLK*")
  (net 1545 "FBGH_REFCLK")
  (net 1546 "GV_TX0*")
  (net 1547 "GV_TX1*")
  (net 1548 "SNN_SPARE_16")
  (net 1549 "SNN_GPU_NC_18")
  (net 1550 "SNN_FBH_D<37>")
  (net 1551 "SNN_SPARE_06")
  (net 1552 "SNN_TS_OBS")
  (net 1553 "SNN_NVVDD_MSUR")
  (net 1554 "NVVDD_SENSE")
  (net 1555 "GPU_CLK*")
  (net 1556 "GPU_CLK")
  (net 1557 "SNN_FBH_DEBUG")
  (net 1558 "FBA_DEBUG")
  (net 1559 "JTAG_TCK")
  (net 1560 "SNN_SPARE_53")
  (net 1561 "SNN_GPU_BUFRST*")
  (net 1562 "JTAG_TMS")
  (net 1563 "SNN_GPU_NC_1")
  (net 1564 "SNN_GPU_NC_2")
  (net 1565 "SNN_GPU_NC_3")
  (net 1566 "SNN_GPU_NC_4")
  (net 1567 "SNN_GPU_NC_5")
  (net 1568 "SNN_GPU_NC_6")
  (net 1569 "SNN_GPU_NC_7")
  (net 1570 "SNN_GPU_NC_8")
  (net 1571 "SNN_FBH_DBI1")
  (net 1572 "SNN_GPU_NC_10")
  (net 1573 "FBABCD_MPLL_AVDD")
  (net 1574 "SNN_SPARE_03")
  (net 1575 "SNN_SPARE_04")
  (net 1576 "SNN_GPU_NC_13")
  (net 1577 "SNN_GPU_NC_14")
  (net 1578 "SNN_GPU_NC_21")
  (net 1579 "SNN_GPU_NC_22")
  (net 1580 "SNN_GPU_NC_23")
  (net 1581 "SNN_GPU_NC_24")
  (net 1582 "SNN_GPU_NC_25")
  (net 1583 "SNN_GPU_NC_26")
  (net 1584 "SNN_GPU_NC_27")
  (net 1585 "SNN_GPU_NC_28")
  (net 1586 "SNN_GPU_NC_29")
  (net 1587 "SNN_GPU_NC_30")
  (net 1588 "SNN_GPU_NC_31")
  (net 1589 "SNN_GPU_NC_32")
  (net 1590 "SNN_SPARE_73")
  (net 1591 "SNN_SPARE_74")
  (net 1592 "FB_CAL_TERM_GND")
  (net 1593 "SNN_GPU_NC_39")
  (net 1594 "SNN_GPU_NC_40")
  (net 1595 "FBG_DEBUG")
  (net 1596 "SNN_SPARE_05")
  (net 1597 "SNN_TSENSE_OVERT")
  (net 1598 "SNN_TS_1V5_SEL")
  (net 1599 "SNN_SPARE_07")
  (net 1600 "SNN_SPARE_08")
  (net 1601 "SNN_SPARE_09")
  (net 1602 "SNN_SPARE_10")
  (net 1603 "SNN_SPARE_12")
  (net 1604 "SNN_SPARE_13")
  (net 1605 "SNN_SPARE_14")
  (net 1606 "SNN_SPARE_15")
  (net 1607 "SNN_SPARE_17")
  (net 1608 "SNN_SPARE_18")
  (net 1609 "SNN_SPARE_19")
  (net 1610 "SNN_SPARE_20")
  (net 1611 "SNN_SPARE_21")
  (net 1612 "SNN_SPARE_22")
  (net 1613 "SNN_SPARE_23")
  (net 1614 "SNN_SPARE_24")
  (net 1615 "FBAB_REFCLK")
  (net 1616 "SNN_FBH_D<36>")
  (net 1617 "SNN_SPARE_27")
  (net 1618 "SNN_SPARE_28")
  (net 1619 "SNN_SPARE_30")
  (net 1620 "SNN_SPARE_31")
  (net 1621 "SNN_SPARE_32")
  (net 1622 "SNN_SPARE_33")
  (net 1623 "GPU_PMC_ISO_RESET*")
  (net 1624 "SNN_SPARE_34")
  (net 1625 "SNN_SPARE_35")
  (net 1626 "SNN_SPARE_36")
  (net 1627 "SNN_SPARE_37")
  (net 1628 "SNN_SPARE_38")
  (net 1629 "SNN_SPARE_39")
  (net 1630 "SNN_SPARE_40")
  (net 1631 "SNN_SPARE_41")
  (net 1632 "SNN_SPARE_42")
  (net 1633 "SNN_SPARE_43")
  (net 1634 "SNN_SPARE_44")
  (net 1635 "SNN_SPARE_54")
  (net 1636 "I2CS_SCL")
  (net 1637 "SNN_SPARE_55")
  (net 1638 "SNN_SPARE_56")
  (net 1639 "SNN_SPARE_57")
  (net 1640 "SNN_SPARE_58")
  (net 1641 "SNN_FBH_D<56>")
  (net 1642 "GV_RX3")
  (net 1643 "PEX_PLLVDD")
  (net 1644 "PEX_TX3")
  (net 1645 "PEX_TX3*")
  (net 1646 "PEX_RX0")
  (net 1647 "PEX_RX8*")
  (net 1648 "PEX_RX10*")
  (net 1649 "PEX_RX12*")
  (net 1650 "GV_TX15*")
  (net 1651 "GV_TX13*")
  (net 1652 "GV_TX9*")
  (net 1653 "SNN_FBH_DBI7")
  (net 1654 "SNN_FBH_DQM4")
  (net 1655 "NVVDD_SENSE_GND")
  (net 1656 "SNN_TSENSE_VREF")
  (net 1657 "SNN_TSENSE_AVDD")
  (net 1658 "SNN_NVVDD_GND_MSUR")
  (net 1659 "NET0009")
  (net 1660 "NET0010")
  (net 1661 "NVIO_GV_PLLAVDD")
  (net 1662 "NVIO_GV_PLLVDD")
  (net 1663 "NVIO_CLK_RSET_GND")
  (net 1664 "NVIO_SP_PLLVDD")
  (net 1665 "NET0011")
  (net 1666 "NVIO_PLLVDD")
  (net 1667 "SNN_DACB_HSYNC")
  (net 1668 "DACB_Y")
  (net 1669 "DACB_PB")
  (net 1670 "DACB_PR")
  (net 1671 "SNN_DACB_CSYNC")
  (net 1672 "DACB_RSET")
  (net 1673 "DACB_VDD")
  (net 1674 "DACB_VREF")
  (net 1675 "SNN_DACB_VSYNC")
  (net 1676 "SNN_I2C0_SCL")
  (net 1677 "SNN_I2C0_SDA")
  (net 1678 "DACA_BLUE")
  (net 1679 "DACA_GREEN")
  (net 1680 "DACA_HSYNC")
  (net 1681 "DACA_RED")
  (net 1682 "DACA_RSET")
  (net 1683 "DACA_VDD")
  (net 1684 "DACA_VREF")
  (net 1685 "DACA_VSYNC")
  (net 1686 "I2C1_SCL")
  (net 1687 "I2C1_SDA")
  (net 1688 "DACC_BLUE")
  (net 1689 "DACC_GREEN")
  (net 1690 "DACC_HSYNC")
  (net 1691 "DACC_RED")
  (net 1692 "DACC_RSET")
  (net 1693 "DACC_VDD")
  (net 1694 "DACC_VREF")
  (net 1695 "DACC_VSYNC")
  (net 1696 "I2C2_SCL")
  (net 1697 "I2C2_SDA")
  (net 1698 "IFPAB_PLLVDD")
  (net 1699 "IFPAB_RSET")
  (net 1700 "SNN_IFPAB_VPROBE")
  (net 1701 "IFPAB_IOVDD")
  (net 1702 "IFPA_TXC")
  (net 1703 "IFPA_TXC*")
  (net 1704 "IFPA_TXD0")
  (net 1705 "IFPA_TXD0*")
  (net 1706 "IFPA_TXD1")
  (net 1707 "IFPA_TXD1*")
  (net 1708 "IFPA_TXD2")
  (net 1709 "IFPA_TXD2*")
  (net 1710 "SNN_IFPA_TXD3")
  (net 1711 "SNN_IFPA_TXD3*")
  (net 1712 "SNN_IFPB_TXC")
  (net 1713 "SNN_IFPB_TXC*")
  (net 1714 "IFPB_TXD4")
  (net 1715 "IFPB_TXD4*")
  (net 1716 "IFPB_TXD5")
  (net 1717 "IFPB_TXD5*")
  (net 1718 "IFPB_TXD6")
  (net 1719 "IFPB_TXD6*")
  (net 1720 "SNN_IFPB_TXD7")
  (net 1721 "SNN_IFPB_TXD7*")
  (net 1722 "IFPCD_PLLVDD")
  (net 1723 "IFPCD_RSET")
  (net 1724 "SNN_IFPCD_VPROBE")
  (net 1725 "IFPCD_IOVDD")
  (net 1726 "IFPC_TXC")
  (net 1727 "IFPC_TXC*")
  (net 1728 "IFPC_TXD0")
  (net 1729 "IFPC_TXD0*")
  (net 1730 "IFPC_TXD1")
  (net 1731 "IFPC_TXD1*")
  (net 1732 "IFPC_TXD2")
  (net 1733 "IFPC_TXD2*")
  (net 1734 "SNN_IFPC_TXD3")
  (net 1735 "SNN_IFPC_TXD3*")
  (net 1736 "SNN_IFPD_TXC")
  (net 1737 "SNN_IFPD_TXC*")
  (net 1738 "IFPD_TXD4")
  (net 1739 "IFPD_TXD4*")
  (net 1740 "IFPD_TXD5")
  (net 1741 "IFPD_TXD5*")
  (net 1742 "IFPD_TXD6")
  (net 1743 "IFPD_TXD6*")
  (net 1744 "SNN_IFPD_TXD7")
  (net 1745 "SNN_IFPD_TXD7*")
  (net 1746 "SNN_MIOA_CAL_PD_VDDQ")
  (net 1747 "SNN_MIOA_CAL_PU_GND")
  (net 1748 "SNN_MIOA_CLKOUT")
  (net 1749 "SNN_MIOA_CLKOUT*")
  (net 1750 "MIOA_CTL3")
  (net 1751 "SNN_MIOA<0>")
  (net 1752 "SNN_MIOA<1>")
  (net 1753 "SNN_MIOA<10>")
  (net 1754 "SNN_MIOA<11>")
  (net 1755 "SNN_MIOA<2>")
  (net 1756 "SNN_MIOA<3>")
  (net 1757 "SNN_MIOA<4>")
  (net 1758 "SNN_MIOA<5>")
  (net 1759 "SNN_MIOA<6>")
  (net 1760 "SNN_MIOA<7>")
  (net 1761 "SNN_MIOA<8>")
  (net 1762 "SNN_MIOA<9>")
  (net 1763 "SNN_MIOA_DE")
  (net 1764 "SNN_MIOA_HSYNC")
  (net 1765 "MIOA_VREF")
  (net 1766 "SNN_MIOA_VSYNC")
  (net 1767 "SNN_MIOB_CAL_PD_VDDQ")
  (net 1768 "SNN_MIOB_CAL_PU_GND")
  (net 1769 "SNN_MIOB_CLKOUT")
  (net 1770 "SNN_MIOB_CLKOUT*")
  (net 1771 "MIOB_CTL3")
  (net 1772 "SNN_MIOB<0>")
  (net 1773 "SNN_MIOB<1>")
  (net 1774 "SNN_MIOB<10>")
  (net 1775 "SNN_MIOB<11>")
  (net 1776 "SNN_MIOB<2>")
  (net 1777 "SNN_MIOB<3>")
  (net 1778 "SNN_MIOB<4>")
  (net 1779 "SNN_MIOB<5>")
  (net 1780 "SNN_MIOB<6>")
  (net 1781 "SNN_MIOB<7>")
  (net 1782 "SNN_MIOB<8>")
  (net 1783 "SNN_MIOB<9>")
  (net 1784 "SNN_MIOB_DE")
  (net 1785 "SNN_MIOB_VSYNC")
  (net 1786 "MIOB_VREF")
  (net 1787 "SNN_MIOB_HSYNC")
  (net 1788 "DR_CAL_PD_VDDQ")
  (net 1789 "DR_CAL_PU_GND")
  (net 1790 "2V5")
  (net 1791 "DR_VREF")
  (net 1792 "NVIO_EXTDEV_RST*")
  (net 1793 "NVIO_EXT_REFCLKA")
  (net 1794 "FAN_PWM_NVIO")
  (net 1795 "GPIO0_DVIAB_HPD")
  (net 1796 "GPIO1_DVICD_HPD")
  (net 1797 "NET0012")
  (net 1798 "GPIO11_RASTERSYNC1")
  (net 1799 "NET0013")
  (net 1800 "SNN_GPIO13_STEREO")
  (net 1801 "GPIO14_RASTERSYNC2")
  (net 1802 "NET0014")
  (net 1803 "NET0015")
  (net 1804 "GPIO4_PS5_NVVDD_VID4")
  (net 1805 "GPIO5_PS5_NVVDD_VID1")
  (net 1806 "GPIO6_PS5_NVVDD_VID2")
  (net 1807 "GPIO7_PS5_NVVDD_VID3")
  (net 1808 "GPIO8_FAN_TACH")
  (net 1809 "I2C3_SCL")
  (net 1810 "I2C4_SCL")
  (net 1811 "I2C3_SDA")
  (net 1812 "I2C4_SDA")
  (net 1813 "SNN_STRAP3")
  (net 1814 "NVIO_TESTMODE")
  (net 1815 "FL_REFCLK_VAIO")
  (net 1816 "SNN_NVIO_NC_39")
  (net 1817 "SNN_NVIO_NC_21")
  (net 1818 "SNN_NVIO_NC_33")
  (net 1819 "SNN_NVIO_NC_40")
  (net 1820 "SNN_NVIO_NC_26")
  (net 1821 "SNN_NVIO_NC_27")
  (net 1822 "SNN_NVIO_NC_32")
  (net 1823 "SNN_NVIO_NC_22")
  (net 1824 "SNN_NVIO_NC_38")
  (net 1825 "SNN_NVIO_NC_20")
  (net 1826 "SNN_NVIO_NC_15")
  (net 1827 "SNN_NVIO_NC_16")
  (net 1828 "SNN_NVIO_NC_01")
  (net 1829 "SNN_NVIO_NC_12")
  (net 1830 "SNN_NVIO_NC_02")
  (net 1831 "SNN_NVIO_NC_23")
  (net 1832 "SNN_NVIO_NC_29")
  (net 1833 "SNN_NVIO_NC_34")
  (net 1834 "SNN_NVIO_NC_14")
  (net 1835 "NVIO_EXT_REFCLKB")
  (net 1836 "SNN_NVIO_NC_13")
  (net 1837 "SNN_DVIA_CLK")
  (net 1838 "SNN_DVIA_CTL0")
  (net 1839 "SNN_DVIA_CTL1")
  (net 1840 "SNN_DVIA_CTL2")
  (net 1841 "DVIA_D0")
  (net 1842 "DVIA_D1")
  (net 1843 "DVIA_D2")
  (net 1844 "DVIA_D3")
  (net 1845 "SNN_DVIA_D4")
  (net 1846 "SNN_DVIA_D5")
  (net 1847 "SNN_DVIA_D6")
  (net 1848 "DVIA_D7")
  (net 1849 "SNN_DVIB_CLK")
  (net 1850 "SNN_DVIB_CTL0")
  (net 1851 "SNN_DVIB_CTL1")
  (net 1852 "SNN_DVIB_CTL2")
  (net 1853 "SNN_DVIB_D0")
  (net 1854 "SNN_DVIB_D1")
  (net 1855 "SNN_DVIB_D2")
  (net 1856 "SNN_DVIB_D3")
  (net 1857 "DVIB_D4")
  (net 1858 "DVIB_D5")
  (net 1859 "SNN_DVIB_D6")
  (net 1860 "SNN_DVIB_D7")
  (net 1861 "SNN_GPIO16_DP_INT*")
  (net 1862 "SNN_NVIO_NC_03")
  (net 1863 "SNN_NVIO_NC_04")
  (net 1864 "SNN_NVIO_NC_05")
  (net 1865 "SNN_NVIO_NC_06")
  (net 1866 "SNN_NVIO_NC_07")
  (net 1867 "SNN_NVIO_NC_08")
  (net 1868 "SNN_NVIO_NC_09")
  (net 1869 "SNN_NVIO_NC_10")
  (net 1870 "SNN_MIOA<13>")
  (net 1871 "SNN_MIOA<14>")
  (net 1872 "SNN_MIOA<12>")
  (net 1873 "SNN_NVIO_NC_11")
  (net 1874 "SPDIF_IN_GPU")
  (net 1875 "SNN_NVIO_NC_17")
  (net 1876 "SNN_NVIO_NC_18")
  (net 1877 "SNN_NVIO_NC_19")
  (net 1878 "SNN_NVIO_NC_24")
  (net 1879 "SNN_NVIO_NC_25")
  (net 1880 "SNN_NVIO_NC_28")
  (net 1881 "SNN_NVIO_NC_30")
  (net 1882 "SNN_NVIO_NC_31")
  (net 1883 "SNN_NVIO_NC_35")
  (net 1884 "SNN_NVIO_NC_36")
  (net 1885 "SNN_NVIO_NC_37")
  (net 1886 "SNN_NVIO_NC_41")
  (net 1887 "SNN_NVIO_NC_42")
  (net 1888 "SNN_NVIO_NC_43")
  (net 1889 "SNN_NVIO_NC_44")
  (net 1890 "SNN_NVIO_NC_45")
  (net 1891 "SNN_NVIO_NC_46")
  (net 1892 "SNN_MIOB<12>")
  (net 1893 "SNN_MIOB<13>")
  (net 1894 "SNN_MIOB<14>")
  (net 1895 "SNN_NVIO_NC_47")
  (net 1896 "SNN_NVIO_NC_48")
  (net 1897 "SNN_NVIO_NC_49")
  (net 1898 "SNN_NVIO_NC_50")
  (net 1899 "SNN_NVIO_NC_51")
  (net 1900 "SNN_NVIO_NC_52")
  (net 1901 "SNN_NVIO_NC_53")
  (net 1902 "SNN_NVIO_NC_54")
  (net 1903 "SNN_NVIO_NC_55")
  (net 1904 "SNN_NVIO_NC_56")
  (net 1905 "SNN_NVIO_NC_57")
  (net 1906 "SNN_NVIO_NC_58")
  (net 1907 "SNN_NVIO_NC_59")
  (net 1908 "SNN_NVIO_NC_60")
  (net 1909 "SNN_NVIO_NC_61")
  (net 1910 "JTAG_TDI_NVIO")
  (net 1911 "JTAG_TDO_NVIO")
  (net 1912 "JTAG_TRST_3V3*")
  (net 1913 "5V_ADJ")
  (net 1914 "5V")
  (net 1915 "PS1_2V5_LDO_DR_AC")
  (net 1916 "PS1_2V5_LDO_FB")
  (net 1917 "PS1_1V15_FS")
  (net 1918 "DACA_BLUE_CON")
  (net 1919 "I2C1_SCL_CON")
  (net 1920 "I2C1_SDA_CON")
  (net 1921 "DACA_GREEN_CON")
  (net 1922 "GPIO1_DVICD_HPD_CON")
  (net 1923 "DACA_HSYNC_CON")
  (net 1924 "DACA_RED_CON")
  (net 1925 "DDC_5V")
  (net 1926 "DACA_VSYNC_CON")
  (net 1927 "DACC_BLUE_CON")
  (net 1928 "I2C2_SCL_CON")
  (net 1929 "I2C2_SDA_CON")
  (net 1930 "DACC_GREEN_CON")
  (net 1931 "GPIO0_DVIAB_HPD_CON")
  (net 1932 "DACC_HSYNC_CON")
  (net 1933 "DACC_RED_CON")
  (net 1934 "DACC_VSYNC_CON")
  (net 1935 "HYBRID_HPD_E")
  (net 1936 "HYBRID_HPD_F")
  (net 1937 "HYBRID_PRG_TP")
  (net 1938 "NET0016")
  (net 1939 "I2CS_SDA_R")
  (net 1940 "HYBRID_HPD_DVICD_DP")
  (net 1941 "I2CS_SCL_R")
  (net 1942 "HYBRID_HPD_DVIAB")
  (net 1943 "NET0017")
  (net 1944 "NET0018")
  (net 1945 "I2C1_SDA_UC")
  (net 1946 "PEX_RST*")
  (net 1947 "SNN_U4_FAN_PWM_PIN5")
  (net 1948 "NET0019")
  (net 1949 "I2C2_SDA_UC")
  (net 1950 "SNN_TV_NC5")
  (net 1951 "DACB_Y_F")
  (net 1952 "SNN_TV_NC7")
  (net 1953 "DACB_PR_F")
  (net 1954 "DACB_PB_F")
  (net 1955 "GPU_RST_RC*")
  (net 1956 "SPDIF_IN")
  (net 1957 "SPDIF_IN_COMP2_Q")
  (net 1958 "PS1_1V15_FB")
  (net 1959 "PS1_1V15_FB_RC")
  (net 1960 "PS1_1V15_FB_SEN")
  (net 1961 "PS1_1V15_BOOT")
  (net 1962 "PS1_1V15_CP")
  (net 1963 "PS1_2V5_LDO_DR")
  (net 1964 "PS1_1V15_UG")
  (net 1965 "PS3_FBVDDQ_CP")
  (net 1966 "PS3_LDO_RC")
  (net 1967 "PS3_FBVDDQ_UG")
  (net 1968 "PS3_FBVDDQ_LG")
  (net 1969 "JTAG_TDI")
  (net 1970 "JTAG_TDO")
  (net 1971 "PEX_PLLVDD_OP_ADJ")
  (net 1972 "PEX_PLLVDD_OP")
  (net 1973 "FAN_PWM")
  (net 1974 "THERM_PWM_ADDR_EN*")
  (net 1975 "FAN_TACH")
  (net 1976 "SNN_TACH2")
  (net 1977 "SNN_7473_2")
  (net 1978 "PS3_FBVDDQ_FB_RC")
  (net 1979 "FAN_PWM_NVIO_R")
  (net 1980 "THERM_LATCH")
  (net 1981 "THERM_SHDN")
  (net 1982 "GPU_RST_R_MOS")
  (net 1983 "VID_PSI")
  (net 1984 "PS5_NVVDD_EN_12V_F2")
  (net 1985 "PS5_NVVDD_EN_12V_F")
  (net 1986 "GPIO1_DVICD_HPD_R")
  (net 1987 "GPIO0_DVIAB_HPD_R")
  (net 1988 "FAN_CUTOFF_RC_Q")
  (net 1989 "PS5_NVVDD_EN*")
  (net 1990 "PS3_NVVDD_PGOOD*")
  (net 1991 "SPDIF_IN_C")
  (net 1992 "SPDIF_IN_R")
  (net 1993 "SPDIF_IN_COMP2_D")
  (net 1994 "THERM_SHDN_D*")
  (net 1995 "PS1_1V15_EN*")
  (net 1996 "PS1_1V15_CP_RC")
  (net 1997 "THERM_SHDN_R")
  (net 1998 "THERM_SHDN_Q")
  (net 1999 "I2C2_SDA_R")
  (net 2000 "I2C2_SCL_R")
  (net 2001 "I2C1_SCL_R")
  (net 2002 "I2C1_SDA_R")
  (net 2003 "PS5_NVVDD_PGOOD_R")
  (net 2004 "JTAG_TRST2")
  (net 2005 "JTAG_TRST_3V3")
  (net 2006 "DACC_HSYNC_BUF_R")
  (net 2007 "DACC_HSYNC_BUF")
  (net 2008 "DACA_HSYNC_BUF_R")
  (net 2009 "DACA_HSYNC_BUF")
  (net 2010 "DACA_VSYNC_BUF_R")
  (net 2011 "DACA_VSYNC_BUF")
  (net 2012 "DACC_VSYNC_BUF_R")
  (net 2013 "DACC_VSYNC_BUF")
  (net 2014 "FBC1_CLK0_R")
  (net 2015 "FBB1_CLK0_R")
  (net 2016 "FBA1_CLK0_R")
  (net 2017 "FBC0_CLK0_R")
  (net 2018 "FBB0_CLK0_R")
  (net 2019 "FBA0_CLK0_R")
  (net 2020 "FBD0_CLK0_R")
  (net 2021 "FBD1_CLK0_R")
  (net 2022 "FBE0_CLK0_R")
  (net 2023 "FBE1_CLK0_R")
  (net 2024 "FBF0_CLK0_R")
  (net 2025 "FBF1_CLK0_R")
  (net 2026 "FBG0_CLK0_R")
  (net 2027 "FBG1_CLK0_R")
  (net 2028 "3V3_AUX")
  (net 2029 "PEX_TX_C0*")
  (net 2030 "PEX_TX_C1*")
  (net 2031 "PEX_TX_C10*")
  (net 2032 "PEX_TX_C11*")
  (net 2033 "PEX_TX_C12*")
  (net 2034 "PEX_TX_C13*")
  (net 2035 "PEX_TX_C14*")
  (net 2036 "PEX_TX_C15*")
  (net 2037 "PEX_TX_C2*")
  (net 2038 "PEX_TX_C3*")
  (net 2039 "PEX_TX_C4*")
  (net 2040 "PEX_TX_C5*")
  (net 2041 "PEX_TX_C6*")
  (net 2042 "PEX_TX_C7*")
  (net 2043 "PEX_TX_C8*")
  (net 2044 "PEX_TX_C9*")
  (net 2045 "PEX_TX_C0")
  (net 2046 "PEX_TX_C1")
  (net 2047 "PEX_TX_C10")
  (net 2048 "PEX_TX_C11")
  (net 2049 "PEX_TX_C12")
  (net 2050 "PEX_TX_C13")
  (net 2051 "PEX_TX_C14")
  (net 2052 "PEX_TX_C15")
  (net 2053 "PEX_TX_C2")
  (net 2054 "PEX_TX_C3")
  (net 2055 "PEX_TX_C4")
  (net 2056 "PEX_TX_C5")
  (net 2057 "PEX_TX_C6")
  (net 2058 "PEX_TX_C7")
  (net 2059 "PEX_TX_C8")
  (net 2060 "PEX_TX_C9")
  (net 2061 "PEX_PRSNT1*")
  (net 2062 "SNN_PEX_20")
  (net 2063 "SNN_PEX_11")
  (net 2064 "SNN_PEX_15")
  (net 2065 "SNN_PEX_10")
  (net 2066 "SNN_PEX_12")
  (net 2067 "SNN_PEX_13")
  (net 2068 "SNN_PEX_14")
  (net 2069 "SNN_PEX_16")
  (net 2070 "SNN_PEX_17")
  (net 2071 "SNN_PEX_18")
  (net 2072 "SNN_PEX_I2CS_SCL")
  (net 2073 "SNN_PEX_I2CS_SDA")
  (net 2074 "SNN_PEX_TCK")
  (net 2075 "SNN_PEX_TDI")
  (net 2076 "SNN_PEX_TDO")
  (net 2077 "SNN_PEX_TMS")
  (net 2078 "SNN_PEX_TRST*")
  (net 2079 "SNN_PEX_08")
  (net 2080 "SPDIF_GND")
  (net 2081 "PS5_NVVDD_EN_Q")
  (net 2082 "PS5_NVVDD_FB_RC")
  (net 2083 "PS5_NVVDD_LG1_D")
  (net 2084 "PS5_NVVDD_LG3_D")
  (net 2085 "PS5_NVVDD_LG4_D")
  (net 2086 "PS5_NVVDD_LG6_D")
  (net 2087 "PS5_NVVDD_LG5_D")
  (net 2088 "PS5_NVVDD_LG2_D")
  (net 2089 "PS3_FBVDDQ_LG_D")
  (net 2090 "I2C4_SDA_R")
  (net 2091 "SNN_HDCP_NC")
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 161.607315 116.307812)
    (fp_text reference "C84" (at -0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 72.812013 124.994815)
    (fp_text reference "C45" (at -0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 75.358313 69.681997 -90)
    (fp_text reference "C51" (at 0 0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 4.023708 142.343015 -90)
    (fp_text reference "C4" (at 0 0.635 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1934 "DACC_VSYNC_CON"))
    (pad "2" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "GEOM0022_1" (layer "F.Cu")
    (tedit 0)
    (at 249.463908 80.645907)
    (fp_text reference "MEC19" (at -1.5875 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 3.5814 3.5814) (drill 3.175) (layers *.Cu *.Mask)
      (net 1 "GND"))
  )
  (footprint "1206_1" (layer "F.Cu")
    (tedit 0)
    (at 233.284108 76.010407)
    (fp_text reference "C136" (at -1.0795 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -1.4732 0) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 981 "12V_PEX6_F1"))
    (pad "2" smd rect (at 1.4732 0) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "1206_1" (layer "F.Cu")
    (tedit 0)
    (at 225.156413 131.141615 -90)
    (fp_text reference "C129" (at 0 1.0795 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -1.4732 0 270) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 983 "12V_PEX6_F2"))
    (pad "2" smd rect (at 1.4732 0 270) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "CAP_TH_D080P035_1" (layer "F.Cu")
    (tedit 0)
    (at 243.434431 86.567409 90)
    (fp_text reference "C143" (at -1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 -1.750111 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 981 "12V_PEX6_F1"))
    (pad "2" thru_hole circle (at 0 1.750085 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 4.684108 111.786815 180)
    (fp_text reference "R2" (at 0.635 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1796 "GPIO1_DVICD_HPD"))
    (pad "2" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "GEOM0005_1" (layer "F.Cu")
    (tedit 0)
    (at 67.071613 118.263815 90)
    (fp_text reference "M4" (at -0.635 1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "A1" smd circle (at -4.400601 -6.4008 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "A2" smd circle (at -3.600399 -6.4008 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "A3" smd circle (at -2.800299 -6.4008 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "A4" smd circle (at -2.000301 -6.4008 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 174 "FBG_ZQ2"))
    (pad "A9" smd circle (at 2.000301 -6.4008 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "A10" smd circle (at 2.800299 -6.4008 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "A11" smd circle (at 3.600399 -6.4008 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "A12" smd circle (at 4.400601 -6.4008 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "B1" smd circle (at -4.400601 -5.6007 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B2" smd circle (at -3.600399 -5.6007 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 175 "FBG_D<58>"))
    (pad "B3" smd circle (at -2.800299 -5.6007 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 176 "FBG_D<63>"))
    (pad "B4" smd circle (at -2.000301 -5.6007 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B9" smd circle (at 2.000301 -5.6007 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B10" smd circle (at 2.800299 -5.6007 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 187 "FBG_D<48>"))
    (pad "B11" smd circle (at 3.600399 -5.6007 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 186 "FBG_D<51>"))
    (pad "B12" smd circle (at 4.400601 -5.6007 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "C1" smd circle (at -4.400601 -4.8006 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "C2" smd circle (at -3.600399 -4.8006 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 177 "FBG_D<57>"))
    (pad "C3" smd circle (at -2.800299 -4.8006 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 178 "FBG_D<62>"))
    (pad "C4" smd circle (at -2.000301 -4.8006 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "C9" smd circle (at 2.000301 -4.8006 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "C10" smd circle (at 2.800299 -4.8006 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 189 "FBG_D<49>"))
    (pad "C11" smd circle (at 3.600399 -4.8006 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 188 "FBG_D<50>"))
    (pad "C12" smd circle (at 4.400601 -4.8006 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "D1" smd circle (at -4.400601 -4.0005 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "D2" smd circle (at -3.600399 -4.0005 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 185 "FBG_DQS_WP7"))
    (pad "D3" smd circle (at -2.800299 -4.0005 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 184 "FBG_DQS_RN7"))
    (pad "D4" smd circle (at -2.000301 -4.0005 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "D9" smd circle (at 2.000301 -4.0005 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "D10" smd circle (at 2.800299 -4.0005 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 195 "FBG_DQS_RN6"))
    (pad "D11" smd circle (at 3.600399 -4.0005 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 196 "FBG_DQS_WP6"))
    (pad "D12" smd circle (at 4.400601 -4.0005 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "E1" smd circle (at -4.400601 -3.2004 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "E2" smd circle (at -3.600399 -3.2004 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 179 "FBG_D<60>"))
    (pad "E3" smd circle (at -2.800299 -3.2004 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 183 "FBG_DQM7"))
    (pad "E4" smd circle (at -2.000301 -3.2004 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "E9" smd circle (at 2.000301 -3.2004 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "E10" smd circle (at 2.800299 -3.2004 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 194 "FBG_DQM6"))
    (pad "E11" smd circle (at 3.600399 -3.2004 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 190 "FBG_D<53>"))
    (pad "E12" smd circle (at 4.400601 -3.2004 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "F1" smd circle (at -4.400601 -2.4003 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "F2" smd circle (at -3.600399 -2.4003 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 181 "FBG_D<59>"))
    (pad "F3" smd circle (at -2.800299 -2.4003 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 180 "FBG_D<56>"))
    (pad "F4" smd circle (at -2.000301 -2.4003 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 108 "FBG_CMD<16>"))
    (pad "F9" smd circle (at 2.000301 -2.4003 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 104 "FBG_CMD<17>"))
    (pad "F10" smd circle (at 2.800299 -2.4003 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 191 "FBG_D<54>"))
    (pad "F11" smd circle (at 3.600399 -2.4003 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 192 "FBG_D<52>"))
    (pad "F12" smd circle (at 4.400601 -2.4003 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "G1" smd circle (at -4.400601 -1.6002 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "G2" smd circle (at -3.600399 -1.6002 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "G3" smd circle (at -2.800299 -1.6002 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 182 "FBG_D<61>"))
    (pad "G4" smd circle (at -2.000301 -1.6002 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 102 "FBG_CMD<11>"))
    (pad "G9" smd circle (at 2.000301 -1.6002 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 101 "FBG_CMD<15>"))
    (pad "G10" smd circle (at 2.800299 -1.6002 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 193 "FBG_D<55>"))
    (pad "G11" smd circle (at 3.600399 -1.6002 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "G12" smd circle (at 4.400601 -1.6002 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "H1" smd circle (at -4.400601 -0.8001 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 172 "FBG_VREF3"))
    (pad "H2" smd circle (at -3.600399 -0.8001 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 164 "FBG_CMD<28>"))
    (pad "H3" smd circle (at -2.800299 -0.8001 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 103 "FBG_CMD<8>"))
    (pad "H4" smd circle (at -2.000301 -0.8001 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 116 "FBG_CMD<7>"))
    (pad "H9" smd circle (at 2.000301 -0.8001 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 105 "FBG_CMD<6>"))
    (pad "H10" smd circle (at 2.800299 -0.8001 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 109 "FBG_CMD<14>"))
    (pad "H11" smd circle (at 3.600399 -0.8001 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 93 "FBG_CMD<12>"))
    (pad "H12" smd circle (at 4.400601 -0.8001 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 173 "FBG_VREF4"))
    (pad "J1" smd circle (at -4.400601 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "J2" smd circle (at -3.600399 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 170 "SNN_FBG_NC04"))
    (pad "J3" smd circle (at -2.800299 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 112 "FBG_CMD<13>"))
    (pad "J4" smd circle (at -2.000301 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "J9" smd circle (at 2.000301 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "J10" smd circle (at 2.800299 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 169 "FBG1_CLK0*"))
    (pad "J11" smd circle (at 3.600399 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 168 "FBG1_CLK0"))
    (pad "J12" smd circle (at 4.400601 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "K1" smd circle (at -4.400601 0.8001 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "K2" smd circle (at -3.600399 0.8001 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 89 "FBG_CMD<19>"))
    (pad "K3" smd circle (at -2.800299 0.8001 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 165 "FBG_CMD<26>"))
    (pad "K4" smd circle (at -2.000301 0.8001 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 162 "FBG_CMD<25>"))
    (pad "K9" smd circle (at 2.000301 0.8001 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 90 "FBG_CMD<21>"))
    (pad "K10" smd circle (at 2.800299 0.8001 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 166 "FBG_CMD<23>"))
    (pad "K11" smd circle (at 3.600399 0.8001 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 91 "FBG_CMD<9>"))
    (pad "K12" smd circle (at 4.400601 0.8001 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "L1" smd circle (at -4.400601 1.6002 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "L2" smd circle (at -3.600399 1.6002 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "L3" smd circle (at -2.800299 1.6002 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 209 "FBG_D<45>"))
    (pad "L4" smd circle (at -2.000301 1.6002 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 163 "FBG_CMD<27>"))
    (pad "L9" smd circle (at 2.000301 1.6002 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 92 "FBG_CMD<20>"))
    (pad "L10" smd circle (at 2.800299 1.6002 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 198 "FBG_D<39>"))
    (pad "L11" smd circle (at 3.600399 1.6002 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "L12" smd circle (at 4.400601 1.6002 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "M1" smd circle (at -4.400601 2.4003 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "M2" smd circle (at -3.600399 2.4003 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 208 "FBG_D<46>"))
    (pad "M3" smd circle (at -2.800299 2.4003 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 211 "FBG_D<47>"))
    (pad "M4" smd circle (at -2.000301 2.4003 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 100 "FBG_CMD<18>"))
    (pad "M9" smd circle (at 2.000301 2.4003 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 167 "FBG_CMD<24>"))
    (pad "M10" smd circle (at 2.800299 2.4003 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 200 "FBG_D<36>"))
    (pad "M11" smd circle (at 3.600399 2.4003 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 197 "FBG_D<37>"))
    (pad "M12" smd circle (at 4.400601 2.4003 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N1" smd circle (at -4.400601 3.2004 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N2" smd circle (at -3.600399 3.2004 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 210 "FBG_D<44>"))
    (pad "N3" smd circle (at -2.800299 3.2004 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 216 "FBG_DQM5"))
    (pad "N4" smd circle (at -2.000301 3.2004 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N9" smd circle (at 2.000301 3.2004 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N10" smd circle (at 2.800299 3.2004 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 205 "FBG_DQM4"))
    (pad "N11" smd circle (at 3.600399 3.2004 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 199 "FBG_D<33>"))
    (pad "N12" smd circle (at 4.400601 3.2004 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "P1" smd circle (at -4.400601 4.0005 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "P2" smd circle (at -3.600399 4.0005 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 218 "FBG_DQS_WP5"))
    (pad "P3" smd circle (at -2.800299 4.0005 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 217 "FBG_DQS_RN5"))
    (pad "P4" smd circle (at -2.000301 4.0005 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "P9" smd circle (at 2.000301 4.0005 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "P10" smd circle (at 2.800299 4.0005 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 206 "FBG_DQS_RN4"))
    (pad "P11" smd circle (at 3.600399 4.0005 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 207 "FBG_DQS_WP4"))
    (pad "P12" smd circle (at 4.400601 4.0005 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "R1" smd circle (at -4.400601 4.8006 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "R2" smd circle (at -3.600399 4.8006 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 212 "FBG_D<40>"))
    (pad "R3" smd circle (at -2.800299 4.8006 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 213 "FBG_D<43>"))
    (pad "R4" smd circle (at -2.000301 4.8006 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "R9" smd circle (at 2.000301 4.8006 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "R10" smd circle (at 2.800299 4.8006 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 202 "FBG_D<34>"))
    (pad "R11" smd circle (at 3.600399 4.8006 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 201 "FBG_D<32>"))
    (pad "R12" smd circle (at 4.400601 4.8006 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "T1" smd circle (at -4.400601 5.6007 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T2" smd circle (at -3.600399 5.6007 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 214 "FBG_D<41>"))
    (pad "T3" smd circle (at -2.800299 5.6007 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 215 "FBG_D<42>"))
    (pad "T4" smd circle (at -2.000301 5.6007 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T9" smd circle (at 2.000301 5.6007 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T10" smd circle (at 2.800299 5.6007 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 204 "FBG_D<38>"))
    (pad "T11" smd circle (at 3.600399 5.6007 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 203 "FBG_D<35>"))
    (pad "T12" smd circle (at 4.400601 5.6007 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "V1" smd circle (at -4.400601 6.4008 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "V2" smd circle (at -3.600399 6.4008 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "V3" smd circle (at -2.800299 6.4008 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "V4" smd circle (at -2.000301 6.4008 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 171 "FBG_SEN2"))
    (pad "V9" smd circle (at 2.000301 6.4008 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 110 "FBG_CMD<10>"))
    (pad "V10" smd circle (at 2.800299 6.4008 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "V11" smd circle (at 3.600399 6.4008 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "V12" smd circle (at 4.400601 6.4008 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 75.376118 98.299415 90)
    (fp_text reference "C52" (at 0 -0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "1206_1" (layer "F.Cu")
    (tedit 0)
    (at 46.314708 134.747907 90)
    (fp_text reference "C33" (at 0 -0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -1.4732 0 90) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 991 "12V_F"))
    (pad "2" smd rect (at 1.4732 0 90) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "1206_1" (layer "F.Cu")
    (tedit 0)
    (at 208.138108 65.342407 -90)
    (fp_text reference "R66" (at 0 0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -1.4732 0 270) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "INPUT_PEX6_IN1"))
    (pad "2" smd rect (at 1.4732 0 270) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 981 "12V_PEX6_F1"))
  )
  (footprint "SOT23_1" (layer "F.Cu")
    (tedit 0)
    (at 8.189308 141.504815 90)
    (fp_text reference "D6" (at -0.635 1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.9525 1.143 90) (size 0.9144 0.9144) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "2" smd rect (at 0.9525 1.143 90) (size 0.9144 0.9144) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1914 "5V"))
    (pad "3" smd rect (at 0 -1.143 90) (size 0.9144 0.9144) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2013 "DACC_VSYNC_BUF"))
  )
  (footprint "GEOM0023_1" (layer "F.Cu")
    (tedit 0)
    (at 146.924108 142.825615)
    (fp_text reference "MEC13" (at -1.5875 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 3.5814 3.5814) (drill 2.4892) (layers *.Cu *.Mask)
      (net 1 "GND"))
  )
  (footprint "GEOM0018_1" (layer "F.Cu")
    (tedit 0)
    (at -1.589692 88.037612 -90)
    (fp_text reference "J2" (at 2.099945 -8.89 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole rect (at 0 0 270) (size 1.2192 1.2192) (drill 0.8636) (layers *.Cu *.Mask)
      (net 1733 "IFPC_TXD2*"))
    (pad "2" thru_hole rect (at 1.905 0 270) (size 1.2192 1.2192) (drill 0.8636) (layers *.Cu *.Mask)
      (net 1732 "IFPC_TXD2"))
    (pad "3" thru_hole rect (at 3.81 0 270) (size 1.2192 1.2192) (drill 0.8636) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "4" thru_hole rect (at 5.715 0 270) (size 1.2192 1.2192) (drill 0.8636) (layers *.Cu *.Mask)
      (net 1741 "IFPD_TXD5*"))
    (pad "5" thru_hole rect (at 7.62 0 270) (size 1.2192 1.2192) (drill 0.8636) (layers *.Cu *.Mask)
      (net 1740 "IFPD_TXD5"))
    (pad "6" thru_hole rect (at 9.525 0 270) (size 1.2192 1.2192) (drill 0.8636) (layers *.Cu *.Mask)
      (net 1919 "I2C1_SCL_CON"))
    (pad "7" thru_hole rect (at 11.43 0 270) (size 1.2192 1.2192) (drill 0.8636) (layers *.Cu *.Mask)
      (net 1920 "I2C1_SDA_CON"))
    (pad "8" thru_hole rect (at 13.335 0 270) (size 1.2192 1.2192) (drill 0.8636) (layers *.Cu *.Mask)
      (net 1926 "DACA_VSYNC_CON"))
    (pad "9" thru_hole rect (at 0 1.905 270) (size 1.2192 1.2192) (drill 0.8636) (layers *.Cu *.Mask)
      (net 1731 "IFPC_TXD1*"))
    (pad "10" thru_hole rect (at 1.905 1.905 270) (size 1.2192 1.2192) (drill 0.8636) (layers *.Cu *.Mask)
      (net 1730 "IFPC_TXD1"))
    (pad "11" thru_hole rect (at 3.81 1.905 270) (size 1.2192 1.2192) (drill 0.8636) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "12" thru_hole rect (at 5.715 1.905 270) (size 1.2192 1.2192) (drill 0.8636) (layers *.Cu *.Mask)
      (net 1739 "IFPD_TXD4*"))
    (pad "13" thru_hole rect (at 7.62 1.905 270) (size 1.2192 1.2192) (drill 0.8636) (layers *.Cu *.Mask)
      (net 1738 "IFPD_TXD4"))
    (pad "14" thru_hole rect (at 9.525 1.905 270) (size 1.2192 1.2192) (drill 0.8636) (layers *.Cu *.Mask)
      (net 1925 "DDC_5V"))
    (pad "15" thru_hole rect (at 11.43 1.905 270) (size 1.2192 1.2192) (drill 0.8636) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "16" thru_hole rect (at 13.335 1.905 270) (size 1.2192 1.2192) (drill 0.8636) (layers *.Cu *.Mask)
      (net 1922 "GPIO1_DVICD_HPD_CON"))
    (pad "17" thru_hole rect (at 0 3.81 270) (size 1.2192 1.2192) (drill 0.8636) (layers *.Cu *.Mask)
      (net 1729 "IFPC_TXD0*"))
    (pad "18" thru_hole rect (at 1.905 3.81 270) (size 1.2192 1.2192) (drill 0.8636) (layers *.Cu *.Mask)
      (net 1728 "IFPC_TXD0"))
    (pad "19" thru_hole rect (at 3.81 3.81 270) (size 1.2192 1.2192) (drill 0.8636) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "20" thru_hole rect (at 5.715 3.81 270) (size 1.2192 1.2192) (drill 0.8636) (layers *.Cu *.Mask)
      (net 1743 "IFPD_TXD6*"))
    (pad "21" thru_hole rect (at 7.62 3.81 270) (size 1.2192 1.2192) (drill 0.8636) (layers *.Cu *.Mask)
      (net 1742 "IFPD_TXD6"))
    (pad "22" thru_hole rect (at 9.525 3.81 270) (size 1.2192 1.2192) (drill 0.8636) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "23" thru_hole rect (at 11.43 3.81 270) (size 1.2192 1.2192) (drill 0.8636) (layers *.Cu *.Mask)
      (net 1726 "IFPC_TXC"))
    (pad "24" thru_hole rect (at 13.335 3.81 270) (size 1.2192 1.2192) (drill 0.8636) (layers *.Cu *.Mask)
      (net 1727 "IFPC_TXC*"))
    (pad "25" thru_hole circle (at -6.3754 5.334 79.7) (size 4.191 4.191) (drill 3.175) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "26" thru_hole circle (at 25.4254 5.334 280.2) (size 4.191 4.191) (drill 3.175) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "27" thru_hole circle (at -3.9751 -2.15011 270) (size 2.159 2.159) (drill 1.397) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "28" thru_hole circle (at 5.862599 -2.067611 270) (size 2.159 2.159) (drill 1.7272) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "29" thru_hole circle (at 12.932385 -2.067611 270) (size 2.159 2.159) (drill 1.7272) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "30" thru_hole circle (at 23.024795 -2.15011 270) (size 2.159 2.159) (drill 1.397) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "31" thru_hole circle (at -5.842 3.81 270) (size 3.048 3.048) (drill 1.9304) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "32" thru_hole circle (at 24.892 3.81 270) (size 3.048 3.048) (drill 1.9304) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "C1" thru_hole circle (at 16.515105 0.632511 270) (size 1.27 1.27) (drill 0.6604) (layers *.Cu *.Mask)
      (net 1924 "DACA_RED_CON"))
    (pad "C2" thru_hole circle (at 19.055105 0.632511 270) (size 1.27 1.27) (drill 0.6604) (layers *.Cu *.Mask)
      (net 1921 "DACA_GREEN_CON"))
    (pad "C3" thru_hole circle (at 16.515105 3.172511 270) (size 1.27 1.27) (drill 0.6604) (layers *.Cu *.Mask)
      (net 1918 "DACA_BLUE_CON"))
    (pad "C4" thru_hole circle (at 19.055105 3.172511 270) (size 1.27 1.27) (drill 0.6604) (layers *.Cu *.Mask)
      (net 1923 "DACA_HSYNC_CON"))
    (pad "C5" thru_hole circle (at 17.785105 4.439895 270) (size 1.27 1.27) (drill 0.6604) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "C5A" thru_hole circle (at 17.785105 -0.640105 270) (size 1.27 1.27) (drill 0.6604) (layers *.Cu *.Mask)
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 242.491608 95.504907 -90)
    (fp_text reference "R76" (at 0 0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1983 "VID_PSI"))
  )
  (footprint "1206_1" (layer "F.Cu")
    (tedit 0)
    (at 225.156413 144.018907 -90)
    (fp_text reference "C130" (at 0 1.0795 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -1.4732 0 270) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 983 "12V_PEX6_F2"))
    (pad "2" smd rect (at 1.4732 0 270) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "GEOM0005_1" (layer "F.Cu")
    (tedit 0)
    (at 167.879108 109.551615 -90)
    (fp_text reference "M12" (at 1.27 -1.5875 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "A1" smd circle (at -4.400601 -6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "A2" smd circle (at -3.600399 -6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "A3" smd circle (at -2.800299 -6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "A4" smd circle (at -2.000301 -6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 751 "FBB_ZQ1"))
    (pad "A9" smd circle (at 2.000301 -6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "A10" smd circle (at 2.800299 -6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "A11" smd circle (at 3.600399 -6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "A12" smd circle (at 4.400601 -6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "B1" smd circle (at -4.400601 -5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B2" smd circle (at -3.600399 -5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 752 "FBB_D<16>"))
    (pad "B3" smd circle (at -2.800299 -5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 753 "FBB_D<17>"))
    (pad "B4" smd circle (at -2.000301 -5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B9" smd circle (at 2.000301 -5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B10" smd circle (at 2.800299 -5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 764 "FBB_D<6>"))
    (pad "B11" smd circle (at 3.600399 -5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 763 "FBB_D<0>"))
    (pad "B12" smd circle (at 4.400601 -5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "C1" smd circle (at -4.400601 -4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "C2" smd circle (at -3.600399 -4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 754 "FBB_D<18>"))
    (pad "C3" smd circle (at -2.800299 -4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 755 "FBB_D<19>"))
    (pad "C4" smd circle (at -2.000301 -4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "C9" smd circle (at 2.000301 -4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "C10" smd circle (at 2.800299 -4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 766 "FBB_D<5>"))
    (pad "C11" smd circle (at 3.600399 -4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 765 "FBB_D<1>"))
    (pad "C12" smd circle (at 4.400601 -4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "D1" smd circle (at -4.400601 -4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "D2" smd circle (at -3.600399 -4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 762 "FBB_DQS_WP2"))
    (pad "D3" smd circle (at -2.800299 -4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 761 "FBB_DQS_RN2"))
    (pad "D4" smd circle (at -2.000301 -4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "D9" smd circle (at 2.000301 -4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "D10" smd circle (at 2.800299 -4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 772 "FBB_DQS_RN0"))
    (pad "D11" smd circle (at 3.600399 -4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 773 "FBB_DQS_WP0"))
    (pad "D12" smd circle (at 4.400601 -4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "E1" smd circle (at -4.400601 -3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "E2" smd circle (at -3.600399 -3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 756 "FBB_D<20>"))
    (pad "E3" smd circle (at -2.800299 -3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 760 "FBB_DQM2"))
    (pad "E4" smd circle (at -2.000301 -3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "E9" smd circle (at 2.000301 -3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "E10" smd circle (at 2.800299 -3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 771 "FBB_DQM0"))
    (pad "E11" smd circle (at 3.600399 -3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 767 "FBB_D<2>"))
    (pad "E12" smd circle (at 4.400601 -3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "F1" smd circle (at -4.400601 -2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "F2" smd circle (at -3.600399 -2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 758 "FBB_D<21>"))
    (pad "F3" smd circle (at -2.800299 -2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 757 "FBB_D<22>"))
    (pad "F4" smd circle (at -2.000301 -2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 685 "FBB_CMD<17>"))
    (pad "F9" smd circle (at 2.000301 -2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 681 "FBB_CMD<16>"))
    (pad "F10" smd circle (at 2.800299 -2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 768 "FBB_D<4>"))
    (pad "F11" smd circle (at 3.600399 -2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 769 "FBB_D<3>"))
    (pad "F12" smd circle (at 4.400601 -2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "G1" smd circle (at -4.400601 -1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "G2" smd circle (at -3.600399 -1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "G3" smd circle (at -2.800299 -1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 759 "FBB_D<23>"))
    (pad "G4" smd circle (at -2.000301 -1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 679 "FBB_CMD<15>"))
    (pad "G9" smd circle (at 2.000301 -1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 678 "FBB_CMD<11>"))
    (pad "G10" smd circle (at 2.800299 -1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 770 "FBB_D<7>"))
    (pad "G11" smd circle (at 3.600399 -1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "G12" smd circle (at 4.400601 -1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "H1" smd circle (at -4.400601 -0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 749 "FBB_VREF1"))
    (pad "H2" smd circle (at -3.600399 -0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 674 "FBB_CMD<12>"))
    (pad "H3" smd circle (at -2.800299 -0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 680 "FBB_CMD<14>"))
    (pad "H4" smd circle (at -2.000301 -0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 693 "FBB_CMD<6>"))
    (pad "H9" smd circle (at 2.000301 -0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 682 "FBB_CMD<7>"))
    (pad "H10" smd circle (at 2.800299 -0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 686 "FBB_CMD<8>"))
    (pad "H11" smd circle (at 3.600399 -0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 742 "FBB_CMD<0>"))
    (pad "H12" smd circle (at 4.400601 -0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 750 "FBB_VREF2"))
    (pad "J1" smd circle (at -4.400601 0 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "J2" smd circle (at -3.600399 0 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 747 "SNN_FBB_NC01"))
    (pad "J3" smd circle (at -2.800299 0 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 689 "FBB_CMD<13>"))
    (pad "J4" smd circle (at -2.000301 0 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "J9" smd circle (at 2.000301 0 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "J10" smd circle (at 2.800299 0 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 746 "FBB0_CLK0*"))
    (pad "J11" smd circle (at 3.600399 0 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 745 "FBB0_CLK0"))
    (pad "J12" smd circle (at 4.400601 0 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "K1" smd circle (at -4.400601 0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "K2" smd circle (at -3.600399 0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 666 "FBB_CMD<9>"))
    (pad "K3" smd circle (at -2.800299 0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 739 "FBB_CMD<5>"))
    (pad "K4" smd circle (at -2.000301 0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 673 "FBB_CMD<21>"))
    (pad "K9" smd circle (at 2.000301 0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 741 "FBB_CMD<3>"))
    (pad "K10" smd circle (at 2.800299 0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 743 "FBB_CMD<2>"))
    (pad "K11" smd circle (at 3.600399 0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 668 "FBB_CMD<19>"))
    (pad "K12" smd circle (at 4.400601 0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "L1" smd circle (at -4.400601 1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "L2" smd circle (at -3.600399 1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "L3" smd circle (at -2.800299 1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 786 "FBB_D<8>"))
    (pad "L4" smd circle (at -2.000301 1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 676 "FBB_CMD<20>"))
    (pad "L9" smd circle (at 2.000301 1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 744 "FBB_CMD<1>"))
    (pad "L10" smd circle (at 2.800299 1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 775 "FBB_D<26>"))
    (pad "L11" smd circle (at 3.600399 1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "L12" smd circle (at 4.400601 1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "M1" smd circle (at -4.400601 2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "M2" smd circle (at -3.600399 2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 785 "FBB_D<12>"))
    (pad "M3" smd circle (at -2.800299 2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 788 "FBB_D<10>"))
    (pad "M4" smd circle (at -2.000301 2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 740 "FBB_CMD<4>"))
    (pad "M9" smd circle (at 2.000301 2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 672 "FBB_CMD<18>"))
    (pad "M10" smd circle (at 2.800299 2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 777 "FBB_D<27>"))
    (pad "M11" smd circle (at 3.600399 2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 774 "FBB_D<25>"))
    (pad "M12" smd circle (at 4.400601 2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N1" smd circle (at -4.400601 3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N2" smd circle (at -3.600399 3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 787 "FBB_D<9>"))
    (pad "N3" smd circle (at -2.800299 3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 793 "FBB_DQM1"))
    (pad "N4" smd circle (at -2.000301 3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N9" smd circle (at 2.000301 3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N10" smd circle (at 2.800299 3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 782 "FBB_DQM3"))
    (pad "N11" smd circle (at 3.600399 3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 776 "FBB_D<28>"))
    (pad "N12" smd circle (at 4.400601 3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "P1" smd circle (at -4.400601 4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "P2" smd circle (at -3.600399 4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 795 "FBB_DQS_WP1"))
    (pad "P3" smd circle (at -2.800299 4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 794 "FBB_DQS_RN1"))
    (pad "P4" smd circle (at -2.000301 4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "P9" smd circle (at 2.000301 4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "P10" smd circle (at 2.800299 4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 783 "FBB_DQS_RN3"))
    (pad "P11" smd circle (at 3.600399 4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 784 "FBB_DQS_WP3"))
    (pad "P12" smd circle (at 4.400601 4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "R1" smd circle (at -4.400601 4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "R2" smd circle (at -3.600399 4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 789 "FBB_D<13>"))
    (pad "R3" smd circle (at -2.800299 4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 790 "FBB_D<14>"))
    (pad "R4" smd circle (at -2.000301 4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "R9" smd circle (at 2.000301 4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "R10" smd circle (at 2.800299 4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 779 "FBB_D<31>"))
    (pad "R11" smd circle (at 3.600399 4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 778 "FBB_D<24>"))
    (pad "R12" smd circle (at 4.400601 4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "T1" smd circle (at -4.400601 5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T2" smd circle (at -3.600399 5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 791 "FBB_D<15>"))
    (pad "T3" smd circle (at -2.800299 5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 792 "FBB_D<11>"))
    (pad "T4" smd circle (at -2.000301 5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T9" smd circle (at 2.000301 5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T10" smd circle (at 2.800299 5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 781 "FBB_D<30>"))
    (pad "T11" smd circle (at 3.600399 5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 780 "FBB_D<29>"))
    (pad "T12" smd circle (at 4.400601 5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "V1" smd circle (at -4.400601 6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "V2" smd circle (at -3.600399 6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "V3" smd circle (at -2.800299 6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "V4" smd circle (at -2.000301 6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 748 "FBB_SEN1"))
    (pad "V9" smd circle (at 2.000301 6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 687 "FBB_CMD<10>"))
    (pad "V10" smd circle (at 2.800299 6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "V11" smd circle (at 3.600399 6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "V12" smd circle (at 4.400601 6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 70.777702 66.682511)
    (fp_text reference "C42" (at -0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "GEOM0005_1" (layer "F.Cu")
    (tedit 0)
    (at 138.543607 63.780815)
    (fp_text reference "M8" (at 1.27 0.635 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "A1" smd circle (at -4.400601 -6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "A2" smd circle (at -3.600399 -6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "A3" smd circle (at -2.800299 -6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "A4" smd circle (at -2.000301 -6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 491 "FBD_ZQ1"))
    (pad "A9" smd circle (at 2.000301 -6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "A10" smd circle (at 2.800299 -6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "A11" smd circle (at 3.600399 -6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "A12" smd circle (at 4.400601 -6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "B1" smd circle (at -4.400601 -5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B2" smd circle (at -3.600399 -5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 492 "FBD_D<16>"))
    (pad "B3" smd circle (at -2.800299 -5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 493 "FBD_D<18>"))
    (pad "B4" smd circle (at -2.000301 -5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B9" smd circle (at 2.000301 -5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B10" smd circle (at 2.800299 -5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 504 "FBD_D<2>"))
    (pad "B11" smd circle (at 3.600399 -5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 503 "FBD_D<3>"))
    (pad "B12" smd circle (at 4.400601 -5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "C1" smd circle (at -4.400601 -4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "C2" smd circle (at -3.600399 -4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 494 "FBD_D<17>"))
    (pad "C3" smd circle (at -2.800299 -4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 495 "FBD_D<19>"))
    (pad "C4" smd circle (at -2.000301 -4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "C9" smd circle (at 2.000301 -4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "C10" smd circle (at 2.800299 -4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 506 "FBD_D<0>"))
    (pad "C11" smd circle (at 3.600399 -4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 505 "FBD_D<1>"))
    (pad "C12" smd circle (at 4.400601 -4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "D1" smd circle (at -4.400601 -4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "D2" smd circle (at -3.600399 -4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 502 "FBD_DQS_WP2"))
    (pad "D3" smd circle (at -2.800299 -4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 501 "FBD_DQS_RN2"))
    (pad "D4" smd circle (at -2.000301 -4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "D9" smd circle (at 2.000301 -4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "D10" smd circle (at 2.800299 -4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 512 "FBD_DQS_RN0"))
    (pad "D11" smd circle (at 3.600399 -4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 513 "FBD_DQS_WP0"))
    (pad "D12" smd circle (at 4.400601 -4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "E1" smd circle (at -4.400601 -3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "E2" smd circle (at -3.600399 -3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 496 "FBD_D<22>"))
    (pad "E3" smd circle (at -2.800299 -3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 500 "FBD_DQM2"))
    (pad "E4" smd circle (at -2.000301 -3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "E9" smd circle (at 2.000301 -3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "E10" smd circle (at 2.800299 -3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 511 "FBD_DQM0"))
    (pad "E11" smd circle (at 3.600399 -3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 507 "FBD_D<6>"))
    (pad "E12" smd circle (at 4.400601 -3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "F1" smd circle (at -4.400601 -2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "F2" smd circle (at -3.600399 -2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 498 "FBD_D<21>"))
    (pad "F3" smd circle (at -2.800299 -2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 497 "FBD_D<23>"))
    (pad "F4" smd circle (at -2.000301 -2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 425 "FBD_CMD<17>"))
    (pad "F9" smd circle (at 2.000301 -2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 421 "FBD_CMD<16>"))
    (pad "F10" smd circle (at 2.800299 -2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 508 "FBD_D<7>"))
    (pad "F11" smd circle (at 3.600399 -2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 509 "FBD_D<4>"))
    (pad "F12" smd circle (at 4.400601 -2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "G1" smd circle (at -4.400601 -1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "G2" smd circle (at -3.600399 -1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "G3" smd circle (at -2.800299 -1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 499 "FBD_D<20>"))
    (pad "G4" smd circle (at -2.000301 -1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 419 "FBD_CMD<15>"))
    (pad "G9" smd circle (at 2.000301 -1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 418 "FBD_CMD<11>"))
    (pad "G10" smd circle (at 2.800299 -1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 510 "FBD_D<5>"))
    (pad "G11" smd circle (at 3.600399 -1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "G12" smd circle (at 4.400601 -1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "H1" smd circle (at -4.400601 -0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 489 "FBD_VREF1"))
    (pad "H2" smd circle (at -3.600399 -0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 414 "FBD_CMD<12>"))
    (pad "H3" smd circle (at -2.800299 -0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 420 "FBD_CMD<14>"))
    (pad "H4" smd circle (at -2.000301 -0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 433 "FBD_CMD<6>"))
    (pad "H9" smd circle (at 2.000301 -0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 422 "FBD_CMD<7>"))
    (pad "H10" smd circle (at 2.800299 -0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 426 "FBD_CMD<8>"))
    (pad "H11" smd circle (at 3.600399 -0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 482 "FBD_CMD<0>"))
    (pad "H12" smd circle (at 4.400601 -0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 490 "FBD_VREF2"))
    (pad "J1" smd circle (at -4.400601 0) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "J2" smd circle (at -3.600399 0) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 487 "SNN_FBD_NC01"))
    (pad "J3" smd circle (at -2.800299 0) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 429 "FBD_CMD<13>"))
    (pad "J4" smd circle (at -2.000301 0) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "J9" smd circle (at 2.000301 0) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "J10" smd circle (at 2.800299 0) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 486 "FBD0_CLK0*"))
    (pad "J11" smd circle (at 3.600399 0) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 485 "FBD0_CLK0"))
    (pad "J12" smd circle (at 4.400601 0) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "K1" smd circle (at -4.400601 0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "K2" smd circle (at -3.600399 0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 406 "FBD_CMD<9>"))
    (pad "K3" smd circle (at -2.800299 0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 479 "FBD_CMD<5>"))
    (pad "K4" smd circle (at -2.000301 0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 413 "FBD_CMD<21>"))
    (pad "K9" smd circle (at 2.000301 0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 481 "FBD_CMD<3>"))
    (pad "K10" smd circle (at 2.800299 0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 483 "FBD_CMD<2>"))
    (pad "K11" smd circle (at 3.600399 0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 408 "FBD_CMD<19>"))
    (pad "K12" smd circle (at 4.400601 0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "L1" smd circle (at -4.400601 1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "L2" smd circle (at -3.600399 1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "L3" smd circle (at -2.800299 1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 526 "FBD_D<8>"))
    (pad "L4" smd circle (at -2.000301 1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 416 "FBD_CMD<20>"))
    (pad "L9" smd circle (at 2.000301 1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 484 "FBD_CMD<1>"))
    (pad "L10" smd circle (at 2.800299 1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 515 "FBD_D<24>"))
    (pad "L11" smd circle (at 3.600399 1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "L12" smd circle (at 4.400601 1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "M1" smd circle (at -4.400601 2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "M2" smd circle (at -3.600399 2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 525 "FBD_D<9>"))
    (pad "M3" smd circle (at -2.800299 2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 528 "FBD_D<10>"))
    (pad "M4" smd circle (at -2.000301 2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 480 "FBD_CMD<4>"))
    (pad "M9" smd circle (at 2.000301 2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 412 "FBD_CMD<18>"))
    (pad "M10" smd circle (at 2.800299 2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 517 "FBD_D<26>"))
    (pad "M11" smd circle (at 3.600399 2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 514 "FBD_D<25>"))
    (pad "M12" smd circle (at 4.400601 2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N1" smd circle (at -4.400601 3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N2" smd circle (at -3.600399 3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 527 "FBD_D<11>"))
    (pad "N3" smd circle (at -2.800299 3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 533 "FBD_DQM1"))
    (pad "N4" smd circle (at -2.000301 3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N9" smd circle (at 2.000301 3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N10" smd circle (at 2.800299 3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 522 "FBD_DQM3"))
    (pad "N11" smd circle (at 3.600399 3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 516 "FBD_D<27>"))
    (pad "N12" smd circle (at 4.400601 3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "P1" smd circle (at -4.400601 4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "P2" smd circle (at -3.600399 4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 535 "FBD_DQS_WP1"))
    (pad "P3" smd circle (at -2.800299 4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 534 "FBD_DQS_RN1"))
    (pad "P4" smd circle (at -2.000301 4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "P9" smd circle (at 2.000301 4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "P10" smd circle (at 2.800299 4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 523 "FBD_DQS_RN3"))
    (pad "P11" smd circle (at 3.600399 4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 524 "FBD_DQS_WP3"))
    (pad "P12" smd circle (at 4.400601 4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "R1" smd circle (at -4.400601 4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "R2" smd circle (at -3.600399 4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 529 "FBD_D<14>"))
    (pad "R3" smd circle (at -2.800299 4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 530 "FBD_D<15>"))
    (pad "R4" smd circle (at -2.000301 4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "R9" smd circle (at 2.000301 4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "R10" smd circle (at 2.800299 4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 519 "FBD_D<30>"))
    (pad "R11" smd circle (at 3.600399 4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 518 "FBD_D<28>"))
    (pad "R12" smd circle (at 4.400601 4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "T1" smd circle (at -4.400601 5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T2" smd circle (at -3.600399 5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 531 "FBD_D<12>"))
    (pad "T3" smd circle (at -2.800299 5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 532 "FBD_D<13>"))
    (pad "T4" smd circle (at -2.000301 5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T9" smd circle (at 2.000301 5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T10" smd circle (at 2.800299 5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 521 "FBD_D<31>"))
    (pad "T11" smd circle (at 3.600399 5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 520 "FBD_D<29>"))
    (pad "T12" smd circle (at 4.400601 5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "V1" smd circle (at -4.400601 6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "V2" smd circle (at -3.600399 6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "V3" smd circle (at -2.800299 6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "V4" smd circle (at -2.000301 6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 488 "FBD_SEN1"))
    (pad "V9" smd circle (at 2.000301 6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 427 "FBD_CMD<10>"))
    (pad "V10" smd circle (at 2.800299 6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "V11" smd circle (at 3.600399 6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "V12" smd circle (at 4.400601 6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
  )
  (footprint "1206_1" (layer "F.Cu")
    (tedit 0)
    (at 215.377108 65.342407 -90)
    (fp_text reference "R69" (at 0 0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -1.4732 0 270) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "INPUT_PEX6_IN1"))
    (pad "2" smd rect (at 1.4732 0 270) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 981 "12V_PEX6_F1"))
  )
  (footprint "0805_1" (layer "F.Cu")
    (tedit 0)
    (at 51.394708 83.084307)
    (fp_text reference "C38" (at -0.787406 0.000013 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.9525 0) (size 1.143 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at 0.9525 0) (size 1.143 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "SOT23_1" (layer "F.Cu")
    (tedit 0)
    (at 7.579708 137.694815 90)
    (fp_text reference "D4" (at -0.635 1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.9525 1.143 90) (size 0.9144 0.9144) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "2" smd rect (at 0.9525 1.143 90) (size 0.9144 0.9144) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1914 "5V"))
    (pad "3" smd rect (at 0 -1.143 90) (size 0.9144 0.9144) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1999 "I2C2_SDA_R"))
  )
  (footprint "GEOM0005_1" (layer "F.Cu")
    (tedit 0)
    (at 167.879108 64.783607 -90)
    (fp_text reference "M9" (at 0.635 -1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "A1" smd circle (at -4.400601 -6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "A2" smd circle (at -3.600399 -6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "A3" smd circle (at -2.800299 -6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "A4" smd circle (at -2.000301 -6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 564 "FBC_ZQ2"))
    (pad "A9" smd circle (at 2.000301 -6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "A10" smd circle (at 2.800299 -6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "A11" smd circle (at 3.600399 -6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "A12" smd circle (at 4.400601 -6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "B1" smd circle (at -4.400601 -5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B2" smd circle (at -3.600399 -5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 565 "FBC_D<63>"))
    (pad "B3" smd circle (at -2.800299 -5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 566 "FBC_D<61>"))
    (pad "B4" smd circle (at -2.000301 -5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B9" smd circle (at 2.000301 -5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B10" smd circle (at 2.800299 -5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 577 "FBC_D<33>"))
    (pad "B11" smd circle (at 3.600399 -5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 576 "FBC_D<34>"))
    (pad "B12" smd circle (at 4.400601 -5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "C1" smd circle (at -4.400601 -4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "C2" smd circle (at -3.600399 -4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 567 "FBC_D<62>"))
    (pad "C3" smd circle (at -2.800299 -4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 568 "FBC_D<60>"))
    (pad "C4" smd circle (at -2.000301 -4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "C9" smd circle (at 2.000301 -4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "C10" smd circle (at 2.800299 -4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 579 "FBC_D<32>"))
    (pad "C11" smd circle (at 3.600399 -4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 578 "FBC_D<35>"))
    (pad "C12" smd circle (at 4.400601 -4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "D1" smd circle (at -4.400601 -4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "D2" smd circle (at -3.600399 -4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 575 "FBC_DQS_WP7"))
    (pad "D3" smd circle (at -2.800299 -4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 574 "FBC_DQS_RN7"))
    (pad "D4" smd circle (at -2.000301 -4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "D9" smd circle (at 2.000301 -4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "D10" smd circle (at 2.800299 -4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 585 "FBC_DQS_RN4"))
    (pad "D11" smd circle (at 3.600399 -4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 586 "FBC_DQS_WP4"))
    (pad "D12" smd circle (at 4.400601 -4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "E1" smd circle (at -4.400601 -3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "E2" smd circle (at -3.600399 -3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 569 "FBC_D<57>"))
    (pad "E3" smd circle (at -2.800299 -3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 573 "FBC_DQM7"))
    (pad "E4" smd circle (at -2.000301 -3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "E9" smd circle (at 2.000301 -3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "E10" smd circle (at 2.800299 -3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 584 "FBC_DQM4"))
    (pad "E11" smd circle (at 3.600399 -3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 580 "FBC_D<37>"))
    (pad "E12" smd circle (at 4.400601 -3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "F1" smd circle (at -4.400601 -2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "F2" smd circle (at -3.600399 -2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 571 "FBC_D<59>"))
    (pad "F3" smd circle (at -2.800299 -2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 570 "FBC_D<56>"))
    (pad "F4" smd circle (at -2.000301 -2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 551 "FBC_CMD<16>"))
    (pad "F9" smd circle (at 2.000301 -2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 555 "FBC_CMD<17>"))
    (pad "F10" smd circle (at 2.800299 -2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 581 "FBC_D<36>"))
    (pad "F11" smd circle (at 3.600399 -2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 582 "FBC_D<38>"))
    (pad "F12" smd circle (at 4.400601 -2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "G1" smd circle (at -4.400601 -1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "G2" smd circle (at -3.600399 -1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "G3" smd circle (at -2.800299 -1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 572 "FBC_D<58>"))
    (pad "G4" smd circle (at -2.000301 -1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 548 "FBC_CMD<11>"))
    (pad "G9" smd circle (at 2.000301 -1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 549 "FBC_CMD<15>"))
    (pad "G10" smd circle (at 2.800299 -1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 583 "FBC_D<39>"))
    (pad "G11" smd circle (at 3.600399 -1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "G12" smd circle (at 4.400601 -1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "H1" smd circle (at -4.400601 -0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 561 "FBC_VREF3"))
    (pad "H2" smd circle (at -3.600399 -0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 540 "FBC_CMD<28>"))
    (pad "H3" smd circle (at -2.800299 -0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 556 "FBC_CMD<8>"))
    (pad "H4" smd circle (at -2.000301 -0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 552 "FBC_CMD<7>"))
    (pad "H9" smd circle (at 2.000301 -0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 563 "FBC_CMD<6>"))
    (pad "H10" smd circle (at 2.800299 -0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 550 "FBC_CMD<14>"))
    (pad "H11" smd circle (at 3.600399 -0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 544 "FBC_CMD<12>"))
    (pad "H12" smd circle (at 4.400601 -0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 562 "FBC_VREF4"))
    (pad "J1" smd circle (at -4.400601 0 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "J2" smd circle (at -3.600399 0 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 558 "SNN_FBC_NC04"))
    (pad "J3" smd circle (at -2.800299 0 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 559 "FBC_CMD<13>"))
    (pad "J4" smd circle (at -2.000301 0 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "J9" smd circle (at 2.000301 0 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "J10" smd circle (at 2.800299 0 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 554 "FBC1_CLK0*"))
    (pad "J11" smd circle (at 3.600399 0 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 553 "FBC1_CLK0"))
    (pad "J12" smd circle (at 4.400601 0 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "K1" smd circle (at -4.400601 0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "K2" smd circle (at -3.600399 0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 538 "FBC_CMD<19>"))
    (pad "K3" smd circle (at -2.800299 0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 541 "FBC_CMD<26>"))
    (pad "K4" smd circle (at -2.000301 0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 537 "FBC_CMD<25>"))
    (pad "K9" smd circle (at 2.000301 0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 543 "FBC_CMD<21>"))
    (pad "K10" smd circle (at 2.800299 0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 545 "FBC_CMD<23>"))
    (pad "K11" smd circle (at 3.600399 0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 536 "FBC_CMD<9>"))
    (pad "K12" smd circle (at 4.400601 0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "L1" smd circle (at -4.400601 1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "L2" smd circle (at -3.600399 1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "L3" smd circle (at -2.800299 1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 599 "FBC_D<45>"))
    (pad "L4" smd circle (at -2.000301 1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 539 "FBC_CMD<27>"))
    (pad "L9" smd circle (at 2.000301 1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 546 "FBC_CMD<20>"))
    (pad "L10" smd circle (at 2.800299 1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 588 "FBC_D<48>"))
    (pad "L11" smd circle (at 3.600399 1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "L12" smd circle (at 4.400601 1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "M1" smd circle (at -4.400601 2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "M2" smd circle (at -3.600399 2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 598 "FBC_D<46>"))
    (pad "M3" smd circle (at -2.800299 2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 601 "FBC_D<41>"))
    (pad "M4" smd circle (at -2.000301 2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 542 "FBC_CMD<18>"))
    (pad "M9" smd circle (at 2.000301 2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 547 "FBC_CMD<24>"))
    (pad "M10" smd circle (at 2.800299 2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 590 "FBC_D<51>"))
    (pad "M11" smd circle (at 3.600399 2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 587 "FBC_D<49>"))
    (pad "M12" smd circle (at 4.400601 2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N1" smd circle (at -4.400601 3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N2" smd circle (at -3.600399 3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 600 "FBC_D<44>"))
    (pad "N3" smd circle (at -2.800299 3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 606 "FBC_DQM5"))
    (pad "N4" smd circle (at -2.000301 3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N9" smd circle (at 2.000301 3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N10" smd circle (at 2.800299 3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 595 "FBC_DQM6"))
    (pad "N11" smd circle (at 3.600399 3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 589 "FBC_D<52>"))
    (pad "N12" smd circle (at 4.400601 3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "P1" smd circle (at -4.400601 4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "P2" smd circle (at -3.600399 4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 608 "FBC_DQS_WP5"))
    (pad "P3" smd circle (at -2.800299 4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 607 "FBC_DQS_RN5"))
    (pad "P4" smd circle (at -2.000301 4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "P9" smd circle (at 2.000301 4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "P10" smd circle (at 2.800299 4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 596 "FBC_DQS_RN6"))
    (pad "P11" smd circle (at 3.600399 4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 597 "FBC_DQS_WP6"))
    (pad "P12" smd circle (at 4.400601 4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "R1" smd circle (at -4.400601 4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "R2" smd circle (at -3.600399 4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 602 "FBC_D<42>"))
    (pad "R3" smd circle (at -2.800299 4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 603 "FBC_D<40>"))
    (pad "R4" smd circle (at -2.000301 4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "R9" smd circle (at 2.000301 4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "R10" smd circle (at 2.800299 4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 592 "FBC_D<55>"))
    (pad "R11" smd circle (at 3.600399 4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 591 "FBC_D<50>"))
    (pad "R12" smd circle (at 4.400601 4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "T1" smd circle (at -4.400601 5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T2" smd circle (at -3.600399 5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 604 "FBC_D<47>"))
    (pad "T3" smd circle (at -2.800299 5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 605 "FBC_D<43>"))
    (pad "T4" smd circle (at -2.000301 5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T9" smd circle (at 2.000301 5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T10" smd circle (at 2.800299 5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 594 "FBC_D<54>"))
    (pad "T11" smd circle (at 3.600399 5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 593 "FBC_D<53>"))
    (pad "T12" smd circle (at 4.400601 5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "V1" smd circle (at -4.400601 6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "V2" smd circle (at -3.600399 6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "V3" smd circle (at -2.800299 6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "V4" smd circle (at -2.000301 6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 560 "FBC_SEN2"))
    (pad "V9" smd circle (at 2.000301 6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 557 "FBC_CMD<10>"))
    (pad "V10" smd circle (at 2.800299 6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "V11" smd circle (at 3.600399 6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "V12" smd circle (at 4.400601 6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
  )
  (footprint "1206_1" (layer "F.Cu")
    (tedit 0)
    (at 227.696413 105.487615 -90)
    (fp_text reference "C132" (at 0 1.0795 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -1.4732 0 270) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 981 "12V_PEX6_F1"))
    (pad "2" smd rect (at 1.4732 0 270) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "CAP_SMD_066X066_1" (layer "F.Cu")
    (tedit 0)
    (at 182.992108 94.234907 180)
    (fp_text reference "C105" (at 1.27 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -2.602992 0 180) (size 3.556 1.651) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at 2.602992 0 180) (size 3.556 1.651) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 193.469608 94.425407)
    (fp_text reference "R53" (at -0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 928 "PS5_NVVDD_VAMP_CSREF"))
  )
  (footprint "CAP_TH_D080P035_1" (layer "F.Cu")
    (tedit 0)
    (at 241.412108 141.765902 90)
    (fp_text reference "C141" (at -1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 -1.750111 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 983 "12V_PEX6_F2"))
    (pad "2" thru_hole circle (at 0 1.750085 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 38.085108 127.610812)
    (fp_text reference "R24" (at -0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1940 "HYBRID_HPD_DVICD_DP"))
    (pad "2" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1009 "3V3"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 193.469608 80.290307)
    (fp_text reference "R51" (at -0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 928 "PS5_NVVDD_VAMP_CSREF"))
  )
  (footprint "DFET_SMD_DPAK_1" (layer "F.Cu")
    (tedit 0)
    (at 225.410108 99.187907 -90)
    (fp_text reference "Q21" (at 2.192477 -1.5875 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -2.290089 5.31241 270) (size 1.6002 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 987 "PS5_NVVDD_UG6_R"))
    (pad "2" smd rect (at 0 -1.867408 270) (size 5.799811 6.200089) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 981 "12V_PEX6_F1"))
    (pad "3" smd rect (at 2.290089 5.31241 270) (size 1.6002 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "PS5_NVVDD_PHASE6"))
  )
  (footprint "0603_1" (layer "F.Cu")
    (tedit 0)
    (at 217.409108 61.494307 90)
    (fp_text reference "C117" (at 0 -1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.762 0 270) (size 0.889 0.7874) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "INPUT_PEX6_IN1"))
    (pad "2" smd rect (at 0.762 0 90) (size 0.889 0.7874) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 159.573308 83.948212 90)
    (fp_text reference "C77" (at 0 -0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "CAP_SMD_066X066_1" (layer "F.Cu")
    (tedit 0)
    (at 182.992108 119.380907 180)
    (fp_text reference "C107" (at 1.27 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -2.602992 0 180) (size 3.556 1.651) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at 2.602992 0 180) (size 3.556 1.651) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "DFET_SMD_DPAK_1" (layer "F.Cu")
    (tedit 0)
    (at 225.410108 124.841907 -90)
    (fp_text reference "Q23" (at 2.192477 -1.5875 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -2.290089 5.31241 270) (size 1.6002 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 985 "PS5_NVVDD_UG4_R"))
    (pad "2" smd rect (at 0 -1.867408 270) (size 5.799811 6.200089) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 983 "12V_PEX6_F2"))
    (pad "3" smd rect (at 2.290089 5.31241 270) (size 1.6002 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "PS5_NVVDD_PHASE4"))
  )
  (footprint "EMIPAD_025X041_1" (layer "F.Cu")
    (tedit 0)
    (at 79.512508 142.952107)
    (fp_text reference "MEC7" (at 1.175106 1.157199 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 0) (size 2.499792 3.000197) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 70.292308 137.668907 -90)
    (fp_text reference "R32" (at 0 0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1808 "GPIO8_FAN_TACH"))
    (pad "2" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1975 "FAN_TACH"))
  )
  (footprint "1206_1" (layer "F.Cu")
    (tedit 0)
    (at 40.904508 139.548507 180)
    (fp_text reference "C25" (at 0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -1.4732 0 180) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1000 "12V"))
    (pad "2" smd rect (at 1.4732 0 180) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 38.085108 126.467812 180)
    (fp_text reference "R23" (at 0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1939 "I2CS_SDA_R"))
  )
  (footprint "GEOM0020_1" (layer "F.Cu")
    (tedit 0)
    (at -5.983892 70.562412 90)
    (fp_text reference "J1" (at -2.749956 -0.635 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at -3.399993 3.800094 90) (size 1.5748 1.5748) (drill 1.0922) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "2" thru_hole circle (at 3.399993 3.800094 90) (size 1.5748 1.5748) (drill 1.0922) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "3" thru_hole circle (at -3.399993 6.299987 90) (size 1.5748 1.5748) (drill 1.0922) (layers *.Cu *.Mask)
      (net 1951 "DACB_Y_F"))
    (pad "4" thru_hole circle (at 3.399993 6.299987 90) (size 1.5748 1.5748) (drill 1.0922) (layers *.Cu *.Mask)
      (net 1953 "DACB_PR_F"))
    (pad "5" thru_hole circle (at -1.299997 6.299987 90) (size 1.5748 1.5748) (drill 1.0922) (layers *.Cu *.Mask)
      (net 1950 "SNN_TV_NC5"))
    (pad "6" thru_hole circle (at 5.399989 6.299987 90) (size 1.5748 1.5748) (drill 1.0922) (layers *.Cu *.Mask)
      (net 1954 "DACB_PB_F"))
    (pad "7" thru_hole circle (at 0.899897 6.299987 90) (size 1.5748 1.5748) (drill 1.0922) (layers *.Cu *.Mask)
      (net 1952 "SNN_TV_NC7"))
    (pad "8" thru_hole circle (at -6.750101 0.8001 90) (size 3.175 3.175) (drill 2.3114) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "9" thru_hole circle (at 6.750101 0.8001 90) (size 3.175 3.175) (drill 2.3114) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "10" thru_hole circle (at 0 0 90) (size 3.175 3.175) (drill 2.3114) (layers *.Cu *.Mask)
      (net 1 "GND"))
  )
  (footprint "0603_1" (layer "F.Cu")
    (tedit 0)
    (at 42.225308 79.375907 -90)
    (fp_text reference "C29" (at 0 0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.762 0 90) (size 0.889 0.7874) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 989 "PS3_FBVDDQ_PHASE"))
    (pad "2" smd rect (at 0.762 0 270) (size 0.889 0.7874) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1104 "PS3_FBVDDQ_RC"))
  )
  (footprint "0805_1" (layer "F.Cu")
    (tedit 0)
    (at 27.036108 146.177907 180)
    (fp_text reference "C22" (at 0.787406 -0.000013 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.9525 0 180) (size 1.143 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at 0.9525 0 180) (size 1.143 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "1206_1" (layer "F.Cu")
    (tedit 0)
    (at 200.518108 119.063407 -90)
    (fp_text reference "R60" (at 0 0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -1.4732 0 270) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1102 "PS5_NVVDD_RC5"))
    (pad "2" smd rect (at 1.4732 0 270) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "SO08_I190X150_1" (layer "F.Cu")
    (tedit 0)
    (at 34.401803 134.011815 -90)
    (fp_text reference "Q4" (at 0.635 -1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -1.905 2.590495 270) (size 0.6096 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "2" smd rect (at -0.635 2.590495 270) (size 0.6096 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1107 "PS1_1V15_LG"))
    (pad "3" smd rect (at 0.635 2.590495 270) (size 0.6096 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "PS1_1V15_PH"))
    (pad "4" smd rect (at 1.905 2.590495 270) (size 0.6096 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1108 "PS1_1V15_UG_R"))
    (pad "5" smd rect (at 1.905 -2.590495 270) (size 0.6096 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 991 "12V_F"))
    (pad "6" smd rect (at 0.635 -2.590495 270) (size 0.6096 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 991 "12V_F"))
    (pad "7" smd rect (at -0.635 -2.590495 270) (size 0.6096 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "PS1_1V15_PH"))
    (pad "8" smd rect (at -1.905 -2.590495 270) (size 0.6096 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "PS1_1V15_PH"))
  )
  (footprint "CAP_TH_D080P035_1" (layer "F.Cu")
    (tedit 0)
    (at 13.904308 72.162815 180)
    (fp_text reference "C11" (at -1.5875 -1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 -1.750111 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 991 "12V_F"))
    (pad "2" thru_hole circle (at 0 1.750085 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "GND"))
  )
  (footprint "GEOM0004_1" (layer "F.Cu")
    (tedit 0)
    (at 193.533108 113.538907 90)
    (fp_text reference "L11" (at -1.27 1.5875 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 3.81 90) (size 4.0132 4.318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "PS5_NVVDD_PHASE5"))
    (pad "2" smd rect (at 0 -3.81 90) (size 4.0132 4.318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
  )
  (footprint "0805_1" (layer "F.Cu")
    (tedit 0)
    (at 154.620308 59.538812)
    (fp_text reference "C73" (at -0.787406 0.000013 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.9525 0) (size 1.143 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at 0.9525 0) (size 1.143 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0805_1" (layer "F.Cu")
    (tedit 0)
    (at 181.722108 78.080507 180)
    (fp_text reference "C96" (at 0.787406 -0.000013 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.9525 0 180) (size 1.143 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at 0.9525 0 180) (size 1.143 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "1206_1" (layer "F.Cu")
    (tedit 0)
    (at 200.518108 144.717407 -90)
    (fp_text reference "R62" (at 0 0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -1.4732 0 270) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1101 "PS5_NVVDD_RC3"))
    (pad "2" smd rect (at 1.4732 0 270) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 164.119908 86.462812)
    (fp_text reference "C90" (at -0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "GEOM0008_1" (layer "F.Cu")
    (tedit 0)
    (at 205.598413 113.869615)
    (fp_text reference "Q9" (at 1.27 1.582877 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -2.290115 5.31241) (size 1.6002 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 997 "PS5_NVVDD_LG5_AC"))
    (pad "2" smd rect (at 0 -1.867408) (size 5.799811 6.200089) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "PS5_NVVDD_PHASE5"))
    (pad "3" smd rect (at 2.290089 5.31241) (size 1.6002 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0805_1" (layer "F.Cu")
    (tedit 0)
    (at 181.722108 70.790707 180)
    (fp_text reference "C93" (at 0.787406 -0.000013 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.9525 0 180) (size 1.143 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at 0.9525 0 180) (size 1.143 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "1206_1" (layer "F.Cu")
    (tedit 0)
    (at 241.742308 135.586107 180)
    (fp_text reference "R74" (at 0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -1.4732 0 180) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "INPUT_PEX6_IN2"))
    (pad "2" smd rect (at 1.4732 0 180) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 983 "12V_PEX6_F2"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 126.541599 72.086615 180)
    (fp_text reference "C67" (at 0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 245.476108 114.491407 -90)
    (fp_text reference "R79" (at 0 0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 930 "PS5_NVVDD_EN"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 223.251387 91.390615 -90)
    (fp_text reference "C121" (at 0 1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 981 "12V_PEX6_F1"))
    (pad "2" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 16.037908 122.073612 180)
    (fp_text reference "R9" (at 0.635 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1697 "I2C2_SDA"))
    (pad "2" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1999 "I2C2_SDA_R"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 159.573308 119.901607 90)
    (fp_text reference "C80" (at 0 -0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0603_1" (layer "F.Cu")
    (tedit 0)
    (at 200.708608 89.218407 -90)
    (fp_text reference "C110" (at 0 1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.762 0 90) (size 0.889 0.7874) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "PS5_NVVDD_PHASE2"))
    (pad "2" smd rect (at 0.762 0 270) (size 0.889 0.7874) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1105 "PS5_NVVDD_RC2"))
  )
  (footprint "1206_1" (layer "F.Cu")
    (tedit 0)
    (at 212.964108 65.342407 -90)
    (fp_text reference "R68" (at 0 0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -1.4732 0 270) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "INPUT_PEX6_IN1"))
    (pad "2" smd rect (at 1.4732 0 270) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 981 "12V_PEX6_F1"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 223.251387 129.871615 -90)
    (fp_text reference "C124" (at 0 1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 983 "12V_PEX6_F2"))
    (pad "2" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 116.875908 68.936812 90)
    (fp_text reference "C65" (at 0 -0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 21.854508 123.115215 180)
    (fp_text reference "R15" (at 0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1809 "I2C3_SCL"))
    (pad "2" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 976 "I2C3_SCL_R"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 223.251387 81.280907 -90)
    (fp_text reference "C120" (at 0 1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 981 "12V_PEX6_F1"))
    (pad "2" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "GEOM0008_1" (layer "F.Cu")
    (tedit 0)
    (at 213.777213 139.523615)
    (fp_text reference "Q18" (at 1.5875 2.217877 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -2.290115 5.31241) (size 1.6002 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 995 "PS5_NVVDD_LG3_AC"))
    (pad "2" smd rect (at 0 -1.867408) (size 5.799811 6.200089) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "PS5_NVVDD_PHASE3"))
    (pad "3" smd rect (at 2.290089 5.31241) (size 1.6002 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0603_1" (layer "F.Cu")
    (tedit 0)
    (at 200.708608 127.826407 -90)
    (fp_text reference "C113" (at 0 1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.762 0 90) (size 0.889 0.7874) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "PS5_NVVDD_PHASE4"))
    (pad "2" smd rect (at 0.762 0 270) (size 0.889 0.7874) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1100 "PS5_NVVDD_RC4"))
  )
  (footprint "DIODE_SMD_MELF_1" (layer "F.Cu")
    (tedit 0)
    (at 202.481503 65.555818 180)
    (fp_text reference "D8" (at 0.635 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 2.325091 0 180) (size 1.5748 3.048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1001 "5V_INPUT"))
    (pad "2" smd rect (at -2.325091 0 180) (size 1.5748 3.048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 981 "12V_PEX6_F1"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 18.908108 122.073612)
    (fp_text reference "R11" (at -0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 977 "I2C3_SDA_R"))
  )
  (footprint "GEOM0022_1" (layer "F.Cu")
    (tedit 0)
    (at 46.128805 124.624 180)
    (fp_text reference "MEC6" (at 1.27 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0 180) (size 3.5814 3.5814) (drill 3.175) (layers *.Cu *.Mask)
      (net 1 "GND"))
  )
  (footprint "0805_1" (layer "F.Cu")
    (tedit 0)
    (at 17.942908 133.198507 90)
    (fp_text reference "C13" (at -0.000013 -0.787406 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.9525 0 90) (size 1.143 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1790 "2V5"))
    (pad "2" smd rect (at 0.9525 0 90) (size 1.143 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0603_1" (layer "F.Cu")
    (tedit 0)
    (at 24.521508 88.265907)
    (fp_text reference "C20" (at -0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.762 0 180) (size 0.889 0.7874) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 991 "12V_F"))
    (pad "2" smd rect (at 0.762 0) (size 0.889 0.7874) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0805_1" (layer "F.Cu")
    (tedit 0)
    (at 181.722108 111.887907 180)
    (fp_text reference "C100" (at 0.7874 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.9525 0 180) (size 1.143 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at 0.9525 0 180) (size 1.143 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "DFET_SMD_DPAK_1" (layer "F.Cu")
    (tedit 0)
    (at 225.410108 112.014907 -90)
    (fp_text reference "Q22" (at 2.192477 -1.5875 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -2.290089 5.31241 270) (size 1.6002 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 986 "PS5_NVVDD_UG5_R"))
    (pad "2" smd rect (at 0 -1.867408 270) (size 5.799811 6.200089) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 983 "12V_PEX6_F2"))
    (pad "3" smd rect (at 2.290089 5.31241 270) (size 1.6002 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "PS5_NVVDD_PHASE5"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 242.809108 113.284907 -90)
    (fp_text reference "R77" (at 0 0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 981 "12V_PEX6_F1"))
    (pad "2" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1989 "PS5_NVVDD_EN*"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 161.859308 86.462812)
    (fp_text reference "C86" (at -0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 137.070203 72.086615)
    (fp_text reference "R43" (at -0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "2" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 488 "FBD_SEN1"))
  )
  (footprint "GEOM0024_1" (layer "F.Cu")
    (tedit 0)
    (at 75.067508 133.910012)
    (fp_text reference "U4" (at 1.27 0.635 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -2.2225 2.6924) (size 0.381 1.6764) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 976 "I2C3_SCL_R"))
    (pad "2" smd rect (at -1.5875 2.6924) (size 0.381 1.6764) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "3" smd rect (at -0.9525 2.6924) (size 0.381 1.6764) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1009 "3V3"))
    (pad "4" smd rect (at -0.3175 2.6924) (size 0.381 1.6764) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1977 "SNN_7473_2"))
    (pad "5" smd rect (at 0.3175 2.6924) (size 0.381 1.6764) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 978 "THERM_SHDN*"))
    (pad "6" smd rect (at 0.9525 2.6924) (size 0.381 1.6764) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1975 "FAN_TACH"))
    (pad "7" smd rect (at 1.5875 2.6924) (size 0.381 1.6764) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1976 "SNN_TACH2"))
    (pad "8" smd rect (at 2.2225 2.6924) (size 0.381 1.6764) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1974 "THERM_PWM_ADDR_EN*"))
    (pad "9" smd rect (at 2.2225 -2.6924) (size 0.381 1.6764) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 973 "GPIO9_THERM_ALERT*"))
    (pad "10" smd rect (at 1.5875 -2.6924) (size 0.381 1.6764) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 975 "THERM_DN"))
    (pad "11" smd rect (at 0.9525 -2.6924) (size 0.381 1.6764) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 974 "THERM_DP"))
    (pad "12" smd rect (at 0.3175 -2.6924) (size 0.381 1.6764) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 975 "THERM_DN"))
    (pad "13" smd rect (at -0.3175 -2.6924) (size 0.381 1.6764) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 974 "THERM_DP"))
    (pad "14" smd rect (at -0.9525 -2.6924) (size 0.381 1.6764) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1009 "3V3"))
    (pad "15" smd rect (at -1.5875 -2.6924) (size 0.381 1.6764) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1973 "FAN_PWM"))
    (pad "16" smd rect (at -2.2225 -2.6924) (size 0.381 1.6764) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 977 "I2C3_SDA_R"))
  )
  (footprint "GEOM0001_1" (layer "F.Cu")
    (tedit 0)
    (at -0.014892 60.071907)
    (fp_text reference "BKT1" (at -1.27 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 6.858 6.858) (drill 3.175) (layers *.Cu *.Mask)
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 242.174108 115.951907 90)
    (fp_text reference "C142" (at 0 -1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1984 "PS5_NVVDD_EN_12V_F2"))
    (pad "2" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "IND_SMD_0603_1" (layer "F.Cu")
    (tedit 0)
    (at 5.166708 127.306215 180)
    (fp_text reference "L2" (at 0.635 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.762 0) (size 0.889 0.7874) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2009 "DACA_HSYNC_BUF"))
    (pad "2" smd rect (at 0.762 0 180) (size 0.889 0.7874) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1923 "DACA_HSYNC_CON"))
  )
  (footprint "0805_1" (layer "F.Cu")
    (tedit 0)
    (at 83.627308 59.030812 90)
    (fp_text reference "C57" (at -0.000013 -0.787406 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.9525 0 90) (size 1.143 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at 0.9525 0 90) (size 1.143 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 75.376118 104.814312 90)
    (fp_text reference "R34" (at 0 -0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "2" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 113 "FBG_SEN1"))
  )
  (footprint "1206_1" (layer "F.Cu")
    (tedit 0)
    (at 43.774708 134.747907 90)
    (fp_text reference "C30" (at 0 -0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -1.4732 0 90) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 991 "12V_F"))
    (pad "2" smd rect (at 1.4732 0 90) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 22.438708 124.766012 90)
    (fp_text reference "C17" (at 0 -0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "1206_1" (layer "F.Cu")
    (tedit 0)
    (at 241.742308 133.173107 180)
    (fp_text reference "R73" (at 0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -1.4732 0 180) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "INPUT_PEX6_IN2"))
    (pad "2" smd rect (at 1.4732 0 180) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 983 "12V_PEX6_F2"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 23.988108 126.696412 180)
    (fp_text reference "R17" (at 0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1050 "GPU_RST*"))
    (pad "2" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "CAP_TH_D080P035_1" (layer "F.Cu")
    (tedit 0)
    (at 240.810915 77.597907 90)
    (fp_text reference "C140" (at -1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 -1.750111 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 981 "12V_PEX6_F1"))
    (pad "2" thru_hole circle (at 0 1.750085 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "GND"))
  )
  (footprint "0805_1" (layer "F.Cu")
    (tedit 0)
    (at 181.722108 89.281907 180)
    (fp_text reference "C97" (at 0.787406 -0.000013 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.9525 0 180) (size 1.143 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at 0.9525 0 180) (size 1.143 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "1206_1" (layer "F.Cu")
    (tedit 0)
    (at 200.518108 131.890407 -90)
    (fp_text reference "R61" (at 0 0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -1.4732 0 270) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1100 "PS5_NVVDD_RC4"))
    (pad "2" smd rect (at 1.4732 0 270) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 193.469608 120.587407)
    (fp_text reference "R55" (at -0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 928 "PS5_NVVDD_VAMP_CSREF"))
  )
  (footprint "GEOM0004_1" (layer "F.Cu")
    (tedit 0)
    (at 38.389908 72.264415 -90)
    (fp_text reference "L6" (at 0.635 -1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 3.81 270) (size 4.0132 4.318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 989 "PS3_FBVDDQ_PHASE"))
    (pad "2" smd rect (at 0 -3.81 270) (size 4.0132 4.318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
  )
  (footprint "GEOM0008_1" (layer "F.Cu")
    (tedit 0)
    (at 205.598413 88.215615)
    (fp_text reference "Q7" (at 1.27 1.582877 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -2.290115 5.31241) (size 1.6002 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 994 "PS5_NVVDD_LG2_AC"))
    (pad "2" smd rect (at 0 -1.867408) (size 5.799811 6.200089) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "PS5_NVVDD_PHASE2"))
    (pad "3" smd rect (at 2.290089 5.31241) (size 1.6002 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 18.908108 126.289707 180)
    (fp_text reference "R13" (at 0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1008 "ROM_CS*"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 159.573308 62.802102 -90)
    (fp_text reference "R45" (at 0 0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "2" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 560 "FBC_SEN2"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 159.573308 78.271515 -90)
    (fp_text reference "R46" (at 0 0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "2" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 618 "FBC_SEN1"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 250.340208 126.327807 180)
    (fp_text reference "R83" (at 0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 991 "12V_F"))
    (pad "2" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1985 "PS5_NVVDD_EN_12V_F"))
  )
  (footprint "GEOM0002_1" (layer "F.Cu")
    (tedit 0)
    (at 224.465203 66.048502)
    (fp_text reference "J5" (at 3.556 2.0955 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 3.175 3.175) (drill 1.8034) (layers *.Cu *.Mask)
      (net 2 "INPUT_PEX6_IN1"))
    (pad "2" thru_hole circle (at 4.191 0) (size 3.175 3.175) (drill 1.8034) (layers *.Cu *.Mask)
      (net 2 "INPUT_PEX6_IN1"))
    (pad "3" thru_hole circle (at 8.382 0) (size 3.175 3.175) (drill 1.8034) (layers *.Cu *.Mask)
      (net 2 "INPUT_PEX6_IN1"))
    (pad "4" thru_hole circle (at 0 4.191) (size 3.175 3.175) (drill 1.8034) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "5" thru_hole circle (at 4.191 4.191) (size 3.175 3.175) (drill 1.8034) (layers *.Cu *.Mask)
      (net 3 "SNN_INPUT_PEX6_DT1*"))
    (pad "6" thru_hole circle (at 8.382 4.191) (size 3.175 3.175) (drill 1.8034) (layers *.Cu *.Mask)
      (net 1 "GND"))
  )
  (footprint "GEOM0008_1" (layer "F.Cu")
    (tedit 0)
    (at 205.598413 126.696615)
    (fp_text reference "Q10" (at 1.5875 2.217877 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -2.290115 5.31241) (size 1.6002 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 996 "PS5_NVVDD_LG4_AC"))
    (pad "2" smd rect (at 0 -1.867408) (size 5.799811 6.200089) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "PS5_NVVDD_PHASE4"))
    (pad "3" smd rect (at 2.290089 5.31241) (size 1.6002 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 163.867915 116.307812)
    (fp_text reference "C89" (at -0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0805_1" (layer "F.Cu")
    (tedit 0)
    (at 154.620308 62.231212)
    (fp_text reference "C74" (at -0.787406 0.000013 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.9525 0) (size 1.143 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at 0.9525 0) (size 1.143 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "GEOM0005_1" (layer "F.Cu")
    (tedit 0)
    (at 67.071613 88.350997 90)
    (fp_text reference "M2" (at -0.635 1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "A1" smd circle (at -4.400601 -6.4008 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "A2" smd circle (at -3.600399 -6.4008 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "A3" smd circle (at -2.800299 -6.4008 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "A4" smd circle (at -2.000301 -6.4008 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 44 "FBF_ZQ2"))
    (pad "A9" smd circle (at 2.000301 -6.4008 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "A10" smd circle (at 2.800299 -6.4008 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "A11" smd circle (at 3.600399 -6.4008 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "A12" smd circle (at 4.400601 -6.4008 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "B1" smd circle (at -4.400601 -5.6007 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B2" smd circle (at -3.600399 -5.6007 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "FBF_D<61>"))
    (pad "B3" smd circle (at -2.800299 -5.6007 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 46 "FBF_D<63>"))
    (pad "B4" smd circle (at -2.000301 -5.6007 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B9" smd circle (at 2.000301 -5.6007 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B10" smd circle (at 2.800299 -5.6007 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 57 "FBF_D<33>"))
    (pad "B11" smd circle (at 3.600399 -5.6007 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 56 "FBF_D<32>"))
    (pad "B12" smd circle (at 4.400601 -5.6007 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "C1" smd circle (at -4.400601 -4.8006 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "C2" smd circle (at -3.600399 -4.8006 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 47 "FBF_D<59>"))
    (pad "C3" smd circle (at -2.800299 -4.8006 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 48 "FBF_D<60>"))
    (pad "C4" smd circle (at -2.000301 -4.8006 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "C9" smd circle (at 2.000301 -4.8006 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "C10" smd circle (at 2.800299 -4.8006 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 59 "FBF_D<34>"))
    (pad "C11" smd circle (at 3.600399 -4.8006 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 58 "FBF_D<35>"))
    (pad "C12" smd circle (at 4.400601 -4.8006 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "D1" smd circle (at -4.400601 -4.0005 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "D2" smd circle (at -3.600399 -4.0005 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 55 "FBF_DQS_WP7"))
    (pad "D3" smd circle (at -2.800299 -4.0005 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 54 "FBF_DQS_RN7"))
    (pad "D4" smd circle (at -2.000301 -4.0005 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "D9" smd circle (at 2.000301 -4.0005 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "D10" smd circle (at 2.800299 -4.0005 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 65 "FBF_DQS_RN4"))
    (pad "D11" smd circle (at 3.600399 -4.0005 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 66 "FBF_DQS_WP4"))
    (pad "D12" smd circle (at 4.400601 -4.0005 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "E1" smd circle (at -4.400601 -3.2004 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "E2" smd circle (at -3.600399 -3.2004 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 49 "FBF_D<56>"))
    (pad "E3" smd circle (at -2.800299 -3.2004 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 53 "FBF_DQM7"))
    (pad "E4" smd circle (at -2.000301 -3.2004 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "E9" smd circle (at 2.000301 -3.2004 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "E10" smd circle (at 2.800299 -3.2004 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 64 "FBF_DQM4"))
    (pad "E11" smd circle (at 3.600399 -3.2004 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "FBF_D<37>"))
    (pad "E12" smd circle (at 4.400601 -3.2004 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "F1" smd circle (at -4.400601 -2.4003 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "F2" smd circle (at -3.600399 -2.4003 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 51 "FBF_D<57>"))
    (pad "F3" smd circle (at -2.800299 -2.4003 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 50 "FBF_D<58>"))
    (pad "F4" smd circle (at -2.000301 -2.4003 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "FBF_CMD<16>"))
    (pad "F9" smd circle (at 2.000301 -2.4003 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "FBF_CMD<17>"))
    (pad "F10" smd circle (at 2.800299 -2.4003 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "FBF_D<39>"))
    (pad "F11" smd circle (at 3.600399 -2.4003 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 62 "FBF_D<36>"))
    (pad "F12" smd circle (at 4.400601 -2.4003 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "G1" smd circle (at -4.400601 -1.6002 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "G2" smd circle (at -3.600399 -1.6002 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "G3" smd circle (at -2.800299 -1.6002 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 52 "FBF_D<62>"))
    (pad "G4" smd circle (at -2.000301 -1.6002 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "FBF_CMD<11>"))
    (pad "G9" smd circle (at 2.000301 -1.6002 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "FBF_CMD<15>"))
    (pad "G10" smd circle (at 2.800299 -1.6002 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 63 "FBF_D<38>"))
    (pad "G11" smd circle (at 3.600399 -1.6002 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "G12" smd circle (at 4.400601 -1.6002 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "H1" smd circle (at -4.400601 -0.8001 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "FBF_VREF3"))
    (pad "H2" smd circle (at -3.600399 -0.8001 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "FBF_CMD<28>"))
    (pad "H3" smd circle (at -2.800299 -0.8001 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "FBF_CMD<8>"))
    (pad "H4" smd circle (at -2.000301 -0.8001 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "FBF_CMD<7>"))
    (pad "H9" smd circle (at 2.000301 -0.8001 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "FBF_CMD<6>"))
    (pad "H10" smd circle (at 2.800299 -0.8001 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "FBF_CMD<14>"))
    (pad "H11" smd circle (at 3.600399 -0.8001 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "FBF_CMD<12>"))
    (pad "H12" smd circle (at 4.400601 -0.8001 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "FBF_VREF4"))
    (pad "J1" smd circle (at -4.400601 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "J2" smd circle (at -3.600399 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "SNN_FBF_NC04"))
    (pad "J3" smd circle (at -2.800299 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "FBF_CMD<13>"))
    (pad "J4" smd circle (at -2.000301 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "J9" smd circle (at 2.000301 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "J10" smd circle (at 2.800299 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "FBF1_CLK0*"))
    (pad "J11" smd circle (at 3.600399 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "FBF1_CLK0"))
    (pad "J12" smd circle (at 4.400601 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "K1" smd circle (at -4.400601 0.8001 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "K2" smd circle (at -3.600399 0.8001 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "FBF_CMD<19>"))
    (pad "K3" smd circle (at -2.800299 0.8001 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "FBF_CMD<26>"))
    (pad "K4" smd circle (at -2.000301 0.8001 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "FBF_CMD<25>"))
    (pad "K9" smd circle (at 2.000301 0.8001 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "FBF_CMD<21>"))
    (pad "K10" smd circle (at 2.800299 0.8001 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "FBF_CMD<23>"))
    (pad "K11" smd circle (at 3.600399 0.8001 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "FBF_CMD<9>"))
    (pad "K12" smd circle (at 4.400601 0.8001 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "L1" smd circle (at -4.400601 1.6002 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "L2" smd circle (at -3.600399 1.6002 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "L3" smd circle (at -2.800299 1.6002 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 79 "FBF_D<47>"))
    (pad "L4" smd circle (at -2.000301 1.6002 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "FBF_CMD<27>"))
    (pad "L9" smd circle (at 2.000301 1.6002 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "FBF_CMD<20>"))
    (pad "L10" smd circle (at 2.800299 1.6002 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 68 "FBF_D<55>"))
    (pad "L11" smd circle (at 3.600399 1.6002 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "L12" smd circle (at 4.400601 1.6002 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "M1" smd circle (at -4.400601 2.4003 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "M2" smd circle (at -3.600399 2.4003 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 78 "FBF_D<45>"))
    (pad "M3" smd circle (at -2.800299 2.4003 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 81 "FBF_D<44>"))
    (pad "M4" smd circle (at -2.000301 2.4003 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "FBF_CMD<18>"))
    (pad "M9" smd circle (at 2.000301 2.4003 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "FBF_CMD<24>"))
    (pad "M10" smd circle (at 2.800299 2.4003 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "FBF_D<53>"))
    (pad "M11" smd circle (at 3.600399 2.4003 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 67 "FBF_D<54>"))
    (pad "M12" smd circle (at 4.400601 2.4003 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N1" smd circle (at -4.400601 3.2004 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N2" smd circle (at -3.600399 3.2004 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 80 "FBF_D<46>"))
    (pad "N3" smd circle (at -2.800299 3.2004 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 86 "FBF_DQM5"))
    (pad "N4" smd circle (at -2.000301 3.2004 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N9" smd circle (at 2.000301 3.2004 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N10" smd circle (at 2.800299 3.2004 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 75 "FBF_DQM6"))
    (pad "N11" smd circle (at 3.600399 3.2004 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 69 "FBF_D<48>"))
    (pad "N12" smd circle (at 4.400601 3.2004 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "P1" smd circle (at -4.400601 4.0005 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "P2" smd circle (at -3.600399 4.0005 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 88 "FBF_DQS_WP5"))
    (pad "P3" smd circle (at -2.800299 4.0005 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 87 "FBF_DQS_RN5"))
    (pad "P4" smd circle (at -2.000301 4.0005 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "P9" smd circle (at 2.000301 4.0005 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "P10" smd circle (at 2.800299 4.0005 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 76 "FBF_DQS_RN6"))
    (pad "P11" smd circle (at 3.600399 4.0005 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 77 "FBF_DQS_WP6"))
    (pad "P12" smd circle (at 4.400601 4.0005 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "R1" smd circle (at -4.400601 4.8006 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "R2" smd circle (at -3.600399 4.8006 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 82 "FBF_D<40>"))
    (pad "R3" smd circle (at -2.800299 4.8006 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 83 "FBF_D<43>"))
    (pad "R4" smd circle (at -2.000301 4.8006 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "R9" smd circle (at 2.000301 4.8006 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "R10" smd circle (at 2.800299 4.8006 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 72 "FBF_D<52>"))
    (pad "R11" smd circle (at 3.600399 4.8006 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 71 "FBF_D<49>"))
    (pad "R12" smd circle (at 4.400601 4.8006 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "T1" smd circle (at -4.400601 5.6007 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T2" smd circle (at -3.600399 5.6007 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 84 "FBF_D<42>"))
    (pad "T3" smd circle (at -2.800299 5.6007 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 85 "FBF_D<41>"))
    (pad "T4" smd circle (at -2.000301 5.6007 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T9" smd circle (at 2.000301 5.6007 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T10" smd circle (at 2.800299 5.6007 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 74 "FBF_D<50>"))
    (pad "T11" smd circle (at 3.600399 5.6007 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 73 "FBF_D<51>"))
    (pad "T12" smd circle (at 4.400601 5.6007 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "V1" smd circle (at -4.400601 6.4008 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "V2" smd circle (at -3.600399 6.4008 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "V3" smd circle (at -2.800299 6.4008 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "V4" smd circle (at -2.000301 6.4008 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 40 "FBF_SEN2"))
    (pad "V9" smd circle (at 2.000301 6.4008 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "FBF_CMD<10>"))
    (pad "V10" smd circle (at 2.800299 6.4008 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "V11" smd circle (at 3.600399 6.4008 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "V12" smd circle (at 4.400601 6.4008 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
  )
  (footprint "GEOM0008_1" (layer "F.Cu")
    (tedit 0)
    (at 205.598413 139.523615)
    (fp_text reference "Q11" (at 1.5875 2.217877 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -2.290115 5.31241) (size 1.6002 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 995 "PS5_NVVDD_LG3_AC"))
    (pad "2" smd rect (at 0 -1.867408) (size 5.799811 6.200089) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "PS5_NVVDD_PHASE3"))
    (pad "3" smd rect (at 2.290089 5.31241) (size 1.6002 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0805_1" (layer "F.Cu")
    (tedit 0)
    (at 181.722108 114.427907 180)
    (fp_text reference "C101" (at 0.7874 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.9525 0 180) (size 1.143 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at 0.9525 0 180) (size 1.143 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 4.023708 134.697615 90)
    (fp_text reference "C2" (at 0 -0.635 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1928 "I2C2_SCL_CON"))
    (pad "2" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "GEOM0004_1" (layer "F.Cu")
    (tedit 0)
    (at 193.533108 74.295907 90)
    (fp_text reference "L8" (at -0.635 1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 3.81 90) (size 4.0132 4.318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "PS5_NVVDD_PHASE1"))
    (pad "2" smd rect (at 0 -3.81 90) (size 4.0132 4.318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 4.658708 101.906215)
    (fp_text reference "C7" (at -0.635 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1926 "DACA_VSYNC_CON"))
    (pad "2" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "GEOM0023_1" (layer "F.Cu")
    (tedit 0)
    (at 146.924108 81.865615)
    (fp_text reference "MEC12" (at -1.5875 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 3.5814 3.5814) (drill 2.4892) (layers *.Cu *.Mask)
      (net 1 "GND"))
  )
  (footprint "SO14_I335X150_1" (layer "F.Cu")
    (tedit 0)
    (at 25.309213 134.570615 180)
    (fp_text reference "U1" (at 0.635 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -3.81 2.5908 180) (size 0.6096 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1961 "PS1_1V15_BOOT"))
    (pad "2" smd rect (at -2.54 2.5908 180) (size 0.6096 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1917 "PS1_1V15_FS"))
    (pad "3" smd rect (at -1.27 2.5908 180) (size 0.6096 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1962 "PS1_1V15_CP"))
    (pad "4" smd rect (at 0 2.5908 180) (size 0.6096 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1958 "PS1_1V15_FB"))
    (pad "5" smd rect (at 1.27 2.5908 180) (size 0.6096 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1963 "PS1_2V5_LDO_DR"))
    (pad "6" smd rect (at 2.54 2.5908 180) (size 0.6096 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1916 "PS1_2V5_LDO_FB"))
    (pad "7" smd rect (at 3.81 2.5908 180) (size 0.6096 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "8" smd rect (at 3.81 -2.5908 180) (size 0.6096 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1049 "PS1_VCC12"))
    (pad "9" smd rect (at 2.54 -2.5908 180) (size 0.6096 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1048 "PS1_VCC5"))
    (pad "10" smd rect (at 1.27 -2.5908 180) (size 0.6096 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1047 "PS1_PVCC5"))
    (pad "11" smd rect (at 0 -2.5908 180) (size 0.6096 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1107 "PS1_1V15_LG"))
    (pad "12" smd rect (at -1.27 -2.5908 180) (size 0.6096 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "13" smd rect (at -2.54 -2.5908 180) (size 0.6096 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "PS1_1V15_PH"))
    (pad "14" smd rect (at -3.81 -2.5908 180) (size 0.6096 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1964 "PS1_1V15_UG"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 21.854508 128.118812 180)
    (fp_text reference "R16" (at 0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1942 "HYBRID_HPD_DVIAB"))
    (pad "2" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1009 "3V3"))
  )
  (footprint "SOT23_1" (layer "F.Cu")
    (tedit 0)
    (at 5.496908 106.351215 -90)
    (fp_text reference "D1" (at 0.635 -1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.9525 1.143 270) (size 0.9144 0.9144) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "2" smd rect (at 0.9525 1.143 270) (size 0.9144 0.9144) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1914 "5V"))
    (pad "3" smd rect (at 0 -1.143 270) (size 0.9144 0.9144) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2011 "DACA_VSYNC_BUF"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 31.557308 137.465707)
    (fp_text reference "R20" (at -0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1964 "PS1_1V15_UG"))
    (pad "2" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1108 "PS1_1V15_UG_R"))
  )
  (footprint "GEOM0012_1" (layer "F.Cu")
    (tedit 0)
    (at 49.108708 104.039307 -90)
    (fp_text reference "Y1" (at 0 0.635 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -2.794 0 270) (size 5.588 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1058 "XTAL_OUT"))
    (pad "2" smd rect (at 2.794 0 270) (size 5.588 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1059 "XTAL_IN"))
  )
  (footprint "CAP_TH_D080P035_1" (layer "F.Cu")
    (tedit 0)
    (at 23.175308 72.162815 180)
    (fp_text reference "C18" (at -1.5875 -1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 -1.750111 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 991 "12V_F"))
    (pad "2" thru_hole circle (at 0 1.750085 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "GND"))
  )
  (footprint "GEOM0003_1" (layer "F.Cu")
    (tedit 0)
    (at 34.148108 142.621907 -90)
    (fp_text reference "L5" (at 0 0.635 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -3.0099 0 270) (size 2.4892 3.8354) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "PS1_1V15_PH"))
    (pad "2" smd rect (at 3.0099 0 270) (size 2.4892 3.8354) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "1V15"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 24.115108 128.118812 180)
    (fp_text reference "R19" (at 0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1946 "PEX_RST*"))
    (pad "2" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1050 "GPU_RST*"))
  )
  (footprint "GEOM0008_1" (layer "F.Cu")
    (tedit 0)
    (at 213.777213 75.388615)
    (fp_text reference "Q13" (at 1.5875 2.217877 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -2.290115 5.31241) (size 1.6002 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 993 "PS5_NVVDD_LG1_AC"))
    (pad "2" smd rect (at 0 -1.867408) (size 5.799811 6.200089) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "PS5_NVVDD_PHASE1"))
    (pad "3" smd rect (at 2.290089 5.31241) (size 1.6002 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "1206_1" (layer "F.Cu")
    (tedit 0)
    (at 48.422908 138.684907)
    (fp_text reference "R27" (at -0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -1.4732 0) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1000 "12V"))
    (pad "2" smd rect (at 1.4732 0) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 991 "12V_F"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 204.963108 60.821207 -90)
    (fp_text reference "C115" (at 0 1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1991 "SPDIF_IN_C"))
    (pad "2" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 3.998308 145.518015 90)
    (fp_text reference "C1" (at 0 -0.635 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1932 "DACC_HSYNC_CON"))
    (pad "2" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "GEOM0010_1" (layer "F.Cu")
    (tedit 0)
    (at 211.884608 65.342407 180)
    (fp_text reference "L14" (at -1.5875 -1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 2.500097) (size 7.500188 3.000197) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "INPUT_PEX6_IN1"))
    (pad "2" smd rect (at 0 -2.500097 180) (size 7.500188 3.000197) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 981 "12V_PEX6_F1"))
  )
  (footprint "GEOM0008_1" (layer "F.Cu")
    (tedit 0)
    (at 213.777213 113.869615)
    (fp_text reference "Q16" (at 1.5875 2.217877 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -2.290115 5.31241) (size 1.6002 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 997 "PS5_NVVDD_LG5_AC"))
    (pad "2" smd rect (at 0 -1.867408) (size 5.799811 6.200089) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "PS5_NVVDD_PHASE5"))
    (pad "3" smd rect (at 2.290089 5.31241) (size 1.6002 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "1206_1" (layer "F.Cu")
    (tedit 0)
    (at 48.422908 143.587107)
    (fp_text reference "R29" (at -0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -1.4732 0) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1000 "12V"))
    (pad "2" smd rect (at 1.4732 0) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 991 "12V_F"))
  )
  (footprint "0805_1" (layer "F.Cu")
    (tedit 0)
    (at 51.394708 85.522707)
    (fp_text reference "C39" (at -0.787406 0.000013 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.9525 0) (size 1.143 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at 0.9525 0) (size 1.143 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 163.486915 117.781012 180)
    (fp_text reference "C88" (at 0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "GEOM0005_1" (layer "F.Cu")
    (tedit 0)
    (at 167.879108 79.706615 -90)
    (fp_text reference "M10" (at 1.27 -1.5875 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "A1" smd circle (at -4.400601 -6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "A2" smd circle (at -3.600399 -6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "A3" smd circle (at -2.800299 -6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "A4" smd circle (at -2.000301 -6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 621 "FBC_ZQ1"))
    (pad "A9" smd circle (at 2.000301 -6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "A10" smd circle (at 2.800299 -6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "A11" smd circle (at 3.600399 -6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "A12" smd circle (at 4.400601 -6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "B1" smd circle (at -4.400601 -5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B2" smd circle (at -3.600399 -5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 622 "FBC_D<18>"))
    (pad "B3" smd circle (at -2.800299 -5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 623 "FBC_D<17>"))
    (pad "B4" smd circle (at -2.000301 -5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B9" smd circle (at 2.000301 -5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B10" smd circle (at 2.800299 -5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 634 "FBC_D<7>"))
    (pad "B11" smd circle (at 3.600399 -5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 633 "FBC_D<6>"))
    (pad "B12" smd circle (at 4.400601 -5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "C1" smd circle (at -4.400601 -4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "C2" smd circle (at -3.600399 -4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 624 "FBC_D<16>"))
    (pad "C3" smd circle (at -2.800299 -4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 625 "FBC_D<23>"))
    (pad "C4" smd circle (at -2.000301 -4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "C9" smd circle (at 2.000301 -4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "C10" smd circle (at 2.800299 -4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 636 "FBC_D<4>"))
    (pad "C11" smd circle (at 3.600399 -4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 635 "FBC_D<0>"))
    (pad "C12" smd circle (at 4.400601 -4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "D1" smd circle (at -4.400601 -4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "D2" smd circle (at -3.600399 -4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 632 "FBC_DQS_WP2"))
    (pad "D3" smd circle (at -2.800299 -4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 631 "FBC_DQS_RN2"))
    (pad "D4" smd circle (at -2.000301 -4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "D9" smd circle (at 2.000301 -4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "D10" smd circle (at 2.800299 -4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 642 "FBC_DQS_RN0"))
    (pad "D11" smd circle (at 3.600399 -4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 643 "FBC_DQS_WP0"))
    (pad "D12" smd circle (at 4.400601 -4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "E1" smd circle (at -4.400601 -3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "E2" smd circle (at -3.600399 -3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 626 "FBC_D<21>"))
    (pad "E3" smd circle (at -2.800299 -3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 630 "FBC_DQM2"))
    (pad "E4" smd circle (at -2.000301 -3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "E9" smd circle (at 2.000301 -3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "E10" smd circle (at 2.800299 -3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 641 "FBC_DQM0"))
    (pad "E11" smd circle (at 3.600399 -3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 637 "FBC_D<1>"))
    (pad "E12" smd circle (at 4.400601 -3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "F1" smd circle (at -4.400601 -2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "F2" smd circle (at -3.600399 -2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 628 "FBC_D<22>"))
    (pad "F3" smd circle (at -2.800299 -2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 627 "FBC_D<20>"))
    (pad "F4" smd circle (at -2.000301 -2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 555 "FBC_CMD<17>"))
    (pad "F9" smd circle (at 2.000301 -2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 551 "FBC_CMD<16>"))
    (pad "F10" smd circle (at 2.800299 -2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 638 "FBC_D<3>"))
    (pad "F11" smd circle (at 3.600399 -2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 639 "FBC_D<5>"))
    (pad "F12" smd circle (at 4.400601 -2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "G1" smd circle (at -4.400601 -1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "G2" smd circle (at -3.600399 -1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "G3" smd circle (at -2.800299 -1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 629 "FBC_D<19>"))
    (pad "G4" smd circle (at -2.000301 -1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 549 "FBC_CMD<15>"))
    (pad "G9" smd circle (at 2.000301 -1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 548 "FBC_CMD<11>"))
    (pad "G10" smd circle (at 2.800299 -1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 640 "FBC_D<2>"))
    (pad "G11" smd circle (at 3.600399 -1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "G12" smd circle (at 4.400601 -1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "H1" smd circle (at -4.400601 -0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 619 "FBC_VREF1"))
    (pad "H2" smd circle (at -3.600399 -0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 544 "FBC_CMD<12>"))
    (pad "H3" smd circle (at -2.800299 -0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 550 "FBC_CMD<14>"))
    (pad "H4" smd circle (at -2.000301 -0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 563 "FBC_CMD<6>"))
    (pad "H9" smd circle (at 2.000301 -0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 552 "FBC_CMD<7>"))
    (pad "H10" smd circle (at 2.800299 -0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 556 "FBC_CMD<8>"))
    (pad "H11" smd circle (at 3.600399 -0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 612 "FBC_CMD<0>"))
    (pad "H12" smd circle (at 4.400601 -0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 620 "FBC_VREF2"))
    (pad "J1" smd circle (at -4.400601 0 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "J2" smd circle (at -3.600399 0 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 617 "SNN_FBC_NC01"))
    (pad "J3" smd circle (at -2.800299 0 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 559 "FBC_CMD<13>"))
    (pad "J4" smd circle (at -2.000301 0 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "J9" smd circle (at 2.000301 0 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "J10" smd circle (at 2.800299 0 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 616 "FBC0_CLK0*"))
    (pad "J11" smd circle (at 3.600399 0 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 615 "FBC0_CLK0"))
    (pad "J12" smd circle (at 4.400601 0 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "K1" smd circle (at -4.400601 0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "K2" smd circle (at -3.600399 0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 536 "FBC_CMD<9>"))
    (pad "K3" smd circle (at -2.800299 0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 609 "FBC_CMD<5>"))
    (pad "K4" smd circle (at -2.000301 0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 543 "FBC_CMD<21>"))
    (pad "K9" smd circle (at 2.000301 0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 611 "FBC_CMD<3>"))
    (pad "K10" smd circle (at 2.800299 0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 613 "FBC_CMD<2>"))
    (pad "K11" smd circle (at 3.600399 0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 538 "FBC_CMD<19>"))
    (pad "K12" smd circle (at 4.400601 0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "L1" smd circle (at -4.400601 1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "L2" smd circle (at -3.600399 1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "L3" smd circle (at -2.800299 1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 656 "FBC_D<24>"))
    (pad "L4" smd circle (at -2.000301 1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 546 "FBC_CMD<20>"))
    (pad "L9" smd circle (at 2.000301 1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 614 "FBC_CMD<1>"))
    (pad "L10" smd circle (at 2.800299 1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 645 "FBC_D<8>"))
    (pad "L11" smd circle (at 3.600399 1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "L12" smd circle (at 4.400601 1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "M1" smd circle (at -4.400601 2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "M2" smd circle (at -3.600399 2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 655 "FBC_D<25>"))
    (pad "M3" smd circle (at -2.800299 2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 658 "FBC_D<26>"))
    (pad "M4" smd circle (at -2.000301 2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 610 "FBC_CMD<4>"))
    (pad "M9" smd circle (at 2.000301 2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 542 "FBC_CMD<18>"))
    (pad "M10" smd circle (at 2.800299 2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 647 "FBC_D<9>"))
    (pad "M11" smd circle (at 3.600399 2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 644 "FBC_D<12>"))
    (pad "M12" smd circle (at 4.400601 2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N1" smd circle (at -4.400601 3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N2" smd circle (at -3.600399 3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 657 "FBC_D<28>"))
    (pad "N3" smd circle (at -2.800299 3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 663 "FBC_DQM3"))
    (pad "N4" smd circle (at -2.000301 3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N9" smd circle (at 2.000301 3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N10" smd circle (at 2.800299 3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 652 "FBC_DQM1"))
    (pad "N11" smd circle (at 3.600399 3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 646 "FBC_D<10>"))
    (pad "N12" smd circle (at 4.400601 3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "P1" smd circle (at -4.400601 4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "P2" smd circle (at -3.600399 4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 665 "FBC_DQS_WP3"))
    (pad "P3" smd circle (at -2.800299 4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 664 "FBC_DQS_RN3"))
    (pad "P4" smd circle (at -2.000301 4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "P9" smd circle (at 2.000301 4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "P10" smd circle (at 2.800299 4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 653 "FBC_DQS_RN1"))
    (pad "P11" smd circle (at 3.600399 4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 654 "FBC_DQS_WP1"))
    (pad "P12" smd circle (at 4.400601 4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "R1" smd circle (at -4.400601 4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "R2" smd circle (at -3.600399 4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 659 "FBC_D<30>"))
    (pad "R3" smd circle (at -2.800299 4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 660 "FBC_D<29>"))
    (pad "R4" smd circle (at -2.000301 4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "R9" smd circle (at 2.000301 4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "R10" smd circle (at 2.800299 4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 649 "FBC_D<14>"))
    (pad "R11" smd circle (at 3.600399 4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 648 "FBC_D<11>"))
    (pad "R12" smd circle (at 4.400601 4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "T1" smd circle (at -4.400601 5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T2" smd circle (at -3.600399 5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 661 "FBC_D<31>"))
    (pad "T3" smd circle (at -2.800299 5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 662 "FBC_D<27>"))
    (pad "T4" smd circle (at -2.000301 5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T9" smd circle (at 2.000301 5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T10" smd circle (at 2.800299 5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 651 "FBC_D<13>"))
    (pad "T11" smd circle (at 3.600399 5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 650 "FBC_D<15>"))
    (pad "T12" smd circle (at 4.400601 5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "V1" smd circle (at -4.400601 6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "V2" smd circle (at -3.600399 6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "V3" smd circle (at -2.800299 6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "V4" smd circle (at -2.000301 6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 618 "FBC_SEN1"))
    (pad "V9" smd circle (at 2.000301 6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 557 "FBC_CMD<10>"))
    (pad "V10" smd circle (at 2.800299 6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "V11" smd circle (at 3.600399 6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "V12" smd circle (at 4.400601 6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
  )
  (footprint "GEOM0022_1" (layer "F.Cu")
    (tedit 0)
    (at 46.128805 88.4036)
    (fp_text reference "MEC5" (at -1.27 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 3.5814 3.5814) (drill 3.175) (layers *.Cu *.Mask)
      (net 1 "GND"))
  )
  (footprint "GEOM0019_1" (layer "F.Cu")
    (tedit 0)
    (at 30.719108 126.213812 -90)
    (fp_text reference "U3" (at 0.635 -1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -2.925089 3.575101 270) (size 0.4064 2.1844) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at -2.275103 3.575101 270) (size 0.4064 2.1844) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1938 "NET0016"))
    (pad "3" smd rect (at -1.625092 3.575101 270) (size 0.4064 2.1844) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 976 "I2C3_SCL_R"))
    (pad "4" smd rect (at -0.975106 3.575101 270) (size 0.4064 2.1844) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1937 "HYBRID_PRG_TP"))
    (pad "5" smd rect (at -0.325095 3.575101 270) (size 0.4064 2.1844) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1947 "SNN_U4_FAN_PWM_PIN5"))
    (pad "6" smd rect (at 0.325095 3.575101 270) (size 0.4064 2.1844) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1050 "GPU_RST*"))
    (pad "7" smd rect (at 0.975106 3.575101 270) (size 0.4064 2.1844) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1946 "PEX_RST*"))
    (pad "8" smd rect (at 1.625092 3.575101 270) (size 0.4064 2.1844) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1948 "NET0019"))
    (pad "9" smd rect (at 2.275103 3.575101 270) (size 0.4064 2.1844) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1949 "I2C2_SDA_UC"))
    (pad "10" smd rect (at 2.925089 3.575101 270) (size 0.4064 2.1844) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1942 "HYBRID_HPD_DVIAB"))
    (pad "11" smd rect (at 2.925089 -3.575101 270) (size 0.4064 2.1844) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1941 "I2CS_SCL_R"))
    (pad "12" smd rect (at 2.275103 -3.575101 270) (size 0.4064 2.1844) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1940 "HYBRID_HPD_DVICD_DP"))
    (pad "13" smd rect (at 1.625092 -3.575101 270) (size 0.4064 2.1844) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1939 "I2CS_SDA_R"))
    (pad "14" smd rect (at 0.975106 -3.575101 270) (size 0.4064 2.1844) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1945 "I2C1_SDA_UC"))
    (pad "15" smd rect (at 0.325095 -3.575101 270) (size 0.4064 2.1844) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1944 "NET0018"))
    (pad "16" smd rect (at -0.325095 -3.575101 270) (size 0.4064 2.1844) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1943 "NET0017"))
    (pad "17" smd rect (at -0.975106 -3.575101 270) (size 0.4064 2.1844) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 977 "I2C3_SDA_R"))
    (pad "18" smd rect (at -1.625092 -3.575101 270) (size 0.4064 2.1844) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1936 "HYBRID_HPD_F"))
    (pad "19" smd rect (at -2.275103 -3.575101 270) (size 0.4064 2.1844) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1935 "HYBRID_HPD_E"))
    (pad "20" smd rect (at -2.925089 -3.575101 270) (size 0.4064 2.1844) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 75.376118 100.560015 -90)
    (fp_text reference "C53" (at 0 0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "DFET_SMD_DPAK_1" (layer "F.Cu")
    (tedit 0)
    (at 225.410108 137.668907 -90)
    (fp_text reference "Q24" (at 2.192477 -1.5875 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -2.290089 5.31241 270) (size 1.6002 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 984 "PS5_NVVDD_UG3_R"))
    (pad "2" smd rect (at 0 -1.867408 270) (size 5.799811 6.200089) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 983 "12V_PEX6_F2"))
    (pad "3" smd rect (at 2.290089 5.31241 270) (size 1.6002 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "PS5_NVVDD_PHASE3"))
  )
  (footprint "0603_1" (layer "F.Cu")
    (tedit 0)
    (at 249.413108 115.342307 180)
    (fp_text reference "C146" (at 1.27 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.762 0) (size 0.889 0.7874) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 980 "NET0006"))
    (pad "2" smd rect (at 0.762 0 180) (size 0.889 0.7874) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 164.145308 87.936012)
    (fp_text reference "C92" (at -0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 145.298508 68.936812 -90)
    (fp_text reference "C71" (at 0 0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "GEOM0022_1" (layer "F.Cu")
    (tedit 0)
    (at 183.373108 60.757707)
    (fp_text reference "MEC16" (at -1.5875 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 3.5814 3.5814) (drill 3.175) (layers *.Cu *.Mask)
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 249.032108 116.675807)
    (fp_text reference "R80" (at -0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 981 "12V_PEX6_F1"))
    (pad "2" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 980 "NET0006"))
  )
  (footprint "GEOM0022_1" (layer "F.Cu")
    (tedit 0)
    (at 183.373108 83.185907)
    (fp_text reference "MEC17" (at -1.5875 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 3.5814 3.5814) (drill 3.175) (layers *.Cu *.Mask)
      (net 1 "GND"))
  )
  (footprint "IND_SMD_0603_1" (layer "F.Cu")
    (tedit 0)
    (at 5.090508 103.455615 180)
    (fp_text reference "L1" (at 0.635 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.762 0) (size 0.889 0.7874) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2011 "DACA_VSYNC_BUF"))
    (pad "2" smd rect (at 0.762 0 180) (size 0.889 0.7874) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1926 "DACA_VSYNC_CON"))
  )
  (footprint "1206_1" (layer "F.Cu")
    (tedit 0)
    (at 249.032108 74.803907 -90)
    (fp_text reference "C145" (at 0 1.0795 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -1.4732 0 270) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "INPUT_PEX6_IN2"))
    (pad "2" smd rect (at 1.4732 0 270) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 193.469608 81.344407)
    (fp_text reference "R52" (at -0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 928 "PS5_NVVDD_VAMP_CSREF"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 60.868908 140.589907 180)
    (fp_text reference "R31" (at 0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1559 "JTAG_TCK"))
    (pad "2" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "EMIPAD_025X041_1" (layer "F.Cu")
    (tedit 0)
    (at 183.182608 65.786907 90)
    (fp_text reference "MEC15" (at -1.240714 1.085622 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 0 90) (size 2.499792 3.000197) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "DFET_SMD_DPAK_1" (layer "F.Cu")
    (tedit 0)
    (at 18.870008 81.204707 90)
    (fp_text reference "Q2" (at -1.557477 1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -2.290089 5.31241 90) (size 1.6002 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 992 "PS3_FBVDDQ_UG_R"))
    (pad "2" smd rect (at 0 -1.867408 90) (size 5.799811 6.200089) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 991 "12V_F"))
    (pad "3" smd rect (at 2.290089 5.31241 90) (size 1.6002 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 989 "PS3_FBVDDQ_PHASE"))
  )
  (footprint "GEOM0005_1" (layer "F.Cu")
    (tedit 0)
    (at 93.724799 63.780815)
    (fp_text reference "M5" (at 1.27 0.635 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "A1" smd circle (at -4.400601 -6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "A2" smd circle (at -3.600399 -6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "A3" smd circle (at -2.800299 -6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "A4" smd circle (at -2.000301 -6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 304 "FBE_ZQ2"))
    (pad "A9" smd circle (at 2.000301 -6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "A10" smd circle (at 2.800299 -6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "A11" smd circle (at 3.600399 -6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "A12" smd circle (at 4.400601 -6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "B1" smd circle (at -4.400601 -5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B2" smd circle (at -3.600399 -5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 305 "FBE_D<62>"))
    (pad "B3" smd circle (at -2.800299 -5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 306 "FBE_D<63>"))
    (pad "B4" smd circle (at -2.000301 -5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B9" smd circle (at 2.000301 -5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B10" smd circle (at 2.800299 -5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 317 "FBE_D<32>"))
    (pad "B11" smd circle (at 3.600399 -5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 316 "FBE_D<35>"))
    (pad "B12" smd circle (at 4.400601 -5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "C1" smd circle (at -4.400601 -4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "C2" smd circle (at -3.600399 -4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 307 "FBE_D<60>"))
    (pad "C3" smd circle (at -2.800299 -4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 308 "FBE_D<61>"))
    (pad "C4" smd circle (at -2.000301 -4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "C9" smd circle (at 2.000301 -4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "C10" smd circle (at 2.800299 -4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 319 "FBE_D<33>"))
    (pad "C11" smd circle (at 3.600399 -4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 318 "FBE_D<34>"))
    (pad "C12" smd circle (at 4.400601 -4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "D1" smd circle (at -4.400601 -4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "D2" smd circle (at -3.600399 -4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 315 "FBE_DQS_WP7"))
    (pad "D3" smd circle (at -2.800299 -4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 314 "FBE_DQS_RN7"))
    (pad "D4" smd circle (at -2.000301 -4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "D9" smd circle (at 2.000301 -4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "D10" smd circle (at 2.800299 -4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 325 "FBE_DQS_RN4"))
    (pad "D11" smd circle (at 3.600399 -4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 326 "FBE_DQS_WP4"))
    (pad "D12" smd circle (at 4.400601 -4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "E1" smd circle (at -4.400601 -3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "E2" smd circle (at -3.600399 -3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 309 "FBE_D<59>"))
    (pad "E3" smd circle (at -2.800299 -3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 313 "FBE_DQM7"))
    (pad "E4" smd circle (at -2.000301 -3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "E9" smd circle (at 2.000301 -3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "E10" smd circle (at 2.800299 -3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 324 "FBE_DQM4"))
    (pad "E11" smd circle (at 3.600399 -3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 320 "FBE_D<38>"))
    (pad "E12" smd circle (at 4.400601 -3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "F1" smd circle (at -4.400601 -2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "F2" smd circle (at -3.600399 -2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 311 "FBE_D<56>"))
    (pad "F3" smd circle (at -2.800299 -2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 310 "FBE_D<58>"))
    (pad "F4" smd circle (at -2.000301 -2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 291 "FBE_CMD<16>"))
    (pad "F9" smd circle (at 2.000301 -2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 295 "FBE_CMD<17>"))
    (pad "F10" smd circle (at 2.800299 -2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 321 "FBE_D<39>"))
    (pad "F11" smd circle (at 3.600399 -2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 322 "FBE_D<36>"))
    (pad "F12" smd circle (at 4.400601 -2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "G1" smd circle (at -4.400601 -1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "G2" smd circle (at -3.600399 -1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "G3" smd circle (at -2.800299 -1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 312 "FBE_D<57>"))
    (pad "G4" smd circle (at -2.000301 -1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 288 "FBE_CMD<11>"))
    (pad "G9" smd circle (at 2.000301 -1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 289 "FBE_CMD<15>"))
    (pad "G10" smd circle (at 2.800299 -1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 323 "FBE_D<37>"))
    (pad "G11" smd circle (at 3.600399 -1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "G12" smd circle (at 4.400601 -1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "H1" smd circle (at -4.400601 -0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 301 "FBE_VREF3"))
    (pad "H2" smd circle (at -3.600399 -0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 280 "FBE_CMD<28>"))
    (pad "H3" smd circle (at -2.800299 -0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 296 "FBE_CMD<8>"))
    (pad "H4" smd circle (at -2.000301 -0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 292 "FBE_CMD<7>"))
    (pad "H9" smd circle (at 2.000301 -0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 303 "FBE_CMD<6>"))
    (pad "H10" smd circle (at 2.800299 -0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 290 "FBE_CMD<14>"))
    (pad "H11" smd circle (at 3.600399 -0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 284 "FBE_CMD<12>"))
    (pad "H12" smd circle (at 4.400601 -0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 302 "FBE_VREF4"))
    (pad "J1" smd circle (at -4.400601 0) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "J2" smd circle (at -3.600399 0) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 298 "SNN_FBE_NC04"))
    (pad "J3" smd circle (at -2.800299 0) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 299 "FBE_CMD<13>"))
    (pad "J4" smd circle (at -2.000301 0) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "J9" smd circle (at 2.000301 0) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "J10" smd circle (at 2.800299 0) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 294 "FBE1_CLK0*"))
    (pad "J11" smd circle (at 3.600399 0) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 293 "FBE1_CLK0"))
    (pad "J12" smd circle (at 4.400601 0) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "K1" smd circle (at -4.400601 0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "K2" smd circle (at -3.600399 0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 278 "FBE_CMD<19>"))
    (pad "K3" smd circle (at -2.800299 0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 281 "FBE_CMD<26>"))
    (pad "K4" smd circle (at -2.000301 0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 277 "FBE_CMD<25>"))
    (pad "K9" smd circle (at 2.000301 0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 283 "FBE_CMD<21>"))
    (pad "K10" smd circle (at 2.800299 0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 285 "FBE_CMD<23>"))
    (pad "K11" smd circle (at 3.600399 0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 276 "FBE_CMD<9>"))
    (pad "K12" smd circle (at 4.400601 0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "L1" smd circle (at -4.400601 1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "L2" smd circle (at -3.600399 1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "L3" smd circle (at -2.800299 1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 339 "FBE_D<47>"))
    (pad "L4" smd circle (at -2.000301 1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 279 "FBE_CMD<27>"))
    (pad "L9" smd circle (at 2.000301 1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 286 "FBE_CMD<20>"))
    (pad "L10" smd circle (at 2.800299 1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 328 "FBE_D<48>"))
    (pad "L11" smd circle (at 3.600399 1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "L12" smd circle (at 4.400601 1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "M1" smd circle (at -4.400601 2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "M2" smd circle (at -3.600399 2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 338 "FBE_D<45>"))
    (pad "M3" smd circle (at -2.800299 2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 341 "FBE_D<46>"))
    (pad "M4" smd circle (at -2.000301 2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 282 "FBE_CMD<18>"))
    (pad "M9" smd circle (at 2.000301 2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 287 "FBE_CMD<24>"))
    (pad "M10" smd circle (at 2.800299 2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 330 "FBE_D<51>"))
    (pad "M11" smd circle (at 3.600399 2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 327 "FBE_D<49>"))
    (pad "M12" smd circle (at 4.400601 2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N1" smd circle (at -4.400601 3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N2" smd circle (at -3.600399 3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 340 "FBE_D<44>"))
    (pad "N3" smd circle (at -2.800299 3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 346 "FBE_DQM5"))
    (pad "N4" smd circle (at -2.000301 3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N9" smd circle (at 2.000301 3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N10" smd circle (at 2.800299 3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 335 "FBE_DQM6"))
    (pad "N11" smd circle (at 3.600399 3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 329 "FBE_D<50>"))
    (pad "N12" smd circle (at 4.400601 3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "P1" smd circle (at -4.400601 4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "P2" smd circle (at -3.600399 4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 348 "FBE_DQS_WP5"))
    (pad "P3" smd circle (at -2.800299 4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 347 "FBE_DQS_RN5"))
    (pad "P4" smd circle (at -2.000301 4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "P9" smd circle (at 2.000301 4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "P10" smd circle (at 2.800299 4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 336 "FBE_DQS_RN6"))
    (pad "P11" smd circle (at 3.600399 4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 337 "FBE_DQS_WP6"))
    (pad "P12" smd circle (at 4.400601 4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "R1" smd circle (at -4.400601 4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "R2" smd circle (at -3.600399 4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 342 "FBE_D<42>"))
    (pad "R3" smd circle (at -2.800299 4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 343 "FBE_D<40>"))
    (pad "R4" smd circle (at -2.000301 4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "R9" smd circle (at 2.000301 4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "R10" smd circle (at 2.800299 4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 332 "FBE_D<55>"))
    (pad "R11" smd circle (at 3.600399 4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 331 "FBE_D<53>"))
    (pad "R12" smd circle (at 4.400601 4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "T1" smd circle (at -4.400601 5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T2" smd circle (at -3.600399 5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 344 "FBE_D<43>"))
    (pad "T3" smd circle (at -2.800299 5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 345 "FBE_D<41>"))
    (pad "T4" smd circle (at -2.000301 5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T9" smd circle (at 2.000301 5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T10" smd circle (at 2.800299 5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 334 "FBE_D<52>"))
    (pad "T11" smd circle (at 3.600399 5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 333 "FBE_D<54>"))
    (pad "T12" smd circle (at 4.400601 5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "V1" smd circle (at -4.400601 6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "V2" smd circle (at -3.600399 6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "V3" smd circle (at -2.800299 6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "V4" smd circle (at -2.000301 6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 300 "FBE_SEN2"))
    (pad "V9" smd circle (at 2.000301 6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 297 "FBE_CMD<10>"))
    (pad "V10" smd circle (at 2.800299 6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "V11" smd circle (at 3.600399 6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "V12" smd circle (at 4.400601 6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 206.131508 60.821207 90)
    (fp_text reference "R65" (at 0 -0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 981 "12V_PEX6_F1"))
    (pad "2" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1993 "SPDIF_IN_COMP2_D"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 70.526013 124.994815)
    (fp_text reference "C41" (at -0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "GEOM0011_1" (layer "F.Cu")
    (tedit 0)
    (at 116.444108 112.345615)
    (fp_text reference "MEC11" (at -1.5875 -0.19685 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at -30.48 0) (size 2.9464 2.9464) (drill 2.4892) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "2" thru_hole circle (at -25.581407 -25.581407) (size 2.9464 2.9464) (drill 2.4892) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "3" thru_hole circle (at 0 -30.48) (size 2.9464 2.9464) (drill 2.4892) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "4" thru_hole circle (at 25.581407 -25.581407) (size 2.9464 2.9464) (drill 2.4892) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "5" thru_hole circle (at 30.48 0) (size 2.9464 2.9464) (drill 2.4892) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "6" thru_hole circle (at 25.581407 25.581407) (size 2.9464 2.9464) (drill 2.4892) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "7" thru_hole circle (at 0 30.48) (size 4.4958 4.4958) (drill 2.4892) (layers *.Cu *.Mask)
      (net 1 "GND"))
  )
  (footprint "SOT23_1" (layer "F.Cu")
    (tedit 0)
    (at 244.650608 117.666407)
    (fp_text reference "Q25" (at 1.359967 1.11125 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.9525 1.143) (size 0.9144 0.9144) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1989 "PS5_NVVDD_EN*"))
    (pad "2" smd rect (at 0.9525 1.143) (size 0.9144 0.9144) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "3" smd rect (at 0 -1.143) (size 0.9144 0.9144) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 930 "PS5_NVVDD_EN"))
  )
  (footprint "0805_1" (layer "F.Cu")
    (tedit 0)
    (at 15.809308 133.198507 90)
    (fp_text reference "C12" (at -0.000013 -0.787406 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.9525 0 90) (size 1.143 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1790 "2V5"))
    (pad "2" smd rect (at 0.9525 0 90) (size 1.143 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 159.598708 97.549607 90)
    (fp_text reference "C81" (at 0 -0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "GEOM0022_1" (layer "F.Cu")
    (tedit 0)
    (at 9.908405 88.4036)
    (fp_text reference "MEC3" (at -1.27 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 3.5814 3.5814) (drill 3.175) (layers *.Cu *.Mask)
      (net 1 "GND"))
  )
  (footprint "CAP_TH_D080P035_1" (layer "F.Cu")
    (tedit 0)
    (at 240.675508 124.077418 90)
    (fp_text reference "C139" (at -1.905 1.905 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 -1.750111 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 983 "12V_PEX6_F2"))
    (pad "2" thru_hole circle (at 0 1.750085 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "GND"))
  )
  (footprint "1206_1" (layer "F.Cu")
    (tedit 0)
    (at 5.954108 120.015907 180)
    (fp_text reference "F1" (at 0.635 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -1.4732 0 180) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1914 "5V"))
    (pad "2" smd rect (at 1.4732 0 180) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1925 "DDC_5V"))
  )
  (footprint "1206_1" (layer "F.Cu")
    (tedit 0)
    (at 235.951108 134.430407 -90)
    (fp_text reference "C138" (at 0 1.0795 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -1.4732 0 270) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 983 "12V_PEX6_F2"))
    (pad "2" smd rect (at 1.4732 0 270) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 145.298508 66.676212 90)
    (fp_text reference "C70" (at 0 -0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 73.645108 129.413907 180)
    (fp_text reference "C49" (at 0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "GEOM0008_1" (layer "F.Cu")
    (tedit 0)
    (at 213.777213 101.042615)
    (fp_text reference "Q15" (at 1.5875 2.217877 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -2.290115 5.31241) (size 1.6002 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 998 "PS5_NVVDD_LG6_AC"))
    (pad "2" smd rect (at 0 -1.867408) (size 5.799811 6.200089) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "PS5_NVVDD_PHASE6"))
    (pad "3" smd rect (at 2.290089 5.31241) (size 1.6002 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 159.573308 113.793212 90)
    (fp_text reference "C79" (at 0 -0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 75.376118 120.245294 90)
    (fp_text reference "R35" (at 0 -0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "2" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 171 "FBG_SEN2"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 38.085108 128.753812 180)
    (fp_text reference "R25" (at 0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1941 "I2CS_SCL_R"))
  )
  (footprint "GEOM0005_1" (layer "F.Cu")
    (tedit 0)
    (at 67.071613 103.340807 90)
    (fp_text reference "M3" (at -0.635 1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "A1" smd circle (at -4.400601 -6.4008 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "A2" smd circle (at -3.600399 -6.4008 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "A3" smd circle (at -2.800299 -6.4008 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "A4" smd circle (at -2.000301 -6.4008 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 117 "FBG_ZQ1"))
    (pad "A9" smd circle (at 2.000301 -6.4008 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "A10" smd circle (at 2.800299 -6.4008 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "A11" smd circle (at 3.600399 -6.4008 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "A12" smd circle (at 4.400601 -6.4008 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "B1" smd circle (at -4.400601 -5.6007 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B2" smd circle (at -3.600399 -5.6007 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 118 "FBG_D<26>"))
    (pad "B3" smd circle (at -2.800299 -5.6007 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 119 "FBG_D<24>"))
    (pad "B4" smd circle (at -2.000301 -5.6007 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B9" smd circle (at 2.000301 -5.6007 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B10" smd circle (at 2.800299 -5.6007 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 130 "FBG_D<3>"))
    (pad "B11" smd circle (at 3.600399 -5.6007 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 129 "FBG_D<1>"))
    (pad "B12" smd circle (at 4.400601 -5.6007 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "C1" smd circle (at -4.400601 -4.8006 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "C2" smd circle (at -3.600399 -4.8006 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 120 "FBG_D<25>"))
    (pad "C3" smd circle (at -2.800299 -4.8006 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 121 "FBG_D<27>"))
    (pad "C4" smd circle (at -2.000301 -4.8006 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "C9" smd circle (at 2.000301 -4.8006 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "C10" smd circle (at 2.800299 -4.8006 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 132 "FBG_D<2>"))
    (pad "C11" smd circle (at 3.600399 -4.8006 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 131 "FBG_D<0>"))
    (pad "C12" smd circle (at 4.400601 -4.8006 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "D1" smd circle (at -4.400601 -4.0005 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "D2" smd circle (at -3.600399 -4.0005 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 128 "FBG_DQS_WP3"))
    (pad "D3" smd circle (at -2.800299 -4.0005 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 127 "FBG_DQS_RN3"))
    (pad "D4" smd circle (at -2.000301 -4.0005 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "D9" smd circle (at 2.000301 -4.0005 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "D10" smd circle (at 2.800299 -4.0005 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 138 "FBG_DQS_RN0"))
    (pad "D11" smd circle (at 3.600399 -4.0005 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 139 "FBG_DQS_WP0"))
    (pad "D12" smd circle (at 4.400601 -4.0005 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "E1" smd circle (at -4.400601 -3.2004 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "E2" smd circle (at -3.600399 -3.2004 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 122 "FBG_D<29>"))
    (pad "E3" smd circle (at -2.800299 -3.2004 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 126 "FBG_DQM3"))
    (pad "E4" smd circle (at -2.000301 -3.2004 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "E9" smd circle (at 2.000301 -3.2004 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "E10" smd circle (at 2.800299 -3.2004 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 137 "FBG_DQM0"))
    (pad "E11" smd circle (at 3.600399 -3.2004 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 133 "FBG_D<7>"))
    (pad "E12" smd circle (at 4.400601 -3.2004 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "F1" smd circle (at -4.400601 -2.4003 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "F2" smd circle (at -3.600399 -2.4003 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 124 "FBG_D<30>"))
    (pad "F3" smd circle (at -2.800299 -2.4003 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 123 "FBG_D<28>"))
    (pad "F4" smd circle (at -2.000301 -2.4003 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 104 "FBG_CMD<17>"))
    (pad "F9" smd circle (at 2.000301 -2.4003 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 108 "FBG_CMD<16>"))
    (pad "F10" smd circle (at 2.800299 -2.4003 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 134 "FBG_D<6>"))
    (pad "F11" smd circle (at 3.600399 -2.4003 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 135 "FBG_D<4>"))
    (pad "F12" smd circle (at 4.400601 -2.4003 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "G1" smd circle (at -4.400601 -1.6002 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "G2" smd circle (at -3.600399 -1.6002 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "G3" smd circle (at -2.800299 -1.6002 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 125 "FBG_D<31>"))
    (pad "G4" smd circle (at -2.000301 -1.6002 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 101 "FBG_CMD<15>"))
    (pad "G9" smd circle (at 2.000301 -1.6002 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 102 "FBG_CMD<11>"))
    (pad "G10" smd circle (at 2.800299 -1.6002 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 136 "FBG_D<5>"))
    (pad "G11" smd circle (at 3.600399 -1.6002 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "G12" smd circle (at 4.400601 -1.6002 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "H1" smd circle (at -4.400601 -0.8001 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 114 "FBG_VREF1"))
    (pad "H2" smd circle (at -3.600399 -0.8001 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 93 "FBG_CMD<12>"))
    (pad "H3" smd circle (at -2.800299 -0.8001 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 109 "FBG_CMD<14>"))
    (pad "H4" smd circle (at -2.000301 -0.8001 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 105 "FBG_CMD<6>"))
    (pad "H9" smd circle (at 2.000301 -0.8001 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 116 "FBG_CMD<7>"))
    (pad "H10" smd circle (at 2.800299 -0.8001 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 103 "FBG_CMD<8>"))
    (pad "H11" smd circle (at 3.600399 -0.8001 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 97 "FBG_CMD<0>"))
    (pad "H12" smd circle (at 4.400601 -0.8001 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 115 "FBG_VREF2"))
    (pad "J1" smd circle (at -4.400601 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "J2" smd circle (at -3.600399 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 111 "SNN_FBG_NC01"))
    (pad "J3" smd circle (at -2.800299 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 112 "FBG_CMD<13>"))
    (pad "J4" smd circle (at -2.000301 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "J9" smd circle (at 2.000301 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "J10" smd circle (at 2.800299 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 107 "FBG0_CLK0*"))
    (pad "J11" smd circle (at 3.600399 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 106 "FBG0_CLK0"))
    (pad "J12" smd circle (at 4.400601 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "K1" smd circle (at -4.400601 0.8001 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "K2" smd circle (at -3.600399 0.8001 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 91 "FBG_CMD<9>"))
    (pad "K3" smd circle (at -2.800299 0.8001 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 94 "FBG_CMD<5>"))
    (pad "K4" smd circle (at -2.000301 0.8001 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 90 "FBG_CMD<21>"))
    (pad "K9" smd circle (at 2.000301 0.8001 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 96 "FBG_CMD<3>"))
    (pad "K10" smd circle (at 2.800299 0.8001 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 98 "FBG_CMD<2>"))
    (pad "K11" smd circle (at 3.600399 0.8001 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 89 "FBG_CMD<19>"))
    (pad "K12" smd circle (at 4.400601 0.8001 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "L1" smd circle (at -4.400601 1.6002 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "L2" smd circle (at -3.600399 1.6002 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "L3" smd circle (at -2.800299 1.6002 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 152 "FBG_D<17>"))
    (pad "L4" smd circle (at -2.000301 1.6002 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 92 "FBG_CMD<20>"))
    (pad "L9" smd circle (at 2.000301 1.6002 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 99 "FBG_CMD<1>"))
    (pad "L10" smd circle (at 2.800299 1.6002 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 141 "FBG_D<10>"))
    (pad "L11" smd circle (at 3.600399 1.6002 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "L12" smd circle (at 4.400601 1.6002 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "M1" smd circle (at -4.400601 2.4003 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "M2" smd circle (at -3.600399 2.4003 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 151 "FBG_D<21>"))
    (pad "M3" smd circle (at -2.800299 2.4003 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 154 "FBG_D<16>"))
    (pad "M4" smd circle (at -2.000301 2.4003 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 95 "FBG_CMD<4>"))
    (pad "M9" smd circle (at 2.000301 2.4003 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 100 "FBG_CMD<18>"))
    (pad "M10" smd circle (at 2.800299 2.4003 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 143 "FBG_D<9>"))
    (pad "M11" smd circle (at 3.600399 2.4003 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 140 "FBG_D<8>"))
    (pad "M12" smd circle (at 4.400601 2.4003 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N1" smd circle (at -4.400601 3.2004 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N2" smd circle (at -3.600399 3.2004 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 153 "FBG_D<22>"))
    (pad "N3" smd circle (at -2.800299 3.2004 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 159 "FBG_DQM2"))
    (pad "N4" smd circle (at -2.000301 3.2004 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N9" smd circle (at 2.000301 3.2004 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N10" smd circle (at 2.800299 3.2004 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 148 "FBG_DQM1"))
    (pad "N11" smd circle (at 3.600399 3.2004 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 142 "FBG_D<11>"))
    (pad "N12" smd circle (at 4.400601 3.2004 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "P1" smd circle (at -4.400601 4.0005 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "P2" smd circle (at -3.600399 4.0005 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 161 "FBG_DQS_WP2"))
    (pad "P3" smd circle (at -2.800299 4.0005 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 160 "FBG_DQS_RN2"))
    (pad "P4" smd circle (at -2.000301 4.0005 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "P9" smd circle (at 2.000301 4.0005 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "P10" smd circle (at 2.800299 4.0005 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 149 "FBG_DQS_RN1"))
    (pad "P11" smd circle (at 3.600399 4.0005 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 150 "FBG_DQS_WP1"))
    (pad "P12" smd circle (at 4.400601 4.0005 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "R1" smd circle (at -4.400601 4.8006 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "R2" smd circle (at -3.600399 4.8006 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 155 "FBG_D<19>"))
    (pad "R3" smd circle (at -2.800299 4.8006 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 156 "FBG_D<18>"))
    (pad "R4" smd circle (at -2.000301 4.8006 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "R9" smd circle (at 2.000301 4.8006 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "R10" smd circle (at 2.800299 4.8006 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 145 "FBG_D<12>"))
    (pad "R11" smd circle (at 3.600399 4.8006 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 144 "FBG_D<15>"))
    (pad "R12" smd circle (at 4.400601 4.8006 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "T1" smd circle (at -4.400601 5.6007 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T2" smd circle (at -3.600399 5.6007 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 157 "FBG_D<23>"))
    (pad "T3" smd circle (at -2.800299 5.6007 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 158 "FBG_D<20>"))
    (pad "T4" smd circle (at -2.000301 5.6007 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T9" smd circle (at 2.000301 5.6007 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T10" smd circle (at 2.800299 5.6007 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 147 "FBG_D<13>"))
    (pad "T11" smd circle (at 3.600399 5.6007 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 146 "FBG_D<14>"))
    (pad "T12" smd circle (at 4.400601 5.6007 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "V1" smd circle (at -4.400601 6.4008 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "V2" smd circle (at -3.600399 6.4008 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "V3" smd circle (at -2.800299 6.4008 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "V4" smd circle (at -2.000301 6.4008 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 113 "FBG_SEN1"))
    (pad "V9" smd circle (at 2.000301 6.4008 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 110 "FBG_CMD<10>"))
    (pad "V10" smd circle (at 2.800299 6.4008 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "V11" smd circle (at 3.600399 6.4008 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "V12" smd circle (at 4.400601 6.4008 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
  )
  (footprint "0805_1" (layer "F.Cu")
    (tedit 0)
    (at 181.722108 75.565907 180)
    (fp_text reference "C95" (at 0.787406 -0.000013 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.9525 0 180) (size 1.143 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at 0.9525 0 180) (size 1.143 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "GEOM0025_1" (layer "F.Cu")
    (tedit 0)
    (at 46.974803 163.017091)
    (fp_text reference "CN2" (at 28.68229 -5.251704 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "A1" smd rect (at -11.500104 -5.251704) (size 3.185211 4.472991) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2061 "PEX_PRSNT1*"))
    (pad "A2" smd rect (at -10.500106 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1000 "12V"))
    (pad "A3" smd rect (at -9.500108 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1000 "12V"))
    (pad "A4" smd rect (at -8.50011 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "A5" smd rect (at -7.500112 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2074 "SNN_PEX_TCK"))
    (pad "A6" smd rect (at -6.500089 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2075 "SNN_PEX_TDI"))
    (pad "A7" smd rect (at -5.500091 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2076 "SNN_PEX_TDO"))
    (pad "A8" smd rect (at -4.500093 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2077 "SNN_PEX_TMS"))
    (pad "A9" smd rect (at -3.500095 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "A10" smd rect (at -2.500097 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "A11" smd rect (at -1.500099 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1946 "PEX_RST*"))
    (pad "A12" smd rect (at 1.500099 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "A13" smd rect (at 2.500097 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1120 "PEX_REFCLK"))
    (pad "A14" smd rect (at 3.500095 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1121 "PEX_REFCLK*"))
    (pad "A15" smd rect (at 4.500093 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "A16" smd rect (at 5.500091 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2045 "PEX_TX_C0"))
    (pad "A17" smd rect (at 6.500089 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2029 "PEX_TX_C0*"))
    (pad "A18" smd rect (at 7.500112 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "A19" smd rect (at 8.50011 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2066 "SNN_PEX_12"))
    (pad "A20" smd rect (at 9.500108 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "A21" smd rect (at 10.500106 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2046 "PEX_TX_C1"))
    (pad "A22" smd rect (at 11.500104 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2030 "PEX_TX_C1*"))
    (pad "A23" smd rect (at 12.500102 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "A24" smd rect (at 13.5001 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "A25" smd rect (at 14.500098 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2053 "PEX_TX_C2"))
    (pad "A26" smd rect (at 15.500096 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2037 "PEX_TX_C2*"))
    (pad "A27" smd rect (at 16.500094 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "A28" smd rect (at 17.500092 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "A29" smd rect (at 18.50009 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2054 "PEX_TX_C3"))
    (pad "A30" smd rect (at 19.500088 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2038 "PEX_TX_C3*"))
    (pad "A31" smd rect (at 20.500111 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "A32" smd rect (at 21.500109 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2068 "SNN_PEX_14"))
    (pad "A33" smd rect (at 22.500107 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2069 "SNN_PEX_16"))
    (pad "A34" smd rect (at 23.500105 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "A35" smd rect (at 24.500103 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2055 "PEX_TX_C4"))
    (pad "A36" smd rect (at 25.500101 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2039 "PEX_TX_C4*"))
    (pad "A37" smd rect (at 26.500099 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "A38" smd rect (at 27.500097 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "A39" smd rect (at 28.500095 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2056 "PEX_TX_C5"))
    (pad "A40" smd rect (at 29.500093 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2040 "PEX_TX_C5*"))
    (pad "A41" smd rect (at 30.500091 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "A42" smd rect (at 31.500089 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "A43" smd rect (at 32.500087 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2057 "PEX_TX_C6"))
    (pad "A44" smd rect (at 33.500111 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2041 "PEX_TX_C6*"))
    (pad "A45" smd rect (at 34.500109 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "A46" smd rect (at 35.500107 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "A47" smd rect (at 36.500105 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2058 "PEX_TX_C7"))
    (pad "A48" smd rect (at 37.500103 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2042 "PEX_TX_C7*"))
    (pad "A49" smd rect (at 38.500101 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "A50" smd rect (at 39.499997 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2070 "SNN_PEX_17"))
    (pad "A51" smd rect (at 40.499995 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "A52" smd rect (at 41.499993 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2059 "PEX_TX_C8"))
    (pad "A53" smd rect (at 42.499991 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2043 "PEX_TX_C8*"))
    (pad "A54" smd rect (at 43.499989 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "A55" smd rect (at 44.500013 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "A56" smd rect (at 45.500011 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2060 "PEX_TX_C9"))
    (pad "A57" smd rect (at 46.500009 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2044 "PEX_TX_C9*"))
    (pad "A58" smd rect (at 47.500007 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "A59" smd rect (at 48.500005 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "A60" smd rect (at 49.500003 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2047 "PEX_TX_C10"))
    (pad "A61" smd rect (at 50.500001 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2031 "PEX_TX_C10*"))
    (pad "A62" smd rect (at 51.499999 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "A63" smd rect (at 52.499997 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "A64" smd rect (at 53.499995 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2048 "PEX_TX_C11"))
    (pad "A65" smd rect (at 54.499993 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2032 "PEX_TX_C11*"))
    (pad "A66" smd rect (at 55.499991 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "A67" smd rect (at 56.499989 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "A68" smd rect (at 57.499987 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2049 "PEX_TX_C12"))
    (pad "A69" smd rect (at 58.499985 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2033 "PEX_TX_C12*"))
    (pad "A70" smd rect (at 59.500008 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "A71" smd rect (at 60.500006 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "A72" smd rect (at 61.500004 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2050 "PEX_TX_C13"))
    (pad "A73" smd rect (at 62.500002 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2034 "PEX_TX_C13*"))
    (pad "A74" smd rect (at 63.5 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "A75" smd rect (at 64.499998 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "A76" smd rect (at 65.499996 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2051 "PEX_TX_C14"))
    (pad "A77" smd rect (at 66.499994 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2035 "PEX_TX_C14*"))
    (pad "A78" smd rect (at 67.499992 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "A79" smd rect (at 68.49999 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "A80" smd rect (at 69.499988 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2052 "PEX_TX_C15"))
    (pad "A81" smd rect (at 70.499986 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2036 "PEX_TX_C15*"))
    (pad "A82" smd rect (at 71.499984 -5.251704) (size 0.699999 3.992397) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "B1" smd rect (at -11.500104 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1000 "12V"))
    (pad "B2" smd rect (at -10.500106 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1000 "12V"))
    (pad "B3" smd rect (at -9.500108 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1000 "12V"))
    (pad "B4" smd rect (at -8.50011 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B5" smd rect (at -7.500112 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2072 "SNN_PEX_I2CS_SCL"))
    (pad "B6" smd rect (at -6.500089 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2073 "SNN_PEX_I2CS_SDA"))
    (pad "B7" smd rect (at -5.500091 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B8" smd rect (at -4.500093 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1009 "3V3"))
    (pad "B9" smd rect (at -3.500095 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2078 "SNN_PEX_TRST*"))
    (pad "B10" smd rect (at -2.500097 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2028 "3V3_AUX"))
    (pad "B11" smd rect (at -1.500099 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2079 "SNN_PEX_08"))
    (pad "B12" smd rect (at 1.500099 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2065 "SNN_PEX_10"))
    (pad "B13" smd rect (at 2.500097 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B14" smd rect (at 3.500095 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1646 "PEX_RX0"))
    (pad "B15" smd rect (at 4.500093 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1125 "PEX_RX0*"))
    (pad "B16" smd rect (at 5.500091 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B17" smd rect (at 6.500089 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2062 "SNN_PEX_20"))
    (pad "B18" smd rect (at 7.500112 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B19" smd rect (at 8.50011 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1122 "PEX_RX1"))
    (pad "B20" smd rect (at 9.500108 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1123 "PEX_RX1*"))
    (pad "B21" smd rect (at 10.500106 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B22" smd rect (at 11.500104 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B23" smd rect (at 12.500102 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1523 "PEX_RX2"))
    (pad "B24" smd rect (at 13.5001 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1124 "PEX_RX2*"))
    (pad "B25" smd rect (at 14.500098 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B26" smd rect (at 15.500096 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B27" smd rect (at 16.500094 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1137 "PEX_RX3"))
    (pad "B28" smd rect (at 17.500092 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1138 "PEX_RX3*"))
    (pad "B29" smd rect (at 18.50009 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B30" smd rect (at 19.500088 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2067 "SNN_PEX_13"))
    (pad "B31" smd rect (at 20.500111 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2063 "SNN_PEX_11"))
    (pad "B32" smd rect (at 21.500109 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B33" smd rect (at 22.500107 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1170 "PEX_RX4"))
    (pad "B34" smd rect (at 23.500105 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1139 "PEX_RX4*"))
    (pad "B35" smd rect (at 24.500103 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B36" smd rect (at 25.500101 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B37" smd rect (at 26.500099 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1141 "PEX_RX5"))
    (pad "B38" smd rect (at 27.500097 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1142 "PEX_RX5*"))
    (pad "B39" smd rect (at 28.500095 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B40" smd rect (at 29.500093 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B41" smd rect (at 30.500091 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1143 "PEX_RX6"))
    (pad "B42" smd rect (at 31.500089 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1144 "PEX_RX6*"))
    (pad "B43" smd rect (at 32.500087 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B44" smd rect (at 33.500111 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B45" smd rect (at 34.500109 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1147 "PEX_RX7"))
    (pad "B46" smd rect (at 35.500107 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1148 "PEX_RX7*"))
    (pad "B47" smd rect (at 36.500105 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B48" smd rect (at 37.500103 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2064 "SNN_PEX_15"))
    (pad "B49" smd rect (at 38.500101 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B50" smd rect (at 39.499997 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1146 "PEX_RX8"))
    (pad "B51" smd rect (at 40.499995 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1647 "PEX_RX8*"))
    (pad "B52" smd rect (at 41.499993 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B53" smd rect (at 42.499991 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B54" smd rect (at 43.499989 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1151 "PEX_RX9"))
    (pad "B55" smd rect (at 44.500013 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1152 "PEX_RX9*"))
    (pad "B56" smd rect (at 45.500011 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B57" smd rect (at 46.500009 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B58" smd rect (at 47.500007 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1150 "PEX_RX10"))
    (pad "B59" smd rect (at 48.500005 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1648 "PEX_RX10*"))
    (pad "B60" smd rect (at 49.500003 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B61" smd rect (at 50.500001 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B62" smd rect (at 51.499999 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1128 "PEX_RX11"))
    (pad "B63" smd rect (at 52.499997 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1129 "PEX_RX11*"))
    (pad "B64" smd rect (at 53.499995 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B65" smd rect (at 54.499993 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B66" smd rect (at 55.499991 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1127 "PEX_RX12"))
    (pad "B67" smd rect (at 56.499989 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1649 "PEX_RX12*"))
    (pad "B68" smd rect (at 57.499987 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B69" smd rect (at 58.499985 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B70" smd rect (at 59.500008 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1132 "PEX_RX13"))
    (pad "B71" smd rect (at 60.500006 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1133 "PEX_RX13*"))
    (pad "B72" smd rect (at 61.500004 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B73" smd rect (at 62.500002 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B74" smd rect (at 63.5 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1131 "PEX_RX14"))
    (pad "B75" smd rect (at 64.499998 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1153 "PEX_RX14*"))
    (pad "B76" smd rect (at 65.499996 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B77" smd rect (at 66.499994 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B78" smd rect (at 67.499992 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1135 "PEX_RX15"))
    (pad "B79" smd rect (at 68.49999 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1136 "PEX_RX15*"))
    (pad "B80" smd rect (at 69.499988 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B81" smd rect (at 70.499707 -5.251704) (size 3.725189 6.1976) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2061 "PEX_PRSNT1*"))
    (pad "B82" smd rect (at 71.499984 -5.251704) (size 0.699999 3.992397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2071 "SNN_PEX_18"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 107.161399 72.105716)
    (fp_text reference "R39" (at -0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "2" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 358 "FBE_SEN1"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 159.573308 108.078212 -90)
    (fp_text reference "R48" (at 0 0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "2" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 748 "FBB_SEN1"))
  )
  (footprint "GEOM0027_1" (layer "F.Cu")
    (tedit 0)
    (at -0.014892 60.071907)
    (fp_text reference "MEC2" (at -1.27 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 71.181613 95.124415)
    (fp_text reference "C43" (at -0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "CAP_SMD_7343_1" (layer "F.Cu")
    (tedit 0)
    (at 51.166108 79.325412)
    (fp_text reference "C37" (at -0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -3.1115 0) (size 2.413 3.048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at 3.1115 0) (size 2.413 3.048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 161.859308 87.936012)
    (fp_text reference "C87" (at -0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0603_1" (layer "F.Cu")
    (tedit 0)
    (at 200.708608 140.653407 -90)
    (fp_text reference "C114" (at 0 1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.762 0 90) (size 0.889 0.7874) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "PS5_NVVDD_PHASE3"))
    (pad "2" smd rect (at 0.762 0 270) (size 0.889 0.7874) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1101 "PS5_NVVDD_RC3"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 241.475608 95.504907 90)
    (fp_text reference "R71" (at 0 -0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1983 "VID_PSI"))
    (pad "2" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0603_1" (layer "F.Cu")
    (tedit 0)
    (at 40.307608 153.289907)
    (fp_text reference "C24" (at -0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.762 0 180) (size 0.889 0.7874) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1000 "12V"))
    (pad "2" smd rect (at 0.762 0) (size 0.889 0.7874) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 20.902008 145.467215)
    (fp_text reference "C14" (at -0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "IND_SMD_0603_1" (layer "F.Cu")
    (tedit 0)
    (at 5.369908 145.568815 -90)
    (fp_text reference "L4" (at 0 0.635 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.762 0 90) (size 0.889 0.7874) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2007 "DACC_HSYNC_BUF"))
    (pad "2" smd rect (at 0.762 0 270) (size 0.889 0.7874) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1932 "DACC_HSYNC_CON"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 241.158108 115.951907 90)
    (fp_text reference "R70" (at 0 -0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1984 "PS5_NVVDD_EN_12V_F2"))
    (pad "2" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 21.422708 124.766012 90)
    (fp_text reference "C16" (at 0 -0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 223.251387 117.171615 -90)
    (fp_text reference "C123" (at 0 1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 983 "12V_PEX6_F2"))
    (pad "2" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "IND_SMD_0603_1" (layer "F.Cu")
    (tedit 0)
    (at 5.090508 109.272215 180)
    (fp_text reference "LB3" (at 0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.762 0) (size 0.889 0.7874) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1986 "GPIO1_DVICD_HPD_R"))
    (pad "2" smd rect (at 0.762 0 180) (size 0.889 0.7874) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1922 "GPIO1_DVICD_HPD_CON"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 75.357805 92.886904 90)
    (fp_text reference "C50" (at 0 -0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "1206_1" (layer "F.Cu")
    (tedit 0)
    (at 48.422908 141.148707)
    (fp_text reference "R28" (at -0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -1.4732 0) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1000 "12V"))
    (pad "2" smd rect (at 1.4732 0) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 991 "12V_F"))
  )
  (footprint "GEOM0008_1" (layer "F.Cu")
    (tedit 0)
    (at 213.777213 88.215615)
    (fp_text reference "Q14" (at 1.5875 2.217877 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -2.290115 5.31241) (size 1.6002 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 994 "PS5_NVVDD_LG2_AC"))
    (pad "2" smd rect (at 0 -1.867408) (size 5.799811 6.200089) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "PS5_NVVDD_PHASE2"))
    (pad "3" smd rect (at 2.290089 5.31241) (size 1.6002 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 6.970108 110.681407)
    (fp_text reference "C9" (at -0.635 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1986 "GPIO1_DVICD_HPD_R"))
    (pad "2" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 75.339821 90.49811 90)
    (fp_text reference "R33" (at 0 -0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "2" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 40 "FBF_SEN2"))
  )
  (footprint "GEOM0028_1" (layer "F.Cu")
    (tedit 0)
    (at 248.475619 137.844904 -90)
    (fp_text reference "J7" (at 0 -2.364994 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0 270) (size 1.5748 1.5748) (drill 0.9144) (layers *.Cu *.Mask)
      (net 1973 "FAN_PWM"))
    (pad "2" thru_hole circle (at 1.999996 0 270) (size 1.5748 1.5748) (drill 0.9144) (layers *.Cu *.Mask)
      (net 1975 "FAN_TACH"))
    (pad "3" thru_hole circle (at 3.999992 0 270) (size 1.5748 1.5748) (drill 0.9144) (layers *.Cu *.Mask)
      (net 983 "12V_PEX6_F2"))
    (pad "4" thru_hole circle (at 5.999988 0 270) (size 1.5748 1.5748) (drill 0.9144) (layers *.Cu *.Mask)
      (net 1 "GND"))
  )
  (footprint "0805_1" (layer "F.Cu")
    (tedit 0)
    (at 181.722108 126.873907 180)
    (fp_text reference "C103" (at 0.7874 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.9525 0 180) (size 1.143 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at 0.9525 0 180) (size 1.143 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 159.573308 60.478612 90)
    (fp_text reference "C75" (at 0 -0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 70.526013 96.572215 180)
    (fp_text reference "C40" (at 0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "SOT23_1" (layer "F.Cu")
    (tedit 0)
    (at 5.496908 114.276015 -90)
    (fp_text reference "D2" (at 0.635 -1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.9525 1.143 270) (size 0.9144 0.9144) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "2" smd rect (at 0.9525 1.143 270) (size 0.9144 0.9144) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1009 "3V3"))
    (pad "3" smd rect (at 0 -1.143 270) (size 0.9144 0.9144) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1796 "GPIO1_DVICD_HPD"))
  )
  (footprint "GEOM0004_1" (layer "F.Cu")
    (tedit 0)
    (at 193.533108 139.700907 90)
    (fp_text reference "L13" (at -1.27 1.5875 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 3.81 90) (size 4.0132 4.318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "PS5_NVVDD_PHASE3"))
    (pad "2" smd rect (at 0 -3.81 90) (size 4.0132 4.318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
  )
  (footprint "GEOM0005_1" (layer "F.Cu")
    (tedit 0)
    (at 123.620599 63.780815)
    (fp_text reference "M7" (at 1.27 0.635 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "A1" smd circle (at -4.400601 -6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "A2" smd circle (at -3.600399 -6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "A3" smd circle (at -2.800299 -6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "A4" smd circle (at -2.000301 -6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 434 "FBD_ZQ2"))
    (pad "A9" smd circle (at 2.000301 -6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "A10" smd circle (at 2.800299 -6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "A11" smd circle (at 3.600399 -6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "A12" smd circle (at 4.400601 -6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "B1" smd circle (at -4.400601 -5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B2" smd circle (at -3.600399 -5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 435 "FBD_D<63>"))
    (pad "B3" smd circle (at -2.800299 -5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 436 "FBD_D<58>"))
    (pad "B4" smd circle (at -2.000301 -5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B9" smd circle (at 2.000301 -5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B10" smd circle (at 2.800299 -5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 447 "FBD_D<35>"))
    (pad "B11" smd circle (at 3.600399 -5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 446 "FBD_D<34>"))
    (pad "B12" smd circle (at 4.400601 -5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "C1" smd circle (at -4.400601 -4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "C2" smd circle (at -3.600399 -4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 437 "FBD_D<60>"))
    (pad "C3" smd circle (at -2.800299 -4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 438 "FBD_D<59>"))
    (pad "C4" smd circle (at -2.000301 -4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "C9" smd circle (at 2.000301 -4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "C10" smd circle (at 2.800299 -4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 449 "FBD_D<33>"))
    (pad "C11" smd circle (at 3.600399 -4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 448 "FBD_D<32>"))
    (pad "C12" smd circle (at 4.400601 -4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "D1" smd circle (at -4.400601 -4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "D2" smd circle (at -3.600399 -4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 445 "FBD_DQS_WP7"))
    (pad "D3" smd circle (at -2.800299 -4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 444 "FBD_DQS_RN7"))
    (pad "D4" smd circle (at -2.000301 -4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "D9" smd circle (at 2.000301 -4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "D10" smd circle (at 2.800299 -4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 455 "FBD_DQS_RN4"))
    (pad "D11" smd circle (at 3.600399 -4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 456 "FBD_DQS_WP4"))
    (pad "D12" smd circle (at 4.400601 -4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "E1" smd circle (at -4.400601 -3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "E2" smd circle (at -3.600399 -3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 439 "FBD_D<56>"))
    (pad "E3" smd circle (at -2.800299 -3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 443 "FBD_DQM7"))
    (pad "E4" smd circle (at -2.000301 -3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "E9" smd circle (at 2.000301 -3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "E10" smd circle (at 2.800299 -3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 454 "FBD_DQM4"))
    (pad "E11" smd circle (at 3.600399 -3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 450 "FBD_D<39>"))
    (pad "E12" smd circle (at 4.400601 -3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "F1" smd circle (at -4.400601 -2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "F2" smd circle (at -3.600399 -2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 441 "FBD_D<57>"))
    (pad "F3" smd circle (at -2.800299 -2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 440 "FBD_D<61>"))
    (pad "F4" smd circle (at -2.000301 -2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 421 "FBD_CMD<16>"))
    (pad "F9" smd circle (at 2.000301 -2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 425 "FBD_CMD<17>"))
    (pad "F10" smd circle (at 2.800299 -2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 451 "FBD_D<38>"))
    (pad "F11" smd circle (at 3.600399 -2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 452 "FBD_D<36>"))
    (pad "F12" smd circle (at 4.400601 -2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "G1" smd circle (at -4.400601 -1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "G2" smd circle (at -3.600399 -1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "G3" smd circle (at -2.800299 -1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 442 "FBD_D<62>"))
    (pad "G4" smd circle (at -2.000301 -1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 418 "FBD_CMD<11>"))
    (pad "G9" smd circle (at 2.000301 -1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 419 "FBD_CMD<15>"))
    (pad "G10" smd circle (at 2.800299 -1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 453 "FBD_D<37>"))
    (pad "G11" smd circle (at 3.600399 -1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "G12" smd circle (at 4.400601 -1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "H1" smd circle (at -4.400601 -0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 431 "FBD_VREF3"))
    (pad "H2" smd circle (at -3.600399 -0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 410 "FBD_CMD<28>"))
    (pad "H3" smd circle (at -2.800299 -0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 426 "FBD_CMD<8>"))
    (pad "H4" smd circle (at -2.000301 -0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 422 "FBD_CMD<7>"))
    (pad "H9" smd circle (at 2.000301 -0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 433 "FBD_CMD<6>"))
    (pad "H10" smd circle (at 2.800299 -0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 420 "FBD_CMD<14>"))
    (pad "H11" smd circle (at 3.600399 -0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 414 "FBD_CMD<12>"))
    (pad "H12" smd circle (at 4.400601 -0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 432 "FBD_VREF4"))
    (pad "J1" smd circle (at -4.400601 0) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "J2" smd circle (at -3.600399 0) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 428 "SNN_FBD_NC04"))
    (pad "J3" smd circle (at -2.800299 0) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 429 "FBD_CMD<13>"))
    (pad "J4" smd circle (at -2.000301 0) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "J9" smd circle (at 2.000301 0) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "J10" smd circle (at 2.800299 0) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 424 "FBD1_CLK0*"))
    (pad "J11" smd circle (at 3.600399 0) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 423 "FBD1_CLK0"))
    (pad "J12" smd circle (at 4.400601 0) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "K1" smd circle (at -4.400601 0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "K2" smd circle (at -3.600399 0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 408 "FBD_CMD<19>"))
    (pad "K3" smd circle (at -2.800299 0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 411 "FBD_CMD<26>"))
    (pad "K4" smd circle (at -2.000301 0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 407 "FBD_CMD<25>"))
    (pad "K9" smd circle (at 2.000301 0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 413 "FBD_CMD<21>"))
    (pad "K10" smd circle (at 2.800299 0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 415 "FBD_CMD<23>"))
    (pad "K11" smd circle (at 3.600399 0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 406 "FBD_CMD<9>"))
    (pad "K12" smd circle (at 4.400601 0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "L1" smd circle (at -4.400601 1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "L2" smd circle (at -3.600399 1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "L3" smd circle (at -2.800299 1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 469 "FBD_D<50>"))
    (pad "L4" smd circle (at -2.000301 1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 409 "FBD_CMD<27>"))
    (pad "L9" smd circle (at 2.000301 1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 416 "FBD_CMD<20>"))
    (pad "L10" smd circle (at 2.800299 1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 458 "FBD_D<43>"))
    (pad "L11" smd circle (at 3.600399 1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "L12" smd circle (at 4.400601 1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "M1" smd circle (at -4.400601 2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "M2" smd circle (at -3.600399 2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 468 "FBD_D<54>"))
    (pad "M3" smd circle (at -2.800299 2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 471 "FBD_D<51>"))
    (pad "M4" smd circle (at -2.000301 2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 412 "FBD_CMD<18>"))
    (pad "M9" smd circle (at 2.000301 2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 417 "FBD_CMD<24>"))
    (pad "M10" smd circle (at 2.800299 2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 460 "FBD_D<40>"))
    (pad "M11" smd circle (at 3.600399 2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 457 "FBD_D<42>"))
    (pad "M12" smd circle (at 4.400601 2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N1" smd circle (at -4.400601 3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N2" smd circle (at -3.600399 3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 470 "FBD_D<48>"))
    (pad "N3" smd circle (at -2.800299 3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 476 "FBD_DQM6"))
    (pad "N4" smd circle (at -2.000301 3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N9" smd circle (at 2.000301 3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N10" smd circle (at 2.800299 3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 465 "FBD_DQM5"))
    (pad "N11" smd circle (at 3.600399 3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 459 "FBD_D<41>"))
    (pad "N12" smd circle (at 4.400601 3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "P1" smd circle (at -4.400601 4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "P2" smd circle (at -3.600399 4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 478 "FBD_DQS_WP6"))
    (pad "P3" smd circle (at -2.800299 4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 477 "FBD_DQS_RN6"))
    (pad "P4" smd circle (at -2.000301 4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "P9" smd circle (at 2.000301 4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "P10" smd circle (at 2.800299 4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 466 "FBD_DQS_RN5"))
    (pad "P11" smd circle (at 3.600399 4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 467 "FBD_DQS_WP5"))
    (pad "P12" smd circle (at 4.400601 4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "R1" smd circle (at -4.400601 4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "R2" smd circle (at -3.600399 4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 472 "FBD_D<53>"))
    (pad "R3" smd circle (at -2.800299 4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 473 "FBD_D<52>"))
    (pad "R4" smd circle (at -2.000301 4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "R9" smd circle (at 2.000301 4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "R10" smd circle (at 2.800299 4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 462 "FBD_D<47>"))
    (pad "R11" smd circle (at 3.600399 4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 461 "FBD_D<44>"))
    (pad "R12" smd circle (at 4.400601 4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "T1" smd circle (at -4.400601 5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T2" smd circle (at -3.600399 5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 474 "FBD_D<55>"))
    (pad "T3" smd circle (at -2.800299 5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 475 "FBD_D<49>"))
    (pad "T4" smd circle (at -2.000301 5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T9" smd circle (at 2.000301 5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T10" smd circle (at 2.800299 5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 464 "FBD_D<45>"))
    (pad "T11" smd circle (at 3.600399 5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 463 "FBD_D<46>"))
    (pad "T12" smd circle (at 4.400601 5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "V1" smd circle (at -4.400601 6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "V2" smd circle (at -3.600399 6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "V3" smd circle (at -2.800299 6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "V4" smd circle (at -2.000301 6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 430 "FBD_SEN2"))
    (pad "V9" smd circle (at 2.000301 6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 427 "FBD_CMD<10>"))
    (pad "V10" smd circle (at 2.800299 6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "V11" smd circle (at 3.600399 6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "V12" smd circle (at 4.400601 6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
  )
  (footprint "GEOM0023_1" (layer "F.Cu")
    (tedit 0)
    (at 85.964108 81.865615)
    (fp_text reference "MEC9" (at -1.27 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 3.5814 3.5814) (drill 2.4892) (layers *.Cu *.Mask)
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 12.126308 113.691612)
    (fp_text reference "R6" (at -0.635 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1750 "MIOA_CTL3"))
    (pad "2" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1009 "3V3"))
  )
  (footprint "GEOM0010_1" (layer "F.Cu")
    (tedit 0)
    (at 241.742308 132.919107 90)
    (fp_text reference "L15" (at -1.27 1.5875 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 2.500097 270) (size 7.500188 3.000197) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "INPUT_PEX6_IN2"))
    (pad "2" smd rect (at 0 -2.500097 90) (size 7.500188 3.000197) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 983 "12V_PEX6_F2"))
  )
  (footprint "GEOM0018_1" (layer "F.Cu")
    (tedit 0)
    (at -1.589692 128.677612 -90)
    (fp_text reference "J3" (at 2.099945 -8.89 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole rect (at 0 0 270) (size 1.2192 1.2192) (drill 0.8636) (layers *.Cu *.Mask)
      (net 1709 "IFPA_TXD2*"))
    (pad "2" thru_hole rect (at 1.905 0 270) (size 1.2192 1.2192) (drill 0.8636) (layers *.Cu *.Mask)
      (net 1708 "IFPA_TXD2"))
    (pad "3" thru_hole rect (at 3.81 0 270) (size 1.2192 1.2192) (drill 0.8636) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "4" thru_hole rect (at 5.715 0 270) (size 1.2192 1.2192) (drill 0.8636) (layers *.Cu *.Mask)
      (net 1717 "IFPB_TXD5*"))
    (pad "5" thru_hole rect (at 7.62 0 270) (size 1.2192 1.2192) (drill 0.8636) (layers *.Cu *.Mask)
      (net 1716 "IFPB_TXD5"))
    (pad "6" thru_hole rect (at 9.525 0 270) (size 1.2192 1.2192) (drill 0.8636) (layers *.Cu *.Mask)
      (net 1928 "I2C2_SCL_CON"))
    (pad "7" thru_hole rect (at 11.43 0 270) (size 1.2192 1.2192) (drill 0.8636) (layers *.Cu *.Mask)
      (net 1929 "I2C2_SDA_CON"))
    (pad "8" thru_hole rect (at 13.335 0 270) (size 1.2192 1.2192) (drill 0.8636) (layers *.Cu *.Mask)
      (net 1934 "DACC_VSYNC_CON"))
    (pad "9" thru_hole rect (at 0 1.905 270) (size 1.2192 1.2192) (drill 0.8636) (layers *.Cu *.Mask)
      (net 1707 "IFPA_TXD1*"))
    (pad "10" thru_hole rect (at 1.905 1.905 270) (size 1.2192 1.2192) (drill 0.8636) (layers *.Cu *.Mask)
      (net 1706 "IFPA_TXD1"))
    (pad "11" thru_hole rect (at 3.81 1.905 270) (size 1.2192 1.2192) (drill 0.8636) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "12" thru_hole rect (at 5.715 1.905 270) (size 1.2192 1.2192) (drill 0.8636) (layers *.Cu *.Mask)
      (net 1715 "IFPB_TXD4*"))
    (pad "13" thru_hole rect (at 7.62 1.905 270) (size 1.2192 1.2192) (drill 0.8636) (layers *.Cu *.Mask)
      (net 1714 "IFPB_TXD4"))
    (pad "14" thru_hole rect (at 9.525 1.905 270) (size 1.2192 1.2192) (drill 0.8636) (layers *.Cu *.Mask)
      (net 1925 "DDC_5V"))
    (pad "15" thru_hole rect (at 11.43 1.905 270) (size 1.2192 1.2192) (drill 0.8636) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "16" thru_hole rect (at 13.335 1.905 270) (size 1.2192 1.2192) (drill 0.8636) (layers *.Cu *.Mask)
      (net 1931 "GPIO0_DVIAB_HPD_CON"))
    (pad "17" thru_hole rect (at 0 3.81 270) (size 1.2192 1.2192) (drill 0.8636) (layers *.Cu *.Mask)
      (net 1705 "IFPA_TXD0*"))
    (pad "18" thru_hole rect (at 1.905 3.81 270) (size 1.2192 1.2192) (drill 0.8636) (layers *.Cu *.Mask)
      (net 1704 "IFPA_TXD0"))
    (pad "19" thru_hole rect (at 3.81 3.81 270) (size 1.2192 1.2192) (drill 0.8636) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "20" thru_hole rect (at 5.715 3.81 270) (size 1.2192 1.2192) (drill 0.8636) (layers *.Cu *.Mask)
      (net 1719 "IFPB_TXD6*"))
    (pad "21" thru_hole rect (at 7.62 3.81 270) (size 1.2192 1.2192) (drill 0.8636) (layers *.Cu *.Mask)
      (net 1718 "IFPB_TXD6"))
    (pad "22" thru_hole rect (at 9.525 3.81 270) (size 1.2192 1.2192) (drill 0.8636) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "23" thru_hole rect (at 11.43 3.81 270) (size 1.2192 1.2192) (drill 0.8636) (layers *.Cu *.Mask)
      (net 1702 "IFPA_TXC"))
    (pad "24" thru_hole rect (at 13.335 3.81 270) (size 1.2192 1.2192) (drill 0.8636) (layers *.Cu *.Mask)
      (net 1703 "IFPA_TXC*"))
    (pad "25" thru_hole circle (at -6.3754 5.334 79.7) (size 4.191 4.191) (drill 3.175) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "26" thru_hole circle (at 25.4254 5.334 280.2) (size 4.191 4.191) (drill 3.175) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "27" thru_hole circle (at -3.9751 -2.15011 270) (size 2.159 2.159) (drill 1.397) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "28" thru_hole circle (at 5.862599 -2.067611 270) (size 2.159 2.159) (drill 1.7272) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "29" thru_hole circle (at 12.932385 -2.067611 270) (size 2.159 2.159) (drill 1.7272) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "30" thru_hole circle (at 23.024795 -2.15011 270) (size 2.159 2.159) (drill 1.397) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "31" thru_hole circle (at -5.842 3.81 270) (size 3.048 3.048) (drill 1.9304) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "32" thru_hole circle (at 24.892 3.81 270) (size 3.048 3.048) (drill 1.9304) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "C1" thru_hole circle (at 16.515105 0.632511 270) (size 1.27 1.27) (drill 0.6604) (layers *.Cu *.Mask)
      (net 1933 "DACC_RED_CON"))
    (pad "C2" thru_hole circle (at 19.055105 0.632511 270) (size 1.27 1.27) (drill 0.6604) (layers *.Cu *.Mask)
      (net 1930 "DACC_GREEN_CON"))
    (pad "C3" thru_hole circle (at 16.515105 3.172511 270) (size 1.27 1.27) (drill 0.6604) (layers *.Cu *.Mask)
      (net 1927 "DACC_BLUE_CON"))
    (pad "C4" thru_hole circle (at 19.055105 3.172511 270) (size 1.27 1.27) (drill 0.6604) (layers *.Cu *.Mask)
      (net 1932 "DACC_HSYNC_CON"))
    (pad "C5" thru_hole circle (at 17.785105 4.439895 270) (size 1.27 1.27) (drill 0.6604) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "C5A" thru_hole circle (at 17.785105 -0.640105 270) (size 1.27 1.27) (drill 0.6604) (layers *.Cu *.Mask)
      (net 1 "GND"))
  )
  (footprint "GEOM0004_1" (layer "F.Cu")
    (tedit 0)
    (at 193.533108 87.376907 90)
    (fp_text reference "L9" (at -0.635 1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 3.81 90) (size 4.0132 4.318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "PS5_NVVDD_PHASE2"))
    (pad "2" smd rect (at 0 -3.81 90) (size 4.0132 4.318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
  )
  (footprint "1206_1" (layer "F.Cu")
    (tedit 0)
    (at 40.912103 142.088812 180)
    (fp_text reference "C26" (at 0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -1.4732 0 180) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1000 "12V"))
    (pad "2" smd rect (at 1.4732 0 180) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "SOT23_1" (layer "F.Cu")
    (tedit 0)
    (at 244.968108 93.536407 180)
    (fp_text reference "Q26" (at -1.359967 -1.11125 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.9525 1.143 180) (size 0.9144 0.9144) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 965 "PS5_NVVDD_VID1"))
    (pad "2" smd rect (at 0.9525 1.143 180) (size 0.9144 0.9144) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "3" smd rect (at 0 -1.143 180) (size 0.9144 0.9144) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1983 "VID_PSI"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 18.908108 123.115012)
    (fp_text reference "R12" (at -0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 976 "I2C3_SCL_R"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 193.469608 133.668407)
    (fp_text reference "R56" (at -0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 928 "PS5_NVVDD_VAMP_CSREF"))
  )
  (footprint "GEOM0017_1" (layer "F.Cu")
    (tedit 0)
    (at 15.961708 138.101215 180)
    (fp_text reference "Q1" (at -1.27 3.34645 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -2.286 0.0381 180) (size 1.397 2.9972) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1963 "PS1_2V5_LDO_DR"))
    (pad "2" smd rect (at 0 0 180) (size 1.4986 2.0066) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1009 "3V3"))
    (pad "3" smd rect (at 2.286 0.0381 180) (size 1.397 2.9972) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1790 "2V5"))
    (pad "4" smd rect (at 0 -6.2484 180) (size 5.9944 6.5024) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1009 "3V3"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 121.639221 72.086615)
    (fp_text reference "R40" (at -0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "2" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 430 "FBD_SEN2"))
  )
  (footprint "0805_1" (layer "F.Cu")
    (tedit 0)
    (at 148.511608 59.030812 90)
    (fp_text reference "C72" (at -0.000013 -0.787406 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.9525 0 90) (size 1.143 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at 0.9525 0 90) (size 1.143 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0805_1" (layer "F.Cu")
    (tedit 0)
    (at 181.722108 124.333907 180)
    (fp_text reference "C102" (at 0.7874 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.9525 0 180) (size 1.143 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at 0.9525 0 180) (size 1.143 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "1206_1" (layer "F.Cu")
    (tedit 0)
    (at 200.518108 106.109407 -90)
    (fp_text reference "R59" (at 0 0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -1.4732 0 270) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1103 "PS5_NVVDD_RC6"))
    (pad "2" smd rect (at 1.4732 0 270) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 159.497108 137.847012 -90)
    (fp_text reference "R44" (at 0 0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "2" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 878 "FBA_SEN1"))
  )
  (footprint "0603_1" (layer "F.Cu")
    (tedit 0)
    (at 39.253508 134.620907 90)
    (fp_text reference "C23" (at 0 -0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.762 0 270) (size 0.889 0.7874) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 991 "12V_F"))
    (pad "2" smd rect (at 0.762 0 90) (size 0.889 0.7874) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 159.573308 92.647102 -90)
    (fp_text reference "R47" (at 0 0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "2" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 690 "FBB_SEN2"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 134.351108 145.594012 180)
    (fp_text reference "R41" (at 0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1636 "I2CS_SCL"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 5.293708 117.806412)
    (fp_text reference "C8" (at -0.635 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1925 "DDC_5V"))
    (pad "2" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "GEOM0005_1" (layer "F.Cu")
    (tedit 0)
    (at 108.647807 63.780815)
    (fp_text reference "M6" (at 1.27 0.635 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "A1" smd circle (at -4.400601 -6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "A2" smd circle (at -3.600399 -6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "A3" smd circle (at -2.800299 -6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "A4" smd circle (at -2.000301 -6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 361 "FBE_ZQ1"))
    (pad "A9" smd circle (at 2.000301 -6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "A10" smd circle (at 2.800299 -6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "A11" smd circle (at 3.600399 -6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "A12" smd circle (at 4.400601 -6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "B1" smd circle (at -4.400601 -5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B2" smd circle (at -3.600399 -5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 362 "FBE_D<17>"))
    (pad "B3" smd circle (at -2.800299 -5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 363 "FBE_D<18>"))
    (pad "B4" smd circle (at -2.000301 -5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B9" smd circle (at 2.000301 -5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B10" smd circle (at 2.800299 -5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 374 "FBE_D<4>"))
    (pad "B11" smd circle (at 3.600399 -5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 373 "FBE_D<3>"))
    (pad "B12" smd circle (at 4.400601 -5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "C1" smd circle (at -4.400601 -4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "C2" smd circle (at -3.600399 -4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 364 "FBE_D<16>"))
    (pad "C3" smd circle (at -2.800299 -4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 365 "FBE_D<19>"))
    (pad "C4" smd circle (at -2.000301 -4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "C9" smd circle (at 2.000301 -4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "C10" smd circle (at 2.800299 -4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 376 "FBE_D<2>"))
    (pad "C11" smd circle (at 3.600399 -4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 375 "FBE_D<1>"))
    (pad "C12" smd circle (at 4.400601 -4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "D1" smd circle (at -4.400601 -4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "D2" smd circle (at -3.600399 -4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 372 "FBE_DQS_WP2"))
    (pad "D3" smd circle (at -2.800299 -4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 371 "FBE_DQS_RN2"))
    (pad "D4" smd circle (at -2.000301 -4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "D9" smd circle (at 2.000301 -4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "D10" smd circle (at 2.800299 -4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 382 "FBE_DQS_RN0"))
    (pad "D11" smd circle (at 3.600399 -4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 383 "FBE_DQS_WP0"))
    (pad "D12" smd circle (at 4.400601 -4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "E1" smd circle (at -4.400601 -3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "E2" smd circle (at -3.600399 -3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 366 "FBE_D<21>"))
    (pad "E3" smd circle (at -2.800299 -3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 370 "FBE_DQM2"))
    (pad "E4" smd circle (at -2.000301 -3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "E9" smd circle (at 2.000301 -3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "E10" smd circle (at 2.800299 -3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 381 "FBE_DQM0"))
    (pad "E11" smd circle (at 3.600399 -3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 377 "FBE_D<0>"))
    (pad "E12" smd circle (at 4.400601 -3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "F1" smd circle (at -4.400601 -2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "F2" smd circle (at -3.600399 -2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 368 "FBE_D<22>"))
    (pad "F3" smd circle (at -2.800299 -2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 367 "FBE_D<23>"))
    (pad "F4" smd circle (at -2.000301 -2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 295 "FBE_CMD<17>"))
    (pad "F9" smd circle (at 2.000301 -2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 291 "FBE_CMD<16>"))
    (pad "F10" smd circle (at 2.800299 -2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 378 "FBE_D<5>"))
    (pad "F11" smd circle (at 3.600399 -2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 379 "FBE_D<7>"))
    (pad "F12" smd circle (at 4.400601 -2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "G1" smd circle (at -4.400601 -1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "G2" smd circle (at -3.600399 -1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "G3" smd circle (at -2.800299 -1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 369 "FBE_D<20>"))
    (pad "G4" smd circle (at -2.000301 -1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 289 "FBE_CMD<15>"))
    (pad "G9" smd circle (at 2.000301 -1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 288 "FBE_CMD<11>"))
    (pad "G10" smd circle (at 2.800299 -1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 380 "FBE_D<6>"))
    (pad "G11" smd circle (at 3.600399 -1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "G12" smd circle (at 4.400601 -1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "H1" smd circle (at -4.400601 -0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 359 "FBE_VREF1"))
    (pad "H2" smd circle (at -3.600399 -0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 284 "FBE_CMD<12>"))
    (pad "H3" smd circle (at -2.800299 -0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 290 "FBE_CMD<14>"))
    (pad "H4" smd circle (at -2.000301 -0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 303 "FBE_CMD<6>"))
    (pad "H9" smd circle (at 2.000301 -0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 292 "FBE_CMD<7>"))
    (pad "H10" smd circle (at 2.800299 -0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 296 "FBE_CMD<8>"))
    (pad "H11" smd circle (at 3.600399 -0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 352 "FBE_CMD<0>"))
    (pad "H12" smd circle (at 4.400601 -0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 360 "FBE_VREF2"))
    (pad "J1" smd circle (at -4.400601 0) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "J2" smd circle (at -3.600399 0) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 357 "SNN_FBE_NC01"))
    (pad "J3" smd circle (at -2.800299 0) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 299 "FBE_CMD<13>"))
    (pad "J4" smd circle (at -2.000301 0) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "J9" smd circle (at 2.000301 0) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "J10" smd circle (at 2.800299 0) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 356 "FBE0_CLK0*"))
    (pad "J11" smd circle (at 3.600399 0) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 355 "FBE0_CLK0"))
    (pad "J12" smd circle (at 4.400601 0) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "K1" smd circle (at -4.400601 0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "K2" smd circle (at -3.600399 0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 276 "FBE_CMD<9>"))
    (pad "K3" smd circle (at -2.800299 0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 349 "FBE_CMD<5>"))
    (pad "K4" smd circle (at -2.000301 0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 283 "FBE_CMD<21>"))
    (pad "K9" smd circle (at 2.000301 0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 351 "FBE_CMD<3>"))
    (pad "K10" smd circle (at 2.800299 0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 353 "FBE_CMD<2>"))
    (pad "K11" smd circle (at 3.600399 0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 278 "FBE_CMD<19>"))
    (pad "K12" smd circle (at 4.400601 0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "L1" smd circle (at -4.400601 1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "L2" smd circle (at -3.600399 1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "L3" smd circle (at -2.800299 1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 396 "FBE_D<27>"))
    (pad "L4" smd circle (at -2.000301 1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 286 "FBE_CMD<20>"))
    (pad "L9" smd circle (at 2.000301 1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 354 "FBE_CMD<1>"))
    (pad "L10" smd circle (at 2.800299 1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 385 "FBE_D<11>"))
    (pad "L11" smd circle (at 3.600399 1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "L12" smd circle (at 4.400601 1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "M1" smd circle (at -4.400601 2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "M2" smd circle (at -3.600399 2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 395 "FBE_D<25>"))
    (pad "M3" smd circle (at -2.800299 2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 398 "FBE_D<24>"))
    (pad "M4" smd circle (at -2.000301 2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 350 "FBE_CMD<4>"))
    (pad "M9" smd circle (at 2.000301 2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 282 "FBE_CMD<18>"))
    (pad "M10" smd circle (at 2.800299 2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 387 "FBE_D<9>"))
    (pad "M11" smd circle (at 3.600399 2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 384 "FBE_D<10>"))
    (pad "M12" smd circle (at 4.400601 2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N1" smd circle (at -4.400601 3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N2" smd circle (at -3.600399 3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 397 "FBE_D<26>"))
    (pad "N3" smd circle (at -2.800299 3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 403 "FBE_DQM3"))
    (pad "N4" smd circle (at -2.000301 3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N9" smd circle (at 2.000301 3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N10" smd circle (at 2.800299 3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 392 "FBE_DQM1"))
    (pad "N11" smd circle (at 3.600399 3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 386 "FBE_D<8>"))
    (pad "N12" smd circle (at 4.400601 3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "P1" smd circle (at -4.400601 4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "P2" smd circle (at -3.600399 4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 405 "FBE_DQS_WP3"))
    (pad "P3" smd circle (at -2.800299 4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 404 "FBE_DQS_RN3"))
    (pad "P4" smd circle (at -2.000301 4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "P9" smd circle (at 2.000301 4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "P10" smd circle (at 2.800299 4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 393 "FBE_DQS_RN1"))
    (pad "P11" smd circle (at 3.600399 4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 394 "FBE_DQS_WP1"))
    (pad "P12" smd circle (at 4.400601 4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "R1" smd circle (at -4.400601 4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "R2" smd circle (at -3.600399 4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 399 "FBE_D<28>"))
    (pad "R3" smd circle (at -2.800299 4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 400 "FBE_D<31>"))
    (pad "R4" smd circle (at -2.000301 4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "R9" smd circle (at 2.000301 4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "R10" smd circle (at 2.800299 4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 389 "FBE_D<13>"))
    (pad "R11" smd circle (at 3.600399 4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 388 "FBE_D<12>"))
    (pad "R12" smd circle (at 4.400601 4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "T1" smd circle (at -4.400601 5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T2" smd circle (at -3.600399 5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 401 "FBE_D<30>"))
    (pad "T3" smd circle (at -2.800299 5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 402 "FBE_D<29>"))
    (pad "T4" smd circle (at -2.000301 5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T9" smd circle (at 2.000301 5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T10" smd circle (at 2.800299 5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 391 "FBE_D<14>"))
    (pad "T11" smd circle (at 3.600399 5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 390 "FBE_D<15>"))
    (pad "T12" smd circle (at 4.400601 5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "V1" smd circle (at -4.400601 6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "V2" smd circle (at -3.600399 6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "V3" smd circle (at -2.800299 6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "V4" smd circle (at -2.000301 6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 358 "FBE_SEN1"))
    (pad "V9" smd circle (at 2.000301 6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 297 "FBE_CMD<10>"))
    (pad "V10" smd circle (at 2.800299 6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "V11" smd circle (at 3.600399 6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "V12" smd circle (at 4.400601 6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
  )
  (footprint "0805_1" (layer "F.Cu")
    (tedit 0)
    (at 181.722108 99.314907 180)
    (fp_text reference "C98" (at 0.787406 -0.000013 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.9525 0 180) (size 1.143 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at 0.9525 0 180) (size 1.143 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "CAP_SMD_066X066_1" (layer "F.Cu")
    (tedit 0)
    (at 182.992108 106.934907 180)
    (fp_text reference "C106" (at 1.27 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -2.602992 0 180) (size 3.556 1.651) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at 2.602992 0 180) (size 3.556 1.651) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 203.947108 58.217707 90)
    (fp_text reference "R63" (at 0 -0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1991 "SPDIF_IN_C"))
    (pad "2" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1992 "SPDIF_IN_R"))
  )
  (footprint "GEOM0023_1" (layer "F.Cu")
    (tedit 0)
    (at 85.964108 142.825615)
    (fp_text reference "MEC10" (at -1.5875 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 3.5814 3.5814) (drill 2.4892) (layers *.Cu *.Mask)
      (net 1 "GND"))
  )
  (footprint "0603_1" (layer "F.Cu")
    (tedit 0)
    (at 246.682608 74.994407 -90)
    (fp_text reference "C144" (at 0 1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.762 0 90) (size 0.889 0.7874) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "INPUT_PEX6_IN2"))
    (pad "2" smd rect (at 0.762 0 270) (size 0.889 0.7874) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "CAP_SMD_7343_1" (layer "F.Cu")
    (tedit 0)
    (at 24.546908 142.368415 180)
    (fp_text reference "C21" (at 0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -3.1115 0 180) (size 2.413 3.048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at 3.1115 0 180) (size 2.413 3.048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "1206_1" (layer "F.Cu")
    (tedit 0)
    (at 227.696413 131.141615 -90)
    (fp_text reference "C134" (at 0 1.0795 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -1.4732 0 270) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 983 "12V_PEX6_F2"))
    (pad "2" smd rect (at 1.4732 0 270) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "GEOM0014_1" (layer "F.Cu")
    (tedit 0)
    (at 22.780109 55.3772)
    (fp_text reference "CN1" (at -0.952525 4.73235 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -11.454409 3.618713) (size 2.140991 4.4958) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "2" smd rect (at -11.454409 3.618713) (size 2.140991 4.4958) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "3" smd rect (at 11.454409 3.618713) (size 2.140991 4.4958) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "4" smd rect (at 11.454409 3.618713) (size 2.140991 4.4958) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "A1" smd rect (at 5.999988 5.249393 180) (size 0.699999 4.4958) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1075 "GPIO14_RASTERSYNC2_R"))
    (pad "A2" smd rect (at 4.99999 5.249393 180) (size 0.699999 4.4958) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1061 "DRB_D0"))
    (pad "A3" smd rect (at 3.999992 5.249393 180) (size 0.699999 4.4958) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "A4" smd rect (at 2.999994 5.249393 180) (size 0.699999 4.4958) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1065 "DRB_D2"))
    (pad "A5" smd rect (at 1.999996 5.249393 180) (size 0.699999 4.4958) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1066 "DRB_D3"))
    (pad "A6" smd rect (at 0.999998 5.249393 180) (size 0.699999 4.4958) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1068 "DRB_D5"))
    (pad "A7" smd rect (at 0 5.249393 180) (size 0.699999 4.4958) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "A8" smd rect (at -0.999998 5.249393 180) (size 0.699999 4.4958) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1069 "DRB_D6"))
    (pad "A9" smd rect (at -1.999996 5.249393 180) (size 0.699999 4.4958) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1077 "DRB_D14"))
    (pad "A10" smd rect (at -2.999994 5.249393 180) (size 0.699999 4.4958) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1072 "DRB_D9"))
    (pad "A11" smd rect (at -3.999992 5.249393 180) (size 0.699999 4.4958) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "A12" smd rect (at -4.99999 5.249393 180) (size 0.699999 4.4958) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1063 "DRB_D11"))
    (pad "A13" smd rect (at -5.999988 5.249393 180) (size 0.699999 4.4958) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1078 "DRB_D12"))
    (pad "B1" smd rect (at 5.999988 5.249393 180) (size 0.699999 4.4958) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1079 "GPIO15_SWAPRDY"))
    (pad "B2" smd rect (at 4.99999 5.249393 180) (size 0.699999 4.4958) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1074 "NVIO_EXT_REFCLKB_R"))
    (pad "B3" smd rect (at 3.999992 5.249393 180) (size 0.699999 4.4958) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B4" smd rect (at 2.999994 5.249393 180) (size 0.699999 4.4958) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1064 "DRB_D1"))
    (pad "B5" smd rect (at 1.999996 5.249393 180) (size 0.699999 4.4958) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1076 "DRB_D13"))
    (pad "B6" smd rect (at 0.999998 5.249393 180) (size 0.699999 4.4958) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1067 "DRB_D4"))
    (pad "B7" smd rect (at 0 5.249393 180) (size 0.699999 4.4958) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B8" smd rect (at -0.999998 5.249393 180) (size 0.699999 4.4958) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1060 "DRB_CLK"))
    (pad "B9" smd rect (at -1.999996 5.249393 180) (size 0.699999 4.4958) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1070 "DRB_D7"))
    (pad "B10" smd rect (at -2.999994 5.249393 180) (size 0.699999 4.4958) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1071 "DRB_D8"))
    (pad "B11" smd rect (at -3.999992 5.249393 180) (size 0.699999 4.4958) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B12" smd rect (at -4.99999 5.249393 180) (size 0.699999 4.4958) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1062 "DRB_D10"))
    (pad "B13" smd rect (at -5.999988 5.249393 180) (size 0.699999 4.4958) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1073 "DRB_CMD"))
  )
  (footprint "GEOM0005_1" (layer "F.Cu")
    (tedit 0)
    (at 167.879108 94.628607 -90)
    (fp_text reference "M11" (at 1.27 -1.5875 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "A1" smd circle (at -4.400601 -6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "A2" smd circle (at -3.600399 -6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "A3" smd circle (at -2.800299 -6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "A4" smd circle (at -2.000301 -6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 694 "FBB_ZQ2"))
    (pad "A9" smd circle (at 2.000301 -6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "A10" smd circle (at 2.800299 -6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "A11" smd circle (at 3.600399 -6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "A12" smd circle (at 4.400601 -6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "B1" smd circle (at -4.400601 -5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B2" smd circle (at -3.600399 -5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 695 "FBB_D<62>"))
    (pad "B3" smd circle (at -2.800299 -5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 696 "FBB_D<63>"))
    (pad "B4" smd circle (at -2.000301 -5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B9" smd circle (at 2.000301 -5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B10" smd circle (at 2.800299 -5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 707 "FBB_D<33>"))
    (pad "B11" smd circle (at 3.600399 -5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 706 "FBB_D<32>"))
    (pad "B12" smd circle (at 4.400601 -5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "C1" smd circle (at -4.400601 -4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "C2" smd circle (at -3.600399 -4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 697 "FBB_D<61>"))
    (pad "C3" smd circle (at -2.800299 -4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 698 "FBB_D<60>"))
    (pad "C4" smd circle (at -2.000301 -4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "C9" smd circle (at 2.000301 -4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "C10" smd circle (at 2.800299 -4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 709 "FBB_D<34>"))
    (pad "C11" smd circle (at 3.600399 -4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 708 "FBB_D<35>"))
    (pad "C12" smd circle (at 4.400601 -4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "D1" smd circle (at -4.400601 -4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "D2" smd circle (at -3.600399 -4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 705 "FBB_DQS_WP7"))
    (pad "D3" smd circle (at -2.800299 -4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 704 "FBB_DQS_RN7"))
    (pad "D4" smd circle (at -2.000301 -4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "D9" smd circle (at 2.000301 -4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "D10" smd circle (at 2.800299 -4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 715 "FBB_DQS_RN4"))
    (pad "D11" smd circle (at 3.600399 -4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 716 "FBB_DQS_WP4"))
    (pad "D12" smd circle (at 4.400601 -4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "E1" smd circle (at -4.400601 -3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "E2" smd circle (at -3.600399 -3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 699 "FBB_D<58>"))
    (pad "E3" smd circle (at -2.800299 -3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 703 "FBB_DQM7"))
    (pad "E4" smd circle (at -2.000301 -3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "E9" smd circle (at 2.000301 -3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "E10" smd circle (at 2.800299 -3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 714 "FBB_DQM4"))
    (pad "E11" smd circle (at 3.600399 -3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 710 "FBB_D<38>"))
    (pad "E12" smd circle (at 4.400601 -3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "F1" smd circle (at -4.400601 -2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "F2" smd circle (at -3.600399 -2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 701 "FBB_D<59>"))
    (pad "F3" smd circle (at -2.800299 -2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 700 "FBB_D<56>"))
    (pad "F4" smd circle (at -2.000301 -2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 681 "FBB_CMD<16>"))
    (pad "F9" smd circle (at 2.000301 -2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 685 "FBB_CMD<17>"))
    (pad "F10" smd circle (at 2.800299 -2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 711 "FBB_D<39>"))
    (pad "F11" smd circle (at 3.600399 -2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 712 "FBB_D<36>"))
    (pad "F12" smd circle (at 4.400601 -2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "G1" smd circle (at -4.400601 -1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "G2" smd circle (at -3.600399 -1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "G3" smd circle (at -2.800299 -1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 702 "FBB_D<57>"))
    (pad "G4" smd circle (at -2.000301 -1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 678 "FBB_CMD<11>"))
    (pad "G9" smd circle (at 2.000301 -1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 679 "FBB_CMD<15>"))
    (pad "G10" smd circle (at 2.800299 -1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 713 "FBB_D<37>"))
    (pad "G11" smd circle (at 3.600399 -1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "G12" smd circle (at 4.400601 -1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "H1" smd circle (at -4.400601 -0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 691 "FBB_VREF3"))
    (pad "H2" smd circle (at -3.600399 -0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 670 "FBB_CMD<28>"))
    (pad "H3" smd circle (at -2.800299 -0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 686 "FBB_CMD<8>"))
    (pad "H4" smd circle (at -2.000301 -0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 682 "FBB_CMD<7>"))
    (pad "H9" smd circle (at 2.000301 -0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 693 "FBB_CMD<6>"))
    (pad "H10" smd circle (at 2.800299 -0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 680 "FBB_CMD<14>"))
    (pad "H11" smd circle (at 3.600399 -0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 674 "FBB_CMD<12>"))
    (pad "H12" smd circle (at 4.400601 -0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 692 "FBB_VREF4"))
    (pad "J1" smd circle (at -4.400601 0 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "J2" smd circle (at -3.600399 0 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 688 "SNN_FBB_NC04"))
    (pad "J3" smd circle (at -2.800299 0 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 689 "FBB_CMD<13>"))
    (pad "J4" smd circle (at -2.000301 0 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "J9" smd circle (at 2.000301 0 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "J10" smd circle (at 2.800299 0 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 684 "FBB1_CLK0*"))
    (pad "J11" smd circle (at 3.600399 0 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 683 "FBB1_CLK0"))
    (pad "J12" smd circle (at 4.400601 0 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "K1" smd circle (at -4.400601 0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "K2" smd circle (at -3.600399 0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 668 "FBB_CMD<19>"))
    (pad "K3" smd circle (at -2.800299 0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 671 "FBB_CMD<26>"))
    (pad "K4" smd circle (at -2.000301 0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 667 "FBB_CMD<25>"))
    (pad "K9" smd circle (at 2.000301 0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 673 "FBB_CMD<21>"))
    (pad "K10" smd circle (at 2.800299 0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 675 "FBB_CMD<23>"))
    (pad "K11" smd circle (at 3.600399 0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 666 "FBB_CMD<9>"))
    (pad "K12" smd circle (at 4.400601 0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "L1" smd circle (at -4.400601 1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "L2" smd circle (at -3.600399 1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "L3" smd circle (at -2.800299 1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 729 "FBB_D<55>"))
    (pad "L4" smd circle (at -2.000301 1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 669 "FBB_CMD<27>"))
    (pad "L9" smd circle (at 2.000301 1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 676 "FBB_CMD<20>"))
    (pad "L10" smd circle (at 2.800299 1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 718 "FBB_D<42>"))
    (pad "L11" smd circle (at 3.600399 1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "L12" smd circle (at 4.400601 1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "M1" smd circle (at -4.400601 2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "M2" smd circle (at -3.600399 2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 728 "FBB_D<54>"))
    (pad "M3" smd circle (at -2.800299 2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 731 "FBB_D<53>"))
    (pad "M4" smd circle (at -2.000301 2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 672 "FBB_CMD<18>"))
    (pad "M9" smd circle (at 2.000301 2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 677 "FBB_CMD<24>"))
    (pad "M10" smd circle (at 2.800299 2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 720 "FBB_D<43>"))
    (pad "M11" smd circle (at 3.600399 2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 717 "FBB_D<40>"))
    (pad "M12" smd circle (at 4.400601 2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N1" smd circle (at -4.400601 3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N2" smd circle (at -3.600399 3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 730 "FBB_D<52>"))
    (pad "N3" smd circle (at -2.800299 3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 736 "FBB_DQM6"))
    (pad "N4" smd circle (at -2.000301 3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N9" smd circle (at 2.000301 3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N10" smd circle (at 2.800299 3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 725 "FBB_DQM5"))
    (pad "N11" smd circle (at 3.600399 3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 719 "FBB_D<41>"))
    (pad "N12" smd circle (at 4.400601 3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "P1" smd circle (at -4.400601 4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "P2" smd circle (at -3.600399 4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 738 "FBB_DQS_WP6"))
    (pad "P3" smd circle (at -2.800299 4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 737 "FBB_DQS_RN6"))
    (pad "P4" smd circle (at -2.000301 4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "P9" smd circle (at 2.000301 4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "P10" smd circle (at 2.800299 4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 726 "FBB_DQS_RN5"))
    (pad "P11" smd circle (at 3.600399 4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 727 "FBB_DQS_WP5"))
    (pad "P12" smd circle (at 4.400601 4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "R1" smd circle (at -4.400601 4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "R2" smd circle (at -3.600399 4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 732 "FBB_D<48>"))
    (pad "R3" smd circle (at -2.800299 4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 733 "FBB_D<51>"))
    (pad "R4" smd circle (at -2.000301 4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "R9" smd circle (at 2.000301 4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "R10" smd circle (at 2.800299 4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 722 "FBB_D<46>"))
    (pad "R11" smd circle (at 3.600399 4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 721 "FBB_D<45>"))
    (pad "R12" smd circle (at 4.400601 4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "T1" smd circle (at -4.400601 5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T2" smd circle (at -3.600399 5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 734 "FBB_D<50>"))
    (pad "T3" smd circle (at -2.800299 5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "FBB_D<49>"))
    (pad "T4" smd circle (at -2.000301 5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T9" smd circle (at 2.000301 5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T10" smd circle (at 2.800299 5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 724 "FBB_D<47>"))
    (pad "T11" smd circle (at 3.600399 5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 723 "FBB_D<44>"))
    (pad "T12" smd circle (at 4.400601 5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "V1" smd circle (at -4.400601 6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "V2" smd circle (at -3.600399 6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "V3" smd circle (at -2.800299 6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "V4" smd circle (at -2.000301 6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 690 "FBB_SEN2"))
    (pad "V9" smd circle (at 2.000301 6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 687 "FBB_CMD<10>"))
    (pad "V10" smd circle (at 2.800299 6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "V11" smd circle (at 3.600399 6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "V12" smd circle (at 4.400601 6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
  )
  (footprint "GEOM0015_1" (layer "F.Cu")
    (tedit 0)
    (at 116.444108 112.345615)
    (fp_text reference "G1" (at -0.635 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "A2" smd circle (at -20.800111 -21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1563 "SNN_GPU_NC_1"))
    (pad "A3" smd circle (at -20.000011 -21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1564 "SNN_GPU_NC_2"))
    (pad "A5" smd circle (at -18.399989 -21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "FBF_CMD<12>"))
    (pad "A6" smd circle (at -17.599889 -21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "FBF_CMD<10>"))
    (pad "A8" smd circle (at -15.999993 -21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "FBF_CMD<7>"))
    (pad "A9" smd circle (at -15.200097 -21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 219 "FBF_CMD<5>"))
    (pad "A11" smd circle (at -13.599897 -21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 223 "FBF_CMD<2>"))
    (pad "A12" smd circle (at -12.800101 -21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 222 "FBF_CMD<0>"))
    (pad "A14" smd circle (at -11.199901 -21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1277 "SNN_FBE_CMD<30>"))
    (pad "A15" smd circle (at -10.400005 -21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 280 "FBE_CMD<28>"))
    (pad "A17" smd circle (at -8.800109 -21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 277 "FBE_CMD<25>"))
    (pad "A18" smd circle (at -8.000009 -21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 285 "FBE_CMD<23>"))
    (pad "A20" smd circle (at -6.400013 -21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 286 "FBE_CMD<20>"))
    (pad "A21" smd circle (at -5.599913 -21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 282 "FBE_CMD<18>"))
    (pad "A23" smd circle (at -3.999992 -21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 289 "FBE_CMD<15>"))
    (pad "A24" smd circle (at -3.199892 -21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 299 "FBE_CMD<13>"))
    (pad "A26" smd circle (at -1.599895 -21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 297 "FBE_CMD<10>"))
    (pad "A27" smd circle (at -0.8001 -21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 296 "FBE_CMD<8>"))
    (pad "A29" smd circle (at 0.8001 -21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 292 "FBE_CMD<7>"))
    (pad "A30" smd circle (at 1.599895 -21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 349 "FBE_CMD<5>"))
    (pad "A32" smd circle (at 3.199892 -21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 351 "FBE_CMD<3>"))
    (pad "A33" smd circle (at 3.999992 -21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 354 "FBE_CMD<1>"))
    (pad "A35" smd circle (at 5.599887 -21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1259 "SNN_FBD_CMD<31>"))
    (pad "A36" smd circle (at 6.399987 -21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1257 "SNN_FBD_CMD<29>"))
    (pad "A38" smd circle (at 8.000009 -21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 411 "FBD_CMD<26>"))
    (pad "A39" smd circle (at 8.800109 -21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 417 "FBD_CMD<24>"))
    (pad "A41" smd circle (at 10.400005 -21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 413 "FBD_CMD<21>"))
    (pad "A42" smd circle (at 11.199901 -21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 408 "FBD_CMD<19>"))
    (pad "A44" smd circle (at 12.800101 -21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 419 "FBD_CMD<15>"))
    (pad "A45" smd circle (at 13.599897 -21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 420 "FBD_CMD<14>"))
    (pad "A47" smd circle (at 15.200097 -21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 418 "FBD_CMD<11>"))
    (pad "A48" smd circle (at 15.999993 -21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 406 "FBD_CMD<9>"))
    (pad "A50" smd circle (at 17.599889 -21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 433 "FBD_CMD<6>"))
    (pad "A51" smd circle (at 18.399989 -21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 479 "FBD_CMD<5>"))
    (pad "A53" smd circle (at 20.000011 -21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1565 "SNN_GPU_NC_3"))
    (pad "A54" smd circle (at 20.800111 -21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1566 "SNN_GPU_NC_4"))
    (pad "AA1" smd circle (at -21.599906 -5.599887) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 93 "FBG_CMD<12>"))
    (pad "AA2" smd circle (at -20.800111 -5.599887) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AA3" smd circle (at -20.000011 -5.599887) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 102 "FBG_CMD<11>"))
    (pad "AA4" smd circle (at -19.200114 -5.599887) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 46 "FBF_D<63>"))
    (pad "AA5" smd circle (at -18.399989 -5.599887) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AA6" smd circle (at -17.599889 -5.599887) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "FBF_D<61>"))
    (pad "AA7" smd circle (at -16.800093 -5.599887) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 48 "FBF_D<60>"))
    (pad "AA8" smd circle (at -15.999993 -5.599887) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AA9" smd circle (at -15.200097 -5.599887) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 135 "FBG_D<4>"))
    (pad "AA10" smd circle (at -14.399997 -5.599887) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 137 "FBG_DQM0"))
    (pad "AA11" smd circle (at -13.599897 -5.599887) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AA13" smd circle (at -12.000001 -5.599887) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AA15" smd circle (at -10.500106 -4.500093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AA16" smd circle (at -9.500108 -4.500093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AA17" smd circle (at -8.50011 -4.500093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AA18" smd circle (at -7.500112 -4.500093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AA19" smd circle (at -6.500089 -4.500093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AA20" smd circle (at -5.500091 -4.500093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AA21" smd circle (at -4.500093 -4.500093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AA22" smd circle (at -3.500095 -4.500093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AA23" smd circle (at -2.500097 -4.500093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AA24" smd circle (at -1.500099 -4.500093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AA25" smd circle (at -0.500101 -4.500093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AA26" smd circle (at 0.500101 -4.500093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AA27" smd circle (at 1.500099 -4.500093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AA28" smd circle (at 2.500097 -4.500093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AA29" smd circle (at 3.500095 -4.500093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AA30" smd circle (at 4.500093 -4.500093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AA31" smd circle (at 5.500091 -4.500093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AA32" smd circle (at 6.500089 -4.500093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AA33" smd circle (at 7.500112 -4.500093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AA34" smd circle (at 8.50011 -4.500093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AA35" smd circle (at 9.500108 -4.500093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AA36" smd circle (at 10.500106 -4.500093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AA43" smd circle (at 12.000001 -5.599887) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AA45" smd circle (at 13.599897 -5.599887) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AA46" smd circle (at 14.399997 -5.599887) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 616 "FBC0_CLK0*"))
    (pad "AA47" smd circle (at 15.200097 -5.599887) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 615 "FBC0_CLK0"))
    (pad "AA48" smd circle (at 15.999993 -5.599887) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AA49" smd circle (at 16.800093 -5.599887) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 634 "FBC_D<7>"))
    (pad "AA50" smd circle (at 17.599889 -5.599887) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 633 "FBC_D<6>"))
    (pad "AA51" smd circle (at 18.399989 -5.599887) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AA52" smd circle (at 19.200089 -5.599887) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 636 "FBC_D<4>"))
    (pad "AA53" smd circle (at 20.000011 -5.599887) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 609 "FBC_CMD<5>"))
    (pad "AA54" smd circle (at 20.800111 -5.599887) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AA55" smd circle (at 21.599906 -5.599887) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 610 "FBC_CMD<4>"))
    (pad "AB3" smd circle (at -20.000011 -4.800092) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1325 "SNN_FBG_DBI2"))
    (pad "AB4" smd circle (at -19.200114 -4.800092) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 154 "FBG_D<16>"))
    (pad "AB5" smd circle (at -18.399989 -4.800092) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 152 "FBG_D<17>"))
    (pad "AB8" smd circle (at -15.999993 -4.800092) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 136 "FBG_D<5>"))
    (pad "AB9" smd circle (at -15.200097 -4.800092) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1332 "SNN_FBG_DBI0"))
    (pad "AB11" smd circle (at -13.599897 -4.800092) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1292 "SNN_FBF1_CLK1"))
    (pad "AB13" smd circle (at -12.000001 -4.800092) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "AB15" smd circle (at -10.500106 -3.500095) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AB16" smd circle (at -9.500108 -3.500095) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AB17" smd circle (at -8.50011 -3.500095) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AB18" smd circle (at -7.500112 -3.500095) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AB19" smd circle (at -6.500089 -3.500095) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AB20" smd circle (at -5.500091 -3.500095) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AB21" smd circle (at -4.500093 -3.500095) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AB22" smd circle (at -3.500095 -3.500095) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AB23" smd circle (at -2.500097 -3.500095) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AB24" smd circle (at -1.500099 -3.500095) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AB25" smd circle (at -0.500101 -3.500095) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AB26" smd circle (at 0.500101 -3.500095) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AB27" smd circle (at 1.500099 -3.500095) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AB28" smd circle (at 2.500097 -3.500095) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AB29" smd circle (at 3.500095 -3.500095) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AB30" smd circle (at 4.500093 -3.500095) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AB31" smd circle (at 5.500091 -3.500095) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AB32" smd circle (at 6.500089 -3.500095) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AB33" smd circle (at 7.500112 -3.500095) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AB34" smd circle (at 8.50011 -3.500095) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AB35" smd circle (at 9.500108 -3.500095) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AB36" smd circle (at 10.500106 -3.500095) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AB43" smd circle (at 12.000001 -4.800092) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "AB45" smd circle (at 13.599897 -4.800092) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1230 "SNN_FBC0_CLK1*"))
    (pad "AB47" smd circle (at 15.200097 -4.800092) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 705 "FBB_DQS_WP7"))
    (pad "AB48" smd circle (at 15.999993 -4.800092) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 701 "FBB_D<59>"))
    (pad "AB51" smd circle (at 18.399989 -4.800092) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 729 "FBB_D<55>"))
    (pad "AB52" smd circle (at 19.200089 -4.800092) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 728 "FBB_D<54>"))
    (pad "AB53" smd circle (at 20.000011 -4.800092) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 635 "FBC_D<0>"))
    (pad "AC1" smd circle (at -21.599906 -3.999992) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 101 "FBG_CMD<15>"))
    (pad "AC2" smd circle (at -20.800111 -3.999992) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 109 "FBG_CMD<14>"))
    (pad "AC3" smd circle (at -20.000011 -3.999992) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 112 "FBG_CMD<13>"))
    (pad "AC4" smd circle (at -19.200114 -3.999992) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 156 "FBG_D<18>"))
    (pad "AC5" smd circle (at -18.399989 -3.999992) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 155 "FBG_D<19>"))
    (pad "AC6" smd circle (at -17.599889 -3.999992) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 133 "FBG_D<7>"))
    (pad "AC7" smd circle (at -16.800093 -3.999992) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 134 "FBG_D<6>"))
    (pad "AC8" smd circle (at -15.999993 -3.999992) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 140 "FBG_D<8>"))
    (pad "AC9" smd circle (at -15.200097 -3.999992) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 143 "FBG_D<9>"))
    (pad "AC10" smd circle (at -14.399997 -3.999992) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 141 "FBG_D<10>"))
    (pad "AC11" smd circle (at -13.599897 -3.999992) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1291 "SNN_FBF1_CLK1*"))
    (pad "AC13" smd circle (at -12.000001 -3.999992) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "AC15" smd circle (at -10.500106 -2.500097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AC16" smd circle (at -9.500108 -2.500097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AC17" smd circle (at -8.50011 -2.500097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AC18" smd circle (at -7.500112 -2.500097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AC19" smd circle (at -6.500089 -2.500097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AC20" smd circle (at -5.500091 -2.500097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AC21" smd circle (at -4.500093 -2.500097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AC22" smd circle (at -3.500095 -2.500097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AC23" smd circle (at -2.500097 -2.500097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AC24" smd circle (at -1.500099 -2.500097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AC25" smd circle (at -0.500101 -2.500097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AC26" smd circle (at 0.500101 -2.500097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AC27" smd circle (at 1.500099 -2.500097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AC28" smd circle (at 2.500097 -2.500097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AC29" smd circle (at 3.500095 -2.500097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AC30" smd circle (at 4.500093 -2.500097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AC31" smd circle (at 5.500091 -2.500097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AC32" smd circle (at 6.500089 -2.500097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AC33" smd circle (at 7.500112 -2.500097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AC34" smd circle (at 8.50011 -2.500097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AC35" smd circle (at 9.500108 -2.500097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AC36" smd circle (at 10.500106 -2.500097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AC43" smd circle (at 12.000001 -3.999992) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "AC45" smd circle (at 13.599897 -3.999992) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1229 "SNN_FBC0_CLK1"))
    (pad "AC46" smd circle (at 14.399997 -3.999992) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 702 "FBB_D<57>"))
    (pad "AC47" smd circle (at 15.200097 -3.999992) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 704 "FBB_DQS_RN7"))
    (pad "AC48" smd circle (at 15.999993 -3.999992) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 699 "FBB_D<58>"))
    (pad "AC49" smd circle (at 16.800093 -3.999992) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 738 "FBB_DQS_WP6"))
    (pad "AC50" smd circle (at 17.599889 -3.999992) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 736 "FBB_DQM6"))
    (pad "AC51" smd circle (at 18.399989 -3.999992) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 731 "FBB_D<53>"))
    (pad "AC52" smd circle (at 19.200089 -3.999992) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 730 "FBB_D<52>"))
    (pad "AC53" smd circle (at 20.000011 -3.999992) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 611 "FBC_CMD<3>"))
    (pad "AC54" smd circle (at 20.800111 -3.999992) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 613 "FBC_CMD<2>"))
    (pad "AC55" smd circle (at 21.599906 -3.999992) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 614 "FBC_CMD<1>"))
    (pad "AD1" smd circle (at -21.599906 -3.199892) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 104 "FBG_CMD<17>"))
    (pad "AD2" smd circle (at -20.800111 -3.199892) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AD3" smd circle (at -20.000011 -3.199892) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 108 "FBG_CMD<16>"))
    (pad "AD4" smd circle (at -19.200114 -3.199892) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 160 "FBG_DQS_RN2"))
    (pad "AD5" smd circle (at -18.399989 -3.199892) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AD6" smd circle (at -17.599889 -3.199892) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 158 "FBG_D<20>"))
    (pad "AD7" smd circle (at -16.800093 -3.199892) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 149 "FBG_DQS_RN1"))
    (pad "AD8" smd circle (at -15.999993 -3.199892) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AD9" smd circle (at -15.200097 -3.199892) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 148 "FBG_DQM1"))
    (pad "AD10" smd circle (at -14.399997 -3.199892) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 142 "FBG_D<11>"))
    (pad "AD11" smd circle (at -13.599897 -3.199892) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AD13" smd circle (at -12.000001 -3.199892) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AD15" smd circle (at -10.500106 -1.500099) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AD16" smd circle (at -9.500108 -1.500099) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AD17" smd circle (at -8.50011 -1.500099) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AD18" smd circle (at -7.500112 -1.500099) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AD19" smd circle (at -6.500089 -1.500099) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AD20" smd circle (at -5.500091 -1.500099) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AD21" smd circle (at -4.500093 -1.500099) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AD22" smd circle (at -3.500095 -1.500099) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AD23" smd circle (at -2.500097 -1.500099) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AD24" smd circle (at -1.500099 -1.500099) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AD25" smd circle (at -0.500101 -1.500099) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AD26" smd circle (at 0.500101 -1.500099) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AD27" smd circle (at 1.500099 -1.500099) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AD28" smd circle (at 2.500097 -1.500099) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AD29" smd circle (at 3.500095 -1.500099) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AD30" smd circle (at 4.500093 -1.500099) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AD31" smd circle (at 5.500091 -1.500099) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AD32" smd circle (at 6.500089 -1.500099) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AD33" smd circle (at 7.500112 -1.500099) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AD34" smd circle (at 8.50011 -1.500099) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AD35" smd circle (at 9.500108 -1.500099) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AD36" smd circle (at 10.500106 -1.500099) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AD43" smd circle (at 12.000001 -3.199892) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AD45" smd circle (at 13.599897 -3.199892) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AD46" smd circle (at 14.399997 -3.199892) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 700 "FBB_D<56>"))
    (pad "AD47" smd circle (at 15.200097 -3.199892) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 724 "FBB_D<47>"))
    (pad "AD48" smd circle (at 15.999993 -3.199892) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AD49" smd circle (at 16.800093 -3.199892) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1225 "SNN_FBB_DBI6"))
    (pad "AD50" smd circle (at 17.599889 -3.199892) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 737 "FBB_DQS_RN6"))
    (pad "AD51" smd circle (at 18.399989 -3.199892) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AD52" smd circle (at 19.200089 -3.199892) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 733 "FBB_D<51>"))
    (pad "AD53" smd circle (at 20.000011 -3.199892) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 612 "FBC_CMD<0>"))
    (pad "AD54" smd circle (at 20.800111 -3.199892) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AD55" smd circle (at 21.599906 -3.199892) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1238 "SNN_FBB_CMD<32>"))
    (pad "AE3" smd circle (at -20.000011 -2.399995) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 161 "FBG_DQS_WP2"))
    (pad "AE4" smd circle (at -19.200114 -2.399995) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 159 "FBG_DQM2"))
    (pad "AE5" smd circle (at -18.399989 -2.399995) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 151 "FBG_D<21>"))
    (pad "AE8" smd circle (at -15.999993 -2.399995) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 150 "FBG_DQS_WP1"))
    (pad "AE9" smd circle (at -15.200097 -2.399995) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 145 "FBG_D<12>"))
    (pad "AE11" smd circle (at -13.599897 -2.399995) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1311 "SNN_FBG0_CLK1"))
    (pad "AE13" smd circle (at -12.000001 -2.399995) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1595 "FBG_DEBUG"))
    (pad "AE15" smd circle (at -10.500106 -0.500101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AE16" smd circle (at -9.500108 -0.500101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AE17" smd circle (at -8.50011 -0.500101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AE18" smd circle (at -7.500112 -0.500101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AE19" smd circle (at -6.500089 -0.500101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AE20" smd circle (at -5.500091 -0.500101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AE21" smd circle (at -4.500093 -0.500101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AE22" smd circle (at -3.500095 -0.500101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AE23" smd circle (at -2.500097 -0.500101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AE24" smd circle (at -1.500099 -0.500101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AE25" smd circle (at -0.500101 -0.500101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1658 "SNN_NVVDD_GND_MSUR"))
    (pad "AE26" smd circle (at 0.500101 -0.500101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1553 "SNN_NVVDD_MSUR"))
    (pad "AE27" smd circle (at 1.500099 -0.500101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AE28" smd circle (at 2.500097 -0.500101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AE29" smd circle (at 3.500095 -0.500101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AE30" smd circle (at 4.500093 -0.500101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AE31" smd circle (at 5.500091 -0.500101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AE32" smd circle (at 6.500089 -0.500101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AE33" smd circle (at 7.500112 -0.500101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AE34" smd circle (at 8.50011 -0.500101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AE35" smd circle (at 9.500108 -0.500101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AE36" smd circle (at 10.500106 -0.500101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AE43" smd circle (at 12.000001 -2.399995) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "AE45" smd circle (at 13.599897 -2.399995) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1228 "FBCD_REFCLK"))
    (pad "AE47" smd circle (at 15.200097 -2.399995) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 722 "FBB_D<46>"))
    (pad "AE48" smd circle (at 15.999993 -2.399995) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 721 "FBB_D<45>"))
    (pad "AE51" smd circle (at 18.399989 -2.399995) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 734 "FBB_D<50>"))
    (pad "AE52" smd circle (at 19.200089 -2.399995) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 735 "FBB_D<49>"))
    (pad "AE53" smd circle (at 20.000011 -2.399995) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 732 "FBB_D<48>"))
    (pad "AF1" smd circle (at -21.599906 -1.599895) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 92 "FBG_CMD<20>"))
    (pad "AF2" smd circle (at -20.800111 -1.599895) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 89 "FBG_CMD<19>"))
    (pad "AF3" smd circle (at -20.000011 -1.599895) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 100 "FBG_CMD<18>"))
    (pad "AF4" smd circle (at -19.200114 -1.599895) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 153 "FBG_D<22>"))
    (pad "AF5" smd circle (at -18.399989 -1.599895) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 157 "FBG_D<23>"))
    (pad "AF6" smd circle (at -17.599889 -1.599895) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 144 "FBG_D<15>"))
    (pad "AF7" smd circle (at -16.800093 -1.599895) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 146 "FBG_D<14>"))
    (pad "AF8" smd circle (at -15.999993 -1.599895) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 147 "FBG_D<13>"))
    (pad "AF9" smd circle (at -15.200097 -1.599895) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 169 "FBG1_CLK0*"))
    (pad "AF10" smd circle (at -14.399997 -1.599895) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 168 "FBG1_CLK0"))
    (pad "AF11" smd circle (at -13.599897 -1.599895) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1310 "SNN_FBG0_CLK1*"))
    (pad "AF13" smd circle (at -12.000001 -1.599895) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "AF15" smd circle (at -10.500106 0.500101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AF16" smd circle (at -9.500108 0.500101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AF17" smd circle (at -8.50011 0.500101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AF18" smd circle (at -7.500112 0.500101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AF19" smd circle (at -6.500089 0.500101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AF20" smd circle (at -5.500091 0.500101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AF21" smd circle (at -4.500093 0.500101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AF22" smd circle (at -3.500095 0.500101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AF23" smd circle (at -2.500097 0.500101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AF24" smd circle (at -1.500099 0.500101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AF25" smd circle (at -0.500101 0.500101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AF26" smd circle (at 0.500101 0.500101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AF27" smd circle (at 1.500099 0.500101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AF28" smd circle (at 2.500097 0.500101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AF29" smd circle (at 3.500095 0.500101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AF30" smd circle (at 4.500093 0.500101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AF31" smd circle (at 5.500091 0.500101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AF32" smd circle (at 6.500089 0.500101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AF33" smd circle (at 7.500112 0.500101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AF34" smd circle (at 8.50011 0.500101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AF35" smd circle (at 9.500108 0.500101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AF36" smd circle (at 10.500106 0.500101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AF43" smd circle (at 12.000001 -1.599895) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "AF45" smd circle (at 13.599897 -1.599895) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1227 "FBCD_REFCLK*"))
    (pad "AF46" smd circle (at 14.399997 -1.599895) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 727 "FBB_DQS_WP5"))
    (pad "AF47" smd circle (at 15.200097 -1.599895) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 726 "FBB_DQS_RN5"))
    (pad "AF48" smd circle (at 15.999993 -1.599895) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 723 "FBB_D<44>"))
    (pad "AF49" smd circle (at 16.800093 -1.599895) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 711 "FBB_D<39>"))
    (pad "AF50" smd circle (at 17.599889 -1.599895) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 710 "FBB_D<38>"))
    (pad "AF51" smd circle (at 18.399989 -1.599895) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 713 "FBB_D<37>"))
    (pad "AF52" smd circle (at 19.200089 -1.599895) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 712 "FBB_D<36>"))
    (pad "AF53" smd circle (at 20.000011 -1.599895) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1217 "SNN_FBB_CMD<31>"))
    (pad "AF54" smd circle (at 20.800111 -1.599895) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1218 "SNN_FBB_CMD<30>"))
    (pad "AF55" smd circle (at 21.599906 -1.599895) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1216 "SNN_FBB_CMD<29>"))
    (pad "AG1" smd circle (at -21.599906 -0.8001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1317 "SNN_FBG_CMD<22>"))
    (pad "AG2" smd circle (at -20.800111 -0.8001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AG3" smd circle (at -20.000011 -0.8001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 90 "FBG_CMD<21>"))
    (pad "AG4" smd circle (at -19.200114 -0.8001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 201 "FBG_D<32>"))
    (pad "AG5" smd circle (at -18.399989 -0.8001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AG6" smd circle (at -17.599889 -0.8001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1329 "SNN_FBG_DBI1"))
    (pad "AG7" smd circle (at -16.800093 -0.8001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 128 "FBG_DQS_WP3"))
    (pad "AG8" smd circle (at -15.999993 -0.8001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AG9" smd circle (at -15.200097 -0.8001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 120 "FBG_D<25>"))
    (pad "AG10" smd circle (at -14.399997 -0.8001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 119 "FBG_D<24>"))
    (pad "AG11" smd circle (at -13.599897 -0.8001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AG13" smd circle (at -12.000001 -0.8001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AG15" smd circle (at -10.500106 1.500099) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AG16" smd circle (at -9.500108 1.500099) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AG17" smd circle (at -8.50011 1.500099) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AG18" smd circle (at -7.500112 1.500099) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AG19" smd circle (at -6.500089 1.500099) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AG20" smd circle (at -5.500091 1.500099) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AG21" smd circle (at -4.500093 1.500099) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AG22" smd circle (at -3.500095 1.500099) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AG23" smd circle (at -2.500097 1.500099) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AG24" smd circle (at -1.500099 1.500099) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AG25" smd circle (at -0.500101 1.500099) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AG26" smd circle (at 0.500101 1.500099) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AG27" smd circle (at 1.500099 1.500099) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AG28" smd circle (at 2.500097 1.500099) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AG29" smd circle (at 3.500095 1.500099) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AG30" smd circle (at 4.500093 1.500099) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AG31" smd circle (at 5.500091 1.500099) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AG32" smd circle (at 6.500089 1.500099) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AG33" smd circle (at 7.500112 1.500099) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AG34" smd circle (at 8.50011 1.500099) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AG35" smd circle (at 9.500108 1.500099) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AG36" smd circle (at 10.500106 1.500099) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AG43" smd circle (at 12.000001 -0.8001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AG45" smd circle (at 13.599897 -0.8001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AG46" smd circle (at 14.399997 -0.8001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1224 "SNN_FB_VREF0"))
    (pad "AG47" smd circle (at 15.200097 -0.8001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 720 "FBB_D<43>"))
    (pad "AG48" smd circle (at 15.999993 -0.8001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AG49" smd circle (at 16.800093 -0.8001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 714 "FBB_DQM4"))
    (pad "AG50" smd circle (at 17.599889 -0.8001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 716 "FBB_DQS_WP4"))
    (pad "AG51" smd circle (at 18.399989 -0.8001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AG52" smd circle (at 19.200089 -0.8001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 708 "FBB_D<35>"))
    (pad "AG53" smd circle (at 20.000011 -0.8001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 670 "FBB_CMD<28>"))
    (pad "AG54" smd circle (at 20.800111 -0.8001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AG55" smd circle (at 21.599906 -0.8001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 669 "FBB_CMD<27>"))
    (pad "AH3" smd circle (at -20.000011 0) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 199 "FBG_D<33>"))
    (pad "AH4" smd circle (at -19.200114 0) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 202 "FBG_D<34>"))
    (pad "AH5" smd circle (at -18.399989 0) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1333 "SNN_FBG_DBI4"))
    (pad "AH8" smd circle (at -15.999993 0) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 127 "FBG_DQS_RN3"))
    (pad "AH9" smd circle (at -15.200097 0) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 118 "FBG_D<26>"))
    (pad "AH11" smd circle (at -13.599897 0) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1463 "SNN_FB_VREF1"))
    (pad "AH13" smd circle (at -12.000001 0) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "AH15" smd circle (at -10.500106 2.500097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AH16" smd circle (at -9.500108 2.500097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AH17" smd circle (at -8.50011 2.500097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AH18" smd circle (at -7.500112 2.500097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AH19" smd circle (at -6.500089 2.500097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AH20" smd circle (at -5.500091 2.500097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AH21" smd circle (at -4.500093 2.500097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AH22" smd circle (at -3.500095 2.500097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AH23" smd circle (at -2.500097 2.500097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AH24" smd circle (at -1.500099 2.500097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AH25" smd circle (at -0.500101 2.500097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AH26" smd circle (at 0.500101 2.500097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AH27" smd circle (at 1.500099 2.500097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AH28" smd circle (at 2.500097 2.500097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AH29" smd circle (at 3.500095 2.500097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AH30" smd circle (at 4.500093 2.500097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AH31" smd circle (at 5.500091 2.500097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AH32" smd circle (at 6.500089 2.500097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AH33" smd circle (at 7.500112 2.500097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AH34" smd circle (at 8.50011 2.500097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AH35" smd circle (at 9.500108 2.500097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AH36" smd circle (at 10.500106 2.500097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AH43" smd circle (at 12.000001 0) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "AH45" smd circle (at 13.599897 0) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1462 "SNN_FBB_DBI5"))
    (pad "AH47" smd circle (at 15.200097 0) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 718 "FBB_D<42>"))
    (pad "AH48" smd circle (at 15.999993 0) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 725 "FBB_DQM5"))
    (pad "AH51" smd circle (at 18.399989 0) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 715 "FBB_DQS_RN4"))
    (pad "AH52" smd circle (at 19.200089 0) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 709 "FBB_D<34>"))
    (pad "AH53" smd circle (at 20.000011 0) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 671 "FBB_CMD<26>"))
    (pad "AJ1" smd circle (at -21.599906 0.8001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 166 "FBG_CMD<23>"))
    (pad "AJ2" smd circle (at -20.800111 0.8001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AJ3" smd circle (at -20.000011 0.8001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 167 "FBG_CMD<24>"))
    (pad "AJ4" smd circle (at -19.200114 0.8001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 203 "FBG_D<35>"))
    (pad "AJ5" smd circle (at -18.399989 0.8001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AJ6" smd circle (at -17.599889 0.8001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 125 "FBG_D<31>"))
    (pad "AJ7" smd circle (at -16.800093 0.8001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 126 "FBG_DQM3"))
    (pad "AJ8" smd circle (at -15.999993 0.8001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AJ9" smd circle (at -15.200097 0.8001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 121 "FBG_D<27>"))
    (pad "AJ10" smd circle (at -14.399997 0.8001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1327 "SNN_FBG_DBI3"))
    (pad "AJ11" smd circle (at -13.599897 0.8001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AJ13" smd circle (at -12.000001 0.8001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AJ15" smd circle (at -10.500106 3.500095) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AJ16" smd circle (at -9.500108 3.500095) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AJ17" smd circle (at -8.50011 3.500095) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AJ18" smd circle (at -7.500112 3.500095) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AJ19" smd circle (at -6.500089 3.500095) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AJ20" smd circle (at -5.500091 3.500095) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AJ21" smd circle (at -4.500093 3.500095) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AJ22" smd circle (at -3.500095 3.500095) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AJ23" smd circle (at -2.500097 3.500095) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AJ24" smd circle (at -1.500099 3.500095) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AJ25" smd circle (at -0.500101 3.500095) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1655 "NVVDD_SENSE_GND"))
    (pad "AJ26" smd circle (at 0.500101 3.500095) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1554 "NVVDD_SENSE"))
    (pad "AJ27" smd circle (at 1.500099 3.500095) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AJ28" smd circle (at 2.500097 3.500095) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AJ29" smd circle (at 3.500095 3.500095) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AJ30" smd circle (at 4.500093 3.500095) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AJ31" smd circle (at 5.500091 3.500095) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AJ32" smd circle (at 6.500089 3.500095) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AJ33" smd circle (at 7.500112 3.500095) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1656 "SNN_TSENSE_VREF"))
    (pad "AJ34" smd circle (at 8.50011 3.500095) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AJ35" smd circle (at 9.500108 3.500095) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AJ36" smd circle (at 10.500106 3.500095) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AJ43" smd circle (at 12.000001 0.8001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AJ45" smd circle (at 13.599897 0.8001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AJ46" smd circle (at 14.399997 0.8001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 717 "FBB_D<40>"))
    (pad "AJ47" smd circle (at 15.200097 0.8001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 719 "FBB_D<41>"))
    (pad "AJ48" smd circle (at 15.999993 0.8001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AJ49" smd circle (at 16.800093 0.8001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1226 "SNN_FBB_DBI4"))
    (pad "AJ50" smd circle (at 17.599889 0.8001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 706 "FBB_D<32>"))
    (pad "AJ51" smd circle (at 18.399989 0.8001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AJ52" smd circle (at 19.200089 0.8001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 707 "FBB_D<33>"))
    (pad "AJ53" smd circle (at 20.000011 0.8001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 677 "FBB_CMD<24>"))
    (pad "AJ54" smd circle (at 20.800111 0.8001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AJ55" smd circle (at 21.599906 0.8001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 667 "FBB_CMD<25>"))
    (pad "AK1" smd circle (at -21.599906 1.599895) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 162 "FBG_CMD<25>"))
    (pad "AK2" smd circle (at -20.800111 1.599895) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 165 "FBG_CMD<26>"))
    (pad "AK3" smd circle (at -20.000011 1.599895) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 163 "FBG_CMD<27>"))
    (pad "AK4" smd circle (at -19.200114 1.599895) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 205 "FBG_DQM4"))
    (pad "AK5" smd circle (at -18.399989 1.599895) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 207 "FBG_DQS_WP4"))
    (pad "AK6" smd circle (at -17.599889 1.599895) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 206 "FBG_DQS_RN4"))
    (pad "AK7" smd circle (at -16.800093 1.599895) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 122 "FBG_D<29>"))
    (pad "AK8" smd circle (at -15.999993 1.599895) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 124 "FBG_D<30>"))
    (pad "AK9" smd circle (at -15.200097 1.599895) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 123 "FBG_D<28>"))
    (pad "AK10" smd circle (at -14.399997 1.599895) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 214 "FBG_D<41>"))
    (pad "AK11" smd circle (at -13.599897 1.599895) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 215 "FBG_D<42>"))
    (pad "AK13" smd circle (at -12.000001 1.599895) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "AK15" smd circle (at -10.500106 4.500093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AK16" smd circle (at -9.500108 4.500093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AK17" smd circle (at -8.50011 4.500093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AK18" smd circle (at -7.500112 4.500093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AK19" smd circle (at -6.500089 4.500093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AK20" smd circle (at -5.500091 4.500093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AK21" smd circle (at -4.500093 4.500093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AK22" smd circle (at -3.500095 4.500093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AK23" smd circle (at -2.500097 4.500093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AK24" smd circle (at -1.500099 4.500093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AK25" smd circle (at -0.500101 4.500093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AK26" smd circle (at 0.500101 4.500093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AK27" smd circle (at 1.500099 4.500093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AK28" smd circle (at 2.500097 4.500093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AK29" smd circle (at 3.500095 4.500093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1552 "SNN_TS_OBS"))
    (pad "AK30" smd circle (at 4.500093 4.500093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AK31" smd circle (at 5.500091 4.500093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AK32" smd circle (at 6.500089 4.500093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AK33" smd circle (at 7.500112 4.500093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AK34" smd circle (at 8.50011 4.500093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1657 "SNN_TSENSE_AVDD"))
    (pad "AK35" smd circle (at 9.500108 4.500093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AK36" smd circle (at 10.500106 4.500093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AK43" smd circle (at 12.000001 1.599895) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "AK45" smd circle (at 13.599897 1.599895) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 683 "FBB1_CLK0"))
    (pad "AK46" smd circle (at 14.399997 1.599895) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 684 "FBB1_CLK0*"))
    (pad "AK47" smd circle (at 15.200097 1.599895) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 781 "FBB_D<30>"))
    (pad "AK48" smd circle (at 15.999993 1.599895) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 779 "FBB_D<31>"))
    (pad "AK49" smd circle (at 16.800093 1.599895) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 756 "FBB_D<20>"))
    (pad "AK50" smd circle (at 17.599889 1.599895) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 758 "FBB_D<21>"))
    (pad "AK51" smd circle (at 18.399989 1.599895) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 757 "FBB_D<22>"))
    (pad "AK52" smd circle (at 19.200089 1.599895) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 759 "FBB_D<23>"))
    (pad "AK53" smd circle (at 20.000011 1.599895) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 673 "FBB_CMD<21>"))
    (pad "AK54" smd circle (at 20.800111 1.599895) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1215 "SNN_FBB_CMD<22>"))
    (pad "AK55" smd circle (at 21.599906 1.599895) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 675 "FBB_CMD<23>"))
    (pad "AL3" smd circle (at -20.000011 2.399995) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 200 "FBG_D<36>"))
    (pad "AL4" smd circle (at -19.200114 2.399995) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 197 "FBG_D<37>"))
    (pad "AL5" smd circle (at -18.399989 2.399995) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 204 "FBG_D<38>"))
    (pad "AL8" smd circle (at -15.999993 2.399995) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 217 "FBG_DQS_RN5"))
    (pad "AL9" smd circle (at -15.200097 2.399995) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 212 "FBG_D<40>"))
    (pad "AL11" smd circle (at -13.599897 2.399995) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 213 "FBG_D<43>"))
    (pad "AL13" smd circle (at -12.000001 2.399995) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "AL15" smd circle (at -10.500106 5.500091) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AL16" smd circle (at -9.500108 5.500091) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AL17" smd circle (at -8.50011 5.500091) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AL18" smd circle (at -7.500112 5.500091) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AL19" smd circle (at -6.500089 5.500091) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AL20" smd circle (at -5.500091 5.500091) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AL21" smd circle (at -4.500093 5.500091) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AL22" smd circle (at -3.500095 5.500091) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AL23" smd circle (at -2.500097 5.500091) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AL24" smd circle (at -1.500099 5.500091) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AL25" smd circle (at -0.500101 5.500091) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AL26" smd circle (at 0.500101 5.500091) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AL27" smd circle (at 1.500099 5.500091) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AL28" smd circle (at 2.500097 5.500091) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AL29" smd circle (at 3.500095 5.500091) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AL30" smd circle (at 4.500093 5.500091) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AL31" smd circle (at 5.500091 5.500091) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AL32" smd circle (at 6.500089 5.500091) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AL33" smd circle (at 7.500112 5.500091) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AL34" smd circle (at 8.50011 5.500091) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AL35" smd circle (at 9.500108 5.500091) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AL36" smd circle (at 10.500106 5.500091) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AL43" smd circle (at 12.000001 2.399995) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "AL45" smd circle (at 13.599897 2.399995) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1212 "SNN_FBB_DBI3"))
    (pad "AL47" smd circle (at 15.200097 2.399995) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 780 "FBB_D<29>"))
    (pad "AL48" smd circle (at 15.999993 2.399995) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 783 "FBB_DQS_RN3"))
    (pad "AL51" smd circle (at 18.399989 2.399995) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 761 "FBB_DQS_RN2"))
    (pad "AL52" smd circle (at 19.200089 2.399995) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 760 "FBB_DQM2"))
    (pad "AL53" smd circle (at 20.000011 2.399995) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 676 "FBB_CMD<20>"))
    (pad "AM1" smd circle (at -21.599906 3.199892) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 164 "FBG_CMD<28>"))
    (pad "AM2" smd circle (at -20.800111 3.199892) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AM3" smd circle (at -20.000011 3.199892) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1318 "SNN_FBG_CMD<29>"))
    (pad "AM4" smd circle (at -19.200114 3.199892) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 198 "FBG_D<39>"))
    (pad "AM5" smd circle (at -18.399989 3.199892) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AM6" smd circle (at -17.599889 3.199892) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 187 "FBG_D<48>"))
    (pad "AM7" smd circle (at -16.800093 3.199892) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 218 "FBG_DQS_WP5"))
    (pad "AM8" smd circle (at -15.999993 3.199892) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AM9" smd circle (at -15.200097 3.199892) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 216 "FBG_DQM5"))
    (pad "AM10" smd circle (at -14.399997 3.199892) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 210 "FBG_D<44>"))
    (pad "AM11" smd circle (at -13.599897 3.199892) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AM13" smd circle (at -12.000001 3.199892) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AM15" smd circle (at -10.500106 6.500114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AM16" smd circle (at -9.500108 6.500114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AM17" smd circle (at -8.50011 6.500114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AM18" smd circle (at -7.500112 6.500114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AM19" smd circle (at -6.500089 6.500114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AM20" smd circle (at -5.500091 6.500114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AM21" smd circle (at -4.500093 6.500114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AM22" smd circle (at -3.500095 6.500114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AM23" smd circle (at -2.500097 6.500114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AM24" smd circle (at -1.500099 6.500114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AM25" smd circle (at -0.500101 6.500114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AM26" smd circle (at 0.500101 6.500114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AM27" smd circle (at 1.500099 6.500114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AM28" smd circle (at 2.500097 6.500114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AM29" smd circle (at 3.500095 6.500114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AM30" smd circle (at 4.500093 6.500114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AM31" smd circle (at 5.500091 6.500114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AM32" smd circle (at 6.500089 6.500114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AM33" smd circle (at 7.500112 6.500114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AM34" smd circle (at 8.50011 6.500114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AM35" smd circle (at 9.500108 6.500114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AM36" smd circle (at 10.500106 6.500114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AM43" smd circle (at 12.000001 3.199892) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AM45" smd circle (at 13.599897 3.199892) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AM46" smd circle (at 14.399997 3.199892) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 782 "FBB_DQM3"))
    (pad "AM47" smd circle (at 15.200097 3.199892) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 784 "FBB_DQS_WP3"))
    (pad "AM48" smd circle (at 15.999993 3.199892) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AM49" smd circle (at 16.800093 3.199892) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 778 "FBB_D<24>"))
    (pad "AM50" smd circle (at 17.599889 3.199892) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 762 "FBB_DQS_WP2"))
    (pad "AM51" smd circle (at 18.399989 3.199892) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AM52" smd circle (at 19.200089 3.199892) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1220 "SNN_FBB_DBI2"))
    (pad "AM53" smd circle (at 20.000011 3.199892) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 672 "FBB_CMD<18>"))
    (pad "AM54" smd circle (at 20.800111 3.199892) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AM55" smd circle (at 21.599906 3.199892) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 668 "FBB_CMD<19>"))
    (pad "AN1" smd circle (at -21.599906 3.999992) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1319 "SNN_FBG_CMD<30>"))
    (pad "AN2" smd circle (at -20.800111 3.999992) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1321 "SNN_FBG_CMD<31>"))
    (pad "AN3" smd circle (at -20.000011 3.999992) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1336 "SNN_FBG_CMD<32>"))
    (pad "AN4" smd circle (at -19.200114 3.999992) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 195 "FBG_DQS_RN6"))
    (pad "AN5" smd circle (at -18.399989 3.999992) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 188 "FBG_D<50>"))
    (pad "AN6" smd circle (at -17.599889 3.999992) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 189 "FBG_D<49>"))
    (pad "AN7" smd circle (at -16.800093 3.999992) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 180 "FBG_D<56>"))
    (pad "AN8" smd circle (at -15.999993 3.999992) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 208 "FBG_D<46>"))
    (pad "AN9" smd circle (at -15.200097 3.999992) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 209 "FBG_D<45>"))
    (pad "AN10" smd circle (at -14.399997 3.999992) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1326 "SNN_FBG_DBI5"))
    (pad "AN11" smd circle (at -13.599897 3.999992) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1312 "SNN_FBG1_CLK1"))
    (pad "AN13" smd circle (at -12.000001 3.999992) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1475 "SNN_FBVDDQ_MSUR"))
    (pad "AN15" smd circle (at -10.500106 7.500112) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AN16" smd circle (at -9.500108 7.500112) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AN17" smd circle (at -8.50011 7.500112) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AN18" smd circle (at -7.500112 7.500112) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AN19" smd circle (at -6.500089 7.500112) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AN20" smd circle (at -5.500091 7.500112) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AN21" smd circle (at -4.500093 7.500112) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AN22" smd circle (at -3.500095 7.500112) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AN23" smd circle (at -2.500097 7.500112) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AN24" smd circle (at -1.500099 7.500112) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AN25" smd circle (at -0.500101 7.500112) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AN26" smd circle (at 0.500101 7.500112) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AN27" smd circle (at 1.500099 7.500112) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AN28" smd circle (at 2.500097 7.500112) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AN29" smd circle (at 3.500095 7.500112) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AN30" smd circle (at 4.500093 7.500112) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AN31" smd circle (at 5.500091 7.500112) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AN32" smd circle (at 6.500089 7.500112) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AN33" smd circle (at 7.500112 7.500112) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AN34" smd circle (at 8.50011 7.500112) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AN35" smd circle (at 9.500108 7.500112) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AN36" smd circle (at 10.500106 7.500112) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AN43" smd circle (at 12.000001 3.999992) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AN45" smd circle (at 13.599897 3.999992) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1214 "SNN_FBB1_CLK1*"))
    (pad "AN46" smd circle (at 14.399997 3.999992) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 776 "FBB_D<28>"))
    (pad "AN47" smd circle (at 15.200097 3.999992) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 777 "FBB_D<27>"))
    (pad "AN48" smd circle (at 15.999993 3.999992) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 775 "FBB_D<26>"))
    (pad "AN49" smd circle (at 16.800093 3.999992) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 774 "FBB_D<25>"))
    (pad "AN50" smd circle (at 17.599889 3.999992) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 755 "FBB_D<19>"))
    (pad "AN51" smd circle (at 18.399989 3.999992) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 754 "FBB_D<18>"))
    (pad "AN52" smd circle (at 19.200089 3.999992) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 753 "FBB_D<17>"))
    (pad "AN53" smd circle (at 20.000011 3.999992) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 681 "FBB_CMD<16>"))
    (pad "AN54" smd circle (at 20.800111 3.999992) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 685 "FBB_CMD<17>"))
    (pad "AN55" smd circle (at 21.599906 3.999992) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 679 "FBB_CMD<15>"))
    (pad "AP3" smd circle (at -20.000011 4.800092) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 194 "FBG_DQM6"))
    (pad "AP4" smd circle (at -19.200114 4.800092) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 196 "FBG_DQS_WP6"))
    (pad "AP5" smd circle (at -18.399989 4.800092) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 186 "FBG_D<51>"))
    (pad "AP8" smd circle (at -15.999993 4.800092) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 211 "FBG_D<47>"))
    (pad "AP9" smd circle (at -15.200097 4.800092) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 177 "FBG_D<57>"))
    (pad "AP11" smd circle (at -13.599897 4.800092) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1313 "SNN_FBG1_CLK1*"))
    (pad "AP13" smd circle (at -12.000001 4.800092) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1476 "SNN_FBVDDQ_GND_MSUR"))
    (pad "AP15" smd circle (at -10.500106 8.50011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AP16" smd circle (at -9.500108 8.50011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AP17" smd circle (at -8.50011 8.50011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AP18" smd circle (at -7.500112 8.50011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AP19" smd circle (at -6.500089 8.50011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AP20" smd circle (at -5.500091 8.50011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AP21" smd circle (at -4.500093 8.50011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AP22" smd circle (at -3.500095 8.50011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AP23" smd circle (at -2.500097 8.50011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AP24" smd circle (at -1.500099 8.50011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AP25" smd circle (at -0.500101 8.50011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AP26" smd circle (at 0.500101 8.50011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AP27" smd circle (at 1.500099 8.50011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AP28" smd circle (at 2.500097 8.50011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AP29" smd circle (at 3.500095 8.50011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AP30" smd circle (at 4.500093 8.50011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AP31" smd circle (at 5.500091 8.50011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AP32" smd circle (at 6.500089 8.50011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AP33" smd circle (at 7.500112 8.50011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AP34" smd circle (at 8.50011 8.50011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AP35" smd circle (at 9.500108 8.50011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AP36" smd circle (at 10.500106 8.50011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AP43" smd circle (at 12.000001 4.800092) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1477 "FBVDDQ_SENSE"))
    (pad "AP45" smd circle (at 13.599897 4.800092) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1213 "SNN_FBB1_CLK1"))
    (pad "AP47" smd circle (at 15.200097 4.800092) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 790 "FBB_D<14>"))
    (pad "AP48" smd circle (at 15.999993 4.800092) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 791 "FBB_D<15>"))
    (pad "AP51" smd circle (at 18.399989 4.800092) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1221 "SNN_FBB_DBI0"))
    (pad "AP52" smd circle (at 19.200089 4.800092) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 752 "FBB_D<16>"))
    (pad "AP53" smd circle (at 20.000011 4.800092) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 680 "FBB_CMD<14>"))
    (pad "AR1" smd circle (at -21.599906 5.599913) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1320 "SNN_FBH_CMD<0>"))
    (pad "AR2" smd circle (at -20.800111 5.599913) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AR3" smd circle (at -20.000011 5.599913) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1324 "SNN_FBH_CMD<1>"))
    (pad "AR4" smd circle (at -19.200114 5.599913) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 192 "FBG_D<52>"))
    (pad "AR5" smd circle (at -18.399989 5.599913) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AR6" smd circle (at -17.599889 5.599913) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1335 "SNN_FBG_DBI6"))
    (pad "AR7" smd circle (at -16.800093 5.599913) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 181 "FBG_D<59>"))
    (pad "AR8" smd circle (at -15.999993 5.599913) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AR9" smd circle (at -15.200097 5.599913) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 175 "FBG_D<58>"))
    (pad "AR10" smd circle (at -14.399997 5.599913) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1330 "SNN_FBG_DBI7"))
    (pad "AR11" smd circle (at -13.599897 5.599913) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AR13" smd circle (at -12.000001 5.599913) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AR15" smd circle (at -10.500106 9.500108) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AR16" smd circle (at -9.500108 9.500108) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AR17" smd circle (at -8.50011 9.500108) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AR18" smd circle (at -7.500112 9.500108) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AR19" smd circle (at -6.500089 9.500108) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AR20" smd circle (at -5.500091 9.500108) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AR21" smd circle (at -4.500093 9.500108) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AR22" smd circle (at -3.500095 9.500108) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AR23" smd circle (at -2.500097 9.500108) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AR24" smd circle (at -1.500099 9.500108) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AR25" smd circle (at -0.500101 9.500108) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AR26" smd circle (at 0.500101 9.500108) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AR27" smd circle (at 1.500099 9.500108) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AR28" smd circle (at 2.500097 9.500108) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AR29" smd circle (at 3.500095 9.500108) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AR30" smd circle (at 4.500093 9.500108) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AR31" smd circle (at 5.500091 9.500108) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AR32" smd circle (at 6.500089 9.500108) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AR33" smd circle (at 7.500112 9.500108) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AR34" smd circle (at 8.50011 9.500108) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AR35" smd circle (at 9.500108 9.500108) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AR36" smd circle (at 10.500106 9.500108) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AR43" smd circle (at 12.000001 5.599913) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AR45" smd circle (at 13.599897 5.599913) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AR46" smd circle (at 14.399997 5.599913) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 789 "FBB_D<13>"))
    (pad "AR47" smd circle (at 15.200097 5.599913) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1222 "SNN_FBB_DBI1"))
    (pad "AR48" smd circle (at 15.999993 5.599913) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AR49" smd circle (at 16.800093 5.599913) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 766 "FBB_D<5>"))
    (pad "AR50" smd circle (at 17.599889 5.599913) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 764 "FBB_D<6>"))
    (pad "AR51" smd circle (at 18.399989 5.599913) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AR52" smd circle (at 19.200089 5.599913) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 770 "FBB_D<7>"))
    (pad "AR53" smd circle (at 20.000011 5.599913) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 674 "FBB_CMD<12>"))
    (pad "AR54" smd circle (at 20.800111 5.599913) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AR55" smd circle (at 21.599906 5.599913) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 689 "FBB_CMD<13>"))
    (pad "AT1" smd circle (at -21.599906 6.400013) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1322 "SNN_FBH_CMD<2>"))
    (pad "AT2" smd circle (at -20.800111 6.400013) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1323 "SNN_FBH_CMD<3>"))
    (pad "AT3" smd circle (at -20.000011 6.400013) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1434 "SNN_FBH_CMD<4>"))
    (pad "AT4" smd circle (at -19.200114 6.400013) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 190 "FBG_D<53>"))
    (pad "AT5" smd circle (at -18.399989 6.400013) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 191 "FBG_D<54>"))
    (pad "AT6" smd circle (at -17.599889 6.400013) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 193 "FBG_D<55>"))
    (pad "AT7" smd circle (at -16.800093 6.400013) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 179 "FBG_D<60>"))
    (pad "AT8" smd circle (at -15.999993 6.400013) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 184 "FBG_DQS_RN7"))
    (pad "AT9" smd circle (at -15.200097 6.400013) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1331 "SNN_FBH0_CLK0*"))
    (pad "AT10" smd circle (at -14.399997 6.400013) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1337 "SNN_FBH0_CLK0"))
    (pad "AT11" smd circle (at -13.599897 6.400013) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1339 "SNN_FBH0_CLK1"))
    (pad "AT13" smd circle (at -12.000001 6.400013) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "AT15" smd circle (at -10.500106 10.500106) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AT16" smd circle (at -9.500108 10.500106) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AT17" smd circle (at -8.50011 10.500106) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AT18" smd circle (at -7.500112 10.500106) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AT19" smd circle (at -6.500089 10.500106) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AT20" smd circle (at -5.500091 10.500106) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AT21" smd circle (at -4.500093 10.500106) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AT22" smd circle (at -3.500095 10.500106) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AT23" smd circle (at -2.500097 10.500106) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AT24" smd circle (at -1.500099 10.500106) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AT25" smd circle (at -0.500101 10.500106) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AT26" smd circle (at 0.500101 10.500106) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AT27" smd circle (at 1.500099 10.500106) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AT28" smd circle (at 2.500097 10.500106) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AT29" smd circle (at 3.500095 10.500106) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AT30" smd circle (at 4.500093 10.500106) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AT31" smd circle (at 5.500091 10.500106) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AT32" smd circle (at 6.500089 10.500106) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AT33" smd circle (at 7.500112 10.500106) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AT34" smd circle (at 8.50011 10.500106) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AT35" smd circle (at 9.500108 10.500106) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "AT36" smd circle (at 10.500106 10.500106) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AT43" smd circle (at 12.000001 6.400013) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "AT45" smd circle (at 13.599897 6.400013) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1210 "SNN_FBB0_CLK1"))
    (pad "AT46" smd circle (at 14.399997 6.400013) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 785 "FBB_D<12>"))
    (pad "AT47" smd circle (at 15.200097 6.400013) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 792 "FBB_D<11>"))
    (pad "AT48" smd circle (at 15.999993 6.400013) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 795 "FBB_DQS_WP1"))
    (pad "AT49" smd circle (at 16.800093 6.400013) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 768 "FBB_D<4>"))
    (pad "AT50" smd circle (at 17.599889 6.400013) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 769 "FBB_D<3>"))
    (pad "AT51" smd circle (at 18.399989 6.400013) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 771 "FBB_DQM0"))
    (pad "AT52" smd circle (at 19.200089 6.400013) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 767 "FBB_D<2>"))
    (pad "AT53" smd circle (at 20.000011 6.400013) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 666 "FBB_CMD<9>"))
    (pad "AT54" smd circle (at 20.800111 6.400013) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 687 "FBB_CMD<10>"))
    (pad "AT55" smd circle (at 21.599906 6.400013) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 678 "FBB_CMD<11>"))
    (pad "AU3" smd circle (at -20.000011 7.199909) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1397 "SNN_FBH_D<0>"))
    (pad "AU4" smd circle (at -19.200114 7.199909) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1453 "SNN_FBH_D<1>"))
    (pad "AU5" smd circle (at -18.399989 7.199909) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1445 "SNN_FBH_DBI0"))
    (pad "AU8" smd circle (at -15.999993 7.199909) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 185 "FBG_DQS_WP7"))
    (pad "AU9" smd circle (at -15.200097 7.199909) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 183 "FBG_DQM7"))
    (pad "AU11" smd circle (at -13.599897 7.199909) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1340 "SNN_FBH0_CLK1*"))
    (pad "AU13" smd circle (at -12.000001 7.199909) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "AU43" smd circle (at 12.000001 7.199909) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1478 "FBB_DEBUG"))
    (pad "AU45" smd circle (at 13.599897 7.199909) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1211 "SNN_FBB0_CLK1*"))
    (pad "AU47" smd circle (at 15.200097 7.199909) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 788 "FBB_D<10>"))
    (pad "AU48" smd circle (at 15.999993 7.199909) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 794 "FBB_DQS_RN1"))
    (pad "AU51" smd circle (at 18.399989 7.199909) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 765 "FBB_D<1>"))
    (pad "AU52" smd circle (at 19.200089 7.199909) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 773 "FBB_DQS_WP0"))
    (pad "AU53" smd circle (at 20.000011 7.199909) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 772 "FBB_DQS_RN0"))
    (pad "AV1" smd circle (at -21.599906 8.000009) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1367 "SNN_FBH_CMD<5>"))
    (pad "AV2" smd circle (at -20.800111 8.000009) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AV3" smd circle (at -20.000011 8.000009) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1345 "SNN_FBH_CMD<6>"))
    (pad "AV4" smd circle (at -19.200114 8.000009) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1435 "SNN_FBH_D<2>"))
    (pad "AV5" smd circle (at -18.399989 8.000009) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AV6" smd circle (at -17.599889 8.000009) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1467 "SNN_FBH_D<3>"))
    (pad "AV7" smd circle (at -16.800093 8.000009) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 182 "FBG_D<61>"))
    (pad "AV8" smd circle (at -15.999993 8.000009) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AV9" smd circle (at -15.200097 8.000009) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 178 "FBG_D<62>"))
    (pad "AV10" smd circle (at -14.399997 8.000009) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 176 "FBG_D<63>"))
    (pad "AV11" smd circle (at -13.599897 8.000009) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AV13" smd circle (at -12.000001 8.000009) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AV43" smd circle (at 12.000001 8.000009) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AV45" smd circle (at 13.599897 8.000009) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AV46" smd circle (at 14.399997 8.000009) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 787 "FBB_D<9>"))
    (pad "AV47" smd circle (at 15.200097 8.000009) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 793 "FBB_DQM1"))
    (pad "AV48" smd circle (at 15.999993 8.000009) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AV49" smd circle (at 16.800093 8.000009) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 858 "FBA_D<63>"))
    (pad "AV50" smd circle (at 17.599889 8.000009) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 859 "FBA_D<62>"))
    (pad "AV51" smd circle (at 18.399989 8.000009) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AV52" smd circle (at 19.200089 8.000009) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 763 "FBB_D<0>"))
    (pad "AV53" smd circle (at 20.000011 8.000009) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 682 "FBB_CMD<7>"))
    (pad "AV54" smd circle (at 20.800111 8.000009) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AV55" smd circle (at 21.599906 8.000009) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 686 "FBB_CMD<8>"))
    (pad "AW1" smd circle (at -21.599906 8.800109) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1356 "SNN_FBH_CMD<7>"))
    (pad "AW2" smd circle (at -20.800111 8.800109) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1371 "SNN_FBH_CMD<8>"))
    (pad "AW3" smd circle (at -20.000011 8.800109) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1419 "SNN_FBH_CMD<9>"))
    (pad "AW4" smd circle (at -19.200114 8.800109) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1408 "SNN_FBH_DQS_WP0"))
    (pad "AW5" smd circle (at -18.399989 8.800109) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1378 "SNN_FBH_DQS_RN0"))
    (pad "AW6" smd circle (at -17.599889 8.800109) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1398 "SNN_FBH_DQM1"))
    (pad "AW7" smd circle (at -16.800093 8.800109) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1456 "SNN_FBH_D<8>"))
    (pad "AW8" smd circle (at -15.999993 8.800109) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1448 "SNN_FBH_D<9>"))
    (pad "AW9" smd circle (at -15.200097 8.800109) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1394 "SNN_FBH_D<10>"))
    (pad "AW10" smd circle (at -14.399997 8.800109) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1338 "SNN_FBH_D<11>"))
    (pad "AW11" smd circle (at -13.599897 8.800109) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1343 "SNN_FBH1_CLK1"))
    (pad "AW13" smd circle (at -12.000001 8.800109) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1557 "SNN_FBH_DEBUG"))
    (pad "AW43" smd circle (at 12.000001 8.800109) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "AW45" smd circle (at 13.599897 8.800109) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1188 "SNN_FBA1_CLK1"))
    (pad "AW46" smd circle (at 14.399997 8.800109) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 746 "FBB0_CLK0*"))
    (pad "AW47" smd circle (at 15.200097 8.800109) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 745 "FBB0_CLK0"))
    (pad "AW48" smd circle (at 15.999993 8.800109) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 786 "FBB_D<8>"))
    (pad "AW49" smd circle (at 16.800093 8.800109) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 863 "FBA_D<59>"))
    (pad "AW50" smd circle (at 17.599889 8.800109) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 861 "FBA_D<60>"))
    (pad "AW51" smd circle (at 18.399989 8.800109) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 860 "FBA_D<61>"))
    (pad "AW52" smd circle (at 19.200089 8.800109) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 866 "FBA_DQM7"))
    (pad "AW53" smd circle (at 20.000011 8.800109) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 740 "FBB_CMD<4>"))
    (pad "AW54" smd circle (at 20.800111 8.800109) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 739 "FBB_CMD<5>"))
    (pad "AW55" smd circle (at 21.599906 8.800109) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 693 "FBB_CMD<6>"))
    (pad "AY3" smd circle (at -20.000011 9.599905) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1386 "SNN_FBH_D<4>"))
    (pad "AY4" smd circle (at -19.200114 9.599905) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1389 "SNN_FBH_D<5>"))
    (pad "AY5" smd circle (at -18.399989 9.599905) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1439 "SNN_FBH_DQM0"))
    (pad "AY8" smd circle (at -15.999993 9.599905) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1393 "SNN_FBH_D<13>"))
    (pad "AY9" smd circle (at -15.200097 9.599905) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1396 "SNN_FBH_D<12>"))
    (pad "AY11" smd circle (at -13.599897 9.599905) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1344 "SNN_FBH1_CLK1*"))
    (pad "AY13" smd circle (at -12.000001 9.599905) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "AY43" smd circle (at 12.000001 9.599905) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1558 "FBA_DEBUG"))
    (pad "AY45" smd circle (at 13.599897 9.599905) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1189 "SNN_FBA1_CLK1*"))
    (pad "AY47" smd circle (at 15.200097 9.599905) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 836 "FBA_D<46>"))
    (pad "AY48" smd circle (at 15.999993 9.599905) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 839 "FBA_D<47>"))
    (pad "AY51" smd circle (at 18.399989 9.599905) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1466 "SNN_FBA_DBI7"))
    (pad "AY52" smd circle (at 19.200089 9.599905) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 868 "FBA_DQS_WP7"))
    (pad "AY53" smd circle (at 20.000011 9.599905) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 867 "FBA_DQS_RN7"))
    (pad "B1" smd circle (at -21.599906 -20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1567 "SNN_GPU_NC_5"))
    (pad "B2" smd circle (at -20.800111 -20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1568 "SNN_GPU_NC_6"))
    (pad "B3" smd circle (at -20.000011 -20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "FBF_CMD<14>"))
    (pad "B5" smd circle (at -18.399989 -20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "FBF_CMD<13>"))
    (pad "B6" smd circle (at -17.599889 -20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B8" smd circle (at -15.999993 -20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "FBF_CMD<8>"))
    (pad "B9" smd circle (at -15.200097 -20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B11" smd circle (at -13.599897 -20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 221 "FBF_CMD<3>"))
    (pad "B12" smd circle (at -12.800101 -20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B14" smd circle (at -11.199901 -20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1275 "SNN_FBE_CMD<31>"))
    (pad "B15" smd circle (at -10.400005 -20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B17" smd circle (at -8.800109 -20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 281 "FBE_CMD<26>"))
    (pad "B18" smd circle (at -8.000009 -20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B20" smd circle (at -6.400013 -20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 283 "FBE_CMD<21>"))
    (pad "B21" smd circle (at -5.599913 -20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B23" smd circle (at -3.999992 -20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 291 "FBE_CMD<16>"))
    (pad "B24" smd circle (at -3.199892 -20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B26" smd circle (at -1.599895 -20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 288 "FBE_CMD<11>"))
    (pad "B27" smd circle (at -0.8001 -20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B29" smd circle (at 0.8001 -20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B30" smd circle (at 1.599895 -20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 350 "FBE_CMD<4>"))
    (pad "B32" smd circle (at 3.199892 -20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B33" smd circle (at 3.999992 -20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 352 "FBE_CMD<0>"))
    (pad "B35" smd circle (at 5.599887 -20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B36" smd circle (at 6.399987 -20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 410 "FBD_CMD<28>"))
    (pad "B38" smd circle (at 8.000009 -20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B39" smd circle (at 8.800109 -20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 415 "FBD_CMD<23>"))
    (pad "B41" smd circle (at 10.400005 -20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B42" smd circle (at 11.199901 -20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 412 "FBD_CMD<18>"))
    (pad "B44" smd circle (at 12.800101 -20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B45" smd circle (at 13.599897 -20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 429 "FBD_CMD<13>"))
    (pad "B47" smd circle (at 15.200097 -20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B48" smd circle (at 15.999993 -20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 426 "FBD_CMD<8>"))
    (pad "B50" smd circle (at 17.599889 -20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B51" smd circle (at 18.399989 -20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 480 "FBD_CMD<4>"))
    (pad "B53" smd circle (at 20.000011 -20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 484 "FBD_CMD<1>"))
    (pad "B54" smd circle (at 20.800111 -20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1569 "SNN_GPU_NC_7"))
    (pad "B55" smd circle (at 21.599906 -20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1570 "SNN_GPU_NC_8"))
    (pad "BA1" smd circle (at -21.599906 10.400005) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1373 "SNN_FBH_CMD<10>"))
    (pad "BA2" smd circle (at -20.800111 10.400005) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BA3" smd circle (at -20.000011 10.400005) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1372 "SNN_FBH_CMD<11>"))
    (pad "BA4" smd circle (at -19.200114 10.400005) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1388 "SNN_FBH_D<6>"))
    (pad "BA5" smd circle (at -18.399989 10.400005) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BA6" smd circle (at -17.599889 10.400005) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1440 "SNN_FBH_DQS_WP1"))
    (pad "BA7" smd circle (at -16.800093 10.400005) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1395 "SNN_FBH_DQS_RN1"))
    (pad "BA8" smd circle (at -15.999993 10.400005) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BA9" smd circle (at -15.200097 10.400005) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1399 "SNN_FBH_D<14>"))
    (pad "BA10" smd circle (at -14.399997 10.400005) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1341 "SNN_FBH_D<15>"))
    (pad "BA11" smd circle (at -13.599897 10.400005) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BA13" smd circle (at -12.000001 10.400005) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BA43" smd circle (at 12.000001 10.400005) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BA45" smd circle (at 13.599897 10.400005) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BA46" smd circle (at 14.399997 10.400005) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 838 "FBA_D<45>"))
    (pad "BA47" smd circle (at 15.200097 10.400005) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 837 "FBA_D<44>"))
    (pad "BA48" smd circle (at 15.999993 10.400005) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BA49" smd circle (at 16.800093 10.400005) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 865 "FBA_D<58>"))
    (pad "BA50" smd circle (at 17.599889 10.400005) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 864 "FBA_D<57>"))
    (pad "BA51" smd circle (at 18.399989 10.400005) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BA52" smd circle (at 19.200089 10.400005) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 862 "FBA_D<56>"))
    (pad "BA53" smd circle (at 20.000011 10.400005) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 743 "FBB_CMD<2>"))
    (pad "BA54" smd circle (at 20.800111 10.400005) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BA55" smd circle (at 21.599906 10.400005) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 741 "FBB_CMD<3>"))
    (pad "BB1" smd circle (at -21.599906 11.199901) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1375 "SNN_FBH_CMD<12>"))
    (pad "BB2" smd circle (at -20.800111 11.199901) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1374 "SNN_FBH_CMD<13>"))
    (pad "BB3" smd circle (at -20.000011 11.199901) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1385 "SNN_FBH_CMD<14>"))
    (pad "BB4" smd circle (at -19.200114 11.199901) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1447 "SNN_FBH_D<17>"))
    (pad "BB5" smd circle (at -18.399989 11.199901) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1455 "SNN_FBH_D<18>"))
    (pad "BB6" smd circle (at -17.599889 11.199901) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1391 "SNN_FBH_D<7>"))
    (pad "BB7" smd circle (at -16.800093 11.199901) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1470 "SNN_FBH_DQS_WP3"))
    (pad "BB8" smd circle (at -15.999993 11.199901) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1379 "SNN_FBH_DQM3"))
    (pad "BB9" smd circle (at -15.200097 11.199901) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1436 "SNN_FBH_D<25>"))
    (pad "BB10" smd circle (at -14.399997 11.199901) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1342 "SNN_FBH_D<24>"))
    (pad "BB11" smd circle (at -13.599897 11.199901) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1571 "SNN_FBH_DBI1"))
    (pad "BB13" smd circle (at -12.000001 11.199901) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1334 "SNN_GPU_NC_9"))
    (pad "BB43" smd circle (at 12.000001 11.199901) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "BB45" smd circle (at 13.599897 11.199901) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 813 "FBA1_CLK0"))
    (pad "BB46" smd circle (at 14.399997 11.199901) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 814 "FBA1_CLK0*"))
    (pad "BB47" smd circle (at 15.200097 11.199901) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 844 "FBA_DQM5"))
    (pad "BB48" smd circle (at 15.999993 11.199901) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 846 "FBA_DQS_WP5"))
    (pad "BB49" smd circle (at 16.800093 11.199901) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 845 "FBA_DQS_RN5"))
    (pad "BB50" smd circle (at 17.599889 11.199901) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1207 "SNN_SPARE_01"))
    (pad "BB51" smd circle (at 18.399989 11.199901) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 826 "FBA_D<50>"))
    (pad "BB52" smd circle (at 19.200089 11.199901) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 825 "FBA_D<48>"))
    (pad "BB53" smd circle (at 20.000011 11.199901) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1219 "SNN_FBA_CMD<32>"))
    (pad "BB54" smd circle (at 20.800111 11.199901) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 742 "FBB_CMD<0>"))
    (pad "BB55" smd circle (at 21.599906 11.199901) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 744 "FBB_CMD<1>"))
    (pad "BC3" smd circle (at -20.000011 12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1368 "SNN_FBH_D<16>"))
    (pad "BC4" smd circle (at -19.200114 12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1390 "SNN_FBH_DQS_RN2"))
    (pad "BC5" smd circle (at -18.399989 12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1392 "SNN_FBH_D<19>"))
    (pad "BC8" smd circle (at -15.999993 12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1438 "SNN_FBH_DQS_RN3"))
    (pad "BC9" smd circle (at -15.200097 12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1381 "SNN_FBH_D<26>"))
    (pad "BC11" smd circle (at -13.599897 12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1282 "FBEFGH_MPLL_AVDD"))
    (pad "BC13" smd circle (at -12.000001 12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "BC14" smd circle (at -11.199901 12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "BC15" smd circle (at -10.400005 12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BC16" smd circle (at -9.599905 12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1545 "FBGH_REFCLK"))
    (pad "BC17" smd circle (at -8.800109 12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1544 "FBGH_REFCLK*"))
    (pad "BC18" smd circle (at -8.000009 12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BC19" smd circle (at -7.199909 12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1555 "GPU_CLK*"))
    (pad "BC20" smd circle (at -6.400013 12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1556 "GPU_CLK"))
    (pad "BC21" smd circle (at -5.599913 12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BC22" smd circle (at -4.800092 12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "BC23" smd circle (at -3.999992 12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "BC24" smd circle (at -3.199892 12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BC25" smd circle (at -2.399995 12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "BC26" smd circle (at -1.599895 12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "BC27" smd circle (at -0.8001 12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BC28" smd circle (at 0 12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "BC29" smd circle (at 0.8001 12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BC30" smd circle (at 1.599895 12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "BC31" smd circle (at 2.399995 12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "BC32" smd circle (at 3.199892 12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BC33" smd circle (at 3.999992 12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "BC34" smd circle (at 4.800092 12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "BC35" smd circle (at 5.599887 12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BC36" smd circle (at 6.399987 12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "BC37" smd circle (at 7.199909 12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "BC38" smd circle (at 8.000009 12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BC39" smd circle (at 8.800109 12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "BC40" smd circle (at 9.599905 12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "BC41" smd circle (at 10.400005 12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BC42" smd circle (at 11.199901 12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "BC43" smd circle (at 12.000001 12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1572 "SNN_GPU_NC_10"))
    (pad "BC45" smd circle (at 13.599897 12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1573 "FBABCD_MPLL_AVDD"))
    (pad "BC47" smd circle (at 15.200097 12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 842 "FBA_D<43>"))
    (pad "BC48" smd circle (at 15.999993 12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 841 "FBA_D<41>"))
    (pad "BC51" smd circle (at 18.399989 12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 827 "FBA_D<53>"))
    (pad "BC52" smd circle (at 19.200089 12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 828 "FBA_D<52>"))
    (pad "BC53" smd circle (at 20.000011 12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 834 "FBA_DQS_RN6"))
    (pad "BD1" smd circle (at -21.599906 12.800101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1376 "SNN_FBH_CMD<15>"))
    (pad "BD2" smd circle (at -20.800111 12.800101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BD3" smd circle (at -20.000011 12.800101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1346 "SNN_FBH_CMD<16>"))
    (pad "BD4" smd circle (at -19.200114 12.800101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1418 "SNN_FBH_DQS_WP2"))
    (pad "BD5" smd circle (at -18.399989 12.800101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BD6" smd circle (at -17.599889 12.800101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1387 "SNN_FBH_DQM2"))
    (pad "BD7" smd circle (at -16.800093 12.800101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1469 "SNN_FBH_D<27>"))
    (pad "BD8" smd circle (at -15.999993 12.800101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BD9" smd circle (at -15.200097 12.800101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1384 "SNN_FBH1_CLK0*"))
    (pad "BD10" smd circle (at -14.399997 12.800101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1382 "SNN_FBH1_CLK0"))
    (pad "BD11" smd circle (at -13.599897 12.800101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BD45" smd circle (at 13.599897 12.800101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BD46" smd circle (at 14.399997 12.800101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1209 "SNN_SPARE_02"))
    (pad "BD47" smd circle (at 15.200097 12.800101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 840 "FBA_D<42>"))
    (pad "BD48" smd circle (at 15.999993 12.800101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BD49" smd circle (at 16.800093 12.800101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 843 "FBA_D<40>"))
    (pad "BD50" smd circle (at 17.599889 12.800101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 833 "FBA_DQM6"))
    (pad "BD51" smd circle (at 18.399989 12.800101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BD52" smd circle (at 19.200089 12.800101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 835 "FBA_DQS_WP6"))
    (pad "BD53" smd circle (at 20.000011 12.800101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1196 "SNN_FBA_CMD<30>"))
    (pad "BD54" smd circle (at 20.800111 12.800101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BD55" smd circle (at 21.599906 12.800101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1195 "SNN_FBA_CMD<31>"))
    (pad "BE1" smd circle (at -21.599906 13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1348 "SNN_FBH_CMD<17>"))
    (pad "BE2" smd circle (at -20.800111 13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1377 "SNN_FBH_CMD<18>"))
    (pad "BE3" smd circle (at -20.000011 13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1370 "SNN_FBH_CMD<19>"))
    (pad "BE4" smd circle (at -19.200114 13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1451 "SNN_FBH_D<20>"))
    (pad "BE5" smd circle (at -18.399989 13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1459 "SNN_FBH_D<22>"))
    (pad "BE6" smd circle (at -17.599889 13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1420 "SNN_FBH_D<23>"))
    (pad "BE7" smd circle (at -16.800093 13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1454 "SNN_FBH_DBI3"))
    (pad "BE8" smd circle (at -15.999993 13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1380 "SNN_FBH_D<28>"))
    (pad "BE9" smd circle (at -15.200097 13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1383 "SNN_FBH_D<29>"))
    (pad "BE10" smd circle (at -14.399997 13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1437 "SNN_GPU_NC_11"))
    (pad "BE11" smd circle (at -13.599897 13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1314 "SNN_GPU_NC_12"))
    (pad "BE12" smd circle (at -12.800101 13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BE13" smd circle (at -12.000001 13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1574 "SNN_SPARE_03"))
    (pad "BE14" smd circle (at -11.199901 13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1575 "SNN_SPARE_04"))
    (pad "BE15" smd circle (at -10.400005 13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BE16" smd circle (at -9.599905 13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "1V15"))
    (pad "BE17" smd circle (at -8.800109 13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1596 "SNN_SPARE_05"))
    (pad "BE18" smd circle (at -8.000009 13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BE19" smd circle (at -7.199909 13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1597 "SNN_TSENSE_OVERT"))
    (pad "BE20" smd circle (at -6.400013 13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1598 "SNN_TS_1V5_SEL"))
    (pad "BE21" smd circle (at -5.599913 13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BE22" smd circle (at -4.800092 13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1551 "SNN_SPARE_06"))
    (pad "BE23" smd circle (at -3.999992 13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "1V15"))
    (pad "BE24" smd circle (at -3.199892 13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BE25" smd circle (at -2.399995 13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1599 "SNN_SPARE_07"))
    (pad "BE26" smd circle (at -1.599895 13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "1V15"))
    (pad "BE27" smd circle (at -0.8001 13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BE28" smd circle (at 0 13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1600 "SNN_SPARE_08"))
    (pad "BE29" smd circle (at 0.8001 13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BE30" smd circle (at 1.599895 13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "1V15"))
    (pad "BE31" smd circle (at 2.399995 13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1601 "SNN_SPARE_09"))
    (pad "BE32" smd circle (at 3.199892 13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BE33" smd circle (at 3.999992 13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "1V15"))
    (pad "BE34" smd circle (at 4.800092 13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1602 "SNN_SPARE_10"))
    (pad "BE35" smd circle (at 5.599887 13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BE36" smd circle (at 6.399987 13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "1V15"))
    (pad "BE37" smd circle (at 7.199909 13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "1V15"))
    (pad "BE38" smd circle (at 8.000009 13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BE39" smd circle (at 8.800109 13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1192 "FBAB_REFCLK*"))
    (pad "BE40" smd circle (at 9.599905 13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1191 "SNN_THERM_LD_STEP1"))
    (pad "BE41" smd circle (at 10.400005 13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BE42" smd circle (at 11.199901 13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1576 "SNN_GPU_NC_13"))
    (pad "BE43" smd circle (at 12.000001 13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1577 "SNN_GPU_NC_14"))
    (pad "BE44" smd circle (at 12.800101 13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BE45" smd circle (at 13.599897 13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1190 "SNN_GPU_NC_15"))
    (pad "BE46" smd circle (at 14.399997 13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1206 "SNN_GPU_NC_16"))
    (pad "BE47" smd circle (at 15.200097 13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 885 "FBA_D<31>"))
    (pad "BE48" smd circle (at 15.999993 13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1201 "SNN_FBA_DBI5"))
    (pad "BE49" smd circle (at 16.800093 13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1202 "SNN_FBA_DBI6"))
    (pad "BE50" smd circle (at 17.599889 13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 829 "FBA_D<49>"))
    (pad "BE51" smd circle (at 18.399989 13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 831 "FBA_D<51>"))
    (pad "BE52" smd circle (at 19.200089 13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 830 "FBA_D<55>"))
    (pad "BE53" smd circle (at 20.000011 13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 798 "FBA_CMD<27>"))
    (pad "BE54" smd circle (at 20.800111 13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 799 "FBA_CMD<28>"))
    (pad "BE55" smd circle (at 21.599906 13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1194 "SNN_FBA_CMD<29>"))
    (pad "BF3" smd circle (at -20.000011 14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1369 "SNN_FBH_D<45>"))
    (pad "BF4" smd circle (at -19.200114 14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1443 "SNN_FBH_D<21>"))
    (pad "BF5" smd circle (at -18.399989 14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1422 "SNN_FBH_DBI2"))
    (pad "BF8" smd circle (at -15.999993 14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1446 "SNN_FBH_D<30>"))
    (pad "BF9" smd circle (at -15.200097 14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1412 "SNN_SPARE_25"))
    (pad "BF11" smd circle (at -13.599897 14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1413 "SNN_FBH_D<32>"))
    (pad "BF12" smd circle (at -12.800101 14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1410 "SNN_FBH_D<33>"))
    (pad "BF14" smd circle (at -11.199901 14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1316 "SNN_GPU_NC_17"))
    (pad "BF15" smd circle (at -10.400005 14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1315 "SNN_SPARE_11"))
    (pad "BF17" smd circle (at -8.800109 14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1603 "SNN_SPARE_12"))
    (pad "BF18" smd circle (at -8.000009 14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1604 "SNN_SPARE_13"))
    (pad "BF20" smd circle (at -6.400013 14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1605 "SNN_SPARE_14"))
    (pad "BF21" smd circle (at -5.599913 14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1606 "SNN_SPARE_15"))
    (pad "BF23" smd circle (at -3.999992 14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1548 "SNN_SPARE_16"))
    (pad "BF24" smd circle (at -3.199892 14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1607 "SNN_SPARE_17"))
    (pad "BF26" smd circle (at -1.599895 14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1608 "SNN_SPARE_18"))
    (pad "BF27" smd circle (at -0.8001 14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1609 "SNN_SPARE_19"))
    (pad "BF29" smd circle (at 0.8001 14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1610 "SNN_SPARE_20"))
    (pad "BF30" smd circle (at 1.599895 14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1611 "SNN_SPARE_21"))
    (pad "BF32" smd circle (at 3.199892 14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1612 "SNN_SPARE_22"))
    (pad "BF33" smd circle (at 3.999992 14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "1V15"))
    (pad "BF35" smd circle (at 5.599887 14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "1V15"))
    (pad "BF36" smd circle (at 6.399987 14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1613 "SNN_SPARE_23"))
    (pad "BF38" smd circle (at 8.000009 14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1614 "SNN_SPARE_24"))
    (pad "BF39" smd circle (at 8.800109 14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1615 "FBAB_REFCLK"))
    (pad "BF41" smd circle (at 10.400005 14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1186 "SNN_FBA0_CLK1"))
    (pad "BF42" smd circle (at 11.199901 14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1187 "SNN_FBA0_CLK1*"))
    (pad "BF44" smd circle (at 12.800101 14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 876 "FBA0_CLK0*"))
    (pad "BF45" smd circle (at 13.599897 14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 875 "FBA0_CLK0"))
    (pad "BF47" smd circle (at 15.200097 14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 890 "FBA_DQM3"))
    (pad "BF48" smd circle (at 15.999993 14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 883 "FBA_D<30>"))
    (pad "BF51" smd circle (at 18.399989 14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1204 "SNN_FBA_DBI4"))
    (pad "BF52" smd circle (at 19.200089 14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 832 "FBA_D<54>"))
    (pad "BF53" smd circle (at 20.000011 14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 800 "FBA_CMD<26>"))
    (pad "BG1" smd circle (at -21.599906 15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1347 "SNN_FBH_CMD<20>"))
    (pad "BG2" smd circle (at -20.800111 15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BG3" smd circle (at -20.000011 15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1352 "SNN_FBH_CMD<21>"))
    (pad "BG4" smd circle (at -19.200114 15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1421 "SNN_FBH_D<40>"))
    (pad "BG5" smd circle (at -18.399989 15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BG6" smd circle (at -17.599889 15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1424 "SNN_FBH_D<46>"))
    (pad "BG7" smd circle (at -16.800093 15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1468 "SNN_FBH_D<31>"))
    (pad "BG8" smd circle (at -15.999993 15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BG9" smd circle (at -15.200097 15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1442 "SNN_SPARE_46"))
    (pad "BG10" smd circle (at -14.399997 15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1409 "SNN_SPARE_26"))
    (pad "BG11" smd circle (at -13.599897 15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1414 "SNN_FBH_D<34>"))
    (pad "BG12" smd circle (at -12.800101 15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1411 "SNN_FBH_D<35>"))
    (pad "BG13" smd circle (at -12.000001 15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1616 "SNN_FBH_D<36>"))
    (pad "BG14" smd circle (at -11.199901 15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1550 "SNN_FBH_D<37>"))
    (pad "BG15" smd circle (at -10.400005 15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1549 "SNN_GPU_NC_18"))
    (pad "BG16" smd circle (at -9.599905 15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1479 "SNN_GPU_NC_19"))
    (pad "BG17" smd circle (at -8.800109 15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1617 "SNN_SPARE_27"))
    (pad "BG18" smd circle (at -8.000009 15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1618 "SNN_SPARE_28"))
    (pad "BG19" smd circle (at -7.199909 15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1485 "SNN_SPARE_29"))
    (pad "BG20" smd circle (at -6.400013 15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "1V15"))
    (pad "BG21" smd circle (at -5.599913 15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1619 "SNN_SPARE_30"))
    (pad "BG22" smd circle (at -4.800092 15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1620 "SNN_SPARE_31"))
    (pad "BG23" smd circle (at -3.999992 15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "1V15"))
    (pad "BG24" smd circle (at -3.199892 15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1621 "SNN_SPARE_32"))
    (pad "BG25" smd circle (at -2.399995 15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1622 "SNN_SPARE_33"))
    (pad "BG26" smd circle (at -1.599895 15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1623 "GPU_PMC_ISO_RESET*"))
    (pad "BG27" smd circle (at -0.8001 15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1624 "SNN_SPARE_34"))
    (pad "BG28" smd circle (at 0 15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1625 "SNN_SPARE_35"))
    (pad "BG29" smd circle (at 0.8001 15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "1V15"))
    (pad "BG30" smd circle (at 1.599895 15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1626 "SNN_SPARE_36"))
    (pad "BG31" smd circle (at 2.399995 15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1627 "SNN_SPARE_37"))
    (pad "BG32" smd circle (at 3.199892 15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "1V15"))
    (pad "BG33" smd circle (at 3.999992 15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1628 "SNN_SPARE_38"))
    (pad "BG34" smd circle (at 4.800092 15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1629 "SNN_SPARE_39"))
    (pad "BG35" smd circle (at 5.599887 15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "1V15"))
    (pad "BG36" smd circle (at 6.399987 15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1630 "SNN_SPARE_40"))
    (pad "BG37" smd circle (at 7.199909 15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1631 "SNN_SPARE_41"))
    (pad "BG38" smd circle (at 8.000009 15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1632 "SNN_SPARE_42"))
    (pad "BG39" smd circle (at 8.800109 15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1633 "SNN_SPARE_43"))
    (pad "BG40" smd circle (at 9.599905 15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1634 "SNN_SPARE_44"))
    (pad "BG41" smd circle (at 10.400005 15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1197 "SNN_THERM_LD_STEP0"))
    (pad "BG42" smd circle (at 11.199901 15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1208 "GPU_TESTMODE"))
    (pad "BG43" smd circle (at 12.000001 15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1199 "SNN_SPARE_45"))
    (pad "BG44" smd circle (at 12.800101 15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1198 "SNN_FBA_DBI1"))
    (pad "BG45" smd circle (at 13.599897 15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1200 "SNN_FBA_DBI3"))
    (pad "BG46" smd circle (at 14.399997 15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 884 "FBA_D<27>"))
    (pad "BG47" smd circle (at 15.200097 15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 882 "FBA_D<28>"))
    (pad "BG48" smd circle (at 15.999993 15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BG49" smd circle (at 16.800093 15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 854 "FBA_D<37>"))
    (pad "BG50" smd circle (at 17.599889 15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 851 "FBA_D<38>"))
    (pad "BG51" smd circle (at 18.399989 15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BG52" smd circle (at 19.200089 15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 852 "FBA_D<39>"))
    (pad "BG53" smd circle (at 20.000011 15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 807 "FBA_CMD<24>"))
    (pad "BG54" smd circle (at 20.800111 15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BG55" smd circle (at 21.599906 15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 796 "FBA_CMD<25>"))
    (pad "BH1" smd circle (at -21.599906 15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1349 "SNN_FBH_CMD<22>"))
    (pad "BH2" smd circle (at -20.800111 15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1351 "SNN_FBH_CMD<23>"))
    (pad "BH3" smd circle (at -20.000011 15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1400 "SNN_FBH_CMD<24>"))
    (pad "BH4" smd circle (at -19.200114 15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1425 "SNN_FBH_DQM5"))
    (pad "BH5" smd circle (at -18.399989 15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1423 "SNN_FBH_DQS_WP5"))
    (pad "BH6" smd circle (at -17.599889 15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1417 "SNN_FBH_DQS_RN5"))
    (pad "BH7" smd circle (at -16.800093 15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1473 "SNN_FBH_D<42>"))
    (pad "BH8" smd circle (at -15.999993 15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1458 "SNN_SPARE_60"))
    (pad "BH9" smd circle (at -15.200097 15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BH10" smd circle (at -14.399997 15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1416 "SNN_SPARE_47"))
    (pad "BH11" smd circle (at -13.599897 15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1472 "SNN_FBH_DQS_RN4"))
    (pad "BH12" smd circle (at -12.800101 15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BH13" smd circle (at -12.000001 15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1488 "SNN_GPU_NC_20"))
    (pad "BH14" smd circle (at -11.199901 15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1498 "SNN_FBH_D<38>"))
    (pad "BH15" smd circle (at -10.400005 15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BH16" smd circle (at -9.599905 15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1480 "SNN_SPARE_48"))
    (pad "BH17" smd circle (at -8.800109 15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "1V15"))
    (pad "BH18" smd circle (at -8.000009 15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BH19" smd circle (at -7.199909 15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1481 "SNN_SPARE_49"))
    (pad "BH20" smd circle (at -6.400013 15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1504 "SNN_SPARE_50"))
    (pad "BH21" smd circle (at -5.599913 15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BH22" smd circle (at -4.800092 15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1482 "SNN_SPARE_51"))
    (pad "BH23" smd circle (at -3.999992 15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "1V15"))
    (pad "BH24" smd circle (at -3.199892 15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BH25" smd circle (at -2.399995 15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1543 "SNN_SPARE_52"))
    (pad "BH26" smd circle (at -1.599895 15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "1V15"))
    (pad "BH27" smd circle (at -0.8001 15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BH28" smd circle (at 0 15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1560 "SNN_SPARE_53"))
    (pad "BH29" smd circle (at 0.8001 15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BH30" smd circle (at 1.599895 15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "1V15"))
    (pad "BH31" smd circle (at 2.399995 15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1635 "SNN_SPARE_54"))
    (pad "BH32" smd circle (at 3.199892 15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BH33" smd circle (at 3.999992 15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1636 "I2CS_SCL"))
    (pad "BH34" smd circle (at 4.800092 15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1637 "SNN_SPARE_55"))
    (pad "BH35" smd circle (at 5.599887 15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BH36" smd circle (at 6.399987 15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1638 "SNN_SPARE_56"))
    (pad "BH37" smd circle (at 7.199909 15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1639 "SNN_SPARE_57"))
    (pad "BH38" smd circle (at 8.000009 15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BH39" smd circle (at 8.800109 15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 912 "FBA_DQM0"))
    (pad "BH40" smd circle (at 9.599905 15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1640 "SNN_SPARE_58"))
    (pad "BH41" smd circle (at 10.400005 15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BH42" smd circle (at 11.199901 15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 909 "FBA_D<7>"))
    (pad "BH43" smd circle (at 12.000001 15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1465 "SNN_SPARE_59"))
    (pad "BH44" smd circle (at 12.800101 15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BH45" smd circle (at 13.599897 15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 899 "FBA_D<15>"))
    (pad "BH46" smd circle (at 14.399997 15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 887 "FBA_D<26>"))
    (pad "BH47" smd circle (at 15.200097 15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BH48" smd circle (at 15.999993 15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 888 "FBA_D<29>"))
    (pad "BH49" smd circle (at 16.800093 15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 853 "FBA_D<36>"))
    (pad "BH50" smd circle (at 17.599889 15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 847 "FBA_D<35>"))
    (pad "BH51" smd circle (at 18.399989 15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 849 "FBA_D<34>"))
    (pad "BH52" smd circle (at 19.200089 15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 855 "FBA_DQM4"))
    (pad "BH53" smd circle (at 20.000011 15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 802 "FBA_CMD<21>"))
    (pad "BH54" smd circle (at 20.800111 15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1193 "SNN_FBA_CMD<22>"))
    (pad "BH55" smd circle (at 21.599906 15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 804 "FBA_CMD<23>"))
    (pad "BJ3" smd circle (at -20.000011 16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1457 "SNN_FBH_D<47>"))
    (pad "BJ4" smd circle (at -19.200114 16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1401 "SNN_FBH_D<41>"))
    (pad "BJ5" smd circle (at -18.399989 16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1407 "SNN_FBH_D<43>"))
    (pad "BJ8" smd circle (at -15.999993 16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1429 "SNN_FBH_DBI4"))
    (pad "BJ9" smd circle (at -15.200097 16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1415 "SNN_SPARE_66"))
    (pad "BJ11" smd circle (at -13.599897 16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1450 "SNN_FBH_DQS_WP4"))
    (pad "BJ12" smd circle (at -12.800101 16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1654 "SNN_FBH_DQM4"))
    (pad "BJ14" smd circle (at -11.199901 16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1489 "SNN_FBH_D<39>"))
    (pad "BJ15" smd circle (at -10.400005 16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1514 "GV_RX1*"))
    (pad "BJ17" smd circle (at -8.800109 16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1511 "GV_RX_RSET_VDD"))
    (pad "BJ18" smd circle (at -8.000009 16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1508 "SNN_SPARE_61"))
    (pad "BJ20" smd circle (at -6.400013 16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1503 "SNN_SPARE_62"))
    (pad "BJ21" smd circle (at -5.599913 16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1530 "GV_TX3*"))
    (pad "BJ23" smd circle (at -3.999992 16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1483 "GV_TX1"))
    (pad "BJ24" smd circle (at -3.199892 16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1546 "GV_TX0*"))
    (pad "BJ26" smd circle (at -1.599895 16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1111 "GPU_BUFCLK_LDT_IN"))
    (pad "BJ27" smd circle (at -0.8001 16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1561 "SNN_GPU_BUFRST*"))
    (pad "BJ29" smd circle (at 0.8001 16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1559 "JTAG_TCK"))
    (pad "BJ30" smd circle (at 1.599895 16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1112 "SNN_SPARE_63"))
    (pad "BJ32" smd circle (at 3.199892 16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1562 "JTAG_TMS"))
    (pad "BJ33" smd circle (at 3.999992 16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1113 "I2CS_SDA"))
    (pad "BJ35" smd circle (at 5.599887 16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1119 "SNN_SPARE_64"))
    (pad "BJ36" smd circle (at 6.399987 16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1116 "SNN_SPARE_65"))
    (pad "BJ38" smd circle (at 8.000009 16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1117 "SNN_FBA_DBI0"))
    (pad "BJ39" smd circle (at 8.800109 16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 906 "FBA_D<3>"))
    (pad "BJ41" smd circle (at 10.400005 16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 910 "FBA_D<5>"))
    (pad "BJ42" smd circle (at 11.199901 16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 911 "FBA_D<6>"))
    (pad "BJ44" smd circle (at 12.800101 16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 897 "FBA_D<14>"))
    (pad "BJ45" smd circle (at 13.599897 16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 893 "FBA_D<13>"))
    (pad "BJ47" smd circle (at 15.200097 16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 886 "FBA_D<25>"))
    (pad "BJ48" smd circle (at 15.999993 16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 892 "FBA_DQS_WP3"))
    (pad "BJ51" smd circle (at 18.399989 16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 850 "FBA_D<33>"))
    (pad "BJ52" smd circle (at 19.200089 16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 857 "FBA_DQS_WP4"))
    (pad "BJ53" smd circle (at 20.000011 16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 805 "FBA_CMD<20>"))
    (pad "BK1" smd circle (at -21.599906 17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1353 "SNN_FBH_CMD<25>"))
    (pad "BK2" smd circle (at -20.800111 17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BK3" smd circle (at -20.000011 17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1359 "SNN_FBH_CMD<26>"))
    (pad "BK4" smd circle (at -19.200114 17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1449 "SNN_FBH_D<44>"))
    (pad "BK5" smd circle (at -18.399989 17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BK6" smd circle (at -17.599889 17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1406 "SNN_FBH_DBI5"))
    (pad "BK8" smd circle (at -15.999993 17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1474 "SNN_FBH_D<59>"))
    (pad "BK9" smd circle (at -15.200097 17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1427 "SNN_FBH_D<58>"))
    (pad "BK11" smd circle (at -13.599897 17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1492 "SNN_FBH_D<57>"))
    (pad "BK12" smd circle (at -12.800101 17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1641 "SNN_FBH_D<56>"))
    (pad "BK14" smd circle (at -11.199901 17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1642 "GV_RX3"))
    (pad "BK15" smd circle (at -10.400005 17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1515 "GV_RX1"))
    (pad "BK17" smd circle (at -8.800109 17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1507 "GV_RXCTL"))
    (pad "BK18" smd circle (at -8.000009 17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1484 "GV_PLLAVDD"))
    (pad "BK20" smd circle (at -6.400013 17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1531 "GV_TX5"))
    (pad "BK21" smd circle (at -5.599913 17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1542 "GV_TX3"))
    (pad "BK23" smd circle (at -3.999992 17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1547 "GV_TX1*"))
    (pad "BK24" smd circle (at -3.199892 17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1110 "GV_TX0"))
    (pad "BK26" smd circle (at -1.599895 17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "1V15"))
    (pad "BK27" smd circle (at -0.8001 17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1114 "GPU_HOT_RESET*"))
    (pad "BK29" smd circle (at 0.8001 17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "1V15"))
    (pad "BK30" smd circle (at 1.599895 17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1115 "JTAG_TDI_GPU"))
    (pad "BK32" smd circle (at 3.199892 17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "1V15"))
    (pad "BK33" smd circle (at 3.999992 17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "1V15"))
    (pad "BK35" smd circle (at 5.599887 17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1643 "PEX_PLLVDD"))
    (pad "BK36" smd circle (at 6.399987 17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1118 "SNN_SPARE_67"))
    (pad "BK38" smd circle (at 8.000009 17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 905 "FBA_D<1>"))
    (pad "BK39" smd circle (at 8.800109 17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 907 "FBA_D<2>"))
    (pad "BK41" smd circle (at 10.400005 17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 914 "FBA_DQS_WP0"))
    (pad "BK42" smd circle (at 11.199901 17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 908 "FBA_D<4>"))
    (pad "BK44" smd circle (at 12.800101 17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 898 "FBA_D<11>"))
    (pad "BK45" smd circle (at 13.599897 17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 894 "FBA_D<12>"))
    (pad "BK47" smd circle (at 15.200097 17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 889 "FBA_D<24>"))
    (pad "BK48" smd circle (at 15.999993 17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 891 "FBA_DQS_RN3"))
    (pad "BK50" smd circle (at 17.599889 17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 848 "FBA_D<32>"))
    (pad "BK51" smd circle (at 18.399989 17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BK52" smd circle (at 19.200089 17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 856 "FBA_DQS_RN4"))
    (pad "BK53" smd circle (at 20.000011 17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 801 "FBA_CMD<18>"))
    (pad "BK54" smd circle (at 20.800111 17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BK55" smd circle (at 21.599906 17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 797 "FBA_CMD<19>"))
    (pad "BL1" smd circle (at -21.599906 18.400014) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1354 "SNN_FBH_CMD<27>"))
    (pad "BL2" smd circle (at -20.800111 18.400014) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1357 "SNN_FBH_CMD<28>"))
    (pad "BL3" smd circle (at -20.000011 18.400014) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1350 "SNN_FBH_D<49>"))
    (pad "BL4" smd circle (at -19.200114 18.400014) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1405 "SNN_FBH_D<50>"))
    (pad "BL5" smd circle (at -18.399989 18.400014) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1404 "SNN_FBH_D<51>"))
    (pad "BL6" smd circle (at -17.599889 18.400014) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BL7" smd circle (at -16.800093 18.400014) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1471 "SNN_FBH_DBI6"))
    (pad "BL8" smd circle (at -15.999993 18.400014) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1452 "SNN_FBH_DQS_RN7"))
    (pad "BL9" smd circle (at -15.200097 18.400014) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BL10" smd circle (at -14.399997 18.400014) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1428 "GV_RX2"))
    (pad "BL11" smd circle (at -13.599897 18.400014) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1493 "SNN_FBH_DQM7"))
    (pad "BL12" smd circle (at -12.800101 18.400014) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BL13" smd circle (at -12.000001 18.400014) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1494 "GV_TX18"))
    (pad "BL14" smd circle (at -11.199901 18.400014) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1495 "GV_RX3*"))
    (pad "BL15" smd circle (at -10.400005 18.400014) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BL16" smd circle (at -9.599905 18.400014) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1528 "GV_TXCLK"))
    (pad "BL17" smd circle (at -8.800109 18.400014) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1525 "GV_RXCTL*"))
    (pad "BL18" smd circle (at -8.000009 18.400014) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BL19" smd circle (at -7.199909 18.400014) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1501 "GV_TX8"))
    (pad "BL20" smd circle (at -6.400013 18.400014) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1502 "GV_TX5*"))
    (pad "BL21" smd circle (at -5.599913 18.400014) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BL22" smd circle (at -4.800092 18.400014) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1526 "GV_TX2"))
    (pad "BL23" smd circle (at -3.999992 18.400014) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1522 "GV_TX_RSET_GND"))
    (pad "BL24" smd circle (at -3.199892 18.400014) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BL25" smd circle (at -2.399995 18.400014) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1155 "PEX_TX0"))
    (pad "BL26" smd circle (at -1.599895 18.400014) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1171 "GPU_PEX_PWR_GOOD*"))
    (pad "BL27" smd circle (at -0.8001 18.400014) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BL28" smd circle (at 0 18.400014) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1172 "PEX_TX2"))
    (pad "BL29" smd circle (at 0.8001 18.400014) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BL30" smd circle (at 1.599895 18.400014) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1175 "JTAG_TDO_GPU"))
    (pad "BL31" smd circle (at 2.399995 18.400014) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1176 "PEX_TX4"))
    (pad "BL32" smd circle (at 3.199892 18.400014) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BL33" smd circle (at 3.999992 18.400014) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1180 "JTAG_TRST*"))
    (pad "BL34" smd circle (at 4.800092 18.400014) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1182 "PEX_TX7"))
    (pad "BL35" smd circle (at 5.599887 18.400014) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BL36" smd circle (at 6.399987 18.400014) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1159 "SNN_SPARE_68"))
    (pad "BL37" smd circle (at 7.199909 18.400014) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1161 "PEX_TX10"))
    (pad "BL38" smd circle (at 8.000009 18.400014) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BL39" smd circle (at 8.800109 18.400014) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 904 "FBA_D<0>"))
    (pad "BL40" smd circle (at 9.599905 18.400014) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1166 "PEX_TX13"))
    (pad "BL41" smd circle (at 10.400005 18.400014) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BL42" smd circle (at 11.199901 18.400014) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 913 "FBA_DQS_RN0"))
    (pad "BL43" smd circle (at 12.000001 18.400014) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 900 "FBA_D<10>"))
    (pad "BL44" smd circle (at 12.800101 18.400014) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BL45" smd circle (at 13.599897 18.400014) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1464 "SNN_SPARE_69"))
    (pad "BL46" smd circle (at 14.399997 18.400014) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1205 "SNN_FBA_DBI2"))
    (pad "BL47" smd circle (at 15.200097 18.400014) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BL48" smd circle (at 15.999993 18.400014) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 917 "FBA_D<19>"))
    (pad "BL49" smd circle (at 16.800093 18.400014) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 922 "FBA_D<20>"))
    (pad "BL50" smd circle (at 17.599889 18.400014) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BL51" smd circle (at 18.399989 18.400014) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 920 "FBA_D<22>"))
    (pad "BL52" smd circle (at 19.200089 18.400014) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 919 "FBA_D<23>"))
    (pad "BL53" smd circle (at 20.000011 18.400014) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 811 "FBA_CMD<16>"))
    (pad "BL54" smd circle (at 20.800111 18.400014) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 815 "FBA_CMD<17>"))
    (pad "BL55" smd circle (at 21.599906 18.400014) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 809 "FBA_CMD<15>"))
    (pad "BM3" smd circle (at -20.000011 19.200114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1355 "SNN_FBH_D<48>"))
    (pad "BM4" smd circle (at -19.200114 19.200114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BM5" smd circle (at -18.399989 19.200114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1402 "SNN_FBH_D<52>"))
    (pad "BM6" smd circle (at -17.599889 19.200114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1403 "SNN_FBH_D<53>"))
    (pad "BM7" smd circle (at -16.800093 19.200114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1441 "SNN_FBH_D<54>"))
    (pad "BM8" smd circle (at -15.999993 19.200114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1460 "SNN_FBH_D<60>"))
    (pad "BM9" smd circle (at -15.200097 19.200114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1431 "SNN_FBH_DQS_WP7"))
    (pad "BM10" smd circle (at -14.399997 19.200114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1433 "GV_RX2*"))
    (pad "BM11" smd circle (at -13.599897 19.200114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1491 "GV_RXCLK"))
    (pad "BM12" smd circle (at -12.800101 19.200114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1486 "GV_RXCLK*"))
    (pad "BM13" smd circle (at -12.000001 19.200114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1518 "GV_TX18*"))
    (pad "BM14" smd circle (at -11.199901 19.200114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1497 "GV_TX14"))
    (pad "BM15" smd circle (at -10.400005 19.200114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1496 "GV_TX14*"))
    (pad "BM16" smd circle (at -9.599905 19.200114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1529 "GV_TXCLK*"))
    (pad "BM17" smd circle (at -8.800109 19.200114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1538 "GV_TX10"))
    (pad "BM18" smd circle (at -8.000009 19.200114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1539 "GV_TX10*"))
    (pad "BM19" smd circle (at -7.199909 19.200114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1534 "GV_TX8*"))
    (pad "BM20" smd circle (at -6.400013 19.200114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1535 "GV_TX4"))
    (pad "BM21" smd circle (at -5.599913 19.200114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1499 "GV_TX4*"))
    (pad "BM22" smd circle (at -4.800092 19.200114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1527 "GV_TX2*"))
    (pad "BM23" smd circle (at -3.999992 19.200114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1120 "PEX_REFCLK"))
    (pad "BM24" smd circle (at -3.199892 19.200114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1121 "PEX_REFCLK*"))
    (pad "BM25" smd circle (at -2.399995 19.200114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1156 "PEX_TX0*"))
    (pad "BM26" smd circle (at -1.599895 19.200114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1157 "PEX_TX1"))
    (pad "BM27" smd circle (at -0.8001 19.200114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1158 "PEX_TX1*"))
    (pad "BM28" smd circle (at 0 19.200114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1173 "PEX_TX2*"))
    (pad "BM29" smd circle (at 0.8001 19.200114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1644 "PEX_TX3"))
    (pad "BM30" smd circle (at 1.599895 19.200114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1645 "PEX_TX3*"))
    (pad "BM31" smd circle (at 2.399995 19.200114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1177 "PEX_TX4*"))
    (pad "BM32" smd circle (at 3.199892 19.200114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1181 "PEX_TX6"))
    (pad "BM33" smd circle (at 3.999992 19.200114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1179 "PEX_TX6*"))
    (pad "BM34" smd circle (at 4.800092 19.200114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1183 "PEX_TX7*"))
    (pad "BM35" smd circle (at 5.599887 19.200114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1184 "PEX_TX9"))
    (pad "BM36" smd circle (at 6.399987 19.200114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1185 "PEX_TX9*"))
    (pad "BM37" smd circle (at 7.199909 19.200114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1162 "PEX_TX10*"))
    (pad "BM38" smd circle (at 8.000009 19.200114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1163 "PEX_TX12"))
    (pad "BM39" smd circle (at 8.800109 19.200114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1164 "PEX_TX12*"))
    (pad "BM40" smd circle (at 9.599905 19.200114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1167 "PEX_TX13*"))
    (pad "BM41" smd circle (at 10.400005 19.200114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1168 "PEX_TX15"))
    (pad "BM42" smd circle (at 11.199901 19.200114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1169 "PEX_TX15*"))
    (pad "BM43" smd circle (at 12.000001 19.200114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1203 "PEX_TSTCLK_OUT"))
    (pad "BM44" smd circle (at 12.800101 19.200114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 901 "FBA_DQM1"))
    (pad "BM45" smd circle (at 13.599897 19.200114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 895 "FBA_D<9>"))
    (pad "BM46" smd circle (at 14.399997 19.200114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 915 "FBA_D<17>"))
    (pad "BM47" smd circle (at 15.200097 19.200114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 918 "FBA_D<18>"))
    (pad "BM48" smd circle (at 15.999993 19.200114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 923 "FBA_DQM2"))
    (pad "BM49" smd circle (at 16.800093 19.200114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 925 "FBA_DQS_WP2"))
    (pad "BM50" smd circle (at 17.599889 19.200114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 924 "FBA_DQS_RN2"))
    (pad "BM51" smd circle (at 18.399989 19.200114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 921 "FBA_D<21>"))
    (pad "BM52" smd circle (at 19.200089 19.200114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BM53" smd circle (at 20.000011 19.200114) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 810 "FBA_CMD<14>"))
    (pad "BN1" smd circle (at -21.599906 20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1578 "SNN_GPU_NC_21"))
    (pad "BN2" smd circle (at -20.800111 20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1358 "SNN_FBH_CMD<29>"))
    (pad "BN3" smd circle (at -20.000011 20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BN4" smd circle (at -19.200114 20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1362 "SNN_FBH_DQS_RN6"))
    (pad "BN5" smd circle (at -18.399989 20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1365 "SNN_FBH_DQS_WP6"))
    (pad "BN6" smd circle (at -17.599889 20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1366 "SNN_FBH_D<55>"))
    (pad "BN7" smd circle (at -16.800093 20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1444 "SNN_FBH_D<63>"))
    (pad "BN8" smd circle (at -15.999993 20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1432 "SNN_FBH_D<62>"))
    (pad "BN9" smd circle (at -15.200097 20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1430 "SNN_FBH_D<61>"))
    (pad "BN10" smd circle (at -14.399997 20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1426 "GV_TX19"))
    (pad "BN11" smd circle (at -13.599897 20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1490 "GV_RX0"))
    (pad "BN12" smd circle (at -12.800101 20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1487 "GV_RX0*"))
    (pad "BN13" smd circle (at -12.000001 20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1516 "GV_TX15"))
    (pad "BN14" smd circle (at -11.199901 20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1541 "GV_TX16"))
    (pad "BN15" smd circle (at -10.400005 20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1519 "GV_TX16*"))
    (pad "BN16" smd circle (at -9.599905 20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1540 "GV_TX13"))
    (pad "BN17" smd circle (at -8.800109 20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1506 "GV_TX12"))
    (pad "BN18" smd circle (at -8.000009 20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1524 "GV_TX12*"))
    (pad "BN19" smd circle (at -7.199909 20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1505 "GV_TX9"))
    (pad "BN20" smd circle (at -6.400013 20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1533 "GV_TX6*"))
    (pad "BN21" smd circle (at -5.599913 20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1500 "GV_TX6"))
    (pad "BN22" smd circle (at -4.800092 20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1532 "SNN_SPARE_70"))
    (pad "BN23" smd circle (at -3.999992 20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1646 "PEX_RX0"))
    (pad "BN24" smd circle (at -3.199892 20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1523 "PEX_RX2"))
    (pad "BN25" smd circle (at -2.399995 20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1124 "PEX_RX2*"))
    (pad "BN26" smd circle (at -1.599895 20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1140 "SNN_SPARE_71"))
    (pad "BN27" smd circle (at -0.8001 20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1170 "PEX_RX4"))
    (pad "BN28" smd circle (at 0 20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1139 "PEX_RX4*"))
    (pad "BN29" smd circle (at 0.8001 20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1174 "SNN_SPARE_72"))
    (pad "BN30" smd circle (at 1.599895 20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1144 "PEX_RX6*"))
    (pad "BN31" smd circle (at 2.399995 20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1145 "PEX_TX5"))
    (pad "BN32" smd circle (at 3.199892 20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1178 "PEX_TX5*"))
    (pad "BN33" smd circle (at 3.999992 20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1647 "PEX_RX8*"))
    (pad "BN34" smd circle (at 4.800092 20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1149 "PEX_TX8"))
    (pad "BN35" smd circle (at 5.599887 20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1160 "PEX_TX8*"))
    (pad "BN36" smd circle (at 6.399987 20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1648 "PEX_RX10*"))
    (pad "BN37" smd circle (at 7.199909 20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1126 "PEX_TX11"))
    (pad "BN38" smd circle (at 8.000009 20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1165 "PEX_TX11*"))
    (pad "BN39" smd circle (at 8.800109 20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1649 "PEX_RX12*"))
    (pad "BN40" smd circle (at 9.599905 20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1130 "PEX_TX14"))
    (pad "BN41" smd circle (at 10.400005 20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1154 "PEX_TX14*"))
    (pad "BN42" smd circle (at 11.199901 20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1153 "PEX_RX14*"))
    (pad "BN43" smd circle (at 12.000001 20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1134 "PEX_TSTCLK_OUT*"))
    (pad "BN44" smd circle (at 12.800101 20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 896 "FBA_D<8>"))
    (pad "BN45" smd circle (at 13.599897 20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 903 "FBA_DQS_WP1"))
    (pad "BN46" smd circle (at 14.399997 20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 916 "FBA_D<16>"))
    (pad "BN47" smd circle (at 15.200097 20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 874 "FBA_CMD<1>"))
    (pad "BN48" smd circle (at 15.999993 20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 870 "FBA_CMD<4>"))
    (pad "BN49" smd circle (at 16.800093 20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 869 "FBA_CMD<5>"))
    (pad "BN50" smd circle (at 17.599889 20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 812 "FBA_CMD<7>"))
    (pad "BN51" smd circle (at 18.399989 20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 818 "FBA_CMD<10>"))
    (pad "BN52" smd circle (at 19.200089 20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 803 "FBA_CMD<12>"))
    (pad "BN53" smd circle (at 20.000011 20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BN54" smd circle (at 20.800111 20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 816 "FBA_CMD<13>"))
    (pad "BN55" smd circle (at 21.599906 20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1579 "SNN_GPU_NC_22"))
    (pad "BP1" smd circle (at -21.599906 20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1580 "SNN_GPU_NC_23"))
    (pad "BP2" smd circle (at -20.800111 20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1581 "SNN_GPU_NC_24"))
    (pad "BP3" smd circle (at -20.000011 20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1360 "SNN_FBH_CMD<30>"))
    (pad "BP5" smd circle (at -18.399989 20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1363 "SNN_FBH_DQM6"))
    (pad "BP6" smd circle (at -17.599889 20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BP8" smd circle (at -15.999993 20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1653 "SNN_FBH_DBI7"))
    (pad "BP9" smd circle (at -15.200097 20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BP11" smd circle (at -13.599897 20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1517 "GV_TX19*"))
    (pad "BP12" smd circle (at -12.800101 20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BP14" smd circle (at -11.199901 20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1650 "GV_TX15*"))
    (pad "BP15" smd circle (at -10.400005 20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BP17" smd circle (at -8.800109 20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1651 "GV_TX13*"))
    (pad "BP18" smd circle (at -8.000009 20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BP20" smd circle (at -6.400013 20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1652 "GV_TX9*"))
    (pad "BP21" smd circle (at -5.599913 20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BP23" smd circle (at -3.999992 20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1125 "PEX_RX0*"))
    (pad "BP24" smd circle (at -3.199892 20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BP26" smd circle (at -1.599895 20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BP27" smd circle (at -0.8001 20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BP29" smd circle (at 0.8001 20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BP30" smd circle (at 1.599895 20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1143 "PEX_RX6"))
    (pad "BP32" smd circle (at 3.199892 20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BP33" smd circle (at 3.999992 20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1146 "PEX_RX8"))
    (pad "BP35" smd circle (at 5.599887 20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BP36" smd circle (at 6.399987 20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1150 "PEX_RX10"))
    (pad "BP38" smd circle (at 8.000009 20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BP39" smd circle (at 8.800109 20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1127 "PEX_RX12"))
    (pad "BP41" smd circle (at 10.400005 20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BP42" smd circle (at 11.199901 20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1131 "PEX_RX14"))
    (pad "BP44" smd circle (at 12.800101 20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BP45" smd circle (at 13.599897 20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 902 "FBA_DQS_RN1"))
    (pad "BP47" smd circle (at 15.200097 20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BP48" smd circle (at 15.999993 20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 871 "FBA_CMD<3>"))
    (pad "BP50" smd circle (at 17.599889 20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "BP51" smd circle (at 18.399989 20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 806 "FBA_CMD<9>"))
    (pad "BP53" smd circle (at 20.000011 20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 808 "FBA_CMD<11>"))
    (pad "BP54" smd circle (at 20.800111 20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1582 "SNN_GPU_NC_25"))
    (pad "BP55" smd circle (at 21.599906 20.800111) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1583 "SNN_GPU_NC_26"))
    (pad "BR2" smd circle (at -20.800111 21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1584 "SNN_GPU_NC_27"))
    (pad "BR3" smd circle (at -20.000011 21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1585 "SNN_GPU_NC_28"))
    (pad "BR5" smd circle (at -18.399989 21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1361 "SNN_FBH_CMD<31>"))
    (pad "BR6" smd circle (at -17.599889 21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1364 "SNN_FBH_CMD<32>"))
    (pad "BR8" smd circle (at -15.999993 21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 975 "THERM_DN"))
    (pad "BR9" smd circle (at -15.200097 21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 974 "THERM_DP"))
    (pad "BR11" smd circle (at -13.599897 21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1520 "GV_TX17"))
    (pad "BR12" smd circle (at -12.800101 21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1521 "GV_TX17*"))
    (pad "BR14" smd circle (at -11.199901 21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1512 "GV_TXCTL"))
    (pad "BR15" smd circle (at -10.400005 21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1513 "GV_TXCTL*"))
    (pad "BR17" smd circle (at -8.800109 21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1509 "GV_TX11"))
    (pad "BR18" smd circle (at -8.000009 21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1510 "GV_TX11*"))
    (pad "BR20" smd circle (at -6.400013 21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1536 "GV_TX7"))
    (pad "BR21" smd circle (at -5.599913 21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1537 "GV_TX7*"))
    (pad "BR23" smd circle (at -3.999992 21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1122 "PEX_RX1"))
    (pad "BR24" smd circle (at -3.199892 21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1123 "PEX_RX1*"))
    (pad "BR26" smd circle (at -1.599895 21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1137 "PEX_RX3"))
    (pad "BR27" smd circle (at -0.8001 21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1138 "PEX_RX3*"))
    (pad "BR29" smd circle (at 0.8001 21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1141 "PEX_RX5"))
    (pad "BR30" smd circle (at 1.599895 21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1142 "PEX_RX5*"))
    (pad "BR32" smd circle (at 3.199892 21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1147 "PEX_RX7"))
    (pad "BR33" smd circle (at 3.999992 21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1148 "PEX_RX7*"))
    (pad "BR35" smd circle (at 5.599887 21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1151 "PEX_RX9"))
    (pad "BR36" smd circle (at 6.399987 21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1152 "PEX_RX9*"))
    (pad "BR38" smd circle (at 8.000009 21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1128 "PEX_RX11"))
    (pad "BR39" smd circle (at 8.800109 21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1129 "PEX_RX11*"))
    (pad "BR41" smd circle (at 10.400005 21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1132 "PEX_RX13"))
    (pad "BR42" smd circle (at 11.199901 21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1133 "PEX_RX13*"))
    (pad "BR44" smd circle (at 12.800101 21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1135 "PEX_RX15"))
    (pad "BR45" smd circle (at 13.599897 21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1136 "PEX_RX15*"))
    (pad "BR47" smd circle (at 15.200097 21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 872 "FBA_CMD<0>"))
    (pad "BR48" smd circle (at 15.999993 21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 873 "FBA_CMD<2>"))
    (pad "BR50" smd circle (at 17.599889 21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 823 "FBA_CMD<6>"))
    (pad "BR51" smd circle (at 18.399989 21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 817 "FBA_CMD<8>"))
    (pad "BR53" smd circle (at 20.000011 21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1586 "SNN_GPU_NC_29"))
    (pad "BR54" smd circle (at 20.800111 21.599906) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1587 "SNN_GPU_NC_30"))
    (pad "C1" smd circle (at -21.599906 -20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1588 "SNN_GPU_NC_31"))
    (pad "C2" smd circle (at -20.800111 -20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "FBF_CMD<15>"))
    (pad "C3" smd circle (at -20.000011 -20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "C4" smd circle (at -19.200114 -20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 239 "FBF_D<28>"))
    (pad "C5" smd circle (at -18.399989 -20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 240 "FBF_DQM3"))
    (pad "C6" smd circle (at -17.599889 -20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "FBF_CMD<11>"))
    (pad "C7" smd circle (at -16.800093 -20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 235 "FBF_D<25>"))
    (pad "C8" smd circle (at -15.999993 -20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "FBF_CMD<9>"))
    (pad "C9" smd circle (at -15.200097 -20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "FBF_CMD<6>"))
    (pad "C10" smd circle (at -14.399997 -20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 313 "FBE_DQM7"))
    (pad "C11" smd circle (at -13.599897 -20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 220 "FBF_CMD<4>"))
    (pad "C12" smd circle (at -12.800101 -20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 224 "FBF_CMD<1>"))
    (pad "C13" smd circle (at -12.000001 -20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 311 "FBE_D<56>"))
    (pad "C14" smd circle (at -11.199901 -20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1278 "SNN_FBE_CMD<32>"))
    (pad "C15" smd circle (at -10.400005 -20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1276 "SNN_FBE_CMD<29>"))
    (pad "C16" smd circle (at -9.599905 -20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 335 "FBE_DQM6"))
    (pad "C17" smd circle (at -8.800109 -20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 279 "FBE_CMD<27>"))
    (pad "C18" smd circle (at -8.000009 -20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 287 "FBE_CMD<24>"))
    (pad "C19" smd circle (at -7.199909 -20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 325 "FBE_DQS_RN4"))
    (pad "C20" smd circle (at -6.400013 -20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1284 "SNN_FBE_CMD<22>"))
    (pad "C21" smd circle (at -5.599913 -20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 278 "FBE_CMD<19>"))
    (pad "C22" smd circle (at -4.800092 -20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 367 "FBE_D<23>"))
    (pad "C23" smd circle (at -3.999992 -20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 295 "FBE_CMD<17>"))
    (pad "C24" smd circle (at -3.199892 -20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 290 "FBE_CMD<14>"))
    (pad "C25" smd circle (at -2.399995 -20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 364 "FBE_D<16>"))
    (pad "C26" smd circle (at -1.599895 -20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 284 "FBE_CMD<12>"))
    (pad "C27" smd circle (at -0.8001 -20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 276 "FBE_CMD<9>"))
    (pad "C28" smd circle (at 0 -20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 443 "FBD_DQM7"))
    (pad "C29" smd circle (at 0.8001 -20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 445 "FBD_DQS_WP7"))
    (pad "C30" smd circle (at 1.599895 -20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 303 "FBE_CMD<6>"))
    (pad "C31" smd circle (at 2.399995 -20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 470 "FBD_D<48>"))
    (pad "C32" smd circle (at 3.199892 -20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 353 "FBE_CMD<2>"))
    (pad "C33" smd circle (at 3.999992 -20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1263 "SNN_FBD_CMD<32>"))
    (pad "C34" smd circle (at 4.800092 -20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 475 "FBD_D<49>"))
    (pad "C35" smd circle (at 5.599887 -20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1258 "SNN_FBD_CMD<30>"))
    (pad "C36" smd circle (at 6.399987 -20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 409 "FBD_CMD<27>"))
    (pad "C37" smd circle (at 7.199909 -20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 448 "FBD_D<32>"))
    (pad "C38" smd circle (at 8.000009 -20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 407 "FBD_CMD<25>"))
    (pad "C39" smd circle (at 8.800109 -20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1256 "SNN_FBD_CMD<22>"))
    (pad "C40" smd circle (at 9.599905 -20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 500 "FBD_DQM2"))
    (pad "C41" smd circle (at 10.400005 -20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 416 "FBD_CMD<20>"))
    (pad "C42" smd circle (at 11.199901 -20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 425 "FBD_CMD<17>"))
    (pad "C43" smd circle (at 12.000001 -20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 492 "FBD_D<16>"))
    (pad "C44" smd circle (at 12.800101 -20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 421 "FBD_CMD<16>"))
    (pad "C45" smd circle (at 13.599897 -20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 414 "FBD_CMD<12>"))
    (pad "C46" smd circle (at 14.399997 -20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 513 "FBD_DQS_WP0"))
    (pad "C47" smd circle (at 15.200097 -20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 427 "FBD_CMD<10>"))
    (pad "C48" smd circle (at 15.999993 -20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 422 "FBD_CMD<7>"))
    (pad "C49" smd circle (at 16.800093 -20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 573 "FBC_DQM7"))
    (pad "C50" smd circle (at 17.599889 -20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 481 "FBD_CMD<3>"))
    (pad "C51" smd circle (at 18.399989 -20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 483 "FBD_CMD<2>"))
    (pad "C52" smd circle (at 19.200089 -20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 570 "FBC_D<56>"))
    (pad "C53" smd circle (at 20.000011 -20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "C54" smd circle (at 20.800111 -20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 482 "FBD_CMD<0>"))
    (pad "C55" smd circle (at 21.599906 -20.000011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1589 "SNN_GPU_NC_32"))
    (pad "D3" smd circle (at -20.000011 -19.200089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 237 "FBF_D<29>"))
    (pad "D4" smd circle (at -19.200114 -19.200089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "D5" smd circle (at -18.399989 -19.200089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 242 "FBF_DQS_WP3"))
    (pad "D6" smd circle (at -17.599889 -19.200089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 233 "FBF_D<27>"))
    (pad "D7" smd circle (at -16.800093 -19.200089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 234 "FBF_D<26>"))
    (pad "D8" smd circle (at -15.999993 -19.200089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 232 "FBF_D<24>"))
    (pad "D9" smd circle (at -15.200097 -19.200089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 308 "FBE_D<61>"))
    (pad "D10" smd circle (at -14.399997 -19.200089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 307 "FBE_D<60>"))
    (pad "D11" smd circle (at -13.599897 -19.200089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 315 "FBE_DQS_WP7"))
    (pad "D12" smd circle (at -12.800101 -19.200089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 312 "FBE_D<57>"))
    (pad "D13" smd circle (at -12.000001 -19.200089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 332 "FBE_D<55>"))
    (pad "D14" smd circle (at -11.199901 -19.200089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 334 "FBE_D<52>"))
    (pad "D15" smd circle (at -10.400005 -19.200089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 330 "FBE_D<51>"))
    (pad "D16" smd circle (at -9.599905 -19.200089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 329 "FBE_D<50>"))
    (pad "D17" smd circle (at -8.800109 -19.200089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 321 "FBE_D<39>"))
    (pad "D18" smd circle (at -8.000009 -19.200089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 324 "FBE_DQM4"))
    (pad "D19" smd circle (at -7.199909 -19.200089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 326 "FBE_DQS_WP4"))
    (pad "D20" smd circle (at -6.400013 -19.200089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 319 "FBE_D<33>"))
    (pad "D21" smd circle (at -5.599913 -19.200089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 317 "FBE_D<32>"))
    (pad "D22" smd circle (at -4.800092 -19.200089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 368 "FBE_D<22>"))
    (pad "D23" smd circle (at -3.999992 -19.200089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 369 "FBE_D<20>"))
    (pad "D24" smd circle (at -3.199892 -19.200089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 372 "FBE_DQS_WP2"))
    (pad "D25" smd circle (at -2.399995 -19.200089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 371 "FBE_DQS_RN2"))
    (pad "D26" smd circle (at -1.599895 -19.200089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 436 "FBD_D<58>"))
    (pad "D27" smd circle (at -0.8001 -19.200089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 438 "FBD_D<59>"))
    (pad "D28" smd circle (at 0 -19.200089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 437 "FBD_D<60>"))
    (pad "D29" smd circle (at 0.8001 -19.200089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 444 "FBD_DQS_RN7"))
    (pad "D30" smd circle (at 1.599895 -19.200089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 469 "FBD_D<50>"))
    (pad "D31" smd circle (at 2.399995 -19.200089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 468 "FBD_D<54>"))
    (pad "D32" smd circle (at 3.199892 -19.200089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 471 "FBD_D<51>"))
    (pad "D33" smd circle (at 3.999992 -19.200089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 474 "FBD_D<55>"))
    (pad "D34" smd circle (at 4.800092 -19.200089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 472 "FBD_D<53>"))
    (pad "D35" smd circle (at 5.599887 -19.200089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 450 "FBD_D<39>"))
    (pad "D36" smd circle (at 6.399987 -19.200089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 455 "FBD_DQS_RN4"))
    (pad "D37" smd circle (at 7.199909 -19.200089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 456 "FBD_DQS_WP4"))
    (pad "D38" smd circle (at 8.000009 -19.200089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 449 "FBD_D<33>"))
    (pad "D39" smd circle (at 8.800109 -19.200089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 496 "FBD_D<22>"))
    (pad "D40" smd circle (at 9.599905 -19.200089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 498 "FBD_D<21>"))
    (pad "D41" smd circle (at 10.400005 -19.200089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 499 "FBD_D<20>"))
    (pad "D42" smd circle (at 11.199901 -19.200089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 493 "FBD_D<18>"))
    (pad "D43" smd circle (at 12.000001 -19.200089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 494 "FBD_D<17>"))
    (pad "D44" smd circle (at 12.800101 -19.200089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 507 "FBD_D<6>"))
    (pad "D45" smd circle (at 13.599897 -19.200089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 511 "FBD_DQM0"))
    (pad "D46" smd circle (at 14.399997 -19.200089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 512 "FBD_DQS_RN0"))
    (pad "D47" smd circle (at 15.200097 -19.200089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 566 "FBC_D<61>"))
    (pad "D48" smd circle (at 15.999993 -19.200089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 568 "FBC_D<60>"))
    (pad "D49" smd circle (at 16.800093 -19.200089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 575 "FBC_DQS_WP7"))
    (pad "D50" smd circle (at 17.599889 -19.200089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1241 "SNN_FBC_DBI7"))
    (pad "D51" smd circle (at 18.399989 -19.200089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 569 "FBC_D<57>"))
    (pad "D52" smd circle (at 19.200089 -19.200089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "D53" smd circle (at 20.000011 -19.200089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 592 "FBC_D<55>"))
    (pad "E1" smd circle (at -21.599906 -18.399989) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "FBF_CMD<18>"))
    (pad "E2" smd circle (at -20.800111 -18.399989) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "FBF_CMD<17>"))
    (pad "E3" smd circle (at -20.000011 -18.399989) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "FBF_CMD<16>"))
    (pad "E4" smd circle (at -19.200114 -18.399989) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 238 "FBF_D<30>"))
    (pad "E5" smd circle (at -18.399989 -18.399989) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 241 "FBF_DQS_RN3"))
    (pad "E6" smd circle (at -17.599889 -18.399989) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "E7" smd circle (at -16.800093 -18.399989) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 257 "FBF_D<16>"))
    (pad "E8" smd circle (at -15.999993 -18.399989) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1309 "SNN_FBF_DBI3"))
    (pad "E9" smd circle (at -15.200097 -18.399989) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "E10" smd circle (at -14.399997 -18.399989) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1301 "SNN_FBE_DBI7"))
    (pad "E11" smd circle (at -13.599897 -18.399989) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 314 "FBE_DQS_RN7"))
    (pad "E12" smd circle (at -12.800101 -18.399989) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "E13" smd circle (at -12.000001 -18.399989) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1304 "SNN_FBE_DBI6"))
    (pad "E14" smd circle (at -11.199901 -18.399989) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 331 "FBE_D<53>"))
    (pad "E15" smd circle (at -10.400005 -18.399989) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "E16" smd circle (at -9.599905 -18.399989) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 337 "FBE_DQS_WP6"))
    (pad "E17" smd circle (at -8.800109 -18.399989) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 327 "FBE_D<49>"))
    (pad "E18" smd circle (at -8.000009 -18.399989) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "E19" smd circle (at -7.199909 -18.399989) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 322 "FBE_D<36>"))
    (pad "E20" smd circle (at -6.400013 -18.399989) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 318 "FBE_D<34>"))
    (pad "E21" smd circle (at -5.599913 -18.399989) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "E22" smd circle (at -4.800092 -18.399989) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 370 "FBE_DQM2"))
    (pad "E23" smd circle (at -3.999992 -18.399989) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1289 "SNN_FBE_DBI2"))
    (pad "E24" smd circle (at -3.199892 -18.399989) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "E25" smd circle (at -2.399995 -18.399989) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 362 "FBE_D<17>"))
    (pad "E26" smd circle (at -1.599895 -18.399989) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 435 "FBD_D<63>"))
    (pad "E27" smd circle (at -0.8001 -18.399989) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "E28" smd circle (at 0 -18.399989) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 440 "FBD_D<61>"))
    (pad "E29" smd circle (at 0.8001 -18.399989) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "E30" smd circle (at 1.599895 -18.399989) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 442 "FBD_D<62>"))
    (pad "E31" smd circle (at 2.399995 -18.399989) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1264 "SNN_FBD_DBI6"))
    (pad "E32" smd circle (at 3.199892 -18.399989) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "E33" smd circle (at 3.999992 -18.399989) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 477 "FBD_DQS_RN6"))
    (pad "E34" smd circle (at 4.800092 -18.399989) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 473 "FBD_D<52>"))
    (pad "E35" smd circle (at 5.599887 -18.399989) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "E36" smd circle (at 6.399987 -18.399989) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 454 "FBD_DQM4"))
    (pad "E37" smd circle (at 7.199909 -18.399989) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 447 "FBD_D<35>"))
    (pad "E38" smd circle (at 8.000009 -18.399989) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "E39" smd circle (at 8.800109 -18.399989) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 497 "FBD_D<23>"))
    (pad "E40" smd circle (at 9.599905 -18.399989) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 501 "FBD_DQS_RN2"))
    (pad "E41" smd circle (at 10.400005 -18.399989) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "E42" smd circle (at 11.199901 -18.399989) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 495 "FBD_D<19>"))
    (pad "E43" smd circle (at 12.000001 -18.399989) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 508 "FBD_D<7>"))
    (pad "E44" smd circle (at 12.800101 -18.399989) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "E45" smd circle (at 13.599897 -18.399989) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 505 "FBD_D<1>"))
    (pad "E46" smd circle (at 14.399997 -18.399989) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 506 "FBD_D<0>"))
    (pad "E47" smd circle (at 15.200097 -18.399989) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "E48" smd circle (at 15.999993 -18.399989) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 567 "FBC_D<62>"))
    (pad "E49" smd circle (at 16.800093 -18.399989) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 574 "FBC_DQS_RN7"))
    (pad "E50" smd circle (at 17.599889 -18.399989) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "E51" smd circle (at 18.399989 -18.399989) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 571 "FBC_D<59>"))
    (pad "E52" smd circle (at 19.200089 -18.399989) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 572 "FBC_D<58>"))
    (pad "E53" smd circle (at 20.000011 -18.399989) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 594 "FBC_D<54>"))
    (pad "E54" smd circle (at 20.800111 -18.399989) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1234 "SNN_FBC_CMD<32>"))
    (pad "E55" smd circle (at 21.599906 -18.399989) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1236 "SNN_FBC_CMD<31>"))
    (pad "F1" smd circle (at -21.599906 -17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "FBF_CMD<20>"))
    (pad "F2" smd circle (at -20.800111 -17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "F3" smd circle (at -20.000011 -17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "FBF_CMD<19>"))
    (pad "F4" smd circle (at -19.200114 -17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 236 "FBF_D<31>"))
    (pad "F5" smd circle (at -18.399989 -17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "F6" smd circle (at -17.599889 -17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 262 "FBF_DQM2"))
    (pad "F8" smd circle (at -15.999993 -17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 256 "FBF_D<17>"))
    (pad "F9" smd circle (at -15.200097 -17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 305 "FBE_D<62>"))
    (pad "F11" smd circle (at -13.599897 -17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 309 "FBE_D<59>"))
    (pad "F12" smd circle (at -12.800101 -17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 310 "FBE_D<58>"))
    (pad "F14" smd circle (at -11.199901 -17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 333 "FBE_D<54>"))
    (pad "F15" smd circle (at -10.400005 -17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 336 "FBE_DQS_RN6"))
    (pad "F17" smd circle (at -8.800109 -17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 328 "FBE_D<48>"))
    (pad "F18" smd circle (at -8.000009 -17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 323 "FBE_D<37>"))
    (pad "F20" smd circle (at -6.400013 -17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 316 "FBE_D<35>"))
    (pad "F21" smd circle (at -5.599913 -17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1280 "SNN_FBE_DBI4"))
    (pad "F23" smd circle (at -3.999992 -17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 366 "FBE_D<21>"))
    (pad "F24" smd circle (at -3.199892 -17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 365 "FBE_D<19>"))
    (pad "F26" smd circle (at -1.599895 -17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 363 "FBE_D<18>"))
    (pad "F27" smd circle (at -0.8001 -17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1287 "SNN_FBD_DBI7"))
    (pad "F29" smd circle (at 0.8001 -17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 439 "FBD_D<56>"))
    (pad "F30" smd circle (at 1.599895 -17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 441 "FBD_D<57>"))
    (pad "F32" smd circle (at 3.199892 -17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 476 "FBD_DQM6"))
    (pad "F33" smd circle (at 3.999992 -17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 478 "FBD_DQS_WP6"))
    (pad "F35" smd circle (at 5.599887 -17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 451 "FBD_D<38>"))
    (pad "F36" smd circle (at 6.399987 -17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 452 "FBD_D<36>"))
    (pad "F38" smd circle (at 8.000009 -17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 446 "FBD_D<34>"))
    (pad "F39" smd circle (at 8.800109 -17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 530 "FBD_D<15>"))
    (pad "F41" smd circle (at 10.400005 -17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 502 "FBD_DQS_WP2"))
    (pad "F42" smd circle (at 11.199901 -17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1268 "SNN_FBD_DBI2"))
    (pad "F44" smd circle (at 12.800101 -17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 510 "FBD_D<5>"))
    (pad "F45" smd circle (at 13.599897 -17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 504 "FBD_D<2>"))
    (pad "F47" smd circle (at 15.200097 -17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 565 "FBC_D<63>"))
    (pad "F48" smd circle (at 15.999993 -17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1242 "SNN_FBC_DBI6"))
    (pad "F50" smd circle (at 17.599889 -17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 591 "FBC_D<50>"))
    (pad "F51" smd circle (at 18.399989 -17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "F52" smd circle (at 19.200089 -17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 593 "FBC_D<53>"))
    (pad "F53" smd circle (at 20.000011 -17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1237 "SNN_FBC_CMD<30>"))
    (pad "F54" smd circle (at 20.800111 -17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "F55" smd circle (at 21.599906 -17.599889) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1235 "SNN_FBC_CMD<29>"))
    (pad "G3" smd circle (at -20.000011 -16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 56 "FBF_D<32>"))
    (pad "G4" smd circle (at -19.200114 -16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 57 "FBF_D<33>"))
    (pad "G5" smd circle (at -18.399989 -16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 59 "FBF_D<34>"))
    (pad "G8" smd circle (at -15.999993 -16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 254 "FBF_D<18>"))
    (pad "G9" smd circle (at -15.200097 -16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 306 "FBE_D<63>"))
    (pad "G11" smd circle (at -13.599897 -16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 248 "FBF_D<4>"))
    (pad "G12" smd circle (at -12.800101 -16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 245 "FBF_D<3>"))
    (pad "G14" smd circle (at -11.199901 -16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 338 "FBE_D<45>"))
    (pad "G15" smd circle (at -10.400005 -16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 340 "FBE_D<44>"))
    (pad "G17" smd circle (at -8.800109 -16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 348 "FBE_DQS_WP5"))
    (pad "G18" smd circle (at -8.000009 -16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 320 "FBE_D<38>"))
    (pad "G20" smd circle (at -6.400013 -16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 401 "FBE_D<30>"))
    (pad "G21" smd circle (at -5.599913 -16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 397 "FBE_D<26>"))
    (pad "G23" smd circle (at -3.999992 -16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 398 "FBE_D<24>"))
    (pad "G24" smd circle (at -3.199892 -16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 393 "FBE_DQS_RN1"))
    (pad "G26" smd circle (at -1.599895 -16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 392 "FBE_DQM1"))
    (pad "G27" smd circle (at -0.8001 -16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 379 "FBE_D<7>"))
    (pad "G29" smd circle (at 0.8001 -16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 377 "FBE_D<0>"))
    (pad "G30" smd circle (at 1.599895 -16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 375 "FBE_D<1>"))
    (pad "G32" smd circle (at 3.199892 -16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1262 "SNN_FBD_DBI5"))
    (pad "G33" smd circle (at 3.999992 -16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 467 "FBD_DQS_WP5"))
    (pad "G35" smd circle (at 5.599887 -16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 453 "FBD_D<37>"))
    (pad "G36" smd circle (at 6.399987 -16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1265 "SNN_FBD_DBI4"))
    (pad "G38" smd circle (at 8.000009 -16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 518 "FBD_D<28>"))
    (pad "G39" smd circle (at 8.800109 -16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 529 "FBD_D<14>"))
    (pad "G41" smd circle (at 10.400005 -16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 531 "FBD_D<12>"))
    (pad "G42" smd circle (at 11.199901 -16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 534 "FBD_DQS_RN1"))
    (pad "G44" smd circle (at 12.800101 -16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 509 "FBD_D<4>"))
    (pad "G45" smd circle (at 13.599897 -16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1261 "SNN_FBD_DBI0"))
    (pad "G47" smd circle (at 15.200097 -16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 598 "FBC_D<46>"))
    (pad "G48" smd circle (at 15.999993 -16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 606 "FBC_DQM5"))
    (pad "G51" smd circle (at 18.399989 -16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 595 "FBC_DQM6"))
    (pad "G52" smd circle (at 19.200089 -16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 596 "FBC_DQS_RN6"))
    (pad "G53" smd circle (at 20.000011 -16.800093) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 597 "FBC_DQS_WP6"))
    (pad "H1" smd circle (at -21.599906 -15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "FBF_CMD<23>"))
    (pad "H2" smd circle (at -20.800111 -15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1294 "SNN_FBF_CMD<22>"))
    (pad "H3" smd circle (at -20.000011 -15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "FBF_CMD<21>"))
    (pad "H4" smd circle (at -19.200114 -15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 58 "FBF_D<35>"))
    (pad "H5" smd circle (at -18.399989 -15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 65 "FBF_DQS_RN4"))
    (pad "H6" smd circle (at -17.599889 -15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 264 "FBF_DQS_WP2"))
    (pad "H7" smd circle (at -16.800093 -15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 263 "FBF_DQS_RN2"))
    (pad "H8" smd circle (at -15.999993 -15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 258 "FBF_D<19>"))
    (pad "H9" smd circle (at -15.200097 -15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "H10" smd circle (at -14.399997 -15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 249 "FBF_D<6>"))
    (pad "H11" smd circle (at -13.599897 -15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 247 "FBF_D<5>"))
    (pad "H12" smd circle (at -12.800101 -15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "H13" smd circle (at -12.000001 -15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 246 "FBF_D<1>"))
    (pad "H14" smd circle (at -11.199901 -15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 341 "FBE_D<46>"))
    (pad "H15" smd circle (at -10.400005 -15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "H16" smd circle (at -9.599905 -15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 346 "FBE_DQM5"))
    (pad "H17" smd circle (at -8.800109 -15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 347 "FBE_DQS_RN5"))
    (pad "H18" smd circle (at -8.000009 -15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "H19" smd circle (at -7.199909 -15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 400 "FBE_D<31>"))
    (pad "H20" smd circle (at -6.400013 -15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 402 "FBE_D<29>"))
    (pad "H21" smd circle (at -5.599913 -15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "H22" smd circle (at -4.800092 -15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 395 "FBE_D<25>"))
    (pad "H23" smd circle (at -3.999992 -15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 390 "FBE_D<15>"))
    (pad "H24" smd circle (at -3.199892 -15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "H25" smd circle (at -2.399995 -15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 394 "FBE_DQS_WP1"))
    (pad "H26" smd circle (at -1.599895 -15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 386 "FBE_D<8>"))
    (pad "H27" smd circle (at -0.8001 -15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "H28" smd circle (at 0 -15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1285 "SNN_FBE_DBI0"))
    (pad "H29" smd circle (at 0.8001 -15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "H30" smd circle (at 1.599895 -15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 376 "FBE_D<2>"))
    (pad "H31" smd circle (at 2.399995 -15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 462 "FBD_D<47>"))
    (pad "H32" smd circle (at 3.199892 -15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "H33" smd circle (at 3.999992 -15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 459 "FBD_D<41>"))
    (pad "H34" smd circle (at 4.800092 -15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 466 "FBD_DQS_RN5"))
    (pad "H35" smd circle (at 5.599887 -15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "H36" smd circle (at 6.399987 -15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 519 "FBD_D<30>"))
    (pad "H37" smd circle (at 7.199909 -15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 520 "FBD_D<29>"))
    (pad "H38" smd circle (at 8.000009 -15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "H39" smd circle (at 8.800109 -15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 516 "FBD_D<27>"))
    (pad "H40" smd circle (at 9.599905 -15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 532 "FBD_D<13>"))
    (pad "H41" smd circle (at 10.400005 -15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "H42" smd circle (at 11.199901 -15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 535 "FBD_DQS_WP1"))
    (pad "H43" smd circle (at 12.000001 -15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 533 "FBD_DQM1"))
    (pad "H44" smd circle (at 12.800101 -15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "H45" smd circle (at 13.599897 -15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 503 "FBD_D<3>"))
    (pad "H46" smd circle (at 14.399997 -15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 599 "FBC_D<45>"))
    (pad "H47" smd circle (at 15.200097 -15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "H48" smd circle (at 15.999993 -15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 600 "FBC_D<44>"))
    (pad "H49" smd circle (at 16.800093 -15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 588 "FBC_D<48>"))
    (pad "H50" smd circle (at 17.599889 -15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 587 "FBC_D<49>"))
    (pad "H51" smd circle (at 18.399989 -15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 590 "FBC_D<51>"))
    (pad "H52" smd circle (at 19.200089 -15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 589 "FBC_D<52>"))
    (pad "H53" smd circle (at 20.000011 -15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 540 "FBC_CMD<28>"))
    (pad "H54" smd circle (at 20.800111 -15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 539 "FBC_CMD<27>"))
    (pad "H55" smd circle (at 21.599906 -15.999993) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 541 "FBC_CMD<26>"))
    (pad "J1" smd circle (at -21.599906 -15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "FBF_CMD<25>"))
    (pad "J2" smd circle (at -20.800111 -15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "J3" smd circle (at -20.000011 -15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "FBF_CMD<24>"))
    (pad "J4" smd circle (at -19.200114 -15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 66 "FBF_DQS_WP4"))
    (pad "J5" smd circle (at -18.399989 -15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "J6" smd circle (at -17.599889 -15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 260 "FBF_D<23>"))
    (pad "J7" smd circle (at -16.800093 -15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 261 "FBF_D<22>"))
    (pad "J8" smd circle (at -15.999993 -15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "J9" smd circle (at -15.200097 -15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 255 "FBF_D<20>"))
    (pad "J10" smd circle (at -14.399997 -15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 250 "FBF_D<7>"))
    (pad "J11" smd circle (at -13.599897 -15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 251 "FBF_DQM0"))
    (pad "J12" smd circle (at -12.800101 -15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 244 "FBF_D<2>"))
    (pad "J13" smd circle (at -12.000001 -15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1281 "SNN_FBF_DBI0"))
    (pad "J14" smd circle (at -11.199901 -15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 339 "FBE_D<47>"))
    (pad "J15" smd circle (at -10.400005 -15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 294 "FBE1_CLK0*"))
    (pad "J16" smd circle (at -9.599905 -15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1283 "SNN_FBE_DBI5"))
    (pad "J17" smd circle (at -8.800109 -15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 344 "FBE_D<43>"))
    (pad "J18" smd circle (at -8.000009 -15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 343 "FBE_D<40>"))
    (pad "J19" smd circle (at -7.199909 -15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 404 "FBE_DQS_RN3"))
    (pad "J20" smd circle (at -6.400013 -15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 399 "FBE_D<28>"))
    (pad "J21" smd circle (at -5.599913 -15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 396 "FBE_D<27>"))
    (pad "J22" smd circle (at -4.800092 -15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1288 "SNN_FBE_DBI3"))
    (pad "J23" smd circle (at -3.999992 -15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 391 "FBE_D<14>"))
    (pad "J24" smd circle (at -3.199892 -15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 388 "FBE_D<12>"))
    (pad "J25" smd circle (at -2.399995 -15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 385 "FBE_D<11>"))
    (pad "J26" smd circle (at -1.599895 -15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 387 "FBE_D<9>"))
    (pad "J27" smd circle (at -0.8001 -15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 380 "FBE_D<6>"))
    (pad "J28" smd circle (at 0 -15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 382 "FBE_DQS_RN0"))
    (pad "J29" smd circle (at 0.8001 -15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 381 "FBE_DQM0"))
    (pad "J30" smd circle (at 1.599895 -15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 373 "FBE_D<3>"))
    (pad "J31" smd circle (at 2.399995 -15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 463 "FBD_D<46>"))
    (pad "J32" smd circle (at 3.199892 -15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 464 "FBD_D<45>"))
    (pad "J33" smd circle (at 3.999992 -15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 457 "FBD_D<42>"))
    (pad "J34" smd circle (at 4.800092 -15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 460 "FBD_D<40>"))
    (pad "J35" smd circle (at 5.599887 -15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 465 "FBD_DQM5"))
    (pad "J36" smd circle (at 6.399987 -15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 523 "FBD_DQS_RN3"))
    (pad "J37" smd circle (at 7.199909 -15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 524 "FBD_DQS_WP3"))
    (pad "J38" smd circle (at 8.000009 -15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 423 "FBD1_CLK0"))
    (pad "J39" smd circle (at 8.800109 -15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 517 "FBD_D<26>"))
    (pad "J40" smd circle (at 9.599905 -15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 515 "FBD_D<24>"))
    (pad "J41" smd circle (at 10.400005 -15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1260 "SNN_FBD_DBI1"))
    (pad "J42" smd circle (at 11.199901 -15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 527 "FBD_D<11>"))
    (pad "J43" smd circle (at 12.000001 -15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 528 "FBD_D<10>"))
    (pad "J44" smd circle (at 12.800101 -15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 486 "FBD0_CLK0*"))
    (pad "J45" smd circle (at 13.599897 -15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1244 "SNN_GPU_NC_33"))
    (pad "J46" smd circle (at 14.399997 -15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1245 "SNN_FBC_DBI5"))
    (pad "J47" smd circle (at 15.200097 -15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 608 "FBC_DQS_WP5"))
    (pad "J48" smd circle (at 15.999993 -15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "J49" smd circle (at 16.800093 -15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 604 "FBC_D<47>"))
    (pad "J50" smd circle (at 17.599889 -15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 583 "FBC_D<39>"))
    (pad "J51" smd circle (at 18.399989 -15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "J52" smd circle (at 19.200089 -15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 582 "FBC_D<38>"))
    (pad "J53" smd circle (at 20.000011 -15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 537 "FBC_CMD<25>"))
    (pad "J54" smd circle (at 20.800111 -15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "J55" smd circle (at 21.599906 -15.200097) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 547 "FBC_CMD<24>"))
    (pad "K3" smd circle (at -20.000011 -14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 62 "FBF_D<36>"))
    (pad "K4" smd circle (at -19.200114 -14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "FBF_D<37>"))
    (pad "K5" smd circle (at -18.399989 -14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 64 "FBF_DQM4"))
    (pad "K8" smd circle (at -15.999993 -14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 259 "FBF_D<21>"))
    (pad "K9" smd circle (at -15.200097 -14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1299 "SNN_FBF_DBI2"))
    (pad "K11" smd circle (at -13.599897 -14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 253 "FBF_DQS_WP0"))
    (pad "K12" smd circle (at -12.800101 -14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1282 "FBEFGH_MPLL_AVDD"))
    (pad "K14" smd circle (at -11.199901 -14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 243 "FBF_D<0>"))
    (pad "K15" smd circle (at -10.400005 -14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 293 "FBE1_CLK0"))
    (pad "K17" smd circle (at -8.800109 -14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 342 "FBE_D<42>"))
    (pad "K18" smd circle (at -8.000009 -14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 345 "FBE_D<41>"))
    (pad "K20" smd circle (at -6.400013 -14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 405 "FBE_DQS_WP3"))
    (pad "K21" smd circle (at -5.599913 -14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 403 "FBE_DQM3"))
    (pad "K23" smd circle (at -3.999992 -14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 389 "FBE_D<13>"))
    (pad "K24" smd circle (at -3.199892 -14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1279 "SNN_FBE_DBI1"))
    (pad "K26" smd circle (at -1.599895 -14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 384 "FBE_D<10>"))
    (pad "K27" smd circle (at -0.8001 -14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 378 "FBE_D<5>"))
    (pad "K29" smd circle (at 0.8001 -14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 383 "FBE_DQS_WP0"))
    (pad "K30" smd circle (at 1.599895 -14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 374 "FBE_D<4>"))
    (pad "K32" smd circle (at 3.199892 -14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 461 "FBD_D<44>"))
    (pad "K33" smd circle (at 3.999992 -14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 458 "FBD_D<43>"))
    (pad "K35" smd circle (at 5.599887 -14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1266 "SNN_GPU_NC_34"))
    (pad "K36" smd circle (at 6.399987 -14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 521 "FBD_D<31>"))
    (pad "K38" smd circle (at 8.000009 -14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 424 "FBD1_CLK0*"))
    (pad "K39" smd circle (at 8.800109 -14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1461 "SNN_FBD_DBI3"))
    (pad "K41" smd circle (at 10.400005 -14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 514 "FBD_D<25>"))
    (pad "K42" smd circle (at 11.199901 -14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 525 "FBD_D<9>"))
    (pad "K44" smd circle (at 12.800101 -14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 485 "FBD0_CLK0"))
    (pad "K45" smd circle (at 13.599897 -14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1243 "SNN_GPU_NC_35"))
    (pad "K47" smd circle (at 15.200097 -14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 607 "FBC_DQS_RN5"))
    (pad "K48" smd circle (at 15.999993 -14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 605 "FBC_D<43>"))
    (pad "K51" smd circle (at 18.399989 -14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 581 "FBC_D<36>"))
    (pad "K52" smd circle (at 19.200089 -14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 580 "FBC_D<37>"))
    (pad "K53" smd circle (at 20.000011 -14.399997) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 584 "FBC_DQM4"))
    (pad "L1" smd circle (at -21.599906 -13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "FBF_CMD<28>"))
    (pad "L2" smd circle (at -20.800111 -13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "FBF_CMD<27>"))
    (pad "L3" smd circle (at -20.000011 -13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "FBF_CMD<26>"))
    (pad "L4" smd circle (at -19.200114 -13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 63 "FBF_D<38>"))
    (pad "L5" smd circle (at -18.399989 -13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "FBF_D<39>"))
    (pad "L6" smd circle (at -17.599889 -13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1302 "SNN_FBF_DBI4"))
    (pad "L7" smd circle (at -16.800093 -13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 274 "FBF_DQS_RN1"))
    (pad "L8" smd circle (at -15.999993 -13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 275 "FBF_DQS_WP1"))
    (pad "L9" smd circle (at -15.200097 -13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1303 "SNN_GPU_NC_38"))
    (pad "L10" smd circle (at -14.399997 -13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1298 "SNN_GPU_NC_36"))
    (pad "L11" smd circle (at -13.599897 -13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 252 "FBF_DQS_RN0"))
    (pad "L12" smd circle (at -12.800101 -13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "L13" smd circle (at -12.000001 -13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1590 "SNN_SPARE_73"))
    (pad "L14" smd circle (at -11.199901 -13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1591 "SNN_SPARE_74"))
    (pad "L15" smd circle (at -10.400005 -13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "L16" smd circle (at -9.599905 -13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1274 "SNN_FBE1_CLK1*"))
    (pad "L17" smd circle (at -8.800109 -13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1273 "SNN_FBE1_CLK1"))
    (pad "L18" smd circle (at -8.000009 -13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "L19" smd circle (at -7.199909 -13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1272 "FBEF_REFCLK"))
    (pad "L20" smd circle (at -6.400013 -13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1271 "FBEF_REFCLK*"))
    (pad "L21" smd circle (at -5.599913 -13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "L22" smd circle (at -4.800092 -13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1269 "SNN_FBE0_CLK1"))
    (pad "L23" smd circle (at -3.999992 -13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1270 "SNN_FBE0_CLK1*"))
    (pad "L24" smd circle (at -3.199892 -13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "L25" smd circle (at -2.399995 -13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 355 "FBE0_CLK0"))
    (pad "L26" smd circle (at -1.599895 -13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 356 "FBE0_CLK0*"))
    (pad "L27" smd circle (at -0.8001 -13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "L28" smd circle (at 0 -13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "L29" smd circle (at 0.8001 -13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "L30" smd circle (at 1.599895 -13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1254 "SNN_FBD1_CLK1"))
    (pad "L31" smd circle (at 2.399995 -13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1255 "SNN_FBD1_CLK1*"))
    (pad "L32" smd circle (at 3.199892 -13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "L33" smd circle (at 3.999992 -13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1252 "SNN_FBD0_CLK1*"))
    (pad "L34" smd circle (at 4.800092 -13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1251 "SNN_FBD0_CLK1"))
    (pad "L35" smd circle (at 5.599887 -13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "L36" smd circle (at 6.399987 -13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1253 "SNN_GPU_NC_37"))
    (pad "L37" smd circle (at 7.199909 -13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 522 "FBD_DQM3"))
    (pad "L38" smd circle (at 8.000009 -13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "L39" smd circle (at 8.800109 -13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1056 "FB_CAL_PD_VDDQ"))
    (pad "L40" smd circle (at 9.599905 -13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1250 "FB_CAL_PU_GND"))
    (pad "L41" smd circle (at 10.400005 -13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "L42" smd circle (at 11.199901 -13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1592 "FB_CAL_TERM_GND"))
    (pad "L43" smd circle (at 12.000001 -13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 526 "FBD_D<8>"))
    (pad "L44" smd circle (at 12.800101 -13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "L45" smd circle (at 13.599897 -13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 603 "FBC_D<40>"))
    (pad "L46" smd circle (at 14.399997 -13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 601 "FBC_D<41>"))
    (pad "L47" smd circle (at 15.200097 -13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 602 "FBC_D<42>"))
    (pad "L48" smd circle (at 15.999993 -13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 659 "FBC_D<30>"))
    (pad "L49" smd circle (at 16.800093 -13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 661 "FBC_D<31>"))
    (pad "L50" smd circle (at 17.599889 -13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 578 "FBC_D<35>"))
    (pad "L51" smd circle (at 18.399989 -13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 586 "FBC_DQS_WP4"))
    (pad "L52" smd circle (at 19.200089 -13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 585 "FBC_DQS_RN4"))
    (pad "L53" smd circle (at 20.000011 -13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 545 "FBC_CMD<23>"))
    (pad "L54" smd circle (at 20.800111 -13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1233 "SNN_FBC_CMD<22>"))
    (pad "L55" smd circle (at 21.599906 -13.599897) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 543 "FBC_CMD<21>"))
    (pad "M1" smd circle (at -21.599906 -12.800101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1297 "SNN_FBF_CMD<30>"))
    (pad "M2" smd circle (at -20.800111 -12.800101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "M3" smd circle (at -20.000011 -12.800101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1295 "SNN_FBF_CMD<29>"))
    (pad "M4" smd circle (at -19.200114 -12.800101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 85 "FBF_D<41>"))
    (pad "M5" smd circle (at -18.399989 -12.800101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "M6" smd circle (at -17.599889 -12.800101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 266 "FBF_D<15>"))
    (pad "M7" smd circle (at -16.800093 -12.800101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 265 "FBF_D<14>"))
    (pad "M8" smd circle (at -15.999993 -12.800101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "M9" smd circle (at -15.200097 -12.800101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 226 "FBF0_CLK0*"))
    (pad "M10" smd circle (at -14.399997 -12.800101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 225 "FBF0_CLK0"))
    (pad "M11" smd circle (at -13.599897 -12.800101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "M45" smd circle (at 13.599897 -12.800101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "M46" smd circle (at 14.399997 -12.800101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 553 "FBC1_CLK0"))
    (pad "M47" smd circle (at 15.200097 -12.800101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 554 "FBC1_CLK0*"))
    (pad "M48" smd circle (at 15.999993 -12.800101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "M49" smd circle (at 16.800093 -12.800101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 665 "FBC_DQS_WP3"))
    (pad "M50" smd circle (at 17.599889 -12.800101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 664 "FBC_DQS_RN3"))
    (pad "M51" smd circle (at 18.399989 -12.800101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "M52" smd circle (at 19.200089 -12.800101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 576 "FBC_D<34>"))
    (pad "M53" smd circle (at 20.000011 -12.800101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 546 "FBC_CMD<20>"))
    (pad "M54" smd circle (at 20.800111 -12.800101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "M55" smd circle (at 21.599906 -12.800101) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 538 "FBC_CMD<19>"))
    (pad "N3" smd circle (at -20.000011 -12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 82 "FBF_D<40>"))
    (pad "N4" smd circle (at -19.200114 -12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 84 "FBF_D<42>"))
    (pad "N5" smd circle (at -18.399989 -12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 83 "FBF_D<43>"))
    (pad "N8" smd circle (at -15.999993 -12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 273 "FBF_DQM1"))
    (pad "N9" smd circle (at -15.200097 -12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 271 "FBF_D<11>"))
    (pad "N11" smd circle (at -13.599897 -12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 272 "FBF_D<8>"))
    (pad "N13" smd circle (at -12.000001 -12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1593 "SNN_GPU_NC_39"))
    (pad "N14" smd circle (at -11.199901 -12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1286 "FBE_DEBUG"))
    (pad "N15" smd circle (at -10.400005 -12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "N16" smd circle (at -9.599905 -12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N17" smd circle (at -8.800109 -12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N18" smd circle (at -8.000009 -12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "N19" smd circle (at -7.199909 -12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N20" smd circle (at -6.400013 -12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N21" smd circle (at -5.599913 -12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "N22" smd circle (at -4.800092 -12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N23" smd circle (at -3.999992 -12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N24" smd circle (at -3.199892 -12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "N25" smd circle (at -2.399995 -12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N26" smd circle (at -1.599895 -12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N27" smd circle (at -0.8001 -12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "N28" smd circle (at 0 -12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N29" smd circle (at 0.8001 -12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "N30" smd circle (at 1.599895 -12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N31" smd circle (at 2.399995 -12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N32" smd circle (at 3.199892 -12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "N33" smd circle (at 3.999992 -12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N34" smd circle (at 4.800092 -12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N35" smd circle (at 5.599887 -12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "N36" smd circle (at 6.399987 -12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N37" smd circle (at 7.199909 -12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N38" smd circle (at 8.000009 -12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "N39" smd circle (at 8.800109 -12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N40" smd circle (at 9.599905 -12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N41" smd circle (at 10.400005 -12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "N42" smd circle (at 11.199901 -12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1267 "FBD_DEBUG"))
    (pad "N43" smd circle (at 12.000001 -12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1594 "SNN_GPU_NC_40"))
    (pad "N45" smd circle (at 13.599897 -12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1573 "FBABCD_MPLL_AVDD"))
    (pad "N47" smd circle (at 15.200097 -12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 662 "FBC_D<27>"))
    (pad "N48" smd circle (at 15.999993 -12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 660 "FBC_D<29>"))
    (pad "N51" smd circle (at 18.399989 -12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 579 "FBC_D<32>"))
    (pad "N52" smd circle (at 19.200089 -12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 577 "FBC_D<33>"))
    (pad "N53" smd circle (at 20.000011 -12.000001) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1239 "SNN_FBC_DBI4"))
    (pad "P1" smd circle (at -21.599906 -11.199901) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 97 "FBG_CMD<0>"))
    (pad "P2" smd circle (at -20.800111 -11.199901) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1296 "SNN_FBF_CMD<32>"))
    (pad "P3" smd circle (at -20.000011 -11.199901) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1300 "SNN_FBF_CMD<31>"))
    (pad "P4" smd circle (at -19.200114 -11.199901) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 87 "FBF_DQS_RN5"))
    (pad "P5" smd circle (at -18.399989 -11.199901) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 88 "FBF_DQS_WP5"))
    (pad "P6" smd circle (at -17.599889 -11.199901) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 69 "FBF_D<48>"))
    (pad "P7" smd circle (at -16.800093 -11.199901) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 268 "FBF_D<13>"))
    (pad "P8" smd circle (at -15.999993 -11.199901) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 267 "FBF_D<12>"))
    (pad "P9" smd circle (at -15.200097 -11.199901) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1308 "SNN_FBF_DBI1"))
    (pad "P10" smd circle (at -14.399997 -11.199901) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 269 "FBF_D<10>"))
    (pad "P11" smd circle (at -13.599897 -11.199901) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 270 "FBF_D<9>"))
    (pad "P13" smd circle (at -12.000001 -11.199901) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1306 "FBF_DEBUG"))
    (pad "P43" smd circle (at 12.000001 -11.199901) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1247 "FBC_DEBUG"))
    (pad "P45" smd circle (at 13.599897 -11.199901) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 656 "FBC_D<24>"))
    (pad "P46" smd circle (at 14.399997 -11.199901) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 655 "FBC_D<25>"))
    (pad "P47" smd circle (at 15.200097 -11.199901) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 658 "FBC_D<26>"))
    (pad "P48" smd circle (at 15.999993 -11.199901) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 657 "FBC_D<28>"))
    (pad "P49" smd circle (at 16.800093 -11.199901) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 663 "FBC_DQM3"))
    (pad "P50" smd circle (at 17.599889 -11.199901) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 627 "FBC_D<20>"))
    (pad "P51" smd circle (at 18.399989 -11.199901) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 626 "FBC_D<21>"))
    (pad "P52" smd circle (at 19.200089 -11.199901) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 628 "FBC_D<22>"))
    (pad "P53" smd circle (at 20.000011 -11.199901) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 551 "FBC_CMD<16>"))
    (pad "P54" smd circle (at 20.800111 -11.199901) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 555 "FBC_CMD<17>"))
    (pad "P55" smd circle (at 21.599906 -11.199901) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 542 "FBC_CMD<18>"))
    (pad "R1" smd circle (at -21.599906 -10.400005) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 98 "FBG_CMD<2>"))
    (pad "R2" smd circle (at -20.800111 -10.400005) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "R3" smd circle (at -20.000011 -10.400005) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 99 "FBG_CMD<1>"))
    (pad "R4" smd circle (at -19.200114 -10.400005) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 81 "FBF_D<44>"))
    (pad "R5" smd circle (at -18.399989 -10.400005) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "R6" smd circle (at -17.599889 -10.400005) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 71 "FBF_D<49>"))
    (pad "R7" smd circle (at -16.800093 -10.400005) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 73 "FBF_D<51>"))
    (pad "R8" smd circle (at -15.999993 -10.400005) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "R9" smd circle (at -15.200097 -10.400005) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "FBF1_CLK0"))
    (pad "R10" smd circle (at -14.399997 -10.400005) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "FBF1_CLK0*"))
    (pad "R11" smd circle (at -13.599897 -10.400005) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "R13" smd circle (at -12.000001 -10.400005) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "R15" smd circle (at -10.500106 -10.500106) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "R16" smd circle (at -9.500108 -10.500106) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "R17" smd circle (at -8.50011 -10.500106) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "R18" smd circle (at -7.500112 -10.500106) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "R19" smd circle (at -6.500089 -10.500106) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "R20" smd circle (at -5.500091 -10.500106) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "R21" smd circle (at -4.500093 -10.500106) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "R22" smd circle (at -3.500095 -10.500106) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "R23" smd circle (at -2.500097 -10.500106) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "R24" smd circle (at -1.500099 -10.500106) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "R25" smd circle (at -0.500101 -10.500106) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "R26" smd circle (at 0.500101 -10.500106) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "R27" smd circle (at 1.500099 -10.500106) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "R28" smd circle (at 2.500097 -10.500106) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "R29" smd circle (at 3.500095 -10.500106) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "R30" smd circle (at 4.500093 -10.500106) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "R31" smd circle (at 5.500091 -10.500106) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "R32" smd circle (at 6.500089 -10.500106) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "R33" smd circle (at 7.500112 -10.500106) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "R34" smd circle (at 8.50011 -10.500106) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "R35" smd circle (at 9.500108 -10.500106) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "R36" smd circle (at 10.500106 -10.500106) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "R43" smd circle (at 12.000001 -10.400005) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "R45" smd circle (at 13.599897 -10.400005) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "R46" smd circle (at 14.399997 -10.400005) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 650 "FBC_D<15>"))
    (pad "R47" smd circle (at 15.200097 -10.400005) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 653 "FBC_DQS_RN1"))
    (pad "R48" smd circle (at 15.999993 -10.400005) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "R49" smd circle (at 16.800093 -10.400005) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1246 "SNN_FBC_DBI3"))
    (pad "R50" smd circle (at 17.599889 -10.400005) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 629 "FBC_D<19>"))
    (pad "R51" smd circle (at 18.399989 -10.400005) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "R52" smd circle (at 19.200089 -10.400005) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 625 "FBC_D<23>"))
    (pad "R53" smd circle (at 20.000011 -10.400005) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 549 "FBC_CMD<15>"))
    (pad "R54" smd circle (at 20.800111 -10.400005) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "R55" smd circle (at 21.599906 -10.400005) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 550 "FBC_CMD<14>"))
    (pad "T3" smd circle (at -20.000011 -9.599905) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 80 "FBF_D<46>"))
    (pad "T4" smd circle (at -19.200114 -9.599905) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 78 "FBF_D<45>"))
    (pad "T5" smd circle (at -18.399989 -9.599905) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 86 "FBF_DQM5"))
    (pad "T8" smd circle (at -15.999993 -9.599905) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 72 "FBF_D<52>"))
    (pad "T9" smd circle (at -15.200097 -9.599905) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 75 "FBF_DQM6"))
    (pad "T11" smd circle (at -13.599897 -9.599905) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 67 "FBF_D<54>"))
    (pad "T13" smd circle (at -12.000001 -9.599905) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "T15" smd circle (at -10.500106 -9.500108) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T16" smd circle (at -9.500108 -9.500108) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T17" smd circle (at -8.50011 -9.500108) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T18" smd circle (at -7.500112 -9.500108) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T19" smd circle (at -6.500089 -9.500108) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T20" smd circle (at -5.500091 -9.500108) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T21" smd circle (at -4.500093 -9.500108) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T22" smd circle (at -3.500095 -9.500108) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T23" smd circle (at -2.500097 -9.500108) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T24" smd circle (at -1.500099 -9.500108) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T25" smd circle (at -0.500101 -9.500108) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T26" smd circle (at 0.500101 -9.500108) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T27" smd circle (at 1.500099 -9.500108) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T28" smd circle (at 2.500097 -9.500108) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T29" smd circle (at 3.500095 -9.500108) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T30" smd circle (at 4.500093 -9.500108) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T31" smd circle (at 5.500091 -9.500108) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T32" smd circle (at 6.500089 -9.500108) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T33" smd circle (at 7.500112 -9.500108) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T34" smd circle (at 8.50011 -9.500108) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T35" smd circle (at 9.500108 -9.500108) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T36" smd circle (at 10.500106 -9.500108) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T43" smd circle (at 12.000001 -9.599905) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "T45" smd circle (at 13.599897 -9.599905) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 649 "FBC_D<14>"))
    (pad "T47" smd circle (at 15.200097 -9.599905) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 648 "FBC_D<11>"))
    (pad "T48" smd circle (at 15.999993 -9.599905) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 654 "FBC_DQS_WP1"))
    (pad "T51" smd circle (at 18.399989 -9.599905) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 630 "FBC_DQM2"))
    (pad "T52" smd circle (at 19.200089 -9.599905) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 631 "FBC_DQS_RN2"))
    (pad "T53" smd circle (at 20.000011 -9.599905) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 632 "FBC_DQS_WP2"))
    (pad "U1" smd circle (at -21.599906 -8.800109) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 94 "FBG_CMD<5>"))
    (pad "U2" smd circle (at -20.800111 -8.800109) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 95 "FBG_CMD<4>"))
    (pad "U3" smd circle (at -20.000011 -8.800109) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 96 "FBG_CMD<3>"))
    (pad "U4" smd circle (at -19.200114 -8.800109) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 79 "FBF_D<47>"))
    (pad "U5" smd circle (at -18.399989 -8.800109) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1307 "SNN_FBF_DBI5"))
    (pad "U6" smd circle (at -17.599889 -8.800109) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 74 "FBF_D<50>"))
    (pad "U7" smd circle (at -16.800093 -8.800109) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 76 "FBF_DQS_RN6"))
    (pad "U8" smd circle (at -15.999993 -8.800109) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 77 "FBF_DQS_WP6"))
    (pad "U9" smd circle (at -15.200097 -8.800109) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1305 "SNN_FBF_DBI6"))
    (pad "U10" smd circle (at -14.399997 -8.800109) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "FBF_D<53>"))
    (pad "U11" smd circle (at -13.599897 -8.800109) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 68 "FBF_D<55>"))
    (pad "U13" smd circle (at -12.000001 -8.800109) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "U15" smd circle (at -10.500106 -8.50011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "U16" smd circle (at -9.500108 -8.50011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "U17" smd circle (at -8.50011 -8.50011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "U18" smd circle (at -7.500112 -8.50011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "U19" smd circle (at -6.500089 -8.50011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "U20" smd circle (at -5.500091 -8.50011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "U21" smd circle (at -4.500093 -8.50011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "U22" smd circle (at -3.500095 -8.50011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "U23" smd circle (at -2.500097 -8.50011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "U24" smd circle (at -1.500099 -8.50011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "U25" smd circle (at -0.500101 -8.50011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "U26" smd circle (at 0.500101 -8.50011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "U27" smd circle (at 1.500099 -8.50011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "U28" smd circle (at 2.500097 -8.50011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "U29" smd circle (at 3.500095 -8.50011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "U30" smd circle (at 4.500093 -8.50011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "U31" smd circle (at 5.500091 -8.50011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "U32" smd circle (at 6.500089 -8.50011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "U33" smd circle (at 7.500112 -8.50011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "U34" smd circle (at 8.50011 -8.50011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "U35" smd circle (at 9.500108 -8.50011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "U36" smd circle (at 10.500106 -8.50011) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "U43" smd circle (at 12.000001 -8.800109) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "U45" smd circle (at 13.599897 -8.800109) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 651 "FBC_D<13>"))
    (pad "U46" smd circle (at 14.399997 -8.800109) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 644 "FBC_D<12>"))
    (pad "U47" smd circle (at 15.200097 -8.800109) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 646 "FBC_D<10>"))
    (pad "U48" smd circle (at 15.999993 -8.800109) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 647 "FBC_D<9>"))
    (pad "U49" smd circle (at 16.800093 -8.800109) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 652 "FBC_DQM1"))
    (pad "U50" smd circle (at 17.599889 -8.800109) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 622 "FBC_D<18>"))
    (pad "U51" smd circle (at 18.399989 -8.800109) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 623 "FBC_D<17>"))
    (pad "U52" smd circle (at 19.200089 -8.800109) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 624 "FBC_D<16>"))
    (pad "U53" smd circle (at 20.000011 -8.800109) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 559 "FBC_CMD<13>"))
    (pad "U54" smd circle (at 20.800111 -8.800109) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 544 "FBC_CMD<12>"))
    (pad "U55" smd circle (at 21.599906 -8.800109) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 548 "FBC_CMD<11>"))
    (pad "V1" smd circle (at -21.599906 -8.000009) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 116 "FBG_CMD<7>"))
    (pad "V2" smd circle (at -20.800111 -8.000009) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "V3" smd circle (at -20.000011 -8.000009) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 105 "FBG_CMD<6>"))
    (pad "V4" smd circle (at -19.200114 -8.000009) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 51 "FBF_D<57>"))
    (pad "V5" smd circle (at -18.399989 -8.000009) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "V6" smd circle (at -17.599889 -8.000009) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 50 "FBF_D<58>"))
    (pad "V7" smd circle (at -16.800093 -8.000009) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 139 "FBG_DQS_WP0"))
    (pad "V8" smd circle (at -15.999993 -8.000009) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "V9" smd circle (at -15.200097 -8.000009) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 107 "FBG0_CLK0*"))
    (pad "V10" smd circle (at -14.399997 -8.000009) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 106 "FBG0_CLK0"))
    (pad "V11" smd circle (at -13.599897 -8.000009) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "V13" smd circle (at -12.000001 -8.000009) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "V15" smd circle (at -10.500106 -7.500087) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "V16" smd circle (at -9.500108 -7.500087) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "V17" smd circle (at -8.50011 -7.500087) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "V18" smd circle (at -7.500112 -7.500087) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "V19" smd circle (at -6.500089 -7.500087) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "V20" smd circle (at -5.500091 -7.500087) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "V21" smd circle (at -4.500093 -7.500087) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "V22" smd circle (at -3.500095 -7.500087) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "V23" smd circle (at -2.500097 -7.500087) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "V24" smd circle (at -1.500099 -7.500087) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "V25" smd circle (at -0.500101 -7.500087) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "V26" smd circle (at 0.500101 -7.500087) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "V27" smd circle (at 1.500099 -7.500087) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "V28" smd circle (at 2.500097 -7.500087) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "V29" smd circle (at 3.500095 -7.500087) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "V30" smd circle (at 4.500093 -7.500087) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "V31" smd circle (at 5.500091 -7.500087) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "V32" smd circle (at 6.500089 -7.500087) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "V33" smd circle (at 7.500112 -7.500087) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "V34" smd circle (at 8.50011 -7.500087) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "V35" smd circle (at 9.500108 -7.500087) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "V36" smd circle (at 10.500106 -7.500087) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "V43" smd circle (at 12.000001 -8.000009) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "V45" smd circle (at 13.599897 -8.000009) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "V46" smd circle (at 14.399997 -8.000009) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 696 "FBB_D<63>"))
    (pad "V47" smd circle (at 15.200097 -8.000009) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1248 "SNN_FBC_DBI1"))
    (pad "V48" smd circle (at 15.999993 -8.000009) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "V49" smd circle (at 16.800093 -8.000009) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 645 "FBC_D<8>"))
    (pad "V50" smd circle (at 17.599889 -8.000009) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1249 "SNN_FBC_DBI2"))
    (pad "V51" smd circle (at 18.399989 -8.000009) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "V52" smd circle (at 19.200089 -8.000009) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1240 "SNN_FBC_DBI0"))
    (pad "V53" smd circle (at 20.000011 -8.000009) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 557 "FBC_CMD<10>"))
    (pad "V54" smd circle (at 20.800111 -8.000009) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "V55" smd circle (at 21.599906 -8.000009) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 536 "FBC_CMD<9>"))
    (pad "W3" smd circle (at -20.000011 -7.199909) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 49 "FBF_D<56>"))
    (pad "W4" smd circle (at -19.200114 -7.199909) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 55 "FBF_DQS_WP7"))
    (pad "W5" smd circle (at -18.399989 -7.199909) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1328 "SNN_FBF_DBI7"))
    (pad "W8" smd circle (at -15.999993 -7.199909) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 138 "FBG_DQS_RN0"))
    (pad "W9" smd circle (at -15.200097 -7.199909) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 129 "FBG_D<1>"))
    (pad "W11" smd circle (at -13.599897 -7.199909) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1290 "SNN_FBF0_CLK1"))
    (pad "W13" smd circle (at -12.000001 -7.199909) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "W15" smd circle (at -10.500106 -6.500089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "W16" smd circle (at -9.500108 -6.500089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "W17" smd circle (at -8.50011 -6.500089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "W18" smd circle (at -7.500112 -6.500089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "W19" smd circle (at -6.500089 -6.500089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "W20" smd circle (at -5.500091 -6.500089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "W21" smd circle (at -4.500093 -6.500089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "W22" smd circle (at -3.500095 -6.500089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "W23" smd circle (at -2.500097 -6.500089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "W24" smd circle (at -1.500099 -6.500089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "W25" smd circle (at -0.500101 -6.500089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "W26" smd circle (at 0.500101 -6.500089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "W27" smd circle (at 1.500099 -6.500089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "W28" smd circle (at 2.500097 -6.500089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "W29" smd circle (at 3.500095 -6.500089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "W30" smd circle (at 4.500093 -6.500089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "W31" smd circle (at 5.500091 -6.500089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "W32" smd circle (at 6.500089 -6.500089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "W33" smd circle (at 7.500112 -6.500089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "W34" smd circle (at 8.50011 -6.500089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "W35" smd circle (at 9.500108 -6.500089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "W36" smd circle (at 10.500106 -6.500089) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "W43" smd circle (at 12.000001 -7.199909) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "W45" smd circle (at 13.599897 -7.199909) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1232 "SNN_FBC1_CLK1*"))
    (pad "W47" smd circle (at 15.200097 -7.199909) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1223 "SNN_FBB_DBI7"))
    (pad "W48" smd circle (at 15.999993 -7.199909) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 697 "FBB_D<61>"))
    (pad "W51" smd circle (at 18.399989 -7.199909) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 641 "FBC_DQM0"))
    (pad "W52" smd circle (at 19.200089 -7.199909) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 640 "FBC_D<2>"))
    (pad "W53" smd circle (at 20.000011 -7.199909) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 637 "FBC_D<1>"))
    (pad "Y1" smd circle (at -21.599906 -6.399987) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 110 "FBG_CMD<10>"))
    (pad "Y2" smd circle (at -20.800111 -6.399987) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 91 "FBG_CMD<9>"))
    (pad "Y3" smd circle (at -20.000011 -6.399987) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 103 "FBG_CMD<8>"))
    (pad "Y4" smd circle (at -19.200114 -6.399987) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 54 "FBF_DQS_RN7"))
    (pad "Y5" smd circle (at -18.399989 -6.399987) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 52 "FBF_D<62>"))
    (pad "Y6" smd circle (at -17.599889 -6.399987) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 53 "FBF_DQM7"))
    (pad "Y7" smd circle (at -16.800093 -6.399987) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 47 "FBF_D<59>"))
    (pad "Y8" smd circle (at -15.999993 -6.399987) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 131 "FBG_D<0>"))
    (pad "Y9" smd circle (at -15.200097 -6.399987) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 132 "FBG_D<2>"))
    (pad "Y10" smd circle (at -14.399997 -6.399987) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 130 "FBG_D<3>"))
    (pad "Y11" smd circle (at -13.599897 -6.399987) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1293 "SNN_FBF0_CLK1*"))
    (pad "Y13" smd circle (at -12.000001 -6.399987) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "Y15" smd circle (at -10.500106 -5.500091) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "Y16" smd circle (at -9.500108 -5.500091) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "Y17" smd circle (at -8.50011 -5.500091) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "Y18" smd circle (at -7.500112 -5.500091) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "Y19" smd circle (at -6.500089 -5.500091) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "Y20" smd circle (at -5.500091 -5.500091) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "Y21" smd circle (at -4.500093 -5.500091) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "Y22" smd circle (at -3.500095 -5.500091) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "Y23" smd circle (at -2.500097 -5.500091) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "Y24" smd circle (at -1.500099 -5.500091) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "Y25" smd circle (at -0.500101 -5.500091) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "Y26" smd circle (at 0.500101 -5.500091) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "Y27" smd circle (at 1.500099 -5.500091) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "Y28" smd circle (at 2.500097 -5.500091) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "Y29" smd circle (at 3.500095 -5.500091) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "Y30" smd circle (at 4.500093 -5.500091) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "Y31" smd circle (at 5.500091 -5.500091) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "Y32" smd circle (at 6.500089 -5.500091) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "Y33" smd circle (at 7.500112 -5.500091) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "Y34" smd circle (at 8.50011 -5.500091) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "Y35" smd circle (at 9.500108 -5.500091) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "Y36" smd circle (at 10.500106 -5.500091) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "Y43" smd circle (at 12.000001 -6.399987) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "Y45" smd circle (at 13.599897 -6.399987) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1231 "SNN_FBC1_CLK1"))
    (pad "Y46" smd circle (at 14.399997 -6.399987) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 695 "FBB_D<62>"))
    (pad "Y47" smd circle (at 15.200097 -6.399987) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 703 "FBB_DQM7"))
    (pad "Y48" smd circle (at 15.999993 -6.399987) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 698 "FBB_D<60>"))
    (pad "Y49" smd circle (at 16.800093 -6.399987) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 642 "FBC_DQS_RN0"))
    (pad "Y50" smd circle (at 17.599889 -6.399987) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 643 "FBC_DQS_WP0"))
    (pad "Y51" smd circle (at 18.399989 -6.399987) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 639 "FBC_D<5>"))
    (pad "Y52" smd circle (at 19.200089 -6.399987) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 638 "FBC_D<3>"))
    (pad "Y53" smd circle (at 20.000011 -6.399987) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 556 "FBC_CMD<8>"))
    (pad "Y54" smd circle (at 20.800111 -6.399987) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 552 "FBC_CMD<7>"))
    (pad "Y55" smd circle (at 21.599906 -6.399987) (size 0.4318 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 563 "FBC_CMD<6>"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 223.251387 142.748907 -90)
    (fp_text reference "C125" (at 0 1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 983 "12V_PEX6_F2"))
    (pad "2" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 250.340208 124.295807)
    (fp_text reference "R82" (at -0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1985 "PS5_NVVDD_EN_12V_F"))
    (pad "2" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 45.806708 106.528507 -90)
    (fp_text reference "C32" (at 0 0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1059 "XTAL_IN"))
    (pad "2" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 75.376118 122.632615 -90)
    (fp_text reference "C55" (at 0 0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 86.980108 66.676212 90)
    (fp_text reference "C58" (at 0 -0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "DFET_SMD_DPAK_1" (layer "F.Cu")
    (tedit 0)
    (at 29.957108 83.186415)
    (fp_text reference "Q3" (at 1.27 1.557477 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -2.290089 5.31241) (size 1.6002 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 990 "PS3_FBVDDQ_LG_G"))
    (pad "2" smd rect (at 0 -1.867408) (size 5.799811 6.200089) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 989 "PS3_FBVDDQ_PHASE"))
    (pad "3" smd rect (at 2.290089 5.31241) (size 1.6002 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "GEOM0005_1" (layer "F.Cu")
    (tedit 0)
    (at 167.879108 124.473607 -90)
    (fp_text reference "M13" (at 1.27 -1.5875 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "A1" smd circle (at -4.400601 -6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "A2" smd circle (at -3.600399 -6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "A3" smd circle (at -2.800299 -6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "A4" smd circle (at -2.000301 -6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 824 "FBA_ZQ2"))
    (pad "A9" smd circle (at 2.000301 -6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "A10" smd circle (at 2.800299 -6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "A11" smd circle (at 3.600399 -6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "A12" smd circle (at 4.400601 -6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "B1" smd circle (at -4.400601 -5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B2" smd circle (at -3.600399 -5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 825 "FBA_D<48>"))
    (pad "B3" smd circle (at -2.800299 -5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 826 "FBA_D<50>"))
    (pad "B4" smd circle (at -2.000301 -5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B9" smd circle (at 2.000301 -5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B10" smd circle (at 2.800299 -5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 837 "FBA_D<44>"))
    (pad "B11" smd circle (at 3.600399 -5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 836 "FBA_D<46>"))
    (pad "B12" smd circle (at 4.400601 -5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "C1" smd circle (at -4.400601 -4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "C2" smd circle (at -3.600399 -4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 827 "FBA_D<53>"))
    (pad "C3" smd circle (at -2.800299 -4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 828 "FBA_D<52>"))
    (pad "C4" smd circle (at -2.000301 -4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "C9" smd circle (at 2.000301 -4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "C10" smd circle (at 2.800299 -4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 839 "FBA_D<47>"))
    (pad "C11" smd circle (at 3.600399 -4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 838 "FBA_D<45>"))
    (pad "C12" smd circle (at 4.400601 -4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "D1" smd circle (at -4.400601 -4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "D2" smd circle (at -3.600399 -4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 835 "FBA_DQS_WP6"))
    (pad "D3" smd circle (at -2.800299 -4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 834 "FBA_DQS_RN6"))
    (pad "D4" smd circle (at -2.000301 -4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "D9" smd circle (at 2.000301 -4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "D10" smd circle (at 2.800299 -4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 845 "FBA_DQS_RN5"))
    (pad "D11" smd circle (at 3.600399 -4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 846 "FBA_DQS_WP5"))
    (pad "D12" smd circle (at 4.400601 -4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "E1" smd circle (at -4.400601 -3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "E2" smd circle (at -3.600399 -3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 829 "FBA_D<49>"))
    (pad "E3" smd circle (at -2.800299 -3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 833 "FBA_DQM6"))
    (pad "E4" smd circle (at -2.000301 -3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "E9" smd circle (at 2.000301 -3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "E10" smd circle (at 2.800299 -3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 844 "FBA_DQM5"))
    (pad "E11" smd circle (at 3.600399 -3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 840 "FBA_D<42>"))
    (pad "E12" smd circle (at 4.400601 -3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "F1" smd circle (at -4.400601 -2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "F2" smd circle (at -3.600399 -2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 831 "FBA_D<51>"))
    (pad "F3" smd circle (at -2.800299 -2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 830 "FBA_D<55>"))
    (pad "F4" smd circle (at -2.000301 -2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 811 "FBA_CMD<16>"))
    (pad "F9" smd circle (at 2.000301 -2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 815 "FBA_CMD<17>"))
    (pad "F10" smd circle (at 2.800299 -2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 841 "FBA_D<41>"))
    (pad "F11" smd circle (at 3.600399 -2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 842 "FBA_D<43>"))
    (pad "F12" smd circle (at 4.400601 -2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "G1" smd circle (at -4.400601 -1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "G2" smd circle (at -3.600399 -1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "G3" smd circle (at -2.800299 -1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 832 "FBA_D<54>"))
    (pad "G4" smd circle (at -2.000301 -1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 808 "FBA_CMD<11>"))
    (pad "G9" smd circle (at 2.000301 -1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 809 "FBA_CMD<15>"))
    (pad "G10" smd circle (at 2.800299 -1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 843 "FBA_D<40>"))
    (pad "G11" smd circle (at 3.600399 -1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "G12" smd circle (at 4.400601 -1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "H1" smd circle (at -4.400601 -0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 821 "FBA_VREF3"))
    (pad "H2" smd circle (at -3.600399 -0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 799 "FBA_CMD<28>"))
    (pad "H3" smd circle (at -2.800299 -0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 817 "FBA_CMD<8>"))
    (pad "H4" smd circle (at -2.000301 -0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 812 "FBA_CMD<7>"))
    (pad "H9" smd circle (at 2.000301 -0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 823 "FBA_CMD<6>"))
    (pad "H10" smd circle (at 2.800299 -0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 810 "FBA_CMD<14>"))
    (pad "H11" smd circle (at 3.600399 -0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 803 "FBA_CMD<12>"))
    (pad "H12" smd circle (at 4.400601 -0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 822 "FBA_VREF4"))
    (pad "J1" smd circle (at -4.400601 0 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "J2" smd circle (at -3.600399 0 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 819 "SNN_FBA_NC04"))
    (pad "J3" smd circle (at -2.800299 0 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 816 "FBA_CMD<13>"))
    (pad "J4" smd circle (at -2.000301 0 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "J9" smd circle (at 2.000301 0 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "J10" smd circle (at 2.800299 0 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 814 "FBA1_CLK0*"))
    (pad "J11" smd circle (at 3.600399 0 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 813 "FBA1_CLK0"))
    (pad "J12" smd circle (at 4.400601 0 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "K1" smd circle (at -4.400601 0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "K2" smd circle (at -3.600399 0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 797 "FBA_CMD<19>"))
    (pad "K3" smd circle (at -2.800299 0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 800 "FBA_CMD<26>"))
    (pad "K4" smd circle (at -2.000301 0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 796 "FBA_CMD<25>"))
    (pad "K9" smd circle (at 2.000301 0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 802 "FBA_CMD<21>"))
    (pad "K10" smd circle (at 2.800299 0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 804 "FBA_CMD<23>"))
    (pad "K11" smd circle (at 3.600399 0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 806 "FBA_CMD<9>"))
    (pad "K12" smd circle (at 4.400601 0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "L1" smd circle (at -4.400601 1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "L2" smd circle (at -3.600399 1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "L3" smd circle (at -2.800299 1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 859 "FBA_D<62>"))
    (pad "L4" smd circle (at -2.000301 1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 798 "FBA_CMD<27>"))
    (pad "L9" smd circle (at 2.000301 1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 805 "FBA_CMD<20>"))
    (pad "L10" smd circle (at 2.800299 1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 848 "FBA_D<32>"))
    (pad "L11" smd circle (at 3.600399 1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "L12" smd circle (at 4.400601 1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "M1" smd circle (at -4.400601 2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "M2" smd circle (at -3.600399 2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 858 "FBA_D<63>"))
    (pad "M3" smd circle (at -2.800299 2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 861 "FBA_D<60>"))
    (pad "M4" smd circle (at -2.000301 2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 801 "FBA_CMD<18>"))
    (pad "M9" smd circle (at 2.000301 2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 807 "FBA_CMD<24>"))
    (pad "M10" smd circle (at 2.800299 2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 850 "FBA_D<33>"))
    (pad "M11" smd circle (at 3.600399 2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 847 "FBA_D<35>"))
    (pad "M12" smd circle (at 4.400601 2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N1" smd circle (at -4.400601 3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N2" smd circle (at -3.600399 3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 860 "FBA_D<61>"))
    (pad "N3" smd circle (at -2.800299 3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 866 "FBA_DQM7"))
    (pad "N4" smd circle (at -2.000301 3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N9" smd circle (at 2.000301 3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N10" smd circle (at 2.800299 3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 855 "FBA_DQM4"))
    (pad "N11" smd circle (at 3.600399 3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 849 "FBA_D<34>"))
    (pad "N12" smd circle (at 4.400601 3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "P1" smd circle (at -4.400601 4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "P2" smd circle (at -3.600399 4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 868 "FBA_DQS_WP7"))
    (pad "P3" smd circle (at -2.800299 4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 867 "FBA_DQS_RN7"))
    (pad "P4" smd circle (at -2.000301 4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "P9" smd circle (at 2.000301 4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "P10" smd circle (at 2.800299 4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 856 "FBA_DQS_RN4"))
    (pad "P11" smd circle (at 3.600399 4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 857 "FBA_DQS_WP4"))
    (pad "P12" smd circle (at 4.400601 4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "R1" smd circle (at -4.400601 4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "R2" smd circle (at -3.600399 4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 862 "FBA_D<56>"))
    (pad "R3" smd circle (at -2.800299 4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 863 "FBA_D<59>"))
    (pad "R4" smd circle (at -2.000301 4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "R9" smd circle (at 2.000301 4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "R10" smd circle (at 2.800299 4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 852 "FBA_D<39>"))
    (pad "R11" smd circle (at 3.600399 4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 851 "FBA_D<38>"))
    (pad "R12" smd circle (at 4.400601 4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "T1" smd circle (at -4.400601 5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T2" smd circle (at -3.600399 5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 864 "FBA_D<57>"))
    (pad "T3" smd circle (at -2.800299 5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 865 "FBA_D<58>"))
    (pad "T4" smd circle (at -2.000301 5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T9" smd circle (at 2.000301 5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T10" smd circle (at 2.800299 5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 854 "FBA_D<37>"))
    (pad "T11" smd circle (at 3.600399 5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 853 "FBA_D<36>"))
    (pad "T12" smd circle (at 4.400601 5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "V1" smd circle (at -4.400601 6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "V2" smd circle (at -3.600399 6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "V3" smd circle (at -2.800299 6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "V4" smd circle (at -2.000301 6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 820 "FBA_SEN2"))
    (pad "V9" smd circle (at 2.000301 6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 818 "FBA_CMD<10>"))
    (pad "V10" smd circle (at 2.800299 6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "V11" smd circle (at 3.600399 6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "V12" smd circle (at 4.400601 6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
  )
  (footprint "GEOM0014_1" (layer "F.Cu")
    (tedit 0)
    (at 48.180109 55.3772)
    (fp_text reference "CN3" (at -0.952525 4.73235 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -11.454409 3.618713) (size 2.140991 4.4958) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "2" smd rect (at -11.454409 3.618713) (size 2.140991 4.4958) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "3" smd rect (at 11.454409 3.618713) (size 2.140991 4.4958) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "4" smd rect (at 11.454409 3.618713) (size 2.140991 4.4958) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "A1" smd rect (at 5.999988 5.249393 180) (size 0.699999 4.4958) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1095 "GPIO11_RASTERSYNC1_R"))
    (pad "A2" smd rect (at 4.99999 5.249393 180) (size 0.699999 4.4958) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1081 "DRA_D0"))
    (pad "A3" smd rect (at 3.999992 5.249393 180) (size 0.699999 4.4958) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "A4" smd rect (at 2.999994 5.249393 180) (size 0.699999 4.4958) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1085 "DRA_D2"))
    (pad "A5" smd rect (at 1.999996 5.249393 180) (size 0.699999 4.4958) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1086 "DRA_D3"))
    (pad "A6" smd rect (at 0.999998 5.249393 180) (size 0.699999 4.4958) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1088 "DRA_D5"))
    (pad "A7" smd rect (at 0 5.249393 180) (size 0.699999 4.4958) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "A8" smd rect (at -0.999998 5.249393 180) (size 0.699999 4.4958) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1089 "DRA_D6"))
    (pad "A9" smd rect (at -1.999996 5.249393 180) (size 0.699999 4.4958) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1097 "DRA_D14"))
    (pad "A10" smd rect (at -2.999994 5.249393 180) (size 0.699999 4.4958) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1092 "DRA_D9"))
    (pad "A11" smd rect (at -3.999992 5.249393 180) (size 0.699999 4.4958) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "A12" smd rect (at -4.99999 5.249393 180) (size 0.699999 4.4958) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1083 "DRA_D11"))
    (pad "A13" smd rect (at -5.999988 5.249393 180) (size 0.699999 4.4958) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1098 "DRA_D12"))
    (pad "B1" smd rect (at 5.999988 5.249393 180) (size 0.699999 4.4958) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1079 "GPIO15_SWAPRDY"))
    (pad "B2" smd rect (at 4.99999 5.249393 180) (size 0.699999 4.4958) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1094 "NVIO_EXT_REFCLKA_R"))
    (pad "B3" smd rect (at 3.999992 5.249393 180) (size 0.699999 4.4958) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B4" smd rect (at 2.999994 5.249393 180) (size 0.699999 4.4958) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1084 "DRA_D1"))
    (pad "B5" smd rect (at 1.999996 5.249393 180) (size 0.699999 4.4958) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1096 "DRA_D13"))
    (pad "B6" smd rect (at 0.999998 5.249393 180) (size 0.699999 4.4958) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1087 "DRA_D4"))
    (pad "B7" smd rect (at 0 5.249393 180) (size 0.699999 4.4958) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B8" smd rect (at -0.999998 5.249393 180) (size 0.699999 4.4958) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1080 "DRA_CLK"))
    (pad "B9" smd rect (at -1.999996 5.249393 180) (size 0.699999 4.4958) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1090 "DRA_D7"))
    (pad "B10" smd rect (at -2.999994 5.249393 180) (size 0.699999 4.4958) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1091 "DRA_D8"))
    (pad "B11" smd rect (at -3.999992 5.249393 180) (size 0.699999 4.4958) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B12" smd rect (at -4.99999 5.249393 180) (size 0.699999 4.4958) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1082 "DRA_D10"))
    (pad "B13" smd rect (at -5.999988 5.249393 180) (size 0.699999 4.4958) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1093 "DRA_CMD"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 73.568908 138.558212 180)
    (fp_text reference "C47" (at 0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 249.286108 119.126907 180)
    (fp_text reference "R81" (at 0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1994 "THERM_SHDN_D*"))
    (pad "2" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 930 "PS5_NVVDD_EN"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 10.119708 132.208415 90)
    (fp_text reference "R3" (at 0 -0.635 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2000 "I2C2_SCL_R"))
    (pad "2" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1914 "5V"))
  )
  (footprint "GEOM0022_1" (layer "F.Cu")
    (tedit 0)
    (at 249.463908 131.509407)
    (fp_text reference "MEC20" (at -1.5875 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 3.5814 3.5814) (drill 3.175) (layers *.Cu *.Mask)
      (net 1 "GND"))
  )
  (footprint "1206_1" (layer "F.Cu")
    (tedit 0)
    (at 200.518108 93.282407 -90)
    (fp_text reference "R58" (at 0 0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -1.4732 0 270) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1105 "PS5_NVVDD_RC2"))
    (pad "2" smd rect (at 1.4732 0 270) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 203.947108 60.821207 90)
    (fp_text reference "R64" (at 0 -0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1991 "SPDIF_IN_C"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 38.085108 123.292812)
    (fp_text reference "R21" (at -0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1935 "HYBRID_HPD_E"))
    (pad "2" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1009 "3V3"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 4.430108 125.349907 90)
    (fp_text reference "C5" (at 0 -0.635 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1923 "DACA_HSYNC_CON"))
    (pad "2" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "1206_1" (layer "F.Cu")
    (tedit 0)
    (at 227.696413 92.660615 -90)
    (fp_text reference "C131" (at 0 1.0795 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -1.4732 0 270) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 981 "12V_PEX6_F1"))
    (pad "2" smd rect (at 1.4732 0 270) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 75.376118 115.622215 -90)
    (fp_text reference "C54" (at 0 0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 4.684108 110.669215)
    (fp_text reference "R1" (at -0.635 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1796 "GPIO1_DVICD_HPD"))
    (pad "2" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1986 "GPIO1_DVICD_HPD_R"))
  )
  (footprint "SOT23_1" (layer "F.Cu")
    (tedit 0)
    (at 5.496908 130.049415 -90)
    (fp_text reference "D3" (at 0.635 -1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.9525 1.143 270) (size 0.9144 0.9144) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "2" smd rect (at 0.9525 1.143 270) (size 0.9144 0.9144) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1914 "5V"))
    (pad "3" smd rect (at 0 -1.143 270) (size 0.9144 0.9144) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2009 "DACA_HSYNC_BUF"))
  )
  (footprint "GEOM0026_1" (layer "F.Cu")
    (tedit 0)
    (at 211.363908 58.583518)
    (fp_text reference "J4" (at 0.365023 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1956 "SPDIF_IN"))
    (pad "2" thru_hole circle (at 2.000021 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 2080 "SPDIF_GND"))
  )
  (footprint "1206_1" (layer "F.Cu")
    (tedit 0)
    (at 227.696413 118.314615 -90)
    (fp_text reference "C133" (at 0 1.0795 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -1.4732 0 270) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 983 "12V_PEX6_F2"))
    (pad "2" smd rect (at 1.4732 0 270) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 76.362908 138.558212 180)
    (fp_text reference "R37" (at 0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1974 "THERM_PWM_ADDR_EN*"))
    (pad "2" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1009 "3V3"))
  )
  (footprint "1206_1" (layer "F.Cu")
    (tedit 0)
    (at 48.854708 134.747907 90)
    (fp_text reference "C34" (at 0 -0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -1.4732 0 90) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 991 "12V_F"))
    (pad "2" smd rect (at 1.4732 0 90) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "IND_SMD_0402_1" (layer "F.Cu")
    (tedit 0)
    (at 5.039708 137.796415 90)
    (fp_text reference "LB2" (at 0 -0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 270) (size 0.6858 0.5334) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1999 "I2C2_SDA_R"))
    (pad "2" smd rect (at 0.5334 0 90) (size 0.6858 0.5334) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1929 "I2C2_SDA_CON"))
  )
  (footprint "GEOM0022_1" (layer "F.Cu")
    (tedit 0)
    (at 183.373108 141.580812)
    (fp_text reference "MEC18" (at -1.5875 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 3.5814 3.5814) (drill 3.175) (layers *.Cu *.Mask)
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 12.126308 115.698415)
    (fp_text reference "R7" (at -0.635 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1765 "MIOA_VREF"))
  )
  (footprint "EMIPAD_025X041_1" (layer "F.Cu")
    (tedit 0)
    (at 249.857608 88.519907 180)
    (fp_text reference "MEC21" (at -1.085622 -1.240714 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 0 180) (size 2.499792 3.000197) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 16.037908 123.115012 180)
    (fp_text reference "R10" (at 0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1696 "I2C2_SCL"))
    (pad "2" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2000 "I2C2_SCL_R"))
  )
  (footprint "1206_1" (layer "F.Cu")
    (tedit 0)
    (at 48.422908 146.025507)
    (fp_text reference "R30" (at -0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -1.4732 0) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1000 "12V"))
    (pad "2" smd rect (at 1.4732 0) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 991 "12V_F"))
  )
  (footprint "SOT23_1" (layer "F.Cu")
    (tedit 0)
    (at 7.605108 133.884815 90)
    (fp_text reference "D5" (at -0.635 1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.9525 1.143 90) (size 0.9144 0.9144) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "2" smd rect (at 0.9525 1.143 90) (size 0.9144 0.9144) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1914 "5V"))
    (pad "3" smd rect (at 0 -1.143 90) (size 0.9144 0.9144) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2000 "I2C2_SCL_R"))
  )
  (footprint "SOT23_1" (layer "F.Cu")
    (tedit 0)
    (at 8.189308 145.314815 90)
    (fp_text reference "D7" (at -0.635 1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.9525 1.143 90) (size 0.9144 0.9144) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "2" smd rect (at 0.9525 1.143 90) (size 0.9144 0.9144) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1914 "5V"))
    (pad "3" smd rect (at 0 -1.143 90) (size 0.9144 0.9144) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2007 "DACC_HSYNC_BUF"))
  )
  (footprint "EMIPAD_025X041_1" (layer "F.Cu")
    (tedit 0)
    (at 79.664908 63.881907)
    (fp_text reference "MEC8" (at 1.175106 1.157199 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 0) (size 2.499792 3.000197) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "1206_1" (layer "F.Cu")
    (tedit 0)
    (at 225.156413 105.487615 -90)
    (fp_text reference "C127" (at 0 1.0795 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -1.4732 0 270) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 981 "12V_PEX6_F1"))
    (pad "2" smd rect (at 1.4732 0 270) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "1206_1" (layer "F.Cu")
    (tedit 0)
    (at 225.156413 118.314615 -90)
    (fp_text reference "C128" (at 0 1.0795 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -1.4732 0 270) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 983 "12V_PEX6_F2"))
    (pad "2" smd rect (at 1.4732 0 270) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "GEOM0005_1" (layer "F.Cu")
    (tedit 0)
    (at 167.879108 139.396615 -90)
    (fp_text reference "M14" (at 1.27 -1.5875 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "A1" smd circle (at -4.400601 -6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "A2" smd circle (at -3.600399 -6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "A3" smd circle (at -2.800299 -6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "A4" smd circle (at -2.000301 -6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 881 "FBA_ZQ1"))
    (pad "A9" smd circle (at 2.000301 -6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "A10" smd circle (at 2.800299 -6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "A11" smd circle (at 3.600399 -6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "A12" smd circle (at 4.400601 -6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "B1" smd circle (at -4.400601 -5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B2" smd circle (at -3.600399 -5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 882 "FBA_D<28>"))
    (pad "B3" smd circle (at -2.800299 -5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 883 "FBA_D<30>"))
    (pad "B4" smd circle (at -2.000301 -5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B9" smd circle (at 2.000301 -5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B10" smd circle (at 2.800299 -5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 894 "FBA_D<12>"))
    (pad "B11" smd circle (at 3.600399 -5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 893 "FBA_D<13>"))
    (pad "B12" smd circle (at 4.400601 -5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "C1" smd circle (at -4.400601 -4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "C2" smd circle (at -3.600399 -4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 884 "FBA_D<27>"))
    (pad "C3" smd circle (at -2.800299 -4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 885 "FBA_D<31>"))
    (pad "C4" smd circle (at -2.000301 -4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "C9" smd circle (at 2.000301 -4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "C10" smd circle (at 2.800299 -4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 896 "FBA_D<8>"))
    (pad "C11" smd circle (at 3.600399 -4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 895 "FBA_D<9>"))
    (pad "C12" smd circle (at 4.400601 -4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "D1" smd circle (at -4.400601 -4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "D2" smd circle (at -3.600399 -4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 892 "FBA_DQS_WP3"))
    (pad "D3" smd circle (at -2.800299 -4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 891 "FBA_DQS_RN3"))
    (pad "D4" smd circle (at -2.000301 -4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "D9" smd circle (at 2.000301 -4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "D10" smd circle (at 2.800299 -4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 902 "FBA_DQS_RN1"))
    (pad "D11" smd circle (at 3.600399 -4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 903 "FBA_DQS_WP1"))
    (pad "D12" smd circle (at 4.400601 -4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "E1" smd circle (at -4.400601 -3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "E2" smd circle (at -3.600399 -3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 886 "FBA_D<25>"))
    (pad "E3" smd circle (at -2.800299 -3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 890 "FBA_DQM3"))
    (pad "E4" smd circle (at -2.000301 -3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "E9" smd circle (at 2.000301 -3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "E10" smd circle (at 2.800299 -3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 901 "FBA_DQM1"))
    (pad "E11" smd circle (at 3.600399 -3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 897 "FBA_D<14>"))
    (pad "E12" smd circle (at 4.400601 -3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "F1" smd circle (at -4.400601 -2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "F2" smd circle (at -3.600399 -2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 888 "FBA_D<29>"))
    (pad "F3" smd circle (at -2.800299 -2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 887 "FBA_D<26>"))
    (pad "F4" smd circle (at -2.000301 -2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 815 "FBA_CMD<17>"))
    (pad "F9" smd circle (at 2.000301 -2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 811 "FBA_CMD<16>"))
    (pad "F10" smd circle (at 2.800299 -2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 898 "FBA_D<11>"))
    (pad "F11" smd circle (at 3.600399 -2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 899 "FBA_D<15>"))
    (pad "F12" smd circle (at 4.400601 -2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "G1" smd circle (at -4.400601 -1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "G2" smd circle (at -3.600399 -1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "G3" smd circle (at -2.800299 -1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 889 "FBA_D<24>"))
    (pad "G4" smd circle (at -2.000301 -1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 809 "FBA_CMD<15>"))
    (pad "G9" smd circle (at 2.000301 -1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 808 "FBA_CMD<11>"))
    (pad "G10" smd circle (at 2.800299 -1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 900 "FBA_D<10>"))
    (pad "G11" smd circle (at 3.600399 -1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "G12" smd circle (at 4.400601 -1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "H1" smd circle (at -4.400601 -0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 879 "FBA_VREF1"))
    (pad "H2" smd circle (at -3.600399 -0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 803 "FBA_CMD<12>"))
    (pad "H3" smd circle (at -2.800299 -0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 810 "FBA_CMD<14>"))
    (pad "H4" smd circle (at -2.000301 -0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 823 "FBA_CMD<6>"))
    (pad "H9" smd circle (at 2.000301 -0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 812 "FBA_CMD<7>"))
    (pad "H10" smd circle (at 2.800299 -0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 817 "FBA_CMD<8>"))
    (pad "H11" smd circle (at 3.600399 -0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 872 "FBA_CMD<0>"))
    (pad "H12" smd circle (at 4.400601 -0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 880 "FBA_VREF2"))
    (pad "J1" smd circle (at -4.400601 0 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "J2" smd circle (at -3.600399 0 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 877 "SNN_FBA_NC01"))
    (pad "J3" smd circle (at -2.800299 0 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 816 "FBA_CMD<13>"))
    (pad "J4" smd circle (at -2.000301 0 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "J9" smd circle (at 2.000301 0 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "J10" smd circle (at 2.800299 0 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 876 "FBA0_CLK0*"))
    (pad "J11" smd circle (at 3.600399 0 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 875 "FBA0_CLK0"))
    (pad "J12" smd circle (at 4.400601 0 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "K1" smd circle (at -4.400601 0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "K2" smd circle (at -3.600399 0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 806 "FBA_CMD<9>"))
    (pad "K3" smd circle (at -2.800299 0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 869 "FBA_CMD<5>"))
    (pad "K4" smd circle (at -2.000301 0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 802 "FBA_CMD<21>"))
    (pad "K9" smd circle (at 2.000301 0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 871 "FBA_CMD<3>"))
    (pad "K10" smd circle (at 2.800299 0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 873 "FBA_CMD<2>"))
    (pad "K11" smd circle (at 3.600399 0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 797 "FBA_CMD<19>"))
    (pad "K12" smd circle (at 4.400601 0.8001 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "L1" smd circle (at -4.400601 1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "L2" smd circle (at -3.600399 1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "L3" smd circle (at -2.800299 1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 916 "FBA_D<16>"))
    (pad "L4" smd circle (at -2.000301 1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 805 "FBA_CMD<20>"))
    (pad "L9" smd circle (at 2.000301 1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 874 "FBA_CMD<1>"))
    (pad "L10" smd circle (at 2.800299 1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 905 "FBA_D<1>"))
    (pad "L11" smd circle (at 3.600399 1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "L12" smd circle (at 4.400601 1.6002 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "M1" smd circle (at -4.400601 2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "M2" smd circle (at -3.600399 2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 915 "FBA_D<17>"))
    (pad "M3" smd circle (at -2.800299 2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 918 "FBA_D<18>"))
    (pad "M4" smd circle (at -2.000301 2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 870 "FBA_CMD<4>"))
    (pad "M9" smd circle (at 2.000301 2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 801 "FBA_CMD<18>"))
    (pad "M10" smd circle (at 2.800299 2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 907 "FBA_D<2>"))
    (pad "M11" smd circle (at 3.600399 2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 904 "FBA_D<0>"))
    (pad "M12" smd circle (at 4.400601 2.4003 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N1" smd circle (at -4.400601 3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N2" smd circle (at -3.600399 3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 917 "FBA_D<19>"))
    (pad "N3" smd circle (at -2.800299 3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 923 "FBA_DQM2"))
    (pad "N4" smd circle (at -2.000301 3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N9" smd circle (at 2.000301 3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N10" smd circle (at 2.800299 3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 912 "FBA_DQM0"))
    (pad "N11" smd circle (at 3.600399 3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 906 "FBA_D<3>"))
    (pad "N12" smd circle (at 4.400601 3.2004 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "P1" smd circle (at -4.400601 4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "P2" smd circle (at -3.600399 4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 925 "FBA_DQS_WP2"))
    (pad "P3" smd circle (at -2.800299 4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 924 "FBA_DQS_RN2"))
    (pad "P4" smd circle (at -2.000301 4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "P9" smd circle (at 2.000301 4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "P10" smd circle (at 2.800299 4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 913 "FBA_DQS_RN0"))
    (pad "P11" smd circle (at 3.600399 4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 914 "FBA_DQS_WP0"))
    (pad "P12" smd circle (at 4.400601 4.0005 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "R1" smd circle (at -4.400601 4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "R2" smd circle (at -3.600399 4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 919 "FBA_D<23>"))
    (pad "R3" smd circle (at -2.800299 4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 920 "FBA_D<22>"))
    (pad "R4" smd circle (at -2.000301 4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "R9" smd circle (at 2.000301 4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "R10" smd circle (at 2.800299 4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 909 "FBA_D<7>"))
    (pad "R11" smd circle (at 3.600399 4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 908 "FBA_D<4>"))
    (pad "R12" smd circle (at 4.400601 4.8006 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "T1" smd circle (at -4.400601 5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T2" smd circle (at -3.600399 5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 921 "FBA_D<21>"))
    (pad "T3" smd circle (at -2.800299 5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 922 "FBA_D<20>"))
    (pad "T4" smd circle (at -2.000301 5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T9" smd circle (at 2.000301 5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T10" smd circle (at 2.800299 5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 911 "FBA_D<6>"))
    (pad "T11" smd circle (at 3.600399 5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 910 "FBA_D<5>"))
    (pad "T12" smd circle (at 4.400601 5.6007 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "V1" smd circle (at -4.400601 6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "V2" smd circle (at -3.600399 6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "V3" smd circle (at -2.800299 6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "V4" smd circle (at -2.000301 6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 878 "FBA_SEN1"))
    (pad "V9" smd circle (at 2.000301 6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 818 "FBA_CMD<10>"))
    (pad "V10" smd circle (at 2.800299 6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "V11" smd circle (at 3.600399 6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "V12" smd circle (at 4.400601 6.4008 270) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
  )
  (footprint "0805_1" (layer "F.Cu")
    (tedit 0)
    (at 181.722108 136.729107 180)
    (fp_text reference "C104" (at 0.7874 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.9525 0 180) (size 1.143 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at 0.9525 0 180) (size 1.143 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0603_1" (layer "F.Cu")
    (tedit 0)
    (at 200.708608 114.999407 -90)
    (fp_text reference "C112" (at 0 1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.762 0 90) (size 0.889 0.7874) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "PS5_NVVDD_PHASE5"))
    (pad "2" smd rect (at 0.762 0 270) (size 0.889 0.7874) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1102 "PS5_NVVDD_RC5"))
  )
  (footprint "1206_1" (layer "F.Cu")
    (tedit 0)
    (at 42.606308 83.516107 -90)
    (fp_text reference "R26" (at 0 0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -1.4732 0 270) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1104 "PS3_FBVDDQ_RC"))
    (pad "2" smd rect (at 1.4732 0 270) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 250.340208 125.311807)
    (fp_text reference "C147" (at -1.27 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1985 "PS5_NVVDD_EN_12V_F"))
    (pad "2" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "1206_1" (layer "F.Cu")
    (tedit 0)
    (at 219.479208 61.049807 90)
    (fp_text reference "C118" (at 0 -1.0795 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -1.4732 0 90) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "INPUT_PEX6_IN1"))
    (pad "2" smd rect (at 1.4732 0 90) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 75.550413 74.880894 90)
    (fp_text reference "R36" (at 0 -0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "2" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 228 "FBF_SEN1"))
  )
  (footprint "GEOM0008_1" (layer "F.Cu")
    (tedit 0)
    (at 205.598413 101.042615)
    (fp_text reference "Q8" (at 1.27 1.582877 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -2.290115 5.31241) (size 1.6002 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 998 "PS5_NVVDD_LG6_AC"))
    (pad "2" smd rect (at 0 -1.867408) (size 5.799811 6.200089) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "PS5_NVVDD_PHASE6"))
    (pad "3" smd rect (at 2.290089 5.31241) (size 1.6002 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 115.402708 68.936812 90)
    (fp_text reference "C63" (at 0 -0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "CAP_SMD_7343_1" (layer "F.Cu")
    (tedit 0)
    (at 51.166108 74.245412)
    (fp_text reference "C36" (at -0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -3.1115 0) (size 2.413 3.048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at 3.1115 0) (size 2.413 3.048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "EMIPAD_025X041_1" (layer "F.Cu")
    (tedit 0)
    (at 151.902508 143.129907 180)
    (fp_text reference "MEC14" (at -1.085622 -1.240714 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 0 180) (size 2.499792 3.000197) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "MEC_SCREW_PH1_1" (layer "F.Cu")
    (tedit 0)
    (at -68.721892 23.953615)
    (fp_text reference "MEC1" (at -1.27 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 4.658708 98.274015)
    (fp_text reference "C6" (at -0.635 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1925 "DDC_5V"))
    (pad "2" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "1206_1" (layer "F.Cu")
    (tedit 0)
    (at 40.912103 144.679612 180)
    (fp_text reference "C27" (at 0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -1.4732 0 180) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1000 "12V"))
    (pad "2" smd rect (at 1.4732 0 180) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 242.174108 118.237907 -90)
    (fp_text reference "R75" (at 0 0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 983 "12V_PEX6_F2"))
    (pad "2" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1984 "PS5_NVVDD_EN_12V_F2"))
  )
  (footprint "0603_1" (layer "F.Cu")
    (tedit 0)
    (at 200.708608 102.045407 -90)
    (fp_text reference "C111" (at 0 1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.762 0 90) (size 0.889 0.7874) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "PS5_NVVDD_PHASE6"))
    (pad "2" smd rect (at 0.762 0 270) (size 0.889 0.7874) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1103 "PS5_NVVDD_RC6"))
  )
  (footprint "0603_1" (layer "F.Cu")
    (tedit 0)
    (at 190.281908 107.214307)
    (fp_text reference "R50" (at -0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.762 0 180) (size 0.889 0.7874) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 927 "NET0001"))
    (pad "2" smd rect (at 0.762 0) (size 0.889 0.7874) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1041 "NET0007"))
  )
  (footprint "1206_1" (layer "F.Cu")
    (tedit 0)
    (at 219.949108 67.818907)
    (fp_text reference "C119" (at -1.0795 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -1.4732 0) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 981 "12V_PEX6_F1"))
    (pad "2" smd rect (at 1.4732 0) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "1206_1" (layer "F.Cu")
    (tedit 0)
    (at 23.657908 86.208507)
    (fp_text reference "C19" (at -0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -1.4732 0) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 991 "12V_F"))
    (pad "2" smd rect (at 1.4732 0) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0603_1" (layer "F.Cu")
    (tedit 0)
    (at 200.708608 76.391407 -90)
    (fp_text reference "C109" (at 0 1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.762 0 90) (size 0.889 0.7874) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "PS5_NVVDD_PHASE1"))
    (pad "2" smd rect (at 0.762 0 270) (size 0.889 0.7874) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1099 "PS5_NVVDD_RC1"))
  )
  (footprint "DFET_SMD_DPAK_1" (layer "F.Cu")
    (tedit 0)
    (at 37.577108 83.186415)
    (fp_text reference "Q5" (at 1.27 1.557477 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -2.290089 5.31241) (size 1.6002 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 990 "PS3_FBVDDQ_LG_G"))
    (pad "2" smd rect (at 0 -1.867408) (size 5.799811 6.200089) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 989 "PS3_FBVDDQ_PHASE"))
    (pad "3" smd rect (at 2.290089 5.31241) (size 1.6002 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 161.226315 117.781012 180)
    (fp_text reference "C83" (at 0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 12.126308 112.675612 180)
    (fp_text reference "R5" (at 0.635 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "2" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1750 "MIOA_CTL3"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 73.594613 95.099015)
    (fp_text reference "C48" (at -0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 159.573308 122.492102 -90)
    (fp_text reference "R49" (at 0 0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "2" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 820 "FBA_SEN2"))
  )
  (footprint "1206_1" (layer "F.Cu")
    (tedit 0)
    (at 200.518108 80.455407 -90)
    (fp_text reference "R57" (at 0 0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -1.4732 0 270) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1099 "PS5_NVVDD_RC1"))
    (pad "2" smd rect (at 1.4732 0 270) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 24.115108 125.324812)
    (fp_text reference "R18" (at -0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1937 "HYBRID_PRG_TP"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 164.145308 58.065612)
    (fp_text reference "C91" (at -0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 10.119708 137.110615 -90)
    (fp_text reference "R4" (at 0 0.635 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1914 "5V"))
    (pad "2" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1999 "I2C2_SDA_R"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 38.085108 124.562812)
    (fp_text reference "R22" (at -0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1936 "HYBRID_HPD_F"))
    (pad "2" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1009 "3V3"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 115.402708 66.676212 90)
    (fp_text reference "C62" (at 0 -0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "GEOM0004_1" (layer "F.Cu")
    (tedit 0)
    (at 193.533108 126.619907 90)
    (fp_text reference "L12" (at -1.27 1.5875 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 3.81 90) (size 4.0132 4.318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "PS5_NVVDD_PHASE4"))
    (pad "2" smd rect (at 0 -3.81 90) (size 4.0132 4.318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
  )
  (footprint "GEOM0005_1" (layer "F.Cu")
    (tedit 0)
    (at 67.071613 73.428014 90)
    (fp_text reference "M1" (at -0.635 1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "A1" smd circle (at -4.400601 -6.4008 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "A2" smd circle (at -3.600399 -6.4008 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "A3" smd circle (at -2.800299 -6.4008 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "A4" smd circle (at -2.000301 -6.4008 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 231 "FBF_ZQ1"))
    (pad "A9" smd circle (at 2.000301 -6.4008 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "A10" smd circle (at 2.800299 -6.4008 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "A11" smd circle (at 3.600399 -6.4008 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "A12" smd circle (at 4.400601 -6.4008 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "B1" smd circle (at -4.400601 -5.6007 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B2" smd circle (at -3.600399 -5.6007 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 232 "FBF_D<24>"))
    (pad "B3" smd circle (at -2.800299 -5.6007 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 233 "FBF_D<27>"))
    (pad "B4" smd circle (at -2.000301 -5.6007 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B9" smd circle (at 2.000301 -5.6007 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B10" smd circle (at 2.800299 -5.6007 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 244 "FBF_D<2>"))
    (pad "B11" smd circle (at 3.600399 -5.6007 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 243 "FBF_D<0>"))
    (pad "B12" smd circle (at 4.400601 -5.6007 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "C1" smd circle (at -4.400601 -4.8006 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "C2" smd circle (at -3.600399 -4.8006 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 234 "FBF_D<26>"))
    (pad "C3" smd circle (at -2.800299 -4.8006 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 235 "FBF_D<25>"))
    (pad "C4" smd circle (at -2.000301 -4.8006 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "C9" smd circle (at 2.000301 -4.8006 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "C10" smd circle (at 2.800299 -4.8006 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 246 "FBF_D<1>"))
    (pad "C11" smd circle (at 3.600399 -4.8006 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 245 "FBF_D<3>"))
    (pad "C12" smd circle (at 4.400601 -4.8006 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "D1" smd circle (at -4.400601 -4.0005 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "D2" smd circle (at -3.600399 -4.0005 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 242 "FBF_DQS_WP3"))
    (pad "D3" smd circle (at -2.800299 -4.0005 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 241 "FBF_DQS_RN3"))
    (pad "D4" smd circle (at -2.000301 -4.0005 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "D9" smd circle (at 2.000301 -4.0005 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "D10" smd circle (at 2.800299 -4.0005 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 252 "FBF_DQS_RN0"))
    (pad "D11" smd circle (at 3.600399 -4.0005 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 253 "FBF_DQS_WP0"))
    (pad "D12" smd circle (at 4.400601 -4.0005 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "E1" smd circle (at -4.400601 -3.2004 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "E2" smd circle (at -3.600399 -3.2004 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 236 "FBF_D<31>"))
    (pad "E3" smd circle (at -2.800299 -3.2004 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 240 "FBF_DQM3"))
    (pad "E4" smd circle (at -2.000301 -3.2004 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "E9" smd circle (at 2.000301 -3.2004 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "E10" smd circle (at 2.800299 -3.2004 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 251 "FBF_DQM0"))
    (pad "E11" smd circle (at 3.600399 -3.2004 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 247 "FBF_D<5>"))
    (pad "E12" smd circle (at 4.400601 -3.2004 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "F1" smd circle (at -4.400601 -2.4003 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "F2" smd circle (at -3.600399 -2.4003 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 238 "FBF_D<30>"))
    (pad "F3" smd circle (at -2.800299 -2.4003 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 237 "FBF_D<29>"))
    (pad "F4" smd circle (at -2.000301 -2.4003 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "FBF_CMD<17>"))
    (pad "F9" smd circle (at 2.000301 -2.4003 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "FBF_CMD<16>"))
    (pad "F10" smd circle (at 2.800299 -2.4003 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 248 "FBF_D<4>"))
    (pad "F11" smd circle (at 3.600399 -2.4003 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 249 "FBF_D<6>"))
    (pad "F12" smd circle (at 4.400601 -2.4003 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "G1" smd circle (at -4.400601 -1.6002 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "G2" smd circle (at -3.600399 -1.6002 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "G3" smd circle (at -2.800299 -1.6002 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 239 "FBF_D<28>"))
    (pad "G4" smd circle (at -2.000301 -1.6002 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "FBF_CMD<15>"))
    (pad "G9" smd circle (at 2.000301 -1.6002 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "FBF_CMD<11>"))
    (pad "G10" smd circle (at 2.800299 -1.6002 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 250 "FBF_D<7>"))
    (pad "G11" smd circle (at 3.600399 -1.6002 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "G12" smd circle (at 4.400601 -1.6002 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "H1" smd circle (at -4.400601 -0.8001 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 229 "FBF_VREF1"))
    (pad "H2" smd circle (at -3.600399 -0.8001 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "FBF_CMD<12>"))
    (pad "H3" smd circle (at -2.800299 -0.8001 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "FBF_CMD<14>"))
    (pad "H4" smd circle (at -2.000301 -0.8001 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "FBF_CMD<6>"))
    (pad "H9" smd circle (at 2.000301 -0.8001 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "FBF_CMD<7>"))
    (pad "H10" smd circle (at 2.800299 -0.8001 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "FBF_CMD<8>"))
    (pad "H11" smd circle (at 3.600399 -0.8001 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 222 "FBF_CMD<0>"))
    (pad "H12" smd circle (at 4.400601 -0.8001 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 230 "FBF_VREF2"))
    (pad "J1" smd circle (at -4.400601 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "J2" smd circle (at -3.600399 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 227 "SNN_FBF_NC01"))
    (pad "J3" smd circle (at -2.800299 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "FBF_CMD<13>"))
    (pad "J4" smd circle (at -2.000301 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "J9" smd circle (at 2.000301 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "J10" smd circle (at 2.800299 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 226 "FBF0_CLK0*"))
    (pad "J11" smd circle (at 3.600399 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 225 "FBF0_CLK0"))
    (pad "J12" smd circle (at 4.400601 0 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "K1" smd circle (at -4.400601 0.8001 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "K2" smd circle (at -3.600399 0.8001 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "FBF_CMD<9>"))
    (pad "K3" smd circle (at -2.800299 0.8001 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 219 "FBF_CMD<5>"))
    (pad "K4" smd circle (at -2.000301 0.8001 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "FBF_CMD<21>"))
    (pad "K9" smd circle (at 2.000301 0.8001 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 221 "FBF_CMD<3>"))
    (pad "K10" smd circle (at 2.800299 0.8001 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 223 "FBF_CMD<2>"))
    (pad "K11" smd circle (at 3.600399 0.8001 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "FBF_CMD<19>"))
    (pad "K12" smd circle (at 4.400601 0.8001 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "L1" smd circle (at -4.400601 1.6002 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "L2" smd circle (at -3.600399 1.6002 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "L3" smd circle (at -2.800299 1.6002 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 266 "FBF_D<15>"))
    (pad "L4" smd circle (at -2.000301 1.6002 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "FBF_CMD<20>"))
    (pad "L9" smd circle (at 2.000301 1.6002 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 224 "FBF_CMD<1>"))
    (pad "L10" smd circle (at 2.800299 1.6002 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 255 "FBF_D<20>"))
    (pad "L11" smd circle (at 3.600399 1.6002 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "L12" smd circle (at 4.400601 1.6002 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "M1" smd circle (at -4.400601 2.4003 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "M2" smd circle (at -3.600399 2.4003 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 265 "FBF_D<14>"))
    (pad "M3" smd circle (at -2.800299 2.4003 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 268 "FBF_D<13>"))
    (pad "M4" smd circle (at -2.000301 2.4003 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 220 "FBF_CMD<4>"))
    (pad "M9" smd circle (at 2.000301 2.4003 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "FBF_CMD<18>"))
    (pad "M10" smd circle (at 2.800299 2.4003 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 257 "FBF_D<16>"))
    (pad "M11" smd circle (at 3.600399 2.4003 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 254 "FBF_D<18>"))
    (pad "M12" smd circle (at 4.400601 2.4003 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N1" smd circle (at -4.400601 3.2004 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N2" smd circle (at -3.600399 3.2004 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 267 "FBF_D<12>"))
    (pad "N3" smd circle (at -2.800299 3.2004 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 273 "FBF_DQM1"))
    (pad "N4" smd circle (at -2.000301 3.2004 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N9" smd circle (at 2.000301 3.2004 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "N10" smd circle (at 2.800299 3.2004 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 262 "FBF_DQM2"))
    (pad "N11" smd circle (at 3.600399 3.2004 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 256 "FBF_D<17>"))
    (pad "N12" smd circle (at 4.400601 3.2004 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "P1" smd circle (at -4.400601 4.0005 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "P2" smd circle (at -3.600399 4.0005 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 275 "FBF_DQS_WP1"))
    (pad "P3" smd circle (at -2.800299 4.0005 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 274 "FBF_DQS_RN1"))
    (pad "P4" smd circle (at -2.000301 4.0005 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "P9" smd circle (at 2.000301 4.0005 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "P10" smd circle (at 2.800299 4.0005 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 263 "FBF_DQS_RN2"))
    (pad "P11" smd circle (at 3.600399 4.0005 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 264 "FBF_DQS_WP2"))
    (pad "P12" smd circle (at 4.400601 4.0005 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "R1" smd circle (at -4.400601 4.8006 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "R2" smd circle (at -3.600399 4.8006 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 269 "FBF_D<10>"))
    (pad "R3" smd circle (at -2.800299 4.8006 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 270 "FBF_D<9>"))
    (pad "R4" smd circle (at -2.000301 4.8006 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "R9" smd circle (at 2.000301 4.8006 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "R10" smd circle (at 2.800299 4.8006 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 259 "FBF_D<21>"))
    (pad "R11" smd circle (at 3.600399 4.8006 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 258 "FBF_D<19>"))
    (pad "R12" smd circle (at 4.400601 4.8006 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "T1" smd circle (at -4.400601 5.6007 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T2" smd circle (at -3.600399 5.6007 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 271 "FBF_D<11>"))
    (pad "T3" smd circle (at -2.800299 5.6007 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 272 "FBF_D<8>"))
    (pad "T4" smd circle (at -2.000301 5.6007 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T9" smd circle (at 2.000301 5.6007 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T10" smd circle (at 2.800299 5.6007 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 261 "FBF_D<22>"))
    (pad "T11" smd circle (at 3.600399 5.6007 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 260 "FBF_D<23>"))
    (pad "T12" smd circle (at 4.400601 5.6007 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "V1" smd circle (at -4.400601 6.4008 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "V2" smd circle (at -3.600399 6.4008 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "V3" smd circle (at -2.800299 6.4008 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "V4" smd circle (at -2.000301 6.4008 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 228 "FBF_SEN1"))
    (pad "V9" smd circle (at 2.000301 6.4008 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "FBF_CMD<10>"))
    (pad "V10" smd circle (at 2.800299 6.4008 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "V11" smd circle (at 3.600399 6.4008 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "V12" smd circle (at 4.400601 6.4008 90) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
  )
  (footprint "GEOM0010_1" (layer "F.Cu")
    (tedit 0)
    (at 48.245108 141.986907 -90)
    (fp_text reference "L7" (at 0.635 -1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 2.500097 90) (size 7.500188 3.000197) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1000 "12V"))
    (pad "2" smd rect (at 0 -2.500097 270) (size 7.500188 3.000197) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 991 "12V_F"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 21.854508 122.073612 180)
    (fp_text reference "R14" (at 0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1811 "I2C3_SDA"))
    (pad "2" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 977 "I2C3_SDA_R"))
  )
  (footprint "0603_1" (layer "F.Cu")
    (tedit 0)
    (at 131.557108 145.898812)
    (fp_text reference "C68" (at -0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.762 0 180) (size 0.889 0.7874) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at 0.762 0) (size 0.889 0.7874) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 73.041096 66.682511)
    (fp_text reference "C46" (at -0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 244.396608 114.491407 90)
    (fp_text reference "R78" (at 0 -0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 930 "PS5_NVVDD_EN"))
    (pad "2" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 141.844108 72.086615 180)
    (fp_text reference "C69" (at 0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "1206_1" (layer "F.Cu")
    (tedit 0)
    (at 225.156413 92.660615 -90)
    (fp_text reference "C126" (at 0 1.0795 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -1.4732 0 270) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 981 "12V_PEX6_F1"))
    (pad "2" smd rect (at 1.4732 0 270) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "IND_SMD_0603_1" (layer "F.Cu")
    (tedit 0)
    (at 5.369908 141.987415 90)
    (fp_text reference "L3" (at 0 -0.635 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.762 0 270) (size 0.889 0.7874) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2013 "DACC_VSYNC_BUF"))
    (pad "2" smd rect (at 0.762 0 90) (size 0.889 0.7874) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1934 "DACC_VSYNC_CON"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 45.806708 102.464507 -90)
    (fp_text reference "C31" (at 0 0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1058 "XTAL_OUT"))
    (pad "2" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 119.048624 72.086615 180)
    (fp_text reference "C66" (at 0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 116.875908 66.676212 90)
    (fp_text reference "C64" (at 0 -0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 86.980108 68.987612 90)
    (fp_text reference "C59" (at 0 -0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 113.091308 72.086615)
    (fp_text reference "C61" (at -0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "SOT23_1" (layer "F.Cu")
    (tedit 0)
    (at 247.254108 120.777907)
    (fp_text reference "Q28" (at 1.359967 1.11125 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.9525 1.143) (size 0.9144 0.9144) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1984 "PS5_NVVDD_EN_12V_F2"))
    (pad "2" smd rect (at 0.9525 1.143) (size 0.9144 0.9144) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2081 "PS5_NVVDD_EN_Q"))
    (pad "3" smd rect (at 0 -1.143) (size 0.9144 0.9144) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1989 "PS5_NVVDD_EN*"))
  )
  (footprint "GEOM0016_1" (layer "F.Cu")
    (tedit 0)
    (at 28.018605 106.5138)
    (fp_text reference "U2" (at -0.635 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "A2" smd circle (at -9.6012 -10.4013) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1668 "DACB_Y"))
    (pad "A3" smd circle (at -8.8011 -10.4013) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1670 "DACB_PR"))
    (pad "A4" smd circle (at -8.001 -10.4013) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1671 "SNN_DACB_CSYNC"))
    (pad "A6" smd circle (at -6.4008 -10.4013) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1725 "IFPCD_IOVDD"))
    (pad "A7" smd circle (at -5.6007 -10.4013) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1672 "DACB_RSET"))
    (pad "A9" smd circle (at -4.0005 -10.4013) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1673 "DACB_VDD"))
    (pad "A10" smd circle (at -3.2004 -10.4013) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1828 "SNN_NVIO_NC_01"))
    (pad "A12" smd circle (at -1.6002 -10.4013) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1830 "SNN_NVIO_NC_02"))
    (pad "A13" smd circle (at -0.8001 -10.4013) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1835 "NVIO_EXT_REFCLKB"))
    (pad "A15" smd circle (at 0.8001 -10.4013) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1839 "SNN_DVIA_CTL1"))
    (pad "A16" smd circle (at 1.6002 -10.4013) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1848 "DVIA_D7"))
    (pad "A18" smd circle (at 3.2004 -10.4013) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1845 "SNN_DVIA_D4"))
    (pad "A19" smd circle (at 4.0005 -10.4013) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1843 "DVIA_D2"))
    (pad "A21" smd circle (at 5.6007 -10.4013) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1072 "DRB_D9"))
    (pad "A22" smd circle (at 6.4008 -10.4013) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1070 "DRB_D7"))
    (pad "A24" smd circle (at 8.001 -10.4013) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1067 "DRB_D4"))
    (pad "A25" smd circle (at 8.8011 -10.4013) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1066 "DRB_D3"))
    (pad "A26" smd circle (at 9.6012 -10.4013) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1064 "DRB_D1"))
    (pad "AA1" smd circle (at -10.4013 5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1755 "SNN_MIOA<2>"))
    (pad "AA2" smd circle (at -9.6012 5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AA3" smd circle (at -8.8011 5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1756 "SNN_MIOA<3>"))
    (pad "AA4" smd circle (at -8.001 5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1707 "IFPA_TXD1*"))
    (pad "AA5" smd circle (at -7.2009 5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1706 "IFPA_TXD1"))
    (pad "AA6" smd circle (at -6.4008 5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1701 "IFPAB_IOVDD"))
    (pad "AA22" smd circle (at 6.4008 5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1651 "GV_TX13*"))
    (pad "AA23" smd circle (at 7.2009 5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1540 "GV_TX13"))
    (pad "AA24" smd circle (at 8.001 5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1513 "GV_TXCTL*"))
    (pad "AA25" smd circle (at 8.8011 5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1512 "GV_TXCTL"))
    (pad "AA26" smd circle (at 9.6012 5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1497 "GV_TX14"))
    (pad "AA27" smd circle (at 10.4013 5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1509 "GV_TX11"))
    (pad "AB1" smd circle (at -10.4013 6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1757 "SNN_MIOA<4>"))
    (pad "AB2" smd circle (at -9.6012 6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1758 "SNN_MIOA<5>"))
    (pad "AB3" smd circle (at -8.8011 6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1748 "SNN_MIOA_CLKOUT"))
    (pad "AB4" smd circle (at -8.001 6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1709 "IFPA_TXD2*"))
    (pad "AB5" smd circle (at -7.2009 6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1710 "SNN_IFPA_TXD3"))
    (pad "AB6" smd circle (at -6.4008 6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1711 "SNN_IFPA_TXD3*"))
    (pad "AB7" smd circle (at -5.6007 6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1699 "IFPAB_RSET"))
    (pad "AB8" smd circle (at -4.8006 6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1863 "SNN_NVIO_NC_04"))
    (pad "AB9" smd circle (at -4.0005 6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1864 "SNN_NVIO_NC_05"))
    (pad "AB10" smd circle (at -3.2004 6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AB11" smd circle (at -2.4003 6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1700 "SNN_IFPAB_VPROBE"))
    (pad "AB12" smd circle (at -1.6002 6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1692 "DACC_RSET"))
    (pad "AB13" smd circle (at -0.8001 6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1814 "NVIO_TESTMODE"))
    (pad "AB14" smd circle (at 0 6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1798 "GPIO11_RASTERSYNC1"))
    (pad "AB15" smd circle (at 0.8001 6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1797 "NET0012"))
    (pad "AB16" smd circle (at 1.6002 6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1808 "GPIO8_FAN_TACH"))
    (pad "AB17" smd circle (at 2.4003 6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1806 "GPIO6_PS5_NVVDD_VID2"))
    (pad "AB18" smd circle (at 3.2004 6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1079 "GPIO15_SWAPRDY"))
    (pad "AB19" smd circle (at 4.0005 6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1114 "GPU_HOT_RESET*"))
    (pad "AB20" smd circle (at 4.8006 6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1861 "SNN_GPIO16_DP_INT*"))
    (pad "AB21" smd circle (at 5.6007 6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1862 "SNN_NVIO_NC_03"))
    (pad "AB22" smd circle (at 6.4008 6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1528 "GV_TXCLK"))
    (pad "AB23" smd circle (at 7.2009 6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1529 "GV_TXCLK*"))
    (pad "AB24" smd circle (at 8.001 6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1506 "GV_TX12"))
    (pad "AB25" smd circle (at 8.8011 6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1524 "GV_TX12*"))
    (pad "AB26" smd circle (at 9.6012 6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AB27" smd circle (at 10.4013 6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1510 "GV_TX11*"))
    (pad "AC2" smd circle (at -9.6012 7.2009) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1749 "SNN_MIOA_CLKOUT*"))
    (pad "AC4" smd circle (at -8.001 7.2009) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1708 "IFPA_TXD2"))
    (pad "AC5" smd circle (at -7.2009 7.2009) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AC6" smd circle (at -6.4008 7.2009) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1712 "SNN_IFPB_TXC"))
    (pad "AC7" smd circle (at -5.6007 7.2009) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1868 "SNN_NVIO_NC_09"))
    (pad "AC8" smd circle (at -4.8006 7.2009) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AC9" smd circle (at -4.0005 7.2009) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1693 "DACC_VDD"))
    (pad "AC10" smd circle (at -3.2004 7.2009) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1698 "IFPAB_PLLVDD"))
    (pad "AC11" smd circle (at -2.4003 7.2009) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AC12" smd circle (at -1.6002 7.2009) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1676 "SNN_I2C0_SCL"))
    (pad "AC13" smd circle (at -0.8001 7.2009) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1694 "DACC_VREF"))
    (pad "AC14" smd circle (at 0 7.2009) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AC15" smd circle (at 0.8001 7.2009) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1799 "NET0013"))
    (pad "AC16" smd circle (at 1.6002 7.2009) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1807 "GPIO7_PS5_NVVDD_VID3"))
    (pad "AC17" smd circle (at 2.4003 7.2009) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AC18" smd circle (at 3.2004 7.2009) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1792 "NVIO_EXTDEV_RST*"))
    (pad "AC19" smd circle (at 4.0005 7.2009) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1562 "JTAG_TMS"))
    (pad "AC20" smd circle (at 4.8006 7.2009) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AC21" smd circle (at 5.6007 7.2009) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1865 "SNN_NVIO_NC_06"))
    (pad "AC22" smd circle (at 6.4008 7.2009) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1866 "SNN_NVIO_NC_07"))
    (pad "AC23" smd circle (at 7.2009 7.2009) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AC24" smd circle (at 8.001 7.2009) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1867 "SNN_NVIO_NC_08"))
    (pad "AC26" smd circle (at 9.6012 7.2009) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1539 "GV_TX10*"))
    (pad "AD1" smd circle (at -10.4013 8.001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1759 "SNN_MIOA<6>"))
    (pad "AD2" smd circle (at -9.6012 8.001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AD3" smd circle (at -8.8011 8.001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1760 "SNN_MIOA<7>"))
    (pad "AD4" smd circle (at -8.001 8.001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1715 "IFPB_TXD4*"))
    (pad "AD5" smd circle (at -7.2009 8.001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1714 "IFPB_TXD4"))
    (pad "AD6" smd circle (at -6.4008 8.001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1713 "SNN_IFPB_TXC*"))
    (pad "AD7" smd circle (at -5.6007 8.001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1701 "IFPAB_IOVDD"))
    (pad "AD8" smd circle (at -4.8006 8.001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AD9" smd circle (at -4.0005 8.001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1695 "DACC_VSYNC"))
    (pad "AD10" smd circle (at -3.2004 8.001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1687 "I2C1_SDA"))
    (pad "AD11" smd circle (at -2.4003 8.001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1686 "I2C1_SCL"))
    (pad "AD12" smd circle (at -1.6002 8.001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1677 "SNN_I2C0_SDA"))
    (pad "AD13" smd circle (at -0.8001 8.001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1008 "ROM_CS*"))
    (pad "AD14" smd circle (at 0 8.001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1801 "GPIO14_RASTERSYNC2"))
    (pad "AD15" smd circle (at 0.8001 8.001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1800 "SNN_GPIO13_STEREO"))
    (pad "AD16" smd circle (at 1.6002 8.001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1805 "GPIO5_PS5_NVVDD_VID1"))
    (pad "AD17" smd circle (at 2.4003 8.001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1794 "FAN_PWM_NVIO"))
    (pad "AD18" smd circle (at 3.2004 8.001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1050 "GPU_RST*"))
    (pad "AD19" smd circle (at 4.0005 8.001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1559 "JTAG_TCK"))
    (pad "AD20" smd circle (at 4.8006 8.001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1530 "GV_TX3*"))
    (pad "AD21" smd circle (at 5.6007 8.001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1542 "GV_TX3"))
    (pad "AD22" smd circle (at 6.4008 8.001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1537 "GV_TX7*"))
    (pad "AD23" smd circle (at 7.2009 8.001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1536 "GV_TX7"))
    (pad "AD24" smd circle (at 8.001 8.001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1652 "GV_TX9*"))
    (pad "AD25" smd circle (at 8.8011 8.001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1505 "GV_TX9"))
    (pad "AD26" smd circle (at 9.6012 8.001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1538 "GV_TX10"))
    (pad "AD27" smd circle (at 10.4013 8.001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1869 "SNN_NVIO_NC_10"))
    (pad "AE1" smd circle (at -10.4013 8.8011) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1761 "SNN_MIOA<8>"))
    (pad "AE2" smd circle (at -9.6012 8.8011) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1762 "SNN_MIOA<9>"))
    (pad "AE3" smd circle (at -8.8011 8.8011) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1754 "SNN_MIOA<11>"))
    (pad "AE4" smd circle (at -8.001 8.8011) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1870 "SNN_MIOA<13>"))
    (pad "AE6" smd circle (at -6.4008 8.8011) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1871 "SNN_MIOA<14>"))
    (pad "AE7" smd circle (at -5.6007 8.8011) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AE9" smd circle (at -4.0005 8.8011) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1690 "DACC_HSYNC"))
    (pad "AE10" smd circle (at -3.2004 8.8011) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1811 "I2C3_SDA"))
    (pad "AE12" smd circle (at -1.6002 8.8011) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1812 "I2C4_SDA"))
    (pad "AE13" smd circle (at -0.8001 8.8011) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1012 "STRAP2"))
    (pad "AE15" smd circle (at 0.8001 8.8011) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 973 "GPIO9_THERM_ALERT*"))
    (pad "AE16" smd circle (at 1.6002 8.8011) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1803 "NET0015"))
    (pad "AE18" smd circle (at 3.2004 8.8011) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AE19" smd circle (at 4.0005 8.8011) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1912 "JTAG_TRST_3V3*"))
    (pad "AE21" smd circle (at 5.6007 8.8011) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1501 "GV_TX8"))
    (pad "AE22" smd circle (at 6.4008 8.8011) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1534 "GV_TX8*"))
    (pad "AE24" smd circle (at 8.001 8.8011) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1500 "GV_TX6"))
    (pad "AE25" smd circle (at 8.8011 8.8011) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1533 "GV_TX6*"))
    (pad "AE26" smd circle (at 9.6012 8.8011) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AE27" smd circle (at 10.4013 8.8011) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1531 "GV_TX5"))
    (pad "AF1" smd circle (at -10.4013 9.6012) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1753 "SNN_MIOA<10>"))
    (pad "AF2" smd circle (at -9.6012 9.6012) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1872 "SNN_MIOA<12>"))
    (pad "AF3" smd circle (at -8.8011 9.6012) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AF4" smd circle (at -8.001 9.6012) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1718 "IFPB_TXD6"))
    (pad "AF5" smd circle (at -7.2009 9.6012) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1721 "SNN_IFPB_TXD7*"))
    (pad "AF6" smd circle (at -6.4008 9.6012) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AF7" smd circle (at -5.6007 9.6012) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AF8" smd circle (at -4.8006 9.6012) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1691 "DACC_RED"))
    (pad "AF9" smd circle (at -4.0005 9.6012) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AF10" smd circle (at -3.2004 9.6012) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1697 "I2C2_SDA"))
    (pad "AF11" smd circle (at -2.4003 9.6012) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1809 "I2C3_SCL"))
    (pad "AF12" smd circle (at -1.6002 9.6012) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AF13" smd circle (at -0.8001 9.6012) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1011 "STRAP1"))
    (pad "AF14" smd circle (at 0 9.6012) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1010 "STRAP0"))
    (pad "AF15" smd circle (at 0.8001 9.6012) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AF16" smd circle (at 1.6002 9.6012) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1796 "GPIO1_DVICD_HPD"))
    (pad "AF17" smd circle (at 2.4003 9.6012) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1795 "GPIO0_DVIAB_HPD"))
    (pad "AF18" smd circle (at 3.2004 9.6012) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AF19" smd circle (at 4.0005 9.6012) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1911 "JTAG_TDO_NVIO"))
    (pad "AF20" smd circle (at 4.8006 9.6012) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1171 "GPU_PEX_PWR_GOOD*"))
    (pad "AF21" smd circle (at 5.6007 9.6012) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AF22" smd circle (at 6.4008 9.6012) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1527 "GV_TX2*"))
    (pad "AF23" smd circle (at 7.2009 9.6012) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1526 "GV_TX2"))
    (pad "AF24" smd circle (at 8.001 9.6012) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "AF25" smd circle (at 8.8011 9.6012) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1873 "SNN_NVIO_NC_11"))
    (pad "AF26" smd circle (at 9.6012 9.6012) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1499 "GV_TX4*"))
    (pad "AF27" smd circle (at 10.4013 9.6012) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1502 "GV_TX5*"))
    (pad "AG2" smd circle (at -9.6012 10.4013) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1717 "IFPB_TXD5*"))
    (pad "AG3" smd circle (at -8.8011 10.4013) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1716 "IFPB_TXD5"))
    (pad "AG4" smd circle (at -8.001 10.4013) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1719 "IFPB_TXD6*"))
    (pad "AG6" smd circle (at -6.4008 10.4013) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1720 "SNN_IFPB_TXD7"))
    (pad "AG7" smd circle (at -5.6007 10.4013) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1688 "DACC_BLUE"))
    (pad "AG9" smd circle (at -4.0005 10.4013) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1689 "DACC_GREEN"))
    (pad "AG10" smd circle (at -3.2004 10.4013) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1696 "I2C2_SCL"))
    (pad "AG12" smd circle (at -1.6002 10.4013) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1810 "I2C4_SCL"))
    (pad "AG13" smd circle (at -0.8001 10.4013) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1813 "SNN_STRAP3"))
    (pad "AG15" smd circle (at 0.8001 10.4013) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1804 "GPIO4_PS5_NVVDD_VID4"))
    (pad "AG16" smd circle (at 1.6002 10.4013) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1802 "NET0014"))
    (pad "AG18" smd circle (at 3.2004 10.4013) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1910 "JTAG_TDI_NVIO"))
    (pad "AG19" smd circle (at 4.0005 10.4013) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1874 "SPDIF_IN_GPU"))
    (pad "AG21" smd circle (at 5.6007 10.4013) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1546 "GV_TX0*"))
    (pad "AG22" smd circle (at 6.4008 10.4013) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1110 "GV_TX0"))
    (pad "AG24" smd circle (at 8.001 10.4013) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1547 "GV_TX1*"))
    (pad "AG25" smd circle (at 8.8011 10.4013) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1483 "GV_TX1"))
    (pad "AG26" smd circle (at 9.6012 10.4013) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1535 "GV_TX4"))
    (pad "B1" smd circle (at -10.4013 -9.6012) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1675 "SNN_DACB_VSYNC"))
    (pad "B2" smd circle (at -9.6012 -9.6012) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1669 "DACB_PB"))
    (pad "B3" smd circle (at -8.8011 -9.6012) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1786 "MIOB_VREF"))
    (pad "B4" smd circle (at -8.001 -9.6012) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B5" smd circle (at -7.2009 -9.6012) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1674 "DACB_VREF"))
    (pad "B6" smd circle (at -6.4008 -9.6012) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1727 "IFPC_TXC*"))
    (pad "B7" smd circle (at -5.6007 -9.6012) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B8" smd circle (at -4.8006 -9.6012) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B9" smd circle (at -4.0005 -9.6012) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B10" smd circle (at -3.2004 -9.6012) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B11" smd circle (at -2.4003 -9.6012) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1829 "SNN_NVIO_NC_12"))
    (pad "B12" smd circle (at -1.6002 -9.6012) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1836 "SNN_NVIO_NC_13"))
    (pad "B13" smd circle (at -0.8001 -9.6012) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B14" smd circle (at 0 -9.6012) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1834 "SNN_NVIO_NC_14"))
    (pad "B15" smd circle (at 0.8001 -9.6012) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1840 "SNN_DVIA_CTL2"))
    (pad "B16" smd circle (at 1.6002 -9.6012) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B17" smd circle (at 2.4003 -9.6012) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1847 "SNN_DVIA_D6"))
    (pad "B18" smd circle (at 3.2004 -9.6012) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1846 "SNN_DVIA_D5"))
    (pad "B19" smd circle (at 4.0005 -9.6012) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B20" smd circle (at 4.8006 -9.6012) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1842 "DVIA_D1"))
    (pad "B21" smd circle (at 5.6007 -9.6012) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1071 "DRB_D8"))
    (pad "B22" smd circle (at 6.4008 -9.6012) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B23" smd circle (at 7.2009 -9.6012) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1069 "DRB_D6"))
    (pad "B24" smd circle (at 8.001 -9.6012) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1068 "DRB_D5"))
    (pad "B25" smd circle (at 8.8011 -9.6012) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "B26" smd circle (at 9.6012 -9.6012) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1061 "DRB_D0"))
    (pad "B27" smd circle (at 10.4013 -9.6012) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1092 "DRA_D9"))
    (pad "C1" smd circle (at -10.4013 -8.8011) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1768 "SNN_MIOB_CAL_PU_GND"))
    (pad "C2" smd circle (at -9.6012 -8.8011) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "C3" smd circle (at -8.8011 -8.8011) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1667 "SNN_DACB_HSYNC"))
    (pad "C4" smd circle (at -8.001 -8.8011) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1877 "SNN_NVIO_NC_19"))
    (pad "C6" smd circle (at -6.4008 -8.8011) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1726 "IFPC_TXC"))
    (pad "C7" smd circle (at -5.6007 -8.8011) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "C9" smd circle (at -4.0005 -8.8011) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1825 "SNN_NVIO_NC_20"))
    (pad "C10" smd circle (at -3.2004 -8.8011) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1826 "SNN_NVIO_NC_15"))
    (pad "C12" smd circle (at -1.6002 -8.8011) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1827 "SNN_NVIO_NC_16"))
    (pad "C13" smd circle (at -0.8001 -8.8011) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1875 "SNN_NVIO_NC_17"))
    (pad "C15" smd circle (at 0.8001 -8.8011) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1837 "SNN_DVIA_CLK"))
    (pad "C16" smd circle (at 1.6002 -8.8011) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1838 "SNN_DVIA_CTL0"))
    (pad "C18" smd circle (at 3.2004 -8.8011) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1876 "SNN_NVIO_NC_18"))
    (pad "C19" smd circle (at 4.0005 -8.8011) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1844 "DVIA_D3"))
    (pad "C21" smd circle (at 5.6007 -8.8011) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1841 "DVIA_D0"))
    (pad "C22" smd circle (at 6.4008 -8.8011) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1073 "DRB_CMD"))
    (pad "C24" smd circle (at 8.001 -8.8011) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1078 "DRB_D12"))
    (pad "C25" smd circle (at 8.8011 -8.8011) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1065 "DRB_D2"))
    (pad "C26" smd circle (at 9.6012 -8.8011) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1091 "DRA_D8"))
    (pad "C27" smd circle (at 10.4013 -8.8011) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1090 "DRA_D7"))
    (pad "D1" smd circle (at -10.4013 -8.001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1771 "MIOB_CTL3"))
    (pad "D2" smd circle (at -9.6012 -8.001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1785 "SNN_MIOB_VSYNC"))
    (pad "D3" smd circle (at -8.8011 -8.001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1787 "SNN_MIOB_HSYNC"))
    (pad "D4" smd circle (at -8.001 -8.001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1731 "IFPC_TXD1*"))
    (pad "D5" smd circle (at -7.2009 -8.001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1728 "IFPC_TXD0"))
    (pad "D6" smd circle (at -6.4008 -8.001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1729 "IFPC_TXD0*"))
    (pad "D7" smd circle (at -5.6007 -8.001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1879 "SNN_NVIO_NC_25"))
    (pad "D8" smd circle (at -4.8006 -8.001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "D9" smd circle (at -4.0005 -8.001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1820 "SNN_NVIO_NC_26"))
    (pad "D10" smd circle (at -3.2004 -8.001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1817 "SNN_NVIO_NC_21"))
    (pad "D11" smd circle (at -2.4003 -8.001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1823 "SNN_NVIO_NC_22"))
    (pad "D12" smd circle (at -1.6002 -8.001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "D13" smd circle (at -0.8001 -8.001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1831 "SNN_NVIO_NC_23"))
    (pad "D14" smd circle (at 0 -8.001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1878 "SNN_NVIO_NC_24"))
    (pad "D15" smd circle (at 0.8001 -8.001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1856 "SNN_DVIB_D3"))
    (pad "D16" smd circle (at 1.6002 -8.001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1858 "DVIB_D5"))
    (pad "D17" smd circle (at 2.4003 -8.001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1009 "3V3"))
    (pad "D18" smd circle (at 3.2004 -8.001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1860 "SNN_DVIB_D7"))
    (pad "D19" smd circle (at 4.0005 -8.001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1849 "SNN_DVIB_CLK"))
    (pad "D20" smd circle (at 4.8006 -8.001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1009 "3V3"))
    (pad "D21" smd circle (at 5.6007 -8.001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1060 "DRB_CLK"))
    (pad "D22" smd circle (at 6.4008 -8.001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1788 "DR_CAL_PD_VDDQ"))
    (pad "D23" smd circle (at 7.2009 -8.001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1791 "DR_VREF"))
    (pad "D24" smd circle (at 8.001 -8.001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1063 "DRB_D11"))
    (pad "D25" smd circle (at 8.8011 -8.001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1080 "DRA_CLK"))
    (pad "D26" smd circle (at 9.6012 -8.001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "D27" smd circle (at 10.4013 -8.001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1089 "DRA_D6"))
    (pad "E2" smd circle (at -9.6012 -7.2009) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1784 "SNN_MIOB_DE"))
    (pad "E4" smd circle (at -8.001 -7.2009) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1730 "IFPC_TXD1"))
    (pad "E5" smd circle (at -7.2009 -7.2009) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "E6" smd circle (at -6.4008 -7.2009) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1735 "SNN_IFPC_TXD3*"))
    (pad "E7" smd circle (at -5.6007 -7.2009) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1882 "SNN_NVIO_NC_31"))
    (pad "E8" smd circle (at -4.8006 -7.2009) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "E9" smd circle (at -4.0005 -7.2009) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "E10" smd circle (at -3.2004 -7.2009) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1821 "SNN_NVIO_NC_27"))
    (pad "E11" smd circle (at -2.4003 -7.2009) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "E12" smd circle (at -1.6002 -7.2009) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1880 "SNN_NVIO_NC_28"))
    (pad "E13" smd circle (at -0.8001 -7.2009) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1832 "SNN_NVIO_NC_29"))
    (pad "E14" smd circle (at 0 -7.2009) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "E15" smd circle (at 0.8001 -7.2009) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1855 "SNN_DVIB_D2"))
    (pad "E16" smd circle (at 1.6002 -7.2009) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1857 "DVIB_D4"))
    (pad "E17" smd circle (at 2.4003 -7.2009) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "E18" smd circle (at 3.2004 -7.2009) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1859 "SNN_DVIB_D6"))
    (pad "E19" smd circle (at 4.0005 -7.2009) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1852 "SNN_DVIB_CTL2"))
    (pad "E20" smd circle (at 4.8006 -7.2009) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "E21" smd circle (at 5.6007 -7.2009) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1881 "SNN_NVIO_NC_30"))
    (pad "E22" smd circle (at 6.4008 -7.2009) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1077 "DRB_D14"))
    (pad "E23" smd circle (at 7.2009 -7.2009) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "E24" smd circle (at 8.001 -7.2009) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1062 "DRB_D10"))
    (pad "E26" smd circle (at 9.6012 -7.2009) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1088 "DRA_D5"))
    (pad "F1" smd circle (at -10.4013 -6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1772 "SNN_MIOB<0>"))
    (pad "F2" smd circle (at -9.6012 -6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "F3" smd circle (at -8.8011 -6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1773 "SNN_MIOB<1>"))
    (pad "F4" smd circle (at -8.001 -6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1733 "IFPC_TXD2*"))
    (pad "F5" smd circle (at -7.2009 -6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1732 "IFPC_TXD2"))
    (pad "F6" smd circle (at -6.4008 -6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1734 "SNN_IFPC_TXD3"))
    (pad "F7" smd circle (at -5.6007 -6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1824 "SNN_NVIO_NC_38"))
    (pad "F8" smd circle (at -4.8006 -6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1816 "SNN_NVIO_NC_39"))
    (pad "F9" smd circle (at -4.0005 -6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1819 "SNN_NVIO_NC_40"))
    (pad "F10" smd circle (at -3.2004 -6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "F11" smd circle (at -2.4003 -6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1822 "SNN_NVIO_NC_32"))
    (pad "F12" smd circle (at -1.6002 -6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1818 "SNN_NVIO_NC_33"))
    (pad "F13" smd circle (at -0.8001 -6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1833 "SNN_NVIO_NC_34"))
    (pad "F14" smd circle (at 0 -6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1883 "SNN_NVIO_NC_35"))
    (pad "F15" smd circle (at 0.8001 -6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1853 "SNN_DVIB_D0"))
    (pad "F16" smd circle (at 1.6002 -6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1854 "SNN_DVIB_D1"))
    (pad "F17" smd circle (at 2.4003 -6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1009 "3V3"))
    (pad "F18" smd circle (at 3.2004 -6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1850 "SNN_DVIB_CTL0"))
    (pad "F19" smd circle (at 4.0005 -6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1851 "SNN_DVIB_CTL1"))
    (pad "F20" smd circle (at 4.8006 -6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1009 "3V3"))
    (pad "F21" smd circle (at 5.6007 -6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1884 "SNN_NVIO_NC_36"))
    (pad "F22" smd circle (at 6.4008 -6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1885 "SNN_NVIO_NC_37"))
    (pad "F23" smd circle (at 7.2009 -6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1076 "DRB_D13"))
    (pad "F24" smd circle (at 8.001 -6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1093 "DRA_CMD"))
    (pad "F25" smd circle (at 8.8011 -6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1097 "DRA_D14"))
    (pad "F26" smd circle (at 9.6012 -6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1087 "DRA_D4"))
    (pad "F27" smd circle (at 10.4013 -6.4008) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1086 "DRA_D3"))
    (pad "G1" smd circle (at -10.4013 -5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1776 "SNN_MIOB<2>"))
    (pad "G2" smd circle (at -9.6012 -5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1777 "SNN_MIOB<3>"))
    (pad "G3" smd circle (at -8.8011 -5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1778 "SNN_MIOB<4>"))
    (pad "G4" smd circle (at -8.001 -5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "G5" smd circle (at -7.2009 -5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1767 "SNN_MIOB_CAL_PD_VDDQ"))
    (pad "G6" smd circle (at -6.4008 -5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1723 "IFPCD_RSET"))
    (pad "G22" smd circle (at 6.4008 -5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1789 "DR_CAL_PU_GND"))
    (pad "G23" smd circle (at 7.2009 -5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1886 "SNN_NVIO_NC_41"))
    (pad "G24" smd circle (at 8.001 -5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1096 "DRA_D13"))
    (pad "G25" smd circle (at 8.8011 -5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1098 "DRA_D12"))
    (pad "G26" smd circle (at 9.6012 -5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "G27" smd circle (at 10.4013 -5.6007) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1085 "DRA_D2"))
    (pad "H2" smd circle (at -9.6012 -4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1779 "SNN_MIOB<5>"))
    (pad "H4" smd circle (at -8.001 -4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1725 "IFPCD_IOVDD"))
    (pad "H5" smd circle (at -7.2009 -4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "H6" smd circle (at -6.4008 -4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "H22" smd circle (at 6.4008 -4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1887 "SNN_NVIO_NC_42"))
    (pad "H23" smd circle (at 7.2009 -4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "H24" smd circle (at 8.001 -4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1664 "NVIO_SP_PLLVDD"))
    (pad "H26" smd circle (at 9.6012 -4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1084 "DRA_D1"))
    (pad "J1" smd circle (at -10.4013 -4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1769 "SNN_MIOB_CLKOUT"))
    (pad "J2" smd circle (at -9.6012 -4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "J3" smd circle (at -8.8011 -4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1770 "SNN_MIOB_CLKOUT*"))
    (pad "J4" smd circle (at -8.001 -4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1739 "IFPD_TXD4*"))
    (pad "J5" smd circle (at -7.2009 -4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1738 "IFPD_TXD4"))
    (pad "J6" smd circle (at -6.4008 -4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1722 "IFPCD_PLLVDD"))
    (pad "J9" smd circle (at -4.0005 -4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "J10" smd circle (at -3.2004 -4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1009 "3V3"))
    (pad "J11" smd circle (at -2.4003 -4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "J12" smd circle (at -1.6002 -4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "J13" smd circle (at -0.8001 -4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "1V15"))
    (pad "J14" smd circle (at 0 -4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "J15" smd circle (at 0.8001 -4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "1V15"))
    (pad "J16" smd circle (at 1.6002 -4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "J17" smd circle (at 2.4003 -4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "J18" smd circle (at 3.2004 -4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1009 "3V3"))
    (pad "J19" smd circle (at 4.0005 -4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "J22" smd circle (at 6.4008 -4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1663 "NVIO_CLK_RSET_GND"))
    (pad "J23" smd circle (at 7.2009 -4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1888 "SNN_NVIO_NC_43"))
    (pad "J24" smd circle (at 8.001 -4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1083 "DRA_D11"))
    (pad "J25" smd circle (at 8.8011 -4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1082 "DRA_D10"))
    (pad "J26" smd circle (at 9.6012 -4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1081 "DRA_D0"))
    (pad "J27" smd circle (at 10.4013 -4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1058 "XTAL_OUT"))
    (pad "K1" smd circle (at -10.4013 -3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1780 "SNN_MIOB<6>"))
    (pad "K2" smd circle (at -9.6012 -3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1781 "SNN_MIOB<7>"))
    (pad "K3" smd circle (at -8.8011 -3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1782 "SNN_MIOB<8>"))
    (pad "K4" smd circle (at -8.001 -3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1741 "IFPD_TXD5*"))
    (pad "K5" smd circle (at -7.2009 -3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1736 "SNN_IFPD_TXC"))
    (pad "K6" smd circle (at -6.4008 -3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1737 "SNN_IFPD_TXC*"))
    (pad "K9" smd circle (at -4.0005 -3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1009 "3V3"))
    (pad "K19" smd circle (at 4.0005 -3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1009 "3V3"))
    (pad "K22" smd circle (at 6.4008 -3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1665 "NET0011"))
    (pad "K23" smd circle (at 7.2009 -3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1889 "SNN_NVIO_NC_44"))
    (pad "K24" smd circle (at 8.001 -3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1890 "SNN_NVIO_NC_45"))
    (pad "K25" smd circle (at 8.8011 -3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1111 "GPU_BUFCLK_LDT_IN"))
    (pad "K26" smd circle (at 9.6012 -3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "K27" smd circle (at 10.4013 -3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1059 "XTAL_IN"))
    (pad "L2" smd circle (at -9.6012 -2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1783 "SNN_MIOB<9>"))
    (pad "L4" smd circle (at -8.001 -2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1740 "IFPD_TXD5"))
    (pad "L5" smd circle (at -7.2009 -2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "L6" smd circle (at -6.4008 -2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1744 "SNN_IFPD_TXD7"))
    (pad "L9" smd circle (at -4.0005 -2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1009 "3V3"))
    (pad "L11" smd circle (at -2.4003 -2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "1V15"))
    (pad "L12" smd circle (at -1.6002 -2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "1V15"))
    (pad "L13" smd circle (at -0.8001 -2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "1V15"))
    (pad "L14" smd circle (at 0 -2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "1V15"))
    (pad "L15" smd circle (at 0.8001 -2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "1V15"))
    (pad "L16" smd circle (at 1.6002 -2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "1V15"))
    (pad "L17" smd circle (at 2.4003 -2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "1V15"))
    (pad "L19" smd circle (at 4.0005 -2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1790 "2V5"))
    (pad "L22" smd circle (at 6.4008 -2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1891 "SNN_NVIO_NC_46"))
    (pad "L23" smd circle (at 7.2009 -2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "L24" smd circle (at 8.001 -2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1662 "NVIO_GV_PLLVDD"))
    (pad "L26" smd circle (at 9.6012 -2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1555 "GPU_CLK*"))
    (pad "M1" smd circle (at -10.4013 -1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1774 "SNN_MIOB<10>"))
    (pad "M2" smd circle (at -9.6012 -1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "M3" smd circle (at -8.8011 -1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1775 "SNN_MIOB<11>"))
    (pad "M4" smd circle (at -8.001 -1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1743 "IFPD_TXD6*"))
    (pad "M5" smd circle (at -7.2009 -1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1742 "IFPD_TXD6"))
    (pad "M6" smd circle (at -6.4008 -1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1745 "SNN_IFPD_TXD7*"))
    (pad "M9" smd circle (at -4.0005 -1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1009 "3V3"))
    (pad "M11" smd circle (at -2.4003 -1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "1V15"))
    (pad "M12" smd circle (at -1.6002 -1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "1V15"))
    (pad "M13" smd circle (at -0.8001 -1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "M14" smd circle (at 0 -1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "1V15"))
    (pad "M15" smd circle (at 0.8001 -1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "M16" smd circle (at 1.6002 -1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "M17" smd circle (at 2.4003 -1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "1V15"))
    (pad "M19" smd circle (at 4.0005 -1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1790 "2V5"))
    (pad "M22" smd circle (at 6.4008 -1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1271 "FBEF_REFCLK*"))
    (pad "M23" smd circle (at 7.2009 -1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1272 "FBEF_REFCLK"))
    (pad "M24" smd circle (at 8.001 -1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1227 "FBCD_REFCLK*"))
    (pad "M25" smd circle (at 8.8011 -1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1228 "FBCD_REFCLK"))
    (pad "M26" smd circle (at 9.6012 -1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1556 "GPU_CLK"))
    (pad "M27" smd circle (at 10.4013 -1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1815 "FL_REFCLK_VAIO"))
    (pad "N1" smd circle (at -10.4013 -0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1892 "SNN_MIOB<12>"))
    (pad "N2" smd circle (at -9.6012 -0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1893 "SNN_MIOB<13>"))
    (pad "N3" smd circle (at -8.8011 -0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1894 "SNN_MIOB<14>"))
    (pad "N4" smd circle (at -8.001 -0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1724 "SNN_IFPCD_VPROBE"))
    (pad "N5" smd circle (at -7.2009 -0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1895 "SNN_NVIO_NC_47"))
    (pad "N6" smd circle (at -6.4008 -0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1896 "SNN_NVIO_NC_48"))
    (pad "N9" smd circle (at -4.0005 -0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1897 "SNN_NVIO_NC_49"))
    (pad "N11" smd circle (at -2.4003 -0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "N12" smd circle (at -1.6002 -0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "N13" smd circle (at -0.8001 -0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "N14" smd circle (at 0 -0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "N15" smd circle (at 0.8001 -0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "N16" smd circle (at 1.6002 -0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "N17" smd circle (at 2.4003 -0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "1V15"))
    (pad "N19" smd circle (at 4.0005 -0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1790 "2V5"))
    (pad "N22" smd circle (at 6.4008 -0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1545 "FBGH_REFCLK"))
    (pad "N23" smd circle (at 7.2009 -0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1544 "FBGH_REFCLK*"))
    (pad "N24" smd circle (at 8.001 -0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1615 "FBAB_REFCLK"))
    (pad "N25" smd circle (at 8.8011 -0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1192 "FBAB_REFCLK*"))
    (pad "N26" smd circle (at 9.6012 -0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "N27" smd circle (at 10.4013 -0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1623 "GPU_PMC_ISO_RESET*"))
    (pad "P2" smd circle (at -9.6012 0) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1678 "DACA_BLUE"))
    (pad "P4" smd circle (at -8.001 0) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1666 "NVIO_PLLVDD"))
    (pad "P5" smd circle (at -7.2009 0) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "P6" smd circle (at -6.4008 0) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1684 "DACA_VREF"))
    (pad "P9" smd circle (at -4.0005 0) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "P11" smd circle (at -2.4003 0) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "P12" smd circle (at -1.6002 0) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "P13" smd circle (at -0.8001 0) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "P14" smd circle (at 0 0) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "P15" smd circle (at 0.8001 0) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "P16" smd circle (at 1.6002 0) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "P17" smd circle (at 2.4003 0) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "P19" smd circle (at 4.0005 0) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "P22" smd circle (at 6.4008 0) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1898 "SNN_NVIO_NC_50"))
    (pad "P23" smd circle (at 7.2009 0) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "P24" smd circle (at 8.001 0) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1661 "NVIO_GV_PLLAVDD"))
    (pad "P26" smd circle (at 9.6012 0) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1659 "NET0009"))
    (pad "R1" smd circle (at -10.4013 0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1681 "DACA_RED"))
    (pad "R2" smd circle (at -9.6012 0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "R3" smd circle (at -8.8011 0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1899 "SNN_NVIO_NC_51"))
    (pad "R4" smd circle (at -8.001 0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1793 "NVIO_EXT_REFCLKA"))
    (pad "R5" smd circle (at -7.2009 0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1682 "DACA_RSET"))
    (pad "R6" smd circle (at -6.4008 0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1900 "SNN_NVIO_NC_52"))
    (pad "R9" smd circle (at -4.0005 0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1683 "DACA_VDD"))
    (pad "R11" smd circle (at -2.4003 0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "1V15"))
    (pad "R12" smd circle (at -1.6002 0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "R13" smd circle (at -0.8001 0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "R14" smd circle (at 0 0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "R15" smd circle (at 0.8001 0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "R16" smd circle (at 1.6002 0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "R17" smd circle (at 2.4003 0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "R19" smd circle (at 4.0005 0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "1V15"))
    (pad "R22" smd circle (at 6.4008 0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1514 "GV_RX1*"))
    (pad "R23" smd circle (at 7.2009 0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1515 "GV_RX1"))
    (pad "R24" smd circle (at 8.001 0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1495 "GV_RX3*"))
    (pad "R25" smd circle (at 8.8011 0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1642 "GV_RX3"))
    (pad "R26" smd circle (at 9.6012 0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1660 "NET0010"))
    (pad "R27" smd circle (at 10.4013 0.8001) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1507 "GV_RXCTL"))
    (pad "T1" smd circle (at -10.4013 1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1679 "DACA_GREEN"))
    (pad "T2" smd circle (at -9.6012 1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1685 "DACA_VSYNC"))
    (pad "T3" smd circle (at -8.8011 1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1901 "SNN_NVIO_NC_53"))
    (pad "T4" smd circle (at -8.001 1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1746 "SNN_MIOA_CAL_PD_VDDQ"))
    (pad "T5" smd circle (at -7.2009 1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T6" smd circle (at -6.4008 1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1902 "SNN_NVIO_NC_54"))
    (pad "T9" smd circle (at -4.0005 1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1009 "3V3"))
    (pad "T11" smd circle (at -2.4003 1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "1V15"))
    (pad "T12" smd circle (at -1.6002 1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T13" smd circle (at -0.8001 1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T14" smd circle (at 0 1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "1V15"))
    (pad "T15" smd circle (at 0.8001 1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T16" smd circle (at 1.6002 1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "1V15"))
    (pad "T17" smd circle (at 2.4003 1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "1V15"))
    (pad "T19" smd circle (at 4.0005 1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "1V15"))
    (pad "T22" smd circle (at 6.4008 1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1428 "GV_RX2"))
    (pad "T23" smd circle (at 7.2009 1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1433 "GV_RX2*"))
    (pad "T24" smd circle (at 8.001 1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1490 "GV_RX0"))
    (pad "T25" smd circle (at 8.8011 1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1487 "GV_RX0*"))
    (pad "T26" smd circle (at 9.6012 1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "T27" smd circle (at 10.4013 1.6002) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1525 "GV_RXCTL*"))
    (pad "U2" smd circle (at -9.6012 2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1680 "DACA_HSYNC"))
    (pad "U4" smd circle (at -8.001 2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1905 "SNN_NVIO_NC_57"))
    (pad "U5" smd circle (at -7.2009 2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "U6" smd circle (at -6.4008 2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1747 "SNN_MIOA_CAL_PU_GND"))
    (pad "U9" smd circle (at -4.0005 2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1009 "3V3"))
    (pad "U11" smd circle (at -2.4003 2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "1V15"))
    (pad "U12" smd circle (at -1.6002 2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "1V15"))
    (pad "U13" smd circle (at -0.8001 2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "1V15"))
    (pad "U14" smd circle (at 0 2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "1V15"))
    (pad "U15" smd circle (at 0.8001 2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "1V15"))
    (pad "U16" smd circle (at 1.6002 2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "1V15"))
    (pad "U17" smd circle (at 2.4003 2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "1V15"))
    (pad "U19" smd circle (at 4.0005 2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "1V15"))
    (pad "U22" smd circle (at 6.4008 2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1903 "SNN_NVIO_NC_55"))
    (pad "U23" smd circle (at 7.2009 2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "U24" smd circle (at 8.001 2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1904 "SNN_NVIO_NC_56"))
    (pad "U26" smd circle (at 9.6012 2.4003) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1486 "GV_RXCLK*"))
    (pad "V1" smd circle (at -10.4013 3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1750 "MIOA_CTL3"))
    (pad "V2" smd circle (at -9.6012 3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "V3" smd circle (at -8.8011 3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1766 "SNN_MIOA_VSYNC"))
    (pad "V4" smd circle (at -8.001 3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1703 "IFPA_TXC*"))
    (pad "V5" smd circle (at -7.2009 3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1702 "IFPA_TXC"))
    (pad "V6" smd circle (at -6.4008 3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1906 "SNN_NVIO_NC_58"))
    (pad "V9" smd circle (at -4.0005 3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1009 "3V3"))
    (pad "V19" smd circle (at 4.0005 3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1009 "3V3"))
    (pad "V22" smd circle (at 6.4008 3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1521 "GV_TX17*"))
    (pad "V23" smd circle (at 7.2009 3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1520 "GV_TX17"))
    (pad "V24" smd circle (at 8.001 3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1517 "GV_TX19*"))
    (pad "V25" smd circle (at 8.8011 3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1426 "GV_TX19"))
    (pad "V26" smd circle (at 9.6012 3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1491 "GV_RXCLK"))
    (pad "V27" smd circle (at 10.4013 3.2004) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1516 "GV_TX15"))
    (pad "W1" smd circle (at -10.4013 4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1764 "SNN_MIOA_HSYNC"))
    (pad "W2" smd circle (at -9.6012 4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1763 "SNN_MIOA_DE"))
    (pad "W3" smd circle (at -8.8011 4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1751 "SNN_MIOA<0>"))
    (pad "W4" smd circle (at -8.001 4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1705 "IFPA_TXD0*"))
    (pad "W5" smd circle (at -7.2009 4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1765 "MIOA_VREF"))
    (pad "W6" smd circle (at -6.4008 4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1907 "SNN_NVIO_NC_59"))
    (pad "W9" smd circle (at -4.0005 4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "W10" smd circle (at -3.2004 4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1009 "3V3"))
    (pad "W11" smd circle (at -2.4003 4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "W12" smd circle (at -1.6002 4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "W13" smd circle (at -0.8001 4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "1V15"))
    (pad "W14" smd circle (at 0 4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "W15" smd circle (at 0.8001 4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "1V15"))
    (pad "W16" smd circle (at 1.6002 4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "W17" smd circle (at 2.4003 4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "W18" smd circle (at 3.2004 4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1009 "3V3"))
    (pad "W19" smd circle (at 4.0005 4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "W22" smd circle (at 6.4008 4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1494 "GV_TX18"))
    (pad "W23" smd circle (at 7.2009 4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1518 "GV_TX18*"))
    (pad "W24" smd circle (at 8.001 4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1541 "GV_TX16"))
    (pad "W25" smd circle (at 8.8011 4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1519 "GV_TX16*"))
    (pad "W26" smd circle (at 9.6012 4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "W27" smd circle (at 10.4013 4.0005) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1650 "GV_TX15*"))
    (pad "Y2" smd circle (at -9.6012 4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1752 "SNN_MIOA<1>"))
    (pad "Y4" smd circle (at -8.001 4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1704 "IFPA_TXD0"))
    (pad "Y5" smd circle (at -7.2009 4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "Y6" smd circle (at -6.4008 4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "Y22" smd circle (at 6.4008 4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1908 "SNN_NVIO_NC_60"))
    (pad "Y23" smd circle (at 7.2009 4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "Y24" smd circle (at 8.001 4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1909 "SNN_NVIO_NC_61"))
    (pad "Y26" smd circle (at 9.6012 4.8006) (size 0.3556 0.3556) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1496 "GV_TX14*"))
  )
  (footprint "DFET_SMD_DPAK_1" (layer "F.Cu")
    (tedit 0)
    (at 225.410108 86.360907 -90)
    (fp_text reference "Q20" (at 2.192477 -1.5875 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -2.290089 5.31241 270) (size 1.6002 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 988 "PS5_NVVDD_UG2_R"))
    (pad "2" smd rect (at 0 -1.867408 270) (size 5.799811 6.200089) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 981 "12V_PEX6_F1"))
    (pad "3" smd rect (at 2.290089 5.31241 270) (size 1.6002 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "PS5_NVVDD_PHASE2"))
  )
  (footprint "1206_1" (layer "F.Cu")
    (tedit 0)
    (at 227.696413 144.018907 -90)
    (fp_text reference "C135" (at 0 1.0795 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -1.4732 0 270) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 983 "12V_PEX6_F2"))
    (pad "2" smd rect (at 1.4732 0 270) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "CAP_SMD_066X066_1" (layer "F.Cu")
    (tedit 0)
    (at 182.992108 131.826907 180)
    (fp_text reference "C108" (at 1.27 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -2.602992 0 180) (size 3.556 1.651) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at 2.602992 0 180) (size 3.556 1.651) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 159.598708 127.394607 90)
    (fp_text reference "C82" (at 0 -0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 12.126308 116.739815 180)
    (fp_text reference "R8" (at 0.635 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1765 "MIOA_VREF"))
    (pad "2" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 161.859308 58.065612)
    (fp_text reference "C85" (at -0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "CAP_SMD_7343_1" (layer "F.Cu")
    (tedit 0)
    (at 51.166108 69.140012)
    (fp_text reference "C35" (at -0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -3.1115 0) (size 2.413 3.048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at 3.1115 0) (size 2.413 3.048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "GEOM0008_1" (layer "F.Cu")
    (tedit 0)
    (at 205.598413 75.388615)
    (fp_text reference "Q6" (at 1.27 1.582877 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -2.290115 5.31241) (size 1.6002 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 993 "PS5_NVVDD_LG1_AC"))
    (pad "2" smd rect (at 0 -1.867408) (size 5.799811 6.200089) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "PS5_NVVDD_PHASE1"))
    (pad "3" smd rect (at 2.290089 5.31241) (size 1.6002 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "1206_1" (layer "F.Cu")
    (tedit 0)
    (at 41.336308 134.773307 90)
    (fp_text reference "C28" (at 0 -0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -1.4732 0 90) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 991 "12V_F"))
    (pad "2" smd rect (at 1.4732 0 90) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 159.573308 67.704607 90)
    (fp_text reference "C76" (at 0 -0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "1206_1" (layer "F.Cu")
    (tedit 0)
    (at 241.742308 130.760107 180)
    (fp_text reference "R72" (at 0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -1.4732 0 180) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "INPUT_PEX6_IN2"))
    (pad "2" smd rect (at 1.4732 0 180) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 983 "12V_PEX6_F2"))
  )
  (footprint "DFET_SMD_DPAK_1" (layer "F.Cu")
    (tedit 0)
    (at 225.410108 76.073907 -90)
    (fp_text reference "Q19" (at 2.192477 -1.5875 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -2.290089 5.31241 270) (size 1.6002 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 982 "PS5_NVVDD_UG1_R"))
    (pad "2" smd rect (at 0 -1.867408 270) (size 5.799811 6.200089) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 981 "12V_PEX6_F1"))
    (pad "3" smd rect (at 2.290089 5.31241 270) (size 1.6002 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "PS5_NVVDD_PHASE1"))
  )
  (footprint "IND_SMD_0402_1" (layer "F.Cu")
    (tedit 0)
    (at 5.039708 134.697615 -90)
    (fp_text reference "LB1" (at 0 0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 90) (size 0.6858 0.5334) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2000 "I2C2_SCL_R"))
    (pad "2" smd rect (at 0.5334 0 270) (size 0.6858 0.5334) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1928 "I2C2_SCL_CON"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 136.637108 145.594012)
    (fp_text reference "R42" (at -0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1113 "I2CS_SDA"))
  )
  (footprint "GEOM0022_1" (layer "F.Cu")
    (tedit 0)
    (at 9.908405 124.624)
    (fp_text reference "MEC4" (at -1.27 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 3.5814 3.5814) (drill 3.175) (layers *.Cu *.Mask)
      (net 1 "GND"))
  )
  (footprint "1206_1" (layer "F.Cu")
    (tedit 0)
    (at 233.284108 78.677407)
    (fp_text reference "C137" (at -1.0795 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -1.4732 0) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 981 "12V_PEX6_F1"))
    (pad "2" smd rect (at 1.4732 0) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "SOT23_1" (layer "F.Cu")
    (tedit 0)
    (at 244.968108 98.235407 180)
    (fp_text reference "Q27" (at -1.359967 -1.11125 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.9525 1.143 180) (size 0.9144 0.9144) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 968 "PS5_NVVDD_VID4"))
    (pad "2" smd rect (at 0.9525 1.143 180) (size 0.9144 0.9144) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1983 "VID_PSI"))
    (pad "3" smd rect (at 0 -1.143 180) (size 0.9144 0.9144) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 943 "NET0002"))
  )
  (footprint "1206_1" (layer "F.Cu")
    (tedit 0)
    (at 210.551108 65.342407 -90)
    (fp_text reference "R67" (at 0 0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -1.4732 0 270) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "INPUT_PEX6_IN1"))
    (pad "2" smd rect (at 1.4732 0 270) (size 1.27 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 981 "12V_PEX6_F1"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 223.251387 104.217615 -90)
    (fp_text reference "C122" (at 0 1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 981 "12V_PEX6_F1"))
    (pad "2" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "GEOM0004_1" (layer "F.Cu")
    (tedit 0)
    (at 193.533108 100.457907 90)
    (fp_text reference "L10" (at -1.27 1.5875 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 3.81 90) (size 4.0132 4.318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "PS5_NVVDD_PHASE6"))
    (pad "2" smd rect (at 0 -3.81 90) (size 4.0132 4.318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 207.211008 60.821207 -90)
    (fp_text reference "C116" (at 0 1.27 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1993 "SPDIF_IN_COMP2_D"))
    (pad "2" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "SOT23_1" (layer "F.Cu")
    (tedit 0)
    (at 247.254108 124.778407)
    (fp_text reference "Q29" (at 1.359967 1.11125 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.9525 1.143) (size 0.9144 0.9144) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1985 "PS5_NVVDD_EN_12V_F"))
    (pad "2" smd rect (at 0.9525 1.143) (size 0.9144 0.9144) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "3" smd rect (at 0 -1.143) (size 0.9144 0.9144) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2081 "PS5_NVVDD_EN_Q"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 159.573308 90.349215 90)
    (fp_text reference "C78" (at 0 -0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "CAP_SMD_3528_1" (layer "F.Cu")
    (tedit 0)
    (at 12.964508 133.706507 90)
    (fp_text reference "C10" (at 0 -0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -1.35001 0 90) (size 1.524 2.8194) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1790 "2V5"))
    (pad "2" smd rect (at 1.35001 0 90) (size 1.524 2.8194) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 193.469608 107.506407)
    (fp_text reference "R54" (at -0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 928 "PS5_NVVDD_VAMP_CSREF"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 78.598108 135.103812 90)
    (fp_text reference "C56" (at 0 -0.9525 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 974 "THERM_DP"))
    (pad "2" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 975 "THERM_DN"))
  )
  (footprint "0805_1" (layer "F.Cu")
    (tedit 0)
    (at 181.722108 73.152907 180)
    (fp_text reference "C94" (at 0.787406 -0.000013 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.9525 0 180) (size 1.143 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at 0.9525 0 180) (size 1.143 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 89.152799 72.086615 180)
    (fp_text reference "C60" (at 0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "GEOM0002_1" (layer "F.Cu")
    (tedit 0)
    (at 240.396108 66.048502)
    (fp_text reference "J6" (at 3.556 2.0955 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 3.175 3.175) (drill 1.8034) (layers *.Cu *.Mask)
      (net 4 "INPUT_PEX6_IN2"))
    (pad "2" thru_hole circle (at 4.191 0) (size 3.175 3.175) (drill 1.8034) (layers *.Cu *.Mask)
      (net 4 "INPUT_PEX6_IN2"))
    (pad "3" thru_hole circle (at 8.382 0) (size 3.175 3.175) (drill 1.8034) (layers *.Cu *.Mask)
      (net 4 "INPUT_PEX6_IN2"))
    (pad "4" thru_hole circle (at 0 4.191) (size 3.175 3.175) (drill 1.8034) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "5" thru_hole circle (at 4.191 4.191) (size 3.175 3.175) (drill 1.8034) (layers *.Cu *.Mask)
      (net 5 "SNN_INPUT_PEX6_DT2*"))
    (pad "6" thru_hole circle (at 8.382 4.191) (size 3.175 3.175) (drill 1.8034) (layers *.Cu *.Mask)
      (net 1 "GND"))
  )
  (footprint "GEOM0008_1" (layer "F.Cu")
    (tedit 0)
    (at 213.777213 126.696615)
    (fp_text reference "Q17" (at 1.5875 2.217877 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -2.290115 5.31241) (size 1.6002 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 996 "PS5_NVVDD_LG4_AC"))
    (pad "2" smd rect (at 0 -1.867408) (size 5.799811 6.200089) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "PS5_NVVDD_PHASE4"))
    (pad "3" smd rect (at 2.290089 5.31241) (size 1.6002 2.999994) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "SOT23_1" (layer "F.Cu")
    (tedit 0)
    (at 206.550608 57.646207 -90)
    (fp_text reference "Q12" (at 1.11125 -1.359967 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.9525 1.143 270) (size 0.9144 0.9144) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1992 "SPDIF_IN_R"))
    (pad "2" smd rect (at 0.9525 1.143 270) (size 0.9144 0.9144) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "3" smd rect (at 0 -1.143 270) (size 0.9144 0.9144) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1993 "SPDIF_IN_COMP2_D"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 91.692621 72.086615)
    (fp_text reference "R38" (at -0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (pad "2" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 300 "FBE_SEN2"))
  )
  (footprint "0603_1" (layer "F.Cu")
    (tedit 0)
    (at 21.346508 146.864215)
    (fp_text reference "C15" (at -0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.762 0 180) (size 0.889 0.7874) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at 0.762 0) (size 0.889 0.7874) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 4.023708 137.796415 -90)
    (fp_text reference "C3" (at 0 0.635 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1929 "I2C2_SDA_CON"))
    (pad "2" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "F.Cu")
    (tedit 0)
    (at 72.812013 96.572215 180)
    (fp_text reference "C44" (at 0.9525 0 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0805_1" (layer "F.Cu")
    (tedit 0)
    (at 181.722108 101.854907 180)
    (fp_text reference "C99" (at 0.787406 -0.000013 unlocked) (layer "F.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.9525 0 180) (size 1.143 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at 0.9525 0 180) (size 1.143 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
  )
  (footprint "0603_1" (layer "B.Cu")
    (tedit 0)
    (at 124.165708 137.466012 180)
    (fp_text reference "C779" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.762 0) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1643 "PEX_PLLVDD"))
    (pad "2" smd rect (at -0.762 0 180) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 15.80372 85.839216)
    (fp_text reference "C1229" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1965 "PS3_FBVDDQ_CP"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1054 "PS3_FBVDDQ_CP_RC"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 6.208108 111.266115 180)
    (fp_text reference "C1242" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1921 "DACA_GREEN_CON"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 24.132405 104.2532 -90)
    (fp_text reference "C1203" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "IND_SMD_0402_1" (layer "B.Cu")
    (tedit 0)
    (at 108.239908 126.213812 180)
    (fp_text reference "LB504" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.6858 0.5334) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.6858 0.5334) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1484 "GV_PLLAVDD"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 192.199608 68.390407 90)
    (fp_text reference "C537" (at 0 -0.7874 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0 90) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1914 "5V"))
    (pad "2" smd rect (at -0.9525 0 90) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 173.483415 74.20241)
    (fp_text reference "C582" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 61.467307 77.531105)
    (fp_text reference "C1077" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 86.189711 62.180412 -90)
    (fp_text reference "R764" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 301 "FBE_VREF3"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 15.047308 79.045707 180)
    (fp_text reference "R924" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 991 "12V_F"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1990 "PS3_NVVDD_PGOOD*"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 30.795308 128.220107)
    (fp_text reference "R873" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1949 "I2C2_SDA_UC"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 135.741504 56.198915 180)
    (fp_text reference "C719" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 119.493607 60.478307 -90)
    (fp_text reference "C813" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 240.104313 105.551115)
    (fp_text reference "R550" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 10 "PS5_NVVDD_PHASE3"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 929 "PS5_NVVDD_VAMP_CSSUM"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 97.827915 67.783804 90)
    (fp_text reference "C970" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 118.882508 126.213812 180)
    (fp_text reference "C818" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 129.842608 115.570907 90)
    (fp_text reference "C737" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 30.302015 97.134114 180)
    (fp_text reference "R874" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1858 "DVIB_D5"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 122.870308 141.479212 180)
    (fp_text reference "R728" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1971 "PEX_PLLVDD_OP_ADJ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "IND_SMD_0603_1" (layer "B.Cu")
    (tedit 0)
    (at 5.827108 102.947615 -90)
    (fp_text reference "L507" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.762 0 90) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1678 "DACA_BLUE"))
    (pad "2" smd rect (at -0.762 0 270) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1918 "DACA_BLUE_CON"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 61.707108 139.777107)
    (fp_text reference "R827" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1180 "JTAG_TRST*"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 166.411013 93.917712)
    (fp_text reference "R663" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 669 "FBB_CMD<27>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 72.400508 132.271407 180)
    (fp_text reference "C1015" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 979 "THERM_VDD"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 59.565913 85.548894 90)
    (fp_text reference "C1099" (at 0 -1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0603_1" (layer "B.Cu")
    (tedit 0)
    (at 21.638608 91.250407 180)
    (fp_text reference "C1211" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.762 0) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1040 "PS3_FBVDDQ_BOOT"))
    (pad "2" smd rect (at -0.762 0 180) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 989 "PS3_FBVDDQ_PHASE"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 127.723715 64.581398 -90)
    (fp_text reference "R719" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 415 "FBD_CMD<23>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 113.642005 100.636698)
    (fp_text reference "C857" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 111.340207 129.058307 90)
    (fp_text reference "C876" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 164.221508 138.495906)
    (fp_text reference "C666" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 26.692217 113.844698 90)
    (fp_text reference "C1180" (at 0 -1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1694 "DACC_VREF"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0603_1" (layer "B.Cu")
    (tedit 0)
    (at 239.634108 98.870407 90)
    (fp_text reference "R555" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.762 0 270) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1043 "PS5_NVVDD_VIN_PWM"))
    (pad "2" smd rect (at -0.762 0 90) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 962 "PS5_NVVDD_VCC"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 4.734908 78.042712 90)
    (fp_text reference "C1254" (at 0 -1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1951 "DACB_Y_F"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0603_1" (layer "B.Cu")
    (tedit 0)
    (at 242.936108 98.870407 -90)
    (fp_text reference "C516" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.762 0 90) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 962 "PS5_NVVDD_VCC"))
    (pad "2" smd rect (at -0.762 0 270) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 85.148311 62.180412 90)
    (fp_text reference "R765" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 301 "FBE_VREF3"))
  )
  (footprint "1206_1" (layer "B.Cu")
    (tedit 0)
    (at 32.090708 130.023812 180)
    (fp_text reference "R867" (at 1.0795 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 1.4732 0 180) (size 1.27 1.5748) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1106 "PS1_1V15_PH_RC"))
    (pad "2" smd rect (at -1.4732 0 180) (size 1.27 1.5748) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 9.433908 81.522207 -90)
    (fp_text reference "R937" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1668 "DACB_Y"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 171.545801 123.574904 180)
    (fp_text reference "C611" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2016 "FBA1_CLK0_R"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 29.619821 109.716207 90)
    (fp_text reference "C1165" (at 0 -1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 110.221108 108.306812 -90)
    (fp_text reference "C884" (at 0 0.7874 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0 270) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.9525 0 270) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 121.016108 125.299412 -90)
    (fp_text reference "C804" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 167.421908 128.601412 180)
    (fp_text reference "R659" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 804 "FBA_CMD<23>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 96.526901 56.275115)
    (fp_text reference "C973" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 64.564608 137.287907 180)
    (fp_text reference "R817" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1981 "THERM_SHDN"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 116.952108 118.212812 90)
    (fp_text reference "C836" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 134.440491 63.080308 90)
    (fp_text reference "C722" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 489 "FBD_VREF1"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 32.997005 100.5702 -90)
    (fp_text reference "R864" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1663 "NVIO_CLK_RSET_GND"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 21.092508 98.172415 180)
    (fp_text reference "R906" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1786 "MIOB_VREF"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "SOT23_1" (layer "B.Cu")
    (tedit 0)
    (at 224.825908 127.928007 90)
    (fp_text reference "D511" (at -1.23825 1.23825 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1028 "PS5_NVVDD_LG4"))
    (pad "2" smd rect (at -0.9525 1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 996 "PS5_NVVDD_LG4_AC"))
    (pad "3" smd rect (at 0 -1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2085 "PS5_NVVDD_LG4_D"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 61.467307 84.247906)
    (fp_text reference "C1079" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 101.966108 129.185612 90)
    (fp_text reference "C953" (at 0 -0.7874 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0 90) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at -0.9525 0 90) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0603_1" (layer "B.Cu")
    (tedit 0)
    (at 102.461408 118.619212)
    (fp_text reference "C951" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.762 0 180) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.762 0) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 118.16572 60.77851 90)
    (fp_text reference "R731" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 431 "FBD_VREF3"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 115.936413 62.053615 90)
    (fp_text reference "R735" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 352 "FBE_CMD<0>"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 59.121413 79.991095 90)
    (fp_text reference "C1107" (at 0 -0.7874 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0 90) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.9525 0 90) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0603_1" (layer "B.Cu")
    (tedit 0)
    (at 26.045508 139.675507 180)
    (fp_text reference "C1185" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.762 0) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1048 "PS1_VCC5"))
    (pad "2" smd rect (at -0.762 0 180) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 164.221508 79.734301)
    (fp_text reference "R678" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 614 "FBC_CMD<1>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 70.978108 141.720207 180)
    (fp_text reference "C1024" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1994 "THERM_SHDN_D*"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 119.365108 119.101812 90)
    (fp_text reference "C816" (at 0 -0.7874 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0 90) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.9525 0 90) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 196.835108 68.390407 90)
    (fp_text reference "C535" (at 0 -0.7874 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0 90) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1001 "5V_INPUT"))
    (pad "2" smd rect (at -0.9525 0 90) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 104.935419 128.220412 90)
    (fp_text reference "C922" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 100.175408 62.320112)
    (fp_text reference "R754" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2023 "FBE1_CLK0_R"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 293 "FBE1_CLK0"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 61.153413 117.363106)
    (fp_text reference "C1092" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 71.359413 69.419615)
    (fp_text reference "R775" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 224 "FBF_CMD<1>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 69.556521 67.795996)
    (fp_text reference "C1027" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 154.925108 57.087407 180)
    (fp_text reference "C697" (at 0.7874 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0 180) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.9525 0 180) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 165.872508 139.066212 90)
    (fp_text reference "R672" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 873 "FBA_CMD<2>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 29.619821 103.261305 -90)
    (fp_text reference "C1164" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 8.205615 140.056812 -90)
    (fp_text reference "C1236" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1688 "DACC_BLUE"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 144.047812 59.7778 -90)
    (fp_text reference "C705" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 104.544691 58.17661 -90)
    (fp_text reference "C929" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 27.244896 100.108911 180)
    (fp_text reference "C1178" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 175.384808 112.353718 -90)
    (fp_text reference "C564" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 59.016511 152.807815 -90)
    (fp_text reference "C1108" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2046 "PEX_TX_C1"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1157 "PEX_TX1"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 173.813615 140.297299 180)
    (fp_text reference "C578" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 38.991405 105.32)
    (fp_text reference "R849" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1659 "NET0009"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 124.826108 115.672812 -90)
    (fp_text reference "C774" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 170.881413 89.124402 180)
    (fp_text reference "R627" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 691 "FBB_VREF3"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 117.333108 153.010812 180)
    (fp_text reference "C830" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2036 "PEX_TX_C15*"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1169 "PEX_TX15*"))
  )
  (footprint "DIODE_SMD_SMA_1" (layer "B.Cu")
    (tedit 0)
    (at 203.058108 129.921907 -90)
    (fp_text reference "D516" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -1.880108 0 270) (size 2.159 2.032) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 11 "PS5_NVVDD_PHASE4"))
    (pad "2" smd rect (at 1.880108 0 270) (size 2.159 2.032) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 160.373408 67.83971 -90)
    (fp_text reference "C687" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 20.640617 106.653704)
    (fp_text reference "R907" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1682 "DACA_RSET"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 64.564608 136.208407)
    (fp_text reference "R816" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1981 "THERM_SHDN"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1998 "THERM_SHDN_Q"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 21.067108 116.180812 90)
    (fp_text reference "C1214" (at 0 -1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1701 "IFPAB_IOVDD"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 160.373408 129.515812 90)
    (fp_text reference "C692" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 71.467109 152.807815 -90)
    (fp_text reference "C1019" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2055 "PEX_TX_C4"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1176 "PEX_TX4"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 116.952108 114.567607 -90)
    (fp_text reference "C835" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 24.765297 98.107416 180)
    (fp_text reference "C1198" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1673 "DACB_VDD"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "SOT23_1" (layer "B.Cu")
    (tedit 0)
    (at 237.144908 136.068707 90)
    (fp_text reference "D505" (at -1.23825 1.23825 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1002 "PS5_NVVDD_BOOT4_RC"))
    (pad "2" smd rect (at -0.9525 1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1003 "PS5_NVVDD_BOOT3_RC"))
    (pad "3" smd rect (at 0 -1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 981 "12V_PEX6_F1"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 104.935419 118.3502 -90)
    (fp_text reference "C920" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 32.362005 103.669 180)
    (fp_text reference "C1150" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1790 "2V5"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 89.621708 58.17661 -90)
    (fp_text reference "C984" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 83.868608 64.008907 180)
    (fp_text reference "R766" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 280 "FBE_CMD<28>"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 176.111197 73.585012 -90)
    (fp_text reference "C547" (at 0 0.7874 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0 270) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.9525 0 270) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 13.523308 98.820115 -90)
    (fp_text reference "R929" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1687 "I2C1_SDA"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2002 "I2C1_SDA_R"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 5.477604 143.76031 90)
    (fp_text reference "C1250" (at 0 -1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1933 "DACC_RED_CON"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 31.244405 110.4254 180)
    (fp_text reference "C1158" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 113.269108 119.101812 90)
    (fp_text reference "C862" (at 0 -0.7874 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0 90) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.9525 0 90) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 5.852508 71.426012 -90)
    (fp_text reference "C1245" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1670 "DACB_PR"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1953 "DACB_PR_F"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 166.990108 131.649412 180)
    (fp_text reference "R662" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 822 "FBA_VREF4"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 110.856108 111.608812 90)
    (fp_text reference "C880" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 123.048108 111.481812 90)
    (fp_text reference "C784" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 63.414013 102.439412)
    (fp_text reference "C1065" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 94.066708 69.571812 180)
    (fp_text reference "C977" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 61.276807 89.258996)
    (fp_text reference "C1089" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 97.827915 64.962398 -90)
    (fp_text reference "R758" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 285 "FBE_CMD<23>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 227.340508 102.413707 90)
    (fp_text reference "R580" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1037 "PS5_NVVDD_LG6"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 998 "PS5_NVVDD_LG6_AC"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 248.968608 97.536907 -90)
    (fp_text reference "R518" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 965 "PS5_NVVDD_VID1"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 166.277917 59.279402)
    (fp_text reference "C648" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 128.052899 106.341004 90)
    (fp_text reference "C753" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 124.673708 126.722015 90)
    (fp_text reference "C776" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "SOT23_1" (layer "B.Cu")
    (tedit 0)
    (at 9.827608 108.218115 90)
    (fp_text reference "D527" (at -1.23825 1.23825 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "2" smd rect (at -0.9525 1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "3" smd rect (at 0 -1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1681 "DACA_RED"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 6.462108 135.586615 90)
    (fp_text reference "C1240" (at 0 -1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1987 "GPIO0_DVIAB_HPD_R"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 175.384808 142.198718 -90)
    (fp_text reference "C568" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 171.545801 125.376298 180)
    (fp_text reference "C612" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 118.16572 63.080308 90)
    (fp_text reference "R732" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 431 "FBD_VREF3"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 221.384208 127.420007 90)
    (fp_text reference "R589" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1028 "PS5_NVVDD_LG4"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2085 "PS5_NVVDD_LG4_D"))
  )
  (footprint "0603_1" (layer "B.Cu")
    (tedit 0)
    (at 103.261508 105.893812 -90)
    (fp_text reference "C941" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.762 0 90) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.762 0 270) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "IND_SMD_0603_1" (layer "B.Cu")
    (tedit 0)
    (at 120.874401 128.057496 -90)
    (fp_text reference "LB503" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.762 0 90) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1643 "PEX_PLLVDD"))
    (pad "2" smd rect (at -0.762 0 270) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 231.620408 138.303907)
    (fp_text reference "R577" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1022 "PS5_NVVDD_UG3"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 984 "PS5_NVVDD_UG3_R"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 249.286108 109.488115 180)
    (fp_text reference "C509" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 931 "PS5_NVVDD_FB"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 926 "PS5_NVVDD_CP"))
  )
  (footprint "0603_1" (layer "B.Cu")
    (tedit 0)
    (at 233.563508 131.725307)
    (fp_text reference "C523" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.762 0 180) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1030 "12V_PH4"))
    (pad "2" smd rect (at -0.762 0) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 126.096108 56.198915 180)
    (fp_text reference "C763" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 52.232908 66.371107 -90)
    (fp_text reference "R840" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1798 "GPIO11_RASTERSYNC1"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1095 "GPIO11_RASTERSYNC1_R"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 30.634805 108.7744 90)
    (fp_text reference "C1162" (at 0 -1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 242.390287 102.757115)
    (fp_text reference "R538" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 954 "PS5_NVVDD_ISEN1"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 8 "PS5_NVVDD_PHASE1"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 177.124708 68.316214 90)
    (fp_text reference "C545" (at 0 -0.7874 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0 90) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.9525 0 90) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 168.579615 104.04741)
    (fp_text reference "R647" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 749 "FBB_VREF1"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 42.784108 153.518812)
    (fp_text reference "C1124" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 171.545801 110.452299 180)
    (fp_text reference "C610" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 247.482708 110.109907 -90)
    (fp_text reference "C512" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 928 "PS5_NVVDD_VAMP_CSREF"))
  )
  (footprint "0603_1" (layer "B.Cu")
    (tedit 0)
    (at 28.839508 79.172707 90)
    (fp_text reference "C1166" (at 0 -1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.762 0 270) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "2" smd rect (at -0.762 0 90) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1046 "PS3_VCC5"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 30.211108 91.822415 90)
    (fp_text reference "R875" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1844 "DVIA_D3"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 160.373408 142.198718 -90)
    (fp_text reference "C694" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "IND_SMD_0402_1" (layer "B.Cu")
    (tedit 0)
    (at 16.063308 111.227812 -90)
    (fp_text reference "LB515" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.6858 0.5334) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.6858 0.5334) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1666 "NVIO_PLLVDD"))
  )
  (footprint "GEOM0013_1" (layer "B.Cu")
    (tedit 0)
    (at -99.585889 0.01)
    (fp_text reference "MEC504" (at -1.905 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 109.103508 128.931612 180)
    (fp_text reference "C893" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1484 "GV_PLLAVDD"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0603_1" (layer "B.Cu")
    (tedit 0)
    (at 25.791508 78.715507 180)
    (fp_text reference "C1187" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.762 0) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1044 "12V_PS3_R"))
    (pad "2" smd rect (at -0.762 0 180) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0603_1" (layer "B.Cu")
    (tedit 0)
    (at 128.097603 125.578812 90)
    (fp_text reference "C751" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.762 0 270) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1573 "FBABCD_MPLL_AVDD"))
    (pad "2" smd rect (at -0.762 0 90) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 67.198613 112.75961)
    (fp_text reference "C1041" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "IND_SMD_0402_1" (layer "B.Cu")
    (tedit 0)
    (at 40.896405 107.1488 180)
    (fp_text reference "LB507" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.6858 0.5334) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1661 "NVIO_GV_PLLAVDD"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.6858 0.5334) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 249.984608 92.202907 90)
    (fp_text reference "R511" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2003 "PS5_NVVDD_PGOOD_R"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 167.726708 100.247595 180)
    (fp_text reference "C643" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 88.466999 152.807815 -90)
    (fp_text reference "C987" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2059 "PEX_TX_C8"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1149 "PEX_TX8"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 167.979209 79.806716 90)
    (fp_text reference "R653" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2017 "FBC0_CLK0_R"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 616 "FBC0_CLK0*"))
  )
  (footprint "GEOM0017_1" (layer "B.Cu")
    (tedit 0)
    (at 198.359108 62.548407 90)
    (fp_text reference "U508" (at 2.07645 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 2.286 0.0381 90) (size 1.397 2.9972) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1913 "5V_ADJ"))
    (pad "2" smd rect (at 0 0 90) (size 1.4986 2.0066) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1914 "5V"))
    (pad "3" smd rect (at -2.286 0.0381 90) (size 1.397 2.9972) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1001 "5V_INPUT"))
    (pad "4" smd rect (at 0 -6.2484 90) (size 5.9944 6.5024) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1914 "5V"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 100.467 152.807815 -90)
    (fp_text reference "C960" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2048 "PEX_TX_C11"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1126 "PEX_TX11"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 157.947708 107.265412 180)
    (fp_text reference "R689" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 739 "FBB_CMD<5>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 173.816612 95.529316 180)
    (fp_text reference "C572" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 72.679908 72.670612 180)
    (fp_text reference "C1010" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 128.432908 100.407412)
    (fp_text reference "C748" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1573 "FBABCD_MPLL_AVDD"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 157.947708 139.167812 180)
    (fp_text reference "R694" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 871 "FBA_CMD<3>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 123.048108 118.085812 90)
    (fp_text reference "C785" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 115.682108 105.004812 90)
    (fp_text reference "C848" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 170.241308 71.680012 180)
    (fp_text reference "R630" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 562 "FBC_VREF4"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 37.670605 96.2522 180)
    (fp_text reference "R851" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1790 "2V5"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1791 "DR_VREF"))
  )
  (footprint "DIODE_SMD_SMA_1" (layer "B.Cu")
    (tedit 0)
    (at 38.135908 82.931907 -90)
    (fp_text reference "D519" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -1.880108 0 270) (size 2.159 2.032) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 989 "PS3_FBVDDQ_PHASE"))
    (pad "2" smd rect (at 1.880108 0 270) (size 2.159 2.032) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 27.036108 133.351212)
    (fp_text reference "R887" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1996 "PS1_1V15_CP_RC"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1958 "PS1_1V15_FB"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 26.464608 131.699907 90)
    (fp_text reference "C1181" (at 0 -1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1962 "PS1_1V15_CP"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1958 "PS1_1V15_FB"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 61.467307 123.767995 180)
    (fp_text reference "C1087" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 32.514405 109.0538 180)
    (fp_text reference "C1149" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 108.417708 65.711012 180)
    (fp_text reference "R741" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 353 "FBE_CMD<2>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 175.384808 84.910618 90)
    (fp_text reference "C561" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 118.730108 115.799812 -90)
    (fp_text reference "C820" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 69.897821 82.936504)
    (fp_text reference "C1026" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 116.850813 66.219215 -90)
    (fp_text reference "R733" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 410 "FBD_CMD<28>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 130.848702 137.663319 180)
    (fp_text reference "R709" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1203 "PEX_TSTCLK_OUT"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1134 "PEX_TSTCLK_OUT*"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 5.477604 147.549812 90)
    (fp_text reference "C1251" (at 0 -1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1930 "DACC_GREEN_CON"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 56.289821 152.807815 -90)
    (fp_text reference "C1117" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2045 "PEX_TX_C0"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1155 "PEX_TX0"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 163.688108 124.174903 90)
    (fp_text reference "C670" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 119.517508 58.17661 -90)
    (fp_text reference "C812" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0603_1" (layer "B.Cu")
    (tedit 0)
    (at 110.449708 125.934412 -90)
    (fp_text reference "C883" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.762 0 90) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at -0.762 0 270) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 24.877108 116.028412 180)
    (fp_text reference "C1196" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1693 "DACC_VDD"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 72.675819 112.75961 180)
    (fp_text reference "C1013" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 133.462413 72.594615 90)
    (fp_text reference "R705" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 479 "FBD_CMD<5>"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 122.413108 114.783812 -90)
    (fp_text reference "C795" (at 0 0.7874 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0 270) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.9525 0 270) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 87.716708 65.380812 -90)
    (fp_text reference "C990" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 250.860908 114.783507 180)
    (fp_text reference "R507" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 934 "PS5_NVVDD_SET_IMON"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 932 "PS5_NVVDD_FBRTN"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 172.044708 85.210795 180)
    (fp_text reference "C602" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 241.970908 137.338707 180)
    (fp_text reference "C518" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1975 "FAN_TACH"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 112.811908 97.130812 -90)
    (fp_text reference "C866" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 172.349508 131.649412 180)
    (fp_text reference "R618" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 823 "FBA_CMD<6>"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 63.414013 109.881612)
    (fp_text reference "R823" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 105 "FBG_CMD<6>"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "CAP_SMD_7343_1" (layer "B.Cu")
    (tedit 0)
    (at 136.510108 142.406312 90)
    (fp_text reference "C717" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 3.1115 0 90) (size 2.413 3.048) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -3.1115 0 90) (size 2.413 3.048) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 117.104508 63.080308 90)
    (fp_text reference "C831" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 431 "FBD_VREF3"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 104.861708 103.379212 -90)
    (fp_text reference "C923" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0603_1" (layer "B.Cu")
    (tedit 0)
    (at 42.657108 152.121812)
    (fp_text reference "C1125" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.762 0 180) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at -0.762 0) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 165.415308 123.574904 180)
    (fp_text reference "R674" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 798 "FBA_CMD<27>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 33.055908 128.220615)
    (fp_text reference "R863" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1945 "I2C1_SDA_UC"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 119.517508 63.080308 90)
    (fp_text reference "R729" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 407 "FBD_CMD<25>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 139.354908 60.097612 -90)
    (fp_text reference "C712" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0603_1" (layer "B.Cu")
    (tedit 0)
    (at 26.045508 141.351907)
    (fp_text reference "C1186" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.762 0 180) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1049 "PS1_VCC12"))
    (pad "2" smd rect (at -0.762 0) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 71.047399 87.642616)
    (fp_text reference "R776" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 26 "FBF_CMD<24>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 244.714108 113.221407)
    (fp_text reference "R535" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 936 "PS5_NVVDD_SET_LSSET"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 927 "NET0001"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 168.979893 124.174903 90)
    (fp_text reference "R641" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2016 "FBA1_CLK0_R"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 814 "FBA1_CLK0*"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 215.910508 130.429907 90)
    (fp_text reference "R601" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 996 "PS5_NVVDD_LG4_AC"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "SOT23_1" (layer "B.Cu")
    (tedit 0)
    (at 237.348108 111.633907 -90)
    (fp_text reference "D504" (at 1.23825 -1.23825 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 1.143 270) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1004 "PS5_NVVDD_BOOT5_RC"))
    (pad "2" smd rect (at -0.9525 1.143 270) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1005 "PS5_NVVDD_BOOT6_RC"))
    (pad "3" smd rect (at 0 -1.143 270) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 981 "12V_PEX6_F1"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 29.525308 115.919395 180)
    (fp_text reference "R877" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1804 "GPIO4_PS5_NVVDD_VID4"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 968 "PS5_NVVDD_VID4"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 118.557617 56.186215 180)
    (fp_text reference "C822" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 163.078508 93.727212 180)
    (fp_text reference "C673" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 112.913508 98.972312 180)
    (fp_text reference "C863" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 113.904108 115.799812 -90)
    (fp_text reference "C855" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "SO08_I190X150_1" (layer "B.Cu")
    (tedit 0)
    (at 39.685308 135.103507 90)
    (fp_text reference "U511" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 1.905 2.590495 90) (size 0.6096 2.032) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "2" smd rect (at 0.635 2.590495 90) (size 0.6096 2.032) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2091 "SNN_HDCP_NC"))
    (pad "3" smd rect (at -0.635 2.590495 90) (size 0.6096 2.032) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2090 "I2C4_SDA_R"))
    (pad "4" smd rect (at -1.905 2.590495 90) (size 0.6096 2.032) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "5" smd rect (at -1.905 -2.590495 90) (size 0.6096 2.032) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1812 "I2C4_SDA"))
    (pad "6" smd rect (at -0.635 -2.590495 90) (size 0.6096 2.032) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1810 "I2C4_SCL"))
    (pad "7" smd rect (at 0.635 -2.590495 90) (size 0.6096 2.032) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "8" smd rect (at 1.905 -2.590495 90) (size 0.6096 2.032) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 251.000608 92.202907 -90)
    (fp_text reference "R506" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2003 "PS5_NVVDD_PGOOD_R"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 61.097 72.591618)
    (fp_text reference "C1093" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 237.170308 129.693307)
    (fp_text reference "R556" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 941 "PS5_NVVDD_DRV_OD1"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1029 "PS5_NVVDD_DRV_PHASE4"))
  )
  (footprint "IND_SMD_0603_1" (layer "B.Cu")
    (tedit 0)
    (at 6.823804 143.98891 -90)
    (fp_text reference "L505" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.762 0 90) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1691 "DACC_RED"))
    (pad "2" smd rect (at -0.762 0 270) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1933 "DACC_RED_CON"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 165.872508 109.221212 90)
    (fp_text reference "R671" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 743 "FBB_CMD<2>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 4.836508 68.225612 -90)
    (fp_text reference "C1252" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1954 "DACB_PB_F"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 62.71371 82.865105)
    (fp_text reference "C1071" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 61.467307 99.237716)
    (fp_text reference "C1080" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 121.778108 111.481812 90)
    (fp_text reference "C802" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 122.413108 121.387812 -90)
    (fp_text reference "C796" (at 0 0.7874 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0 270) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.9525 0 270) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 173.483415 108.650906 180)
    (fp_text reference "C591" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 166.277917 105.448499)
    (fp_text reference "C651" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 249.984608 97.536907 90)
    (fp_text reference "R513" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 943 "NET0002"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 68.672804 107.443898 180)
    (fp_text reference "C1032" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 104.544691 63.080308 90)
    (fp_text reference "C931" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 359 "FBE_VREF1"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 64.669815 84.247906 180)
    (fp_text reference "C1051" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 129.626708 108.738612)
    (fp_text reference "C740" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 250.746608 125.349907 -90)
    (fp_text reference "R510" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1988 "FAN_CUTOFF_RC_Q"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 170.781312 133.89241)
    (fp_text reference "R629" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 879 "FBA_VREF1"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 17.638108 108.687812 180)
    (fp_text reference "C1223" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1666 "NVIO_PLLVDD"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 93.457108 67.641412 -90)
    (fp_text reference "R761" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 279 "FBE_CMD<27>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 61.491208 130.556907 90)
    (fp_text reference "R828" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1994 "THERM_SHDN_D*"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 125.946197 102.546016 90)
    (fp_text reference "C766" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 106.538108 115.926812 -90)
    (fp_text reference "C913" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 176.111197 133.275012 90)
    (fp_text reference "C550" (at 0 -0.7874 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0 90) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.9525 0 90) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 99.781708 57.684612)
    (fp_text reference "R756" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 302 "FBE_VREF4"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 51.064508 81.712707 180)
    (fp_text reference "C1120" (at 0.7874 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0 180) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.9525 0 180) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 252.524608 110.109907 -90)
    (fp_text reference "R504" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 980 "NET0006"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 952 "NET0004"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 171.110013 118.969402 180)
    (fp_text reference "R624" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 821 "FBA_VREF3"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 170.628404 78.805906 180)
    (fp_text reference "C624" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2017 "FBC0_CLK0_R"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 163.876119 143.499706)
    (fp_text reference "C669" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 248.574908 114.783507 180)
    (fp_text reference "C511" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2082 "PS5_NVVDD_FB_RC"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 999 "NVVDD_SENSE_R"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 8.243715 147.549812 -90)
    (fp_text reference "C1235" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1689 "DACC_GREEN"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 59.565913 70.625912 90)
    (fp_text reference "C1098" (at 0 -1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 175.461008 79.154419 90)
    (fp_text reference "R612" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 621 "FBC_ZQ1"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 128.661508 113.513812)
    (fp_text reference "C746" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 168.579615 118.969402)
    (fp_text reference "C640" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 821 "FBA_VREF3"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 173.483415 90.525516 180)
    (fp_text reference "C587" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 94.625508 57.87181 90)
    (fp_text reference "C975" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 236.865508 146.889107)
    (fp_text reference "R559" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 942 "PS5_NVVDD_DRV_ODN"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1024 "PS5_NVVDD_DRV_PHASE3"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 35.765605 103.01871)
    (fp_text reference "C1140" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1662 "NVIO_GV_PLLVDD"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 99.781708 60.491312 180)
    (fp_text reference "C962" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 302 "FBE_VREF4"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 108.417708 69.216212 180)
    (fp_text reference "C898" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 168.579615 117.958812)
    (fp_text reference "R648" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 742 "FBB_CMD<0>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 122.870308 140.463212)
    (fp_text reference "R727" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1972 "PEX_PLLVDD_OP"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1971 "PEX_PLLVDD_OP_ADJ"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 166.024908 79.350812 90)
    (fp_text reference "R670" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 613 "FBC_CMD<2>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 66.371005 107.443898 180)
    (fp_text reference "C1045" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 114 "FBG_VREF1"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 59.565913 88.903218 -90)
    (fp_text reference "R830" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 44 "FBF_ZQ2"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 227.340508 114.859707 90)
    (fp_text reference "R581" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1033 "PS5_NVVDD_LG5"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 997 "PS5_NVVDD_LG5_AC"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 126.769208 124.35471 -90)
    (fp_text reference "C759" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1573 "FBABCD_MPLL_AVDD"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "IND_SMD_0402_1" (layer "B.Cu")
    (tedit 0)
    (at 24.765297 100.108911)
    (fp_text reference "LB511" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.6858 0.5334) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at -0.5334 0) (size 0.6858 0.5334) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1673 "DACB_VDD"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 171.545801 65.685612 180)
    (fp_text reference "C606" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 8.243715 143.866812 -90)
    (fp_text reference "C1234" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1691 "DACC_RED"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 97.827915 61.379016 90)
    (fp_text reference "C969" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 239.761108 134.341507 90)
    (fp_text reference "C519" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1973 "FAN_PWM"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 101.534308 68.961907 90)
    (fp_text reference "C954" (at 0 -0.7874 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0 90) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.9525 0 90) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 136.231013 72.924815 -90)
    (fp_text reference "R703" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 481 "FBD_CMD<3>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 61.492199 92.49201)
    (fp_text reference "C1074" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 22.01402 112.017904 -90)
    (fp_text reference "C1210" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1701 "IFPAB_IOVDD"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 130.972908 57.938612 -90)
    (fp_text reference "R708" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 433 "FBD_CMD<6>"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 77.714213 107.672015)
    (fp_text reference "R769" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 94 "FBG_CMD<5>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 242.390287 104.154115)
    (fp_text reference "R539" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 955 "PS5_NVVDD_ISEN2"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 14 "PS5_NVVDD_PHASE2"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 75.466999 152.807815 -90)
    (fp_text reference "C1002" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2056 "PEX_TX_C5"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1145 "PEX_TX5"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 162.274801 100.247595)
    (fp_text reference "C680" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 252.524608 113.170607 -90)
    (fp_text reference "R505" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1042 "NET0008"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 960 "PS5_NVVDD_SET_TRDET"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 16.622108 100.686812 180)
    (fp_text reference "C1227" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 62.575813 112.75961)
    (fp_text reference "C1072" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 155.331508 107.773615 90)
    (fp_text reference "C696" (at 0 -0.7874 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0 90) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.9525 0 90) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0603_1" (layer "B.Cu")
    (tedit 0)
    (at 27.874308 117.349212 180)
    (fp_text reference "C1171" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.762 0) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1698 "IFPAB_PLLVDD"))
    (pad "2" smd rect (at -0.762 0 180) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 157.947708 108.281412 180)
    (fp_text reference "R690" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 740 "FBB_CMD<4>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 59.565913 91.1531 -90)
    (fp_text reference "C1100" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 169.651012 145.901504 180)
    (fp_text reference "C636" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 880 "FBA_VREF2"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 165.477309 104.04741 180)
    (fp_text reference "C656" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 124.826108 109.068812 -90)
    (fp_text reference "C773" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 34.021108 91.822415 90)
    (fp_text reference "R857" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1841 "DVIA_D0"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 177.200908 113.356002 90)
    (fp_text reference "C542" (at 0 -0.7874 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0 90) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.9525 0 90) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 29.131608 133.821112 90)
    (fp_text reference "R879" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1960 "PS1_1V15_FB_SEN"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 27.848908 136.069012 -90)
    (fp_text reference "C1172" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1959 "PS1_1V15_FB_RC"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1960 "PS1_1V15_FB_SEN"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 116.444413 60.402615)
    (fp_text reference "R734" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 360 "FBE_VREF2"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 24.432608 91.567907)
    (fp_text reference "R896" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1967 "PS3_FBVDDQ_UG"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 992 "PS3_FBVDDQ_UG_R"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 67.198613 114.160699)
    (fp_text reference "R794" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 166 "FBG_CMD<23>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 169.651012 116.056504 180)
    (fp_text reference "R635" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 750 "FBB_VREF2"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 28.941108 91.822415 90)
    (fp_text reference "R882" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1857 "DVIB_D4"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 162.773708 105.411212 180)
    (fp_text reference "C675" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 173.483415 105.448499 180)
    (fp_text reference "C590" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 69.473412 97.836602)
    (fp_text reference "C1028" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 15.80372 83.770107)
    (fp_text reference "R919" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1055 "PS3_FBVDDQ_FB"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 164.221508 139.523412)
    (fp_text reference "R680" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 874 "FBA_CMD<1>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 244.841108 97.536907 90)
    (fp_text reference "R532" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 970 "PS5_NVVDD_VID6"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 157.947708 109.322812 180)
    (fp_text reference "R691" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 741 "FBB_CMD<3>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 162.274801 104.04741)
    (fp_text reference "C681" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 65.970701 103.240706 -90)
    (fp_text reference "R809" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2026 "FBG0_CLK0_R"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 106 "FBG0_CLK0"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 26.756708 123.673507 90)
    (fp_text reference "R891" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1050 "GPU_RST*"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1051 "GPU_RST_R*"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 128.204308 128.931612 -90)
    (fp_text reference "R718" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1208 "GPU_TESTMODE"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 168.131609 94.406103 90)
    (fp_text reference "R651" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2015 "FBB1_CLK0_R"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 684 "FBB1_CLK0*"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 21.448108 102.845812 180)
    (fp_text reference "C1212" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1722 "IFPCD_PLLVDD"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0603_1" (layer "B.Cu")
    (tedit 0)
    (at 232.293508 99.162507)
    (fp_text reference "C528" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.762 0 180) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1005 "PS5_NVVDD_BOOT6_RC"))
    (pad "2" smd rect (at -0.762 0) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 13 "PS5_NVVDD_PHASE6"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 61.707108 138.659507 180)
    (fp_text reference "R826" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1180 "JTAG_TRST*"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2004 "JTAG_TRST2"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 98.435508 121.311815)
    (fp_text reference "C967" (at -0.7874 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.9525 0) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 129.124804 66.182614 -90)
    (fp_text reference "C743" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 111.364108 144.374812 180)
    (fp_text reference "C874" (at 0.7874 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0 180) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at -0.9525 0 180) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "SOT23_1" (layer "B.Cu")
    (tedit 0)
    (at 30.566708 85.167107 90)
    (fp_text reference "D520" (at -1.23825 1.23825 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1968 "PS3_FBVDDQ_LG"))
    (pad "2" smd rect (at -0.9525 1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 990 "PS3_FBVDDQ_LG_G"))
    (pad "3" smd rect (at 0 -1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2089 "PS3_FBVDDQ_LG_D"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 63.414013 117.363106)
    (fp_text reference "C1066" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 44.054108 150.750212)
    (fp_text reference "C1123" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2028 "3V3_AUX"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 94.625508 60.123012 -90)
    (fp_text reference "C976" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 20.525605 95.2108 -90)
    (fp_text reference "C1215" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1674 "DACB_VREF"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 221.384208 101.715207 90)
    (fp_text reference "R587" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1037 "PS5_NVVDD_LG6"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2086 "PS5_NVVDD_LG6_D"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 249.286108 110.504115 180)
    (fp_text reference "R515" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 931 "PS5_NVVDD_FB"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1039 "PS5_NVVDD_CP_RC"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 166.277917 90.525516)
    (fp_text reference "R667" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 671 "FBB_CMD<26>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 102.651908 108.611612)
    (fp_text reference "R751" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1595 "FBG_DEBUG"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 66.971512 103.240706 -90)
    (fp_text reference "R797" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2026 "FBG0_CLK0_R"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 107 "FBG0_CLK0*"))
  )
  (footprint "SOT23_1" (layer "B.Cu")
    (tedit 0)
    (at 31.150908 119.076107 90)
    (fp_text reference "Q512" (at -1.23825 1.23825 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1794 "FAN_PWM_NVIO"))
    (pad "2" smd rect (at -0.9525 1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "3" smd rect (at 0 -1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1979 "FAN_PWM_NVIO_R"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 168.579615 90.525516)
    (fp_text reference "R646" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 667 "FBB_CMD<25>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 16.622108 99.137107)
    (fp_text reference "R916" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1771 "MIOB_CTL3"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 169.752612 85.210795 180)
    (fp_text reference "C633" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 620 "FBC_VREF2"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0603_1" (layer "B.Cu")
    (tedit 0)
    (at 233.512708 119.838107 180)
    (fp_text reference "R570" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.762 0) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 981 "12V_PEX6_F1"))
    (pad "2" smd rect (at -0.762 0 180) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1034 "12V_PH5"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 106.436508 125.455622 90)
    (fp_text reference "C915" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 8.900508 74.397507 -90)
    (fp_text reference "R938" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1670 "DACB_PR"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 244.714108 110.123115)
    (fp_text reference "R534" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 927 "NET0001"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1041 "NET0007"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 132.496908 130.379412 180)
    (fp_text reference "C727" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 171.181616 105.448499 180)
    (fp_text reference "C616" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "SOT23_1" (layer "B.Cu")
    (tedit 0)
    (at 60.945108 133.795407 90)
    (fp_text reference "Q507" (at -1.23825 1.23825 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1998 "THERM_SHDN_Q"))
    (pad "2" smd rect (at -0.9525 1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1982 "GPU_RST_R_MOS"))
    (pad "3" smd rect (at 0 -1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1994 "THERM_SHDN_D*"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 12.761308 80.391907)
    (fp_text reference "R931" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1109 "PS3_FBVDDQ_VSEN"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1477 "FBVDDQ_SENSE"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 160.005108 132.538412 180)
    (fp_text reference "R684" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 818 "FBA_CMD<10>"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 65.598413 96.800815)
    (fp_text reference "R812" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 115 "FBG_VREF2"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 102.766208 115.926812)
    (fp_text reference "C950" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 119.365108 112.484807 90)
    (fp_text reference "C815" (at 0 -0.7874 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0 90) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.9525 0 90) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 66.233921 92.527519 180)
    (fp_text reference "R806" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "FBF_CMD<25>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 19.9109 108.681411 180)
    (fp_text reference "R908" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1793 "NVIO_EXT_REFCLKA"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1094 "NVIO_EXT_REFCLKA_R"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 217.917108 58.192307 -90)
    (fp_text reference "R596" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2080 "SPDIF_GND"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 103.617413 76.150615 135)
    (fp_text reference "C939" (at 0.556776 -0.556776 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0 135) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.9525 0 135) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 127.723715 58.17661 -90)
    (fp_text reference "C756" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 143.493609 56.275115 180)
    (fp_text reference "C706" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 133.039401 68.962212 -90)
    (fp_text reference "C726" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "SOT23_1" (layer "B.Cu")
    (tedit 0)
    (at 224.825908 89.548607 90)
    (fp_text reference "D508" (at -1.23825 1.23825 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1019 "PS5_NVVDD_LG2"))
    (pad "2" smd rect (at -0.9525 1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 994 "PS5_NVVDD_LG2_AC"))
    (pad "3" smd rect (at 0 -1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2088 "PS5_NVVDD_LG2_D"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 39.736108 98.527812 -90)
    (fp_text reference "C1131" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1664 "NVIO_SP_PLLVDD"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 227.365908 140.996307 90)
    (fp_text reference "R578" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1023 "PS5_NVVDD_LG3"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 995 "PS5_NVVDD_LG3_AC"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 169.758708 88.012212 180)
    (fp_text reference "R633" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 612 "FBC_CMD<0>"))
  )
  (footprint "SOT23_1" (layer "B.Cu")
    (tedit 0)
    (at 18.425508 78.690107 90)
    (fp_text reference "Q515" (at -1.23825 1.23825 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2003 "PS5_NVVDD_PGOOD_R"))
    (pad "2" smd rect (at -0.9525 1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "3" smd rect (at 0 -1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1990 "PS3_NVVDD_PGOOD*"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 78.928308 115.114012 180)
    (fp_text reference "C998" (at 0.7874 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0 180) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.9525 0 180) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 168.579615 60.679704)
    (fp_text reference "R644" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 537 "FBC_CMD<25>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 234.147708 100.534107)
    (fp_text reference "R562" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1035 "PS5_NVVDD_BOOT6"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1005 "PS5_NVVDD_BOOT6_RC"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 168.479615 135.293499)
    (fp_text reference "C641" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 879 "FBA_VREF1"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 31.633508 113.488615 90)
    (fp_text reference "R868" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1792 "NVIO_EXTDEV_RST*"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 177.200908 128.626812 90)
    (fp_text reference "C543" (at 0 -0.7874 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0 90) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.9525 0 90) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "GEOM0009_1" (layer "B.Cu")
    (tedit 0)
    (at 233.855608 128.969407 90)
    (fp_text reference "U505" (at -1.353464 1.35349 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.750113 1.376883 270) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1026 "PS5_NVVDD_BOOT4"))
    (pad "2" smd rect (at 0.249911 1.376883 270) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 948 "PS5_NVVDD_PWM4"))
    (pad "3" smd rect (at -0.249911 1.376883 270) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1029 "PS5_NVVDD_DRV_PHASE4"))
    (pad "4" smd rect (at -0.750087 1.376883 270) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1030 "12V_PH4"))
    (pad "5" smd rect (at -0.750087 -1.376909 90) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1028 "PS5_NVVDD_LG4"))
    (pad "6" smd rect (at -0.249911 -1.376909 90) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "7" smd rect (at 0.249911 -1.376909 90) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 11 "PS5_NVVDD_PHASE4"))
    (pad "8" smd rect (at 0.750113 -1.376909 90) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1027 "PS5_NVVDD_UG4"))
    (pad "9" smd rect (at 0 0 90) (size 1.850111 1.5494) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 131.811413 68.911615 -90)
    (fp_text reference "C729" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 28.991908 141.301412)
    (fp_text reference "R880" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 991 "12V_F"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1049 "PS1_VCC12"))
  )
  (footprint "0603_1" (layer "B.Cu")
    (tedit 0)
    (at 199.883108 57.404907 -90)
    (fp_text reference "C533" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.762 0 90) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1913 "5V_ADJ"))
    (pad "2" smd rect (at -0.762 0 270) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 177.200908 100.737612 -90)
    (fp_text reference "C540" (at 0 0.7874 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0 270) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.9525 0 270) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 115.682108 118.212812 90)
    (fp_text reference "C849" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "IND_SMD_0402_1" (layer "B.Cu")
    (tedit 0)
    (at 103.934608 125.431695 90)
    (fp_text reference "LB505" (at 0 -1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.6858 0.5334) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1282 "FBEFGH_MPLL_AVDD"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.6858 0.5334) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 51.928108 145.263507 90)
    (fp_text reference "R841" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1175 "JTAG_TDO_GPU"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1910 "JTAG_TDI_NVIO"))
  )
  (footprint "SOT23_1" (layer "B.Cu")
    (tedit 0)
    (at 16.876108 89.535907)
    (fp_text reference "Q516" (at 1.23825 1.23825 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 1.143) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1990 "PS3_NVVDD_PGOOD*"))
    (pad "2" smd rect (at -0.9525 1.143) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "3" smd rect (at 0 -1.143) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1057 "PS3_FS_DIS"))
  )
  (footprint "LTPT28C49P18C10P_1" (layer "B.Cu")
    (tedit 0)
    (at 115.351908 116.358612)
    (fp_text reference "TP503" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 0.7112 0.7112) (drill 0.254) (layers *.Cu *.Mask)
      (net 1655 "NVVDD_SENSE_GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 99.070508 71.286515 180)
    (fp_text reference "C964" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 69.473412 108.845012)
    (fp_text reference "C1029" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 244.714108 112.205407)
    (fp_text reference "C515" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 929 "PS5_NVVDD_VAMP_CSSUM"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 927 "NET0001"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 55.992108 145.263812 -90)
    (fp_text reference "R834" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1562 "JTAG_TMS"))
  )
  (footprint "SOT23_1" (layer "B.Cu")
    (tedit 0)
    (at 224.851308 140.805807 90)
    (fp_text reference "D506" (at -1.23825 1.23825 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1023 "PS5_NVVDD_LG3"))
    (pad "2" smd rect (at -0.9525 1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 995 "PS5_NVVDD_LG3_AC"))
    (pad "3" smd rect (at 0 -1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2084 "PS5_NVVDD_LG3_D"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 124.546708 67.235012 -90)
    (fp_text reference "R722" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 417 "FBD_CMD<24>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 107.808108 109.322812 -90)
    (fp_text reference "C903" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 172.070108 88.012212)
    (fp_text reference "R619" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 691 "FBB_VREF3"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 221.409608 140.297807 90)
    (fp_text reference "R584" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1023 "PS5_NVVDD_LG3"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2084 "PS5_NVVDD_LG3_D"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 247.952608 97.536907 -90)
    (fp_text reference "R522" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 966 "PS5_NVVDD_VID2"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0603_1" (layer "B.Cu")
    (tedit 0)
    (at 36.484908 110.084812 180)
    (fp_text reference "C1138" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.762 0) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at -0.762 0 180) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 215.910508 79.210807 90)
    (fp_text reference "R597" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 993 "PS5_NVVDD_LG1_AC"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 59.565913 68.224012 -90)
    (fp_text reference "C1097" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 244.714108 111.189407)
    (fp_text reference "C514" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 929 "PS5_NVVDD_VAMP_CSSUM"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 927 "NET0001"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 175.461008 64.231411 90)
    (fp_text reference "R611" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 564 "FBC_ZQ2"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 118.730108 122.403812 -90)
    (fp_text reference "C821" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 70.089413 73.73792 -90)
    (fp_text reference "R782" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 221 "FBF_CMD<3>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 167.739408 130.09262 180)
    (fp_text reference "C642" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 61.467307 114.160699)
    (fp_text reference "C1084" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "SOT23_1" (layer "B.Cu")
    (tedit 0)
    (at 67.739608 138.938907 90)
    (fp_text reference "Q504" (at -1.23825 1.23825 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1997 "THERM_SHDN_R"))
    (pad "2" smd rect (at -0.9525 1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "3" smd rect (at 0 -1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1981 "THERM_SHDN"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 33.868708 97.334012 -90)
    (fp_text reference "C1145" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 59.444705 73.920495 -90)
    (fp_text reference "R833" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 231 "FBF_ZQ1"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 162.274801 145.901504 180)
    (fp_text reference "R683" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 872 "FBA_CMD<0>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 248.714608 121.285907 -90)
    (fp_text reference "R519" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1050 "GPU_RST*"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1955 "GPU_RST_RC*"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 66.371005 77.5308 180)
    (fp_text reference "C1044" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 229 "FBF_VREF1"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 15.021908 109.805412 90)
    (fp_text reference "R925" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1679 "DACA_GREEN"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 54.722108 139.116707 -90)
    (fp_text reference "R837" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1912 "JTAG_TRST_3V3*"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 227.340508 128.118507 90)
    (fp_text reference "R582" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1028 "PS5_NVVDD_LG4"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 996 "PS5_NVVDD_LG4_AC"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 129.017108 121.095407 180)
    (fp_text reference "R716" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1558 "FBA_DEBUG"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 167.015508 101.550412 180)
    (fp_text reference "R661" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 692 "FBB_VREF4"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 202.042108 59.690907 180)
    (fp_text reference "R608" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1874 "SPDIF_IN_GPU"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 93.483016 152.807815 -90)
    (fp_text reference "C978" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2044 "PEX_TX_C9*"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1185 "PEX_TX9*"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 64.669815 99.237716 180)
    (fp_text reference "C1052" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "DIODE_SMD_SMA_1" (layer "B.Cu")
    (tedit 0)
    (at 203.058108 91.440907 -90)
    (fp_text reference "D513" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -1.880108 0 270) (size 2.159 2.032) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 14 "PS5_NVVDD_PHASE2"))
    (pad "2" smd rect (at 1.880108 0 270) (size 2.159 2.032) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 248.498708 112.395907 90)
    (fp_text reference "R520" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 931 "PS5_NVVDD_FB"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2082 "PS5_NVVDD_FB_RC"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 123.048108 104.877812 90)
    (fp_text reference "C783" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 130.363308 99.289812 180)
    (fp_text reference "R711" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1267 "FBD_DEBUG"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 168.004609 64.484903 90)
    (fp_text reference "R652" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2014 "FBC1_CLK0_R"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 554 "FBC1_CLK0*"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 57.724413 100.712212 -90)
    (fp_text reference "C1111" (at 0 0.7874 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0 270) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.9525 0 270) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "IND_SMD_0402_1" (layer "B.Cu")
    (tedit 0)
    (at 5.446108 135.586412 90)
    (fp_text reference "LB519" (at 0 -1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.6858 0.5334) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1987 "GPIO0_DVIAB_HPD_R"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.6858 0.5334) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1931 "GPIO0_DVIAB_HPD_CON"))
  )
  (footprint "SOT23_1" (layer "B.Cu")
    (tedit 0)
    (at 6.335108 64.389907 -90)
    (fp_text reference "D531" (at 1.23825 -1.23825 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 1.143 270) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "2" smd rect (at -0.9525 1.143 270) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "3" smd rect (at 0 -1.143 270) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1669 "DACB_PB"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 33.944908 84.582907 90)
    (fp_text reference "R860" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1968 "PS3_FBVDDQ_LG"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2089 "PS3_FBVDDQ_LG_D"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 172.044708 86.211504)
    (fp_text reference "R620" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 620 "FBC_VREF2"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 66.217615 122.366906 180)
    (fp_text reference "R807" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 162 "FBG_CMD<25>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 108.417708 124.918412 180)
    (fp_text reference "C899" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 157.947708 137.110412 180)
    (fp_text reference "R692" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 869 "FBA_CMD<5>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 99.781708 59.475312 180)
    (fp_text reference "R757" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 302 "FBE_VREF4"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 252.994508 141.311521 -90)
    (fp_text reference "C502" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 983 "12V_PEX6_F2"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 14.412308 111.863015)
    (fp_text reference "C1230" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 124.521308 60.148412 -90)
    (fp_text reference "C778" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 104.544691 67.793812 90)
    (fp_text reference "C933" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 97.483008 152.807815 -90)
    (fp_text reference "C971" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2031 "PEX_TX_C10*"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1162 "PEX_TX10*"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 138.567508 67.438212 90)
    (fp_text reference "R700" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 484 "FBD_CMD<1>"))
  )
  (footprint "0603_1" (layer "B.Cu")
    (tedit 0)
    (at 232.293508 77.851907)
    (fp_text reference "C526" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.762 0 180) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1006 "PS5_NVVDD_BOOT1_RC"))
    (pad "2" smd rect (at -0.762 0) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 8 "PS5_NVVDD_PHASE1"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 61.438401 93.802802 180)
    (fp_text reference "C1088" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 165.445305 100.247595 180)
    (fp_text reference "C660" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 109.586108 105.004812 90)
    (fp_text reference "C887" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 125.461108 118.974812 90)
    (fp_text reference "C770" (at 0 -0.7874 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0 90) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.9525 0 90) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 103.134508 116.942812)
    (fp_text reference "C948" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 128.077308 111.862812 90)
    (fp_text reference "C752" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 164.221508 109.678412)
    (fp_text reference "R679" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 744 "FBB_CMD<1>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 31.328708 100.001012)
    (fp_text reference "C1156" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "GEOM0009_1" (layer "B.Cu")
    (tedit 0)
    (at 233.855608 103.544007 90)
    (fp_text reference "U504" (at -1.353464 1.35349 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.750113 1.376883 270) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1035 "PS5_NVVDD_BOOT6"))
    (pad "2" smd rect (at 0.249911 1.376883 270) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 950 "PS5_NVVDD_PWM6"))
    (pad "3" smd rect (at -0.249911 1.376883 270) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 942 "PS5_NVVDD_DRV_ODN"))
    (pad "4" smd rect (at -0.750087 1.376883 270) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1038 "12V_PH6"))
    (pad "5" smd rect (at -0.750087 -1.376909 90) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1037 "PS5_NVVDD_LG6"))
    (pad "6" smd rect (at -0.249911 -1.376909 90) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "7" smd rect (at 0.249911 -1.376909 90) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 13 "PS5_NVVDD_PHASE6"))
    (pad "8" smd rect (at 0.750113 -1.376909 90) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1036 "PS5_NVVDD_UG6"))
    (pad "9" smd rect (at 0 0 90) (size 1.850111 1.5494) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 133.039401 65.801614 -90)
    (fp_text reference "C725" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 74.577313 115.207712 90)
    (fp_text reference "C1006" (at 0 -1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 26.578908 93.955507 -90)
    (fp_text reference "R892" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1835 "NVIO_EXT_REFCLKB"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1074 "NVIO_EXT_REFCLKB_R"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 60.797813 97.836602 180)
    (fp_text reference "C1094" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 171.181616 135.293499 180)
    (fp_text reference "C618" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 13.523308 95.200615 -90)
    (fp_text reference "R928" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1686 "I2C1_SCL"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2001 "I2C1_SCL_R"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 112.8368 152.934612 180)
    (fp_text reference "C865" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2035 "PEX_TX_C14*"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1154 "PEX_TX14*"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 152.283508 109.729212 90)
    (fp_text reference "C700" (at 0 -0.7874 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0 90) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.9525 0 90) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 246.936608 94.869907 90)
    (fp_text reference "R526" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1806 "GPIO6_PS5_NVVDD_VID2"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 966 "PS5_NVVDD_VID2"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 80.483017 152.807815 -90)
    (fp_text reference "C996" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2041 "PEX_TX_C6*"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1179 "PEX_TX6*"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 138.643708 63.680714 180)
    (fp_text reference "R699" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2020 "FBD0_CLK0_R"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 486 "FBD0_CLK0*"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 168.479615 133.89241)
    (fp_text reference "R650" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 879 "FBA_VREF1"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 63.809212 94.916618)
    (fp_text reference "C1061" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 41 "FBF_VREF3"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "SOT23_1" (layer "B.Cu")
    (tedit 0)
    (at 224.825908 102.223207 90)
    (fp_text reference "D509" (at -1.23825 1.23825 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1037 "PS5_NVVDD_LG6"))
    (pad "2" smd rect (at -0.9525 1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 998 "PS5_NVVDD_LG6_AC"))
    (pad "3" smd rect (at 0 -1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2086 "PS5_NVVDD_LG6_D"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 126.629508 126.645612 -90)
    (fp_text reference "C761" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 101.712413 72.721615 90)
    (fp_text reference "R753" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 297 "FBE_CMD<10>"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0603_1" (layer "B.Cu")
    (tedit 0)
    (at 233.284108 145.720707 180)
    (fp_text reference "R571" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.762 0) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 981 "12V_PEX6_F1"))
    (pad "2" smd rect (at -0.762 0 180) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1025 "12V_PH3"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 31.346005 101.3068 180)
    (fp_text reference "C1155" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 107.747123 67.4343 90)
    (fp_text reference "C907" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 16.812608 86.995907)
    (fp_text reference "R915" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1057 "PS3_FS_DIS"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 172.298708 130.09262 180)
    (fp_text reference "C600" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 118.545704 100.509698 180)
    (fp_text reference "C823" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 169.651012 115.05582 180)
    (fp_text reference "C635" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 750 "FBB_VREF2"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "IND_SMD_0402_1" (layer "B.Cu")
    (tedit 0)
    (at 24.115616 108.7744 -90)
    (fp_text reference "LB512" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.6858 0.5334) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.6858 0.5334) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1683 "DACA_VDD"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 122.78852 68.682812 -90)
    (fp_text reference "C790" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 90.922696 56.224315 180)
    (fp_text reference "C983" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 162.274801 70.307116 180)
    (fp_text reference "C678" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 130.210908 63.094812 -90)
    (fp_text reference "R712" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 432 "FBD_VREF4"))
  )
  (footprint "SOT23_1" (layer "B.Cu")
    (tedit 0)
    (at 224.825908 114.669207 90)
    (fp_text reference "D510" (at -1.23825 1.23825 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1033 "PS5_NVVDD_LG5"))
    (pad "2" smd rect (at -0.9525 1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 997 "PS5_NVVDD_LG5_AC"))
    (pad "3" smd rect (at 0 -1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2087 "PS5_NVVDD_LG5_D"))
  )
  (footprint "0603_1" (layer "B.Cu")
    (tedit 0)
    (at 100.467508 123.369215)
    (fp_text reference "C959" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.762 0 180) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1282 "FBEFGH_MPLL_AVDD"))
    (pad "2" smd rect (at -0.762 0) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 193.977608 68.326907 90)
    (fp_text reference "C536" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1914 "5V"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 31.277908 67.793507 180)
    (fp_text reference "R871" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1079 "GPIO15_SWAPRDY"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 114.742816 124.855115 180)
    (fp_text reference "C851" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 246.377808 113.716707 90)
    (fp_text reference "R529" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 928 "PS5_NVVDD_VAMP_CSREF"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 936 "PS5_NVVDD_SET_LSSET"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 167.421908 68.911412 180)
    (fp_text reference "R657" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 545 "FBC_CMD<23>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 34.823697 112.39131 180)
    (fp_text reference "R855" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1814 "NVIO_TESTMODE"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 74.577313 106.01591 -90)
    (fp_text reference "C1005" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 66.270015 93.784616 180)
    (fp_text reference "R804" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 41 "FBF_VREF3"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 196.327108 58.039907 180)
    (fp_text reference "R610" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1914 "5V"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1913 "5V_ADJ"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 103.143601 58.17661 90)
    (fp_text reference "C944" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 166.277917 88.012212)
    (fp_text reference "R666" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 670 "FBB_CMD<28>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 63.827017 77.512614)
    (fp_text reference "C1060" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 127.723715 61.379016 90)
    (fp_text reference "C757" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 167.434608 70.307116 180)
    (fp_text reference "C647" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 35.138708 133.071507 -90)
    (fp_text reference "C1144" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1107 "PS1_1V15_LG"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 163.129308 135.293499 180)
    (fp_text reference "C671" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 102.296308 121.260812 -90)
    (fp_text reference "C952" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 126.096108 109.068812 -90)
    (fp_text reference "C764" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 112.750923 61.379016 90)
    (fp_text reference "C867" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 161.935508 139.523412)
    (fp_text reference "C684" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 106.817508 74.067612 -90)
    (fp_text reference "R743" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 351 "FBE_CMD<3>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 166.277917 89.124402)
    (fp_text reference "C650" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 97.827915 58.17661 -90)
    (fp_text reference "C968" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 4.049108 130.429907 -90)
    (fp_text reference "C1255" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1925 "DDC_5V"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 246.263508 119.431707)
    (fp_text reference "C513" (at -0.7874 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1955 "GPU_RST_RC*"))
    (pad "2" smd rect (at -0.9525 0) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 29.449108 113.361107 90)
    (fp_text reference "R878" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1797 "NET0012"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 968 "PS5_NVVDD_VID4"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 120.000108 109.195812 -90)
    (fp_text reference "C808" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 69.009608 124.905407)
    (fp_text reference "R785" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 164 "FBG_CMD<28>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 245.920608 97.536907 -90)
    (fp_text reference "R531" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 968 "PS5_NVVDD_VID4"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 171.545801 140.297299 180)
    (fp_text reference "C613" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "GEOM0013_1" (layer "B.Cu")
    (tedit 0)
    (at -99.086093 0.634916)
    (fp_text reference "MEC501" (at -1.905 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 27.418099 103.261305 -90)
    (fp_text reference "C1175" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 17.765108 129.413907)
    (fp_text reference "R914" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2012 "DACC_VSYNC_BUF_R"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2013 "DACC_VSYNC_BUF"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 101.483 152.807815 -90)
    (fp_text reference "C956" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2032 "PEX_TX_C11*"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1165 "PEX_TX11*"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 172.019308 70.307116 180)
    (fp_text reference "C603" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 133.039401 58.17661 90)
    (fp_text reference "C724" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 177.200908 105.030212 -90)
    (fp_text reference "C541" (at 0 0.7874 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0 270) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.9525 0 270) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 51.064508 71.806707 180)
    (fp_text reference "C1118" (at 0.7874 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0 180) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.9525 0 180) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 118.16572 65.380812 90)
    (fp_text reference "C826" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 120.818496 56.198915 180)
    (fp_text reference "C806" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 50.886708 145.263812 90)
    (fp_text reference "R842" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1175 "JTAG_TDO_GPU"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1970 "JTAG_TDO"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 115.936108 114.567607 -90)
    (fp_text reference "C846" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 157.947708 77.166412 180)
    (fp_text reference "R686" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 609 "FBC_CMD<5>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 166.277917 120.370516)
    (fp_text reference "R669" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 800 "FBA_CMD<26>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 171.104908 138.495906 180)
    (fp_text reference "C619" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2019 "FBA0_CLK0_R"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 110.945008 102.538396 90)
    (fp_text reference "C878" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 165.477309 74.20241 180)
    (fp_text reference "C655" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 170.012708 100.247595 180)
    (fp_text reference "C631" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 692 "FBB_VREF4"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 18.349308 110.643612 90)
    (fp_text reference "C1221" (at 0 -1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1666 "NVIO_PLLVDD"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0603_1" (layer "B.Cu")
    (tedit 0)
    (at 233.563508 84.989307)
    (fp_text reference "C520" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.762 0 180) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1016 "12V_PH1"))
    (pad "2" smd rect (at -0.762 0) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 68.925813 103.633212 -90)
    (fp_text reference "R786" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 98 "FBG_CMD<2>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 145.120708 62.078812 -90)
    (fp_text reference "R697" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 490 "FBD_VREF2"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 166.277917 60.679704)
    (fp_text reference "R665" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 541 "FBC_CMD<26>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 66.353022 78.885916 180)
    (fp_text reference "R803" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 229 "FBF_VREF1"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 129.461608 123.190907 180)
    (fp_text reference "C741" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 26.417415 103.261305 -90)
    (fp_text reference "C1182" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "SOT23_1" (layer "B.Cu")
    (tedit 0)
    (at 251.254608 122.111407 180)
    (fp_text reference "Q501" (at -1.23825 -1.23825 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 1.143 180) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1955 "GPU_RST_RC*"))
    (pad "2" smd rect (at -0.9525 1.143 180) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "3" smd rect (at 0 -1.143 180) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1988 "FAN_CUTOFF_RC_Q"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 168.579615 105.448499)
    (fp_text reference "C639" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 749 "FBB_VREF1"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 123.44892 63.579114 180)
    (fp_text reference "R724" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2021 "FBD1_CLK0_R"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 424 "FBD1_CLK0*"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 89.621708 65.380812 90)
    (fp_text reference "R763" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 281 "FBE_CMD<26>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 106.182508 64.212412)
    (fp_text reference "C916" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 103.143601 65.801614 -90)
    (fp_text reference "C945" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 161.538201 133.89241 180)
    (fp_text reference "C686" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 253.540608 115.431207 -90)
    (fp_text reference "R503" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 944 "NET0003"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 175.384808 144.600618 90)
    (fp_text reference "C569" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 8.621108 68.225612 90)
    (fp_text reference "C1231" (at 0 -1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1669 "DACB_PB"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 170.881413 58.040212)
    (fp_text reference "R625" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 561 "FBC_VREF3"))
  )
  (footprint "IND_SMD_0603_1" (layer "B.Cu")
    (tedit 0)
    (at 7.249508 71.197412 -90)
    (fp_text reference "L502" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.762 0 90) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1670 "DACB_PR"))
    (pad "2" smd rect (at -0.762 0 270) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1953 "DACB_PR_F"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 107.747123 61.031519 -90)
    (fp_text reference "C906" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2022 "FBE0_CLK0_R"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 104.822592 115.347895 90)
    (fp_text reference "C928" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0603_1" (layer "B.Cu")
    (tedit 0)
    (at 22.489508 78.715507 180)
    (fp_text reference "R902" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.762 0) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 991 "12V_F"))
    (pad "2" smd rect (at -0.762 0 180) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1044 "12V_PS3_R"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 221.384208 89.040607 90)
    (fp_text reference "R586" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1019 "PS5_NVVDD_LG2"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2088 "PS5_NVVDD_LG2_D"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 59.464313 121.065918 -90)
    (fp_text reference "C1105" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 121.976203 102.543501 90)
    (fp_text reference "C800" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 73.675613 123.775412)
    (fp_text reference "C1008" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0603_1" (layer "B.Cu")
    (tedit 0)
    (at 32.090708 132.716212)
    (fp_text reference "C1152" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.762 0 180) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 6 "PS1_1V15_PH"))
    (pad "2" smd rect (at -0.762 0) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1106 "PS1_1V15_PH_RC"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 25.410508 103.354015 90)
    (fp_text reference "C1190" (at 0 -1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 39.685308 130.709307 -90)
    (fp_text reference "R848" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1812 "I2C4_SDA"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 166.277917 75.603499)
    (fp_text reference "C649" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 175.461008 108.999419 90)
    (fp_text reference "R614" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 751 "FBB_ZQ1"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0603_1" (layer "B.Cu")
    (tedit 0)
    (at 17.003108 102.845812 -90)
    (fp_text reference "C1226" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.762 0 90) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1722 "IFPCD_PLLVDD"))
    (pad "2" smd rect (at -0.762 0 270) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 68.065998 84.230101)
    (fp_text reference "R790" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 24 "FBF_CMD<23>"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 57.724413 114.428212 -90)
    (fp_text reference "C1113" (at 0 0.7874 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0 270) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.9525 0 270) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 202.042108 58.547907)
    (fp_text reference "R607" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1874 "SPDIF_IN_GPU"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 104.467017 152.807815 -90)
    (fp_text reference "C934" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2049 "PEX_TX_C12"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1163 "PEX_TX12"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 5.573108 99.074115 90)
    (fp_text reference "C1248" (at 0 -1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1920 "I2C1_SDA_CON"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 101.813708 60.427812 90)
    (fp_text reference "R752" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 303 "FBE_CMD<6>"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 244.714108 109.107115 180)
    (fp_text reference "R533" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 933 "PS5_NVVDD_SET_ILIMFS"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 927 "NET0001"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 60.032511 152.807815 -90)
    (fp_text reference "C1095" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2030 "PEX_TX_C1*"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1158 "PEX_TX1*"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 25.537508 93.955507 -90)
    (fp_text reference "R894" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1672 "DACB_RSET"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 74.026616 87.453615)
    (fp_text reference "R772" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 37 "FBF_CMD<10>"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 121.778108 104.877812 90)
    (fp_text reference "C801" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 21.213412 118.824596 90)
    (fp_text reference "R905" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1688 "DACC_BLUE"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 110.856108 105.004812 90)
    (fp_text reference "C879" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 175.461008 61.981504 90)
    (fp_text reference "C552" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 115.936108 111.608812 90)
    (fp_text reference "C845" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 138.643708 62.680004 180)
    (fp_text reference "R698" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2020 "FBD0_CLK0_R"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 485 "FBD0_CLK0"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 116.317108 108.306812 -90)
    (fp_text reference "C840" (at 0 0.7874 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0 270) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.9525 0 270) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "SOT23_1" (layer "B.Cu")
    (tedit 0)
    (at 9.827608 95.518115 90)
    (fp_text reference "D524" (at -1.23825 1.23825 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "2" smd rect (at -0.9525 1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1914 "5V"))
    (pad "3" smd rect (at 0 -1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2001 "I2C1_SCL_R"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 112.8368 151.918612 180)
    (fp_text reference "C864" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2051 "PEX_TX_C14"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1130 "PEX_TX14"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 173.483415 83.809706 180)
    (fp_text reference "C585" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "SOT23_1" (layer "B.Cu")
    (tedit 0)
    (at 6.335108 74.727707 -90)
    (fp_text reference "D532" (at 1.23825 -1.23825 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 1.143 270) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "2" smd rect (at -0.9525 1.143 270) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "3" smd rect (at 0 -1.143 270) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1670 "DACB_PR"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 64.836413 112.75961)
    (fp_text reference "C1049" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 173 "FBG_VREF4"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 54.976108 145.263507 -90)
    (fp_text reference "R836" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1969 "JTAG_TDI"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 247.457308 112.395907 90)
    (fp_text reference "R525" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 931 "PS5_NVVDD_FB"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1042 "NET0008"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 171.545801 95.531298 180)
    (fp_text reference "C609" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 76.482999 152.807815 -90)
    (fp_text reference "C1001" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2040 "PEX_TX_C5*"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1178 "PEX_TX5*"))
  )
  (footprint "GEOM0009_1" (layer "B.Cu")
    (tedit 0)
    (at 233.576208 141.313807 90)
    (fp_text reference "U507" (at -1.353464 1.35349 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.750113 1.376883 270) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1021 "PS5_NVVDD_BOOT3"))
    (pad "2" smd rect (at 0.249911 1.376883 270) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 947 "PS5_NVVDD_PWM3"))
    (pad "3" smd rect (at -0.249911 1.376883 270) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1024 "PS5_NVVDD_DRV_PHASE3"))
    (pad "4" smd rect (at -0.750087 1.376883 270) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1025 "12V_PH3"))
    (pad "5" smd rect (at -0.750087 -1.376909 90) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1023 "PS5_NVVDD_LG3"))
    (pad "6" smd rect (at -0.249911 -1.376909 90) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "7" smd rect (at 0.249911 -1.376909 90) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 10 "PS5_NVVDD_PHASE3"))
    (pad "8" smd rect (at 0.750113 -1.376909 90) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1022 "PS5_NVVDD_UG3"))
    (pad "9" smd rect (at 0 0 90) (size 1.850111 1.5494) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 105.540904 56.224315 180)
    (fp_text reference "C918" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 168.979893 79.806716 90)
    (fp_text reference "R639" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2017 "FBC0_CLK0_R"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 615 "FBC0_CLK0"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 43.730512 105.112711 180)
    (fp_text reference "R845" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1815 "FL_REFCLK_VAIO"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 164.424708 65.584012 180)
    (fp_text reference "R677" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 547 "FBC_CMD<24>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 171.943108 145.901504 180)
    (fp_text reference "R622" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 880 "FBA_VREF2"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 246.377808 111.443407 -90)
    (fp_text reference "R528" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1041 "NET0007"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 929 "PS5_NVVDD_VAMP_CSSUM"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 61.467307 104.241516)
    (fp_text reference "C1081" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 34.021108 95.073615 90)
    (fp_text reference "R858" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1841 "DVIA_D0"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 165.415308 64.085412 180)
    (fp_text reference "R673" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 539 "FBC_CMD<27>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 218.806108 112.218107 90)
    (fp_text reference "R594" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 986 "PS5_NVVDD_UG5_R"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "PS5_NVVDD_PHASE5"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 71.232413 66.752615 180)
    (fp_text reference "C1020" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 170.280907 68.886698)
    (fp_text reference "C625" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 173.483415 120.370516 180)
    (fp_text reference "C594" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 168.579615 59.279402)
    (fp_text reference "R643" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 561 "FBC_VREF3"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 30.634805 104.2532 -90)
    (fp_text reference "C1160" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 25.123005 118.0962 180)
    (fp_text reference "C1194" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1693 "DACC_VDD"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 12.494608 98.820115 -90)
    (fp_text reference "R933" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1914 "5V"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2002 "I2C1_SDA_R"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 242.390287 101.106115 180)
    (fp_text reference "R537" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 962 "PS5_NVVDD_VCC"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 949 "PS5_NVVDD_PWM5"))
  )
  (footprint "SOT23_1" (layer "B.Cu")
    (tedit 0)
    (at 28.433108 144.806612 -90)
    (fp_text reference "Q513" (at 1.23825 -1.23825 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 1.143 270) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1994 "THERM_SHDN_D*"))
    (pad "2" smd rect (at -0.9525 1.143 270) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "3" smd rect (at 0 -1.143 270) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1995 "PS1_1V15_EN*"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 36.230908 130.709307 -90)
    (fp_text reference "C1139" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 157.947708 79.960412 180)
    (fp_text reference "R688" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 611 "FBC_CMD<3>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 22.481405 95.878795 180)
    (fp_text reference "C1206" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1725 "IFPCD_IOVDD"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 61.467307 122.366906)
    (fp_text reference "C1086" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 251.762608 125.349907 90)
    (fp_text reference "C504" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1988 "FAN_CUTOFF_RC_Q"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 109.483009 152.807815 -90)
    (fp_text reference "C890" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2034 "PEX_TX_C13*"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1167 "PEX_TX13*"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 231.899808 125.959507)
    (fp_text reference "R575" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1027 "PS5_NVVDD_UG4"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 985 "PS5_NVVDD_UG4_R"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 246.936608 97.536907 -90)
    (fp_text reference "R527" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 967 "PS5_NVVDD_VID3"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 164.881908 68.911412)
    (fp_text reference "C662" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 227.340508 79.198107 90)
    (fp_text reference "R579" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1015 "PS5_NVVDD_LG1"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 993 "PS5_NVVDD_LG1_AC"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 37.670605 98.2842 180)
    (fp_text reference "C1137" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1791 "DR_VREF"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 105.845704 71.261115 180)
    (fp_text reference "C917" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 122.844908 129.465012 180)
    (fp_text reference "C788" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1643 "PEX_PLLVDD"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0603_1" (layer "B.Cu")
    (tedit 0)
    (at 233.563508 106.299907)
    (fp_text reference "C522" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.762 0 180) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1038 "12V_PH6"))
    (pad "2" smd rect (at -0.762 0) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0603_1" (layer "B.Cu")
    (tedit 0)
    (at 242.148708 96.419307 180)
    (fp_text reference "C517" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.762 0) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1043 "PS5_NVVDD_VIN_PWM"))
    (pad "2" smd rect (at -0.762 0 180) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 32.514405 107.0218 180)
    (fp_text reference "C1147" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 27.925108 85.217907 90)
    (fp_text reference "R886" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1968 "PS3_FBVDDQ_LG"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 990 "PS3_FBVDDQ_LG_G"))
  )
  (footprint "GEOM0006_1" (layer "B.Cu")
    (tedit 0)
    (at 248.486313 103.646115)
    (fp_text reference "U501" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 3.376905 -2.750109 270) (size 0.2794 0.753796) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 937 "SNN_PS5_NVVDD_PIN1"))
    (pad "2" smd rect (at 3.376905 -2.249907 270) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 938 "SNN_PS5_NVVDD_PIN3"))
    (pad "3" smd rect (at 3.376905 -1.750111 270) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 939 "SNN_PS5_NVVDD_PIN2"))
    (pad "4" smd rect (at 3.376905 -1.249909 270) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 940 "SNN_PS5_NVVDD_PIN4"))
    (pad "5" smd rect (at 3.376905 -0.750087 270) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 930 "PS5_NVVDD_EN"))
    (pad "6" smd rect (at 3.376905 -0.249911 270) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "7" smd rect (at 3.376905 0.249911 270) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 944 "NET0003"))
    (pad "8" smd rect (at 3.376905 0.750113 270) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 936 "PS5_NVVDD_SET_LSSET"))
    (pad "9" smd rect (at 3.376905 1.249909 270) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 934 "PS5_NVVDD_SET_IMON"))
    (pad "10" smd rect (at 3.376905 1.750111 270) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 961 "NET0005"))
    (pad "11" smd rect (at 3.376905 2.249907 270) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 972 "SNN_PS5_NVVDD_VRHOT"))
    (pad "12" smd rect (at 3.376905 2.750109 270) (size 0.2794 0.753796) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 935 "PS5_NVVDD_IDES"))
    (pad "13" smd rect (at 2.750083 3.376905 180) (size 0.2794 0.753796) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 953 "PS5_NVVDD_FS"))
    (pad "14" smd rect (at 2.249881 3.376905 180) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 952 "NET0004"))
    (pad "15" smd rect (at 1.750085 3.376905 180) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 960 "PS5_NVVDD_SET_TRDET"))
    (pad "16" smd rect (at 1.249883 3.376905 180) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 932 "PS5_NVVDD_FBRTN"))
    (pad "17" smd rect (at 0.750087 3.376905 180) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 926 "PS5_NVVDD_CP"))
    (pad "18" smd rect (at 0.249885 3.376905 180) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 931 "PS5_NVVDD_FB"))
    (pad "19" smd rect (at -0.249911 3.376905 180) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 928 "PS5_NVVDD_VAMP_CSREF"))
    (pad "20" smd rect (at -0.750113 3.376905 180) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 929 "PS5_NVVDD_VAMP_CSSUM"))
    (pad "21" smd rect (at -1.249909 3.376905 180) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 927 "NET0001"))
    (pad "22" smd rect (at -1.750111 3.376905 180) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 933 "PS5_NVVDD_SET_ILIMFS"))
    (pad "23" smd rect (at -2.249907 3.376905 180) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 942 "PS5_NVVDD_DRV_ODN"))
    (pad "24" smd rect (at -2.750109 3.376905 180) (size 0.2794 0.753796) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 941 "PS5_NVVDD_DRV_OD1"))
    (pad "25" smd rect (at -3.376905 2.750109 90) (size 0.2794 0.753796) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 959 "PS5_NVVDD_ISEN6"))
    (pad "26" smd rect (at -3.376905 2.249907 90) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 958 "PS5_NVVDD_ISEN5"))
    (pad "27" smd rect (at -3.376905 1.750111 90) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 957 "PS5_NVVDD_ISEN4"))
    (pad "28" smd rect (at -3.376905 1.249909 90) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 956 "PS5_NVVDD_ISEN3"))
    (pad "29" smd rect (at -3.376905 0.750113 90) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 955 "PS5_NVVDD_ISEN2"))
    (pad "30" smd rect (at -3.376905 0.249911 90) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 954 "PS5_NVVDD_ISEN1"))
    (pad "31" smd rect (at -3.376905 -0.249911 90) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 950 "PS5_NVVDD_PWM6"))
    (pad "32" smd rect (at -3.376905 -0.750087 90) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 949 "PS5_NVVDD_PWM5"))
    (pad "33" smd rect (at -3.376905 -1.249909 90) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 948 "PS5_NVVDD_PWM4"))
    (pad "34" smd rect (at -3.376905 -1.750111 90) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 947 "PS5_NVVDD_PWM3"))
    (pad "35" smd rect (at -3.376905 -2.249907 90) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 946 "PS5_NVVDD_PWM2"))
    (pad "36" smd rect (at -3.376905 -2.750109 90) (size 0.2794 0.753796) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 945 "PS5_NVVDD_PWM1"))
    (pad "37" smd rect (at -2.750109 -3.376905) (size 0.2794 0.753796) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 962 "PS5_NVVDD_VCC"))
    (pad "38" smd rect (at -2.249907 -3.376905) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 971 "SNN_PS5_NVVDD_VID7"))
    (pad "39" smd rect (at -1.750111 -3.376905) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 970 "PS5_NVVDD_VID6"))
    (pad "40" smd rect (at -1.249909 -3.376905) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 969 "SNN_PS5_NVVDD_VID5"))
    (pad "41" smd rect (at -0.750113 -3.376905) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 968 "PS5_NVVDD_VID4"))
    (pad "42" smd rect (at -0.249911 -3.376905) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 967 "PS5_NVVDD_VID3"))
    (pad "43" smd rect (at 0.249885 -3.376905) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 966 "PS5_NVVDD_VID2"))
    (pad "44" smd rect (at 0.750087 -3.376905) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 965 "PS5_NVVDD_VID1"))
    (pad "45" smd rect (at 1.249883 -3.376905) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 964 "PS5_NVVDD_VID0"))
    (pad "46" smd rect (at 1.750085 -3.376905) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 943 "NET0002"))
    (pad "47" smd rect (at 2.249881 -3.376905) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 951 "PS5_NVVDD_PGOOD"))
    (pad "48" smd rect (at 2.750083 -3.376905) (size 0.2794 0.753796) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 963 "PS5_NVVDD_VCC_VCC3"))
    (pad "49" smd rect (at 0 0) (size 5.461 5.461) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 59.464313 101.458718 90)
    (fp_text reference "C1103" (at 0 -1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 71.074603 114.160699 180)
    (fp_text reference "C1022" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 6.271608 61.913407)
    (fp_text reference "R943" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1669 "DACB_PB"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 168.579615 75.603499)
    (fp_text reference "C637" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 619 "FBC_VREF1"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "LTPT18C10P_1" (layer "B.Cu")
    (tedit 0)
    (at 129.398108 116.993612)
    (fp_text reference "TP501" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu *.Mask)
      (net 1477 "FBVDDQ_SENSE"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 164.754908 71.095812 180)
    (fp_text reference "C663" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 98.928801 56.275115 180)
    (fp_text reference "C965" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 249.540108 112.395907 90)
    (fp_text reference "R514" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 931 "PS5_NVVDD_FB"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 999 "NVVDD_SENSE_R"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 26.959908 129.947307)
    (fp_text reference "R889" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1917 "PS1_1V15_FS"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 45.806708 98.730707 180)
    (fp_text reference "C1121" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 63.942308 123.767995 180)
    (fp_text reference "R821" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 172 "FBG_VREF3"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 28.619011 103.261305 -90)
    (fp_text reference "C1167" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 61.222705 87.409216)
    (fp_text reference "C1090" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 64.186402 74.387601)
    (fp_text reference "C1055" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2024 "FBF0_CLK0_R"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 65.598413 97.836602)
    (fp_text reference "C1047" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 115 "FBG_VREF2"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 62.318511 79.991095)
    (fp_text reference "R825" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 43 "FBF_CMD<6>"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 35.765605 97.573 90)
    (fp_text reference "R854" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1790 "2V5"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1788 "DR_CAL_PD_VDDQ"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 240.104313 104.154115)
    (fp_text reference "R549" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 14 "PS5_NVVDD_PHASE2"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 929 "PS5_NVVDD_VAMP_CSSUM"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 101.077108 65.279212 90)
    (fp_text reference "C958" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2023 "FBE1_CLK0_R"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 53.960108 145.263812 -90)
    (fp_text reference "R838" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1115 "JTAG_TDI_GPU"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1969 "JTAG_TDI"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 103.143601 63.080308 90)
    (fp_text reference "R750" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 359 "FBE_VREF1"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 168.579615 120.370516)
    (fp_text reference "R649" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 796 "FBA_CMD<25>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 247.952608 94.869907 90)
    (fp_text reference "R521" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1805 "GPIO5_PS5_NVVDD_VID1"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 965 "PS5_NVVDD_VID1"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 242.390287 107.329115)
    (fp_text reference "R541" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 957 "PS5_NVVDD_ISEN4"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 11 "PS5_NVVDD_PHASE4"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 134.440491 65.382006 90)
    (fp_text reference "C723" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 70.978108 138.672207 180)
    (fp_text reference "R777" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 978 "THERM_SHDN*"))
  )
  (footprint "SOT23_1" (layer "B.Cu")
    (tedit 0)
    (at 67.739608 142.939407 90)
    (fp_text reference "Q505" (at -1.23825 1.23825 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1994 "THERM_SHDN_D*"))
    (pad "2" smd rect (at -0.9525 1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "3" smd rect (at 0 -1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1980 "THERM_LATCH"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 26.832908 136.069012 90)
    (fp_text reference "R890" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1958 "PS1_1V15_FB"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1959 "PS1_1V15_FB_RC"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 108.943513 102.543501 90)
    (fp_text reference "C895" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 19.695508 112.548612)
    (fp_text reference "C1217" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1701 "IFPAB_IOVDD"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 108.747908 63.680714 180)
    (fp_text reference "R740" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2022 "FBE0_CLK0_R"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 356 "FBE0_CLK0*"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 61.467307 78.932194 180)
    (fp_text reference "C1078" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 23.715312 111.6684)
    (fp_text reference "R900" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1699 "IFPAB_RSET"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 104.823608 113.056612 -90)
    (fp_text reference "C927" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 108.239908 127.255212)
    (fp_text reference "C900" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1484 "GV_PLLAVDD"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 63.396208 72.591618)
    (fp_text reference "C1067" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 169.733308 70.307116 180)
    (fp_text reference "C634" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 562 "FBC_VREF4"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 129.753708 61.456512 180)
    (fp_text reference "C738" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 432 "FBD_VREF4"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 64.836413 111.761212)
    (fp_text reference "R815" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 173 "FBG_VREF4"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 111.240105 132.260714 90)
    (fp_text reference "R737" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1522 "GV_TX_RSET_GND"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 37.670605 97.2682 180)
    (fp_text reference "R852" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1791 "DR_VREF"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 68.658605 89.061206 180)
    (fp_text reference "R787" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 18 "FBF_CMD<27>"))
  )
  (footprint "GEOM0009_1" (layer "B.Cu")
    (tedit 0)
    (at 233.855608 92.698207 90)
    (fp_text reference "U503" (at -1.353464 1.35349 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.750113 1.376883 270) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1017 "PS5_NVVDD_BOOT2"))
    (pad "2" smd rect (at 0.249911 1.376883 270) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 946 "PS5_NVVDD_PWM2"))
    (pad "3" smd rect (at -0.249911 1.376883 270) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 942 "PS5_NVVDD_DRV_ODN"))
    (pad "4" smd rect (at -0.750087 1.376883 270) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1020 "12V_PH2"))
    (pad "5" smd rect (at -0.750087 -1.376909 90) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1019 "PS5_NVVDD_LG2"))
    (pad "6" smd rect (at -0.249911 -1.376909 90) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "7" smd rect (at 0.249911 -1.376909 90) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 14 "PS5_NVVDD_PHASE2"))
    (pad "8" smd rect (at 0.750113 -1.376909 90) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1018 "PS5_NVVDD_UG2"))
    (pad "9" smd rect (at 0 0 90) (size 1.850111 1.5494) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 57.305821 152.807815 -90)
    (fp_text reference "C1116" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2029 "PEX_TX_C0*"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1156 "PEX_TX0*"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 104.544691 65.382006 90)
    (fp_text reference "C932" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "SOT23_1" (layer "B.Cu")
    (tedit 0)
    (at 9.827608 99.391615 90)
    (fp_text reference "D525" (at -1.23825 1.23825 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "2" smd rect (at -0.9525 1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1914 "5V"))
    (pad "3" smd rect (at 0 -1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2002 "I2C1_SDA_R"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 108.747908 62.680004 180)
    (fp_text reference "R739" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2022 "FBE0_CLK0_R"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 355 "FBE0_CLK0"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 124.521308 57.887812 -90)
    (fp_text reference "C777" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 74.657806 85.181814 90)
    (fp_text reference "C1003" (at 0 -1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 74.838908 71.731015 90)
    (fp_text reference "R770" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 219 "FBF_CMD<5>"))
  )
  (footprint "DIODE_SMD_SMA_1" (layer "B.Cu")
    (tedit 0)
    (at 203.058108 78.740907 -90)
    (fp_text reference "D512" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -1.880108 0 270) (size 2.159 2.032) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 8 "PS5_NVVDD_PHASE1"))
    (pad "2" smd rect (at 1.880108 0 270) (size 2.159 2.032) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 103.143601 68.225612 -90)
    (fp_text reference "C946" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 123.349301 126.78201 90)
    (fp_text reference "C781" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 30.795308 121.666907)
    (fp_text reference "R872" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1979 "FAN_PWM_NVIO_R"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1973 "FAN_PWM"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 12.494608 95.200615 90)
    (fp_text reference "R932" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2001 "I2C1_SCL_R"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1914 "5V"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 133.039401 63.080308 90)
    (fp_text reference "R707" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 489 "FBD_VREF1"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 38.085108 107.417812 90)
    (fp_text reference "C1135" (at 0 -1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1661 "NVIO_GV_PLLAVDD"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 55.738108 139.116707 -90)
    (fp_text reference "R835" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2005 "JTAG_TRST_3V3"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 17.130108 111.227812 90)
    (fp_text reference "C1225" (at 0 -1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1666 "NVIO_PLLVDD"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 9.891108 111.824915)
    (fp_text reference "R936" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1679 "DACA_GREEN"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "SOT23_5_1" (layer "B.Cu")
    (tedit 0)
    (at 123.810108 144.273212)
    (fp_text reference "U509" (at 1.362685 1.390345 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 1.2954) (size 0.6858 0.9906) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at 0 1.2954) (size 0.6858 0.9906) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "3" smd rect (at -0.9525 1.2954) (size 0.6858 0.9906) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "4" smd rect (at -0.9525 -1.2954) (size 0.6858 0.9906) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1971 "PEX_PLLVDD_OP_ADJ"))
    (pad "5" smd rect (at 0.9525 -1.2954) (size 0.6858 0.9906) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1972 "PEX_PLLVDD_OP"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 129.753708 60.440512 180)
    (fp_text reference "R715" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 432 "FBD_VREF4"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 173.483415 133.89241)
    (fp_text reference "C596" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 72.675819 108.845012 180)
    (fp_text reference "C1012" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "IND_SMD_0402_1" (layer "B.Cu")
    (tedit 0)
    (at 15.606108 102.743907 90)
    (fp_text reference "LB516" (at 0 -1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.6858 0.5334) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.6858 0.5334) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1722 "IFPCD_PLLVDD"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 83.467009 152.807815 -90)
    (fp_text reference "C994" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2058 "PEX_TX_C7"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1182 "PEX_TX7"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 153.705908 131.903412)
    (fp_text reference "C699" (at -0.7874 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.9525 0) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 28.619011 109.716207 90)
    (fp_text reference "C1168" (at 0 -1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 160.373408 76.904512 90)
    (fp_text reference "C688" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 171.545801 93.729904 180)
    (fp_text reference "C608" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2015 "FBB1_CLK0_R"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 107.812223 98.935406 -90)
    (fp_text reference "C902" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 203.756608 59.119407 90)
    (fp_text reference "C532" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1956 "SPDIF_IN"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1874 "SPDIF_IN_GPU"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 173.816612 93.727898 180)
    (fp_text reference "C571" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 115.321707 57.583215 180)
    (fp_text reference "C850" (at 0.7874 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0 180) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.9525 0 180) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 120.000108 115.799812 -90)
    (fp_text reference "C809" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 19.289108 118.060615)
    (fp_text reference "R910" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1052 "IFP_IOVDD_EN"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1053 "IFP_IOVDD"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 242.390287 108.726115)
    (fp_text reference "R542" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 958 "PS5_NVVDD_ISEN5"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "PS5_NVVDD_PHASE5"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 162.341908 72.188012 180)
    (fp_text reference "R682" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 557 "FBC_CMD<10>"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 173.483415 75.603499 180)
    (fp_text reference "C583" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 107.173108 119.228812 90)
    (fp_text reference "C910" (at 0 -0.7874 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0 90) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.9525 0 90) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 79.467017 152.807815 -90)
    (fp_text reference "C997" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2057 "PEX_TX_C6"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1181 "PEX_TX6"))
  )
  (footprint "SOT23_1" (layer "B.Cu")
    (tedit 0)
    (at 224.825908 78.753607 90)
    (fp_text reference "D507" (at -1.23825 1.23825 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1015 "PS5_NVVDD_LG1"))
    (pad "2" smd rect (at -0.9525 1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 993 "PS5_NVVDD_LG1_AC"))
    (pad "3" smd rect (at 0 -1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2083 "PS5_NVVDD_LG1_D"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 15.21952 82.080016 -90)
    (fp_text reference "R922" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1055 "PS3_FBVDDQ_FB"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1978 "PS3_FBVDDQ_FB_RC"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 113.537307 126.75661 -90)
    (fp_text reference "C858" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 22.214197 118.824596 90)
    (fp_text reference "R903" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1691 "DACC_RED"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 130.007708 104.014212 180)
    (fp_text reference "R714" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1247 "FBC_DEBUG"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 61.467307 119.164499)
    (fp_text reference "C1085" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 88.220619 60.478307 90)
    (fp_text reference "C989" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 77.714213 105.640015)
    (fp_text reference "R767" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 96 "FBG_CMD<3>"))
  )
  (footprint "0603_1" (layer "B.Cu")
    (tedit 0)
    (at 233.563508 133.376307 180)
    (fp_text reference "R569" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.762 0) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 981 "12V_PEX6_F1"))
    (pad "2" smd rect (at -0.762 0 180) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1030 "12V_PH4"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 122.721997 124.855115 180)
    (fp_text reference "C792" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 34.013005 100.5702 -90)
    (fp_text reference "R859" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1789 "DR_CAL_PU_GND"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 68.615908 78.893612 180)
    (fp_text reference "C1033" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 9.954608 105.741615)
    (fp_text reference "R934" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1678 "DACA_BLUE"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "SOT23_1" (layer "B.Cu")
    (tedit 0)
    (at 16.495108 114.326815 90)
    (fp_text reference "Q517" (at -1.23825 1.23825 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1052 "IFP_IOVDD_EN"))
    (pad "2" smd rect (at -0.9525 1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1053 "IFP_IOVDD"))
    (pad "3" smd rect (at 0 -1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 16.23552 82.080016 -90)
    (fp_text reference "R918" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1055 "PS3_FBVDDQ_FB"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1109 "PS3_FBVDDQ_VSEN"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 105.483017 152.807815 -90)
    (fp_text reference "C919" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2033 "PEX_TX_C12*"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1164 "PEX_TX12*"))
  )
  (footprint "LTPT28C49P18C10P_1" (layer "B.Cu")
    (tedit 0)
    (at 117.460108 116.358307)
    (fp_text reference "TP502" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 0.7112 0.7112) (drill 0.254) (layers *.Cu *.Mask)
      (net 1554 "NVVDD_SENSE"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 173.816612 63.882898 180)
    (fp_text reference "C570" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 57.724413 91.974815 -90)
    (fp_text reference "C1110" (at 0 0.7874 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0 270) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.9525 0 270) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 117.960513 102.541012 90)
    (fp_text reference "C828" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 170.927108 108.650906 180)
    (fp_text reference "C620" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2018 "FBB0_CLK0_R"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 130.134708 97.151106 90)
    (fp_text reference "R713" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1592 "FB_CAL_TERM_GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 162.274801 144.900795)
    (fp_text reference "C683" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 164.221508 78.706896)
    (fp_text reference "C664" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 164.990899 95.219716 180)
    (fp_text reference "R676" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 677 "FBB_CMD<24>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 173.483415 143.499706 180)
    (fp_text reference "C599" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 245.920608 94.869907 90)
    (fp_text reference "R530" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1807 "GPIO7_PS5_NVVDD_VID3"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 967 "PS5_NVVDD_VID3"))
  )
  (footprint "0603_1" (layer "B.Cu")
    (tedit 0)
    (at 233.563508 95.454107)
    (fp_text reference "C521" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.762 0 180) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1020 "12V_PH2"))
    (pad "2" smd rect (at -0.762 0) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0603_1" (layer "B.Cu")
    (tedit 0)
    (at 233.563508 97.105107 180)
    (fp_text reference "R567" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.762 0) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 981 "12V_PEX6_F1"))
    (pad "2" smd rect (at -0.762 0 180) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1020 "12V_PH2"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 130.795108 73.407212 90)
    (fp_text reference "R710" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 427 "FBD_CMD<10>"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 131.684108 145.949612 180)
    (fp_text reference "C730" (at 0.7874 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0 180) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at -0.9525 0 180) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 113.269108 112.497812 90)
    (fp_text reference "C861" (at 0 -0.7874 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0 90) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.9525 0 90) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 8.621108 71.426012 -90)
    (fp_text reference "C1232" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1670 "DACB_PR"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 15.606108 105.791907 -90)
    (fp_text reference "R921" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1678 "DACA_BLUE"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 104.935419 125.9051 90)
    (fp_text reference "C921" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 171.943108 115.05582 180)
    (fp_text reference "C604" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 116.317108 121.514812 -90)
    (fp_text reference "C841" (at 0 0.7874 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0 270) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.9525 0 270) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 38.102405 100.367 180)
    (fp_text reference "C1134" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1664 "NVIO_SP_PLLVDD"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 64.069308 108.845012 180)
    (fp_text reference "R819" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 114 "FBG_VREF1"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 233.868308 138.303907)
    (fp_text reference "R565" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1021 "PS5_NVVDD_BOOT3"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1003 "PS5_NVVDD_BOOT3_RC"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 12.761308 79.045707 180)
    (fp_text reference "R930" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1109 "PS3_FBVDDQ_VSEN"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 67.293609 81.266404)
    (fp_text reference "R792" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 42 "FBF_VREF4"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 70.978108 140.704207)
    (fp_text reference "R779" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 978 "THERM_SHDN*"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1994 "THERM_SHDN_D*"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 103.134 103.786806)
    (fp_text reference "C949" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0603_1" (layer "B.Cu")
    (tedit 0)
    (at 128.044313 103.620512 90)
    (fp_text reference "C754" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.762 0 270) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1573 "FBABCD_MPLL_AVDD"))
    (pad "2" smd rect (at -0.762 0 90) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 62.965703 152.807815 -90)
    (fp_text reference "C1070" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2053 "PEX_TX_C2"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1172 "PEX_TX2"))
  )
  (footprint "SOT23_1" (layer "B.Cu")
    (tedit 0)
    (at 248.270108 124.460907)
    (fp_text reference "Q502" (at 1.23825 1.23825 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 1.143) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1988 "FAN_CUTOFF_RC_Q"))
    (pad "2" smd rect (at -0.9525 1.143) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "3" smd rect (at 0 -1.143) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1973 "FAN_PWM"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 163.967508 75.603499)
    (fp_text reference "C668" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 57.724413 106.833612 90)
    (fp_text reference "C1112" (at 0 -0.7874 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0 90) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.9525 0 90) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 218.933108 75.896107 90)
    (fp_text reference "R590" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 982 "PS5_NVVDD_UG1_R"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 8 "PS5_NVVDD_PHASE1"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 175.461008 94.076411 90)
    (fp_text reference "R613" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 694 "FBB_ZQ2"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 29.677708 100.686812 -90)
    (fp_text reference "C1163" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 169.005293 64.484903 90)
    (fp_text reference "R638" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2014 "FBC1_CLK0_R"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 553 "FBC1_CLK0"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 120.000108 122.403812 -90)
    (fp_text reference "C810" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 19.028504 92.902906 -90)
    (fp_text reference "R911" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1670 "DACB_PR"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 33.055908 121.666907)
    (fp_text reference "R862" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1794 "FAN_PWM_NVIO"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 77.714213 106.656015)
    (fp_text reference "R768" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 95 "FBG_CMD<4>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 63.769105 107.443898)
    (fp_text reference "C1063" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "IND_SMD_0402_1" (layer "B.Cu")
    (tedit 0)
    (at 125.02372 124.855115)
    (fp_text reference "LB501" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.6858 0.5334) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1573 "FBABCD_MPLL_AVDD"))
    (pad "2" smd rect (at -0.5334 0) (size 0.6858 0.5334) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 64.322317 104.241516)
    (fp_text reference "C1054" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2026 "FBG0_CLK0_R"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 122.841098 130.506412 180)
    (fp_text reference "C789" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1643 "PEX_PLLVDD"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 65.970701 118.384694 -90)
    (fp_text reference "R810" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2027 "FBG1_CLK0_R"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 168 "FBG1_CLK0"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 28.941108 95.073615 90)
    (fp_text reference "R883" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1848 "DVIA_D7"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 168.979893 109.651716 90)
    (fp_text reference "R640" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2018 "FBB0_CLK0_R"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 745 "FBB0_CLK0"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 160.373408 106.749512 90)
    (fp_text reference "C690" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 206.868108 59.119407 90)
    (fp_text reference "R603" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1956 "SPDIF_IN"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 8.815215 141.707812)
    (fp_text reference "R940" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1691 "DACC_RED"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 107.173108 106.020812 90)
    (fp_text reference "C908" (at 0 -0.7874 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0 90) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.9525 0 90) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 175.384808 127.27571 -90)
    (fp_text reference "C566" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 137.991411 56.198915 180)
    (fp_text reference "R702" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 491 "FBD_ZQ1"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 175.384808 114.755618 90)
    (fp_text reference "C565" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 109.586108 118.212812 90)
    (fp_text reference "C889" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 128.280813 76.684015 -90)
    (fp_text reference "C750" (at 0 0.7874 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0 270) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.9525 0 270) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 7.224108 113.869615 -90)
    (fp_text reference "C1239" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1679 "DACA_GREEN"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "SOT23_1" (layer "B.Cu")
    (tedit 0)
    (at 64.945608 133.795407 -90)
    (fp_text reference "Q506" (at 1.23825 -1.23825 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 1.143 270) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1980 "THERM_LATCH"))
    (pad "2" smd rect (at -0.9525 1.143 270) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "3" smd rect (at 0 -1.143 270) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1997 "THERM_SHDN_R"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 173.483415 135.293499 180)
    (fp_text reference "C597" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 119.365108 105.893812 90)
    (fp_text reference "C814" (at 0 -0.7874 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0 90) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.9525 0 90) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 173.483415 118.969402)
    (fp_text reference "C593" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 94.498508 66.676212 -90)
    (fp_text reference "R759" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 287 "FBE_CMD<24>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 5.852508 68.225612 90)
    (fp_text reference "C1244" (at 0 -1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1669 "DACB_PB"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1954 "DACB_PB_F"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 66.371005 108.845012 180)
    (fp_text reference "R802" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 114 "FBG_VREF1"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 103.143601 70.511612 -90)
    (fp_text reference "C947" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 87.204619 62.180412 -90)
    (fp_text reference "C991" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 301 "FBE_VREF3"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 69.022308 73.686612 -90)
    (fp_text reference "R784" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 223 "FBF_CMD<2>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 72.483109 152.807815 -90)
    (fp_text reference "C1014" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2039 "PEX_TX_C4*"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1177 "PEX_TX4*"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 231.899808 79.223507)
    (fp_text reference "R572" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1014 "PS5_NVVDD_UG1"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 982 "PS5_NVVDD_UG1_R"))
  )
  (footprint "0603_1" (layer "B.Cu")
    (tedit 0)
    (at 125.644217 129.515812 90)
    (fp_text reference "C767" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.762 0 270) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at -0.762 0 90) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 99.959508 66.269812 -90)
    (fp_text reference "C961" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 170.881413 74.20241)
    (fp_text reference "R626" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 619 "FBC_VREF1"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 27.798108 123.673507 -90)
    (fp_text reference "C1173" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1051 "GPU_RST_R*"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 134.440491 58.17661 -90)
    (fp_text reference "C720" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 68.519413 123.767995 180)
    (fp_text reference "C1035" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "SOT23_1" (layer "B.Cu")
    (tedit 0)
    (at 202.613608 62.294407)
    (fp_text reference "D518" (at 1.23825 1.23825 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 1.143) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "2" smd rect (at -0.9525 1.143) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "3" smd rect (at 0 -1.143) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1874 "SPDIF_IN_GPU"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 170.628404 63.884904 180)
    (fp_text reference "C623" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2014 "FBC1_CLK0_R"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 218.933108 98.756107 90)
    (fp_text reference "R592" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 987 "PS5_NVVDD_UG6_R"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 13 "PS5_NVVDD_PHASE6"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 122.413108 108.179812 -90)
    (fp_text reference "C794" (at 0 0.7874 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0 270) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.9525 0 270) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 173.816612 123.572898 180)
    (fp_text reference "C573" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 118.342504 130.289216 90)
    (fp_text reference "C825" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 167.979209 124.174903 90)
    (fp_text reference "R655" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2016 "FBA1_CLK0_R"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 813 "FBA1_CLK0"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 27.925108 82.474707 -90)
    (fp_text reference "R885" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1045 "PS3_PVCC5_DRV"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1046 "PS3_VCC5"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 116.444413 59.386615)
    (fp_text reference "C838" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 167.244108 71.680012 180)
    (fp_text reference "R660" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 562 "FBC_VREF4"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 236.865508 145.847707)
    (fp_text reference "R558" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 941 "PS5_NVVDD_DRV_OD1"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1024 "PS5_NVVDD_DRV_PHASE3"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 28.991908 142.342812)
    (fp_text reference "R881" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 991 "12V_F"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1995 "PS1_1V15_EN*"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 64.994605 81.266404)
    (fp_text reference "R813" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 42 "FBF_VREF4"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 104.544691 60.478307 -90)
    (fp_text reference "C930" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 231.899808 100.534107)
    (fp_text reference "R574" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1036 "PS5_NVVDD_UG6"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 987 "PS5_NVVDD_UG6_R"))
  )
  (footprint "SO14_I335X150_1" (layer "B.Cu")
    (tedit 0)
    (at 18.222308 134.824615)
    (fp_text reference "U514" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 3.81 2.5908) (size 0.6096 2.032) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1690 "DACC_HSYNC"))
    (pad "2" smd rect (at 2.54 2.5908) (size 0.6096 2.032) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1690 "DACC_HSYNC"))
    (pad "3" smd rect (at 1.27 2.5908) (size 0.6096 2.032) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2006 "DACC_HSYNC_BUF_R"))
    (pad "4" smd rect (at 0 2.5908) (size 0.6096 2.032) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1680 "DACA_HSYNC"))
    (pad "5" smd rect (at -1.27 2.5908) (size 0.6096 2.032) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1680 "DACA_HSYNC"))
    (pad "6" smd rect (at -2.54 2.5908) (size 0.6096 2.032) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2008 "DACA_HSYNC_BUF_R"))
    (pad "7" smd rect (at -3.81 2.5908) (size 0.6096 2.032) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "8" smd rect (at -3.81 -2.5908) (size 0.6096 2.032) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2010 "DACA_VSYNC_BUF_R"))
    (pad "9" smd rect (at -2.54 -2.5908) (size 0.6096 2.032) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1685 "DACA_VSYNC"))
    (pad "10" smd rect (at -1.27 -2.5908) (size 0.6096 2.032) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1685 "DACA_VSYNC"))
    (pad "11" smd rect (at 0 -2.5908) (size 0.6096 2.032) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2012 "DACC_VSYNC_BUF_R"))
    (pad "12" smd rect (at 1.27 -2.5908) (size 0.6096 2.032) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1695 "DACC_VSYNC"))
    (pad "13" smd rect (at 2.54 -2.5908) (size 0.6096 2.032) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1695 "DACC_VSYNC"))
    (pad "14" smd rect (at 3.81 -2.5908) (size 0.6096 2.032) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1914 "5V"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 157.947708 78.182412 180)
    (fp_text reference "R687" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 610 "FBC_CMD<4>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 134.605413 72.823215 -90)
    (fp_text reference "R704" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 480 "FBD_CMD<4>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 16.265009 92.902906 -90)
    (fp_text reference "R917" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1669 "DACB_PB"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 25.402405 108.7744 90)
    (fp_text reference "C1192" (at 0 -1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 6.462108 133.325812 90)
    (fp_text reference "R942" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1795 "GPIO0_DVIAB_HPD"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1987 "GPIO0_DVIAB_HPD_R"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 158.735108 104.623812)
    (fp_text reference "R685" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 687 "FBB_CMD<10>"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 215.910508 117.628307 90)
    (fp_text reference "R600" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 997 "PS5_NVVDD_LG5_AC"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 167.979209 109.651716 90)
    (fp_text reference "R654" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2018 "FBB0_CLK0_R"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 746 "FBB0_CLK0*"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 19.162108 105.157212 180)
    (fp_text reference "C1219" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1666 "NVIO_PLLVDD"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 67.118121 152.807815 -90)
    (fp_text reference "C1042" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2054 "PEX_TX_C3"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1644 "PEX_TX3"))
  )
  (footprint "IND_SMD_0402_1" (layer "B.Cu")
    (tedit 0)
    (at 19.289108 116.688812 180)
    (fp_text reference "LB514" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.6858 0.5334) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1053 "IFP_IOVDD"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.6858 0.5334) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1701 "IFPAB_IOVDD"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 8.815215 145.517812)
    (fp_text reference "R941" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1689 "DACC_GREEN"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 114.133013 62.256815 -90)
    (fp_text reference "C852" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 360 "FBE_VREF2"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "SOT23_1" (layer "B.Cu")
    (tedit 0)
    (at 32.370108 124.689507 -90)
    (fp_text reference "Q511" (at 1.23825 -1.23825 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 1.143 270) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1051 "GPU_RST_R*"))
    (pad "2" smd rect (at -0.9525 1.143 270) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "3" smd rect (at 0 -1.143 270) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1052 "IFP_IOVDD_EN"))
  )
  (footprint "SOT23_1" (layer "B.Cu")
    (tedit 0)
    (at 9.827608 103.265115 90)
    (fp_text reference "D526" (at -1.23825 1.23825 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "2" smd rect (at -0.9525 1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "3" smd rect (at 0 -1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1678 "DACA_BLUE"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 103.234101 123.053722 180)
    (fp_text reference "C942" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1282 "FBEFGH_MPLL_AVDD"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 129.124804 69.385096 90)
    (fp_text reference "C744" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 63.068497 67.923809)
    (fp_text reference "C1068" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "SOT23_1" (layer "B.Cu")
    (tedit 0)
    (at 11.037715 139.294812 90)
    (fp_text reference "D521" (at -1.23825 1.23825 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "2" smd rect (at -0.9525 1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "3" smd rect (at 0 -1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1688 "DACC_BLUE"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 144.079308 65.279212 90)
    (fp_text reference "C703" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 27.391708 121.133507 180)
    (fp_text reference "C1177" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 166.277917 118.969402)
    (fp_text reference "C652" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 170.012708 101.550412 180)
    (fp_text reference "R632" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 692 "FBB_VREF4"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 28.679005 111.6954 180)
    (fp_text reference "R884" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1692 "DACC_RSET"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 241.970908 136.322707)
    (fp_text reference "R544" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1975 "FAN_TACH"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 175.461008 76.904512 90)
    (fp_text reference "C553" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 104.201308 99.924812 180)
    (fp_text reference "C936" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1282 "FBEFGH_MPLL_AVDD"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 61.153413 102.439412)
    (fp_text reference "C1091" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 128.636108 118.766506 -90)
    (fp_text reference "R717" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1478 "FBB_DEBUG"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 234.147708 89.688307)
    (fp_text reference "R561" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1017 "PS5_NVVDD_BOOT2"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1007 "PS5_NVVDD_BOOT2_RC"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 18.027719 92.902906 -90)
    (fp_text reference "R913" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1668 "DACB_Y"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 125.461108 112.370812 90)
    (fp_text reference "C769" (at 0 -0.7874 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0 90) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.9525 0 90) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 240.104313 110.123115)
    (fp_text reference "R553" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 13 "PS5_NVVDD_PHASE6"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 929 "PS5_NVVDD_VAMP_CSSUM"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 170.280907 128.576698)
    (fp_text reference "C629" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 67.117613 94.921215 180)
    (fp_text reference "R795" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 19 "FBF_CMD<28>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 128.356708 56.198915 180)
    (fp_text reference "C749" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 170.038108 131.649412 180)
    (fp_text reference "R631" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 822 "FBA_VREF4"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 144.053908 62.078812 -90)
    (fp_text reference "C704" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 490 "FBD_VREF2"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 141.218811 56.275115)
    (fp_text reference "C710" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 175.384808 99.83261 90)
    (fp_text reference "C563" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 231.849008 112.421307)
    (fp_text reference "R576" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1032 "PS5_NVVDD_UG5"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 986 "PS5_NVVDD_UG5_R"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 100.175408 63.336112)
    (fp_text reference "R755" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2023 "FBE1_CLK0_R"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 294 "FBE1_CLK0*"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 17.46742 85.305816 -90)
    (fp_text reference "C1224" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1965 "PS3_FBVDDQ_CP"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1055 "PS3_FBVDDQ_FB"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 59.565913 113.059914 -90)
    (fp_text reference "C1101" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 113.537307 129.058307 -90)
    (fp_text reference "C859" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 141.590108 111.812012 180)
    (fp_text reference "C709" (at 0.7874 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0 180) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.9525 0 180) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 174.864108 102.058412 180)
    (fp_text reference "R617" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 693 "FBB_CMD<6>"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 65.012715 82.865105)
    (fp_text reference "C1048" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 42 "FBF_VREF4"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 137.566697 58.17661 -90)
    (fp_text reference "C714" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 5.573108 95.264115 -90)
    (fp_text reference "C1247" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1919 "I2C1_SCL_CON"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 166.126508 143.499706)
    (fp_text reference "C654" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 138.313508 69.216212 180)
    (fp_text reference "C713" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 170.881413 104.04741)
    (fp_text reference "R628" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 749 "FBB_VREF1"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 68.672804 77.531105 180)
    (fp_text reference "C1031" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 83.246308 58.954612 -90)
    (fp_text reference "C995" (at 0 0.7874 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0 270) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.9525 0 270) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "IND_SMD_0603_1" (layer "B.Cu")
    (tedit 0)
    (at 6.823804 140.68691 -90)
    (fp_text reference "L504" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.762 0 90) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1688 "DACC_BLUE"))
    (pad "2" smd rect (at -0.762 0 270) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1927 "DACC_BLUE_CON"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 168.579615 89.124402)
    (fp_text reference "C638" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 691 "FBB_VREF3"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 165.161308 128.601412 180)
    (fp_text reference "C661" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 72.400508 131.255407)
    (fp_text reference "R774" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 979 "THERM_VDD"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 253.540608 113.170607 -90)
    (fp_text reference "R502" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 935 "PS5_NVVDD_IDES"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 146.746308 62.993212)
    (fp_text reference "R696" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 482 "FBD_CMD<0>"))
  )
  (footprint "0603_1" (layer "B.Cu")
    (tedit 0)
    (at 232.293508 124.587907)
    (fp_text reference "C529" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.762 0 180) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1002 "PS5_NVVDD_BOOT4_RC"))
    (pad "2" smd rect (at -0.762 0) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 11 "PS5_NVVDD_PHASE4"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 250.860908 115.799507 180)
    (fp_text reference "C507" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 934 "PS5_NVVDD_SET_IMON"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 932 "PS5_NVVDD_FBRTN"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 24.318308 113.310612 -90)
    (fp_text reference "C1201" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1698 "IFPAB_PLLVDD"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 107.173108 112.624812 90)
    (fp_text reference "C909" (at 0 -0.7874 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0 90) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.9525 0 90) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 42.141005 101.6878 90)
    (fp_text reference "C1127" (at 0 -1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0603_1" (layer "B.Cu")
    (tedit 0)
    (at 232.293508 88.316707)
    (fp_text reference "C527" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.762 0 180) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1007 "PS5_NVVDD_BOOT2_RC"))
    (pad "2" smd rect (at -0.762 0) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 14 "PS5_NVVDD_PHASE2"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 28.018605 101.334512 180)
    (fp_text reference "C1169" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 63.942308 122.366906)
    (fp_text reference "C1059" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 165.477309 115.05582 180)
    (fp_text reference "C657" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 67.365517 82.846817)
    (fp_text reference "C1039" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 126.096108 115.672812 -90)
    (fp_text reference "C765" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 129.124804 63.888511 -90)
    (fp_text reference "C742" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 31.489998 95.079508 90)
    (fp_text reference "R869" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1843 "DVIA_D2"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 71.873712 80.709407)
    (fp_text reference "C1016" (at -0.7874 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.9525 0) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 26.417415 109.716207 90)
    (fp_text reference "C1183" (at 0 -1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 70.978108 139.688207)
    (fp_text reference "R778" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 978 "THERM_SHDN*"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1997 "THERM_SHDN_R"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 113.952419 102.538396 90)
    (fp_text reference "C853" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 125.450923 100.636698)
    (fp_text reference "C771" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 169.752612 86.211504 180)
    (fp_text reference "R634" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 620 "FBC_VREF2"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 119.918803 102.538396 90)
    (fp_text reference "C811" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "IND_SMD_0603_1" (layer "B.Cu")
    (tedit 0)
    (at 122.463908 139.117012 180)
    (fp_text reference "LB502" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.762 0) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1643 "PEX_PLLVDD"))
    (pad "2" smd rect (at -0.762 0 180) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1972 "PEX_PLLVDD_OP"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 165.477309 144.900795 180)
    (fp_text reference "C659" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 67.422413 75.744215 180)
    (fp_text reference "C1038" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 167.421908 98.756412 180)
    (fp_text reference "R658" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 675 "FBB_CMD<23>"))
  )
  (footprint "0603_1" (layer "B.Cu")
    (tedit 0)
    (at 251.381608 97.092407 90)
    (fp_text reference "C505" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.762 0 270) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "2" smd rect (at -0.762 0 90) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 963 "PS5_NVVDD_VCC_VCC3"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 171.943108 116.056504)
    (fp_text reference "R621" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 750 "FBB_VREF2"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 202.296108 65.075707)
    (fp_text reference "R606" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 981 "12V_PEX6_F1"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1001 "5V_INPUT"))
  )
  (footprint "GEOM0013_1" (layer "B.Cu")
    (tedit 0)
    (at -99.086093 0.634916)
    (fp_text reference "MEC503" (at -1.905 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 167.979209 139.496716 90)
    (fp_text reference "R656" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2019 "FBA0_CLK0_R"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 876 "FBA0_CLK0*"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 31.269805 102.6022 180)
    (fp_text reference "C1157" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 103.312308 121.159212 -90)
    (fp_text reference "C940" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 27.607608 131.699907 90)
    (fp_text reference "C1174" (at 0 -1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1962 "PS1_1V15_CP"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1996 "PS1_1V15_CP_RC"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 112.634108 115.799812 -90)
    (fp_text reference "C870" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 60.106908 130.556907 -90)
    (fp_text reference "R829" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1982 "GPU_RST_R_MOS"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 118.342504 127.887418 90)
    (fp_text reference "C824" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "SOT23_1" (layer "B.Cu")
    (tedit 0)
    (at 52.131308 138.456307 90)
    (fp_text reference "Q510" (at -1.23825 1.23825 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2005 "JTAG_TRST_3V3"))
    (pad "2" smd rect (at -0.9525 1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "3" smd rect (at 0 -1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1912 "JTAG_TRST_3V3*"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 170.280907 143.499706)
    (fp_text reference "C630" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 8.815215 137.897812)
    (fp_text reference "R939" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1688 "DACC_BLUE"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 37.297708 130.709307 90)
    (fp_text reference "R853" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1810 "I2C4_SCL"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 25.416604 111.117296 90)
    (fp_text reference "C1189" (at 0 -1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "GEOM0021_1" (layer "B.Cu")
    (tedit 0)
    (at 57.897108 144.755812)
    (fp_text reference "J501" (at -3.1496 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 1.0668 1.0668) (drill 0.6604) (layers *.Cu *.Mask)
      (net 1562 "JTAG_TMS"))
    (pad "2" thru_hole circle (at 0 -2.54) (size 1.0668 1.0668) (drill 0.6604) (layers *.Cu *.Mask)
      (net 1180 "JTAG_TRST*"))
    (pad "3" thru_hole circle (at 1.27 0) (size 1.0668 1.0668) (drill 0.6604) (layers *.Cu *.Mask)
      (net 1969 "JTAG_TDI"))
    (pad "4" thru_hole circle (at 1.27 -2.54) (size 1.0668 1.0668) (drill 0.6604) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "5" thru_hole circle (at 2.54 0) (size 1.0668 1.0668) (drill 0.6604) (layers *.Cu *.Mask)
      (net 1009 "3V3"))
    (pad "7" thru_hole circle (at 3.81 0) (size 1.0668 1.0668) (drill 0.6604) (layers *.Cu *.Mask)
      (net 1970 "JTAG_TDO"))
    (pad "8" thru_hole circle (at 3.81 -2.54) (size 1.0668 1.0668) (drill 0.6604) (layers *.Cu *.Mask)
      (net 1559 "JTAG_TCK"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 30.211108 95.073615 90)
    (fp_text reference "R876" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1844 "DVIA_D3"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 243.926708 136.754507 -90)
    (fp_text reference "R536" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1973 "FAN_PWM"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 168.979893 139.496716 90)
    (fp_text reference "R642" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2019 "FBA0_CLK0_R"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 875 "FBA0_CLK0"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 27.418099 109.716207 90)
    (fp_text reference "C1176" (at 0 -1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 66.872198 88.631896 -90)
    (fp_text reference "R799" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2025 "FBF1_CLK0_R"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 33 "FBF1_CLK0*"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 173.813615 80.607299 180)
    (fp_text reference "C576" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 168.579615 74.20241)
    (fp_text reference "R645" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 619 "FBC_VREF1"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 5.750908 78.042712 -90)
    (fp_text reference "C1246" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1668 "DACB_Y"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1951 "DACB_Y_F"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 129.118708 58.789512 -90)
    (fp_text reference "C745" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 93.457108 64.999812 -90)
    (fp_text reference "R760" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 277 "FBE_CMD<25>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 96.467008 152.807815 -90)
    (fp_text reference "C974" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2047 "PEX_TX_C10"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1161 "PEX_TX10"))
  )
  (footprint "0603_1" (layer "B.Cu")
    (tedit 0)
    (at 241.285108 98.870407 90)
    (fp_text reference "R546" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.762 0 270) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1043 "PS5_NVVDD_VIN_PWM"))
    (pad "2" smd rect (at -0.762 0 90) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 962 "PS5_NVVDD_VCC"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 215.910508 104.801307 90)
    (fp_text reference "R599" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 998 "PS5_NVVDD_LG6_AC"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 32.362005 104.685 180)
    (fp_text reference "C1151" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1790 "2V5"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 63.981703 152.807815 -90)
    (fp_text reference "C1058" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2037 "PEX_TX_C2*"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1173 "PEX_TX2*"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 112.634108 122.403812 -90)
    (fp_text reference "C871" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 92.467016 152.807815 -90)
    (fp_text reference "C982" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2060 "PEX_TX_C9"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1184 "PEX_TX9"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 111.323011 56.275115)
    (fp_text reference "C877" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 122.311508 97.283212 -90)
    (fp_text reference "C797" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 63.486099 87.409216)
    (fp_text reference "C1064" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 61.467307 108.845012 180)
    (fp_text reference "C1083" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 164.221508 108.650906)
    (fp_text reference "C665" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 92.824115 57.87181 -90)
    (fp_text reference "C979" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 139.354908 57.837012 -90)
    (fp_text reference "C711" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 104.760413 73.737615 -90)
    (fp_text reference "R747" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 349 "FBE_CMD<5>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 66.671309 67.923809 180)
    (fp_text reference "C1043" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 230 "FBF_VREF2"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 126.676701 71.286515)
    (fp_text reference "C760" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 253.197708 101.092907 -90)
    (fp_text reference "C501" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 930 "PS5_NVVDD_EN"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 58.528806 85.540995 -90)
    (fp_text reference "C1109" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 146.746308 61.469212)
    (fp_text reference "R695" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 490 "FBD_VREF2"))
  )
  (footprint "IND_SMD_0603_1" (layer "B.Cu")
    (tedit 0)
    (at 5.827108 113.488615 -90)
    (fp_text reference "L509" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.762 0 90) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1679 "DACA_GREEN"))
    (pad "2" smd rect (at -0.762 0 270) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1921 "DACA_GREEN_CON"))
  )
  (footprint "SOT23_1" (layer "B.Cu")
    (tedit 0)
    (at 9.052908 133.554615 90)
    (fp_text reference "D529" (at -1.23825 1.23825 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "2" smd rect (at -0.9525 1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "3" smd rect (at 0 -1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1795 "GPIO0_DVIAB_HPD"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 171.181616 75.603499 180)
    (fp_text reference "C614" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 96.780901 71.286515)
    (fp_text reference "C972" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 163.078508 64.085412 180)
    (fp_text reference "C672" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 237.170308 130.760107)
    (fp_text reference "R557" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 942 "PS5_NVVDD_DRV_ODN"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1029 "PS5_NVVDD_DRV_PHASE4"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 177.200908 83.519714 90)
    (fp_text reference "C539" (at 0 -0.7874 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0 90) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.9525 0 90) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 40.896405 108.1648 180)
    (fp_text reference "C1128" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1661 "NVIO_GV_PLLAVDD"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 74.657298 82.88291 -90)
    (fp_text reference "C1004" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 110.566523 98.960806 -90)
    (fp_text reference "C882" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "SOT23_1" (layer "B.Cu")
    (tedit 0)
    (at 11.037715 143.104812 90)
    (fp_text reference "D522" (at -1.23825 1.23825 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "2" smd rect (at -0.9525 1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "3" smd rect (at 0 -1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1691 "DACC_RED"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 22.329005 94.6266 180)
    (fp_text reference "C1208" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1725 "IFPCD_IOVDD"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 173.813615 110.452299 180)
    (fp_text reference "C577" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 130.642708 56.198915 180)
    (fp_text reference "C734" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 123.934593 102.538396 90)
    (fp_text reference "C780" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 101.102508 125.858212)
    (fp_text reference "C957" (at -0.7874 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at -0.9525 0) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 18.958908 140.692015)
    (fp_text reference "R912" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2006 "DACC_HSYNC_BUF_R"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2007 "DACC_HSYNC_BUF"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 110.221108 114.910812 -90)
    (fp_text reference "C885" (at 0 0.7874 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0 270) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.9525 0 270) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 25.716807 101.334512 180)
    (fp_text reference "C1188" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 112.634108 109.195812 -90)
    (fp_text reference "C869" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 34.681508 87.529307 180)
    (fp_text reference "R856" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 990 "PS3_FBVDDQ_LG_G"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 78.928308 117.552615 180)
    (fp_text reference "C999" (at 0.7874 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0 180) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.9525 0 180) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 160.373408 97.37991 -90)
    (fp_text reference "C689" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 15.80372 80.391907 180)
    (fp_text reference "C1228" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1978 "PS3_FBVDDQ_FB_RC"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1109 "PS3_FBVDDQ_VSEN"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 67.351013 105.792212 180)
    (fp_text reference "C1040" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 175.461008 136.594512 90)
    (fp_text reference "C557" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 8.519508 78.042712 -90)
    (fp_text reference "C1233" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1668 "DACB_Y"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 234.147708 125.959507)
    (fp_text reference "R563" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1026 "PS5_NVVDD_BOOT4"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1002 "PS5_NVVDD_BOOT4_RC"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 113.269108 105.893812 90)
    (fp_text reference "C860" (at 0 -0.7874 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0 90) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.9525 0 90) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 109.433708 57.811612 -90)
    (fp_text reference "C891" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 42.572805 107.5552 90)
    (fp_text reference "C1126" (at 0 -1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 4.836508 71.426012 90)
    (fp_text reference "C1253" (at 0 -1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1953 "DACB_PR_F"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 19.179405 100.6972 180)
    (fp_text reference "C1218" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1725 "IFPCD_IOVDD"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "IND_SMD_0402_1" (layer "B.Cu")
    (tedit 0)
    (at 7.224108 95.264115 90)
    (fp_text reference "LB517" (at 0 -1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.6858 0.5334) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2001 "I2C1_SCL_R"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.6858 0.5334) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1919 "I2C1_SCL_CON"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 69.459213 118.974812 180)
    (fp_text reference "R783" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 163 "FBG_CMD<27>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 137.566697 61.031519 -90)
    (fp_text reference "C715" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2020 "FBD0_CLK0_R"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 49.870708 145.263812 -90)
    (fp_text reference "R843" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1970 "JTAG_TDO"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1911 "JTAG_TDO_NVIO"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 19.011715 102.811014)
    (fp_text reference "C1220" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1722 "IFPCD_PLLVDD"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 115.943703 100.509698)
    (fp_text reference "C843" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 175.384808 129.67761 90)
    (fp_text reference "C567" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 24.432608 130.683907)
    (fp_text reference "C1200" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1915 "PS1_2V5_LDO_DR_AC"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1916 "PS1_2V5_LDO_FB"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 247.787508 117.806107 180)
    (fp_text reference "R524" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 999 "NVVDD_SENSE_R"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 22.133908 115.266412 90)
    (fp_text reference "C1209" (at 0 -1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1701 "IFPAB_IOVDD"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 23.861108 129.032907 90)
    (fp_text reference "R897" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1790 "2V5"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1916 "PS1_2V5_LDO_FB"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 126.604108 73.356412 180)
    (fp_text reference "C762" (at 0.7874 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0 180) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.9525 0 180) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 127.952797 109.24331 -90)
    (fp_text reference "C755" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 134.440491 60.478307 -90)
    (fp_text reference "C721" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 251.064108 110.109907 90)
    (fp_text reference "C506" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 932 "PS5_NVVDD_FBRTN"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 162.418108 79.376212 90)
    (fp_text reference "C677" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 66.971512 118.384694 -90)
    (fp_text reference "R798" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2027 "FBG1_CLK0_R"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 169 "FBG1_CLK0*"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 117.333108 151.994812 180)
    (fp_text reference "C829" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2052 "PEX_TX_C15"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1168 "PEX_TX15"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 67.198613 111.227812)
    (fp_text reference "R793" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 173 "FBG_VREF4"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 103.143601 60.77851 90)
    (fp_text reference "R749" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 359 "FBE_VREF1"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 103.185308 113.437612)
    (fp_text reference "C943" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "SOT23_1" (layer "B.Cu")
    (tedit 0)
    (at 9.827608 114.250615 90)
    (fp_text reference "D528" (at -1.23825 1.23825 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "2" smd rect (at -0.9525 1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "3" smd rect (at 0 -1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1679 "DACA_GREEN"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 176.111197 118.245502 -90)
    (fp_text reference "C549" (at 0 0.7874 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0 270) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.9525 0 270) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 71.872213 119.152815)
    (fp_text reference "C1017" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 160.373408 136.594512 90)
    (fp_text reference "C693" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 57.724413 120.829012 90)
    (fp_text reference "C1114" (at 0 -0.7874 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0 90) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.9525 0 90) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 119.517508 65.380812 90)
    (fp_text reference "R730" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 411 "FBD_CMD<26>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 15.148908 140.692015)
    (fp_text reference "R923" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2008 "DACA_HSYNC_BUF_R"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2009 "DACA_HSYNC_BUF"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 40.777508 104.598412 -90)
    (fp_text reference "R846" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1660 "NET0010"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "IND_SMD_0603_1" (layer "B.Cu")
    (tedit 0)
    (at 6.823804 147.16391 -90)
    (fp_text reference "L506" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.762 0 90) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1689 "DACC_GREEN"))
    (pad "2" smd rect (at -0.762 0 270) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1930 "DACC_GREEN_CON"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 59.464313 118.816011 -90)
    (fp_text reference "R832" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 174 "FBG_ZQ2"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "IND_SMD_0402_1" (layer "B.Cu")
    (tedit 0)
    (at 7.224108 99.074115 -90)
    (fp_text reference "LB518" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.6858 0.5334) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2002 "I2C1_SDA_R"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.6858 0.5334) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1920 "I2C1_SDA_CON"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 99.229004 69.385096 90)
    (fp_text reference "C963" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 86.421308 58.954612 -90)
    (fp_text reference "C992" (at 0 0.7874 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0 270) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.9525 0 270) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "GEOM0009_1" (layer "B.Cu")
    (tedit 0)
    (at 233.855608 82.233407 90)
    (fp_text reference "U502" (at -1.353464 1.35349 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.750113 1.376883 270) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1013 "PS5_NVVDD_BOOT1"))
    (pad "2" smd rect (at 0.249911 1.376883 270) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 945 "PS5_NVVDD_PWM1"))
    (pad "3" smd rect (at -0.249911 1.376883 270) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 941 "PS5_NVVDD_DRV_OD1"))
    (pad "4" smd rect (at -0.750087 1.376883 270) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1016 "12V_PH1"))
    (pad "5" smd rect (at -0.750087 -1.376909 90) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1015 "PS5_NVVDD_LG1"))
    (pad "6" smd rect (at -0.249911 -1.376909 90) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "7" smd rect (at 0.249911 -1.376909 90) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 8 "PS5_NVVDD_PHASE1"))
    (pad "8" smd rect (at 0.750113 -1.376909 90) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1014 "PS5_NVVDD_UG1"))
    (pad "9" smd rect (at 0 0 90) (size 1.850111 1.5494) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 221.384208 78.245607 90)
    (fp_text reference "R585" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1015 "PS5_NVVDD_LG1"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2083 "PS5_NVVDD_LG1_D"))
  )
  (footprint "SOT23_1" (layer "B.Cu")
    (tedit 0)
    (at 27.467908 127.381907 -90)
    (fp_text reference "Q514" (at 1.23825 -1.23825 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 1.143 270) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1995 "PS1_1V15_EN*"))
    (pad "2" smd rect (at -0.9525 1.143 270) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "3" smd rect (at 0 -1.143 270) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1917 "PS1_1V15_FS"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 177.200908 142.828714 90)
    (fp_text reference "C544" (at 0 -0.7874 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0 90) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.9525 0 90) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "GEOM0007_1" (layer "B.Cu")
    (tedit 0)
    (at 72.146508 134.824107 90)
    (fp_text reference "U510" (at -1.905 1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.975411 2.1717 90) (size 0.4064 1.905) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 979 "THERM_VDD"))
    (pad "2" smd rect (at 0.325095 2.1717 90) (size 0.4064 1.905) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 974 "THERM_DP"))
    (pad "3" smd rect (at -0.325095 2.1717 90) (size 0.4064 1.905) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 975 "THERM_DN"))
    (pad "4" smd rect (at -0.975385 2.1717 90) (size 0.4064 1.905) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 978 "THERM_SHDN*"))
    (pad "5" smd rect (at -0.975385 -2.1717 90) (size 0.4064 1.905) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "6" smd rect (at -0.325095 -2.1717 90) (size 0.4064 1.905) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 973 "GPIO9_THERM_ALERT*"))
    (pad "7" smd rect (at 0.325095 -2.1717 90) (size 0.4064 1.905) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 977 "I2C3_SDA_R"))
    (pad "8" smd rect (at 0.975411 -2.1717 90) (size 0.4064 1.905) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 976 "I2C3_SCL_R"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 165.415308 124.918412 180)
    (fp_text reference "R675" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 807 "FBA_CMD<24>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 130.083908 105.385812 180)
    (fp_text reference "C736" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 66.244005 124.815516 180)
    (fp_text reference "C1046" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 172 "FBG_VREF3"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 24.140508 106.503412 -90)
    (fp_text reference "C1202" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1683 "DACA_VDD"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 127.416908 97.816612 90)
    (fp_text reference "R720" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1250 "FB_CAL_PU_GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 32.514405 108.0378 180)
    (fp_text reference "C1148" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 167.650508 57.329012)
    (fp_text reference "C644" (at -0.7874 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.9525 0) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "SOT23_1" (layer "B.Cu")
    (tedit 0)
    (at 242.326508 133.884307 -90)
    (fp_text reference "D501" (at 1.23825 -1.23825 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 1.143 270) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1975 "FAN_TACH"))
    (pad "2" smd rect (at -0.9525 1.143 270) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1973 "FAN_PWM"))
    (pad "3" smd rect (at 0 -1.143 270) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 175.461008 123.921411 90)
    (fp_text reference "R615" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 824 "FBA_ZQ2"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "DIODE_SMD_SMA_1" (layer "B.Cu")
    (tedit 0)
    (at 203.058108 104.267907 -90)
    (fp_text reference "D514" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -1.880108 0 270) (size 2.159 2.032) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 13 "PS5_NVVDD_PHASE6"))
    (pad "2" smd rect (at 1.880108 0 270) (size 2.159 2.032) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 117.044615 124.855115)
    (fp_text reference "C832" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 175.461008 138.844394 90)
    (fp_text reference "R616" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 881 "FBA_ZQ1"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 63.068497 96.800815 180)
    (fp_text reference "R824" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 115 "FBG_VREF2"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 171.181616 90.525516 180)
    (fp_text reference "C615" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 166.277917 117.958812)
    (fp_text reference "R668" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 799 "FBA_CMD<28>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 123.068403 56.198915 180)
    (fp_text reference "R725" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 434 "FBD_ZQ2"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 7.224108 107.900615 -90)
    (fp_text reference "C1238" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1681 "DACA_RED"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 165.477309 133.89241 180)
    (fp_text reference "C658" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 205.788608 59.119407 90)
    (fp_text reference "R604" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1956 "SPDIF_IN"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1957 "SPDIF_IN_COMP2_Q"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 14.082108 107.569907)
    (fp_text reference "R927" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1681 "DACA_RED"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 124.750416 98.935406 -90)
    (fp_text reference "R721" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1056 "FB_CAL_PD_VDDQ"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 93.172603 56.224315 180)
    (fp_text reference "R762" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 304 "FBE_ZQ2"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 38.313708 130.709307 -90)
    (fp_text reference "R850" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1810 "I2C4_SCL"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 5.446108 133.325812 90)
    (fp_text reference "R944" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1795 "GPIO0_DVIAB_HPD"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 158.379508 69.800412 90)
    (fp_text reference "C695" (at 0 -0.7874 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0 90) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.9525 0 90) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 130.134708 66.182614 -90)
    (fp_text reference "C735" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 24.940608 129.032907 -90)
    (fp_text reference "R895" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1916 "PS1_2V5_LDO_FB"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "IND_SMD_0603_1" (layer "B.Cu")
    (tedit 0)
    (at 7.147908 78.271312 -90)
    (fp_text reference "L503" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.762 0 90) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1668 "DACB_Y"))
    (pad "2" smd rect (at -0.762 0 270) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1951 "DACB_Y_F"))
  )
  (footprint "0603_1" (layer "B.Cu")
    (tedit 0)
    (at 233.563508 86.640307 180)
    (fp_text reference "R566" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.762 0) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 981 "12V_PEX6_F1"))
    (pad "2" smd rect (at -0.762 0 180) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1016 "12V_PH1"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 175.384808 69.98761 90)
    (fp_text reference "C559" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 189.786608 68.390407 90)
    (fp_text reference "C538" (at 0 -0.7874 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0 90) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1914 "5V"))
    (pad "2" smd rect (at -0.9525 0 90) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "IND_SMD_0603_1" (layer "B.Cu")
    (tedit 0)
    (at 7.249508 67.997012 90)
    (fp_text reference "L501" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.762 0 270) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1669 "DACB_PB"))
    (pad "2" smd rect (at -0.762 0 90) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1954 "DACB_PB_F"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 105.801508 74.067612 -90)
    (fp_text reference "R746" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 350 "FBE_CMD<4>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 116.825108 126.493212 -90)
    (fp_text reference "C837" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "IND_SMD_0402_1" (layer "B.Cu")
    (tedit 0)
    (at 25.105708 119.952712 -90)
    (fp_text reference "LB510" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.6858 0.5334) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.6858 0.5334) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1693 "DACC_VDD"))
  )
  (footprint "0603_1" (layer "B.Cu")
    (tedit 0)
    (at 233.563508 107.950907 180)
    (fp_text reference "R568" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.762 0) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 981 "12V_PEX6_F1"))
    (pad "2" smd rect (at -0.762 0 180) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1038 "12V_PH6"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 227.315108 89.967707 90)
    (fp_text reference "R583" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1019 "PS5_NVVDD_LG2"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 994 "PS5_NVVDD_LG2_AC"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 63.786911 92.500316)
    (fp_text reference "C1062" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "GEOM0009_1" (layer "B.Cu")
    (tedit 0)
    (at 233.804808 115.431207 90)
    (fp_text reference "U506" (at -1.353464 1.35349 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.750113 1.376883 270) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1031 "PS5_NVVDD_BOOT5"))
    (pad "2" smd rect (at 0.249911 1.376883 270) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 949 "PS5_NVVDD_PWM5"))
    (pad "3" smd rect (at -0.249911 1.376883 270) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 942 "PS5_NVVDD_DRV_ODN"))
    (pad "4" smd rect (at -0.750087 1.376883 270) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1034 "12V_PH5"))
    (pad "5" smd rect (at -0.750087 -1.376909 90) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1033 "PS5_NVVDD_LG5"))
    (pad "6" smd rect (at -0.249911 -1.376909 90) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "7" smd rect (at 0.249911 -1.376909 90) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "PS5_NVVDD_PHASE5"))
    (pad "8" smd rect (at 0.750113 -1.376909 90) (size 0.2794 0.753897) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1032 "PS5_NVVDD_UG5"))
    (pad "9" smd rect (at 0 0 90) (size 1.850111 1.5494) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 51.064508 76.708907 180)
    (fp_text reference "C1119" (at 0.7874 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0 180) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.9525 0 180) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 138.186508 65.634812 180)
    (fp_text reference "R701" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 483 "FBD_CMD<2>"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 145.908108 57.849407 -90)
    (fp_text reference "C701" (at 0 0.7874 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0 270) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.9525 0 270) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 106.538108 109.322812 -90)
    (fp_text reference "C912" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 175.461008 91.826504 90)
    (fp_text reference "C554" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 61.467307 107.443898)
    (fp_text reference "C1082" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 110.221108 121.514812 -90)
    (fp_text reference "C886" (at 0 0.7874 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0 270) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.9525 0 270) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 162.799108 58.040212 180)
    (fp_text reference "R681" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 540 "FBC_CMD<28>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 71.867413 67.76892 180)
    (fp_text reference "C1018" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 62.507208 130.556907 -90)
    (fp_text reference "C1073" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1998 "THERM_SHDN_Q"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 5.477604 140.056812 90)
    (fp_text reference "C1249" (at 0 -1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1927 "DACC_BLUE_CON"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 27.217997 116.020995 180)
    (fp_text reference "C1179" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1698 "IFPAB_PLLVDD"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 88.220619 58.17661 90)
    (fp_text reference "C988" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 173.813615 65.685612 180)
    (fp_text reference "C575" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0603_1" (layer "B.Cu")
    (tedit 0)
    (at 232.014108 136.932307)
    (fp_text reference "C531" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.762 0 180) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1003 "PS5_NVVDD_BOOT3_RC"))
    (pad "2" smd rect (at -0.762 0) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 10 "PS5_NVVDD_PHASE3"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 23.715312 110.416714)
    (fp_text reference "C1204" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "SOT23_1" (layer "B.Cu")
    (tedit 0)
    (at 11.037715 146.914812 90)
    (fp_text reference "D523" (at -1.23825 1.23825 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "2" smd rect (at -0.9525 1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "3" smd rect (at 0 -1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1689 "DACC_GREEN"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 7.224108 103.328615 -90)
    (fp_text reference "C1237" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1678 "DACA_BLUE"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 64.669815 114.160699 180)
    (fp_text reference "C1053" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 109.433708 60.072212 -90)
    (fp_text reference "C892" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 249.984608 94.869907 -90)
    (fp_text reference "R512" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 951 "PS5_NVVDD_PGOOD"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2003 "PS5_NVVDD_PGOOD_R"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 248.968608 92.202907 -90)
    (fp_text reference "C510" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2003 "PS5_NVVDD_PGOOD_R"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 25.123005 117.0802 180)
    (fp_text reference "C1193" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1693 "DACC_VDD"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 167.650508 77.268012 -90)
    (fp_text reference "C645" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 154.925108 59.538812 180)
    (fp_text reference "C698" (at 0.7874 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0 180) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.9525 0 180) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 59.464313 103.893003 -90)
    (fp_text reference "R831" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 117 "FBG_ZQ1"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 6.144608 100.788615 180)
    (fp_text reference "C1243" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1918 "DACA_BLUE_CON"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 19.312019 95.205212 90)
    (fp_text reference "R909" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1786 "MIOB_VREF"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 6.208108 105.360615 180)
    (fp_text reference "C1241" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1924 "DACA_RED_CON"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 20.457508 110.110212)
    (fp_text reference "C1216" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 170.280907 83.809706)
    (fp_text reference "C626" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 40.701308 130.709307 90)
    (fp_text reference "R847" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1812 "I2C4_SDA"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2090 "I2C4_SDA_R"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 32.02162 97.707112 -90)
    (fp_text reference "C1153" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 129.677508 106.389112 180)
    (fp_text reference "C739" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "IND_SMD_0603_1" (layer "B.Cu")
    (tedit 0)
    (at 5.827108 107.519615 -90)
    (fp_text reference "L508" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.762 0 90) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1681 "DACA_RED"))
    (pad "2" smd rect (at -0.762 0 270) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1924 "DACA_RED_CON"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 104.455308 98.883412 180)
    (fp_text reference "C935" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1282 "FBEFGH_MPLL_AVDD"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 122.921108 65.888812 90)
    (fp_text reference "R726" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 409 "FBD_CMD<27>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 124.826108 122.276812 -90)
    (fp_text reference "C775" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 250.606908 112.395907 -90)
    (fp_text reference "C508" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1039 "PS5_NVVDD_CP_RC"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 926 "PS5_NVVDD_CP"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 118.730108 109.195812 -90)
    (fp_text reference "C819" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 173.483415 59.279402)
    (fp_text reference "C579" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 30.634805 106.5138 90)
    (fp_text reference "C1161" (at 0 -1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 176.108708 95.759212 180)
    (fp_text reference "C551" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 110.856108 118.212812 90)
    (fp_text reference "C881" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 234.147708 79.223507)
    (fp_text reference "R560" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1013 "PS5_NVVDD_BOOT1"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1006 "PS5_NVVDD_BOOT1_RC"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 23.861108 132.398407 -90)
    (fp_text reference "R898" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1963 "PS1_2V5_LDO_DR"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1915 "PS1_2V5_LDO_DR_AC"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 170.881413 60.679704 180)
    (fp_text reference "C622" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 167.625108 107.189212 -90)
    (fp_text reference "C646" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 103.921908 128.220412 90)
    (fp_text reference "C938" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 162.274801 130.09262)
    (fp_text reference "C682" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 248.968608 89.840707 90)
    (fp_text reference "R516" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2003 "PS5_NVVDD_PGOOD_R"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 23.131595 106.5138 -90)
    (fp_text reference "C1205" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1683 "DACA_VDD"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 67.635011 69.358401)
    (fp_text reference "C1037" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 170.280907 113.654706)
    (fp_text reference "C628" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "SOT23_1" (layer "B.Cu")
    (tedit 0)
    (at 6.919308 81.852407 -90)
    (fp_text reference "D530" (at 1.23825 -1.23825 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 1.143 270) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "2" smd rect (at -0.9525 1.143 270) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "3" smd rect (at 0 -1.143 270) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1668 "DACB_Y"))
  )
  (footprint "SOT23_1" (layer "B.Cu")
    (tedit 0)
    (at 242.097908 93.574507 180)
    (fp_text reference "D502" (at -1.23825 -1.23825 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 1.143 180) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 981 "12V_PEX6_F1"))
    (pad "2" smd rect (at -0.9525 1.143 180) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "3" smd rect (at 0 -1.143 180) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1043 "PS5_NVVDD_VIN_PWM"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 92.824115 60.123012 -90)
    (fp_text reference "C980" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 65.970701 73.327913 -90)
    (fp_text reference "R808" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2024 "FBF0_CLK0_R"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 226 "FBF0_CLK0*"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 240.104313 102.757115)
    (fp_text reference "R548" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 8 "PS5_NVVDD_PHASE1"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 929 "PS5_NVVDD_VAMP_CSSUM"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 15.80372 84.823216 180)
    (fp_text reference "R920" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1054 "PS3_FBVDDQ_CP_RC"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1055 "PS3_FBVDDQ_FB"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 123.44892 62.578404 180)
    (fp_text reference "R723" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2021 "FBD1_CLK0_R"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 423 "FBD1_CLK0"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 161.681508 109.703812 -90)
    (fp_text reference "C685" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 35.537005 107.6822)
    (fp_text reference "C1142" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1661 "NVIO_GV_PLLAVDD"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 64.669815 69.324898 180)
    (fp_text reference "C1050" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 27.036108 134.392612 180)
    (fp_text reference "R888" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1958 "PS1_1V15_FB"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1960 "PS1_1V15_FB_SEN"))
  )
  (footprint "SO14_I335X150_1" (layer "B.Cu")
    (tedit 0)
    (at 23.080617 85.305816 -90)
    (fp_text reference "U512" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 3.81 2.5908 270) (size 0.6096 2.032) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1040 "PS3_FBVDDQ_BOOT"))
    (pad "2" smd rect (at 2.54 2.5908 270) (size 0.6096 2.032) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1057 "PS3_FS_DIS"))
    (pad "3" smd rect (at 1.27 2.5908 270) (size 0.6096 2.032) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1965 "PS3_FBVDDQ_CP"))
    (pad "4" smd rect (at 0 2.5908 270) (size 0.6096 2.032) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1055 "PS3_FBVDDQ_FB"))
    (pad "5" smd rect (at -1.27 2.5908 270) (size 0.6096 2.032) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1966 "PS3_LDO_RC"))
    (pad "6" smd rect (at -2.54 2.5908 270) (size 0.6096 2.032) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1966 "PS3_LDO_RC"))
    (pad "7" smd rect (at -3.81 2.5908 270) (size 0.6096 2.032) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "8" smd rect (at -3.81 -2.5908 270) (size 0.6096 2.032) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1044 "12V_PS3_R"))
    (pad "9" smd rect (at -2.54 -2.5908 270) (size 0.6096 2.032) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1046 "PS3_VCC5"))
    (pad "10" smd rect (at -1.27 -2.5908 270) (size 0.6096 2.032) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1045 "PS3_PVCC5_DRV"))
    (pad "11" smd rect (at 0 -2.5908 270) (size 0.6096 2.032) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1968 "PS3_FBVDDQ_LG"))
    (pad "12" smd rect (at 1.27 -2.5908 270) (size 0.6096 2.032) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "13" smd rect (at 2.54 -2.5908 270) (size 0.6096 2.032) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 989 "PS3_FBVDDQ_PHASE"))
    (pad "14" smd rect (at 3.81 -2.5908 270) (size 0.6096 2.032) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1967 "PS3_FBVDDQ_UG"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 173.483415 68.886698 180)
    (fp_text reference "C581" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 240.104313 107.329115)
    (fp_text reference "R551" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 11 "PS5_NVVDD_PHASE4"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 929 "PS5_NVVDD_VAMP_CSSUM"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 177.048508 65.025212 -90)
    (fp_text reference "C546" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 218.933108 125.172107 90)
    (fp_text reference "R593" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 985 "PS5_NVVDD_UG4_R"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 11 "PS5_NVVDD_PHASE4"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 106.284108 127.763415 90)
    (fp_text reference "R745" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1511 "GV_RX_RSET_VDD"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 40.515405 102.1958 180)
    (fp_text reference "C1130" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1662 "NVIO_GV_PLLVDD"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 71.047399 89.07952 180)
    (fp_text reference "C1023" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 63.068497 97.836602)
    (fp_text reference "C1069" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 84.483009 152.807815 -90)
    (fp_text reference "C993" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2042 "PEX_TX_C7*"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1183 "PEX_TX7*"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 25.402405 106.5138 -90)
    (fp_text reference "C1191" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 25.816908 136.069012 90)
    (fp_text reference "R893" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1958 "PS1_1V15_FB"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 104.823608 108.535412 90)
    (fp_text reference "C926" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 59.445009 76.18361 -90)
    (fp_text reference "C1106" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 33.538508 67.793507)
    (fp_text reference "R861" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1801 "GPIO14_RASTERSYNC2"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1075 "GPIO14_RASTERSYNC2_R"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 59.464313 106.14291 -90)
    (fp_text reference "C1104" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 118.116393 58.17661 90)
    (fp_text reference "C827" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 115.809108 126.493212 -90)
    (fp_text reference "C847" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 250.860908 117.831507)
    (fp_text reference "R509" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 932 "PS5_NVVDD_FBRTN"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "GEOM0013_1" (layer "B.Cu")
    (tedit 0)
    (at -99.086093 0.634916)
    (fp_text reference "MEC502" (at -1.905 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 171.943108 144.900795 180)
    (fp_text reference "C605" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 66.244005 123.767995 180)
    (fp_text reference "R805" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 172 "FBG_VREF3"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 131.6709 143.500214 180)
    (fp_text reference "C731" (at 0.7874 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0 180) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at -0.9525 0 180) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 113.904108 109.195812 -90)
    (fp_text reference "C854" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 64.564608 138.621407)
    (fp_text reference "R818" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1980 "THERM_LATCH"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 252.524608 115.431207 90)
    (fp_text reference "C503" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1042 "NET0008"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 250.860908 116.815507)
    (fp_text reference "R508" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 932 "PS5_NVVDD_FBRTN"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1655 "NVVDD_SENSE_GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 14.971108 129.413907 180)
    (fp_text reference "R926" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2010 "DACA_VSYNC_BUF_R"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2011 "DACA_VSYNC_BUF"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 98.537108 128.499812)
    (fp_text reference "C966" (at -0.7874 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at -0.9525 0) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 108.798708 67.438212 90)
    (fp_text reference "R738" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 354 "FBE_CMD<1>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 173.816612 125.374316 180)
    (fp_text reference "C574" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 119.346312 124.855115)
    (fp_text reference "C817" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 113.904108 122.403812 -90)
    (fp_text reference "C856" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "SOT23_1" (layer "B.Cu")
    (tedit 0)
    (at 58.278108 138.354707 90)
    (fp_text reference "Q508" (at -1.23825 1.23825 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2004 "JTAG_TRST2"))
    (pad "2" smd rect (at -0.9525 1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "3" smd rect (at 0 -1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2005 "JTAG_TRST_3V3"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 104.835317 106.263306 90)
    (fp_text reference "C925" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 32.751108 91.822415 90)
    (fp_text reference "R865" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1842 "DVIA_D1"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 123.1492 100.636698 180)
    (fp_text reference "C782" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 52.944108 145.263812 90)
    (fp_text reference "R839" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1969 "JTAG_TDI"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1910 "JTAG_TDI_NVIO"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 40.752108 98.527812 -90)
    (fp_text reference "C1129" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1664 "NVIO_SP_PLLVDD"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 122.273916 126.78201 -90)
    (fp_text reference "C798" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 68.134121 152.807815 -90)
    (fp_text reference "C1036" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2038 "PEX_TX_C3*"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1645 "PEX_TX3*"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 171.181616 120.370516 180)
    (fp_text reference "C617" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "SOT23_1" (layer "B.Cu")
    (tedit 0)
    (at 238.008508 91.847307 90)
    (fp_text reference "D503" (at -1.23825 1.23825 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1006 "PS5_NVVDD_BOOT1_RC"))
    (pad "2" smd rect (at -0.9525 1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1007 "PS5_NVVDD_BOOT2_RC"))
    (pad "3" smd rect (at 0 -1.143 90) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 981 "12V_PEX6_F1"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 231.899808 89.688307)
    (fp_text reference "R573" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1018 "PS5_NVVDD_UG2"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 988 "PS5_NVVDD_UG2_R"))
  )
  (footprint "0603_1" (layer "B.Cu")
    (tedit 0)
    (at 26.045508 138.024507)
    (fp_text reference "C1184" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.762 0 180) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "2" smd rect (at -0.762 0) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1047 "PS1_PVCC5"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 122.844908 128.423612 180)
    (fp_text reference "C787" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1643 "PEX_PLLVDD"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 107.808108 115.926812 -90)
    (fp_text reference "C904" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 166.329708 73.000812)
    (fp_text reference "R664" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 563 "FBC_CMD<6>"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 114.133013 59.970815 -90)
    (fp_text reference "R736" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 360 "FBE_VREF2"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 104.201308 101.728212)
    (fp_text reference "R748" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1306 "FBF_DEBUG"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 121.778108 118.085812 90)
    (fp_text reference "C803" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 170.280907 98.731698)
    (fp_text reference "C627" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 166.177816 135.293499)
    (fp_text reference "C653" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 176.111197 88.520212 -90)
    (fp_text reference "C548" (at 0 0.7874 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0 270) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.9525 0 270) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 24.470708 124.664107 90)
    (fp_text reference "C1199" (at 0 -1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 74.437613 110.948412 -90)
    (fp_text reference "R771" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 110 "FBG_CMD<10>"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 106.766708 100.661412)
    (fp_text reference "R744" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1286 "FBE_DEBUG"))
  )
  (footprint "0603_1" (layer "B.Cu")
    (tedit 0)
    (at 232.242708 111.049707)
    (fp_text reference "C530" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.762 0 180) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1004 "PS5_NVVDD_BOOT5_RC"))
    (pad "2" smd rect (at -0.762 0) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "PS5_NVVDD_PHASE5"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 108.467009 152.807815 -90)
    (fp_text reference "C897" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2050 "PEX_TX_C13"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1166 "PEX_TX13"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 77.557013 71.12172 90)
    (fp_text reference "C1000" (at 0 -0.7874 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0 90) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.9525 0 90) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 21.413615 105.163511)
    (fp_text reference "C1213" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1684 "DACA_VREF"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 57.516616 72.924815 90)
    (fp_text reference "C1115" (at 0 -0.7874 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0 90) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.9525 0 90) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 127.723715 67.783804 90)
    (fp_text reference "C758" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 65.871413 88.631896 -90)
    (fp_text reference "R811" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2025 "FBF1_CLK0_R"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 32 "FBF1_CLK0"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 125.461108 105.766812 90)
    (fp_text reference "C768" (at 0 -0.7874 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0 90) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.9525 0 90) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 71.083315 84.194008 180)
    (fp_text reference "C1021" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 112.441119 124.855115 180)
    (fp_text reference "C872" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 31.244405 111.6954 180)
    (fp_text reference "C1159" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 107.790811 56.224315 180)
    (fp_text reference "R742" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 361 "FBE_ZQ1"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 253.540608 110.109907 -90)
    (fp_text reference "R501" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 953 "PS5_NVVDD_FS"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 106.512708 122.403812 -90)
    (fp_text reference "C914" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 133.039401 60.77851 90)
    (fp_text reference "R706" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 489 "FBD_VREF1"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 21.440005 100.6718 180)
    (fp_text reference "R904" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1723 "IFPCD_RSET"))
  )
  (footprint "0603_1" (layer "B.Cu")
    (tedit 0)
    (at 233.512708 118.187107)
    (fp_text reference "C524" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.762 0 180) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1034 "12V_PH5"))
    (pad "2" smd rect (at -0.762 0) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0603_1" (layer "B.Cu")
    (tedit 0)
    (at 131.17052 141.398592 180)
    (fp_text reference "C732" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.762 0) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at -0.762 0 180) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 162.274801 74.20241)
    (fp_text reference "C679" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 59.570714 83.277804 -90)
    (fp_text reference "C1096" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 130.922108 113.513812 180)
    (fp_text reference "C733" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "SO08_I190X150_1" (layer "B.Cu")
    (tedit 0)
    (at 19.924108 123.368707 -90)
    (fp_text reference "U513" (at 1.905 -1.905 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 1.905 2.590495 270) (size 0.6096 2.032) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1008 "ROM_CS*"))
    (pad "2" smd rect (at 0.635 2.590495 270) (size 0.6096 2.032) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1012 "STRAP2"))
    (pad "3" smd rect (at -0.635 2.590495 270) (size 0.6096 2.032) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "4" smd rect (at -1.905 2.590495 270) (size 0.6096 2.032) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "5" smd rect (at -1.905 -2.590495 270) (size 0.6096 2.032) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1011 "STRAP1"))
    (pad "6" smd rect (at -0.635 -2.590495 270) (size 0.6096 2.032) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1010 "STRAP0"))
    (pad "7" smd rect (at 0.635 -2.590495 270) (size 0.6096 2.032) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "8" smd rect (at 1.905 -2.590495 270) (size 0.6096 2.032) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
  )
  (footprint "0603_1" (layer "B.Cu")
    (tedit 0)
    (at 103.921908 111.049707)
    (fp_text reference "C937" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.762 0 180) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.762 0) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 240.104313 101.106115)
    (fp_text reference "R547" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 962 "PS5_NVVDD_VCC"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 950 "PS5_NVVDD_PWM6"))
  )
  (footprint "IND_SMD_0402_1" (layer "B.Cu")
    (tedit 0)
    (at 22.329005 93.6106)
    (fp_text reference "LB513" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.6858 0.5334) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1053 "IFP_IOVDD"))
    (pad "2" smd rect (at -0.5334 0) (size 0.6858 0.5334) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1725 "IFPCD_IOVDD"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 173.483415 78.805906 180)
    (fp_text reference "C584" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0603_1" (layer "B.Cu")
    (tedit 0)
    (at 44.308108 110.186412)
    (fp_text reference "C1122" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.762 0 180) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at -0.762 0) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 23.861108 138.253107 -90)
    (fp_text reference "R899" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1048 "PS1_VCC5"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1047 "PS1_PVCC5"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 24.877108 97.054612 180)
    (fp_text reference "C1195" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1673 "DACB_VDD"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 68.519413 122.366906 180)
    (fp_text reference "R788" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 165 "FBG_CMD<26>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 107.747123 58.17661 -90)
    (fp_text reference "C905" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 89.482999 152.807815 -90)
    (fp_text reference "C986" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2043 "PEX_TX_C8*"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1160 "PEX_TX8*"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 22.464616 108.365918)
    (fp_text reference "C1207" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1683 "DACA_VDD"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 173.483415 60.680516 180)
    (fp_text reference "C580" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 173.483415 128.576698 180)
    (fp_text reference "C595" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 116.444108 128.132198)
    (fp_text reference "C839" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 61.467307 74.328698)
    (fp_text reference "C1076" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 242.390287 105.551115)
    (fp_text reference "R540" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 956 "PS5_NVVDD_ISEN3"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 10 "PS5_NVVDD_PHASE3"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 136.357708 64.110812)
    (fp_text reference "C718" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "DIODE_SMD_SMA_1" (layer "B.Cu")
    (tedit 0)
    (at 203.058108 117.094907 -90)
    (fp_text reference "D515" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -1.880108 0 270) (size 2.159 2.032) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "PS5_NVVDD_PHASE5"))
    (pad "2" smd rect (at 1.880108 0 270) (size 2.159 2.032) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0603_1" (layer "B.Cu")
    (tedit 0)
    (at 233.284108 144.069707)
    (fp_text reference "C525" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.762 0 180) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1025 "12V_PH3"))
    (pad "2" smd rect (at -0.762 0) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 73.218413 103.506415 90)
    (fp_text reference "C1009" (at 0 -1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 116.952108 111.608812 90)
    (fp_text reference "C834" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 160.373408 127.22491 -90)
    (fp_text reference "C691" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 248.968608 94.869907 90)
    (fp_text reference "R517" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 964 "PS5_NVVDD_VID0"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 70.725099 104.317716 180)
    (fp_text reference "C1025" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0603_1" (layer "B.Cu")
    (tedit 0)
    (at 132.471508 108.789412 180)
    (fp_text reference "C728" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.762 0) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.762 0 180) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 66.971512 73.327913 -90)
    (fp_text reference "R796" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2024 "FBF0_CLK0_R"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 225 "FBF0_CLK0"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 162.900708 128.601412)
    (fp_text reference "C674" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 109.038509 100.662098)
    (fp_text reference "C894" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 240.104313 108.726115)
    (fp_text reference "R552" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "PS5_NVVDD_PHASE5"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 929 "PS5_NVVDD_VAMP_CSSUM"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 128.559908 101.423412)
    (fp_text reference "C747" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1573 "FBABCD_MPLL_AVDD"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 64.119117 119.162492)
    (fp_text reference "C1056" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2027 "FBG1_CLK0_R"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 73.391616 73.737615)
    (fp_text reference "R773" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 220 "FBF_CMD<4>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 175.384808 82.508718 -90)
    (fp_text reference "C560" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 175.461008 106.749512 90)
    (fp_text reference "C555" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 170.012708 130.09262 180)
    (fp_text reference "C632" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 822 "FBA_VREF4"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 116.143905 129.959016 90)
    (fp_text reference "C842" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 169.132293 94.406103 90)
    (fp_text reference "R637" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2015 "FBB1_CLK0_R"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 683 "FBB1_CLK0"))
  )
  (footprint "0603_1" (layer "B.Cu")
    (tedit 0)
    (at 124.876908 140.006012 -90)
    (fp_text reference "C772" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.762 0 90) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1972 "PEX_PLLVDD_OP"))
    (pad "2" smd rect (at -0.762 0 270) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 111.340207 100.636698)
    (fp_text reference "C875" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 104.836308 121.210012 -90)
    (fp_text reference "C924" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0603_1" (layer "B.Cu")
    (tedit 0)
    (at 198.867108 68.136407 90)
    (fp_text reference "C534" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.762 0 270) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1001 "5V_INPUT"))
    (pad "2" smd rect (at -0.762 0 90) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 92.824115 62.409012 -90)
    (fp_text reference "C981" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "1206_1" (layer "B.Cu")
    (tedit 0)
    (at 241.742308 130.582307)
    (fp_text reference "R545" (at -1.0795 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 1.4732 0) (size 1.27 1.5748) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "INPUT_PEX6_IN2"))
    (pad "2" smd rect (at -1.4732 0) (size 1.27 1.5748) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 983 "12V_PEX6_F2"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 175.461008 121.671504 90)
    (fp_text reference "C556" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 72.675819 82.846817 180)
    (fp_text reference "C1011" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 171.110013 117.958812)
    (fp_text reference "R623" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 821 "FBA_VREF3"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 31.481108 91.822415 90)
    (fp_text reference "R870" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1843 "DVIA_D2"))
  )
  (footprint "1206_1" (layer "B.Cu")
    (tedit 0)
    (at 219.720508 58.522507 -90)
    (fp_text reference "F501" (at 0 1.0795 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 1.4732 0 270) (size 1.27 1.5748) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2080 "SPDIF_GND"))
    (pad "2" smd rect (at -1.4732 0 270) (size 1.27 1.5748) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 37.848913 102.490212 -90)
    (fp_text reference "C1136" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1662 "NVIO_GV_PLLVDD"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 115.941213 102.538396 90)
    (fp_text reference "C844" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 198.295608 57.404907 -90)
    (fp_text reference "R609" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1913 "5V_ADJ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "IND_SMD_0402_1" (layer "B.Cu")
    (tedit 0)
    (at 40.515405 101.1798 180)
    (fp_text reference "LB508" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.6858 0.5334) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1662 "NVIO_GV_PLLVDD"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.6858 0.5334) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
  )
  (footprint "IND_SMD_0402_1" (layer "B.Cu")
    (tedit 0)
    (at 26.883708 119.381212 -90)
    (fp_text reference "LB509" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.6858 0.5334) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.6858 0.5334) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1698 "IFPAB_PLLVDD"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 18.298508 98.502412 -90)
    (fp_text reference "C1222" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1725 "IFPCD_IOVDD"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 122.721997 60.828319 -90)
    (fp_text reference "C791" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2021 "FBD1_CLK0_R"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 63.809212 93.802802 180)
    (fp_text reference "R822" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 41 "FBF_VREF3"))
  )
  (footprint "0603_1" (layer "B.Cu")
    (tedit 0)
    (at 120.076308 98.400812 -90)
    (fp_text reference "C807" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.762 0 90) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.762 0 270) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 215.910508 92.025107 90)
    (fp_text reference "R598" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 994 "PS5_NVVDD_LG2_AC"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 64.051299 78.885916 180)
    (fp_text reference "R820" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 229 "FBF_VREF1"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 31.633508 134.595812 180)
    (fp_text reference "C1154" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1961 "PS1_1V15_BOOT"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 6 "PS1_1V15_PH"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 239.761108 136.652907 -90)
    (fp_text reference "R554" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1975 "FAN_TACH"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 70.526013 117.501612)
    (fp_text reference "R781" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 167 "FBG_CMD<24>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 59.565913 115.461712 90)
    (fp_text reference "C1102" (at 0 -1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 44.117608 148.209907 180)
    (fp_text reference "R844" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 973 "GPIO9_THERM_ALERT*"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 9.891108 110.694615)
    (fp_text reference "R935" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1681 "DACA_RED"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 68.532799 93.785098 180)
    (fp_text reference "C1034" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 112.634413 58.116615 -90)
    (fp_text reference "C868" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 64.024807 89.276802)
    (fp_text reference "C1057" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2025 "FBF1_CLK0_R"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 70.725099 103.315915 180)
    (fp_text reference "R780" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 99 "FBG_CMD<1>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 120.847401 100.636698 180)
    (fp_text reference "C805" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 215.910508 143.345807 90)
    (fp_text reference "R602" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 995 "PS5_NVVDD_LG3_AC"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0603_1" (layer "B.Cu")
    (tedit 0)
    (at 123.048108 147.321212 180)
    (fp_text reference "C786" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.762 0) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at -0.762 0 180) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 164.021915 98.598602)
    (fp_text reference "C667" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 173.483415 89.124402)
    (fp_text reference "C586" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 24.841497 99.1081 180)
    (fp_text reference "C1197" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1673 "DACB_VDD"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0603_1" (layer "B.Cu")
    (tedit 0)
    (at 108.849508 132.309812 90)
    (fp_text reference "C896" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.762 0 270) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1484 "GV_PLLAVDD"))
    (pad "2" smd rect (at -0.762 0 90) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 89.621708 60.478307 -90)
    (fp_text reference "C985" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 173.483415 98.731698 180)
    (fp_text reference "C588" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 242.390287 110.123115)
    (fp_text reference "R543" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 959 "PS5_NVVDD_ISEN6"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 13 "PS5_NVVDD_PHASE6"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 111.840612 126.73121 -90)
    (fp_text reference "C873" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 142.646723 61.379016 90)
    (fp_text reference "C708" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 116.952108 105.004812 90)
    (fp_text reference "C833" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 74.153108 67.895412 180)
    (fp_text reference "C1007" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 218.653708 137.516507 90)
    (fp_text reference "R595" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 984 "PS5_NVVDD_UG3_R"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 10 "PS5_NVVDD_PHASE3"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 66.671309 66.922998 180)
    (fp_text reference "R800" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 230 "FBF_VREF2"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 61.467307 69.324898)
    (fp_text reference "C1075" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 35.689405 100.5956)
    (fp_text reference "C1141" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1664 "NVIO_SP_PLLVDD"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 175.384808 97.43071 -90)
    (fp_text reference "C562" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 68.514816 92.510018 180)
    (fp_text reference "R789" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 20 "FBF_CMD<26>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 106.946997 102.543501 90)
    (fp_text reference "C911" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0603_1" (layer "B.Cu")
    (tedit 0)
    (at 35.494308 84.938507 -90)
    (fp_text reference "C1143" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.762 0 90) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "2" smd rect (at -0.762 0 270) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1045 "PS3_PVCC5_DRV"))
  )
  (footprint "SOT23_1" (layer "B.Cu")
    (tedit 0)
    (at 56.944608 133.795407 -90)
    (fp_text reference "Q509" (at 1.23825 -1.23825 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 1.143 270) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1051 "GPU_RST_R*"))
    (pad "2" smd rect (at -0.9525 1.143 270) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "3" smd rect (at 0 -1.143 270) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1982 "GPU_RST_R_MOS"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 170.881413 59.279402 180)
    (fp_text reference "C621" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 561 "FBC_VREF3"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 27.925108 119.381212 -90)
    (fp_text reference "C1170" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 171.545801 80.607299 180)
    (fp_text reference "C607" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 64.970017 67.375194 -90)
    (fp_text reference "R814" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 230 "FBF_VREF2"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 137.566697 67.4343 90)
    (fp_text reference "C716" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 173.483415 138.495906 180)
    (fp_text reference "C598" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 23.214907 118.824596 90)
    (fp_text reference "R901" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1689 "DACC_GREEN"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 218.933108 86.056107 90)
    (fp_text reference "R591" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 988 "PS5_NVVDD_UG2_R"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 14 "PS5_NVVDD_PHASE2"))
  )
  (footprint "DIODE_SMD_SMA_1" (layer "B.Cu")
    (tedit 0)
    (at 203.058108 142.748907 -90)
    (fp_text reference "D517" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -1.880108 0 270) (size 2.159 2.032) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 10 "PS5_NVVDD_PHASE3"))
    (pad "2" smd rect (at 1.880108 0 270) (size 2.159 2.032) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 39.145304 107.4139 90)
    (fp_text reference "C1132" (at 0 -1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1661 "NVIO_GV_PLLAVDD"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 172.273308 100.247595 180)
    (fp_text reference "C601" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 107.884308 122.480012 -90)
    (fp_text reference "C901" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 162.595908 68.911412)
    (fp_text reference "C676" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 142.646723 58.17661 -90)
    (fp_text reference "C707" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 122.719915 58.17661 -90)
    (fp_text reference "C793" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 109.586108 111.608812 90)
    (fp_text reference "C888" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 204.772608 59.119407 90)
    (fp_text reference "R605" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1956 "SPDIF_IN"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1991 "SPDIF_IN_C"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 234.096908 112.421307)
    (fp_text reference "R564" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1031 "PS5_NVVDD_BOOT5"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1004 "PS5_NVVDD_BOOT5_RC"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 221.384208 114.161207 90)
    (fp_text reference "R588" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1033 "PS5_NVVDD_LG5"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2087 "PS5_NVVDD_LG5_D"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 247.787508 116.790107 180)
    (fp_text reference "R523" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 999 "NVVDD_SENSE_R"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1554 "NVVDD_SENSE"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 38.872508 103.658612 90)
    (fp_text reference "C1133" (at 0 -1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1662 "NVIO_GV_PLLVDD"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "IND_SMD_0402_1" (layer "B.Cu")
    (tedit 0)
    (at 44.130308 99.365707 -90)
    (fp_text reference "LB506" (at 0 1.5875 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.6858 0.5334) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "1V15"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.6858 0.5334) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1664 "NVIO_SP_PLLVDD"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 169.651012 144.900795 180)
    (fp_text reference "R636" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 880 "FBA_VREF2"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 69.473412 112.75961)
    (fp_text reference "C1030" (at -1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 32.514405 106.0058 180)
    (fp_text reference "C1146" (at 1.5875 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1790 "2V5"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 32.751108 95.073615 90)
    (fp_text reference "R866" (at 0 -1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1842 "DVIA_D1"))
    (pad "2" smd rect (at -0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1009 "3V3"))
  )
  (footprint "SOT23_1" (layer "B.Cu")
    (tedit 0)
    (at 206.487108 62.294407)
    (fp_text reference "Q503" (at 1.23825 1.23825 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 1.143) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1993 "SPDIF_IN_COMP2_D"))
    (pad "2" smd rect (at -0.9525 1.143) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "3" smd rect (at 0 -1.143) (size 0.9144 0.9144) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1957 "SPDIF_IN_COMP2_Q"))
  )
  (footprint "0805_1" (layer "B.Cu")
    (tedit 0)
    (at 145.679508 124.283615)
    (fp_text reference "C702" (at -0.7874 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.9525 0) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NVVDD"))
    (pad "2" smd rect (at -0.9525 0) (size 1.143 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0603_1" (layer "B.Cu")
    (tedit 0)
    (at 101.483508 101.499612)
    (fp_text reference "C955" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.762 0 180) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1282 "FBEFGH_MPLL_AVDD"))
    (pad "2" smd rect (at -0.762 0) (size 0.889 0.7874) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 173.483415 104.04741)
    (fp_text reference "C589" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 175.384808 67.58571 -90)
    (fp_text reference "C558" (at 0 1.27 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 67.956016 96.038815 180)
    (fp_text reference "R791" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 97 "FBG_CMD<0>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 66.665417 65.874308 180)
    (fp_text reference "R801" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 222 "FBF_CMD<0>"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 122.057508 98.959612)
    (fp_text reference "C799" (at -1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 173.483415 113.654706 180)
    (fp_text reference "C592" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
  )
  (footprint "0402_1" (layer "B.Cu")
    (tedit 0)
    (at 157.947708 138.126412 180)
    (fp_text reference "R693" (at 1.27 0 unlocked) (layer "B.SilkS"))
    (fp_text value "{Value}" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.5334 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "FBVDDQ"))
    (pad "2" smd rect (at -0.5334 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 870 "FBA_CMD<4>"))
  )
)
